3GPP TSG-RAN WG4 Meeting # 98-e R4-210xxxx

Electronic Meeting, Jan. 25-Feb. 5, 2021

**Agenda item:** 7.10.1

**Source:** Moderator (China Telecom)

**Title:** Email discussion summary for [98e][325] NR\_DL256QAM\_FR2\_Demod

**Document for:** Information

# Introduction

This email thread discusses the demodulation and CSI reporting requirements for FR2 DL 256QAM in agenda 7.10.1.

List of candidate target of email discussion for 1st round and 2nd round:

* 1st round: Invite companies to provide comments (if any) on open issues and CRs in section 1.3, 2.3 and 3.3.
* 2nd round: TBD

# Topic #1: PDSCH normal demodulation requirements

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| [R4-2100880](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98_e/Docs/R4-2100880.zip) | China Telecom | Offline e-mail discussion summary on the TDLD30 channel simplification |
| [R4-2100881](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98_e/Docs/R4-2100881.zip) | China Telecom | Simulation results. |
| R4-2101116 | ZTE corporation | CR on demodulation performance requirements for DL 256QAM for FR2 |
| [R4-2101250](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98_e/Docs/R4-2101250.zip) | Intel Corporation | Proposal 1: Use the following channel model for FR2 256QAM requirements:   |  |  |  |  | | --- | --- | --- | --- | | Tap # | Delay | Power | Fading distribution | | 1 | 0 | -0.2 | LOS path | | 0 | -12.4 | Rayleigh | | 2 | 20 | -21 | Rayleigh | | 3 | 40 | -16.7 | Rayleigh | | 4 | 55 | -18.3 | Rayleigh | | 5 | 80 | -21.9 | Rayleigh | | 6 | 120 | -27.8 | Rayleigh | | 7 | 240 | -23.6 | Rayleigh | | 8 | 285 | -24.8 | Rayleigh | | 9 | 290 | -30.0 | Rayleigh | | 10 | 375 | -27.6 | Rayleigh | |
| R4-2101251 | Intel Corporation | Simulation result summary. |
| [R4-2101252](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98_e/Docs/R4-2101252.zip) | Intel Corporation | CR on simplified TDL-D channel model for FR2 DL 256QAM demodulation requirements |
| [R4-2101296](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98_e/Docs/R4-2101296.zip) | Huawei, HiSilicon | Simulation results |
| [R4-2101297](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98_e/Docs/R4-2101297.zip) | Huawei, HiSilicon | CR on applicability and FRC for PDSCH normal demodulation for DL 256QAM for FR2 |
| R4-2101369 | NTT DOCOMO, INC. | In this contribution, we present our views on 256QAM UE requirements for FR2. Our observation is summarized below.  Observation 1  Table 1. Summary of ideal simulation results   |  |  | | --- | --- | | Channel Model | SNR point (dB) @70%TP  Using MCS index:20 | | TDLD  30-75 | 16.5 dB | |
| [R4-2101419](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98_e/Docs/R4-2101419.zip) | Ericsson | Simulation results |
| [R4-2101420](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98_e/Docs/R4-2101420.zip) | Ericsson | Proposal 1: Define DL 256QAM PDSCH demodulation requirements in FR2 with TDLD30-75.  Proposal 2: Specify the following path delay profile for TDLD30 in TS38.101-4 B.2.1.2.   |  |  |  |  | | --- | --- | --- | --- | | Tap # | Delay [ns] | Power [dB] | Fading distribution | | 1 | 0 | -0.2 | LOS path | | 1 | 0 | -12.4 | Rayleigh | | 2 | 20 | -21.0 | Rayleigh | | 3 | 40 | -16.7 | Rayleigh | | 4 | 55 | -18.3 | Rayleigh | | 5 | 80 | -21.9 | Rayleigh | | 6 | 120 | -27.8 | Rayleigh | | 7 | 240 | -23.6 | Rayleigh | | 8 | 285 | -24.8 | Rayleigh | | 9 | 290 | -30.0 | Rayleigh | | 10 | 375 | -27.6 | Rayleigh | | Note 1: Tap #1 follows a Ricean distribution.  Note 2: LOS path applies the channel matrix specified in B.1 according to the antenna configuration. | | | |   Proposal 3: Add the following note in the delay profile simplification procedure in TS38.101-4 B.2.1:  Note: The paths containing both LOS path and Rayleigh distribution are considered as single path. |
| R4- 2102373 | Qualcomm Incorporated | Simulation result. |

## Open issues summary

### PDSCH normal test parameters

**Issue 1-1: Simplification of TDLD30 channel model in TS 38.101-4**

* *Agreement in RAN4 #97e (R4-2017536, WF)*
  + *Specification of TDLD30 channel model into TS38.101-4*
    - *Option 1: derived using only Steps 1-5 from methodology in Section B.2.1 of TS 38.101-4 for Rayleigh components*

|  |  |  |  |
| --- | --- | --- | --- |
| *Tap #* | *Delay* | *Power in [dB]* | *Fading distribution* |
| *1* | *0* | *-0.2* | *LOS path* |
| *0* | *-12.4* | *Rayleigh* |
| *2* | *20* | *-21* | *Rayleigh* |
| *3* | *40* | *-16.7* | *Rayleigh* |
| *4* | *55* | *-18.3* | *Rayleigh* |
| *5* | *80* | *-21.9* | *Rayleigh* |
| *6* | *120* | *-27.8* | *Rayleigh* |
| *7* | *240* | *-23.6* | *Rayleigh* |
| *8* | *285* | *-24.8* | *Rayleigh* |
| *9* | *290* | *-30.0* | *Rayleigh* |
| *10* | *375* | *-27.7* | *Rayleigh* |

* + - *Option 2:*

|  |  |  |  |
| --- | --- | --- | --- |
| *Tap #* | *Delay* | *Power in [dB]* | *Fading distribution* |
| *1* | *0* | *-0.2* | *LOS path* |
| *0* | *-13.5* | *Rayleigh* |
| *2* | *2* | *-18.8* | *Rayleigh* |
| *3* | *18* | *-21* | *Rayleigh* |
| *4* | *40* | *-22.8* | *Rayleigh* |
| *5* | *42* | *-17.9* | *Rayleigh* |
| *6* | *54* | *-18.3* | *Rayleigh* |
| *7* | *78* | *-21.9* | *Rayleigh* |
| *8* | *122* | *-27.8* | *Rayleigh* |
| *9* | *238* | *-23.6* | *Rayleigh* |
| *10* | *282* | *-24.8* | *Rayleigh* |
| *11* | *292* | *-30* | *Rayleigh* |
| *12* | *376* | *-27.7* | *Rayleigh* |

* + - *Companies are encouraged to check if the above option 1 is agreeable and provide feedback in RAN4 draft reflector during 16th - 27th Nov after the meeting.*
* *Consensus in offline e-mail discussion*
  + *For the two components with 0 ns delay in TDLD (one with LOS path, the other with Rayleigh distribution), are they considered as two taps or one tap from the TE implementation perspective?*
    - *Proposed agreement: One tap*
  + *Final proposal on the simplified TDLD channel*
    - *Proposed agreement: Use Intel’s proposal with adjusting the power of tap#10 to -27.6dB (Target DS is 30ns).*

|  |  |  |  |
| --- | --- | --- | --- |
| *Tap #* | *Delay* | *Power in [dB]* | *Fading distribution* |
| *1* | *0* | *-0.2* | *LOS path* |
| *0* | *-12.4* | *Rayleigh* |
| *2* | *20* | *-21* | *Rayleigh* |
| *3* | *40* | *-16.7* | *Rayleigh* |
| *4* | *55* | *-18.3* | *Rayleigh* |
| *5* | *80* | *-21.9* | *Rayleigh* |
| *6* | *120* | *-27.8* | *Rayleigh* |
| *7* | *240* | *-23.6* | *Rayleigh* |
| *8* | *285* | *-24.8* | *Rayleigh* |
| *9* | *290* | *-30.0* | *Rayleigh* |
| *10* | *375* | *-27.6* | *Rayleigh* |

* Proposals on the channel model for simulation:
  + Option 1: Use following model and confirm negligible performance difference compared with the original TDLD30 channel model in TR 38.901 (Intel, E///, offline discussion proposal in [R4-2100880](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98_e/Docs/R4-2100880.zip))

|  |  |  |  |
| --- | --- | --- | --- |
| Tap # | Delay | Power in [dB] | Fading distribution |
| 1 | 0 | -0.2 | LOS path |
| 0 | -12.4 | Rayleigh |
| 2 | 20 | -21 | Rayleigh |
| 3 | 40 | -16.7 | Rayleigh |
| 4 | 55 | -18.3 | Rayleigh |
| 5 | 80 | -21.9 | Rayleigh |
| 6 | 120 | -27.8 | Rayleigh |
| 7 | 240 | -23.6 | Rayleigh |
| 8 | 285 | -24.8 | Rayleigh |
| 9 | 290 | -30.0 | Rayleigh |
| 10 | 375 | -27.6 | Rayleigh |

* Proposals on the additional notes for the 38.101-4 CR on the simplified TDLD30 channel model
  + Option 1: (Intel)
    - 1 additional note in clause B.2.1: ‘Delay profile for TDLD30 is generated under assumption that Steps 1-8 are applied for taps with Rayleigh distribution.’
  + Option 2: (E///)
    - 1 additional note in clause B.2.1: ‘The paths containing both LOS path and Rayleigh distribution are consider as single path.’
* E///: Avoid the confusion if RAN4 decide to define new PDP in the future.
  + - 2 additional notes in Table B.2.1.2-4 as below:
* ‘Note 1: Tap #1 follows a Ricean distribution.’
* ‘Note 2: LOS path applies the channel matrix specified in B.1 according to the antenna configuration.’
* Recommendation for the first-round
  + On the channel model for simulation
    - Use option1.
  + On the additional note for the 38.101-4 CR on the simplified TDLD30 channel model
    - Encourage feedback from more companies.

**Issue 1-2: Propagation condition**

* *Agreement in RAN4 #97e (R4-2017536, WF)*
  + *Propagation condition*
    - *Introduce test case with TDLD30-75 based on the assumption that we can complete the work for introducing TDL-D channel model into specification in RAN4#98e. If no conclusion for introducing TDL-D channel model in RAN4#98e, then RAN4 will adopt TDLA30-300 instead of TDLD30-75.*
* Proposals:
  + Option 1: TDLD30-75 (E///)
* Recommendation for the first-round
  + Use option1 if the proposed simplified TDLD30 channel model for simulation in issue 1-1 can be agreeable.

**Issue 1-3: Simulation results and SNR requirement for PDSCH normal demodulation**

* *Agreement in RAN4 #97e (R4-2017536, WF)*
  + *Propagation condition*
    - *In RAN4#98e, companies provide simulation results (including 70%TP ideal and impairment SNR points and TP curves) in the template provided by Intel.*
* Recommendation for the first-round
  + Companies to provide and align the simulation results in the summary template by 6pm UTC Jan 27th.
  + Add the requirement value with [] in the CR in this meeting.

## Companies views’ collection for 1st round

### Open issues

|  |  |
| --- | --- |
| **Company** | Comments collection for 1st round |
| XXX | **Issue 1-1: Simplification of TDLD30 channel model in TS 38.101-4**  **Issue 1-2: Propagation condition**  **Issue 1-3: Simulation results and SNR requirement for PDSCH normal demodulation**  **Others** |
|  |  |
|  |  |
|  |  |

### CRs

|  |  |
| --- | --- |
| **CR/TP number** | **Comments** |
| R4-2101116: CR on demodulation performance requirements, ZTE | Moderator’s note: Resubmission of endorsed Draft CR R4-2017537 without additional update. This CR should be a category B CR. |
|  |
|  |
|  |
|  |
| [R4-2101252](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98_e/Docs/R4-2101252.zip): CR on simplified TDL-D channel model, Intel |  |
|  |
|  |
|  |
|  |
| [R4-2101297](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98_e/Docs/R4-2101297.zip), CR on applicability and FRC for PDSCH normal demodulation, Huawei | Moderator’s note: Resubmission of endorsed Draft CR R4-2015596 without additional update. |
|  |
|  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary** |
|  |  |

### CRs

*Moderator tries to summarize discussion status for 1st round and provides recommendation on CRs/TPs Status update*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation** |
|  |  |
|  |  |
|  |  |

## Discussion on 2nd round

## Summary on 2nd round

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation** |
| XXX | *Based on 2nd round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |
|  |  |
|  |  |
|  |  |
|  |  |

# Topic #2: SDR requirements

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| [R4-2100885](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98_e/Docs/R4-2100885.zip) | China Telecom | ***Proposal 1:*** *Add following row in Table 7.1.1.3-1 of TS 38.101-4 (marked yellow), and no additional change is needed to the test requirement in clause 7.5A.1 in TS 38.101-4.*   |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | | **7.1.1.3 Applicability of requirements for optional UE features** The performance requirements in Table 7.1.1.3-1 shall apply for UEs which support optional UE features only.  Table 7.1.1.3-1: Requirements applicability for optional UE features   |  |  |  |  |  | | --- | --- | --- | --- | --- | | UE feature/capability [14] | Test type | | Test list | Applicability notes | | SU-MIMO Interference Mitigation advanced receiver | FR2 TDD | PDSCH | Clause 7.2.2.2.1 (Test 3-1) |  | | Basic DL NR-NR CA operation (*supportedBandCombinationList*) | NR CA | SDR | Clause 7.5A.1 | 1) Up to 16 DL carriers  2) Same numerology across carrier for data/control channel at a given time | | PDSCH repetitions over multiple slots *(pdsch-RepetitionMultiSlots)* | FR2 TDD | PDSCH | Clause 7.2.2.2.2 |  | | 256QAM for PDSCH  (*pdsch-256QAM-FR2*) | FR2 TDD | SDR | Clause 7.5A.1 | For UE capable of PDSCH 256QAM for certain band(s), the MCS table is configured to ‘*64QAM*’ for SDR test, i.e., no additional SDR test for UE capable of PDSCH 256QAM feature. | | |
| [R4-2101299](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98_e/Docs/R4-2101299.zip) | Huawei, HiSilicon | CR on SDR requirements for DL 256QAM for FR2 |

## Open issues summary

**Issue 2-1: Applicability of SDR requirements for UE capable of 256QAM in certain band(s)**

* Proposals:
  + Option 1: Add following applicability in Table 7.1.1.3-1 and no additional change is needed to the test requirement in clause 7.5A.1 in TS 38.101-4 (CTC, [R4-2100885](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98_e/Docs/R4-2100885.zip))

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Table 7.1.1.3-1: Requirements applicability for optional UE features   |  |  |  |  |  | | --- | --- | --- | --- | --- | | UE feature/capability [14] | Test type | | Test list | Applicability notes | | 256QAM for PDSCH  (*pdsch-256QAM-FR2*) | FR2 TDD | SDR | Clause 7.5A.1 | For UE capable of PDSCH 256QAM for certain band(s), the MCS table is configured to ‘*64QAM*’ for SDR test, i.e., no additional SDR test for UE capable of PDSCH 256QAM feature. | |

* + Option 2: Add following notes in Table 7.5A.1-3 in the test requirement in clause 7.5A.1 in TS 38.101-4 (HW, [R4-2101299](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98_e/Docs/R4-2101299.zip))
    - Note 1: MCS Index is based on MCS index Table 1 defined in clause 5.1.3.1 of TS 38.214 [12].
    - Note 2: For the band(s) on which UE supporting “Maximum modulation format” of 8, the MCS index is derived from the rows with “Maximum modulation format” of 6.
* Recommendation for the first-round
  + Encourage feedback from more companies.

## Companies views’ collection for 1st round

### Open issues

|  |  |
| --- | --- |
| **Company** | Comments collection for 1st round |
| XXX | **Issue 2-1: Applicability of SDR requirements for UE capable of 256QAM in certain band(s)**  **Others** |
|  |  |
|  |  |
|  |  |

### CRs

|  |  |
| --- | --- |
| **CR/TP number** | **Comments** |
| [R4-2101299](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98_e/Docs/R4-2101299.zip), CR on SDR requirements, Huawei |  |
|  |
|  |
|  |

## Summary for 1st round

### CRs

*Moderator tries to summarize discussion status for 1st round and provides recommendation on CRs/TPs Status update*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation** |
| XXX | *Based on 1st round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |
|  |  |

# Topic #3: CQI reporting requirements

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| [R4-2100882](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98_e/Docs/R4-2100882.zip) | China Telecom | This paper provided simulation results and discussed the open issues on the CQI reporting requirements for FR2 DL 256QAM.  The following observations and proposal were given for CQI reporting requirements:  Observation 1: 256QAM corresponding CQI index (CQI > 11) can be reported with around 50% possibility when the SNR point is 17/18 dB, in which case 256QAM can be considered covered without testability issue.  Observation 2: For UEs supporting DL 256QAM in FR2, the capability of reporting CQI indexes corresponding 256QAM under proper scenario should be verified. Otherwise, it will remain uncertainty that whether 256QAM will be correctly scheduled.  Proposal 1: Configure the higher SNR point as 17/18dB for CQI reporting requirements under fading condition. |
| R4-2100883 | China Telecom | Summary of simulation results. |
| [R4-2100884](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98_e/Docs/R4-2100884.zip) | China Telecom | CR on adding applicability, requirements and measurement channel for FR2 DL 256QAM CQI reporting test under fading condition |
| [R4-2101114](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98_e/Docs/R4-2101114.zip) | ZTE Corporation | In this contribution, we provide our simulation result on CQI reporting requirements for FR2 DL 256QAM. In summary, we make the following proposal:  Proposal: Support the SNR point 18 dB for CQI reporting requirements if the SNR point in the testable SNR range. |
| [R4-2101253](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98_e/Docs/R4-2101253.zip) | Intel Corporation | CR on applicability rules and FRC for FR2 DL 256QAM CQI requirements |
| R4-2101298 | Huawei, HiSilicon | Not available. |
| [R4-2101421](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98_e/Docs/R4-2101421.zip) | Ericsson | Simulation result. |
| [R4-2101422](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98_e/Docs/R4-2101422.zip) | Ericsson | Observation 1: SNR testing points for 256QAM in CQI table 2 should be 19dB or more if the purpose of this test is to make sure UE report CQI index corresponding to 256QAM, regardless of TDLA30-35 or TDLD30-75.  Observation 2: Percentage of reported CQI not in {medCQI-1, medCQI, medCQI+1} is more than 20% in SNR rage between 0dB to 22dB for TDLA30-35, but almost 0% for TDLD30-75.  Observation 3: BLER of PDSCH with the followed CQI is more than 5% in SNR range from 1dB to 22dB for both TDLA30-35 and TDLD30-75.  Observation 4: TP ratio with following CQI and fixed median CQI is more than 1.1 in SNR ranges from 0dB to 12dB, and 16dB to 23dB for TDLA30-35, but TP ratio becomes below 1.0 with some test points for TDLD30-75.  Proposal 1: RAN4 specify the FR2 CQI reporting requirements with CQI table 2 in FR2 with TDLA30-35.  Proposal 2: RAN4 set the SNR test points and requirements for FR2 CQI reporting test under fading condition as follows:   |  |  |  |  | | --- | --- | --- | --- | | SNR test points (dB) | α: Minimum percentage (%) of reported CQI not in {median CQI – 1, median CQI, median CQI + 1} | γ: Minimum TP ratio of followed CQI and fixed median CQI | Minimum PDSCH BLER with followed CQI | | 6 and 7 | 20% | 1.1 | 0.02 | | 17 and 18 | 20% | 1.1 | 0.02 | |
| R4-2101848 | Huawei, HiSilicon | Withdrawn. |
| R4- 2102406 | Qualcomm Incorporated | Proposal 1: Define FR2 256QAM CQI reporting test for at least 21dB SNR to see the impact of 256QAM CQI table. |

## Open issues summary

### CQI test parameters

**Issue 3-1: SNR testing point for FR2 CQI Table 2 test**

* *Agreement in RAN4 #97e (R4-2017536, WF)*
  + *Fading CQI test cases under rank1 transmission with CQI table 2:*
    - *SNR: FFS for higher test points*
    - *Options for further consideration:*
* *Option 1: 17/18 dB*
* *Other options are not precluded.*
* Proposal
  + Option 1: 17/18 dB (CTC, [ZTE], E///)
    - CTC: 256QAM corresponding CQI index (CQI > 11) can be reported with around 50% possibility when the SNR point is 17/18 dB, in which case 256QAM can be considered covered without testability issue.
    - ZTE: Considering the simulation result and the information, we could support the SNR point 18dB for CQI reporting requirements if the SNR point in the testable SNR range.
    - E///: Propose to set SNR to 17/18dB in the CQI table 2 reporting tests in FR2, because testability is more important.
  + Option 2: At least 19dB without impairments (21dB with adding 2dB for impairment) (QC)
    - QC: Following CQI throughput with 256QAM CQI table has significant gain compared to following 64QAM CQI table starting at 19dB SNR. Adding 2dB for impairments, RAN4 should define the 256QAM CQI reporting requirements at least for 21dB SNR.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **SNR (dB)** | **Median CQI (256QAM)** | **Percentage not in Median CQI+/-1** | **Percentage 256QAM CQI > 11** | **Following 256QAM CQI BLER** | **Following 256QAM CQI Thpt** | **Following 64QAM CQI Thpt** |
| 17 | 10 | 33.62 | 22.17 | 0.08 | 58.7 | 57.2 |
| 18 | 10 | 36.91 | 29.84 | 0.08 | 61.5 | 58.7 |
| 19 | 11 | 34.59 | 39.22 | 0.07 | 65.3 | 60.2 |
| 20 | 11 | 34.84 | 49.94 | 0.07 | 68.1 | 61.3 |

* Recommendation for the first round
  + Among all companies’ simulation results under SNR 17/18 dB without impairments, since 22%~47% of the reported CQI indexes have covered 256QAM, can we go with option 1 based on majority’s view?

**Issue 3-2: Propagation condition for FR2 CQI Table 2 test**

* *Agreement in RAN4 #97e (R4-2017536, WF)*
  + *If it is agreed to define FR2 CQI reporting test for CQI table 2,* 
    - *Use channel bandwidth of 50MHz and reuse the other parameters in Rel-15 FR2 CQI tests, i.e., parameters in Table 8.2.2.2.2.1-1 in TS38.101-4.*
* Proposal
  + Option 1: TDLA30-35 (E///, Last meeting’s agreement in the WF)
* Recommendation for the first round
  + Confirm to use TDLA30-35 for FR2 CQI Table2 test.

**Issue 3-3: Test metric for FR2 CQI Table 2 test**

* Proposal:

|  |  |  |
| --- | --- | --- |
| **Test metric under SNR 6/7/17/18 dB** | | |
|  | Option 1 (E///) | Option 2 (Existing test requirements in Rel-15 FR2 CQI table 1 Test with 100MHz CBW) |
| α: Minimum percentage (%) of reported CQI not in {median CQI – 1, median CQI, median CQI + 1} | 20% | 2% |
| γ: Minimum TP ratio of followed CQI and fixed median CQI | 1.1 | 1.05 |
| Minimum PDSCH BLER with followed CQI | 0.02 | 0.01 |

* Recommendation for the first round
  + Encourage more companies’ feedback during the first-round discussion.

## Companies views’ collection for 1st round

### Open issues

|  |  |
| --- | --- |
| **Company** | Comments collection for 1st round |
| XXX | **Issue 3-1: SNR testing point for FR2 CQI Table 2 test**  **Issue 3-2: Propagation condition for FR2 CQI Table 2 test**  **Issue 3-3: Test requirement for FR2 CQI Table 2 test**  **Others** |
|  |  |

### CR

|  |  |
| --- | --- |
| **CR/TP number** | **Comments** |
| R4-2100884: CR on applicability, requirements and measurement channel, CTC | Moderator’s note: According to the updated WP agreed in the last meeting (R4-2014674), the CR on applicability and FRC is scheduled to be provided by Intel. |
|  |
|  |
|  |
|  |
| [R4-2101253](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98_e/Docs/R4-2101253.zip): CR on applicability rules and FRC, Intel |  |
|  |
|  |
|  |
|  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary** |
|  |  |

### CRs

*Moderator tries to summarize discussion status for 1st round and provides recommendation on CRs/TPs Status update*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation** |
| XXX | *Based on 1st round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |
|  |  |

## Discussion on 2nd round

## Summary on 2nd round

*Moderator tries to summarize discussion status for 2nd round and provided recommendation on CRs/TPs/WFs/LSs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation** |
| XXX | *Based on 2nd round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |
|  |  |