**3GPP TSG-RAN WG4 Meeting #99-e R4-2111087**

**Electronic Meeting, 19 May – 27 May 2021**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **-1** | **CR** | **0847** | **rev** | **1** | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR for corrections 38.101-1 |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_CADC\_R17\_2BDL\_xBUL |  | ***Date:*** | 2021-05-19 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Corrections 38.101-1 |
|  |  |
| ***Summary of change:*** | Adding missing cross band isolation for CA\_n41-n77 for the n77 UL case |
|  |  |
| ***Consequences if not approved:*** | Corrections 38.101-1 are not made |
|  |  |
| ***Clauses affected:*** | 5.5 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** | **X** |  |  Test specifications | TS 38.521-3 |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

---Start of changes---

Table 7.3A.6-1: Reference sensitivity exceptions (MSD) due to cross band isolation for NR CA FR1

|  |
| --- |
| NR Band / Channel bandwidth of the affected DL band |
| UL band | DL band | 5MHz (dB) | 10MHz (dB) | 15MHz (dB) | 20MHz (dB) | 25MHz (dB) | 30 MHz (dB) | 40 MHz (dB) | 50 MHz (dB) | 60 MHz (dB) | 70MHz(dB) | 80 MHz (dB) | 90 MHz (dB) | 100 MHz (dB) |
| n1 | n3 | 3 | 2.2 | 1.9 | 1.7 | 1.6 | 1.5 |  |  |  |  |  |  |  |
| n1 | n40 | 6.6 | 6.6 | 6.6 | 6.6 | 6.6 | 6.6 | 6.6 | 6.6 | 6.6 |  | 6.6 |  |  |
| n1 | n41 |  | 6.1 | 6.1 | 6.1 |  |  | 6.1 | 6.1 | 6.1 |  | 6.1 | 6.1 | 6.1 |
| n3 | n41 |  | 0.7 | 0.7 | 0.7 |  |  | 0.7 | 0.7 | 0.7 |  | 0.7 | 0.7 | 0.7 |
| n38 | n78 |  | 8.3 | 8.3 | 8.3 | 7.3 | 6.5 | 6.3 | 5.3 | 4.5 |  | 4.0 | 3.9 | 3.8 |
| n40 | n1 | 8.3 | 8.3 | 8.3 | 8.3 |  |  |  |  |  |  |  |  |  |
| n41 | n1 | 9.1 | 9.1 | 9.1 | 9.1 |  |  |  |  |  |  |  |  |  |
| n41 | n3 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 |  |  |  |  |  |  |  |
| n7 | n3 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 |  |  |  |  |  |  |
| n41 | n25 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 |  |  |  |  |  |  |
| n38 | n25 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 |  |  |  |  |  |  |
| n411 | n66 | 3.5 | 3.5 | 3.5 | 3.5 |  |  | 3.5 |  |  |  |  |  |  |
| n41 | n77 |  | 8.3 | 8.3 | 8.3 | 7.3 | 6.5 | 6.3 | 5.3 | 4.5 | 4.3 | 4.0 | 3.9 | 3.8 |
| n41 | n78 |  | 8.3 | 8.3 | 8.3 | 7.3 | 6.5 | 6.3 | 5.3 | 4.5 | 4.3 | 4.0 | 3.9 | 3.8 |
| n77 | n411 |  | 4.5 | 4.5 | 4.5 |  | 4.5 | 4.5 | 4.5 | 4.5 | 4.5 | 4.5 | 4.5 | 4.5 |
| n78 | n71 | 4.5 | 4.5 | 4.5 | 4.5 | 4.5 | 4.5 | 4.5 | 4.5 |  |  |  |  |  |
| n78 | n38 | 3.3 | 3.3 | 3.3 | 3.3 |  |  |  |  |  |  |  |  |  |
| n78 | n401 | 4.5 | 4.5 | 4.5 | 4.5 | 4.5 | 4.5 | 4.5 | 4.5 | 4.5 |  | 4.5 |  |  |
| n78 | n411 |  | 4.5 | 4.5 | 4.5 |  | 4.5 | 4.5 | 4.5 | 4.5 |  | 4.5 | 4.5 | 4.5 |
| n783 | n79 |  |  |  |  |  |  | 2 | 2 | 2 |  | 2 |  | 2 |
| n79 | n783 |  | 2.6 | 2.6 | 2.6 |  |  | 2.6 | 2.6 | 2.6 |  | 2.6 | 2.6 | 2.6 |
| NOTE 1: Applicable only when harmonic mixing MSD for this combination is not applied.NOTE 2: VoidNOTE 3: The requirements only apply for UEs supporting inter-band carrier aggregation with simultaneous Rx/Tx capability. Simultaneous Rx/Tx capability does not apply for UEs supporting band n78 with a n77 implementation.NOTE 4: The requirements only apply for UEs supporting inter-band carrier aggregation with simultaneous Rx/Tx capability. Simultaneous Rx/Tx capability does not apply for UEs supporting band n78 with a n77 implementation. |

Table 7.3A.6.2: Uplink configuration for reference sensitivity exceptions due to cross band isolation for NR CA FR1

|  |
| --- |
| NR Band / SCS / Channel bandwidth of the affected DL band |
| UL band | DL band | SCS of UL band (kHz) | 5 MHz | 10 MHz | 15 MHz | 20 MHz | 25 MHz | 30 MHz | 40 MHz | 50 MHz | 60 MHz | 70MHz | 80 MHz | 90 MHz | 100 MHz |
| n1 | n3 | 15 | 25 | 25 | 25 | 25 | 25 | 25 |  |  |  |  |  |  |  |
| n1 | n40 | 15 | 25 | 50 | 75 | 100 | 100 | 100 | 100 | 100 | 100 |  | 100 |  |  |
| n1 | n41 | 15 |  | 100 | 100 | 100 |  |  | 100 | 100 | 100 |  | 100 | 100 | 100 |
| n3 | n41 | 15 |  | 50 | 50 | 50 |  |  | 50 | 50 | 50 |  | 50 | 50 | 50 |
| n38 | n78 | 15 |  | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 |  | 100 | 100 | 100 |
| n40 | n1 | 30 | 25 | 50 | 75 | 100 |  |  |  |  |  |  |  |  |  |
| n41 | n1 | 30 | 128 | 128 | 128 | 128 |  |  |  |  |  |  |  |  |  |
| n41 | n3 | 30 | 160 | 160 | 160 | 160 | 160 | 160 |  |  |  |  |  |  |  |
| n7 | n3 | 15 | 270 | 270 | 270 | 270 | 270 | 270 | 270 |  |  |  |  |  |  |
| n41 | n25 | 15 | 160 | 160 | 160 | 160 | 160 | 160 | 160 |  |  |  |  |  |  |
| n38 | n25 | 15 | 160 | 160 | 160 | 160 | 160 | 160 | 160 |  |  |  |  |  |  |
| n41 | n66 | 30 | 128 | 128 | 128 | 128 | 128 | 128 | 128 |  |  |  |  |  |  |
| n41 | n77 | 15 |  | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 |
| n41 | n78 | 15 |  | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 | 100 |
| n77 | n41 | 30 |  | 270 | 270 | 270 |  | 270 | 270 | 270 | 270 | 270 | 270 | 270 | 270 |
| n78 | n7 | 30 | 270 | 270 | 270 | 270 | 270 | 270 | 270 | 270 |  |  |  |  |  |
| n78 | n38 | 30 | 270 | 270 | 270 | 270 |  |  |  |  |  |  |  |  |  |
| n78 | n40 | 30 | 270 | 270 | 270 | 270 | 270 | 270 | 270 | 270 | 270 |  | 270 |  |  |
| n78 | n41 | 30 |  | 270 | 270 | 270 |  | 270 | 270 | 270 | 270 |  | 270 | 270 | 270 |
| n783 | n79 | 30 |  |  |  |  |  | 270 | 270 | 270 | 270 |  | 270 |  | 270 |
| n79 | n783 | 30 |  | 270 | 270 | 270 | 270 | 270 | 270 | 270 | 270 |  | 270 | 270 | 270 |
| NOTE 1: The UL configuration applies regardless of the channel bandwidth of the UL band unless the UL resource blocks exceed that specified in Table 7.3.2-3 for the uplink bandwidth in which case the allocation according to Table 7.3.2-3 applies.NOTE 2: Refers to the UL resource blocks shall be located as close as possible to the downlink operating band but confined within the transmission bandwidth configuration for the channel bandwidth in Table 5.3.2-1.NOTE 3: The requirements only apply for UEs supporting inter-band carrier aggregation with simultaneous Rx/Tx capability. Simultaneous Rx/Tx capability does not apply for UEs supporting band n78 with a n77 implementation. |

---End of changes---