**3GPP TSG-RAN4 Meeting #99-e *8754***

**Online, 19th May – 27th May 2021**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.101-4** | **CR** | **0177** | **rev** | **1** | **Current version:** | **15.9.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | CR to the definition of explicitly HARQ feedback timing in DCI format 1\_0 for PDCCH demodulation tests | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Anritsu corporation | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_newRAT-Perf | | | | |  | ***Date:*** | | | 2021-05-25 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | F |  | | | | | ***Release:*** | | | Rel-15 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | PDCCH Demodulation testcase requirements does not define a particular K1 value for HARQ feedback timing for PDSCH. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Added “The number of slots between PDSCH and corresponding HARQ-ACK information” as common test parameter. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Test implementations for each test environment would not be standardization. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.3, 7.3  **Isolated impact analysis:**  No change to UE requirements, changes test parameters only. | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | | **X** |  | Test specifications | | | | TS 38.521-4 | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | Revised from R4-2108846. | | | | | | | | |

<<Unchaged sections skipped>>

<<Start of change>>

## 5.3 PDCCH demodulation requirements

The receiver characteristics of the PDCCH are determined by the probability of miss-detection of the Downlink Scheduling Grant (Pm-dsg).

The parameters specified in Table 5.3-1 are valid for all PDCCH tests unless otherwise stated.

Table 5.3-1: Common test Parameters

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Parameter** | | | **Unit** | **Value** |
| Carrier configuration | Offset between Point A and the lowest usable subcarrier on this carrier (Note 1) | |  | 0 |
| DL BWP configuration #1 | Cyclic prefix | |  | Normal |
| RB offset | | RBs | 0 |
| Common serving cell parameters | Physical Cell ID | |  | 0 |
| SSB position in burst | |  | 1 |
| SSB periodicity | | ms | 20 |
| PDCCH configuration | Slots for PDCCH monitoring | |  | Each slot |
| Number of PDCCH candidates | |  | 1 |
| Frequency domain resource allocation for CORESET | |  | Start from RB = 0 with contiguous RB allocation |
| TCI state | |  | TCI state #1 |
| CSI-RS for tracking | First subcarrier index in the PRB used for CSI-RS (*k0*) | |  | 0 |
| First OFDM symbol in the PRB used for CSI-RS (*l0*) | |  | CSI-RS resource 1: 4 CSI-RS resource 2: 8 CSI-RS resource 3: 4 CSI-RS resource 4: 8 |
| Number of CSI-RS ports (*X*) | |  | 1 |
| CDM Type | |  | No CDM |
| Density (*ρ*) | |  | 3 |
| CSI-RS periodicity | | Slots | 15 kHz SCS: 20  30 kHz SCS: 40 |
| CSI-RS offset | | Slots | 15 kHz SCS:  10 for CSI-RS resource 1 and 2  11 for CSI-RS resource 3 and 4  30 kHz SCS:  20 for CSI-RS resource 1 and 2  21 for CSI-RS resource 3 and 4 |
| Frequency Occupation | |  | Start PRB 0  Number of PRB = BWP size |
| QCL info | |  | TCI state #0 |
| TCI state #0 | Type 1 QCL information | SSB index |  | SSB #0 |
| QCL Type |  | Type C |
| Type 2 QCL information | SSB index |  | SSB #0 |
| QCL Type |  | Type D |
| TCI state #1 | Type 1 QCL information | CSI-RS resource |  | CSI-RS resource 1 from 'CSI-RS for tracking' configuration |
| QCL Type |  | Type A |
| Type 2 QCL information | CSI-RS resource |  | CSI-RS resource 1 from 'CSI-RS for tracking' configuration |
| QCL Type |  | Type D |
| PDCCH Precoding configuration | | |  | Single Panel Type I, Random precoder selection updated per slot, with equal probability of each applicable i1, i2 combination with REG bundling granularity for number of Tx larger than 1 |
| Symbols for all unused REs | | |  | OP.1 FDD as defined in Annex A.5.1.1  OP.1 TDD as defined in Annex A.5.2.1 |
| Physical signals, channels mapping and precoding | | |  | As specified in Annex B.4.1 |
| The number of slots between PDSCH and corresponding HARQ-ACK information | | |  | 2 for FDD.  For TDD, specific to each TDD UL-DL pattern and as defined in Annex A.1.2. |
| Note 1: Point A coincides with minimum guard band as specified in Table 5.3.3-1 from TS 38.101-1 [6] for tested channel bandwidth and subcarrier spacing. | | | | |

<<End of change>>

<<Unchaged sections skipped>>

<<Start of change>>

## 7.3 PDCCH demodulation requirements

The receiver characteristics of the PDCCH are determined by the probability of miss-detection of the Downlink Scheduling Grant (Pm-dsg).

The parameters specified in Table 7.3-1 are valid for all PDCCH tests unless otherwise stated.

Table 7.3-1: Common test Parameters

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Parameter** | | | **Unit** | **Value** |
| Carrier configuration | Offset between Point A and the lowest usable subcarrier on this carrier (Note 1) | |  | 0 |
| DL BWP configuration #1 | Cyclic prefix | |  | Normal |
| Common serving cell parameters | Physical Cell ID | |  | 0 |
| SSB position in burst | |  | 1 |
| SSB periodicity | | ms | 20 |
| PDCCH configuration | Slots for PDCCH monitoring | |  | Each slot |
| Number of PDCCH candidates | |  | 1 |
| Frequency domain resource allocation for CORESET | |  | Start from RB = 0 with contiguous RB allocation |
| TCI state | |  | TCI state #1 |
| CSI-RS for tracking | First subcarrier index in the PRB used for CSI-RS (k0) | |  | 0 |
| First OFDM symbol in the PRB used for CSI-RS (l0) | |  | CSI-RS resource 1: 4 CSI-RS resource 2: 8 CSI-RS resource 3: 4 CSI-RS resource 4: 8 |
| Number of CSI-RS ports (X) | |  | 1 |
| CDM Type | |  | No CDM |
| Density (ρ) | |  | 3 |
| CSI-RS periodicity | | Slots | 160 |
| CSI-RS offset | | Slots | 80 for CSI-RS resource 1 and 2  81 for CSI-RS resource 3 and 4 |
| Frequency Occupation | |  | Start PRB 0  Number of PRB = BWP size |
| QCL info | |  | TCI state #0 |
| NZP CSI-RS for beam management | First subcarrier index in the PRB used for CSI-RS (k0) | |  | 0 |
| First OFDM symbol in the PRB used for CSI-RS (l0) | |  | CSI-RS resource 1: 8  CSI-RS resource 2: 9 |
| Number of CSI-RS ports (X) | |  | 1 |
| CDM Type | |  | No CDM |
| Density (ρ) | |  | 3 |
| CSI-RS periodicity | | Slots | 120 kHz SCS: 160 for CSI-RS resource 1,2 |
| CSI-RS offset | | Slots | 0 for CSI-RS resource 1,2 |
| Repetition | |  | ON |
| QCL info | |  | TCI state #1 |
| PDCCH & PDCCH DMRS Precoding configuration | | |  | Single Panel Type I, Random per slot with equal probability of each applicable i1, i2 combination, and with REG bundling granularity for number of Tx larger than 1 |
| TCI state #0 | Type 1 QCL information | SSB index |  | SSB #0 |
| QCL Type |  | Type C |
| Type 2 QCL information | SSB index |  | SSB #0 |
| QCL Type |  | Type D |
| TCI state #1 | Type 1 QCL information | CSI-RS resource |  | CSI-RS resource 1 from 'CSI-RS for tracking' configuration |
| QCL Type |  | Type A |
| Type 2 QCL information | CSI-RS resource |  | CSI-RS resource 1 from 'CSI-RS for tracking' configuration |
| QCL Type |  | Type D |
| Physical signals, channels mapping and precoding | | |  | As specified in Annex B.4.1 |
| Symbols for all unused REs | | |  | OP.1 FDD as defined in Annex A.5.1.1  OP.1 TDD as defined in Annex A.5.2.1 |
| The number of slots between PDSCH and corresponding HARQ-ACK information | | |  | Specific to each TDD UL-DL pattern and as defined in Annex A.1.3. |
| Note 1: Point A coincides with minimum guard band as specified in Table 5.3.3-1 from TS 38.101-1 [6] for tested channel bandwidth and subcarrier spacing. | | | | |

<<End of change>>