{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["TDoc_List","CR_Packs_List","Parameters"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":5,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"TDoc_List","index":0,"n_rows":89,"n_cols":31,"rows_kept":89,"cut":false,"hidden":false,"merged":[]}
["TDoc #","Title","Source","Contact","Contact ID","Type","Type supplement","For","Abstract","Agenda item sort order","Agenda item #","Agenda item description","TDoc sort order within agenda item","TDoc Status","Reservation date","Uploaded","Is revision of","Revised to","Release","Spec #","Version","Related WIs","CR #","CR revision #","CR category","TSG CR Pack","Reply to","To","Cc","Original LS","Reply in"]
["R4-75AH-AAS-0001","RAN4-75AH-AAS adhoc meeting agenda","Chairman","Issam Toufik",53262,"agenda","","","Meeting Agenda","2","2","Approval of the agenda",0,"Available","2015-06-16T00:48:36.860","2015-06-22T22:05:09.673","","","","","","","","","","","","","","",""]
["R4-75AH-AAS-0002","Power amplifier accuracy for active antennas with multi amplifiers","KATHREIN-Werke KG","Stefan Fritze",10457,"other","","","For active antennas with more than one power amplifier is a transceiver accuracy from at least 1 dB needed.","10","3.2.5","Value",0,"Available","2015-06-17T12:06:36.657","2015-06-22T16:54:02.273","","","","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0003","Uplink Near Field Measurement Method for Active Antennas","KATHREIN-Werke KG","Stefan Fritze",10457,"other","","","This paper proposes a method for near field UL measurement that requires only standardized power measurements.","31","3.6","Performance",0,"Available","2015-06-17T12:21:12.893","2015-06-22T16:54:02.303","","","","","","AAS_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-75AH-AAS-0004","One dimensional Compact Range Chamber","KATHREIN-Werke KG","Stefan Fritze",10457,"other","","","This paper proposes a novel method for a one dimensional compact range chamber.","31","3.6","Performance",0,"Available","2015-06-17T12:24:32.377","2015-06-22T16:54:02.337","","","","","","AAS_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-75AH-AAS-0005","Discussion on EIRP accuracy requirement for AAS","China Mobile Com. Corporation","Xiaoran Zhang",58560,"other","","","The EIRP accuracy requirement is one of the most important RF requirements for AAS BS and there is no consensus on this requirement after several meeting discussion. This paper further analyses the transceiver accuracy, array accuracy and steering accuracy of AAS, which are considered to be the most important factors for deriving EIRP requirements. ","10","3.2.5","Value",0,"Available","2015-06-19T08:11:28.957","2015-06-19T08:21:40.553","","","","","","","","","","","","","","",""]
["R4-75AH-AAS-0006","Theoretical model of EIRP and EIS requirements","CATT","Yuexia Song",34261,"other","","","EIRP and EIS model","3","3","Rel-13 Work Items",0,"Available","2015-06-21T21:03:35.940","2015-06-22T06:14:07.697","","","","","","","","","","","","","","",""]
["R4-75AH-AAS-0007","TP on symbols for OTA requirement","CATT","Yuexia Song",34261,"pCR","","","symbols for AAS","3","3","Rel-13 Work Items",0,"Available","2015-06-21T21:03:35.957","2015-06-22T06:14:07.727","","","","","","","","","","","","","","",""]
["R4-75AH-AAS-0008","How to specify EIRP accuracy value","NTT DOCOMO INC.","Suguru Okuyama",61038,"other","","","Document for approval.\nThe vales for discussion on EIRP accuracy are proposed by venders. However, the values are not evaluated based on the same condition. In this contribution, we discuss how to specify the value of EIRP accuracy.","10","3.2.5","Value",0,"Available","2015-06-22T00:20:22.690","2015-06-22T10:17:40.050","","","Rel-13","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0009","How to weight and combine the received signals for OTA sensitivity requirement","NTT DOCOMO INC.","Suguru Okuyama",61038,"other","","","Document for approval.\nWhen the array combiner is not included in AAS BS, how to combine the received signals should be discussed. In this contribution, we discuss on how to weight and combine the received signals for OTA sensitivity requirement.","11","3.3","OTA Sensitivity",0,"Available","2015-06-22T00:22:08.780","2015-06-22T10:17:40.067","","","Rel-13","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0010","Consideration on how to define OTA sensitivity requirements","NTT DOCOMO INC.","Suguru Okuyama",61038,"other","","","Document for approval.\nThis contribution discusses on the core and test requirement for OTA sensitivity.","12","3.3.1","RoAoA",0,"Available","2015-06-22T00:23:38.780","2015-06-22T10:17:40.127","","","Rel-13","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0011","Unwanted emission requirements for AAS BS","NTT DOCOMO INC.","Suguru Okuyama",61038,"other","","","Document for approval.\nIn this contribution, we discuss these open issues and present our views and proposals on the unwanted emission requirements.","22","3.5.2.1","Multi-band, multi-cell, multi-carrier issues.",0,"Available","2015-06-22T00:24:35.543","2015-06-22T10:17:40.157","","","Rel-13","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0012","Unwanted emission requirement","SEI","Li Yue",58006,"other","","","","24","3.5.2.3","UEM scaling.",0,"Available","2015-06-22T07:54:32.323","2015-06-24T07:34:39.570","","","Rel-13","","","","","","","","","","","",""]
["R4-75AH-AAS-0013","On OTA sensitivity","SEI","Li Yue",58006,"other","","","","11","3.3","OTA Sensitivity",0,"Available","2015-06-22T08:00:48.350","2015-06-24T07:34:39.600","","","","","","","","","","","","","","",""]
["R4-75AH-AAS-0014","TP for TR 36.842: Text proposal on EIRP","Ericsson","Thomas Chapman",46692,"pCR","","","TP capturing decisions on EIRP, as reviewed and updated from RAN4#74","5","3.2","EIRP (2.2.2)",0,"Available","2015-06-22T10:56:08.833","2015-06-22T19:19:03.530","","","Rel-13","37.842","1.6.0","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0015","OTA sensitivity testing","Ericsson","Thomas Chapman",46692,"other","","","This paper outlines some options for settingt he test points for OTA sensitivity","12","3.3.1","RoAoA",0,"Available","2015-06-22T10:56:08.847","2015-06-22T19:19:03.563","","","Rel-13","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0016","On the need for declaring combining for OTA sensitivity","Ericsson","Thomas Chapman",46692,"other","","","At RAN4#75 there was some question as to whether there is a need to declare the type of combining in baseband. This contribution examines the issue","13","3.3.2","OTA sensitivity declaration power level definition",0,"Available","2015-06-22T10:56:08.847","2015-06-22T19:19:03.610","","","Rel-13","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0017","Ambiguities to be resolved in counting the number of AAS-ETAC","Ericsson","Thomas Chapman",46692,"other","","","A WF for emissions was approved at RAN4#74bis. The WF does not exactly capture how to count the number of AAS-ETAC. This contribution lists the issues that need to be decided to get an exact way of counting","27","3.5.2.6","AAS-ETAC.",0,"Available","2015-06-22T10:56:08.847","2015-06-22T19:19:03.640","","","Rel-13","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0018","Transmitter conducted power","Ericsson","Thomas Chapman",46692,"other","","","This paper considers how to set the conducted emissions requirement and how the power limits for small basestations should operate","26","3.5.2.5","Conducted power definitions",0,"Available","2015-06-22T10:56:08.863","2015-06-22T19:19:03.670","","","Rel-13","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0019","OTA sensitivity framework","Ericsson","Thomas Chapman",46692,"other","","","Discussion on how to define the OTA sensitivity requirement considering the proposals and architectures discussed at RAN4#75","12","3.3.1","RoAoA",0,"Available","2015-06-22T10:56:08.863","2015-06-22T19:19:03.343","","","Rel-13","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0020","Emissions requirements for multi-band systems","Ericsson","Thomas Chapman",46692,"other","","","Discussion on how to set requiremetns for basestations with multiband transmitters","22","3.5.2.1","Multi-band, multi-cell, multi-carrier issues.",0,"Available","2015-06-22T10:56:08.863","2015-06-22T19:19:03.377","","","Rel-13","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0021","Setting the emissions requirement for AAS","Ericsson","Thomas Chapman",46692,"other","","","Proposals on how to resolve the remaining issues for emissions scaling","24","3.5.2.3","UEM scaling.",0,"Available","2015-06-22T10:56:08.880","2015-06-22T19:19:03.390","","","Rel-13","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0022","TP for 37.842 on the OTA sensitivity requirement","Ericsson","Thomas Chapman",46692,"pCR","","","Text proposal capturing means to set the OTA sensitivity requirement","11","3.3","OTA Sensitivity",0,"Available","2015-06-22T10:56:08.880","2015-06-22T19:19:03.423","","","Rel-13","37.842","1.6.0","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0023","RAN4 requirements and EBF/FD-MIMO","Ericsson","Thomas Chapman",46692,"other","","","Summary of issues to consider when developign EBF/FD-MIMO","32","4","Any other business",0,"Available","2015-06-22T10:56:08.893","2015-06-24T20:55:44.703","","","Rel-13","","","","","","","","","","","",""]
["R4-75AH-AAS-0024","Examination of the impact of larger numbers of radios on requirements","Ericsson","Thomas Chapman",46692,"other","","","Examination of technical effects of more radios on the requirements","32","4","Any other business",0,"Available","2015-06-22T10:56:08.893","2015-06-24T20:55:44.670","","","Rel-13","","","","","","","","","","","",""]
["R4-75AH-AAS-0025","On AAS specification structure","Ericsson","Thomas Chapman",46692,"other","","","Proposal for specification structure, in case discussed","32","4","Any other business",0,"Available","2015-06-22T10:56:08.893","2015-06-22T19:19:03.453","","","Rel-13","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0026","TP for TR 37.842: Emissions scaling for AAS","Ericsson","Thomas Chapman",46692,"pCR","","","","24","3.5.2.3","UEM scaling.",0,"Available","2015-06-22T11:26:58.347","2015-06-22T19:19:03.500","","","Rel-13","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0027","On coordinate system and direction diagram","Ericsson","Torbjorn Elfstrom",44796,"other","","","At last RAN4 meeting in Fukuoka (RAN4#75) a coordinate system required for radiated AAS base station requirements was agreed and included in TR 37.842. Also a way forward for AAS OTA coordinate system was approved in [1].  This contribution continues the discussion about open issues identified in the way-forward.","4","3.1","Coordinate system",0,"Available","2015-06-22T12:17:10.650","2015-06-22T17:49:30.967","","","Rel-13","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0028","Declarations relating to the OTA sensitivity requirement","Ericsson","Torbjorn Elfstrom",44796,"other","","","Following recent progress and agreements on the OTA sensitivity requirement, a draft core specification text is provided for discussion in [1]. This contribution collects together a list of declarations that should be made specifically for the OTA sensitivity requirement. In addition to these declarations, it should be noted that a large number of other MSR declarations will be needed as in today’s specifications. These are summarized in a companion contribution [2].","11","3.3","OTA Sensitivity",0,"Available","2015-06-22T12:17:10.650","2015-06-22T17:49:30.980","","","Rel-13","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0029","On how to test AAS base station radiated transmit power","Ericsson","Torbjorn Elfstrom",44796,"other","","","The discussion related to how radiated transmit power as an RF core requirement shall be defined for AAS base stations has been ongoing for a long time. It have been noticed that to conclude the discussion and settle the definition, it is necessary to look into how to measure EIRP. This paper is influenced from section 7.1 of TR 37.842 [1], defining radiated transmit power requirement for AAS base stations.","31","3.6","Performance",0,"Available","2015-06-22T12:17:10.667","2015-06-22T17:49:30.997","","","Rel-13","","","AAS_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-75AH-AAS-0030","On how to test AAS base station OTA sensitivity","Ericsson","Torbjorn Elfstrom",44796,"other","","","On how to test AAS base station OTA sensitivity","31","3.6","Performance",0,"Available","2015-06-22T12:17:10.667","2015-06-22T17:49:31.043","","","Rel-13","","","AAS_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-75AH-AAS-0031","On Near-Field scanner testing on AAS base station UL","Ericsson","Torbjorn Elfstrom",44796,"other","","","This contribution continues the discussion about near-field scanner based test methods and UL testing. Earlier in the discussion a few issues related to the applicability for near-field scanner based methods where raised.  This is an updated version of R4-153006.","18","3.4.1","Measurement Uncertainty",0,"Available","2015-06-22T12:17:10.667","2015-06-22T17:49:31.090","","","Rel-13","","","AAS_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-75AH-AAS-0032","On radiated transmit power and polarization","Ericsson","Torbjorn Elfstrom",44796,"other","","","This contribution gives some background on how polarization properties for radiated transmit power can be captured for AAS base stations in an implementation neutral testing efficient and future proof manner.","5","3.2","EIRP (2.2.2)",0,"Available","2015-06-22T12:17:10.680","2015-06-22T17:49:31.123","","","Rel-13","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0033","On OTA sensitivity and polarization","Ericsson","Torbjorn Elfstrom",44796,"other","","","This contribution gives the background for how polarization properties of an AAS base station can be handled with respect to OTA sensitivity.","11","3.3","OTA Sensitivity",0,"Available","2015-06-22T12:17:10.680","2015-06-22T17:49:31.153","","","Rel-13","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0034","OTA sensitivity draft specification text, updated version","Ericsson","Torbjorn Elfstrom",44796,"other","","","The RF core OTA sensitivity has been discussed for a long time. This contribution holds draft text for a section capturing OTA sensitivity in the AAS RF core specification to be developed by RAN4. We encourage all involved parties in the discussion to use this draft as a starting point for formulating the OTA sensitivity requirement for AAS base stations. We have presented a series of similar contributions already; this is the latest version, based on [1]. This version is revised and updated based on the discussion at last meeting and feedback received after last meeting.","16","3.3.5","TS draft text",0,"Available","2015-06-22T12:17:10.697","2015-06-22T17:49:31.170","","","Rel-13","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0035","Radiated transmit power draft specification text, updated version","Ericsson","Torbjorn Elfstrom",44796,"other","","","This document captures a first draft for specification text for the radiated TX power requirement, including comments received during RAN4#75. The document is not intended for approval and is likely to be revised further, but since comments from companies have been collected in the document it should be attempted to use this as a starting point for refining and getting to final specification text in future meetings. We encourage all involved parties in the discussion to use this draft as a starting point for formulating the radiated transmit power requirement for AAS base stations. We have presented a series of similar contributions already; this is the latest version, based on [1]. This version is revised and updated based on the discussion at last meeting and feedback received after last meeting.","15","3.3.4","Min value vs. declared only",0,"Available","2015-06-22T12:17:10.697","2015-06-22T17:49:31.183","","","Rel-13","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0036","On AAS conformance test requirements","Ericsson","Torbjorn Elfstrom",44796,"other","","","The main discussion in the AAS WI has so far been on RF core requirements for AAS base stations. It have been noticed that to conclude the RF core discussion and create a specification, it is necessary to look into how to measure parameters required for radiated transmit power and OTA sensitivity requirements. It is also good to start the discussion about how to create a conformance test specification for AAS base stations.","18","3.4.1","Measurement Uncertainty",0,"Available","2015-06-22T12:17:10.713","2015-06-22T17:49:31.217","","","Rel-13","","","AAS_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-75AH-AAS-0037","TP for TR 37.842: Beam pointing direction and reference steering","Ericsson","Torbjorn Elfstrom",44796,"pCR","","","This contribution evaluates two concepts for defining beam pointing direction as part of radiated transmit power requirement for AAS base stations.  In RAN4 two different ways of define beam pointing direction have been discussed; peak direction and centre direction. This contribution introduces a generic definition of centre beam pointing direction for beam steering in two dimensions.","4","3.1","Coordinate system",0,"Available","2015-06-22T12:17:10.713","2015-06-22T17:49:31.263","","","Rel-13","37.842","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0038","TP for TR 37.842: Adding introduction text to section 9 about manufacturer declaration for AAS base stations","Ericsson","Torbjorn Elfstrom",44796,"pCR","","","This contribution presents some ideas on how to capture manufactures declarations required for AAS conformance testing. At the end of the contribution a text proposal is attached. The text proposal captures identified parameters applicable for AAS base stations in section 9 of TR 37.842 [2].","31","3.6","Performance",0,"Available","2015-06-22T12:17:10.727","2015-06-22T17:49:31.293","","","Rel-13","37.842","","AAS_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-75AH-AAS-0039","TP for TR 37.842: Scaling of conducted sensitivity for AAS BS in section 8.2","Ericsson","Torbjorn Elfstrom",44796,"pCR","","","This contribution holds a text proposal for section 8.2 of TR 37.842 [2]. This contribution is a revised version of the original version (R4-152468). Comments received after discussion has been implemented. This version is a resubmitted version of R4-153012, which was not presented due to lack of meeting time in Fukuoka.","30","3.5.3","Receiver",0,"Available","2015-06-22T12:17:10.743","2015-06-22T17:49:31.340","","","Rel-13","37.842","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0040","TP for TR 37.842: Adding structure to section 10 for OTA test methodologies","Ericsson","Torbjorn Elfstrom",44796,"pCR","","","This contribution elaborates around how background information shall be captured in the TR 37.842 in a way making it easy to develop an AAS base station conformance specification. The contribution proposals some general principles for handling test methods for AAS base stations. Before adding aspects of AAS base station testing in TR 37.842, a structure must be agreed.","17","3.4","OTA Testing",0,"Available","2015-06-22T12:17:10.743","2015-06-22T17:49:31.370","","","Rel-13","37.842","","AAS_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-75AH-AAS-0041","Intra-system transmitter intermodulation emission requirement background summary","Ericsson","Torbjorn Elfstrom",44796,"other","","","Text proposals [1, 2, 3] based on agreed way-forward contributions [4, 5] was presented at RAN4#75 in Fukuoka. These text proposals was not approved, even though contribution and agreed way forwards clearly indicates that intra-system is a potential issue for AAS base stations.","29","3.5.2.8","Intermodulation",0,"Available","2015-06-22T12:17:10.760","2015-06-22T17:49:31.387","","","Rel-13","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0042","OTA Test Method Uncertainty Budget","Ericsson","Torbjorn Elfstrom",44796,"other","","","In RAN4#75 in Fukuoka, ongoing discussions regarding conformance testing of an AAS were continued.  This contribution will continue the discussion regarding uncertainty sources for EIRP measurements.  This contribution will also discuss the need for each test method and requirement to have its own uncertainty budget.","18","3.4.1","Measurement Uncertainty",0,"Available","2015-06-22T12:17:10.760","2015-06-22T17:49:31.417","","","Rel-13","","","AAS_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-75AH-AAS-0043","Near Field Scanner Testing","Ericsson","Torbjorn Elfstrom",44796,"other","","","The discussions relating to over the air testing has led to a list of potential test methods.  These discussions started in the AAS SI, details of this can be found in section 8 of the TR 37.114 [1].  So far, there have been two main candidates for OTA testing: Near field scanner method, and far field in compact antenna test range (CATR) [2, 3].","18","3.4.1","Measurement Uncertainty",0,"Available","2015-06-22T12:17:10.773","2015-06-22T17:49:31.433","","","Rel-13","","","AAS_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-75AH-AAS-0044","TP for TR 37.842: Adding uncertainty list for EIRP in CATR in section 10","Ericsson","Torbjorn Elfstrom",44796,"pCR","","","This contribution tries to summarize the uncertainty budget contributions up to date in a text proposal for TR 37.842.","18","3.4.1","Measurement Uncertainty",0,"Available","2015-06-22T12:17:10.790","2015-06-22T17:49:31.467","","","Rel-13","37.842","","AAS_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-75AH-AAS-0045","TP for TR 37.842: Adding uncertainty list for EIS in CATR","Ericsson","Torbjorn Elfstrom",44796,"pCR","","","In RAN4#74bis in Rio de Janeiro, it was agreed that each test method that brought forth should list the uncertainty contributions in the format in TS 34.114 (UE TRS measurement specification).  The probability distribution and divisor of each uncertainty are important aspects of the uncertainty source and to the overall uncertainty figure for each test method but will be discussed once the list of uncertainty sources has been agreed.","18","3.4.1","Measurement Uncertainty",0,"Available","2015-06-22T12:17:10.790","2015-06-22T17:49:31.480","","","Rel-13","37.842","","AAS_BS_LTE_UTRA-Perf","","","","","","","","",""]
["R4-75AH-AAS-0046","TP for TR 37.842: Adding text to section 8.1.5 about intra-system TX IMD emission requirement","Ericsson, Huawei","Torbjorn Elfstrom",44796,"pCR","","","In RAN4#75, the contributions [1], [2], [3] and [4] have been found to have sufficient commonalities to warrant a merger effort in order to get an agreeable text proposal. This test proposal represents the result of the merger with respect to the requirement definition.","29","3.5.2.8","Intermodulation",0,"Available","2015-06-22T12:17:10.807","2015-06-22T17:49:31.513","","","Rel-13","37.842","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0047","TP on OTA coordinate location and origin","NEC","Nader Zein",27226,"pCR","","","The coordinate system was discussed extensively during the last RAN4#75 meeting. As a result, RAN4 agreed the coordinate system for AAS BS as described in [1]. A way forward in [2] was also agreed identifying the remaining open issue related to Specifics of the coordinate system declaration and the Formalization of a direction diagram to be used for declarations and requirements. This contribution addresses the open issue in this way forward.","4","3.1","Coordinate system",0,"Available","2015-06-22T14:09:46.940","2015-06-22T18:55:20.497","","","Rel-13","37.842","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0048","TP on EIRP accuracy and beam declaration","NEC","Nader Zein",27226,"pCR","","","A Way Forward on EIRP requirements was approved in [1]. During RAN4#75, several TP on EIRP accuracy and beam declaration [2, 3, 4, 5, 6] were proposed but none could be agreed.\nIn this contribution, we provide a revised text proposal trying to merge contributions discussed in RAN4#75.","5","3.2","EIRP (2.2.2)",0,"Available","2015-06-22T14:09:46.940","2015-06-22T18:55:20.527","","","Rel-13","37.842","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0049","Proposal on EIRP Level Declaration","NEC","Nader Zein",27226,"other","","","The current AAS TR [1] includes radiated transmit power requirements. The radiated transmit power requirements are placed on the accuracy of the declared EIRP that is presumed to correspond to an AAS BS beam. A beam is currently defined in the TR, however, for the purpose of declaration of the EIRP value, the current definition needs to be further clarified. In this contribution, we consider the options for which a beam could be defined for the purpose of EIRP declaration and make a proposal accordingly.","8","3.2.3","Basis of beam definition",0,"Available","2015-06-22T14:09:46.957","2015-06-22T18:55:20.577","","","Rel-13","37.842","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0050","Proposal on Declaration for AAS OTA Sensitivity requirements","NEC","Nader Zein",27226,"other","","","OTA sensitivity requirements were investigated and discussed extensively in the recent meetings. Way Forwards [1, 2] on OTA sensitivity were approved during the last RAN4#74 and RAN4#74bis meetings, but a new Way Forward [3] was not approved in RAN4#75.\nThis contribution addresses the open issue on vendor declared coverage range and makes corresponding proposal on the OTA sensitivity requirements.","12","3.3.1","RoAoA",0,"Available","2015-06-22T14:09:46.957","2015-06-22T18:55:20.607","","","Rel-13","37.842","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0051","Mapping of Transceivers into AAS-ETAC","NEC","Nader Zein",27226,"other","","","The definition of AAS-ETAC was approved in [1] during RAN4#74bis. Contribution [2] presented a wide range of examples for configurations and mapping of transceiver units into AAS-ETAC with various capabilities such as multiband and multicarrier support. In this contribution we present NEC views and make two proposals on the mapping and grouping of transceiver units into AAS-ETAC.","23","3.5.2.2","Groups/Mapping",0,"Available","2015-06-22T14:09:46.973","2015-06-22T18:55:20.637","","","Rel-13","37.842","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0052","Proposal for Unwanted Emission requirements for AAS BS","NEC","Nader Zein",27226,"other","","","During RAN4#74bis, an agreement in [1] was made on the definition of AAS equivalent transmitter antenna connector (AAS-ETAC) for which the unwanted emission limits from current non-AAS can be applied. Open issues for further consideration are presented in [2]. In this contribution, we analyse the open issues in [2] and propose unwanted emission limits to be specified per AAS-ETAC while scaling is only required for conformance testing.","24","3.5.2.3","UEM scaling.",0,"Available","2015-06-22T14:09:46.973","2015-06-22T18:55:20.653","","","Rel-13","37.842","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0053","Time Alignment Error in AAS","NEC","Nader Zein",27226,"pCR","","","Time Alignment Error (TAE) has been identified in [1] as an open issue. This paper is submitted to aid in finalization of the TAE issue.","25","3.5.2.4","TAE",0,"Available","2015-06-22T14:09:46.973","2015-06-22T18:55:20.357","","","Rel-13","37.842","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0054","Conducted Output Power Requirements for AAS BS","NEC","Nader Zein",27226,"pCR","","","This contribution is submitted to confirm the PRAT values for Medium Range and Local Area AAS BS in the text proposal below with the requirement to be applied per AAS Equivalent transmitter antenna connector (AAS-ETAC).","26","3.5.2.5","Conducted power definitions",0,"Available","2015-06-22T14:09:46.987","2015-06-22T18:55:20.387","","","Rel-13","37.842","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0055","TP AAS-ETAC Definition and its application for AAS BS transmitter requirements","NEC","Nader Zein",27226,"pCR","","","During RAN4#74bis, an agreement in [1] was made on the definition of AAS equivalent transmitter antenna connector (AAS-ETAC) for which the unwanted emission limits from current non-AAS can be applied. In this contribution, we make a Text Proposal to capture the agreed AAS-ETAC definition in [1] and taking into account the WF in [2].","27","3.5.2.6","AAS-ETAC.",0,"Available","2015-06-22T14:09:46.987","2015-06-22T18:55:20.437","","","Rel-13","37.842","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0056","Consideration on conducted receiver requirements","NEC","Nader Zein",27226,"other","","","Receiver sensitivity requirement is one of the remaining open topics in the AAS BS TR [1]. A number of contributions [2, 3] were submitted on the topic during the last RAN4 meeting but no conclusion is yet achieved to conclude the requirements for conducted receiver sensitivity. This contribution discusses current options being considered for setting the conducted receiver requirements and their implication.","30","3.5.3","Receiver",0,"Available","2015-06-22T14:09:46.987","2015-06-22T18:55:20.467","","","Rel-13","37.842","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0057","Ad-Hoc Agenda","Huawei","Richard Kybett",47339,"other","","","Appoval","2","2","Approval of the agenda",0,"Withdrawn","2015-06-22T16:42:47.610",null,"","","","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0058","TR37.842 v160","Huawei","Richard Kybett",47339,"other","","","Discussion","3","3","Rel-13 Work Items",0,"Available","2015-06-22T16:42:47.610","2015-06-22T19:38:32.437","","","","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0059","On beam definition","Huawei","Richard Kybett",47339,"other","","","Discussion","8","3.2.3","Basis of beam definition",0,"Available","2015-06-22T16:42:47.627","2015-06-22T19:38:32.487","","","","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0060","EIRP accuracy value","Huawei","Richard Kybett",47339,"other","","","Discussion","10","3.2.5","Value",0,"Available","2015-06-22T16:42:47.627","2015-06-22T19:38:32.500","","","","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0061","Beams and AAS-ETAC","Huawei","Richard Kybett",47339,"other","","","Discussion","8","3.2.3","Basis of beam definition",0,"Available","2015-06-22T16:42:47.627","2015-06-22T19:38:32.547","","","","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0062","On Multi carrier Multi band Multi cell issues","Huawei","Richard Kybett",47339,"other","","","Discussion","22","3.5.2.1","Multi-band, multi-cell, multi-carrier issues.",0,"Available","2015-06-22T16:42:47.643","2015-06-22T19:38:32.173","","","","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0063","UEM scaling and number of AAS- ETAC","Huawei","Richard Kybett",47339,"other","","","Discussion","24","3.5.2.3","UEM scaling.",0,"Available","2015-06-22T16:42:47.643","2015-06-22T19:38:32.220","","","","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0064","TAE for AAS","Huawei","Richard Kybett",47339,"other","","","Discussion","25","3.5.2.4","TAE",0,"Available","2015-06-22T16:42:47.657","2015-06-22T19:38:32.250","","","","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0065","Output power declarations and number of AAS-ETAC","Huawei","Richard Kybett",47339,"other","","","Discussion","26","3.5.2.5","Conducted power definitions",0,"Available","2015-06-22T16:42:47.657","2015-06-22T19:38:32.297","","","","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0066","Definition of AAS-ETAC","Huawei","Richard Kybett",47339,"other","","","Discussion","27","3.5.2.6","AAS-ETAC.",0,"Available","2015-06-22T16:42:47.657","2015-06-22T19:38:32.330","","","","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0067","Discussion on FFS conducted requirements","Huawei","Richard Kybett",47339,"other","","","Discussion","30","3.5.3","Receiver",0,"Available","2015-06-22T16:42:47.673","2015-06-22T19:38:32.377","","","","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0068","TP to change the elevation range","KATHREIN-Werke KG","Stefan Fritze",10457,"other","","","","4","3.1","Coordinate system",0,"Available","2015-06-22T16:47:49.350","2015-06-22T16:54:02.367","","","Rel-13","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0069","TP for Coordinate System Further Details","Alcatel-Lucent","Torsten Wildschek",59806,"pCR","","","This contribution presents a text proposal to fill in some of the details of the agreed coordinate system.","4","3.1","Coordinate system",0,"Available","2015-06-22T18:01:51.103","2015-06-22T22:40:11.957","","","","","","","","","","","","","","",""]
["R4-75AH-AAS-0070","On Beam Direction","Alcatel-Lucent","Torsten Wildschek",59806,"other","","","This contribution presents some views on the “beam direction” concept.","8","3.2.3","Basis of beam definition",0,"Available","2015-06-22T18:01:51.117","2015-06-22T22:40:11.923","","","","","","","","","","","","","","",""]
["R4-75AH-AAS-0071","Views on Unwanted Emission for AAS BS","Alcatel-Lucent","Torsten Wildschek",59806,"other","","","Views on Unwanted Emission for AAS","24","3.5.2.3","UEM scaling.",0,"Available","2015-06-22T18:01:51.117","2015-06-22T22:40:11.877","","","","","","","","","","","","","","",""]
["R4-75AH-AAS-0072","Updated introduction of direction diagrams","Huawei","Alf Ahlström",23580,"other","","","Directions diagram introduction with agreed coordinate system","4","3.1","Coordinate system",0,"Available","2015-06-22T20:39:45.413","2015-06-22T21:52:12.937","","","","","","","","","","","","","","",""]
["R4-75AH-AAS-0073","OTA sensitivty terminology discussion","Huawei","Alf Ahlström",23580,"other","","","Terminology for OTA sensitivity requirement is discussed","14","3.3.3","Terminology",0,"Available","2015-06-22T20:39:45.427","2015-06-22T21:52:35.963","","","","","","","","","","","","","","",""]
["R4-75AH-AAS-0074","OTA sensitivity declarations discussion","Huawei","Alf Ahlström",23580,"other","","","Declarations for OTA sensitivity discussion","13","3.3.2","OTA sensitivity declaration power level definition",0,"Available","2015-06-22T20:39:45.427","2015-06-22T21:57:04.053","","","","","","","","","","","","","","",""]
["R4-75AH-AAS-0075","OTA sensitivty conformance test directions discussion","Huawei","Alf Ahlström",23580,"other","","","Discussion on how to define directions for conformance testing","12","3.3.1","RoAoA",0,"Available","2015-06-22T20:39:45.443","2015-06-22T21:57:04.100","","","","","","","","","","","","","","",""]
["R4-75AH-AAS-0076","OTA sensitivity and reference sensitivity","Huawei","Alf Ahlström",23580,"other","","","Recapitulation on proposed way of connecting refernce sensitivity with OTA sensitivty","15","3.3.4","Min value vs. declared only",0,"Available","2015-06-22T20:39:45.443","2015-06-22T21:57:04.130","","","","","","","","","","","","","","",""]
["R4-75AH-AAS-0077","TP OTA sensitivity","Huawei","Alf Ahlström",23580,"pCR","","","TP on OTA senstivity","12","3.3.1","RoAoA",0,"Available","2015-06-22T20:39:45.443","2015-06-22T21:57:04.193","","","","","","","","","","","","","","",""]
["R4-75AH-AAS-0078","TP suggesting ways to put test requirements on OTA parameters","Huawei","Alf Ahlström",23580,"pCR","","","TP on suggesting ways to find conformance requirements on OTA requirements","18","3.4.1","Measurement Uncertainty",0,"Available","2015-06-22T20:39:45.460","2015-06-22T21:57:04.227","","","","","","","","","","","","","","",""]
["R4-75AH-AAS-0079","EIRP measurement uncertainty (CATR) - example budget","Huawei","Alf Ahlström",23580,"other","","","Example EIRP unceratinty budget","18","3.4.1","Measurement Uncertainty",0,"Available","2015-06-22T20:39:45.460","2015-06-22T21:57:46.470","","","","","","","","","","","","","","",""]
["R4-75AH-AAS-0080","Discussion on current OTA conformance specification","Huawei","Alf Ahlström",23580,"other","","","Discussion on the content of TS34.114 and its applicability for AAS","18","3.4.1","Measurement Uncertainty",0,"Available","2015-06-22T20:39:45.473","2015-06-22T21:57:46.440","","","","","","","","","","","","","","",""]
["R4-75AH-AAS-0081","OTA sensitivity testing example","Huawei","Alf Ahlström",23580,"other","","","Example of testing OTA sensitivity using CATR","18","3.4.1","Measurement Uncertainty",0,"Available","2015-06-22T20:39:45.473","2015-06-22T21:57:46.393","","","","","","","","","","","","","","",""]
["R4-75AH-AAS-0082","TP for TR 37.842: Adding text to section 8.1.5.2 about determination of intra array leakage power","Huawei, Ericsson","Alf Ahlström",23580,"pCR","","","TP describing estimation of intra AAS array transmit leakage power","29","3.5.2.8","Intermodulation",0,"Available","2015-06-22T20:39:45.490","2015-06-22T21:57:46.330","","","","","","","","","","","","","","",""]
["R4-75AH-AAS-0083","TP Manufacturer declaration matrix","Huawei","Alf Ahlström",23580,"pCR","","","TP introducing empty matrix for capturing and cross linkdeclarations","31","3.6","Performance",0,"Available","2015-06-22T20:39:45.490","2015-06-22T21:57:46.300","","","","","","","","","","","","","","",""]
["R4-75AH-AAS-0084","Discussion on E-BF/FD-MIMO","Huawei Tech.(UK) Co., Ltd","Richard Kybett",47339,"other","","","Considerations on the RAN1 E-BF/FD-MIMO  WI for RAN4  AAS.","32","4","Any other business",0,"Available","2015-06-22T21:20:54.330","2015-06-24T15:39:23.087","","","Rel-13","","","AAS_BS_LTE_UTRA-Core","","","","","","","","",""]
["R4-75AH-AAS-0085","EIRP and EIS Testing Procedures for an AAS BS implementation when using Near Field Measurement Technique","MVG Industries","Alessandro Scannavini",52688,"other","","","During the 3GPP TSG RAN4 #71, R4-142684 was presented. This contribution was highlighting the near field measurement technique for radiated measurements (EIRP, and EIS) of an AAS BS. Due to lack of an AAS BS, MVG Industries did use a passive BTS antenna connected to a modem data card for the testing campaign. Some questions were arisen whether the highlighted testing procedures and used equipments could have been fully applied when testing a real AAS BS. This contribution is trying to answer to some of them.","17","3.4","OTA Testing",0,"Available","2015-06-22T22:08:24.427","2015-06-22T22:22:48.257","","","Rel-13","","","","","","","","","","","",""]
["R4-75AH-AAS-0086","Consideration of directions for AAS OTA coverage areas","Nokia Networks","Iwajlo Angelow",34448,"other","","","","12","3.3.1","RoAoA",0,"Available","2015-06-22T22:26:48.607","2015-06-22T22:29:10.397","","","","","","","","","","","","","","",""]
["R4-75AH-AAS-0087","EIRP accuracy for AAS","Vodafone","Luis Anaya",46360,"other","","","","5","3.2","EIRP (2.2.2)",0,"Available","2015-06-24T12:28:24.813","2015-06-24T12:31:20.893","","","","","","","","","","","","","","",""]
["R4-75AH-AAS-0088","View on eNB core requirements for EBF/FD-MIMO","Samsung Electronics Co., Ltd","Xutao Zhou",40317,"other","","","In this paper, view on whether there is a need for additional eNB core requirements that are not addressed in the AAS WI is provided.","32","4","Any other business",0,"Reserved","2015-06-24T13:11:33.390",null,"","","Rel-13","","","","","","","","","","","",""]

{"sheet":"CR_Packs_List","index":1,"n_rows":1,"n_cols":11,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["CR Pack TDoc #","WG TDoc #","WG TDoc decision","CR Individual TSG decision","Spec #","CR #","CR revision #","CR category","Release","Version","CR title"]

{"sheet":"Parameters","index":2,"n_rows":16,"n_cols":3,"rows_kept":16,"cut":false,"hidden":true,"merged":[]}
["Types of Tdocs","Possible statuses of Tdocs","Categories"]
[]
["agenda","Reserved","A"]
["LS in","Available","B"]
["LS out","Revised","C"]
["pCR","Approved","D"]
["CR","Agreed","E"]
["CR pack","Postponed","F"]
["WID","Noted"]
["WI status report","Rejected"]
["TS or TR","Withdrawn"]
["report","Treated"]
["other","Partially approved"]
[null,"Technically endorsed"]
[null,"Merged"]
[null,"Reissued"]