    Log Viewer 392.10.0.0
    Copyright © 2021, Keysight Technologies

    LogFile            : TC_7_34_20210420_060000_n41_PASS_v66.0_part1.alf
    Created            : 23/04/2021 15:12:20

| Details | Summary

    timerEvent = 9
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\Common\CommonDefs.ttcn
    testName = TC_7_34_NR5GC
    lineNo = 593
    outStr = Timer: t_Delay, Expired: 06:15:18

    Timer: t_Delay, Expired: 06:15:18

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1873
    text = Parameter: IMS_Component.v_IgnoreReset = False
    File: IMS_Component.ttcn [Line: 1873]

    Parameter: IMS_Component.v_IgnoreReset = False
    File: IMS_Component.ttcn [Line: 1873]

    SipMessage
    	Message Header = UPDATE sip:PeerUE-Public@stf160.etsi.org:6543 SIP/2.0
    From: ;tag=1583834582
    To: ;tag=abc-INVITE-Fromtag
    Call-ID: INVITE-0-7dec-11d0-a765-00a0c91e6bf6@FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7
    CSeq: 4712 UPDATE
    Accept: application/sdp,application/3gpp-ims+xml
    Max-Forwards: 70
    Content-Length: 0
    P-Access-Network-Info: 3GPP-NR-TDD;utran-cell-id-3gpp=00101000001000000400
    Privacy: none
    Contact: ;+g.3gpp.icsi-ref="urn%3Aurn-7%3A3gpp-service.ims.icsi.mmtel";audio;+g.3gpp.nw-init-ussi
    Via: SIP/2.0/TCP [3000::2:6c61:18ff:fe5d:9f1e]:44724;branch=z9hG4bK2236085594
    Security-Verify: ipsec-3gpp;alg=hmac-md5-96;spi-c=260;spi-s=256;port-c=5061;port-s=5062;q=0.9,ipsec-3gpp;alg=hmac-sha-1-96;spi-c=260;spi-s=256;port-c=5061;port-s=5062;q=0.7
    Route: ,,,
    Allow: INVITE,ACK,CANCEL,BYE,UPDATE,PRACK,MESSAGE,REFER,NOTIFY,INFO
    P-Preferred-Identity:
    Supported: timer
    Session-Expires: 1800;refresher=uac
    Require: sec-agree
    Proxy-Require: sec-agree
    User-Agent: qti_Lahaina for arm64_RKQ1.210107.001

    Request:UPDATE sip:PeerUE-Public@stf160.etsi.org:6543 SIP/2.0

    IP_SOCKET_IND
    	DATA
    		ConnectionId
    			Protocol = tcp (1)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 5062
    			Remote
    				IpAddr
    					V6
    						Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    						ScopeId = Omit
    				Port = 43642
    		Ind
    			TCP
    				Recv = '555044415445207369703A5065657255452D5075626C6963407374663136302E657473692E6F72673A36353433205349502F322E300D0A46726F6D3A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E3B7461673D313538333833343538320D0A546F3A203C7369703A5065657255452D5075626C6963407374663136302E657473692E6F72673E3B7461673D6162632D494E564954452D46726F6D7461670D0A43616C6C2D49443A20494E564954452D302D376465632D313164302D613736352D30306130633931653662663640464432393A434334333A374642393A303030323A303230433A323946463A464536363A423443370D0A435365713A2034373132205550444154450D0A4163636570743A206170706C69636174696F6E2F7364702C6170706C69636174696F6E2F336770702D696D732B786D6C0D0A4D61782D466F7277617264733A2037300D0A436F6E74656E742D4C656E6774683A20300D0A502D4163636573732D4E6574776F726B2D496E666F3A20334750502D4E522D5444443B757472616E2D63656C6C2D69642D336770703D30303130313030303030313030303030303430300D0A507269766163793A206E6F6E650D0A436F6E746163743A203C7369703A37643530646431382D356565332D346561662D613134352D643331643834393837636239405B333030303A3A323A366336313A313866663A666535643A396631655D3A34343732343E3B2B672E336770702E696373692D7265663D2275726E25334175726E2D37253341336770702D736572766963652E696D732E696373692E6D6D74656C223B617564696F3B2B672E336770702E6E772D696E69742D757373690D0A5669613A205349502F322E302F544350205B333030303A3A323A366336313A313866663A666535643A396631655D3A34343732343B6272616E63683D7A39684734624B323233363038353539340D0A53656375726974792D5665726966793A2069707365632D336770703B616C673D686D61632D6D64352D39363B7370692D633D3236303B7370692D733D3235363B706F72742D633D353036313B706F72742D733D353036323B713D302E392C69707365632D336770703B616C673D686D61632D7368612D312D39363B7370692D633D3236303B7370692D733D3235363B706F72742D633D353036313B706F72742D733D353036323B713D302E370D0A526F7574653A203C7369703A5B666432393A636334333A376662393A323A3230633A323966663A666536363A623463375D3A353036323B6C723E2C3C7369703A7465726D407363736366312E336770702E6F72673B6C723E2C3C7369703A6F726967407363736366322E336770702E6F72673B6C723E2C3C7369703A7063736366322E336770702E6F72673B6C723E0D0A416C6C6F773A20494E564954452C41434B2C43414E43454C2C4259452C5550444154452C505241434B2C4D4553534147452C52454645522C4E4F544946592C494E464F0D0A502D5072656665727265642D4964656E746974793A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E0D0A537570706F727465643A2074696D65720D0A53657373696F6E2D457870697265733A20313830303B7265667265736865723D7561630D0A526571756972653A207365632D61677265650D0A50726F78792D526571756972653A207365632D61677265650D0A557365722D4167656E743A207174695F4C616861696E6120666F722061726D36345F524B51312E3231303130372E3030310D0A0D0A'O

    Received on port: IPMUX:IP_SOCK

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_Main.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 596
    text = Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 596]

    Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 596]

    summary = Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol
    		DATA
    			ConnectionId
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5062
    				Remote
    					IpAddr
    						V6
    							Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    							ScopeId = Omit
    					Port = 43642
    			Ind
    				TCP
    					Recv = '555044415445207369703A5065657255452D5075626C6963407374663136302E657473692E6F72673A36353433205349502F322E300D0A46726F6D3A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E3B7461673D313538333833343538320D0A546F3A203C7369703A5065657255452D5075626C6963407374663136302E657473692E6F72673E3B7461673D6162632D494E564954452D46726F6D7461670D0A43616C6C2D49443A20494E564954452D302D376465632D313164302D613736352D30306130633931653662663640464432393A434334333A374642393A303030323A303230433A323946463A464536363A423443370D0A435365713A2034373132205550444154450D0A4163636570743A206170706C69636174696F6E2F7364702C6170706C69636174696F6E2F336770702D696D732B786D6C0D0A4D61782D466F7277617264733A2037300D0A436F6E74656E742D4C656E6774683A20300D0A502D4163636573732D4E6574776F726B2D496E666F3A20334750502D4E522D5444443B757472616E2D63656C6C2D69642D336770703D30303130313030303030313030303030303430300D0A507269766163793A206E6F6E650D0A436F6E746163743A203C7369703A37643530646431382D356565332D346561662D613134352D643331643834393837636239405B333030303A3A323A366336313A313866663A666535643A396631655D3A34343732343E3B2B672E336770702E696373692D7265663D2275726E25334175726E2D37253341336770702D736572766963652E696D732E696373692E6D6D74656C223B617564696F3B2B672E336770702E6E772D696E69742D757373690D0A5669613A205349502F322E302F544350205B333030303A3A323A366336313A313866663A666535643A396631655D3A34343732343B6272616E63683D7A39684734624B323233363038353539340D0A53656375726974792D5665726966793A2069707365632D336770703B616C673D686D61632D6D64352D39363B7370692D633D3236303B7370692D733D3235363B706F72742D633D353036313B706F72742D733D353036323B713D302E392C69707365632D336770703B616C673D686D61632D7368612D312D39363B7370692D633D3236303B7370692D733D3235363B706F72742D633D353036313B706F72742D733D353036323B713D302E370D0A526F7574653A203C7369703A5B666432393A636334333A376662393A323A3230633A323966663A666536363A623463375D3A353036323B6C723E2C3C7369703A7465726D407363736366312E336770702E6F72673B6C723E2C3C7369703A6F726967407363736366322E336770702E6F72673B6C723E2C3C7369703A7063736366322E336770702E6F72673B6C723E0D0A416C6C6F773A20494E564954452C41434B2C43414E43454C2C4259452C5550444154452C505241434B2C4D4553534147452C52454645522C4E4F544946592C494E464F0D0A502D5072656665727265642D4964656E746974793A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E0D0A537570706F727465643A2074696D65720D0A53657373696F6E2D457870697265733A20313830303B7265667265736865723D7561630D0A526571756972653A207365632D61677265650D0A50726F78792D526571756972653A207365632D61677265650D0A557365722D4167656E743A207174695F4C616861696E6120666F722061726D36345F524B51312E3231303130372E3030310D0A0D0A'O

    Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_Main.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 741
    text = Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 741]

    Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 741]

    summary = Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol
    		DATA
    			ConnectionId
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5062
    				Remote
    					IpAddr
    						V6
    							Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    							ScopeId = Omit
    					Port = 43642
    			Ind
    				TCP
    					Recv = '555044415445207369703A5065657255452D5075626C6963407374663136302E657473692E6F72673A36353433205349502F322E300D0A46726F6D3A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E3B7461673D313538333833343538320D0A546F3A203C7369703A5065657255452D5075626C6963407374663136302E657473692E6F72673E3B7461673D6162632D494E564954452D46726F6D7461670D0A43616C6C2D49443A20494E564954452D302D376465632D313164302D613736352D30306130633931653662663640464432393A434334333A374642393A303030323A303230433A323946463A464536363A423443370D0A435365713A2034373132205550444154450D0A4163636570743A206170706C69636174696F6E2F7364702C6170706C69636174696F6E2F336770702D696D732B786D6C0D0A4D61782D466F7277617264733A2037300D0A436F6E74656E742D4C656E6774683A20300D0A502D4163636573732D4E6574776F726B2D496E666F3A20334750502D4E522D5444443B757472616E2D63656C6C2D69642D336770703D30303130313030303030313030303030303430300D0A507269766163793A206E6F6E650D0A436F6E746163743A203C7369703A37643530646431382D356565332D346561662D613134352D643331643834393837636239405B333030303A3A323A366336313A313866663A666535643A396631655D3A34343732343E3B2B672E336770702E696373692D7265663D2275726E25334175726E2D37253341336770702D736572766963652E696D732E696373692E6D6D74656C223B617564696F3B2B672E336770702E6E772D696E69742D757373690D0A5669613A205349502F322E302F544350205B333030303A3A323A366336313A313866663A666535643A396631655D3A34343732343B6272616E63683D7A39684734624B323233363038353539340D0A53656375726974792D5665726966793A2069707365632D336770703B616C673D686D61632D6D64352D39363B7370692D633D3236303B7370692D733D3235363B706F72742D633D353036313B706F72742D733D353036323B713D302E392C69707365632D336770703B616C673D686D61632D7368612D312D39363B7370692D633D3236303B7370692D733D3235363B706F72742D633D353036313B706F72742D733D353036323B713D302E370D0A526F7574653A203C7369703A5B666432393A636334333A376662393A323A3230633A323966663A666536363A623463375D3A353036323B6C723E2C3C7369703A7465726D407363736366312E336770702E6F72673B6C723E2C3C7369703A6F726967407363736366322E336770702E6F72673B6C723E2C3C7369703A7063736366322E336770702E6F72673B6C723E0D0A416C6C6F773A20494E564954452C41434B2C43414E43454C2C4259452C5550444154452C505241434B2C4D4553534147452C52454645522C4E4F544946592C494E464F0D0A502D5072656665727265642D4964656E746974793A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E0D0A537570706F727465643A2074696D65720D0A53657373696F6E2D457870697265733A20313830303B7265667265736865723D7561630D0A526571756972653A207365632D61677265650D0A50726F78792D526571756972653A207365632D61677265650D0A557365722D4167656E743A207174695F4C616861696E6120666F722061726D36345F524B51312E3231303130372E3030310D0A0D0A'O

    Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 801
    text = Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 802
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 803
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 103
    text = Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 762
    text = Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 763
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 764
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    summary = Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol
    		DATA
    			ConnectionId
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5062
    				Remote
    					IpAddr
    						V6
    							Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    							ScopeId = Omit
    					Port = 43642
    			Ind
    				TCP
    					Recv = '555044415445207369703A5065657255452D5075626C6963407374663136302E657473692E6F72673A36353433205349502F322E300D0A46726F6D3A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E3B7461673D313538333833343538320D0A546F3A203C7369703A5065657255452D5075626C6963407374663136302E657473692E6F72673E3B7461673D6162632D494E564954452D46726F6D7461670D0A43616C6C2D49443A20494E564954452D302D376465632D313164302D613736352D30306130633931653662663640464432393A434334333A374642393A303030323A303230433A323946463A464536363A423443370D0A435365713A2034373132205550444154450D0A4163636570743A206170706C69636174696F6E2F7364702C6170706C69636174696F6E2F336770702D696D732B786D6C0D0A4D61782D466F7277617264733A2037300D0A436F6E74656E742D4C656E6774683A20300D0A502D4163636573732D4E6574776F726B2D496E666F3A20334750502D4E522D5444443B757472616E2D63656C6C2D69642D336770703D30303130313030303030313030303030303430300D0A507269766163793A206E6F6E650D0A436F6E746163743A203C7369703A37643530646431382D356565332D346561662D613134352D643331643834393837636239405B333030303A3A323A366336313A313866663A666535643A396631655D3A34343732343E3B2B672E336770702E696373692D7265663D2275726E25334175726E2D37253341336770702D736572766963652E696D732E696373692E6D6D74656C223B617564696F3B2B672E336770702E6E772D696E69742D757373690D0A5669613A205349502F322E302F544350205B333030303A3A323A366336313A313866663A666535643A396631655D3A34343732343B6272616E63683D7A39684734624B323233363038353539340D0A53656375726974792D5665726966793A2069707365632D336770703B616C673D686D61632D6D64352D39363B7370692D633D3236303B7370692D733D3235363B706F72742D633D353036313B706F72742D733D353036323B713D302E392C69707365632D336770703B616C673D686D61632D7368612D312D39363B7370692D633D3236303B7370692D733D3235363B706F72742D633D353036313B706F72742D733D353036323B713D302E370D0A526F7574653A203C7369703A5B666432393A636334333A376662393A323A3230633A323966663A666536363A623463375D3A353036323B6C723E2C3C7369703A7465726D407363736366312E336770702E6F72673B6C723E2C3C7369703A6F726967407363736366322E336770702E6F72673B6C723E2C3C7369703A7063736366322E336770702E6F72673B6C723E0D0A416C6C6F773A20494E564954452C41434B2C43414E43454C2C4259452C5550444154452C505241434B2C4D4553534147452C52454645522C4E4F544946592C494E464F0D0A502D5072656665727265642D4964656E746974793A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E0D0A537570706F727465643A2074696D65720D0A53657373696F6E2D457870697265733A20313830303B7265667265736865723D7561630D0A526571756972653A207365632D61677265650D0A50726F78792D526571756972653A207365632D61677265650D0A557365722D4167656E743A207174695F4C616861696E6120666F722061726D36345F524B51312E3231303130372E3030310D0A0D0A'O

    Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 103
    text = Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 762
    text = Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 763
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 764
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    summary = Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol
    		DATA
    			ConnectionId
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5062
    				Remote
    					IpAddr
    						V6
    							Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    							ScopeId = Omit
    					Port = 43642
    			Ind
    				TCP
    					Recv = '555044415445207369703A5065657255452D5075626C6963407374663136302E657473692E6F72673A36353433205349502F322E300D0A46726F6D3A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E3B7461673D313538333833343538320D0A546F3A203C7369703A5065657255452D5075626C6963407374663136302E657473692E6F72673E3B7461673D6162632D494E564954452D46726F6D7461670D0A43616C6C2D49443A20494E564954452D302D376465632D313164302D613736352D30306130633931653662663640464432393A434334333A374642393A303030323A303230433A323946463A464536363A423443370D0A435365713A2034373132205550444154450D0A4163636570743A206170706C69636174696F6E2F7364702C6170706C69636174696F6E2F336770702D696D732B786D6C0D0A4D61782D466F7277617264733A2037300D0A436F6E74656E742D4C656E6774683A20300D0A502D4163636573732D4E6574776F726B2D496E666F3A20334750502D4E522D5444443B757472616E2D63656C6C2D69642D336770703D30303130313030303030313030303030303430300D0A507269766163793A206E6F6E650D0A436F6E746163743A203C7369703A37643530646431382D356565332D346561662D613134352D643331643834393837636239405B333030303A3A323A366336313A313866663A666535643A396631655D3A34343732343E3B2B672E336770702E696373692D7265663D2275726E25334175726E2D37253341336770702D736572766963652E696D732E696373692E6D6D74656C223B617564696F3B2B672E336770702E6E772D696E69742D757373690D0A5669613A205349502F322E302F544350205B333030303A3A323A366336313A313866663A666535643A396631655D3A34343732343B6272616E63683D7A39684734624B323233363038353539340D0A53656375726974792D5665726966793A2069707365632D336770703B616C673D686D61632D6D64352D39363B7370692D633D3236303B7370692D733D3235363B706F72742D633D353036313B706F72742D733D353036323B713D302E392C69707365632D336770703B616C673D686D61632D7368612D312D39363B7370692D633D3236303B7370692D733D3235363B706F72742D633D353036313B706F72742D733D353036323B713D302E370D0A526F7574653A203C7369703A5B666432393A636334333A376662393A323A3230633A323966663A666536363A623463375D3A353036323B6C723E2C3C7369703A7465726D407363736366312E336770702E6F72673B6C723E2C3C7369703A6F726967407363736366322E336770702E6F72673B6C723E2C3C7369703A7063736366322E336770702E6F72673B6C723E0D0A416C6C6F773A20494E564954452C41434B2C43414E43454C2C4259452C5550444154452C505241434B2C4D4553534147452C52454645522C4E4F544946592C494E464F0D0A502D5072656665727265642D4964656E746974793A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E0D0A537570706F727465643A2074696D65720D0A53657373696F6E2D457870697265733A20313830303B7265667265736865723D7561630D0A526571756972653A207365632D61677265650D0A50726F78792D526571756972653A207365632D61677265650D0A557365722D4167656E743A207174695F4C616861696E6120666F722061726D36345F524B51312E3231303130372E3030310D0A0D0A'O

    Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 722
    text = Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 723
    text = Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 724
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 725
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 722
    text = Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 723
    text = Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 724
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 725
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    IP_SOCKET_IND
    	DATA
    		ConnectionId
    			Protocol = tcp (1)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 5062
    			Remote
    				IpAddr
    					V6
    						Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    						ScopeId = Omit
    				Port = 43642
    		Ind
    			TCP
    				Recv = '555044415445207369703A5065657255452D5075626C6963407374663136302E657473692E6F72673A36353433205349502F322E300D0A46726F6D3A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E3B7461673D313538333833343538320D0A546F3A203C7369703A5065657255452D5075626C6963407374663136302E657473692E6F72673E3B7461673D6162632D494E564954452D46726F6D7461670D0A43616C6C2D49443A20494E564954452D302D376465632D313164302D613736352D30306130633931653662663640464432393A434334333A374642393A303030323A303230433A323946463A464536363A423443370D0A435365713A2034373132205550444154450D0A4163636570743A206170706C69636174696F6E2F7364702C6170706C69636174696F6E2F336770702D696D732B786D6C0D0A4D61782D466F7277617264733A2037300D0A436F6E74656E742D4C656E6774683A20300D0A502D4163636573732D4E6574776F726B2D496E666F3A20334750502D4E522D5444443B757472616E2D63656C6C2D69642D336770703D30303130313030303030313030303030303430300D0A507269766163793A206E6F6E650D0A436F6E746163743A203C7369703A37643530646431382D356565332D346561662D613134352D643331643834393837636239405B333030303A3A323A366336313A313866663A666535643A396631655D3A34343732343E3B2B672E336770702E696373692D7265663D2275726E25334175726E2D37253341336770702D736572766963652E696D732E696373692E6D6D74656C223B617564696F3B2B672E336770702E6E772D696E69742D757373690D0A5669613A205349502F322E302F544350205B333030303A3A323A366336313A313866663A666535643A396631655D3A34343732343B6272616E63683D7A39684734624B323233363038353539340D0A53656375726974792D5665726966793A2069707365632D336770703B616C673D686D61632D6D64352D39363B7370692D633D3236303B7370692D733D3235363B706F72742D633D353036313B706F72742D733D353036323B713D302E392C69707365632D336770703B616C673D686D61632D7368612D312D39363B7370692D633D3236303B7370692D733D3235363B706F72742D633D353036313B706F72742D733D353036323B713D302E370D0A526F7574653A203C7369703A5B666432393A636334333A376662393A323A3230633A323966663A666536363A623463375D3A353036323B6C723E2C3C7369703A7465726D407363736366312E336770702E6F72673B6C723E2C3C7369703A6F726967407363736366322E336770702E6F72673B6C723E2C3C7369703A7063736366322E336770702E6F72673B6C723E0D0A416C6C6F773A20494E564954452C41434B2C43414E43454C2C4259452C5550444154452C505241434B2C4D4553534147452C52454645522C4E4F544946592C494E464F0D0A502D5072656665727265642D4964656E746974793A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E0D0A537570706F727465643A2074696D65720D0A53657373696F6E2D457870697265733A20313830303B7265667265736865723D7561630D0A526571756972653A207365632D61677265650D0A50726F78792D526571756972653A207365632D61677265650D0A557365722D4167656E743A207174695F4C616861696E6120666F722061726D36345F524B51312E3231303130372E3030310D0A0D0A'O

    Inter-component message: IP_SOCK_DATA -> IP:IP_SOCK_DATA

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 742
    text = Parameter: IP_PTC_IMS_Handler.v_Data = '555044415445207369703A5065657255452D5075626C6963407374663136302E657473692E6F72673A36353433205349502F322E300D0A46726F6D3A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E3B7461673D313538333833343538320D0A546F3A203C7369703A5065657255452D5075626C6963407374663136302E657473692E6F72673E3B7461673D6162632D494E564954452D46726F6D7461670D0A43616C6C2D49443A20494E564954452D302D376465632D313164302D613736352D30306130633931653662663640464432393A434334333A374642393A303030323A303230433A323946463A464536363A423443370D0A435365713A2034373132205550444154450D0A4163636570743A206170706C69636174696F6E2F7364702C6170706C69636174696F6E2F336770702D696D732B786D6C0D0A4D61782D466F7277617264733A2037300D0A436F6E74656E742D4C656E6774683A20300D0A502D4163636573732D4E6574776F726B2D496E666F3A20334750502D4E522D5444443B7574726...

    Parameter: IP_PTC_IMS_Handler.v_Data = '555044415445207369703A5065657255452D5075626C6963407374663136302E657473692E6F72673A36353433205349502F322E300D0A46726F6D3A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E3B7461673D313538333833343538320D0A546F3A203C7369703A5065657255452D5075626C6963407374663136302E657473692E6F72673E3B7461673D6162632D494E564954452D46726F6D7461670D0A43616C6C2D49443A20494E564954452D302D376465632D313164302D613736352D30306130633931653662663640464432393A434334333A374642393A303030323A303230433A323946463A464536363A423443370D0A435365713A2034373132205550444154450D0A4163636570743A206170706C69636174696F6E2F7364702C6170706C69636174696F6E2F336770702D696D732B786D6C0D0A4D61782D466F7277617264733A2037300D0A436F6E74656E742D4C656E6774683A20300D0A502D4163636573732D4E6574776F726B2D496E666F3A20334750502D4E522D5444443B7574726...

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 697
    text = Parameter: IP_PTC_IMS_Handler.v_Bitstring = '010101010101000001000100010000010101010001000101001000000111001101101001011100000011101001010000011001010110010101110010010101010100010100101101010100000111010101100010011011000110100101100011010000000111001101110100011001100011000100110110001100000010111001100101011101000111001101101001001011100110111101110010011001110011101000110110001101010011010000110011001000000101001101001001010100000010111100110010001011100011000000001101000010100100011001110010011011110110110100111010001000000011110001110011011010010111000000111010001100000011000000110001001100000011000100110000001100010011001000110011001101000011010100110110001101110011100000111001010000000110100101101101011100110010111001101101011011100110001100110000001100000011000100101110011011010110001101100011001100000011000000110001001011100011001101100111011100000111000001101110011001010111...

    Parameter: IP_PTC_IMS_Handler.v_Bitstring = '010101010101000001000100010000010101010001000101001000000111001101101001011100000011101001010000011001010110010101110010010101010100010100101101010100000111010101100010011011000110100101100011010000000111001101110100011001100011000100110110001100000010111001100101011101000111001101101001001011100110111101110010011001110011101000110110001101010011010000110011001000000101001101001001010100000010111100110010001011100011000000001101000010100100011001110010011011110110110100111010001000000011110001110011011010010111000000111010001100000011000000110001001100000011000100110000001100010011001000110011001101000011010100110110001101110011100000111001010000000110100101101101011100110010111001101101011011100110001100110000001100000011000100101110011011010110001101100011001100000011000000110001001011100011001101100111011100000111000001101110011001010111...

    IMS_DATA_REQ
    	RoutingInfo
    		Protocol = tcp (1)
    		Security = protectedContext1 (1)
    		UE_Address
    			V6
    				Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    				ScopeId = Omit
    		NW_Address
    			V6
    				Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    				ScopeId = Omit
    	Request
    		Update
    			requestLine
    				method = UPDATE_E (11)
    				requestUri
    					scheme = 'sip'
    					components
    						sip
    							userInfo
    								userOrTelephoneSubscriber = 'PeerUE-Public'
    								password = Omit
    							hostPort
    								host = 'stf160.etsi.org'
    								portField = 6543
    					urlParameters = Omit
    					headers = Omit
    				sipVersion = 'SIP/2.0'
    			msgHeader
    				accept
    					fieldName = ACCEPT_E (0)
    					acceptArgs
    						AcceptBody
    							mediaRange = 'application/sdp'
    							acceptParam = Omit
    						AcceptBody
    							mediaRange = 'application/3gpp-ims+xml'
    							acceptParam = Omit
    				acceptContact = Omit
    				acceptEncoding = Omit
    				acceptLanguage = Omit
    				alertInfo = Omit
    				allow
    					fieldName = ALLOW_E (4)
    					methods
    						CharacterStringType = 'INVITE'
    						CharacterStringType = 'ACK'
    						CharacterStringType = 'CANCEL'
    						CharacterStringType = 'BYE'
    						CharacterStringType = 'UPDATE'
    						CharacterStringType = 'PRACK'
    						CharacterStringType = 'MESSAGE'
    						CharacterStringType = 'REFER'
    						CharacterStringType = 'NOTIFY'
    						CharacterStringType = 'INFO'
    				allowEvents = Omit
    				authenticationInfo = Omit
    				authorization = Omit
    				callId
    					fieldName = CALL_ID_E (7)
    					callid = 'INVITE-0-7dec-11d0-a765-00a0c91e6bf6@FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    				callInfo = Omit
    				contact
    					fieldName = CONTACT_E (9)
    					contactBody
    						contactAddresses
    							ContactAddress
    								addressField
    									nameAddr
    										displayName = Omit
    										addrSpec
    											scheme = 'sip'
    											components
    												sip
    													userInfo
    														userOrTelephoneSubscriber = '7d50dd18-5ee3-4eaf-a145-d31d84987cb9'
    														password = Omit
    													hostPort
    														host = '3000::2:6c61:18ff:fe5d:9f1e'
    														portField = 44724
    											urlParameters = Omit
    											headers = Omit
    								contactParams
    									GenericParam
    										id = '+g.3gpp.icsi-ref'
    										paramValue
    											quotedString = 'urn%3Aurn-7%3A3gpp-service.ims.icsi.mmtel'
    									GenericParam
    										id = 'audio'
    										paramValue = Omit
    									GenericParam
    										id = '+g.3gpp.nw-init-ussi'
    										paramValue = Omit
    				contentDisposition = Omit
    				contentEncoding = Omit
    				contentLanguage = Omit
    				contentLength
    					fieldName = CONTENT_LENGTH_E (13)
    					len = 0
    				contentType = Omit
    				cSeq
    					fieldName = CSEQ_E (15)
    					seqNumber = 4712
    					method = 'UPDATE'
    				date = Omit
    				errorInfo = Omit
    				event = Omit
    				expires = Omit
    				featureCaps = Omit
    				fromField
    					fieldName = FROM_E (19)
    					addressField
    						nameAddr
    							displayName = Omit
    							addrSpec
    								scheme = 'sip'
    								components
    									sip
    										userInfo
    											userOrTelephoneSubscriber = '001010123456789'
    											password = Omit
    										hostPort
    											host = 'ims.mnc001.mcc001.3gppnetwork.org'
    											portField = Omit
    								urlParameters = Omit
    								headers = Omit
    					fromParams
    						GenericParam
    							id = 'tag'
    							paramValue
    								tokenOrHost = '1583834582'
    				geolocation = Omit
    				geolocationRouting = Omit
    				historyInfo = Omit
    				infoPackage = Omit
    				inReplyTo = Omit
    				maxForwards
    					fieldName = MAX_FORWARDS_E (21)
    					forwards = 70
    				mimeVersion = Omit
    				minExpires = Omit
    				minSE = Omit
    				organization = Omit
    				pAccessNetworkInfo
    					fieldName = P_ACCESS_NETWORK_INFO_E (65)
    					accessType = '3GPP-NR-TDD'
    					genericParams
    						GenericParam
    							id = 'utran-cell-id-3gpp'
    							paramValue
    								tokenOrHost = '00101000001000000400'
    				pAssertedID = Omit
    				pAssertedService = Omit
    				pAssociatedURI = Omit
    				path = Omit
    				pCalledPartyID = Omit
    				pChargingFunctionAddresses = Omit
    				pChargingVector = Omit
    				pEarlyMedia = Omit
    				pMediaAuthorization = Omit
    				pPreferredID
    					fieldName = P_PREFERRED_ID_E (52)
    					pPreferredIDValueList
    						PPreferredIDValue
    							nameAddr
    								displayName = Omit
    								addrSpec
    									scheme = 'sip'
    									components
    										sip
    											userInfo
    												userOrTelephoneSubscriber = '001010123456789'
    												password = Omit
    											hostPort
    												host = 'ims.mnc001.mcc001.3gppnetwork.org'
    												portField = Omit
    									urlParameters = Omit
    									headers = Omit
    				pPreferredService = Omit
    				priority = Omit
    				privacy
    					fieldName = PRIVACY_E (50)
    					privValueList
    						CharacterStringType = 'none'
    				proxyAuthenticate = Omit
    				proxyAuthorization = Omit
    				proxyRequire
    					fieldName = PROXY_REQUIRE_E (28)
    					optionsTags
    						CharacterStringType = 'sec-agree'
    				pVisitedNetworkID = Omit
    				rAck = Omit
    				rSeq = Omit
    				reason = Omit
    				recordRoute = Omit
    				recvInfo = Omit
    				requestDisposition = Omit
    				referredBy = Omit
    				referTo = Omit
    				referSub = Omit
    				replaces = Omit
    				replyTo = Omit
    				require
    					fieldName = REQUIRE_E (31)
    					optionsTags
    						CharacterStringType = 'sec-agree'
    				retryAfter = Omit
    				route
    					fieldName = ROUTE_E (33)
    					routeBody
    						RouteBody
    							nameAddr
    								displayName = Omit
    								addrSpec
    									scheme = 'sip'
    									components
    										sip
    											userInfo = Omit
    											hostPort
    												host = 'fd29:cc43:7fb9:2:20c:29ff:fe66:b4c7'
    												portField = 5062
    									urlParameters
    										GenericParam
    											id = 'lr'
    											paramValue = Omit
    									headers = Omit
    							rrParam = Omit
    						RouteBody
    							nameAddr
    								displayName = Omit
    								addrSpec
    									scheme = 'sip'
    									components
    										sip
    											userInfo
    												userOrTelephoneSubscriber = 'term'
    												password = Omit
    											hostPort
    												host = 'scscf1.3gpp.org'
    												portField = Omit
    									urlParameters
    										GenericParam
    											id = 'lr'
    											paramValue = Omit
    									headers = Omit
    							rrParam = Omit
    						RouteBody
    							nameAddr
    								displayName = Omit
    								addrSpec
    									scheme = 'sip'
    									components
    										sip
    											userInfo
    												userOrTelephoneSubscriber = 'orig'
    												password = Omit
    											hostPort
    												host = 'scscf2.3gpp.org'
    												portField = Omit
    									urlParameters
    										GenericParam
    											id = 'lr'
    											paramValue = Omit
    									headers = Omit
    							rrParam = Omit
    						RouteBody
    							nameAddr
    								displayName = Omit
    								addrSpec
    									scheme = 'sip'
    									components
    										sip
    											userInfo = Omit
    											hostPort
    												host = 'pcscf2.3gpp.org'
    												portField = Omit
    									urlParameters
    										GenericParam
    											id = 'lr'
    											paramValue = Omit
    									headers = Omit
    							rrParam = Omit
    				securityClient = Omit
    				securityServer = Omit
    				securityVerify
    					fieldName = SECURITY_VERIFY_E (64)
    					securityMech
    						SecurityMechanism
    							mechName = 'ipsec-3gpp'
    							mechParams
    								GenericParam
    									id = 'alg'
    									paramValue
    										tokenOrHost = 'hmac-md5-96'
    								GenericParam
    									id = 'spi-c'
    									paramValue
    										tokenOrHost = '260'
    								GenericParam
    									id = 'spi-s'
    									paramValue
    										tokenOrHost = '256'
    								GenericParam
    									id = 'port-c'
    									paramValue
    										tokenOrHost = '5061'
    								GenericParam
    									id = 'port-s'
    									paramValue
    										tokenOrHost = '5062'
    								GenericParam
    									id = 'q'
    									paramValue
    										tokenOrHost = '0.9'
    						SecurityMechanism
    							mechName = 'ipsec-3gpp'
    							mechParams
    								GenericParam
    									id = 'alg'
    									paramValue
    										tokenOrHost = 'hmac-sha-1-96'
    								GenericParam
    									id = 'spi-c'
    									paramValue
    										tokenOrHost = '260'
    								GenericParam
    									id = 'spi-s'
    									paramValue
    										tokenOrHost = '256'
    								GenericParam
    									id = 'port-c'
    									paramValue
    										tokenOrHost = '5061'
    								GenericParam
    									id = 'port-s'
    									paramValue
    										tokenOrHost = '5062'
    								GenericParam
    									id = 'q'
    									paramValue
    										tokenOrHost = '0.7'
    				server = Omit
    				serviceRoute = Omit
    				sessionExpires
    					fieldName = SESSION_EXPIRES_E (75)
    					deltaSec = '1800'
    					seParam
    						GenericParam
    							id = 'refresher'
    							paramValue
    								tokenOrHost = 'uac'
    				sessionId = Omit
    				sipETag = Omit
    				sipIfMatch = Omit
    				subject = Omit
    				subscriptionState = Omit
    				supported
    					fieldName = SUPPORTED_E (36)
    					optionsTags
    						CharacterStringType = 'timer'
    				timestamp = Omit
    				toField
    					fieldName = TO_E (38)
    					addressField
    						nameAddr
    							displayName = Omit
    							addrSpec
    								scheme = 'sip'
    								components
    									sip
    										userInfo
    											userOrTelephoneSubscriber = 'PeerUE-Public'
    											password = Omit
    										hostPort
    											host = 'stf160.etsi.org'
    											portField = Omit
    								urlParameters = Omit
    								headers = Omit
    					toParams
    						GenericParam
    							id = 'tag'
    							paramValue
    								tokenOrHost = 'abc-INVITE-Fromtag'
    				unsupported = Omit
    				userToUser = Omit
    				userAgent
    					fieldName = USER_AGENT_E (40)
    					userAgentBody
    						CharacterStringType = 'qti_Lahaina for arm64_RKQ1.210107.001'
    				via
    					fieldName = VIA_E (41)
    					viaBody
    						ViaBody
    							sentProtocol
    								protocolName = 'SIP'
    								protocolVersion = '2.0'
    								transport = 'TCP'
    							sentBy
    								host = '3000::2:6c61:18ff:fe5d:9f1e'
    								portField = 44724
    							viaParams
    								GenericParam
    									id = 'branch'
    									paramValue
    										tokenOrHost = 'z9hG4bK2236085594'
    				warning = Omit
    				wwwAuthenticate = Omit
    				resourcePriority = Omit
    				answerMode = Omit
    				privAnswerMode = Omit
    				targetDialog = Omit
    				pAnswerState = Omit
    				undefinedHeader_List = Omit
    			messageBody = Omit
    			payload = Omit

    Inter-component message: IMS_Server -> IMS1:IMS_Server

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_Main.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 596
    text = Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 596]

    Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 596]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 993
    text = Parameter: IMS_Procedures_Common.v_MessageBody = Omit
    File: IMS_Procedures_Common.ttcn [Line: 993]

    Parameter: IMS_Procedures_Common.v_MessageBody = Omit
    File: IMS_Procedures_Common.ttcn [Line: 993]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_Main.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 741
    text = Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 741]

    Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 741]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 801
    text = Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    timerEvent = 7
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\IMS\Common\IMS_CC_SessionTimerCommon.ttcn
    testName = TC_7_34_NR5GC
    lineNo = 210
    outStr = Timer: t_Timer, Stopped: 06:16:48

    Timer: t_Timer, Stopped: 06:16:48

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 802
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 803
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 103
    text = Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 762
    text = Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 763
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 764
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 103
    text = Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 762
    text = Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 763
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 764
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 722
    text = Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 723
    text = Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 724
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 725
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 722
    text = Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 723
    text = Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 724
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 725
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 801
    text = Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 802
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 803
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1074
    text = Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 1074]

    Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 1074]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1075
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 1075]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 1075]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1076
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1076]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1076]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 103
    text = Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 281
    text = Parameter: IMS_CommonTemplates.i = 0
    File: IMS_CommonTemplates.ttcn [Line: 281]

    Parameter: IMS_CommonTemplates.i = 0
    File: IMS_CommonTemplates.ttcn [Line: 281]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 281
    text = Parameter: IMS_CommonTemplates.i = 1
    File: IMS_CommonTemplates.ttcn [Line: 281]

    Parameter: IMS_CommonTemplates.i = 1
    File: IMS_CommonTemplates.ttcn [Line: 281]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 216
    text = Parameter: IMS_CommonTemplates.v_NoOfParams = 1
    File: IMS_CommonTemplates.ttcn [Line: 216]

    Parameter: IMS_CommonTemplates.v_NoOfParams = 1
    File: IMS_CommonTemplates.ttcn [Line: 216]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 274
    text = Parameter: IP_PTC_IMS_Handler.v_TcpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 274]

    Parameter: IP_PTC_IMS_Handler.v_TcpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 274]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 103
    text = Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 217
    text = Parameter: IMS_CommonTemplates.v_RequestedParamId = 'refresher'
    File: IMS_CommonTemplates.ttcn [Line: 217]

    Parameter: IMS_CommonTemplates.v_RequestedParamId = 'refresher'
    File: IMS_CommonTemplates.ttcn [Line: 217]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 221
    text = Parameter: IMS_CommonTemplates.i = 0
    File: IMS_CommonTemplates.ttcn [Line: 221]

    Parameter: IMS_CommonTemplates.i = 0
    File: IMS_CommonTemplates.ttcn [Line: 221]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 222
    text = Parameter: IMS_CommonTemplates.v_ParamId = 'refresher'
    File: IMS_CommonTemplates.ttcn [Line: 222]

    Parameter: IMS_CommonTemplates.v_ParamId = 'refresher'
    File: IMS_CommonTemplates.ttcn [Line: 222]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 240
    text = Parameter: IMS_CommonTemplates.i = 0
    File: IMS_CommonTemplates.ttcn [Line: 240]

    Parameter: IMS_CommonTemplates.i = 0
    File: IMS_CommonTemplates.ttcn [Line: 240]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 274
    text = Parameter: IP_PTC_IMS_Handler.v_TcpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 274]

    Parameter: IP_PTC_IMS_Handler.v_TcpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 274]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 247
    text = Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 247]

    Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 247]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 248
    text = Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 248]

    Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 248]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 247
    text = Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 247]

    Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 247]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 248
    text = Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 248]

    Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 248]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1074
    text = Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1074]

    Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1074]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1075
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1075]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1075]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1076
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1076]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1076]

    IntermediateVerdict = (Pass)
    summary = Intermediate verdict: (PASS)
    TTCN-3 message: Step 21

    Intermediate verdict: (PASS)
    TTCN-3 message: Step 21

    recordType = 24
    summary = Step 22

    Step 22

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 281
    text = Parameter: IMS_CommonTemplates.i = 0
    File: IMS_CommonTemplates.ttcn [Line: 281]

    Parameter: IMS_CommonTemplates.i = 0
    File: IMS_CommonTemplates.ttcn [Line: 281]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 281
    text = Parameter: IMS_CommonTemplates.i = 1
    File: IMS_CommonTemplates.ttcn [Line: 281]

    Parameter: IMS_CommonTemplates.i = 1
    File: IMS_CommonTemplates.ttcn [Line: 281]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 216
    text = Parameter: IMS_CommonTemplates.v_NoOfParams = 1
    File: IMS_CommonTemplates.ttcn [Line: 216]

    Parameter: IMS_CommonTemplates.v_NoOfParams = 1
    File: IMS_CommonTemplates.ttcn [Line: 216]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 217
    text = Parameter: IMS_CommonTemplates.v_RequestedParamId = 'tag'
    File: IMS_CommonTemplates.ttcn [Line: 217]

    Parameter: IMS_CommonTemplates.v_RequestedParamId = 'tag'
    File: IMS_CommonTemplates.ttcn [Line: 217]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 221
    text = Parameter: IMS_CommonTemplates.i = 0
    File: IMS_CommonTemplates.ttcn [Line: 221]

    Parameter: IMS_CommonTemplates.i = 0
    File: IMS_CommonTemplates.ttcn [Line: 221]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 222
    text = Parameter: IMS_CommonTemplates.v_ParamId = 'tag'
    File: IMS_CommonTemplates.ttcn [Line: 222]

    Parameter: IMS_CommonTemplates.v_ParamId = 'tag'
    File: IMS_CommonTemplates.ttcn [Line: 222]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 240
    text = Parameter: IMS_CommonTemplates.i = 0
    File: IMS_CommonTemplates.ttcn [Line: 240]

    Parameter: IMS_CommonTemplates.i = 0
    File: IMS_CommonTemplates.ttcn [Line: 240]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_SIP_Templates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1649
    text = Parameter: IMS_SIP_Templates.v_ToTag = Omit
    File: IMS_SIP_Templates.ttcn [Line: 1649]

    Parameter: IMS_SIP_Templates.v_ToTag = Omit
    File: IMS_SIP_Templates.ttcn [Line: 1649]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_SIP_Templates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1652
    text = Parameter: IMS_SIP_Templates.v_ToTag = 'abc-INVITE-Fromtag'
    File: IMS_SIP_Templates.ttcn [Line: 1652]

    Parameter: IMS_SIP_Templates.v_ToTag = 'abc-INVITE-Fromtag'
    File: IMS_SIP_Templates.ttcn [Line: 1652]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 139
    text = Parameter: IMS_Procedures_Common.v_ToTag = 'abc-INVITE-Fromtag'
    File: IMS_Procedures_Common.ttcn [Line: 139]

    Parameter: IMS_Procedures_Common.v_ToTag = 'abc-INVITE-Fromtag'
    File: IMS_Procedures_Common.ttcn [Line: 139]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 175
    text = Parameter: IMS_Procedures_Common.v_ToTag = 'abc-INVITE-Fromtag'
    File: IMS_Procedures_Common.ttcn [Line: 175]

    Parameter: IMS_Procedures_Common.v_ToTag = 'abc-INVITE-Fromtag'
    File: IMS_Procedures_Common.ttcn [Line: 175]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 114
    text = Parameter: IMS_CommonTemplates.v_GenValue = Omit
    File: IMS_CommonTemplates.ttcn [Line: 114]

    Parameter: IMS_CommonTemplates.v_GenValue = Omit
    File: IMS_CommonTemplates.ttcn [Line: 114]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_CallControl4G5G.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 317
    text = Parameter: IMS_Procedures_CallControl4G5G.v_Method = 'UPDATE'
    File: IMS_Procedures_CallControl4G5G.ttcn [Line: 317]

    Parameter: IMS_Procedures_CallControl4G5G.v_Method = 'UPDATE'
    File: IMS_Procedures_CallControl4G5G.ttcn [Line: 317]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_CallControl4G5G.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 318
    text = Parameter: IMS_Procedures_CallControl4G5G.v_A1A3 = False
    File: IMS_Procedures_CallControl4G5G.ttcn [Line: 318]

    Parameter: IMS_Procedures_CallControl4G5G.v_A1A3 = False
    File: IMS_Procedures_CallControl4G5G.ttcn [Line: 318]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_CallControl4G5G.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 319
    text = Parameter: IMS_Procedures_CallControl4G5G.v_A18 = False
    File: IMS_Procedures_CallControl4G5G.ttcn [Line: 319]

    Parameter: IMS_Procedures_CallControl4G5G.v_A18 = False
    File: IMS_Procedures_CallControl4G5G.ttcn [Line: 319]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_CallControl4G5G.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 320
    text = Parameter: IMS_Procedures_CallControl4G5G.v_A19 = False
    File: IMS_Procedures_CallControl4G5G.ttcn [Line: 320]

    Parameter: IMS_Procedures_CallControl4G5G.v_A19 = False
    File: IMS_Procedures_CallControl4G5G.ttcn [Line: 320]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_CallControl4G5G.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 322
    text = Parameter: IMS_Procedures_CallControl4G5G.v_Require = Omit
    File: IMS_Procedures_CallControl4G5G.ttcn [Line: 322]

    Parameter: IMS_Procedures_CallControl4G5G.v_Require = Omit
    File: IMS_Procedures_CallControl4G5G.ttcn [Line: 322]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_CallControl4G5G.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 323
    text = Parameter: IMS_Procedures_CallControl4G5G.v_ContactParams = Omit
    File: IMS_Procedures_CallControl4G5G.ttcn [Line: 323]

    Parameter: IMS_Procedures_CallControl4G5G.v_ContactParams = Omit
    File: IMS_Procedures_CallControl4G5G.ttcn [Line: 323]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_CallControl4G5G.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 335
    text = Parameter: IMS_Procedures_CallControl4G5G.v_A1A3 = True
    File: IMS_Procedures_CallControl4G5G.ttcn [Line: 335]

    Parameter: IMS_Procedures_CallControl4G5G.v_A1A3 = True
    File: IMS_Procedures_CallControl4G5G.ttcn [Line: 335]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_CallControl4G5G.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 338
    text = Parameter: IMS_Procedures_CallControl4G5G.v_MessageHeader_Response.require = Omit
    File: IMS_Procedures_CallControl4G5G.ttcn [Line: 338]

    Parameter: IMS_Procedures_CallControl4G5G.v_MessageHeader_Response.require = Omit
    File: IMS_Procedures_CallControl4G5G.ttcn [Line: 338]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_CallControl4G5G.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 339
    text = Parameter: IMS_Procedures_CallControl4G5G.v_MessageHeader_Response.contentType = Omit
    File: IMS_Procedures_CallControl4G5G.ttcn [Line: 339]

    Parameter: IMS_Procedures_CallControl4G5G.v_MessageHeader_Response.contentType = Omit
    File: IMS_Procedures_CallControl4G5G.ttcn [Line: 339]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 230
    text = Parameter: IMS_Procedures_Common.v_SigCompParam = Omit
    File: IMS_Procedures_Common.ttcn [Line: 230]

    Parameter: IMS_Procedures_Common.v_SigCompParam = Omit
    File: IMS_Procedures_Common.ttcn [Line: 230]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 231
    text = Parameter: IMS_Procedures_Common.v_Port_ps = Omit
    File: IMS_Procedures_Common.ttcn [Line: 231]

    Parameter: IMS_Procedures_Common.v_Port_ps = Omit
    File: IMS_Procedures_Common.ttcn [Line: 231]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 100
    text = Parameter: IMS_Procedures_Common.v_Port_ps = 5060
    File: IMS_Procedures_Common.ttcn [Line: 100]

    Parameter: IMS_Procedures_Common.v_Port_ps = 5060
    File: IMS_Procedures_Common.ttcn [Line: 100]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 104
    text = Parameter: IMS_Procedures_Common.v_Port_ps = 5062
    File: IMS_Procedures_Common.ttcn [Line: 104]

    Parameter: IMS_Procedures_Common.v_Port_ps = 5062
    File: IMS_Procedures_Common.ttcn [Line: 104]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 236
    text = Parameter: IMS_Procedures_Common.v_Port_ps = 5062
    File: IMS_Procedures_Common.ttcn [Line: 236]

    Parameter: IMS_Procedures_Common.v_Port_ps = 5062
    File: IMS_Procedures_Common.ttcn [Line: 236]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 867
    text = Parameter: IMS_Component.v_P_CSCF_Address = 'fd29:cc43:7fb9:2:20c:29ff:fe66:b4c7'
    File: IMS_Component.ttcn [Line: 867]

    Parameter: IMS_Component.v_P_CSCF_Address = 'fd29:cc43:7fb9:2:20c:29ff:fe66:b4c7'
    File: IMS_Component.ttcn [Line: 867]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 114
    text = Parameter: IMS_CommonTemplates.v_GenValue = Omit
    File: IMS_CommonTemplates.ttcn [Line: 114]

    Parameter: IMS_CommonTemplates.v_GenValue = Omit
    File: IMS_CommonTemplates.ttcn [Line: 114]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_SIP_Templates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1159
    text = Parameter: IMS_SIP_Templates.v_RRParamList = Omit
    File: IMS_SIP_Templates.ttcn [Line: 1159]

    Parameter: IMS_SIP_Templates.v_RRParamList = Omit
    File: IMS_SIP_Templates.ttcn [Line: 1159]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 114
    text = Parameter: IMS_CommonTemplates.v_GenValue = Omit
    File: IMS_CommonTemplates.ttcn [Line: 114]

    Parameter: IMS_CommonTemplates.v_GenValue = Omit
    File: IMS_CommonTemplates.ttcn [Line: 114]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_SIP_Templates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1734
    text = Parameter: IMS_SIP_Templates.v_BitStr = '01110011011010010111000000111010011100000110001101110011011000110110011000101110011011110111010001101000011001010111001000101110011000110110111101101101'B
    File: IMS_SIP_Templates.ttcn [Line: 1734]

    Parameter: IMS_SIP_Templates.v_BitStr = '01110011011010010111000000111010011100000110001101110011011000110110011000101110011011110111010001101000011001010111001000101110011000110110111101101101'B
    File: IMS_SIP_Templates.ttcn [Line: 1734]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 114
    text = Parameter: IMS_CommonTemplates.v_GenValue = Omit
    File: IMS_CommonTemplates.ttcn [Line: 114]

    Parameter: IMS_CommonTemplates.v_GenValue = Omit
    File: IMS_CommonTemplates.ttcn [Line: 114]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_SIP_Templates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1734
    text = Parameter: IMS_SIP_Templates.v_BitStr = '01110011011010010111000000111010011100110110001101110011011000110110011000101110011011110111010001101000011001010111001000101110011000110110111101101101'B
    File: IMS_SIP_Templates.ttcn [Line: 1734]

    Parameter: IMS_SIP_Templates.v_BitStr = '01110011011010010111000000111010011100110110001101110011011000110110011000101110011011110111010001101000011001010111001000101110011000110110111101101101'B
    File: IMS_SIP_Templates.ttcn [Line: 1734]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 114
    text = Parameter: IMS_CommonTemplates.v_GenValue = Omit
    File: IMS_CommonTemplates.ttcn [Line: 114]

    Parameter: IMS_CommonTemplates.v_GenValue = Omit
    File: IMS_CommonTemplates.ttcn [Line: 114]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_SIP_Templates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1734
    text = Parameter: IMS_SIP_Templates.v_BitStr = '0111001101101001011100000011101001101111011100100110100101100111010000000111001101100011011100110110001101100110001011100011001101100111011100000111000000101110011011110111001001100111'B
    File: IMS_SIP_Templates.ttcn [Line: 1734]

    Parameter: IMS_SIP_Templates.v_BitStr = '0111001101101001011100000011101001101111011100100110100101100111010000000111001101100011011100110110001101100110001011100011001101100111011100000111000000101110011011110111001001100111'B
    File: IMS_SIP_Templates.ttcn [Line: 1734]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 114
    text = Parameter: IMS_CommonTemplates.v_GenValue = Omit
    File: IMS_CommonTemplates.ttcn [Line: 114]

    Parameter: IMS_CommonTemplates.v_GenValue = Omit
    File: IMS_CommonTemplates.ttcn [Line: 114]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 28
    text = Parameter: IMS_CommonTemplates.i = 0
    File: IMS_CommonTemplates.ttcn [Line: 28]

    Parameter: IMS_CommonTemplates.i = 0
    File: IMS_CommonTemplates.ttcn [Line: 28]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 35
    text = Parameter: IMS_CommonTemplates.k = 0
    File: IMS_CommonTemplates.ttcn [Line: 35]

    Parameter: IMS_CommonTemplates.k = 0
    File: IMS_CommonTemplates.ttcn [Line: 35]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 35
    text = Parameter: IMS_CommonTemplates.k = 1
    File: IMS_CommonTemplates.ttcn [Line: 35]

    Parameter: IMS_CommonTemplates.k = 1
    File: IMS_CommonTemplates.ttcn [Line: 35]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_SIP_Templates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1734
    text = Parameter: IMS_SIP_Templates.v_BitStr = '0111010001100101011011000011101000110001001100100011001100111011011100000110100001101111011011100110010100101101011000110110111101101110011101000110010101111000011101000011110101110100011001010111001101110100001011100011001101100111011100000111000000101110011000110110111101101101'B
    File: IMS_SIP_Templates.ttcn [Line: 1734]

    Parameter: IMS_SIP_Templates.v_BitStr = '0111010001100101011011000011101000110001001100100011001100111011011100000110100001101111011011100110010100101101011000110110111101101110011101000110010101111000011101000011110101110100011001010111001101110100001011100011001101100111011100000111000000101110011000110110111101101101'B
    File: IMS_SIP_Templates.ttcn [Line: 1734]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\IMS\Common\IMS_CC_SessionTimerCommon.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 166
    text = Parameter: IMS_CC_SessionTimerCommon.v_MessageHeader_200.allow = Omit
    File: IMS_CC_SessionTimerCommon.ttcn [Line: 166]

    Parameter: IMS_CC_SessionTimerCommon.v_MessageHeader_200.allow = Omit
    File: IMS_CC_SessionTimerCommon.ttcn [Line: 166]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\IMS\Common\IMS_CC_SessionTimerCommon.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 167
    text = Parameter: IMS_CC_SessionTimerCommon.v_MessageHeader_200.require = Omit
    File: IMS_CC_SessionTimerCommon.ttcn [Line: 167]

    Parameter: IMS_CC_SessionTimerCommon.v_MessageHeader_200.require = Omit
    File: IMS_CC_SessionTimerCommon.ttcn [Line: 167]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\IMS\Common\IMS_CC_SessionTimerCommon.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 168
    text = Parameter: IMS_CC_SessionTimerCommon.v_MessageHeader_200.supported = Omit
    File: IMS_CC_SessionTimerCommon.ttcn [Line: 168]

    Parameter: IMS_CC_SessionTimerCommon.v_MessageHeader_200.supported = Omit
    File: IMS_CC_SessionTimerCommon.ttcn [Line: 168]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\IMS\Common\IMS_CC_SessionTimerCommon.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 169
    text = Parameter: IMS_CC_SessionTimerCommon.v_MessageHeader_200.sessionExpires = Omit
    File: IMS_CC_SessionTimerCommon.ttcn [Line: 169]

    Parameter: IMS_CC_SessionTimerCommon.v_MessageHeader_200.sessionExpires = Omit
    File: IMS_CC_SessionTimerCommon.ttcn [Line: 169]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\IMS\Common\IMS_CC_SessionTimerCommon.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 170
    text = Parameter: IMS_CC_SessionTimerCommon.v_MessageHeader_200.minSE = Omit
    File: IMS_CC_SessionTimerCommon.ttcn [Line: 170]

    Parameter: IMS_CC_SessionTimerCommon.v_MessageHeader_200.minSE = Omit
    File: IMS_CC_SessionTimerCommon.ttcn [Line: 170]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_Main.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 596
    text = Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 596]

    Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 596]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_Main.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 741
    text = Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 741]

    Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 741]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 801
    text = Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 802
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 803
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 103
    text = Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    recordType = 24
    summary = Step 16 - 19

    Step 16 - 19

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 338
    text = Parameter: IMS_Procedures_Common.v_SigCompParam = Omit
    File: IMS_Procedures_Common.ttcn [Line: 338]

    Parameter: IMS_Procedures_Common.v_SigCompParam = Omit
    File: IMS_Procedures_Common.ttcn [Line: 338]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 867
    text = Parameter: IMS_Component.v_P_CSCF_Address = 'fd29:cc43:7fb9:2:20c:29ff:fe66:b4c7'
    File: IMS_Component.ttcn [Line: 867]

    Parameter: IMS_Component.v_P_CSCF_Address = 'fd29:cc43:7fb9:2:20c:29ff:fe66:b4c7'
    File: IMS_Component.ttcn [Line: 867]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 762
    text = Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 339
    text = Parameter: IMS_Procedures_Common.v_Host = 'fd29:cc43:7fb9:2:20c:29ff:fe66:b4c7'
    File: IMS_Procedures_Common.ttcn [Line: 339]

    Parameter: IMS_Procedures_Common.v_Host = 'fd29:cc43:7fb9:2:20c:29ff:fe66:b4c7'
    File: IMS_Procedures_Common.ttcn [Line: 339]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 763
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 764
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 100
    text = Parameter: IMS_Procedures_Common.v_Port_ps = 5060
    File: IMS_Procedures_Common.ttcn [Line: 100]

    Parameter: IMS_Procedures_Common.v_Port_ps = 5060
    File: IMS_Procedures_Common.ttcn [Line: 100]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 104
    text = Parameter: IMS_Procedures_Common.v_Port_ps = 5062
    File: IMS_Procedures_Common.ttcn [Line: 104]

    Parameter: IMS_Procedures_Common.v_Port_ps = 5062
    File: IMS_Procedures_Common.ttcn [Line: 104]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 340
    text = Parameter: IMS_Procedures_Common.v_Port_ps = 5062
    File: IMS_Procedures_Common.ttcn [Line: 340]

    Parameter: IMS_Procedures_Common.v_Port_ps = 5062
    File: IMS_Procedures_Common.ttcn [Line: 340]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 341
    text = Parameter: IMS_Procedures_Common.v_InternetProtocol = udp
    File: IMS_Procedures_Common.ttcn [Line: 341]

    Parameter: IMS_Procedures_Common.v_InternetProtocol = udp
    File: IMS_Procedures_Common.ttcn [Line: 341]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonFunctions.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 154
    text = Parameter: IMS_CommonFunctions.v_ProtocolString = ''
    File: IMS_CommonFunctions.ttcn [Line: 154]

    Parameter: IMS_CommonFunctions.v_ProtocolString = ''
    File: IMS_CommonFunctions.ttcn [Line: 154]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonFunctions.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 161
    text = Parameter: IMS_CommonFunctions.v_ProtocolString = 'UDP'
    File: IMS_CommonFunctions.ttcn [Line: 161]

    Parameter: IMS_CommonFunctions.v_ProtocolString = 'UDP'
    File: IMS_CommonFunctions.ttcn [Line: 161]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 103
    text = Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 342
    text = Parameter: IMS_Procedures_Common.v_TransportProtocol1 = 'UDP'
    File: IMS_Procedures_Common.ttcn [Line: 342]

    Parameter: IMS_Procedures_Common.v_TransportProtocol1 = 'UDP'
    File: IMS_Procedures_Common.ttcn [Line: 342]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 343
    text = Parameter: IMS_Procedures_Common.v_TransportProtocol2 = 'UDP'
    File: IMS_Procedures_Common.ttcn [Line: 343]

    Parameter: IMS_Procedures_Common.v_TransportProtocol2 = 'UDP'
    File: IMS_Procedures_Common.ttcn [Line: 343]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 344
    text = Parameter: IMS_Procedures_Common.v_IsMCX = False
    File: IMS_Procedures_Common.ttcn [Line: 344]

    Parameter: IMS_Procedures_Common.v_IsMCX = False
    File: IMS_Procedures_Common.ttcn [Line: 344]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 762
    text = Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1656
    text = Parameter: IMS_Component.v_Branch = 'z9hG4bK3200987654'
    File: IMS_Component.ttcn [Line: 1656]

    Parameter: IMS_Component.v_Branch = 'z9hG4bK3200987654'
    File: IMS_Component.ttcn [Line: 1656]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 763
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1657
    text = Parameter: IMS_Component.vc_IMS_Global.ImsInfo.BranchIndex = 28
    File: IMS_Component.ttcn [Line: 1657]

    Parameter: IMS_Component.vc_IMS_Global.ImsInfo.BranchIndex = 28
    File: IMS_Component.ttcn [Line: 1657]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 764
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 114
    text = Parameter: IMS_CommonTemplates.v_GenValue = Omit
    File: IMS_CommonTemplates.ttcn [Line: 114]

    Parameter: IMS_CommonTemplates.v_GenValue = Omit
    File: IMS_CommonTemplates.ttcn [Line: 114]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 722
    text = Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 723
    text = Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 724
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 725
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1656
    text = Parameter: IMS_Component.v_Branch = 'z9hG4bK2009876543'
    File: IMS_Component.ttcn [Line: 1656]

    Parameter: IMS_Component.v_Branch = 'z9hG4bK2009876543'
    File: IMS_Component.ttcn [Line: 1656]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 722
    text = Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1657
    text = Parameter: IMS_Component.vc_IMS_Global.ImsInfo.BranchIndex = 29
    File: IMS_Component.ttcn [Line: 1657]

    Parameter: IMS_Component.vc_IMS_Global.ImsInfo.BranchIndex = 29
    File: IMS_Component.ttcn [Line: 1657]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 723
    text = Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 724
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 725
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 114
    text = Parameter: IMS_CommonTemplates.v_GenValue = Omit
    File: IMS_CommonTemplates.ttcn [Line: 114]

    Parameter: IMS_CommonTemplates.v_GenValue = Omit
    File: IMS_CommonTemplates.ttcn [Line: 114]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 801
    text = Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 802
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 803
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1656
    text = Parameter: IMS_Component.v_Branch = 'z9hG4bK0098765432'
    File: IMS_Component.ttcn [Line: 1656]

    Parameter: IMS_Component.v_Branch = 'z9hG4bK0098765432'
    File: IMS_Component.ttcn [Line: 1656]

    IMS_DATA_RSP
    	RoutingInfo
    		Protocol = udp (0)
    		Security = Omit
    		UE_Address = Omit
    		NW_Address = Omit
    	Response
    		statusLine
    			sipVersion = 'SIP/2.0'
    			statusCode = 200
    			reasonPhrase = 'OK'
    		msgHeader
    			accept = Omit
    			acceptContact = Omit
    			acceptEncoding = Omit
    			acceptLanguage = Omit
    			alertInfo = Omit
    			allow = Omit
    			allowEvents = Omit
    			authenticationInfo = Omit
    			authorization = Omit
    			callId
    				fieldName = CALL_ID_E (7)
    				callid = 'INVITE-0-7dec-11d0-a765-00a0c91e6bf6@FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    			callInfo = Omit
    			contact
    				fieldName = CONTACT_E (9)
    				contactBody
    					contactAddresses
    						ContactAddress
    							addressField
    								nameAddr
    									displayName = Omit
    									addrSpec
    										scheme = 'tel'
    										components
    											tel
    												subscriber = '123;phone-context=test.3gpp.com'
    										urlParameters = Omit
    										headers = Omit
    							contactParams
    								GenericParam
    									id = 'audio'
    									paramValue = Omit
    			contentDisposition = Omit
    			contentEncoding = Omit
    			contentLanguage = Omit
    			contentLength
    				fieldName = CONTENT_LENGTH_E (13)
    				len = 0
    			contentType = Omit
    			cSeq
    				fieldName = CSEQ_E (15)
    				seqNumber = 4712
    				method = 'UPDATE'
    			date = Omit
    			errorInfo = Omit
    			event = Omit
    			expires = Omit
    			featureCaps = Omit
    			fromField
    				fieldName = FROM_E (19)
    				addressField
    					nameAddr
    						displayName = Omit
    						addrSpec
    							scheme = 'sip'
    							components
    								sip
    									userInfo
    										userOrTelephoneSubscriber = '001010123456789'
    										password = Omit
    									hostPort
    										host = 'ims.mnc001.mcc001.3gppnetwork.org'
    										portField = Omit
    							urlParameters = Omit
    							headers = Omit
    				fromParams
    					GenericParam
    						id = 'tag'
    						paramValue
    							tokenOrHost = '1583834582'
    			geolocation = Omit
    			geolocationRouting = Omit
    			historyInfo = Omit
    			infoPackage = Omit
    			inReplyTo = Omit
    			maxForwards = Omit
    			mimeVersion = Omit
    			minExpires = Omit
    			minSE = Omit
    			organization = Omit
    			pAccessNetworkInfo = Omit
    			pAssertedID = Omit
    			pAssertedService = Omit
    			pAssociatedURI = Omit
    			path = Omit
    			pCalledPartyID = Omit
    			pChargingFunctionAddresses = Omit
    			pChargingVector = Omit
    			pEarlyMedia = Omit
    			pMediaAuthorization = Omit
    			pPreferredID = Omit
    			pPreferredService = Omit
    			priority = Omit
    			privacy = Omit
    			proxyAuthenticate = Omit
    			proxyAuthorization = Omit
    			proxyRequire = Omit
    			pVisitedNetworkID = Omit
    			rAck = Omit
    			rSeq = Omit
    			reason = Omit
    			recordRoute
    				fieldName = RECORD_ROUTE_E (29)
    				routeBody
    					RouteBody
    						nameAddr
    							displayName = Omit
    							addrSpec
    								scheme = 'sip'
    								components
    									sip
    										userInfo = Omit
    										hostPort
    											host = 'pcscf.other.com'
    											portField = Omit
    								urlParameters
    									GenericParam
    										id = 'lr'
    										paramValue = Omit
    								headers = Omit
    						rrParam = Omit
    					RouteBody
    						nameAddr
    							displayName = Omit
    							addrSpec
    								scheme = 'sip'
    								components
    									sip
    										userInfo = Omit
    										hostPort
    											host = 'scscf.other.com'
    											portField = Omit
    								urlParameters
    									GenericParam
    										id = 'lr'
    										paramValue = Omit
    								headers = Omit
    						rrParam = Omit
    					RouteBody
    						nameAddr
    							displayName = Omit
    							addrSpec
    								scheme = 'sip'
    								components
    									sip
    										userInfo
    											userOrTelephoneSubscriber = 'orig'
    											password = Omit
    										hostPort
    											host = 'scscf.3gpp.org'
    											portField = Omit
    								urlParameters
    									GenericParam
    										id = 'lr'
    										paramValue = Omit
    								headers = Omit
    						rrParam = Omit
    					RouteBody
    						nameAddr
    							displayName = Omit
    							addrSpec
    								scheme = 'sip'
    								components
    									sip
    										userInfo = Omit
    										hostPort
    											host = 'fd29:cc43:7fb9:2:20c:29ff:fe66:b4c7'
    											portField = 5062
    								urlParameters
    									GenericParam
    										id = 'lr'
    										paramValue = Omit
    								headers = Omit
    						rrParam = Omit
    			recvInfo = Omit
    			requestDisposition = Omit
    			referredBy = Omit
    			referTo = Omit
    			referSub = Omit
    			replaces = Omit
    			replyTo = Omit
    			require = Omit
    			retryAfter = Omit
    			route = Omit
    			securityClient = Omit
    			securityServer = Omit
    			securityVerify = Omit
    			server = Omit
    			serviceRoute = Omit
    			sessionExpires = Omit
    			sessionId = Omit
    			sipETag = Omit
    			sipIfMatch = Omit
    			subject = Omit
    			subscriptionState = Omit
    			supported = Omit
    			timestamp = Omit
    			toField
    				fieldName = TO_E (38)
    				addressField
    					nameAddr
    						displayName = Omit
    						addrSpec
    							scheme = 'sip'
    							components
    								sip
    									userInfo
    										userOrTelephoneSubscriber = 'PeerUE-Public'
    										password = Omit
    									hostPort
    										host = 'stf160.etsi.org'
    										portField = Omit
    							urlParameters = Omit
    							headers = Omit
    				toParams
    					GenericParam
    						id = 'tag'
    						paramValue
    							tokenOrHost = 'abc-INVITE-Fromtag'
    			unsupported = Omit
    			userToUser = Omit
    			userAgent = Omit
    			via
    				fieldName = VIA_E (41)
    				viaBody
    					ViaBody
    						sentProtocol
    							protocolName = 'SIP'
    							protocolVersion = '2.0'
    							transport = 'TCP'
    						sentBy
    							host = '3000::2:6c61:18ff:fe5d:9f1e'
    							portField = 44724
    						viaParams
    							GenericParam
    								id = 'branch'
    								paramValue
    									tokenOrHost = 'z9hG4bK2236085594'
    			warning = Omit
    			wwwAuthenticate = Omit
    			resourcePriority = Omit
    			answerMode = Omit
    			privAnswerMode = Omit
    			targetDialog = Omit
    			pAnswerState = Omit
    			undefinedHeader_List = Omit
    		messageBody = Omit
    		payload = Omit

    Inter-component message: IMS_Server -> IP:IMS_Server

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1657
    text = Parameter: IMS_Component.vc_IMS_Global.ImsInfo.BranchIndex = 30
    File: IMS_Component.ttcn [Line: 1657]

    Parameter: IMS_Component.vc_IMS_Global.ImsInfo.BranchIndex = 30
    File: IMS_Component.ttcn [Line: 1657]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 114
    text = Parameter: IMS_CommonTemplates.v_GenValue = Omit
    File: IMS_CommonTemplates.ttcn [Line: 114]

    Parameter: IMS_CommonTemplates.v_GenValue = Omit
    File: IMS_CommonTemplates.ttcn [Line: 114]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 951
    text = Parameter: IP_PTC_IMS_Handler.v_Data = '01010011010010010101000000101111001100100010111000110000001000000011001000110000001100000010000001001111010010110000110100001010010101100110100101100001001110100010000001010011010010010101000000101111001100100010111000110000001011110101010001000011010100000010000001011011001100110011000000110000001100000011101000111010001100100011101000110110011000110011011000110001001110100011000100111000011001100110011000111010011001100110010100110101011001000011101000111001011001100011000101100101010111010011101000110100001101000011011100110010001101000011101101100010011100100110000101101110011000110110100000111101011110100011100101101000010001110011010001100010010010110011001000110010001100110011011000110000001110000011010100110101001110010011010000001101000010100100011001110010011011110110110100111010001000000011110001110011011010010111000000111010001100000...

    Parameter: IP_PTC_IMS_Handler.v_Data = '01010011010010010101000000101111001100100010111000110000001000000011001000110000001100000010000001001111010010110000110100001010010101100110100101100001001110100010000001010011010010010101000000101111001100100010111000110000001011110101010001000011010100000010000001011011001100110011000000110000001100000011101000111010001100100011101000110110011000110011011000110001001110100011000100111000011001100110011000111010011001100110010100110101011001000011101000111001011001100011000101100101010111010011101000110100001101000011011100110010001101000011101101100010011100100110000101101110011000110110100000111101011110100011100101101000010001110011010001100010010010110011001000110010001100110011011000110000001110000011010100110101001110010011010000001101000010100100011001110010011011110110110100111010001000000011110001110011011010010111000000111010001100000...

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 837
    text = Parameter: IP_PTC_IMS_Handler.v_Protocol = udp
    File: IP_PTC_IMS_Handler.ttcn [Line: 837]

    Parameter: IP_PTC_IMS_Handler.v_Protocol = udp
    File: IP_PTC_IMS_Handler.ttcn [Line: 837]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 847
    text = Parameter: IP_PTC_IMS_Handler.v_TCP_Connection = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 847]

    Parameter: IP_PTC_IMS_Handler.v_TCP_Connection = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 847]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 849
    text = Parameter: IP_PTC_IMS_Handler.v_Data = '5349502F322E3020323030204F4B0D0A5669613A205349502F322E302F544350205B333030303A3A323A366336313A313866663A666535643A396631655D3A34343732343B6272616E63683D7A39684734624B323233363038353539340D0A46726F6D3A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E3B7461673D313538333833343538320D0A546F3A203C7369703A5065657255452D5075626C6963407374663136302E657473692E6F72673E3B7461673D6162632D494E564954452D46726F6D7461670D0A43616C6C2D49443A20494E564954452D302D376465632D313164302D613736352D30306130633931653662663640464432393A434334333A374642393A303030323A303230433A323946463A464536363A423443370D0A435365713A2034373132205550444154450D0A436F6E746163743A203C74656C3A3132333B70686F6E652D636F6E746578743D746573742E336770702E636F6D3E3B617564696F0D0A5265636F72642D526F7574653A203C7369703A70637363662E6F746865722E6...

    Parameter: IP_PTC_IMS_Handler.v_Data = '5349502F322E3020323030204F4B0D0A5669613A205349502F322E302F544350205B333030303A3A323A366336313A313866663A666535643A396631655D3A34343732343B6272616E63683D7A39684734624B323233363038353539340D0A46726F6D3A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E3B7461673D313538333833343538320D0A546F3A203C7369703A5065657255452D5075626C6963407374663136302E657473692E6F72673E3B7461673D6162632D494E564954452D46726F6D7461670D0A43616C6C2D49443A20494E564954452D302D376465632D313164302D613736352D30306130633931653662663640464432393A434334333A374642393A303030323A303230433A323946463A464536363A423443370D0A435365713A2034373132205550444154450D0A436F6E746163743A203C74656C3A3132333B70686F6E652D636F6E746578743D746573742E336770702E636F6D3E3B617564696F0D0A5265636F72642D526F7574653A203C7369703A70637363662E6F746865722E6...

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1656
    text = Parameter: IMS_Component.v_Branch = 'z9hG4bK0987654300'
    File: IMS_Component.ttcn [Line: 1656]

    Parameter: IMS_Component.v_Branch = 'z9hG4bK0987654300'
    File: IMS_Component.ttcn [Line: 1656]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1657
    text = Parameter: IMS_Component.vc_IMS_Global.ImsInfo.BranchIndex = 31
    File: IMS_Component.ttcn [Line: 1657]

    Parameter: IMS_Component.vc_IMS_Global.ImsInfo.BranchIndex = 31
    File: IMS_Component.ttcn [Line: 1657]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 114
    text = Parameter: IMS_CommonTemplates.v_GenValue = Omit
    File: IMS_CommonTemplates.ttcn [Line: 114]

    Parameter: IMS_CommonTemplates.v_GenValue = Omit
    File: IMS_CommonTemplates.ttcn [Line: 114]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 862
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContextEnum = protectedContext1
    File: IP_PTC_IMS_Handler.ttcn [Line: 862]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContextEnum = protectedContext1
    File: IP_PTC_IMS_Handler.ttcn [Line: 862]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1656
    text = Parameter: IMS_Component.v_Branch = 'z9hG4bK9876543000'
    File: IMS_Component.ttcn [Line: 1656]

    Parameter: IMS_Component.v_Branch = 'z9hG4bK9876543000'
    File: IMS_Component.ttcn [Line: 1656]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1657
    text = Parameter: IMS_Component.vc_IMS_Global.ImsInfo.BranchIndex = 32
    File: IMS_Component.ttcn [Line: 1657]

    Parameter: IMS_Component.vc_IMS_Global.ImsInfo.BranchIndex = 32
    File: IMS_Component.ttcn [Line: 1657]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 114
    text = Parameter: IMS_CommonTemplates.v_GenValue = Omit
    File: IMS_CommonTemplates.ttcn [Line: 114]

    Parameter: IMS_CommonTemplates.v_GenValue = Omit
    File: IMS_CommonTemplates.ttcn [Line: 114]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 764
    text = Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 764]

    Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 764]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 777
    text = Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 777]

    Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 777]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 872
    text = Parameter: IP_PTC_IMS_Handler.v_IsUnprotected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 872]

    Parameter: IP_PTC_IMS_Handler.v_IsUnprotected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 872]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 560
    text = Parameter: IP_PTC_IMS_Handler.v_LocalRemotePort.Local = 5061
    File: IP_PTC_IMS_Handler.ttcn [Line: 560]

    Parameter: IP_PTC_IMS_Handler.v_LocalRemotePort.Local = 5061
    File: IP_PTC_IMS_Handler.ttcn [Line: 560]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 561
    text = Parameter: IP_PTC_IMS_Handler.v_LocalRemotePort.Remote = 44724
    File: IP_PTC_IMS_Handler.ttcn [Line: 561]

    Parameter: IP_PTC_IMS_Handler.v_LocalRemotePort.Remote = 44724
    File: IP_PTC_IMS_Handler.ttcn [Line: 561]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 875
    text = Parameter: IP_PTC_IMS_Handler.v_LocalPort = 5061
    File: IP_PTC_IMS_Handler.ttcn [Line: 875]

    Parameter: IP_PTC_IMS_Handler.v_LocalPort = 5061
    File: IP_PTC_IMS_Handler.ttcn [Line: 875]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 876
    text = Parameter: IP_PTC_IMS_Handler.v_RemotePort = 44724
    File: IP_PTC_IMS_Handler.ttcn [Line: 876]

    Parameter: IP_PTC_IMS_Handler.v_RemotePort = 44724
    File: IP_PTC_IMS_Handler.ttcn [Line: 876]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 658
    text = Parameter: IMS_Procedures_Common.v_ToTag = '1583834582'
    File: IMS_Procedures_Common.ttcn [Line: 658]

    Parameter: IMS_Procedures_Common.v_ToTag = '1583834582'
    File: IMS_Procedures_Common.ttcn [Line: 658]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 764
    text = Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 764]

    Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 764]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 777
    text = Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 777]

    Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 777]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1263
    text = Parameter: IMS_Component.v_SipUrl = Omit
    File: IMS_Component.ttcn [Line: 1263]

    Parameter: IMS_Component.v_SipUrl = Omit
    File: IMS_Component.ttcn [Line: 1263]

    IP_SOCKET_REQ
    	DATA
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 5061
    			Remote
    				IpAddr
    					V6
    						Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    						ScopeId = Omit
    				Port = 44724
    		Req
    			UDP
    				SendTo
    					Buffer = '5349502F322E3020323030204F4B0D0A5669613A205349502F322E302F544350205B333030303A3A323A366336313A313866663A666535643A396631655D3A34343732343B6272616E63683D7A39684734624B323233363038353539340D0A46726F6D3A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E3B7461673D313538333833343538320D0A546F3A203C7369703A5065657255452D5075626C6963407374663136302E657473692E6F72673E3B7461673D6162632D494E564954452D46726F6D7461670D0A43616C6C2D49443A20494E564954452D302D376465632D313164302D613736352D30306130633931653662663640464432393A434334333A374642393A303030323A303230433A323946463A464536363A423443370D0A435365713A2034373132205550444154450D0A436F6E746163743A203C74656C3A3132333B70686F6E652D636F6E746578743D746573742E336770702E636F6D3E3B617564696F0D0A5265636F72642D526F7574653A203C7369703A70637363662E6F746865722E636F6D3B6C723E2C3C7369703A73637363662E6F746865722E636F6D3B6C723E2C3C7369703A6F7269674073637363662E336770702E6F72673B6C723E2C3C7369703A5B666432393A636334333A376662393A323A3230633A323966663A666536363A623463375D3A353036323B6C723E0D0A436F6E74656E742D4C656E6774683A20300D0A0D0A'O

    Inter-component message: IP_SOCK_DATA -> IPMUX:IP_SOCK_DATA

    SipMessage
    	Message Header = SIP/2.0 200 OK
    Via: SIP/2.0/TCP [3000::2:6c61:18ff:fe5d:9f1e]:44724;branch=z9hG4bK2236085594
    From: ;tag=1583834582
    To: ;tag=abc-INVITE-Fromtag
    Call-ID: INVITE-0-7dec-11d0-a765-00a0c91e6bf6@FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7
    CSeq: 4712 UPDATE
    Contact: ;audio
    Record-Route: ,,,
    Content-Length: 0

    Status:SIP/2.0 200 OK

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 114
    text = Parameter: IMS_CommonTemplates.v_GenValue = Omit
    File: IMS_CommonTemplates.ttcn [Line: 114]

    Parameter: IMS_CommonTemplates.v_GenValue = Omit
    File: IMS_CommonTemplates.ttcn [Line: 114]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 764
    text = Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 764]

    Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 764]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 777
    text = Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 777]

    Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 777]

    IP_SOCKET_REQ
    	DATA
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 5061
    			Remote
    				IpAddr
    					V6
    						Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    						ScopeId = Omit
    				Port = 44724
    		Req
    			UDP
    				SendTo
    					Buffer = '5349502F322E3020323030204F4B0D0A5669613A205349502F322E302F544350205B333030303A3A323A366336313A313866663A666535643A396631655D3A34343732343B6272616E63683D7A39684734624B323233363038353539340D0A46726F6D3A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E3B7461673D313538333833343538320D0A546F3A203C7369703A5065657255452D5075626C6963407374663136302E657473692E6F72673E3B7461673D6162632D494E564954452D46726F6D7461670D0A43616C6C2D49443A20494E564954452D302D376465632D313164302D613736352D30306130633931653662663640464432393A434334333A374642393A303030323A303230433A323946463A464536363A423443370D0A435365713A2034373132205550444154450D0A436F6E746163743A203C74656C3A3132333B70686F6E652D636F6E746578743D746573742E336770702E636F6D3E3B617564696F0D0A5265636F72642D526F7574653A203C7369703A70637363662E6F746865722E636F6D3B6C723E2C3C7369703A73637363662E6F746865722E636F6D3B6C723E2C3C7369703A6F7269674073637363662E336770702E6F72673B6C723E2C3C7369703A5B666432393A636334333A376662393A323A3230633A323966663A666536363A623463375D3A353036323B6C723E0D0A436F6E74656E742D4C656E6774683A20300D0A0D0A'O

    Sent from port: IPMUX:IP_SOCK

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_Main.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 596
    text = Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 596]

    Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 596]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_Main.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 741
    text = Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 741]

    Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 741]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 645
    text = Parameter: IMS_Procedures_Common.v_FromTag = 'abc-INVITE-Fromtag'
    File: IMS_Procedures_Common.ttcn [Line: 645]

    Parameter: IMS_Procedures_Common.v_FromTag = 'abc-INVITE-Fromtag'
    File: IMS_Procedures_Common.ttcn [Line: 645]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 764
    text = Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 764]

    Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 764]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 777
    text = Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 777]

    Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 777]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1263
    text = Parameter: IMS_Component.v_SipUrl = Omit
    File: IMS_Component.ttcn [Line: 1263]

    Parameter: IMS_Component.v_SipUrl = Omit
    File: IMS_Component.ttcn [Line: 1263]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 801
    text = Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 802
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 114
    text = Parameter: IMS_CommonTemplates.v_GenValue = Omit
    File: IMS_CommonTemplates.ttcn [Line: 114]

    Parameter: IMS_CommonTemplates.v_GenValue = Omit
    File: IMS_CommonTemplates.ttcn [Line: 114]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 764
    text = Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 764]

    Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 764]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 777
    text = Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 777]

    Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 777]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 803
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 103
    text = Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 764
    text = Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 764]

    Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 764]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 777
    text = Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 777]

    Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 777]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 762
    text = Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 763
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 764
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1560
    text = Parameter: IMS_Component.v_CseqValue = 4714
    File: IMS_Component.ttcn [Line: 1560]

    Parameter: IMS_Component.v_CseqValue = 4714
    File: IMS_Component.ttcn [Line: 1560]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1576
    text = Parameter: IMS_Component.v_Cseq = 4714
    File: IMS_Component.ttcn [Line: 1576]

    Parameter: IMS_Component.v_Cseq = 4714
    File: IMS_Component.ttcn [Line: 1576]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1615
    text = Parameter: IMS_Component.v_CseqValue = 4715
    File: IMS_Component.ttcn [Line: 1615]

    Parameter: IMS_Component.v_CseqValue = 4715
    File: IMS_Component.ttcn [Line: 1615]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 764
    text = Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 764]

    Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 764]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 777
    text = Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 777]

    Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 777]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 103
    text = Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1599
    text = Parameter: IMS_Component.v_Dialog.LocalCseq = 4715
    File: IMS_Component.ttcn [Line: 1599]

    Parameter: IMS_Component.v_Dialog.LocalCseq = 4715
    File: IMS_Component.ttcn [Line: 1599]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 764
    text = Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 764]

    Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 764]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 790
    text = Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 790]

    Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 790]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 762
    text = Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 763
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 764
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 722
    text = Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 723
    text = Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 724
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 725
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_CallControlCommon.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 693
    text = Parameter: IMS_Procedures_CallControlCommon.v_CSeqValue = 4715
    File: IMS_Procedures_CallControlCommon.ttcn [Line: 693]

    Parameter: IMS_Procedures_CallControlCommon.v_CSeqValue = 4715
    File: IMS_Procedures_CallControlCommon.ttcn [Line: 693]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 372
    text = Parameter: IMS_Procedures_Common.v_IsMCX = False
    File: IMS_Procedures_Common.ttcn [Line: 372]

    Parameter: IMS_Procedures_Common.v_IsMCX = False
    File: IMS_Procedures_Common.ttcn [Line: 372]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 378
    text = Parameter: IMS_Procedures_Common.v_Value = 67
    File: IMS_Procedures_Common.ttcn [Line: 378]

    Parameter: IMS_Procedures_Common.v_Value = 67
    File: IMS_Procedures_Common.ttcn [Line: 378]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_CallControlCommon.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 701
    text = Parameter: IMS_Procedures_CallControlCommon.v_MessageHeader_Bye.contentType = Omit
    File: IMS_Procedures_CallControlCommon.ttcn [Line: 701]

    Parameter: IMS_Procedures_CallControlCommon.v_MessageHeader_Bye.contentType = Omit
    File: IMS_Procedures_CallControlCommon.ttcn [Line: 701]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 722
    text = Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 723
    text = Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 724
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 725
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 801
    text = Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 802
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 803
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1074
    text = Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 1074]

    Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 1074]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1075
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 1075]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 1075]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_SIP_Templates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1562
    text = Parameter: IMS_SIP_Templates.i = 0
    File: IMS_SIP_Templates.ttcn [Line: 1562]

    Parameter: IMS_SIP_Templates.i = 0
    File: IMS_SIP_Templates.ttcn [Line: 1562]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_SIP_Templates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1563
    text = Parameter: IMS_SIP_Templates.v_ViaRespone.viaBody[i].sentBy.host = AnyValue
    File: IMS_SIP_Templates.ttcn [Line: 1563]

    Parameter: IMS_SIP_Templates.v_ViaRespone.viaBody[i].sentBy.host = AnyValue
    File: IMS_SIP_Templates.ttcn [Line: 1563]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_SIP_Templates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1562
    text = Parameter: IMS_SIP_Templates.i = 1
    File: IMS_SIP_Templates.ttcn [Line: 1562]

    Parameter: IMS_SIP_Templates.i = 1
    File: IMS_SIP_Templates.ttcn [Line: 1562]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_SIP_Templates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1563
    text = Parameter: IMS_SIP_Templates.v_ViaRespone.viaBody[i].sentBy.host = AnyValue
    File: IMS_SIP_Templates.ttcn [Line: 1563]

    Parameter: IMS_SIP_Templates.v_ViaRespone.viaBody[i].sentBy.host = AnyValue
    File: IMS_SIP_Templates.ttcn [Line: 1563]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_SIP_Templates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1562
    text = Parameter: IMS_SIP_Templates.i = 2
    File: IMS_SIP_Templates.ttcn [Line: 1562]

    Parameter: IMS_SIP_Templates.i = 2
    File: IMS_SIP_Templates.ttcn [Line: 1562]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_SIP_Templates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1563
    text = Parameter: IMS_SIP_Templates.v_ViaRespone.viaBody[i].sentBy.host = AnyValue
    File: IMS_SIP_Templates.ttcn [Line: 1563]

    Parameter: IMS_SIP_Templates.v_ViaRespone.viaBody[i].sentBy.host = AnyValue
    File: IMS_SIP_Templates.ttcn [Line: 1563]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_SIP_Templates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1562
    text = Parameter: IMS_SIP_Templates.i = 3
    File: IMS_SIP_Templates.ttcn [Line: 1562]

    Parameter: IMS_SIP_Templates.i = 3
    File: IMS_SIP_Templates.ttcn [Line: 1562]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_SIP_Templates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1563
    text = Parameter: IMS_SIP_Templates.v_ViaRespone.viaBody[i].sentBy.host = AnyValue
    File: IMS_SIP_Templates.ttcn [Line: 1563]

    Parameter: IMS_SIP_Templates.v_ViaRespone.viaBody[i].sentBy.host = AnyValue
    File: IMS_SIP_Templates.ttcn [Line: 1563]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_SIP_Templates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1562
    text = Parameter: IMS_SIP_Templates.i = 4
    File: IMS_SIP_Templates.ttcn [Line: 1562]

    Parameter: IMS_SIP_Templates.i = 4
    File: IMS_SIP_Templates.ttcn [Line: 1562]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1076
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1076]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1076]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_SIP_Templates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1563
    text = Parameter: IMS_SIP_Templates.v_ViaRespone.viaBody[i].sentBy.host = AnyValue
    File: IMS_SIP_Templates.ttcn [Line: 1563]

    Parameter: IMS_SIP_Templates.v_ViaRespone.viaBody[i].sentBy.host = AnyValue
    File: IMS_SIP_Templates.ttcn [Line: 1563]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_SIP_Templates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1562
    text = Parameter: IMS_SIP_Templates.i = 5
    File: IMS_SIP_Templates.ttcn [Line: 1562]

    Parameter: IMS_SIP_Templates.i = 5
    File: IMS_SIP_Templates.ttcn [Line: 1562]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 103
    text = Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 274
    text = Parameter: IP_PTC_IMS_Handler.v_TcpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 274]

    Parameter: IP_PTC_IMS_Handler.v_TcpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 274]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 103
    text = Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 281
    text = Parameter: IMS_CommonTemplates.i = 0
    File: IMS_CommonTemplates.ttcn [Line: 281]

    Parameter: IMS_CommonTemplates.i = 0
    File: IMS_CommonTemplates.ttcn [Line: 281]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 281
    text = Parameter: IMS_CommonTemplates.i = 1
    File: IMS_CommonTemplates.ttcn [Line: 281]

    Parameter: IMS_CommonTemplates.i = 1
    File: IMS_CommonTemplates.ttcn [Line: 281]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 216
    text = Parameter: IMS_CommonTemplates.v_NoOfParams = 1
    File: IMS_CommonTemplates.ttcn [Line: 216]

    Parameter: IMS_CommonTemplates.v_NoOfParams = 1
    File: IMS_CommonTemplates.ttcn [Line: 216]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 274
    text = Parameter: IP_PTC_IMS_Handler.v_TcpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 274]

    Parameter: IP_PTC_IMS_Handler.v_TcpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 274]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 217
    text = Parameter: IMS_CommonTemplates.v_RequestedParamId = 'tag'
    File: IMS_CommonTemplates.ttcn [Line: 217]

    Parameter: IMS_CommonTemplates.v_RequestedParamId = 'tag'
    File: IMS_CommonTemplates.ttcn [Line: 217]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 221
    text = Parameter: IMS_CommonTemplates.i = 0
    File: IMS_CommonTemplates.ttcn [Line: 221]

    Parameter: IMS_CommonTemplates.i = 0
    File: IMS_CommonTemplates.ttcn [Line: 221]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 222
    text = Parameter: IMS_CommonTemplates.v_ParamId = 'tag'
    File: IMS_CommonTemplates.ttcn [Line: 222]

    Parameter: IMS_CommonTemplates.v_ParamId = 'tag'
    File: IMS_CommonTemplates.ttcn [Line: 222]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 240
    text = Parameter: IMS_CommonTemplates.i = 0
    File: IMS_CommonTemplates.ttcn [Line: 240]

    Parameter: IMS_CommonTemplates.i = 0
    File: IMS_CommonTemplates.ttcn [Line: 240]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 247
    text = Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 247]

    Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 247]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 248
    text = Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 248]

    Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 248]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 247
    text = Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 247]

    Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 247]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 248
    text = Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 248]

    Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 248]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 215
    text = Parameter: IMS_Procedures_Common.v_FromTagFromRequest = 'abc-INVITE-Fromtag'
    File: IMS_Procedures_Common.ttcn [Line: 215]

    Parameter: IMS_Procedures_Common.v_FromTagFromRequest = 'abc-INVITE-Fromtag'
    File: IMS_Procedures_Common.ttcn [Line: 215]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1074
    text = Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1074]

    Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1074]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1075
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1075]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1075]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1076
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1076]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1076]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 281
    text = Parameter: IMS_CommonTemplates.i = 0
    File: IMS_CommonTemplates.ttcn [Line: 281]

    Parameter: IMS_CommonTemplates.i = 0
    File: IMS_CommonTemplates.ttcn [Line: 281]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 281
    text = Parameter: IMS_CommonTemplates.i = 1
    File: IMS_CommonTemplates.ttcn [Line: 281]

    Parameter: IMS_CommonTemplates.i = 1
    File: IMS_CommonTemplates.ttcn [Line: 281]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 216
    text = Parameter: IMS_CommonTemplates.v_NoOfParams = 1
    File: IMS_CommonTemplates.ttcn [Line: 216]

    Parameter: IMS_CommonTemplates.v_NoOfParams = 1
    File: IMS_CommonTemplates.ttcn [Line: 216]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 217
    text = Parameter: IMS_CommonTemplates.v_RequestedParamId = 'tag'
    File: IMS_CommonTemplates.ttcn [Line: 217]

    Parameter: IMS_CommonTemplates.v_RequestedParamId = 'tag'
    File: IMS_CommonTemplates.ttcn [Line: 217]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 221
    text = Parameter: IMS_CommonTemplates.i = 0
    File: IMS_CommonTemplates.ttcn [Line: 221]

    Parameter: IMS_CommonTemplates.i = 0
    File: IMS_CommonTemplates.ttcn [Line: 221]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 222
    text = Parameter: IMS_CommonTemplates.v_ParamId = 'tag'
    File: IMS_CommonTemplates.ttcn [Line: 222]

    Parameter: IMS_CommonTemplates.v_ParamId = 'tag'
    File: IMS_CommonTemplates.ttcn [Line: 222]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_CommonTemplates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 240
    text = Parameter: IMS_CommonTemplates.i = 0
    File: IMS_CommonTemplates.ttcn [Line: 240]

    Parameter: IMS_CommonTemplates.i = 0
    File: IMS_CommonTemplates.ttcn [Line: 240]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_SIP_Templates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1649
    text = Parameter: IMS_SIP_Templates.v_ToTag = Omit
    File: IMS_SIP_Templates.ttcn [Line: 1649]

    Parameter: IMS_SIP_Templates.v_ToTag = Omit
    File: IMS_SIP_Templates.ttcn [Line: 1649]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_SIP_Templates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1652
    text = Parameter: IMS_SIP_Templates.v_ToTag = '1583834582'
    File: IMS_SIP_Templates.ttcn [Line: 1652]

    Parameter: IMS_SIP_Templates.v_ToTag = '1583834582'
    File: IMS_SIP_Templates.ttcn [Line: 1652]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 191
    text = Parameter: IMS_Procedures_Common.v_ToTagFromRequest = '1583834582'
    File: IMS_Procedures_Common.ttcn [Line: 191]

    Parameter: IMS_Procedures_Common.v_ToTagFromRequest = '1583834582'
    File: IMS_Procedures_Common.ttcn [Line: 191]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_SIP_Templates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 743
    text = Parameter: IMS_SIP_Templates.v_RanString = AnyValue
    File: IMS_SIP_Templates.ttcn [Line: 743]

    Parameter: IMS_SIP_Templates.v_RanString = AnyValue
    File: IMS_SIP_Templates.ttcn [Line: 743]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_SIP_Templates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 747
    text = Parameter: IMS_SIP_Templates.v_RAN_Type = NR
    File: IMS_SIP_Templates.ttcn [Line: 747]

    Parameter: IMS_SIP_Templates.v_RAN_Type = NR
    File: IMS_SIP_Templates.ttcn [Line: 747]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_SIP_Templates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 755
    text = Parameter: IMS_SIP_Templates.v_RanString = '3GPP-NR', '3GPP-NR-FDD', '3GPP-NR-TDD'
    File: IMS_SIP_Templates.ttcn [Line: 755]

    Parameter: IMS_SIP_Templates.v_RanString = '3GPP-NR', '3GPP-NR-FDD', '3GPP-NR-TDD'
    File: IMS_SIP_Templates.ttcn [Line: 755]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_SIP_Templates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 772
    text = Parameter: IMS_SIP_Templates.v_ParamList = AnyOrOmit
    File: IMS_SIP_Templates.ttcn [Line: 772]

    Parameter: IMS_SIP_Templates.v_ParamList = AnyOrOmit
    File: IMS_SIP_Templates.ttcn [Line: 772]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_SIP_Templates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 776
    text = Parameter: IMS_SIP_Templates.v_RAN_Type = NR
    File: IMS_SIP_Templates.ttcn [Line: 776]

    Parameter: IMS_SIP_Templates.v_RAN_Type = NR
    File: IMS_SIP_Templates.ttcn [Line: 776]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 765
    text = Parameter: IMS_Procedures_Common.v_A2A4 = False
    File: IMS_Procedures_Common.ttcn [Line: 765]

    Parameter: IMS_Procedures_Common.v_A2A4 = False
    File: IMS_Procedures_Common.ttcn [Line: 765]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 766
    text = Parameter: IMS_Procedures_Common.v_A8 = True
    File: IMS_Procedures_Common.ttcn [Line: 766]

    Parameter: IMS_Procedures_Common.v_A8 = True
    File: IMS_Procedures_Common.ttcn [Line: 766]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 767
    text = Parameter: IMS_Procedures_Common.v_A20 = False
    File: IMS_Procedures_Common.ttcn [Line: 767]

    Parameter: IMS_Procedures_Common.v_A20 = False
    File: IMS_Procedures_Common.ttcn [Line: 767]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 768
    text = Parameter: IMS_Procedures_Common.v_A18 = False
    File: IMS_Procedures_Common.ttcn [Line: 768]

    Parameter: IMS_Procedures_Common.v_A18 = False
    File: IMS_Procedures_Common.ttcn [Line: 768]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 769
    text = Parameter: IMS_Procedures_Common.v_Method = 'BYE'
    File: IMS_Procedures_Common.ttcn [Line: 769]

    Parameter: IMS_Procedures_Common.v_Method = 'BYE'
    File: IMS_Procedures_Common.ttcn [Line: 769]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 117
    text = Parameter: IMS_Procedures_Common.v_Port_us = 5060
    File: IMS_Procedures_Common.ttcn [Line: 117]

    Parameter: IMS_Procedures_Common.v_Port_us = 5060
    File: IMS_Procedures_Common.ttcn [Line: 117]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 121
    text = Parameter: IMS_Procedures_Common.v_Port_us = 44724
    File: IMS_Procedures_Common.ttcn [Line: 121]

    Parameter: IMS_Procedures_Common.v_Port_us = 44724
    File: IMS_Procedures_Common.ttcn [Line: 121]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 770
    text = Parameter: IMS_Procedures_Common.v_Port_us = 44724
    File: IMS_Procedures_Common.ttcn [Line: 770]

    Parameter: IMS_Procedures_Common.v_Port_us = 44724
    File: IMS_Procedures_Common.ttcn [Line: 770]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_SIP_Templates.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1364
    text = Parameter: IMS_SIP_Templates.v_Port = 44724
    File: IMS_SIP_Templates.ttcn [Line: 1364]

    Parameter: IMS_SIP_Templates.v_Port = 44724
    File: IMS_SIP_Templates.ttcn [Line: 1364]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 819
    text = Parameter: IMS_Procedures_Common.v_MessageHeader_Response.contentType = Omit
    File: IMS_Procedures_Common.ttcn [Line: 819]

    Parameter: IMS_Procedures_Common.v_MessageHeader_Response.contentType = Omit
    File: IMS_Procedures_Common.ttcn [Line: 819]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_CallControlCommon.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1039
    text = Parameter: IMS_Procedures_CallControlCommon.v_Protocol = udp
    File: IMS_Procedures_CallControlCommon.ttcn [Line: 1039]

    Parameter: IMS_Procedures_CallControlCommon.v_Protocol = udp
    File: IMS_Procedures_CallControlCommon.ttcn [Line: 1039]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_Main.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 596
    text = Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 596]

    Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 596]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_Main.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 741
    text = Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 741]

    Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 741]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 801
    text = Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 802
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 803
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 103
    text = Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 762
    text = Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 763
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 764
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 103
    text = Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 762
    text = Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 763
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 764
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 722
    text = Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 723
    text = Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 724
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 725
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 722
    text = Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 723
    text = Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 724
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 725
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 801
    text = Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 802
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 803
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    IMS_DATA_REQ
    	RoutingInfo
    		Protocol = udp (0)
    		Security = Omit
    		UE_Address = Omit
    		NW_Address = Omit
    	Request
    		Bye
    			requestLine
    				method = BYE_E (1)
    				requestUri
    					scheme = 'sip'
    					components
    						sip
    							userInfo
    								userOrTelephoneSubscriber = '7d50dd18-5ee3-4eaf-a145-d31d84987cb9'
    								password = Omit
    							hostPort
    								host = '3000::2:6c61:18ff:fe5d:9f1e'
    								portField = 44724
    					urlParameters = Omit
    					headers = Omit
    				sipVersion = 'SIP/2.0'
    			msgHeader
    				accept = Omit
    				acceptContact = Omit
    				acceptEncoding = Omit
    				acceptLanguage = Omit
    				alertInfo = Omit
    				allow = Omit
    				allowEvents = Omit
    				authenticationInfo = Omit
    				authorization = Omit
    				callId
    					fieldName = CALL_ID_E (7)
    					callid = 'INVITE-0-7dec-11d0-a765-00a0c91e6bf6@FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    				callInfo = Omit
    				contact = Omit
    				contentDisposition = Omit
    				contentEncoding = Omit
    				contentLanguage = Omit
    				contentLength
    					fieldName = CONTENT_LENGTH_E (13)
    					len = 0
    				contentType = Omit
    				cSeq
    					fieldName = CSEQ_E (15)
    					seqNumber = 4715
    					method = 'BYE'
    				date = Omit
    				errorInfo = Omit
    				event = Omit
    				expires = Omit
    				featureCaps = Omit
    				fromField
    					fieldName = FROM_E (19)
    					addressField
    						nameAddr
    							displayName = Omit
    							addrSpec
    								scheme = 'sip'
    								components
    									sip
    										userInfo
    											userOrTelephoneSubscriber = 'PeerUE-Public'
    											password = Omit
    										hostPort
    											host = 'stf160.etsi.org'
    											portField = Omit
    								urlParameters = Omit
    								headers = Omit
    					fromParams
    						GenericParam
    							id = 'tag'
    							paramValue
    								tokenOrHost = 'abc-INVITE-Fromtag'
    				geolocation = Omit
    				geolocationRouting = Omit
    				historyInfo = Omit
    				infoPackage = Omit
    				inReplyTo = Omit
    				maxForwards
    					fieldName = MAX_FORWARDS_E (21)
    					forwards = 67
    				mimeVersion = Omit
    				minExpires = Omit
    				minSE = Omit
    				organization = Omit
    				pAccessNetworkInfo = Omit
    				pAssertedID = Omit
    				pAssertedService = Omit
    				pAssociatedURI = Omit
    				path = Omit
    				pCalledPartyID = Omit
    				pChargingFunctionAddresses = Omit
    				pChargingVector = Omit
    				pEarlyMedia = Omit
    				pMediaAuthorization = Omit
    				pPreferredID = Omit
    				pPreferredService = Omit
    				priority = Omit
    				privacy = Omit
    				proxyAuthenticate = Omit
    				proxyAuthorization = Omit
    				proxyRequire = Omit
    				pVisitedNetworkID = Omit
    				rAck = Omit
    				rSeq = Omit
    				reason = Omit
    				recordRoute = Omit
    				recvInfo = Omit
    				requestDisposition = Omit
    				referredBy = Omit
    				referTo = Omit
    				referSub = Omit
    				replaces = Omit
    				replyTo = Omit
    				require = Omit
    				retryAfter = Omit
    				route = Omit
    				securityClient = Omit
    				securityServer = Omit
    				securityVerify = Omit
    				server = Omit
    				serviceRoute = Omit
    				sessionExpires = Omit
    				sessionId = Omit
    				sipETag = Omit
    				sipIfMatch = Omit
    				subject = Omit
    				subscriptionState = Omit
    				supported = Omit
    				timestamp = Omit
    				toField
    					fieldName = TO_E (38)
    					addressField
    						nameAddr
    							displayName = Omit
    							addrSpec
    								scheme = 'sip'
    								components
    									sip
    										userInfo
    											userOrTelephoneSubscriber = '001010123456789'
    											password = Omit
    										hostPort
    											host = 'ims.mnc001.mcc001.3gppnetwork.org'
    											portField = Omit
    								urlParameters = Omit
    								headers = Omit
    					toParams
    						GenericParam
    							id = 'tag'
    							paramValue
    								tokenOrHost = '1583834582'
    				unsupported = Omit
    				userToUser = Omit
    				userAgent = Omit
    				via
    					fieldName = VIA_E (41)
    					viaBody
    						ViaBody
    							sentProtocol
    								protocolName = 'SIP'
    								protocolVersion = '2.0'
    								transport = 'UDP'
    							sentBy
    								host = 'fd29:cc43:7fb9:2:20c:29ff:fe66:b4c7'
    								portField = 5062
    							viaParams
    								GenericParam
    									id = 'branch'
    									paramValue
    										tokenOrHost = 'z9hG4bK3200987654'
    						ViaBody
    							sentProtocol
    								protocolName = 'SIP'
    								protocolVersion = '2.0'
    								transport = 'UDP'
    							sentBy
    								host = 'scscf1.3gpp.org'
    								portField = Omit
    							viaParams
    								GenericParam
    									id = 'branch'
    									paramValue
    										tokenOrHost = 'z9hG4bK2009876543'
    						ViaBody
    							sentProtocol
    								protocolName = 'SIP'
    								protocolVersion = '2.0'
    								transport = 'UDP'
    							sentBy
    								host = 'scscf2.3gpp.org'
    								portField = Omit
    							viaParams
    								GenericParam
    									id = 'branch'
    									paramValue
    										tokenOrHost = 'z9hG4bK0098765432'
    						ViaBody
    							sentProtocol
    								protocolName = 'SIP'
    								protocolVersion = '2.0'
    								transport = 'UDP'
    							sentBy
    								host = 'pcscf2.3gpp.org'
    								portField = Omit
    							viaParams
    								GenericParam
    									id = 'branch'
    									paramValue
    										tokenOrHost = 'z9hG4bK0987654300'
    						ViaBody
    							sentProtocol
    								protocolName = 'SIP'
    								protocolVersion = '2.0'
    								transport = 'UDP'
    							sentBy
    								host = 'stf160.etsi.org'
    								portField = 6543
    							viaParams
    								GenericParam
    									id = 'branch'
    									paramValue
    										tokenOrHost = 'z9hG4bK9876543000'
    				warning = Omit
    				wwwAuthenticate = Omit
    				resourcePriority = Omit
    				answerMode = Omit
    				privAnswerMode = Omit
    				targetDialog = Omit
    				pAnswerState = Omit
    				undefinedHeader_List = Omit
    			messageBody = Omit
    			payload = Omit

    Inter-component message: IMS_Client -> IP:IMS_Client

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 956
    text = Parameter: IP_PTC_IMS_Handler.v_Data = '01000010010110010100010100100000011100110110100101110000001110100011011101100100001101010011000001100100011001000011000100111000001011010011010101100101011001010011001100101101001101000110010101100001011001100010110101100001001100010011010000110101001011010110010000110011001100010110010000111000001101000011100100111000001101110110001101100010001110010100000001011011001100110011000000110000001100000011101000111010001100100011101000110110011000110011011000110001001110100011000100111000011001100110011000111010011001100110010100110101011001000011101000111001011001100011000101100101010111010011101000110100001101000011011100110010001101000010000001010011010010010101000000101111001100100010111000110000000011010000101001010110011010010110000100111010001000000101001101001001010100000010111100110010001011100011000000101111010101010100010001010000001000000...

    Parameter: IP_PTC_IMS_Handler.v_Data = '01000010010110010100010100100000011100110110100101110000001110100011011101100100001101010011000001100100011001000011000100111000001011010011010101100101011001010011001100101101001101000110010101100001011001100010110101100001001100010011010000110101001011010110010000110011001100010110010000111000001101000011100100111000001101110110001101100010001110010100000001011011001100110011000000110000001100000011101000111010001100100011101000110110011000110011011000110001001110100011000100111000011001100110011000111010011001100110010100110101011001000011101000111001011001100011000101100101010111010011101000110100001101000011011100110010001101000010000001010011010010010101000000101111001100100010111000110000000011010000101001010110011010010110000100111010001000000101001101001001010100000010111100110010001011100011000000101111010101010100010001010000001000000...

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 837
    text = Parameter: IP_PTC_IMS_Handler.v_Protocol = udp
    File: IP_PTC_IMS_Handler.ttcn [Line: 837]

    Parameter: IP_PTC_IMS_Handler.v_Protocol = udp
    File: IP_PTC_IMS_Handler.ttcn [Line: 837]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 847
    text = Parameter: IP_PTC_IMS_Handler.v_TCP_Connection = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 847]

    Parameter: IP_PTC_IMS_Handler.v_TCP_Connection = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 847]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 849
    text = Parameter: IP_PTC_IMS_Handler.v_Data = '425945207369703A37643530646431382D356565332D346561662D613134352D643331643834393837636239405B333030303A3A323A366336313A313866663A666535643A396631655D3A3434373234205349502F322E300D0A5669613A205349502F322E302F554450205B666432393A636334333A376662393A323A3230633A323966663A666536363A623463375D3A353036323B6272616E63683D7A39684734624B333230303938373635340D0A5669613A205349502F322E302F554450207363736366312E336770702E6F72673B6272616E63683D7A39684734624B323030393837363534330D0A5669613A205349502F322E302F554450207363736366322E336770702E6F72673B6272616E63683D7A39684734624B303039383736353433320D0A5669613A205349502F322E302F554450207063736366322E336770702E6F72673B6272616E63683D7A39684734624B303938373635343330300D0A5669613A205349502F322E302F554450207374663136302E657473692E6F72673A363534333B6272616E63683D7A39684734624B393837363534333030300D0A46726F6D3A203C7369703A5...

    Parameter: IP_PTC_IMS_Handler.v_Data = '425945207369703A37643530646431382D356565332D346561662D613134352D643331643834393837636239405B333030303A3A323A366336313A313866663A666535643A396631655D3A3434373234205349502F322E300D0A5669613A205349502F322E302F554450205B666432393A636334333A376662393A323A3230633A323966663A666536363A623463375D3A353036323B6272616E63683D7A39684734624B333230303938373635340D0A5669613A205349502F322E302F554450207363736366312E336770702E6F72673B6272616E63683D7A39684734624B323030393837363534330D0A5669613A205349502F322E302F554450207363736366322E336770702E6F72673B6272616E63683D7A39684734624B303039383736353433320D0A5669613A205349502F322E302F554450207063736366322E336770702E6F72673B6272616E63683D7A39684734624B303938373635343330300D0A5669613A205349502F322E302F554450207374663136302E657473692E6F72673A363534333B6272616E63683D7A39684734624B393837363534333030300D0A46726F6D3A203C7369703A5...

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1873
    text = Parameter: IMS_Component.v_IgnoreReset = False
    File: IMS_Component.ttcn [Line: 1873]

    Parameter: IMS_Component.v_IgnoreReset = False
    File: IMS_Component.ttcn [Line: 1873]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 862
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContextEnum = protectedContext1
    File: IP_PTC_IMS_Handler.ttcn [Line: 862]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContextEnum = protectedContext1
    File: IP_PTC_IMS_Handler.ttcn [Line: 862]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 872
    text = Parameter: IP_PTC_IMS_Handler.v_IsUnprotected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 872]

    Parameter: IP_PTC_IMS_Handler.v_IsUnprotected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 872]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 560
    text = Parameter: IP_PTC_IMS_Handler.v_LocalRemotePort.Local = 5061
    File: IP_PTC_IMS_Handler.ttcn [Line: 560]

    Parameter: IP_PTC_IMS_Handler.v_LocalRemotePort.Local = 5061
    File: IP_PTC_IMS_Handler.ttcn [Line: 560]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 561
    text = Parameter: IP_PTC_IMS_Handler.v_LocalRemotePort.Remote = 44724
    File: IP_PTC_IMS_Handler.ttcn [Line: 561]

    Parameter: IP_PTC_IMS_Handler.v_LocalRemotePort.Remote = 44724
    File: IP_PTC_IMS_Handler.ttcn [Line: 561]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 875
    text = Parameter: IP_PTC_IMS_Handler.v_LocalPort = 5061
    File: IP_PTC_IMS_Handler.ttcn [Line: 875]

    Parameter: IP_PTC_IMS_Handler.v_LocalPort = 5061
    File: IP_PTC_IMS_Handler.ttcn [Line: 875]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 876
    text = Parameter: IP_PTC_IMS_Handler.v_RemotePort = 44724
    File: IP_PTC_IMS_Handler.ttcn [Line: 876]

    Parameter: IP_PTC_IMS_Handler.v_RemotePort = 44724
    File: IP_PTC_IMS_Handler.ttcn [Line: 876]

    IP_SOCKET_REQ
    	DATA
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 5061
    			Remote
    				IpAddr
    					V6
    						Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    						ScopeId = Omit
    				Port = 44724
    		Req
    			UDP
    				SendTo
    					Buffer = '425945207369703A37643530646431382D356565332D346561662D613134352D643331643834393837636239405B333030303A3A323A366336313A313866663A666535643A396631655D3A3434373234205349502F322E300D0A5669613A205349502F322E302F554450205B666432393A636334333A376662393A323A3230633A323966663A666536363A623463375D3A353036323B6272616E63683D7A39684734624B333230303938373635340D0A5669613A205349502F322E302F554450207363736366312E336770702E6F72673B6272616E63683D7A39684734624B323030393837363534330D0A5669613A205349502F322E302F554450207363736366322E336770702E6F72673B6272616E63683D7A39684734624B303039383736353433320D0A5669613A205349502F322E302F554450207063736366322E336770702E6F72673B6272616E63683D7A39684734624B303938373635343330300D0A5669613A205349502F322E302F554450207374663136302E657473692E6F72673A363534333B6272616E63683D7A39684734624B393837363534333030300D0A46726F6D3A203C7369703A5065657255452D5075626C6963407374663136302E657473692E6F72673E3B7461673D6162632D494E564954452D46726F6D7461670D0A546F3A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E3B7461673D313538333833343538320D0A43616C6C2D49443A20494E564954452D302D376465632D313164302D613736352D30306130633931653662663640464432393A434334333A374642393A303030323A303230433A323946463A464536363A423443370D0A435365713A2034373135204259450D0A4D61782D466F7277617264733A2036370D0A436F6E74656E742D4C656E6774683A20300D0A0D0A'O

    Inter-component message: IP_SOCK_DATA -> IPMUX:IP_SOCK_DATA

    SipMessage
    	Message Header = BYE sip:7d50dd18-5ee3-4eaf-a145-d31d84987cb9@[3000::2:6c61:18ff:fe5d:9f1e]:44724 SIP/2.0
    Via: SIP/2.0/UDP [fd29:cc43:7fb9:2:20c:29ff:fe66:b4c7]:5062;branch=z9hG4bK3200987654
    Via: SIP/2.0/UDP scscf1.3gpp.org;branch=z9hG4bK2009876543
    Via: SIP/2.0/UDP scscf2.3gpp.org;branch=z9hG4bK0098765432
    Via: SIP/2.0/UDP pcscf2.3gpp.org;branch=z9hG4bK0987654300
    Via: SIP/2.0/UDP stf160.etsi.org:6543;branch=z9hG4bK9876543000
    From: ;tag=abc-INVITE-Fromtag
    To: ;tag=1583834582
    Call-ID: INVITE-0-7dec-11d0-a765-00a0c91e6bf6@FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7
    CSeq: 4715 BYE
    Max-Forwards: 67
    Content-Length: 0

    Request:BYE sip:7d50dd18-5ee3-4eaf-a145-d31d84987cb9@[3000::2:6c61:18ff:fe5d:9f1e]:44724 SIP/2.0

    IP_SOCKET_REQ
    	DATA
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 5061
    			Remote
    				IpAddr
    					V6
    						Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    						ScopeId = Omit
    				Port = 44724
    		Req
    			UDP
    				SendTo
    					Buffer = '425945207369703A37643530646431382D356565332D346561662D613134352D643331643834393837636239405B333030303A3A323A366336313A313866663A666535643A396631655D3A3434373234205349502F322E300D0A5669613A205349502F322E302F554450205B666432393A636334333A376662393A323A3230633A323966663A666536363A623463375D3A353036323B6272616E63683D7A39684734624B333230303938373635340D0A5669613A205349502F322E302F554450207363736366312E336770702E6F72673B6272616E63683D7A39684734624B323030393837363534330D0A5669613A205349502F322E302F554450207363736366322E336770702E6F72673B6272616E63683D7A39684734624B303039383736353433320D0A5669613A205349502F322E302F554450207063736366322E336770702E6F72673B6272616E63683D7A39684734624B303938373635343330300D0A5669613A205349502F322E302F554450207374663136302E657473692E6F72673A363534333B6272616E63683D7A39684734624B393837363534333030300D0A46726F6D3A203C7369703A5065657255452D5075626C6963407374663136302E657473692E6F72673E3B7461673D6162632D494E564954452D46726F6D7461670D0A546F3A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E3B7461673D313538333833343538320D0A43616C6C2D49443A20494E564954452D302D376465632D313164302D613736352D30306130633931653662663640464432393A434334333A374642393A303030323A303230433A323946463A464536363A423443370D0A435365713A2034373135204259450D0A4D61782D466F7277617264733A2036370D0A436F6E74656E742D4C656E6774683A20300D0A0D0A'O

    Sent from port: IPMUX:IP_SOCK

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_Main.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 596
    text = Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 596]

    Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 596]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_Main.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 741
    text = Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 741]

    Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 741]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 801
    text = Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 802
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 803
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 103
    text = Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 762
    text = Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 763
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 764
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 103
    text = Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 762
    text = Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 763
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 764
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 722
    text = Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 723
    text = Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 724
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 725
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 722
    text = Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 723
    text = Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 724
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 725
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 801
    text = Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 802
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 803
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1074
    text = Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 1074]

    Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 1074]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1075
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 1075]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 1075]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1076
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1076]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1076]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 103
    text = Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 274
    text = Parameter: IP_PTC_IMS_Handler.v_TcpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 274]

    Parameter: IP_PTC_IMS_Handler.v_TcpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 274]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 103
    text = Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 274
    text = Parameter: IP_PTC_IMS_Handler.v_TcpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 274]

    Parameter: IP_PTC_IMS_Handler.v_TcpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 274]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 247
    text = Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 247]

    Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 247]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 248
    text = Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 248]

    Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 248]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 247
    text = Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 247]

    Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 247]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 248
    text = Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 248]

    Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 248]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1074
    text = Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1074]

    Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1074]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1075
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1075]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1075]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1076
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1076]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1076]

    SipMessage
    	Message Header = SIP/2.0 200 OK
    Via: SIP/2.0/UDP [fd29:cc43:7fb9:2:20c:29ff:fe66:b4c7]:5062;branch=z9hG4bK3200987654,SIP/2.0/UDP scscf1.3gpp.org;branch=z9hG4bK2009876543,SIP/2.0/UDP scscf2.3gpp.org;branch=z9hG4bK0098765432,SIP/2.0/UDP pcscf2.3gpp.org;branch=z9hG4bK0987654300,SIP/2.0/UDP stf160.etsi.org:6543;branch=z9hG4bK9876543000
    From: ;tag=abc-INVITE-Fromtag
    To: ;tag=1583834582
    Call-ID: INVITE-0-7dec-11d0-a765-00a0c91e6bf6@FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7
    CSeq: 4715 BYE
    Content-Length: 0
    Server: qti_Lahaina for arm64_RKQ1.210107.001
    P-Access-Network-Info: 3GPP-NR-TDD;utran-cell-id-3gpp=00101000001000000400

    Status:SIP/2.0 200 OK

    IP_SOCKET_IND
    	DATA
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 5062
    			Remote
    				IpAddr
    					V6
    						Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    						ScopeId = Omit
    				Port = 43642
    		Ind
    			UDP
    				RecvFrom
    					Buffer = '5349502F322E3020323030204F4B0D0A5669613A205349502F322E302F554450205B666432393A636334333A376662393A323A3230633A323966663A666536363A623463375D3A353036323B6272616E63683D7A39684734624B333230303938373635342C5349502F322E302F554450207363736366312E336770702E6F72673B6272616E63683D7A39684734624B323030393837363534332C5349502F322E302F554450207363736366322E336770702E6F72673B6272616E63683D7A39684734624B303039383736353433322C5349502F322E302F554450207063736366322E336770702E6F72673B6272616E63683D7A39684734624B303938373635343330302C5349502F322E302F554450207374663136302E657473692E6F72673A363534333B6272616E63683D7A39684734624B393837363534333030300D0A46726F6D3A203C7369703A5065657255452D5075626C6963407374663136302E657473692E6F72673E3B7461673D6162632D494E564954452D46726F6D7461670D0A546F3A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E3B7461673D313538333833343538320D0A43616C6C2D49443A20494E564954452D302D376465632D313164302D613736352D30306130633931653662663640464432393A434334333A374642393A303030323A303230433A323946463A464536363A423443370D0A435365713A2034373135204259450D0A436F6E74656E742D4C656E6774683A20300D0A5365727665723A207174695F4C616861696E6120666F722061726D36345F524B51312E3231303130372E3030310D0A502D4163636573732D4E6574776F726B2D496E666F3A20334750502D4E522D5444443B757472616E2D63656C6C2D69642D336770703D30303130313030303030313030303030303430300D0A0D0A'O
    					DrbInfo
    						Eutra
    							CellId = eutra_Cell1 (1)
    							DrbId = 0

    Received on port: IPMUX:IP_SOCK

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_Main.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 596
    text = Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 596]

    Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 596]

    summary = Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Local.Port
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Local.Port
    		DATA
    			ConnectionId
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5062
    				Remote
    					IpAddr
    						V6
    							Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    							ScopeId = Omit
    					Port = 43642
    			Ind
    				UDP
    					RecvFrom
    						Buffer = '5349502F322E3020323030204F4B0D0A5669613A205349502F322E302F554450205B666432393A636334333A376662393A323A3230633A323966663A666536363A623463375D3A353036323B6272616E63683D7A39684734624B333230303938373635342C5349502F322E302F554450207363736366312E336770702E6F72673B6272616E63683D7A39684734624B323030393837363534332C5349502F322E302F554450207363736366322E336770702E6F72673B6272616E63683D7A39684734624B303039383736353433322C5349502F322E302F554450207063736366322E336770702E6F72673B6272616E63683D7A39684734624B303938373635343330302C5349502F322E302F554450207374663136302E657473692E6F72673A363534333B6272616E63683D7A39684734624B393837363534333030300D0A46726F6D3A203C7369703A5065657255452D5075626C6963407374663136302E657473692E6F72673E3B7461673D6162632D494E564954452D46726F6D7461670D0A546F3A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E3B7461673D313538333833343538320D0A43616C6C2D49443A20494E564954452D302D376465632D313164302D613736352D30306130633931653662663640464432393A434334333A374642393A303030323A303230433A323946463A464536363A423443370D0A435365713A2034373135204259450D0A436F6E74656E742D4C656E6774683A20300D0A5365727665723A207174695F4C616861696E6120666F722061726D36345F524B51312E3231303130372E3030310D0A502D4163636573732D4E6574776F726B2D496E666F3A20334750502D4E522D5444443B757472616E2D63656C6C2D69642D336770703D30303130313030303030313030303030303430300D0A0D0A'O
    						DrbInfo
    							Eutra
    								CellId = eutra_Cell1 (1)
    								DrbId = 0

    Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Local.Port

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_Main.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 741
    text = Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 741]

    Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 741]

    summary = Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol
    		DATA
    			ConnectionId
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5062
    				Remote
    					IpAddr
    						V6
    							Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    							ScopeId = Omit
    					Port = 43642
    			Ind
    				UDP
    					RecvFrom
    						Buffer = '5349502F322E3020323030204F4B0D0A5669613A205349502F322E302F554450205B666432393A636334333A376662393A323A3230633A323966663A666536363A623463375D3A353036323B6272616E63683D7A39684734624B333230303938373635342C5349502F322E302F554450207363736366312E336770702E6F72673B6272616E63683D7A39684734624B323030393837363534332C5349502F322E302F554450207363736366322E336770702E6F72673B6272616E63683D7A39684734624B303039383736353433322C5349502F322E302F554450207063736366322E336770702E6F72673B6272616E63683D7A39684734624B303938373635343330302C5349502F322E302F554450207374663136302E657473692E6F72673A363534333B6272616E63683D7A39684734624B393837363534333030300D0A46726F6D3A203C7369703A5065657255452D5075626C6963407374663136302E657473692E6F72673E3B7461673D6162632D494E564954452D46726F6D7461670D0A546F3A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E3B7461673D313538333833343538320D0A43616C6C2D49443A20494E564954452D302D376465632D313164302D613736352D30306130633931653662663640464432393A434334333A374642393A303030323A303230433A323946463A464536363A423443370D0A435365713A2034373135204259450D0A436F6E74656E742D4C656E6774683A20300D0A5365727665723A207174695F4C616861696E6120666F722061726D36345F524B51312E3231303130372E3030310D0A502D4163636573732D4E6574776F726B2D496E666F3A20334750502D4E522D5444443B757472616E2D63656C6C2D69642D336770703D30303130313030303030313030303030303430300D0A0D0A'O
    						DrbInfo
    							Eutra
    								CellId = eutra_Cell1 (1)
    								DrbId = 0

    Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 801
    text = Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 802
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 803
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 103
    text = Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 762
    text = Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 763
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 764
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    summary = Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Local.Port
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Local.Port
    		DATA
    			ConnectionId
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5062
    				Remote
    					IpAddr
    						V6
    							Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    							ScopeId = Omit
    					Port = 43642
    			Ind
    				UDP
    					RecvFrom
    						Buffer = '5349502F322E3020323030204F4B0D0A5669613A205349502F322E302F554450205B666432393A636334333A376662393A323A3230633A323966663A666536363A623463375D3A353036323B6272616E63683D7A39684734624B333230303938373635342C5349502F322E302F554450207363736366312E336770702E6F72673B6272616E63683D7A39684734624B323030393837363534332C5349502F322E302F554450207363736366322E336770702E6F72673B6272616E63683D7A39684734624B303039383736353433322C5349502F322E302F554450207063736366322E336770702E6F72673B6272616E63683D7A39684734624B303938373635343330302C5349502F322E302F554450207374663136302E657473692E6F72673A363534333B6272616E63683D7A39684734624B393837363534333030300D0A46726F6D3A203C7369703A5065657255452D5075626C6963407374663136302E657473692E6F72673E3B7461673D6162632D494E564954452D46726F6D7461670D0A546F3A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E3B7461673D313538333833343538320D0A43616C6C2D49443A20494E564954452D302D376465632D313164302D613736352D30306130633931653662663640464432393A434334333A374642393A303030323A303230433A323946463A464536363A423443370D0A435365713A2034373135204259450D0A436F6E74656E742D4C656E6774683A20300D0A5365727665723A207174695F4C616861696E6120666F722061726D36345F524B51312E3231303130372E3030310D0A502D4163636573732D4E6574776F726B2D496E666F3A20334750502D4E522D5444443B757472616E2D63656C6C2D69642D336770703D30303130313030303030313030303030303430300D0A0D0A'O
    						DrbInfo
    							Eutra
    								CellId = eutra_Cell1 (1)
    								DrbId = 0

    Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Local.Port

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 103
    text = Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 762
    text = Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 763
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 764
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    Sender = RequestServer
    Text = Received NO CARRIER from Device Under Test

    RequestServer:Received NO CARRIER from Device Under Test

    IP_SOCKET_IND
    	DATA
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 5062
    			Remote
    				IpAddr
    					V6
    						Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    						ScopeId = Omit
    				Port = 43642
    		Ind
    			UDP
    				RecvFrom
    					Buffer = '5349502F322E3020323030204F4B0D0A5669613A205349502F322E302F554450205B666432393A636334333A376662393A323A3230633A323966663A666536363A623463375D3A353036323B6272616E63683D7A39684734624B333230303938373635342C5349502F322E302F554450207363736366312E336770702E6F72673B6272616E63683D7A39684734624B323030393837363534332C5349502F322E302F554450207363736366322E336770702E6F72673B6272616E63683D7A39684734624B303039383736353433322C5349502F322E302F554450207063736366322E336770702E6F72673B6272616E63683D7A39684734624B303938373635343330302C5349502F322E302F554450207374663136302E657473692E6F72673A363534333B6272616E63683D7A39684734624B393837363534333030300D0A46726F6D3A203C7369703A5065657255452D5075626C6963407374663136302E657473692E6F72673E3B7461673D6162632D494E564954452D46726F6D7461670D0A546F3A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E3B7461673D313538333833343538320D0A43616C6C2D49443A20494E564954452D302D376465632D313164302D613736352D30306130633931653662663640464432393A434334333A374642393A303030323A303230433A323946463A464536363A423443370D0A435365713A2034373135204259450D0A436F6E74656E742D4C656E6774683A20300D0A5365727665723A207174695F4C616861696E6120666F722061726D36345F524B51312E3231303130372E3030310D0A502D4163636573732D4E6574776F726B2D496E666F3A20334750502D4E522D5444443B757472616E2D63656C6C2D69642D336770703D30303130313030303030313030303030303430300D0A0D0A'O
    					DrbInfo
    						Eutra
    							CellId = eutra_Cell1 (1)
    							DrbId = 0

    Inter-component message: IP_SOCK_DATA -> IP:IP_SOCK_DATA

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 776
    text = Parameter: IP_PTC_IMS_Handler.v_Data = '5349502F322E3020323030204F4B0D0A5669613A205349502F322E302F554450205B666432393A636334333A376662393A323A3230633A323966663A666536363A623463375D3A353036323B6272616E63683D7A39684734624B333230303938373635342C5349502F322E302F554450207363736366312E336770702E6F72673B6272616E63683D7A39684734624B323030393837363534332C5349502F322E302F554450207363736366322E336770702E6F72673B6272616E63683D7A39684734624B303039383736353433322C5349502F322E302F554450207063736366322E336770702E6F72673B6272616E63683D7A39684734624B303938373635343330302C5349502F322E302F554450207374663136302E657473692E6F72673A363534333B6272616E63683D7A39684734624B393837363534333030300D0A46726F6D3A203C7369703A5065657255452D5075626C6963407374663136302E657473692E6F72673E3B7461673D6162632D494E564954452D46726F6D7461670D0A546F3A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E3...

    Parameter: IP_PTC_IMS_Handler.v_Data = '5349502F322E3020323030204F4B0D0A5669613A205349502F322E302F554450205B666432393A636334333A376662393A323A3230633A323966663A666536363A623463375D3A353036323B6272616E63683D7A39684734624B333230303938373635342C5349502F322E302F554450207363736366312E336770702E6F72673B6272616E63683D7A39684734624B323030393837363534332C5349502F322E302F554450207363736366322E336770702E6F72673B6272616E63683D7A39684734624B303039383736353433322C5349502F322E302F554450207063736366322E336770702E6F72673B6272616E63683D7A39684734624B303938373635343330302C5349502F322E302F554450207374663136302E657473692E6F72673A363534333B6272616E63683D7A39684734624B393837363534333030300D0A46726F6D3A203C7369703A5065657255452D5075626C6963407374663136302E657473692E6F72673E3B7461673D6162632D494E564954452D46726F6D7461670D0A546F3A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E3...

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 618
    text = Parameter: IP_PTC_IMS_Handler.v_SIP_Message = 'SIP/2.0 200 OK
    Via:'
    File: IP_PTC_IMS_Handler.ttcn [Line: 618]

    Parameter: IP_PTC_IMS_Handler.v_SIP_Message = 'SIP/2.0 200 OK
    Via:'
    File: IP_PTC_IMS_Handler.ttcn [Line: 618]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 619
    text = Parameter: IP_PTC_IMS_Handler.v_AnyResponse = 'SIP/[1-9][.][0-9] [1-9][0-9][0-9]*'
    File: IP_PTC_IMS_Handler.ttcn [Line: 619]

    Parameter: IP_PTC_IMS_Handler.v_AnyResponse = 'SIP/[1-9][.][0-9] [1-9][0-9][0-9]*'
    File: IP_PTC_IMS_Handler.ttcn [Line: 619]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 777
    text = Parameter: IP_PTC_IMS_Handler.v_RequestResponse = response
    File: IP_PTC_IMS_Handler.ttcn [Line: 777]

    Parameter: IP_PTC_IMS_Handler.v_RequestResponse = response
    File: IP_PTC_IMS_Handler.ttcn [Line: 777]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 697
    text = Parameter: IP_PTC_IMS_Handler.v_Bitstring = '010100110100100101010000001011110011001000101110001100000010000000110010001100000011000000100000010011110100101100001101000010100101011001101001011000010011101000100000010100110100100101010000001011110011001000101110001100000010111101010101010001000101000000100000010110110110011001100100001100100011100100111010011000110110001100110100001100110011101000110111011001100110001000111001001110100011001000111010001100100011000001100011001110100011001000111001011001100110011000111010011001100110010100110110001101100011101001100010001101000110001100110111010111010011101000110101001100000011011000110010001110110110001001110010011000010110111001100011011010000011110101111010001110010110100001000111001101000110001001001011001100110011001000110000001100000011100100111000001101110011011000110101001101000010110001010011010010010101000000101111001100100010...

    Parameter: IP_PTC_IMS_Handler.v_Bitstring = '010100110100100101010000001011110011001000101110001100000010000000110010001100000011000000100000010011110100101100001101000010100101011001101001011000010011101000100000010100110100100101010000001011110011001000101110001100000010111101010101010001000101000000100000010110110110011001100100001100100011100100111010011000110110001100110100001100110011101000110111011001100110001000111001001110100011001000111010001100100011000001100011001110100011001000111001011001100110011000111010011001100110010100110110001101100011101001100010001101000110001100110111010111010011101000110101001100000011011000110010001110110110001001110010011000010110111001100011011010000011110101111010001110010110100001000111001101000110001001001011001100110011001000110000001100000011100100111000001101110011011000110101001101000010110001010011010010010101000000101111001100100010...

    IMS_DATA_RSP
    	RoutingInfo
    		Protocol = udp (0)
    		Security = protectedContext1 (1)
    		UE_Address = Omit
    		NW_Address = Omit
    	Response
    		statusLine
    			sipVersion = 'SIP/2.0'
    			statusCode = 200
    			reasonPhrase = 'OK'
    		msgHeader
    			accept = Omit
    			acceptContact = Omit
    			acceptEncoding = Omit
    			acceptLanguage = Omit
    			alertInfo = Omit
    			allow = Omit
    			allowEvents = Omit
    			authenticationInfo = Omit
    			authorization = Omit
    			callId
    				fieldName = CALL_ID_E (7)
    				callid = 'INVITE-0-7dec-11d0-a765-00a0c91e6bf6@FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    			callInfo = Omit
    			contact = Omit
    			contentDisposition = Omit
    			contentEncoding = Omit
    			contentLanguage = Omit
    			contentLength
    				fieldName = CONTENT_LENGTH_E (13)
    				len = 0
    			contentType = Omit
    			cSeq
    				fieldName = CSEQ_E (15)
    				seqNumber = 4715
    				method = 'BYE'
    			date = Omit
    			errorInfo = Omit
    			event = Omit
    			expires = Omit
    			featureCaps = Omit
    			fromField
    				fieldName = FROM_E (19)
    				addressField
    					nameAddr
    						displayName = Omit
    						addrSpec
    							scheme = 'sip'
    							components
    								sip
    									userInfo
    										userOrTelephoneSubscriber = 'PeerUE-Public'
    										password = Omit
    									hostPort
    										host = 'stf160.etsi.org'
    										portField = Omit
    							urlParameters = Omit
    							headers = Omit
    				fromParams
    					GenericParam
    						id = 'tag'
    						paramValue
    							tokenOrHost = 'abc-INVITE-Fromtag'
    			geolocation = Omit
    			geolocationRouting = Omit
    			historyInfo = Omit
    			infoPackage = Omit
    			inReplyTo = Omit
    			maxForwards = Omit
    			mimeVersion = Omit
    			minExpires = Omit
    			minSE = Omit
    			organization = Omit
    			pAccessNetworkInfo
    				fieldName = P_ACCESS_NETWORK_INFO_E (65)
    				accessType = '3GPP-NR-TDD'
    				genericParams
    					GenericParam
    						id = 'utran-cell-id-3gpp'
    						paramValue
    							tokenOrHost = '00101000001000000400'
    			pAssertedID = Omit
    			pAssertedService = Omit
    			pAssociatedURI = Omit
    			path = Omit
    			pCalledPartyID = Omit
    			pChargingFunctionAddresses = Omit
    			pChargingVector = Omit
    			pEarlyMedia = Omit
    			pMediaAuthorization = Omit
    			pPreferredID = Omit
    			pPreferredService = Omit
    			priority = Omit
    			privacy = Omit
    			proxyAuthenticate = Omit
    			proxyAuthorization = Omit
    			proxyRequire = Omit
    			pVisitedNetworkID = Omit
    			rAck = Omit
    			rSeq = Omit
    			reason = Omit
    			recordRoute = Omit
    			recvInfo = Omit
    			requestDisposition = Omit
    			referredBy = Omit
    			referTo = Omit
    			referSub = Omit
    			replaces = Omit
    			replyTo = Omit
    			require = Omit
    			retryAfter = Omit
    			route = Omit
    			securityClient = Omit
    			securityServer = Omit
    			securityVerify = Omit
    			server
    				fieldName = SERVER_E (34)
    				serverBody
    					CharacterStringType = 'qti_Lahaina for arm64_RKQ1.210107.001'
    			serviceRoute = Omit
    			sessionExpires = Omit
    			sessionId = Omit
    			sipETag = Omit
    			sipIfMatch = Omit
    			subject = Omit
    			subscriptionState = Omit
    			supported = Omit
    			timestamp = Omit
    			toField
    				fieldName = TO_E (38)
    				addressField
    					nameAddr
    						displayName = Omit
    						addrSpec
    							scheme = 'sip'
    							components
    								sip
    									userInfo
    										userOrTelephoneSubscriber = '001010123456789'
    										password = Omit
    									hostPort
    										host = 'ims.mnc001.mcc001.3gppnetwork.org'
    										portField = Omit
    							urlParameters = Omit
    							headers = Omit
    				toParams
    					GenericParam
    						id = 'tag'
    						paramValue
    							tokenOrHost = '1583834582'
    			unsupported = Omit
    			userToUser = Omit
    			userAgent = Omit
    			via
    				fieldName = VIA_E (41)
    				viaBody
    					ViaBody
    						sentProtocol
    							protocolName = 'SIP'
    							protocolVersion = '2.0'
    							transport = 'UDP'
    						sentBy
    							host = 'fd29:cc43:7fb9:2:20c:29ff:fe66:b4c7'
    							portField = 5062
    						viaParams
    							GenericParam
    								id = 'branch'
    								paramValue
    									tokenOrHost = 'z9hG4bK3200987654'
    					ViaBody
    						sentProtocol
    							protocolName = 'SIP'
    							protocolVersion = '2.0'
    							transport = 'UDP'
    						sentBy
    							host = 'scscf1.3gpp.org'
    							portField = Omit
    						viaParams
    							GenericParam
    								id = 'branch'
    								paramValue
    									tokenOrHost = 'z9hG4bK2009876543'
    					ViaBody
    						sentProtocol
    							protocolName = 'SIP'
    							protocolVersion = '2.0'
    							transport = 'UDP'
    						sentBy
    							host = 'scscf2.3gpp.org'
    							portField = Omit
    						viaParams
    							GenericParam
    								id = 'branch'
    								paramValue
    									tokenOrHost = 'z9hG4bK0098765432'
    					ViaBody
    						sentProtocol
    							protocolName = 'SIP'
    							protocolVersion = '2.0'
    							transport = 'UDP'
    						sentBy
    							host = 'pcscf2.3gpp.org'
    							portField = Omit
    						viaParams
    							GenericParam
    								id = 'branch'
    								paramValue
    									tokenOrHost = 'z9hG4bK0987654300'
    					ViaBody
    						sentProtocol
    							protocolName = 'SIP'
    							protocolVersion = '2.0'
    							transport = 'UDP'
    						sentBy
    							host = 'stf160.etsi.org'
    							portField = 6543
    						viaParams
    							GenericParam
    								id = 'branch'
    								paramValue
    									tokenOrHost = 'z9hG4bK9876543000'
    			warning = Omit
    			wwwAuthenticate = Omit
    			resourcePriority = Omit
    			answerMode = Omit
    			privAnswerMode = Omit
    			targetDialog = Omit
    			pAnswerState = Omit
    			undefinedHeader_List = Omit
    		messageBody = Omit
    		payload = Omit

    Inter-component message: IMS_Client -> IMS1:IMS_Client

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_Main.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 596
    text = Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 596]

    Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 596]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_Main.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 741
    text = Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 741]

    Parameter: IP_PTC_Main.v_DrbInfo = Omit
    File: IP_PTC_Main.ttcn [Line: 741]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 801
    text = Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 466
    text = Parameter: IMS_Procedures_Common.v_LengthOfViaBody_Request = 5
    File: IMS_Procedures_Common.ttcn [Line: 466]

    Parameter: IMS_Procedures_Common.v_LengthOfViaBody_Request = 5
    File: IMS_Procedures_Common.ttcn [Line: 466]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 467
    text = Parameter: IMS_Procedures_Common.v_LengthOfViaBody_Response = 5
    File: IMS_Procedures_Common.ttcn [Line: 467]

    Parameter: IMS_Procedures_Common.v_LengthOfViaBody_Response = 5
    File: IMS_Procedures_Common.ttcn [Line: 467]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 468
    text = Parameter: IMS_Procedures_Common.v_Mismatch = False
    File: IMS_Procedures_Common.ttcn [Line: 468]

    Parameter: IMS_Procedures_Common.v_Mismatch = False
    File: IMS_Procedures_Common.ttcn [Line: 468]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 474
    text = Parameter: IMS_Procedures_Common.i = 0
    File: IMS_Procedures_Common.ttcn [Line: 474]

    Parameter: IMS_Procedures_Common.i = 0
    File: IMS_Procedures_Common.ttcn [Line: 474]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 802
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 803
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 103
    text = Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 762
    text = Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 763
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 764
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 103
    text = Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 213
    text = Parameter: CommonIP.v_FieldCnt = 8
    File: CommonIP.ttcn [Line: 213]

    Parameter: CommonIP.v_FieldCnt = 8
    File: CommonIP.ttcn [Line: 213]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 221
    text = Parameter: CommonIP.i = 0
    File: CommonIP.ttcn [Line: 221]

    Parameter: CommonIP.i = 0
    File: CommonIP.ttcn [Line: 221]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 222
    text = Parameter: CommonIP.v_Field = 'fd29'
    File: CommonIP.ttcn [Line: 222]

    Parameter: CommonIP.v_Field = 'fd29'
    File: CommonIP.ttcn [Line: 222]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 223
    text = Parameter: CommonIP.v_FieldLength = 4
    File: CommonIP.ttcn [Line: 223]

    Parameter: CommonIP.v_FieldLength = 4
    File: CommonIP.ttcn [Line: 223]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 224
    text = Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(4)'
    File: CommonIP.ttcn [Line: 224]

    Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(4)'
    File: CommonIP.ttcn [Line: 224]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 221
    text = Parameter: CommonIP.i = 1
    File: CommonIP.ttcn [Line: 221]

    Parameter: CommonIP.i = 1
    File: CommonIP.ttcn [Line: 221]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 762
    text = Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    Parameter: IP_PTC_IMS_Handler.v_UdpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 762]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 222
    text = Parameter: CommonIP.v_Field = 'cc43'
    File: CommonIP.ttcn [Line: 222]

    Parameter: CommonIP.v_Field = 'cc43'
    File: CommonIP.ttcn [Line: 222]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 763
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 763]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 223
    text = Parameter: CommonIP.v_FieldLength = 4
    File: CommonIP.ttcn [Line: 223]

    Parameter: CommonIP.v_FieldLength = 4
    File: CommonIP.ttcn [Line: 223]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 764
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 764]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 224
    text = Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(4)'
    File: CommonIP.ttcn [Line: 224]

    Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(4)'
    File: CommonIP.ttcn [Line: 224]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 221
    text = Parameter: CommonIP.i = 2
    File: CommonIP.ttcn [Line: 221]

    Parameter: CommonIP.i = 2
    File: CommonIP.ttcn [Line: 221]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 222
    text = Parameter: CommonIP.v_Field = '7fb9'
    File: CommonIP.ttcn [Line: 222]

    Parameter: CommonIP.v_Field = '7fb9'
    File: CommonIP.ttcn [Line: 222]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 223
    text = Parameter: CommonIP.v_FieldLength = 4
    File: CommonIP.ttcn [Line: 223]

    Parameter: CommonIP.v_FieldLength = 4
    File: CommonIP.ttcn [Line: 223]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 224
    text = Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(4)'
    File: CommonIP.ttcn [Line: 224]

    Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(4)'
    File: CommonIP.ttcn [Line: 224]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 221
    text = Parameter: CommonIP.i = 3
    File: CommonIP.ttcn [Line: 221]

    Parameter: CommonIP.i = 3
    File: CommonIP.ttcn [Line: 221]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 222
    text = Parameter: CommonIP.v_Field = '2'
    File: CommonIP.ttcn [Line: 222]

    Parameter: CommonIP.v_Field = '2'
    File: CommonIP.ttcn [Line: 222]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 223
    text = Parameter: CommonIP.v_FieldLength = 1
    File: CommonIP.ttcn [Line: 223]

    Parameter: CommonIP.v_FieldLength = 1
    File: CommonIP.ttcn [Line: 223]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 224
    text = Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(1)'
    File: CommonIP.ttcn [Line: 224]

    Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(1)'
    File: CommonIP.ttcn [Line: 224]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 221
    text = Parameter: CommonIP.i = 4
    File: CommonIP.ttcn [Line: 221]

    Parameter: CommonIP.i = 4
    File: CommonIP.ttcn [Line: 221]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 222
    text = Parameter: CommonIP.v_Field = '20c'
    File: CommonIP.ttcn [Line: 222]

    Parameter: CommonIP.v_Field = '20c'
    File: CommonIP.ttcn [Line: 222]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 223
    text = Parameter: CommonIP.v_FieldLength = 3
    File: CommonIP.ttcn [Line: 223]

    Parameter: CommonIP.v_FieldLength = 3
    File: CommonIP.ttcn [Line: 223]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 224
    text = Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(3)'
    File: CommonIP.ttcn [Line: 224]

    Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(3)'
    File: CommonIP.ttcn [Line: 224]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 722
    text = Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 723
    text = Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 221
    text = Parameter: CommonIP.i = 5
    File: CommonIP.ttcn [Line: 221]

    Parameter: CommonIP.i = 5
    File: CommonIP.ttcn [Line: 221]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 724
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 222
    text = Parameter: CommonIP.v_Field = '29ff'
    File: CommonIP.ttcn [Line: 222]

    Parameter: CommonIP.v_Field = '29ff'
    File: CommonIP.ttcn [Line: 222]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 725
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 223
    text = Parameter: CommonIP.v_FieldLength = 4
    File: CommonIP.ttcn [Line: 223]

    Parameter: CommonIP.v_FieldLength = 4
    File: CommonIP.ttcn [Line: 223]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 224
    text = Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(4)'
    File: CommonIP.ttcn [Line: 224]

    Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(4)'
    File: CommonIP.ttcn [Line: 224]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 221
    text = Parameter: CommonIP.i = 6
    File: CommonIP.ttcn [Line: 221]

    Parameter: CommonIP.i = 6
    File: CommonIP.ttcn [Line: 221]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 222
    text = Parameter: CommonIP.v_Field = 'fe66'
    File: CommonIP.ttcn [Line: 222]

    Parameter: CommonIP.v_Field = 'fe66'
    File: CommonIP.ttcn [Line: 222]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 223
    text = Parameter: CommonIP.v_FieldLength = 4
    File: CommonIP.ttcn [Line: 223]

    Parameter: CommonIP.v_FieldLength = 4
    File: CommonIP.ttcn [Line: 223]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 224
    text = Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(4)'
    File: CommonIP.ttcn [Line: 224]

    Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(4)'
    File: CommonIP.ttcn [Line: 224]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 221
    text = Parameter: CommonIP.i = 7
    File: CommonIP.ttcn [Line: 221]

    Parameter: CommonIP.i = 7
    File: CommonIP.ttcn [Line: 221]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 222
    text = Parameter: CommonIP.v_Field = 'b4c7'
    File: CommonIP.ttcn [Line: 222]

    Parameter: CommonIP.v_Field = 'b4c7'
    File: CommonIP.ttcn [Line: 222]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 223
    text = Parameter: CommonIP.v_FieldLength = 4
    File: CommonIP.ttcn [Line: 223]

    Parameter: CommonIP.v_FieldLength = 4
    File: CommonIP.ttcn [Line: 223]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 224
    text = Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(4)'
    File: CommonIP.ttcn [Line: 224]

    Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(4)'
    File: CommonIP.ttcn [Line: 224]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 221
    text = Parameter: CommonIP.i = 8
    File: CommonIP.ttcn [Line: 221]

    Parameter: CommonIP.i = 8
    File: CommonIP.ttcn [Line: 221]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 348
    text = Parameter: CommonIP.v_Addr1IsV6 = True
    File: CommonIP.ttcn [Line: 348]

    Parameter: CommonIP.v_Addr1IsV6 = True
    File: CommonIP.ttcn [Line: 348]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 722
    text = Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 722]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 723
    text = Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 723]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 724
    text = Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    Parameter: IP_PTC_IMS_Handler.v_NW_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 724]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 725
    text = Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    Parameter: IP_PTC_IMS_Handler.v_UE_Address = Omit
    File: IP_PTC_IMS_Handler.ttcn [Line: 725]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 801
    text = Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 801]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 802
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 802]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 803
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 803]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1074
    text = Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 1074]

    Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 1074]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1075
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 1075]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 1075]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 213
    text = Parameter: CommonIP.v_FieldCnt = 8
    File: CommonIP.ttcn [Line: 213]

    Parameter: CommonIP.v_FieldCnt = 8
    File: CommonIP.ttcn [Line: 213]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 221
    text = Parameter: CommonIP.i = 0
    File: CommonIP.ttcn [Line: 221]

    Parameter: CommonIP.i = 0
    File: CommonIP.ttcn [Line: 221]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 222
    text = Parameter: CommonIP.v_Field = 'fd29'
    File: CommonIP.ttcn [Line: 222]

    Parameter: CommonIP.v_Field = 'fd29'
    File: CommonIP.ttcn [Line: 222]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 223
    text = Parameter: CommonIP.v_FieldLength = 4
    File: CommonIP.ttcn [Line: 223]

    Parameter: CommonIP.v_FieldLength = 4
    File: CommonIP.ttcn [Line: 223]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1076
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1076]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1076]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 224
    text = Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(4)'
    File: CommonIP.ttcn [Line: 224]

    Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(4)'
    File: CommonIP.ttcn [Line: 224]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 221
    text = Parameter: CommonIP.i = 1
    File: CommonIP.ttcn [Line: 221]

    Parameter: CommonIP.i = 1
    File: CommonIP.ttcn [Line: 221]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 222
    text = Parameter: CommonIP.v_Field = 'cc43'
    File: CommonIP.ttcn [Line: 222]

    Parameter: CommonIP.v_Field = 'cc43'
    File: CommonIP.ttcn [Line: 222]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 223
    text = Parameter: CommonIP.v_FieldLength = 4
    File: CommonIP.ttcn [Line: 223]

    Parameter: CommonIP.v_FieldLength = 4
    File: CommonIP.ttcn [Line: 223]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 224
    text = Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(4)'
    File: CommonIP.ttcn [Line: 224]

    Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(4)'
    File: CommonIP.ttcn [Line: 224]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 103
    text = Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 221
    text = Parameter: CommonIP.i = 2
    File: CommonIP.ttcn [Line: 221]

    Parameter: CommonIP.i = 2
    File: CommonIP.ttcn [Line: 221]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 222
    text = Parameter: CommonIP.v_Field = '7fb9'
    File: CommonIP.ttcn [Line: 222]

    Parameter: CommonIP.v_Field = '7fb9'
    File: CommonIP.ttcn [Line: 222]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 223
    text = Parameter: CommonIP.v_FieldLength = 4
    File: CommonIP.ttcn [Line: 223]

    Parameter: CommonIP.v_FieldLength = 4
    File: CommonIP.ttcn [Line: 223]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 224
    text = Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(4)'
    File: CommonIP.ttcn [Line: 224]

    Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(4)'
    File: CommonIP.ttcn [Line: 224]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 221
    text = Parameter: CommonIP.i = 3
    File: CommonIP.ttcn [Line: 221]

    Parameter: CommonIP.i = 3
    File: CommonIP.ttcn [Line: 221]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 222
    text = Parameter: CommonIP.v_Field = '2'
    File: CommonIP.ttcn [Line: 222]

    Parameter: CommonIP.v_Field = '2'
    File: CommonIP.ttcn [Line: 222]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 223
    text = Parameter: CommonIP.v_FieldLength = 1
    File: CommonIP.ttcn [Line: 223]

    Parameter: CommonIP.v_FieldLength = 1
    File: CommonIP.ttcn [Line: 223]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 224
    text = Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(1)'
    File: CommonIP.ttcn [Line: 224]

    Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(1)'
    File: CommonIP.ttcn [Line: 224]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 221
    text = Parameter: CommonIP.i = 4
    File: CommonIP.ttcn [Line: 221]

    Parameter: CommonIP.i = 4
    File: CommonIP.ttcn [Line: 221]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 222
    text = Parameter: CommonIP.v_Field = '20c'
    File: CommonIP.ttcn [Line: 222]

    Parameter: CommonIP.v_Field = '20c'
    File: CommonIP.ttcn [Line: 222]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 223
    text = Parameter: CommonIP.v_FieldLength = 3
    File: CommonIP.ttcn [Line: 223]

    Parameter: CommonIP.v_FieldLength = 3
    File: CommonIP.ttcn [Line: 223]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 224
    text = Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(3)'
    File: CommonIP.ttcn [Line: 224]

    Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(3)'
    File: CommonIP.ttcn [Line: 224]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 221
    text = Parameter: CommonIP.i = 5
    File: CommonIP.ttcn [Line: 221]

    Parameter: CommonIP.i = 5
    File: CommonIP.ttcn [Line: 221]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 222
    text = Parameter: CommonIP.v_Field = '29ff'
    File: CommonIP.ttcn [Line: 222]

    Parameter: CommonIP.v_Field = '29ff'
    File: CommonIP.ttcn [Line: 222]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 223
    text = Parameter: CommonIP.v_FieldLength = 4
    File: CommonIP.ttcn [Line: 223]

    Parameter: CommonIP.v_FieldLength = 4
    File: CommonIP.ttcn [Line: 223]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 224
    text = Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(4)'
    File: CommonIP.ttcn [Line: 224]

    Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(4)'
    File: CommonIP.ttcn [Line: 224]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 221
    text = Parameter: CommonIP.i = 6
    File: CommonIP.ttcn [Line: 221]

    Parameter: CommonIP.i = 6
    File: CommonIP.ttcn [Line: 221]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 222
    text = Parameter: CommonIP.v_Field = 'fe66'
    File: CommonIP.ttcn [Line: 222]

    Parameter: CommonIP.v_Field = 'fe66'
    File: CommonIP.ttcn [Line: 222]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 223
    text = Parameter: CommonIP.v_FieldLength = 4
    File: CommonIP.ttcn [Line: 223]

    Parameter: CommonIP.v_FieldLength = 4
    File: CommonIP.ttcn [Line: 223]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 224
    text = Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(4)'
    File: CommonIP.ttcn [Line: 224]

    Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(4)'
    File: CommonIP.ttcn [Line: 224]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 221
    text = Parameter: CommonIP.i = 7
    File: CommonIP.ttcn [Line: 221]

    Parameter: CommonIP.i = 7
    File: CommonIP.ttcn [Line: 221]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 222
    text = Parameter: CommonIP.v_Field = 'b4c7'
    File: CommonIP.ttcn [Line: 222]

    Parameter: CommonIP.v_Field = 'b4c7'
    File: CommonIP.ttcn [Line: 222]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 223
    text = Parameter: CommonIP.v_FieldLength = 4
    File: CommonIP.ttcn [Line: 223]

    Parameter: CommonIP.v_FieldLength = 4
    File: CommonIP.ttcn [Line: 223]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 224
    text = Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(4)'
    File: CommonIP.ttcn [Line: 224]

    Parameter: CommonIP.v_Pattern = '[0-9a-fA-F]#(4)'
    File: CommonIP.ttcn [Line: 224]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 221
    text = Parameter: CommonIP.i = 8
    File: CommonIP.ttcn [Line: 221]

    Parameter: CommonIP.i = 8
    File: CommonIP.ttcn [Line: 221]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 349
    text = Parameter: CommonIP.v_Addr2IsV6 = True
    File: CommonIP.ttcn [Line: 349]

    Parameter: CommonIP.v_Addr2IsV6 = True
    File: CommonIP.ttcn [Line: 349]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 274
    text = Parameter: IP_PTC_IMS_Handler.v_TcpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 274]

    Parameter: IP_PTC_IMS_Handler.v_TcpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 274]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 103
    text = Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    Parameter: IP_PTC_IMS_Handler.v_ServerAddr = AnyValue
    File: IP_PTC_IMS_Handler.ttcn [Line: 103]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 274
    text = Parameter: IP_PTC_IMS_Handler.v_TcpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 274]

    Parameter: IP_PTC_IMS_Handler.v_TcpServerIsStarted = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 274]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 247
    text = Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 247]

    Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 247]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 248
    text = Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 248]

    Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 248]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 291
    text = Parameter: CommonIP.v_IPv6AddrOct = ''O
    File: CommonIP.ttcn [Line: 291]

    Parameter: CommonIP.v_IPv6AddrOct = ''O
    File: CommonIP.ttcn [Line: 291]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 292
    text = Parameter: CommonIP.v_FieldCnt = 8
    File: CommonIP.ttcn [Line: 292]

    Parameter: CommonIP.v_FieldCnt = 8
    File: CommonIP.ttcn [Line: 292]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 293
    text = Parameter: CommonIP.v_EmptyBlocksExpanded = False
    File: CommonIP.ttcn [Line: 293]

    Parameter: CommonIP.v_EmptyBlocksExpanded = False
    File: CommonIP.ttcn [Line: 293]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 302
    text = Parameter: CommonIP.i = 0
    File: CommonIP.ttcn [Line: 302]

    Parameter: CommonIP.i = 0
    File: CommonIP.ttcn [Line: 302]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 247
    text = Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 247]

    Parameter: IP_PTC_IMS_Handler.v_ClientIsConnected = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 247]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 303
    text = Parameter: CommonIP.v_Field = 'fd29'
    File: CommonIP.ttcn [Line: 303]

    Parameter: CommonIP.v_Field = 'fd29'
    File: CommonIP.ttcn [Line: 303]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 248
    text = Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 248]

    Parameter: IP_PTC_IMS_Handler.v_ServerIsConnected = True
    File: IP_PTC_IMS_Handler.ttcn [Line: 248]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 326
    text = Parameter: CommonIP.v_IPv6AddrOct = 'fd29'O
    File: CommonIP.ttcn [Line: 326]

    Parameter: CommonIP.v_IPv6AddrOct = 'fd29'O
    File: CommonIP.ttcn [Line: 326]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 302
    text = Parameter: CommonIP.i = 1
    File: CommonIP.ttcn [Line: 302]

    Parameter: CommonIP.i = 1
    File: CommonIP.ttcn [Line: 302]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 303
    text = Parameter: CommonIP.v_Field = 'cc43'
    File: CommonIP.ttcn [Line: 303]

    Parameter: CommonIP.v_Field = 'cc43'
    File: CommonIP.ttcn [Line: 303]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 326
    text = Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc43'O
    File: CommonIP.ttcn [Line: 326]

    Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc43'O
    File: CommonIP.ttcn [Line: 326]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 302
    text = Parameter: CommonIP.i = 2
    File: CommonIP.ttcn [Line: 302]

    Parameter: CommonIP.i = 2
    File: CommonIP.ttcn [Line: 302]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1074
    text = Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1074]

    Parameter: IP_PTC_IMS_Handler.v_ImsServer_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1074]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1075
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1075]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext1_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1075]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 303
    text = Parameter: CommonIP.v_Field = '7fb9'
    File: CommonIP.ttcn [Line: 303]

    Parameter: CommonIP.v_Field = '7fb9'
    File: CommonIP.ttcn [Line: 303]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IP_PTC\IP_PTC_IMS_Handler.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1076
    text = Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1076]

    Parameter: IP_PTC_IMS_Handler.v_SecurityContext2_IsStarted = False
    File: IP_PTC_IMS_Handler.ttcn [Line: 1076]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 326
    text = Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc437fb9'O
    File: CommonIP.ttcn [Line: 326]

    Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc437fb9'O
    File: CommonIP.ttcn [Line: 326]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 302
    text = Parameter: CommonIP.i = 3
    File: CommonIP.ttcn [Line: 302]

    Parameter: CommonIP.i = 3
    File: CommonIP.ttcn [Line: 302]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 303
    text = Parameter: CommonIP.v_Field = '2'
    File: CommonIP.ttcn [Line: 303]

    Parameter: CommonIP.v_Field = '2'
    File: CommonIP.ttcn [Line: 303]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 317
    text = Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc437fb90002'O
    File: CommonIP.ttcn [Line: 317]

    Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc437fb90002'O
    File: CommonIP.ttcn [Line: 317]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 302
    text = Parameter: CommonIP.i = 4
    File: CommonIP.ttcn [Line: 302]

    Parameter: CommonIP.i = 4
    File: CommonIP.ttcn [Line: 302]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 303
    text = Parameter: CommonIP.v_Field = '20c'
    File: CommonIP.ttcn [Line: 303]

    Parameter: CommonIP.v_Field = '20c'
    File: CommonIP.ttcn [Line: 303]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 323
    text = Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc437fb90002020c'O
    File: CommonIP.ttcn [Line: 323]

    Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc437fb90002020c'O
    File: CommonIP.ttcn [Line: 323]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 302
    text = Parameter: CommonIP.i = 5
    File: CommonIP.ttcn [Line: 302]

    Parameter: CommonIP.i = 5
    File: CommonIP.ttcn [Line: 302]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 303
    text = Parameter: CommonIP.v_Field = '29ff'
    File: CommonIP.ttcn [Line: 303]

    Parameter: CommonIP.v_Field = '29ff'
    File: CommonIP.ttcn [Line: 303]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 326
    text = Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc437fb90002020c29ff'O
    File: CommonIP.ttcn [Line: 326]

    Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc437fb90002020c29ff'O
    File: CommonIP.ttcn [Line: 326]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 302
    text = Parameter: CommonIP.i = 6
    File: CommonIP.ttcn [Line: 302]

    Parameter: CommonIP.i = 6
    File: CommonIP.ttcn [Line: 302]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 303
    text = Parameter: CommonIP.v_Field = 'fe66'
    File: CommonIP.ttcn [Line: 303]

    Parameter: CommonIP.v_Field = 'fe66'
    File: CommonIP.ttcn [Line: 303]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 326
    text = Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc437fb90002020c29fffe66'O
    File: CommonIP.ttcn [Line: 326]

    Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc437fb90002020c29fffe66'O
    File: CommonIP.ttcn [Line: 326]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 302
    text = Parameter: CommonIP.i = 7
    File: CommonIP.ttcn [Line: 302]

    Parameter: CommonIP.i = 7
    File: CommonIP.ttcn [Line: 302]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 303
    text = Parameter: CommonIP.v_Field = 'b4c7'
    File: CommonIP.ttcn [Line: 303]

    Parameter: CommonIP.v_Field = 'b4c7'
    File: CommonIP.ttcn [Line: 303]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 326
    text = Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc437fb90002020c29fffe66b4c7'O
    File: CommonIP.ttcn [Line: 326]

    Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc437fb90002020c29fffe66b4c7'O
    File: CommonIP.ttcn [Line: 326]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 302
    text = Parameter: CommonIP.i = 8
    File: CommonIP.ttcn [Line: 302]

    Parameter: CommonIP.i = 8
    File: CommonIP.ttcn [Line: 302]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 291
    text = Parameter: CommonIP.v_IPv6AddrOct = ''O
    File: CommonIP.ttcn [Line: 291]

    Parameter: CommonIP.v_IPv6AddrOct = ''O
    File: CommonIP.ttcn [Line: 291]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 292
    text = Parameter: CommonIP.v_FieldCnt = 8
    File: CommonIP.ttcn [Line: 292]

    Parameter: CommonIP.v_FieldCnt = 8
    File: CommonIP.ttcn [Line: 292]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 293
    text = Parameter: CommonIP.v_EmptyBlocksExpanded = False
    File: CommonIP.ttcn [Line: 293]

    Parameter: CommonIP.v_EmptyBlocksExpanded = False
    File: CommonIP.ttcn [Line: 293]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 302
    text = Parameter: CommonIP.i = 0
    File: CommonIP.ttcn [Line: 302]

    Parameter: CommonIP.i = 0
    File: CommonIP.ttcn [Line: 302]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 303
    text = Parameter: CommonIP.v_Field = 'fd29'
    File: CommonIP.ttcn [Line: 303]

    Parameter: CommonIP.v_Field = 'fd29'
    File: CommonIP.ttcn [Line: 303]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 326
    text = Parameter: CommonIP.v_IPv6AddrOct = 'fd29'O
    File: CommonIP.ttcn [Line: 326]

    Parameter: CommonIP.v_IPv6AddrOct = 'fd29'O
    File: CommonIP.ttcn [Line: 326]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 302
    text = Parameter: CommonIP.i = 1
    File: CommonIP.ttcn [Line: 302]

    Parameter: CommonIP.i = 1
    File: CommonIP.ttcn [Line: 302]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 303
    text = Parameter: CommonIP.v_Field = 'cc43'
    File: CommonIP.ttcn [Line: 303]

    Parameter: CommonIP.v_Field = 'cc43'
    File: CommonIP.ttcn [Line: 303]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 326
    text = Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc43'O
    File: CommonIP.ttcn [Line: 326]

    Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc43'O
    File: CommonIP.ttcn [Line: 326]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 302
    text = Parameter: CommonIP.i = 2
    File: CommonIP.ttcn [Line: 302]

    Parameter: CommonIP.i = 2
    File: CommonIP.ttcn [Line: 302]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 303
    text = Parameter: CommonIP.v_Field = '7fb9'
    File: CommonIP.ttcn [Line: 303]

    Parameter: CommonIP.v_Field = '7fb9'
    File: CommonIP.ttcn [Line: 303]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 326
    text = Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc437fb9'O
    File: CommonIP.ttcn [Line: 326]

    Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc437fb9'O
    File: CommonIP.ttcn [Line: 326]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 302
    text = Parameter: CommonIP.i = 3
    File: CommonIP.ttcn [Line: 302]

    Parameter: CommonIP.i = 3
    File: CommonIP.ttcn [Line: 302]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 303
    text = Parameter: CommonIP.v_Field = '2'
    File: CommonIP.ttcn [Line: 303]

    Parameter: CommonIP.v_Field = '2'
    File: CommonIP.ttcn [Line: 303]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 317
    text = Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc437fb90002'O
    File: CommonIP.ttcn [Line: 317]

    Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc437fb90002'O
    File: CommonIP.ttcn [Line: 317]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 302
    text = Parameter: CommonIP.i = 4
    File: CommonIP.ttcn [Line: 302]

    Parameter: CommonIP.i = 4
    File: CommonIP.ttcn [Line: 302]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 303
    text = Parameter: CommonIP.v_Field = '20c'
    File: CommonIP.ttcn [Line: 303]

    Parameter: CommonIP.v_Field = '20c'
    File: CommonIP.ttcn [Line: 303]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 323
    text = Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc437fb90002020c'O
    File: CommonIP.ttcn [Line: 323]

    Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc437fb90002020c'O
    File: CommonIP.ttcn [Line: 323]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 302
    text = Parameter: CommonIP.i = 5
    File: CommonIP.ttcn [Line: 302]

    Parameter: CommonIP.i = 5
    File: CommonIP.ttcn [Line: 302]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 303
    text = Parameter: CommonIP.v_Field = '29ff'
    File: CommonIP.ttcn [Line: 303]

    Parameter: CommonIP.v_Field = '29ff'
    File: CommonIP.ttcn [Line: 303]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 326
    text = Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc437fb90002020c29ff'O
    File: CommonIP.ttcn [Line: 326]

    Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc437fb90002020c29ff'O
    File: CommonIP.ttcn [Line: 326]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 302
    text = Parameter: CommonIP.i = 6
    File: CommonIP.ttcn [Line: 302]

    Parameter: CommonIP.i = 6
    File: CommonIP.ttcn [Line: 302]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 303
    text = Parameter: CommonIP.v_Field = 'fe66'
    File: CommonIP.ttcn [Line: 303]

    Parameter: CommonIP.v_Field = 'fe66'
    File: CommonIP.ttcn [Line: 303]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 326
    text = Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc437fb90002020c29fffe66'O
    File: CommonIP.ttcn [Line: 326]

    Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc437fb90002020c29fffe66'O
    File: CommonIP.ttcn [Line: 326]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 302
    text = Parameter: CommonIP.i = 7
    File: CommonIP.ttcn [Line: 302]

    Parameter: CommonIP.i = 7
    File: CommonIP.ttcn [Line: 302]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 303
    text = Parameter: CommonIP.v_Field = 'b4c7'
    File: CommonIP.ttcn [Line: 303]

    Parameter: CommonIP.v_Field = 'b4c7'
    File: CommonIP.ttcn [Line: 303]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 326
    text = Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc437fb90002020c29fffe66b4c7'O
    File: CommonIP.ttcn [Line: 326]

    Parameter: CommonIP.v_IPv6AddrOct = 'fd29cc437fb90002020c29fffe66b4c7'O
    File: CommonIP.ttcn [Line: 326]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 302
    text = Parameter: CommonIP.i = 8
    File: CommonIP.ttcn [Line: 302]

    Parameter: CommonIP.i = 8
    File: CommonIP.ttcn [Line: 302]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 474
    text = Parameter: IMS_Procedures_Common.i = 1
    File: IMS_Procedures_Common.ttcn [Line: 474]

    Parameter: IMS_Procedures_Common.i = 1
    File: IMS_Procedures_Common.ttcn [Line: 474]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 213
    text = Parameter: CommonIP.v_FieldCnt = 1
    File: CommonIP.ttcn [Line: 213]

    Parameter: CommonIP.v_FieldCnt = 1
    File: CommonIP.ttcn [Line: 213]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 348
    text = Parameter: CommonIP.v_Addr1IsV6 = False
    File: CommonIP.ttcn [Line: 348]

    Parameter: CommonIP.v_Addr1IsV6 = False
    File: CommonIP.ttcn [Line: 348]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 213
    text = Parameter: CommonIP.v_FieldCnt = 1
    File: CommonIP.ttcn [Line: 213]

    Parameter: CommonIP.v_FieldCnt = 1
    File: CommonIP.ttcn [Line: 213]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 349
    text = Parameter: CommonIP.v_Addr2IsV6 = False
    File: CommonIP.ttcn [Line: 349]

    Parameter: CommonIP.v_Addr2IsV6 = False
    File: CommonIP.ttcn [Line: 349]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 474
    text = Parameter: IMS_Procedures_Common.i = 2
    File: IMS_Procedures_Common.ttcn [Line: 474]

    Parameter: IMS_Procedures_Common.i = 2
    File: IMS_Procedures_Common.ttcn [Line: 474]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 213
    text = Parameter: CommonIP.v_FieldCnt = 1
    File: CommonIP.ttcn [Line: 213]

    Parameter: CommonIP.v_FieldCnt = 1
    File: CommonIP.ttcn [Line: 213]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 348
    text = Parameter: CommonIP.v_Addr1IsV6 = False
    File: CommonIP.ttcn [Line: 348]

    Parameter: CommonIP.v_Addr1IsV6 = False
    File: CommonIP.ttcn [Line: 348]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 213
    text = Parameter: CommonIP.v_FieldCnt = 1
    File: CommonIP.ttcn [Line: 213]

    Parameter: CommonIP.v_FieldCnt = 1
    File: CommonIP.ttcn [Line: 213]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 349
    text = Parameter: CommonIP.v_Addr2IsV6 = False
    File: CommonIP.ttcn [Line: 349]

    Parameter: CommonIP.v_Addr2IsV6 = False
    File: CommonIP.ttcn [Line: 349]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 474
    text = Parameter: IMS_Procedures_Common.i = 3
    File: IMS_Procedures_Common.ttcn [Line: 474]

    Parameter: IMS_Procedures_Common.i = 3
    File: IMS_Procedures_Common.ttcn [Line: 474]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 213
    text = Parameter: CommonIP.v_FieldCnt = 1
    File: CommonIP.ttcn [Line: 213]

    Parameter: CommonIP.v_FieldCnt = 1
    File: CommonIP.ttcn [Line: 213]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 348
    text = Parameter: CommonIP.v_Addr1IsV6 = False
    File: CommonIP.ttcn [Line: 348]

    Parameter: CommonIP.v_Addr1IsV6 = False
    File: CommonIP.ttcn [Line: 348]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 213
    text = Parameter: CommonIP.v_FieldCnt = 1
    File: CommonIP.ttcn [Line: 213]

    Parameter: CommonIP.v_FieldCnt = 1
    File: CommonIP.ttcn [Line: 213]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 349
    text = Parameter: CommonIP.v_Addr2IsV6 = False
    File: CommonIP.ttcn [Line: 349]

    Parameter: CommonIP.v_Addr2IsV6 = False
    File: CommonIP.ttcn [Line: 349]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 474
    text = Parameter: IMS_Procedures_Common.i = 4
    File: IMS_Procedures_Common.ttcn [Line: 474]

    Parameter: IMS_Procedures_Common.i = 4
    File: IMS_Procedures_Common.ttcn [Line: 474]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 213
    text = Parameter: CommonIP.v_FieldCnt = 1
    File: CommonIP.ttcn [Line: 213]

    Parameter: CommonIP.v_FieldCnt = 1
    File: CommonIP.ttcn [Line: 213]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 348
    text = Parameter: CommonIP.v_Addr1IsV6 = False
    File: CommonIP.ttcn [Line: 348]

    Parameter: CommonIP.v_Addr1IsV6 = False
    File: CommonIP.ttcn [Line: 348]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 213
    text = Parameter: CommonIP.v_FieldCnt = 1
    File: CommonIP.ttcn [Line: 213]

    Parameter: CommonIP.v_FieldCnt = 1
    File: CommonIP.ttcn [Line: 213]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\CommonIP\CommonIP.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 349
    text = Parameter: CommonIP.v_Addr2IsV6 = False
    File: CommonIP.ttcn [Line: 349]

    Parameter: CommonIP.v_Addr2IsV6 = False
    File: CommonIP.ttcn [Line: 349]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Procedures_Common.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 474
    text = Parameter: IMS_Procedures_Common.i = 5
    File: IMS_Procedures_Common.ttcn [Line: 474]

    Parameter: IMS_Procedures_Common.i = 5
    File: IMS_Procedures_Common.ttcn [Line: 474]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 764
    text = Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 764]

    Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 764]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 790
    text = Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 790]

    Parameter: IMS_Component.i = 0
    File: IMS_Component.ttcn [Line: 790]

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\IMS\IMS_Component.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 1785
    text = Parameter: IMS_Component.vc_IMS_Global.Ctrl.TestBody = False

    Parameter: IMS_Component.vc_IMS_Global.Ctrl.TestBody = False

    timerEvent = 6
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\Common\CommonDefs.ttcn
    testName = TC_7_34_NR5GC
    lineNo = 592
    outStr = Timer: t_Delay, Duration: 2s, Started: 06:16:48

    Timer: t_Delay, Duration: 2s, Started: 06:16:48

    timerEvent = 9
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\Common\CommonDefs.ttcn
    testName = TC_7_34_NR5GC
    lineNo = 593
    outStr = Timer: t_Delay, Expired: 06:16:50

    Timer: t_Delay, Expired: 06:16:50

    IMS_IPCAN_Coordination_MSG
    	IMS_IPCAN_Command
    		Name = IPCAN_ENDPROCEDURE (2)
    		TestConfiguration = Omit
    		TestProcedure = IPCAN_MT_SpeechCall (5)

    Inter-component message: IMS -> NR5GC:IMS

    summary = Message Mismatch: IntegerType
    MATCH_MISMATCH
    	Message Mismatch: IntegerType
    		DRB_Id = 1

    Message Mismatch: IntegerType

    summary = Message Mismatch: IntegerType
    MATCH_MISMATCH
    	Message Mismatch: IntegerType
    		DRB_Id = 1

    Message Mismatch: IntegerType

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		RadioBearerList
    			NR_RadioBearer_Type
    				Id
    					Drb = 2
    				Config
    					Release = True

    Sent from port: NR5GC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		RadioBearerList = True

    Received on port: NR5GC:SYS

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		PdcpCount
    			Get
    				AllRBs = True

    Sent from port: NR5GC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		PdcpCount
    			Get
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 1
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000100'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000011'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 2
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000001'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Drb = 1
    					UL
    						Format = PdcpCount_DrbSQN18 (2)
    						Value = 00000000000000000000000000001110'B
    					DL
    						Format = PdcpCount_DrbSQN18 (2)
    						Value = 00000000000000000000000000001010'B

    Received on port: NR5GC:SYS

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		AS_Security
    			StartRestart
    				Integrity
    					Algorithm = nia1 (1)
    					KRRCint = 00101001100010110011010001010110001111010010001011110010001110001110000100011000110111100001110001100101110010011000110010011010'B
    					KUPint = 11101010000101100010000110111100010100011100111001000100001110100101010011110010010001110000101101100000000010001011101110001000'B
    					ActTimeList = Omit
    				Ciphering
    					Algorithm = nea1 (1)
    					KRRCenc = 01100000011100001110000011111001100101001101110111110011110011011000001001101010010011110101010110110111110011110001001101100101'B
    					KUPenc = 10110100110101011001010100010011000010111101110001001101100100110001100011110001100001111010110000001001011000110101001000100010'B
    					ActTimeList
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Srb = 1
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 4
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 3
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Srb = 2
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 1
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 0
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Drb = 1
    							UL
    								SQN
    									Format = PdcpCount_DrbSQN18 (2)
    									Value = 14
    							DL
    								SQN
    									Format = PdcpCount_DrbSQN18 (2)
    									Value = 10

    Sent from port: NR5GC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		AS_Security = True

    Received on port: NR5GC:SYS

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcReconfiguration
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcReconfiguration
    									radioBearerConfig
    										srb_ToAddModList = Omit
    										srb3_ToRelease = Omit
    										drb_ToAddModList = Omit
    										drb_ToReleaseList
    											DRB_Identity = 2
    										securityConfig = Omit
    									secondaryCellGroup = Omit
    									measConfig = Omit
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension
    										masterCellGroup = '200040'O
    										fullConfig = Omit
    										dedicatedNAS_MessageList = Omit
    										masterKeyUpdate = Omit
    										dedicatedSIB1_Delivery = Omit
    										dedicatedSystemInformationDelivery = Omit
    										otherConfig = Omit
    										nonCriticalExtension = Omit
    		Nas
    			NG_NAS_MSG_Request_Type
    				SecurityProtection
    					Status = 0010'B
    					ForceMacError = False
    				Pdu
    					Msg
    						dl_Nas_Transport
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01101000'B
    							spareHalfOctet2 = '0'H
    							payloadContainerType
    								iei = Omit
    								container = 0001'B
    							payload
    								iei = Omit
    								iel = '0000'O
    								payload = ''O
    							pduSessionId
    								iei = '12'O
    								sessionId = '01'O
    							additionalInfo = Omit
    							gmmCause = Omit
    							backOffTimerValue = Omit
    					PiggybackedPduList
    						NG_NAS_DL_Pdu_Type
    							Msg
    								pdu_Session_Modification_Command
    									protocolDiscriminator = 00101110'B
    									pduSessionId
    										iei = Omit
    										sessionId = '01'O
    									procedureTransactionIdentifier = '00'O
    									messageType = 11001011'B
    									gsmCause = Omit
    									sessionAMBR = Omit
    									rqTimerValue = Omit
    									alwaysOnPDUSessionInd = Omit
    									authorizedQoSRules
    										iei = '7A'O
    										iel = '0004'O
    										listofQoSRules
    											QoS_Rule
    												identifier = '03'O
    												iel = '0001'O
    												ruleOperationCode = 010'B
    												dqrBit = 0'B
    												numOfPacketFilters = 0000'B
    												packetFilterList = Omit
    												precedence = Omit
    												spare = Omit
    												segregation = Omit
    												flowIdentifier = Omit
    									mappedEPSContexts = Omit
    									authorizedQoSFlowDescr
    										iei = '79'O
    										iel = '0003'O
    										listofFlows
    											QoS_Flow
    												spare2 = 00'B
    												qfi = 000111'B
    												operationCode = 010'B
    												spare6 = 000000'B
    												eBit = 0'B
    												numOfParameters = 000000'B
    												parameterList = Omit
    									extdProtocolConfigurationOptions = Omit
    									atsssContainer = Omit
    									ipHeaderCompressionConfig = Omit
    									portManagementInfoContainer = Omit
    									servingPLMNRateControl = Omit
    									ethernetHeaderCompressConfig = Omit
    							PiggybackedPduList = Omit

    Inter-component message: TC_SRB -> NASEMU_NRNG:TC_SRB

    PDU SESSION MODIFICATION COMMAND
    	Extended protocol discriminator = 0x2E [ 46 ]
    	pdu_sesn_id [8 bits] = 0x1 [ 1 ]
    	pti [8 bits] = 0x0 [ 0 ]
    	pdu_sesn_modification_cmd_msg_id [8 bits] = 0xCB [ 203 ]
    	authorized_qos_rule
    		iei [8 bits] = 0x7A [ 122 ]
    		qriel [16 bits] = 0x4 [ 4 ]
    		qiei [8 bits] = 0x3 [ 3 ]
    		qiel [16 bits] = 0x1 [ 1 ]
    		rule_op_code [3 bits] = 0x2 [ 2 ]
    		dqr_bit [1 bit] = 0x0 [ 0 ]
    		numof_pack_flt [4 bits] = 0x0 [ 0 ]
    	authorized_qos_flow
    		iei [8 bits] = 0x79 [ 121 ]
    		auiel [16 bits] = 0x3 [ 3 ]
    		Spare bits [2 bits] = 0x0 [ 0 ]
    		qfi [6 bits] = 0x7 [ 7 ]
    		opn_cod [3 bits] = 0x2 [ 2 ]
    		spar [5 bits] = 0x0 [ 0 ]
    		spare_1 [1 bit] = 0x0 [ 0 ]
    		e [1 bit] = 0x0 [ 0 ]
    		numof_par [6 bits] = 0x0 [ 0 ]

    PDU SESSION MODIFICATION COMMAND PDU

    DL NAS TRANSPORT
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Spare half octet [4 bits] = 0x0 [ 0 ]
    	Message Type [8 bits] = 0x68 [ 104 ]
    	sht2 [4 bits] = 0x0 [ 0 ]
    	payload_typ
    		val [4 bits] = 0x1 [ 1 ]
    	payload_cont
    		iel [16 bits] = 0x11 [ 17 ]
    		val = 0x2E0100CB7A000403000140790003074000
    	pdu_sess_id
    		iei [8 bits] = 0x12 [ 18 ]
    		val = 0x01 [ 1 ]

    DL NAS TRANSPORT PDU

    DL-DCCH-Message
    	message = c1 = rrcReconfiguration =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcReconfiguration =
    			radioBearerConfig
    				drb-ToReleaseList = SEQUENCE OF DRB-Identity
    					DRB-Identity(1) = 2
    			nonCriticalExtension
    				masterCellGroup = CONTAINING =
    					cellGroupId = 0
    					rlc-BearerToReleaseList = SEQUENCE OF LogicalChannelIdentity
    						LogicalChannelIdentity(1) = 5
    				dedicatedNAS-MessageList = SEQUENCE OF DedicatedNAS-Message
    					DedicatedNAS-Message(1) = 7E02F7672F0406F8F4657F21E705774452566A9CF13D01916226B033DD7CC6FA

    rrcReconfiguration

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcReconfiguration
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcReconfiguration
    								radioBearerConfig
    									srb_ToAddModList = Omit
    									srb3_ToRelease = Omit
    									drb_ToAddModList = Omit
    									drb_ToReleaseList
    										DRB_Identity = 2
    									securityConfig = Omit
    								secondaryCellGroup = Omit
    								measConfig = Omit
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension
    									masterCellGroup = '200040'O
    									fullConfig = Omit
    									dedicatedNAS_MessageList
    										NG_NAS_Message = '7E02F7672F0406F8F4657F21E705774452566A9CF13D01916226B033DD7CC6FA'O
    									masterKeyUpdate = Omit
    									dedicatedSIB1_Delivery = Omit
    									dedicatedSystemInformationDelivery = Omit
    									otherConfig = Omit
    									nonCriticalExtension = Omit

    Sent from port: NASEMU_NRNG:SYS_SRB

    UL-DCCH-Message
    	message = c1 = rrcReconfigurationComplete =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcReconfigurationComplete =

    rrcReconfigurationComplete

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 11
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcReconfigurationComplete
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcReconfigurationComplete
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Received on port: NASEMU_NRNG:SYS_SRB

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 11
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcReconfigurationComplete
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcReconfigurationComplete
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: SRB -> NR5GC:SRB

    UL-DCCH-Message
    	message = c1 = ulInformationTransfer =
    		criticalExtensions = ulInformationTransfer =
    			dedicatedNAS-Message = 7E02BA790C980626498C171401B4B11207CA7B

    ulInformationTransfer

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 2
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 12
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ulInformationTransfer
    						criticalExtensions
    							ulInformationTransfer
    								dedicatedNAS_Message = '7E02BA790C980626498C171401B4B11207CA7B'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Received on port: NASEMU_NRNG:SYS_SRB

    PDU SESSION MODIFICATION COMPLETE
    	Extended protocol discriminator = 0x2E [ 46 ]
    	pdu_sesn_id [8 bits] = 0x1 [ 1 ]
    	pti [8 bits] = 0x0 [ 0 ]
    	pdu_sesn_modification_cmp_msg_id [8 bits] = 0xCC [ 204 ]

    PDU SESSION MODIFICATION COMPLETE PDU

    UL NAS TRANSPORT
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Spare half octet [4 bits] = 0x0 [ 0 ]
    	Message Type [8 bits] = 0x67 [ 103 ]
    	payload_typ
    		val [4 bits] = 0x0 [ 0 ]
    	shoct2 [4 bits] = 0x1 [ 1 ]
    	payload_cont
    		iel [16 bits] = 0x4 [ 4 ]
    		val = 0x2E0100CC [ 771817676 ]
    	pdu_sess_id
    		iei [8 bits] = 0x12 [ 18 ]
    		val = 0x01 [ 1 ]

    UL NAS TRANSPORT PDU

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 2
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 12
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0010'B
    					NasCount = '00000006'O
    				Pdu
    					Msg
    						ul_Nas_Transport
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01100111'B
    							spareHalfOctet2 = '0'H
    							payloadContainerType
    								iei = Omit
    								container = 0001'B
    							payload
    								iei = Omit
    								iel = '0004'O
    								payload = '2E0100CC'O
    							pduSessionId
    								iei = '12'O
    								sessionId = '01'O
    							oldPDUSessionId = Omit
    							requestType = Omit
    							s_NSSAI = Omit
    							dnn = Omit
    							additionalInfo = Omit
    							maPDUSessionInfo = Omit
    							releaseAssistanceInd = Omit
    					PiggybackedPduList
    						NG_NAS_UL_Pdu_Type
    							Msg
    								pdu_Session_Modification_Complete
    									protocolDiscriminator = 00101110'B
    									pduSessionId
    										iei = Omit
    										sessionId = '01'O
    									procedureTransactionIdentifier = '00'O
    									messageType = 11001100'B
    									extdProtocolConfigurationOptions = Omit
    									portManagementInfoContainer = Omit
    							PiggybackedPduList = Omit

    Inter-component message: SRB -> NR5GC:SRB

    IP_ConfigReq_Type
    	ExplicitRouting
    		Remove
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '1.2.1.10'
    				Port = 60350
    			Remote = Omit

    Inter-component message: NR_CTRL -> IP:NR_CTRL

    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V4.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V4.Addr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 53
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr.V4.Addr

    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V4.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V4.Addr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 67
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr.V4.Addr

    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V4.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V4.Addr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr.V4.Addr

    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5062
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5062
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5061
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5062
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5062
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5061
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '1.2.1.10'
    					Port = 60351
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 7
    			DataMode = loopbackRTCP (2)
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = '2002:0db8:0000:0000:0000:0000:1428:5720'
    							ScopeId = Omit
    					Port = 60350
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 7
    			DataMode = loopbackRTP (1)
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = '2002:0db8:0000:0000:0000:0000:1428:5720'
    							ScopeId = Omit
    					Port = 60351
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 7
    			DataMode = loopbackRTCP (2)

    Sent from port: IP:IP_CTRL

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    Received on port: IP:IP_CTRL

    IP_Indication_Type
    	Cnf = True

    Inter-component message: IP -> NR5GC:IP

    IP_ConfigReq_Type
    	ExplicitRouting
    		Remove
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '1.2.1.10'
    				Port = 60351
    			Remote = Omit

    Inter-component message: NR_CTRL -> IP:NR_CTRL

    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V4.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V4.Addr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 53
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr.V4.Addr

    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V4.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V4.Addr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 67
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr.V4.Addr

    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V4.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V4.Addr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr.V4.Addr

    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5062
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5062
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5061
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5062
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5062
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5061
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = '2002:0db8:0000:0000:0000:0000:1428:5720'
    							ScopeId = Omit
    					Port = 60350
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 7
    			DataMode = loopbackRTP (1)
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = '2002:0db8:0000:0000:0000:0000:1428:5720'
    							ScopeId = Omit
    					Port = 60351
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 7
    			DataMode = loopbackRTCP (2)

    Sent from port: IP:IP_CTRL

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    Received on port: IP:IP_CTRL

    IP_Indication_Type
    	Cnf = True

    Inter-component message: IP -> NR5GC:IP

    IP_ConfigReq_Type
    	ExplicitRouting
    		Remove
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = '2002:0db8:0000:0000:0000:0000:1428:5720'
    						ScopeId = Omit
    				Port = 60350
    			Remote = Omit

    Inter-component message: NR_CTRL -> IP:NR_CTRL

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '2002:0db8:0000:0000:0000:0000:1428:5720'
    					ScopeId = Omit
    			Port = 60350
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '2002:0db8:0000:0000:0000:0000:1428:5720'
    					ScopeId = Omit
    			Port = 60350
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '2002:0db8:0000:0000:0000:0000:1428:5720'
    					ScopeId = Omit
    			Port = 60350
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '2002:0db8:0000:0000:0000:0000:1428:5720'
    					ScopeId = Omit
    			Port = 60350
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5062
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr

    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5062
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5061
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5062
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5062
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5061
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = '2002:0db8:0000:0000:0000:0000:1428:5720'
    							ScopeId = Omit
    					Port = 60351
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 7
    			DataMode = loopbackRTCP (2)

    Sent from port: IP:IP_CTRL

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    Received on port: IP:IP_CTRL

    IP_Indication_Type
    	Cnf = True

    Inter-component message: IP -> NR5GC:IP

    IP_ConfigReq_Type
    	ExplicitRouting
    		Remove
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = '2002:0db8:0000:0000:0000:0000:1428:5720'
    						ScopeId = Omit
    				Port = 60351
    			Remote = Omit

    Inter-component message: NR_CTRL -> IP:NR_CTRL

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '2002:0db8:0000:0000:0000:0000:1428:5720'
    					ScopeId = Omit
    			Port = 60351
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '2002:0db8:0000:0000:0000:0000:1428:5720'
    					ScopeId = Omit
    			Port = 60351
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '2002:0db8:0000:0000:0000:0000:1428:5720'
    					ScopeId = Omit
    			Port = 60351
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '2002:0db8:0000:0000:0000:0000:1428:5720'
    					ScopeId = Omit
    			Port = 60351
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5062
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr

    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5062
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5061
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5062
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5062
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5061
    				Remote = Omit
    			DRB
    				Nr5GC
    					CellId = nr_Cell1 (1)
    					QosFlow
    						PDU_SessionId = 1
    						QFI = 2
    			DataMode = Omit

    Sent from port: IP:IP_CTRL

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    Received on port: IP:IP_CTRL

    IP_Indication_Type
    	Cnf = True

    Inter-component message: IP -> NR5GC:IP

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		EnquireTiming = True

    Sent from port: NR5GC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 25
    				Subframe
    					Number = 0
    				HSFN
    					Number = 92
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		Result
    			Success = True
    	Confirm
    		EnquireTiming = True

    Received on port: NR5GC:SYS

    timerEvent = 6
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\NR5GC\NR5GC_RRCSteps.ttcn
    testName = TC_7_34_NR5GC
    lineNo = 326
    outStr = Timer: t_Timer, Duration: 1.22s, Started: 06:16:50

    Timer: t_Timer, Duration: 1.22s, Started: 06:16:50

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 55
    				Subframe
    					Number = 2
    				HSFN
    					Number = 92
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcRelease
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcRelease
    									redirectedCarrierInfo = Omit
    									cellReselectionPriorities = Omit
    									suspendConfig = Omit
    									deprioritisationReq = Omit
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: TC_SRB -> NASEMU_NRNG:TC_SRB

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		PdcpCount
    			Get
    				AllRBs = True

    Sent from port: NR5GC:SYS

    DL-DCCH-Message
    	message = c1 = rrcRelease =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcRelease =

    rrcRelease

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 55
    				Subframe
    					Number = 2
    				HSFN
    					Number = 92
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcRelease
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcRelease
    								redirectedCarrierInfo = Omit
    								cellReselectionPriorities = Omit
    								suspendConfig = Omit
    								deprioritisationReq = Omit
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Sent from port: NASEMU_NRNG:SYS_SRB

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		PdcpCount
    			Get
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 1
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000101'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000100'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 2
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000010'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Drb = 1
    					UL
    						Format = PdcpCount_DrbSQN18 (2)
    						Value = 00000000000000000000000000001110'B
    					DL
    						Format = PdcpCount_DrbSQN18 (2)
    						Value = 00000000000000000000000000001010'B

    Received on port: NR5GC:SYS

    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 55
    			Subframe
    				Number = 2
    			HSFN
    				Number = 92
    			Slot
    				SlotOffset
    					Numerology1 = 0

    Message Mismatch: TimingInfo_Type

    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 55
    			Subframe
    				Number = 2
    			HSFN
    				Number = 92
    			Slot
    				SlotOffset
    					Numerology1 = 0

    Message Mismatch: TimingInfo_Type

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 55
    				Subframe
    					Number = 2
    				HSFN
    					Number = 92
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		Cell
    			AddOrReconfigure
    				StaticResourceConfig = Omit
    				CellConfigCommon = Omit
    				PhysicalLayer = Omit
    				BcchConfig = Omit
    				PcchConfig = Omit
    				RachProcedureConfig = Omit
    				DcchDtchConfig
    					DL = Omit
    					UL
    						SearchSpaceAndDci
    							AssignedBWPs = Omit
    							SearchSpaceType = Omit
    							DciInfo = Omit
    						PUCCH_Synch
    							None = True
    						GrantConfig
    							None = True
    					DrxCtrl = Omit
    					MeasGapCtrl = Omit
    				ServingCellConfig = Omit

    Sent from port: NR5GC:SYS

    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 55
    			Subframe
    				Number = 7
    			HSFN
    				Number = 92
    			Slot
    				SlotOffset
    					Numerology1 = 0

    Message Mismatch: TimingInfo_Type

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 55
    				Subframe
    					Number = 7
    				HSFN
    					Number = 92
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		AS_Security
    			Release = True

    Sent from port: NR5GC:SYS

    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 60
    			Subframe
    				Number = 7
    			HSFN
    				Number = 92
    			Slot
    				SlotOffset
    					Numerology1 = 0

    Message Mismatch: TimingInfo_Type

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 60
    				Subframe
    					Number = 7
    				HSFN
    					Number = 92
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		RadioBearerList
    			NR_RadioBearer_Type
    				Id
    					Srb = 1
    				Config
    					Release = True
    			NR_RadioBearer_Type
    				Id
    					Srb = 2
    				Config
    					Release = True
    			NR_RadioBearer_Type
    				Id
    					Drb = 1
    				Config
    					Release = True

    Sent from port: NR5GC:SYS

    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 61
    			Subframe
    				Number = 2
    			HSFN
    				Number = 92
    			Slot
    				SlotOffset
    					Numerology1 = 0

    Message Mismatch: TimingInfo_Type

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 61
    				Subframe
    					Number = 2
    				HSFN
    					Number = 92
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		RadioBearerList
    			NR_RadioBearer_Type
    				Id
    					Srb = 1
    				Config
    					AddOrReconfigure
    						Sdap
    							None = True
    						Pdcp
    							RBTerminating
    								RbConfig
    									Params
    										Rb
    											Srb = True
    								LinkToOtherCellGroup
    									None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										AM
    											Tx
    												R15
    													sn_FieldLength = size12 (0)
    													t_PollRetransmit = ms45 (8)
    													pollPDU = infinity_ (23)
    													pollByte = infinity_ (43)
    													maxRetxThreshold = t8 (5)
    											Rx
    												R15
    													sn_FieldLength = size12 (0)
    													t_Reassembly = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    									TestMode
    										None = True
    								LogicalChannelId = 1
    								Mac
    									LogicalChannel
    										Priority = 1
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit
    			NR_RadioBearer_Type
    				Id
    					Srb = 2
    				Config
    					AddOrReconfigure
    						Sdap
    							None = True
    						Pdcp
    							RBTerminating
    								RbConfig
    									Params
    										Rb
    											Srb = True
    								LinkToOtherCellGroup
    									None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										AM
    											Tx
    												R15
    													sn_FieldLength = size12 (0)
    													t_PollRetransmit = ms45 (8)
    													pollPDU = infinity_ (23)
    													pollByte = infinity_ (43)
    													maxRetxThreshold = t8 (5)
    											Rx
    												R15
    													sn_FieldLength = size12 (0)
    													t_Reassembly = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    									TestMode
    										None = True
    								LogicalChannelId = 2
    								Mac
    									LogicalChannel
    										Priority = 3
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit

    Sent from port: NR5GC:SYS

    timerEvent = 9
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\NR5GC\NR5GC_RRCSteps.ttcn
    testName = TC_7_34_NR5GC
    lineNo = 334
    outStr = Timer: t_Timer, Expired: 06:16:51

    Timer: t_Timer, Expired: 06:16:51

    IMS_IPCAN_Coordination_MSG
    	TriggerEvent = True

    Inter-component message: IPCAN -> IMS1:IPCAN

    IMS_IPCAN_Coordination_MSG
    	IMS_IPCAN_Command
    		Name = IPCAN_RELEASE (3)
    		TestConfiguration = Omit
    		TestProcedure = Omit

    Inter-component message: IMS -> NR5GC:IMS

    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = CNF_REQUIRED (1)

    Message Mismatch: Ut_CnfReq_Type

    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = LOCAL_CNF_REQUIRED (2)

    Message Mismatch: Ut_CnfReq_Type

    UT_COMMON_CMD
    	Cmd = SWITCH_OFF (119)
    	CnfReq = NO_CNF_REQUIRED (0)
    	ParameterList = Omit

    Inter-component message: PTC_Ut -> MTC_IMS:PTC_Ut

    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = CNF_REQUIRED (1)

    Message Mismatch: Ut_CnfReq_Type

    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = LOCAL_CNF_REQUIRED (2)

    Message Mismatch: Ut_CnfReq_Type

    Sender = RequestServer
    Text = Request received [!SWITCH_OFF]

    RequestServer:Request received [!SWITCH_OFF]

    Sender = RequestServer
    Text = [!SWITCH_OFF] Started

    RequestServer:[!SWITCH_OFF] Started

    UT_SYSTEM_REQ
    	Cmd
    		MMI
    			Cmd = 'SWITCH_OFF'
    			ParameterList = Omit
    	CnfRequired = NO_CNF_REQUIRED (0)

    Sent from port: MTC_IMS:Ut

    Sender = RequestServer
    Text = Received !SWITCH_OFF from SAT Controller PC

    RequestServer:Received !SWITCH_OFF from SAT Controller PC

    Sender = SAT Controller PC
    Text = Sent "!OK"

    SAT Controller PC:Sent "!OK"

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		Cell
    			AddOrReconfigure
    				StaticResourceConfig = Omit
    				CellConfigCommon = Omit
    				PhysicalLayer = Omit
    				BcchConfig = Omit
    				PcchConfig = Omit
    				RachProcedureConfig = Omit
    				DcchDtchConfig
    					DL = Omit
    					UL
    						SearchSpaceAndDci
    							AssignedBWPs = Omit
    							SearchSpaceType = Omit
    							DciInfo
    								ResoureAssignment
    									ResourceAllocationType = Omit
    									FreqDomain
    										FirstRbIndex = 0
    										Nprb = 24
    									TimeDomain = Omit
    									TransportBlockScheduling
    										NR_TransportBlockSingleTransmission_Type
    											TimingOffset
    												None = True
    											ImcsValue = 9
    											RedundancyVersion = 0
    											ToggleNDI = True
    									HarqProcessConfig = Omit
    								PuschHoppingCtrl = Omit
    								TpcCommandPusch = Omit
    								UL_SUL_Indicator = Omit
    								Format = Omit
    						PUCCH_Synch
    							None = True
    						GrantConfig
    							OnSR_Reception = True
    					DrxCtrl = Omit
    					MeasGapCtrl = Omit
    				ServingCellConfig = Omit

    Sent from port: NR5GC:SYS

    Sender = !SWITCH_OFF
    Text = Sending AT+CFUN=0

    !SWITCH_OFF:Sending AT+CFUN=0

    Sender = Device Under Test
    Text = Sent "AT+CFUN=0"

    Device Under Test:Sent "AT+CFUN=0"

    Sender = RequestServer
    Text = Received AT+CFUN=0 from Device Under Test

    RequestServer:Received AT+CFUN=0 from Device Under Test

    UL-CCCH-Message
    	message = c1 = rrcSetupRequest =
    		rrcSetupRequest
    			ue-Identity = ng-5G-S-TMSI-Part1 = 100000111000010001101000101011001111000
    			establishmentCause = mo-Data
    			spare = 0

    rrcSetupRequest

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 0
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 362
    				Subframe
    					Number = 9
    				HSFN
    					Number = 92
    				Slot
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Ccch
    			message_
    				c1
    					rrcSetupRequest
    						rrcSetupRequest
    							ue_Identity
    								ng_5G_S_TMSI_Part1 = 100000111000010001101000101011001111000'B
    							establishmentCause = mo_Data (4)
    							spare = 0'B

    Received on port: NASEMU_NRNG:SYS_SRB

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 0
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 362
    				Subframe
    					Number = 9
    				HSFN
    					Number = 92
    				Slot
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Ccch
    				message_
    					c1
    						rrcSetupRequest
    							rrcSetupRequest
    								ue_Identity
    									ng_5G_S_TMSI_Part1 = 100000111000010001101000101011001111000'B
    								establishmentCause = mo_Data (4)
    								spare = 0'B
    		Nas = Omit

    Inter-component message: SRB -> NR5GC:SRB

    SERVICE REQUEST
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Spare half octet [4 bits] = 0x0 [ 0 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Message Type [8 bits] = 0x4C [ 76 ]
    	ser_typ
    		Value [4 bits] = 0x1 [ 1 ]
    	sr_ngksi
    		Type of security context flag [1 bit] = 0x0 [ 0 ]
    		key sequence indicator [3 bits] = 0x0 [ 0 ]
    	fiveg_s_tmsi
    		length [16 bits] = 0x7 [ 7 ]
    		id_dig [4 bits] = 0xF [ 15 ]
    		Spare bits [1 bit] = 0x0 [ 0 ]
    		typ_id [3 bits] = 0x4 [ 4 ]
    		amf_set_id = 0x00 [ 0 ]
    		amf_set_id_cont [2 bits] = 0x1 [ 1 ]
    		amf_pntr [6 bits] = 0x1 [ 1 ]
    		fiveg_tmsi = 0xC23456 [ 12727382 ]

    SERVICE REQUEST PDU

    UL-DCCH-Message
    	message = c1 = rrcSetupComplete =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcSetupComplete =
    			selectedPLMN-Identity = 1
    			dedicatedNAS-Message = 7E01D09DBEDC077E004C100007F40041C234567871001572EEDCC411219FB68681079A0CC2D56F12E5650FBB
    			ng-5G-S-TMSI-Value = ng-5G-S-TMSI-Part2 = 000000000

    rrcSetupComplete

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 365
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcSetupComplete
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcSetupComplete
    								selectedPLMN_Identity = 1
    								registeredAMF = Omit
    								guami_Type = Omit
    								s_NSSAI_List = Omit
    								dedicatedNAS_Message = '7E01D09DBEDC077E004C100007F40041C234567871001572EEDCC411219FB68681079A0CC2D56F12E5650FBB'O
    								ng_5G_S_TMSI_Value
    									ng_5G_S_TMSI_Part2 = 000000000'B
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Received on port: NASEMU_NRNG:SYS_SRB

    SERVICE REQUEST
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Spare half octet [4 bits] = 0x0 [ 0 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Message Type [8 bits] = 0x4C [ 76 ]
    	ser_typ
    		Value [4 bits] = 0x1 [ 1 ]
    	sr_ngksi
    		Type of security context flag [1 bit] = 0x0 [ 0 ]
    		key sequence indicator [3 bits] = 0x0 [ 0 ]
    	fiveg_s_tmsi
    		length [16 bits] = 0x7 [ 7 ]
    		id_dig [4 bits] = 0xF [ 15 ]
    		Spare bits [1 bit] = 0x0 [ 0 ]
    		typ_id [3 bits] = 0x4 [ 4 ]
    		amf_set_id = 0x00 [ 0 ]
    		amf_set_id_cont [2 bits] = 0x1 [ 1 ]
    		amf_pntr [6 bits] = 0x1 [ 1 ]
    		fiveg_tmsi = 0xC23456 [ 12727382 ]

    SERVICE REQUEST PDU

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 365
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcSetupComplete
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcSetupComplete
    									selectedPLMN_Identity = 1
    									registeredAMF = Omit
    									guami_Type = Omit
    									s_NSSAI_List = Omit
    									dedicatedNAS_Message = '7E01D09DBEDC077E004C100007F40041C234567871001572EEDCC411219FB68681079A0CC2D56F12E5650FBB'O
    									ng_5G_S_TMSI_Value
    										ng_5G_S_TMSI_Part2 = 000000000'B
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0001'B
    					NasCount = '00000007'O
    				Pdu
    					Msg
    						service_Request
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01001100'B
    							serviceType = 0001'B
    							ngKSI
    								iei = Omit
    								tsc = 0'B
    								nasKeySetId = 000'B
    							s_TMSI
    								iei = Omit
    								iel = '0007'O
    								idDigit1 = 1111'B
    								oddEvenInd = 0'B
    								typeOfId = 100'B
    								otherDigits = '0041C2345678'O
    							ulDataStatus = Omit
    							pduSessionStatus = Omit
    							allowedPDUSessionStatus = Omit
    							nasMsg
    								iei = '71'O
    								iel = '0015'O
    								replayedNASMsgContainerValue = '72EEDCC411219FB68681079A0CC2D56F12E5650FBB'O
    					PiggybackedPduList
    						NG_NAS_UL_Pdu_Type
    							Msg
    								service_Request
    									protocolDiscriminator = 01111110'B
    									spareHalfOctet = '0'H
    									securityHeaderType = 0000'B
    									messageType = 01001100'B
    									serviceType = 0001'B
    									ngKSI
    										iei = Omit
    										tsc = 0'B
    										nasKeySetId = 000'B
    									s_TMSI
    										iei = Omit
    										iel = '0007'O
    										idDigit1 = 1111'B
    										oddEvenInd = 0'B
    										typeOfId = 100'B
    										otherDigits = '0041C2345678'O
    									ulDataStatus
    										iei = '40'O
    										iel = '02'O
    										psi0_7 = 00000010'B
    										psi8_15 = 00000000'B
    										spare = Omit
    									pduSessionStatus
    										iei = '50'O
    										iel = '02'O
    										psi0_7 = 00000010'B
    										psi8_15 = 00000000'B
    										spare = Omit
    									allowedPDUSessionStatus = Omit
    									nasMsg = Omit
    							PiggybackedPduList = Omit

    Inter-component message: SRB -> NR5GC:SRB

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		Cell
    			AddOrReconfigure
    				StaticResourceConfig = Omit
    				CellConfigCommon = Omit
    				PhysicalLayer = Omit
    				BcchConfig = Omit
    				PcchConfig = Omit
    				RachProcedureConfig = Omit
    				DcchDtchConfig
    					DL = Omit
    					UL
    						SearchSpaceAndDci
    							AssignedBWPs = Omit
    							SearchSpaceType = Omit
    							DciInfo = Omit
    						PUCCH_Synch
    							Auto
    								TimingAdvance = 31
    								TA_Period = 600
    						GrantConfig = Omit
    					DrxCtrl = Omit
    					MeasGapCtrl = Omit
    				ServingCellConfig = Omit

    Sent from port: NR5GC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		Cell = True

    Received on port: NR5GC:SYS

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		PdcpCount
    			Get
    				AllRBs = True

    Sent from port: NR5GC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		PdcpCount
    			Get
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 1
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000001'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 2
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B

    Received on port: NR5GC:SYS

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		AS_Security
    			StartRestart
    				Integrity
    					Algorithm = nia1 (1)
    					KRRCint = 11010001100110000000111100001011111110110000000011101111001011101011111001100011011111100100010100110111110110101100101110011011'B
    					KUPint = 00110010110010010000001000000101110010000010101001101111111011011001100010010001011101001110010001101101010000011111001111111110'B
    					ActTimeList = Omit
    				Ciphering
    					Algorithm = nea1 (1)
    					KRRCenc = 01001001000011010111000100101000001000100000011100011000010001101110000000101100001000100001001110101000010111101111101001010110'B
    					KUPenc = 01100000010000010010101100111011100000110001000000010010111010100001010101011100111011110111000111001000001010000101010110000101'B
    					ActTimeList
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Srb = 1
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 2
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 1
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Srb = 2
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 0
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 0

    Sent from port: NR5GC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		AS_Security = True

    Received on port: NR5GC:SYS

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						securityModeCommand
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								securityModeCommand
    									securityConfigSMC
    										securityAlgorithmConfig
    											cipheringAlgorithm = nea1 (1)
    											integrityProtAlgorithm = nia1 (1)
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: TC_SRB -> NASEMU_NRNG:TC_SRB

    DL-DCCH-Message
    	message = c1 = securityModeCommand =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = securityModeCommand =
    			securityConfigSMC
    				securityAlgorithmConfig
    					cipheringAlgorithm = nea1
    					integrityProtAlgorithm = nia1

    securityModeCommand

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					securityModeCommand
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							securityModeCommand
    								securityConfigSMC
    									securityAlgorithmConfig
    										cipheringAlgorithm = nea1 (1)
    										integrityProtAlgorithm = nia1 (1)
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Sent from port: NASEMU_NRNG:SYS_SRB

    UL-DCCH-Message
    	message = c1 = securityModeComplete =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = securityModeComplete =

    securityModeComplete

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 383
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					securityModeComplete
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							securityModeComplete
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Received on port: NASEMU_NRNG:SYS_SRB

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 383
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						securityModeComplete
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								securityModeComplete
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: SRB -> NR5GC:SRB

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		RadioBearerList
    			SS_Config
    				Id
    					Drb = 1
    				Config
    					AddOrReconfigure
    						Sdap
    							Config
    								SdapConfig
    									Pdu_SessionId = 1
    									Sdap_HeaderDL = Absent (1)
    									Sdap_HeaderUL = Present (0)
    									MappedQoS_Flows
    										IntegerType = 2
    						Pdcp
    							RBTerminating
    								RbConfig
    									Params
    										Rb
    											Drb
    												SN_SizeUL = PDCP_SNLength18 (1)
    												SN_SizeDL = PDCP_SNLength18 (1)
    												HeaderCompression
    													None = True
    												IntegrityProtectionEnabled = False
    								LinkToOtherCellGroup
    									None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										AM
    											Tx
    												R15
    													sn_FieldLength = size18 (1)
    													t_PollRetransmit = ms80 (15)
    													pollPDU = p32768 (18)
    													pollByte = kB750 (14)
    													maxRetxThreshold = t8 (5)
    											Rx
    												R15
    													sn_FieldLength = size18 (1)
    													t_Reassembly = ms80 (16)
    													t_StatusProhibit = ms30 (6)
    									TestMode = Omit
    								LogicalChannelId = 4
    								Mac
    									LogicalChannel
    										Priority = 1
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit

    Sent from port: NR5GC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		RadioBearerList = True

    Received on port: NR5GC:SYS

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		PdcpCount
    			Get
    				AllRBs = True

    Sent from port: NR5GC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		PdcpCount
    			Get
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 1
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000010'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000001'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 2
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Drb = 1
    					UL
    						Format = PdcpCount_DrbSQN18 (2)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_DrbSQN18 (2)
    						Value = 00000000000000000000000000000000'B

    Received on port: NR5GC:SYS

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		AS_Security
    			StartRestart
    				Integrity
    					Algorithm = nia1 (1)
    					KRRCint = 11010001100110000000111100001011111110110000000011101111001011101011111001100011011111100100010100110111110110101100101110011011'B
    					KUPint = 00110010110010010000001000000101110010000010101001101111111011011001100010010001011101001110010001101101010000011111001111111110'B
    					ActTimeList = Omit
    				Ciphering
    					Algorithm = nea1 (1)
    					KRRCenc = 01001001000011010111000100101000001000100000011100011000010001101110000000101100001000100001001110101000010111101111101001010110'B
    					KUPenc = 01100000010000010010101100111011100000110001000000010010111010100001010101011100111011110111000111001000001010000101010110000101'B
    					ActTimeList
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Srb = 1
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 2
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 1
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Srb = 2
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 0
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 0
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Drb = 1
    							UL
    								SQN
    									Format = PdcpCount_DrbSQN18 (2)
    									Value = 0
    							DL
    								SQN
    									Format = PdcpCount_DrbSQN18 (2)
    									Value = 0

    Sent from port: NR5GC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		AS_Security = True

    Received on port: NR5GC:SYS

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcReconfiguration
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcReconfiguration
    									radioBearerConfig
    										srb_ToAddModList
    											SRB_ToAddMod
    												srb_Identity = 2
    												reestablishPDCP = Omit
    												discardOnPDCP = Omit
    												pdcp_Config = Omit
    										srb3_ToRelease = Omit
    										drb_ToAddModList
    											DRB_ToAddMod
    												cnAssociation
    													sdap_Config
    														pdu_Session = 1
    														sdap_HeaderDL = absent (1)
    														sdap_HeaderUL = present_ (0)
    														defaultDRB = True
    														mappedQoS_FlowsToAdd
    															IntegerType = 2
    														mappedQoS_FlowsToRelease = Omit
    												drb_Identity = 1
    												reestablishPDCP = Omit
    												recoverPDCP = Omit
    												pdcp_Config
    													drb
    														discardTimer = infinity_ (15)
    														pdcp_SN_SizeUL = len18bits (1)
    														pdcp_SN_SizeDL = len18bits (1)
    														headerCompression
    															notUsed = Null
    														integrityProtection = Omit
    														statusReportRequired = true_ (0)
    														outOfOrderDelivery = Omit
    													moreThanOneRLC = Omit
    													t_Reordering = Omit
    													cipheringDisabled = Omit
    													discardTimerExt_r16 = Omit
    													moreThanTwoRLC_DRB_r16 = Omit
    													ethernetHeaderCompression_r16 = Omit
    												daps_Config_r16 = Omit
    										drb_ToReleaseList = Omit
    										securityConfig
    											securityAlgorithmConfig
    												cipheringAlgorithm = nea1 (1)
    												integrityProtAlgorithm = nia1 (1)
    											keyToUse = master (0)
    									secondaryCellGroup = Omit
    									measConfig = Omit
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension
    										masterCellGroup = '400290941979802C700CF91D780C830F3200'O
    										fullConfig = Omit
    										dedicatedNAS_MessageList = Omit
    										masterKeyUpdate = Omit
    										dedicatedSIB1_Delivery = Omit
    										dedicatedSystemInformationDelivery = Omit
    										otherConfig = Omit
    										nonCriticalExtension = Omit
    		Nas
    			NG_NAS_MSG_Request_Type
    				SecurityProtection
    					Status = 0010'B
    					ForceMacError = False
    				Pdu
    					Msg
    						service_Accept
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01001110'B
    							pduSessionStatus = Omit
    							pduSessionReactivationResult = Omit
    							pduSessionReactResultError = Omit
    							eapMessage = Omit
    							t3448 = Omit
    					PiggybackedPduList = Omit

    Inter-component message: TC_SRB -> NASEMU_NRNG:TC_SRB

    SERVICE ACCEPT
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Spare half octet [4 bits] = 0x0 [ 0 ]
    	Message Type [8 bits] = 0x4E [ 78 ]

    SERVICE ACCEPT PDU

    DL-DCCH-Message
    	message = c1 = rrcReconfiguration =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcReconfiguration =
    			radioBearerConfig
    				srb-ToAddModList = SEQUENCE OF SRB-ToAddMod
    					SRB-ToAddMod(1)
    						srb-Identity = 2
    				drb-ToAddModList = SEQUENCE OF DRB-ToAddMod
    					DRB-ToAddMod(1)
    						cnAssociation = sdap-Config =
    							pdu-Session = 1
    							sdap-HeaderDL = absent
    							sdap-HeaderUL = present
    							defaultDRB = TRUE
    							mappedQoS-FlowsToAdd = SEQUENCE OF QFI
    								QFI(1) = 2
    						drb-Identity = 1
    						pdcp-Config
    							drb
    								discardTimer = infinity
    								pdcp-SN-SizeUL = len18bits
    								pdcp-SN-SizeDL = len18bits
    								headerCompression = notUsed = NULL
    								statusReportRequired = true
    				securityConfig
    					securityAlgorithmConfig
    						cipheringAlgorithm = nea1
    						integrityProtAlgorithm = nia1
    					keyToUse = master
    			nonCriticalExtension
    				masterCellGroup = CONTAINING =
    					cellGroupId = 0
    					rlc-BearerToAddModList = SEQUENCE OF RLC-BearerConfig
    						RLC-BearerConfig(1)
    							logicalChannelIdentity = 2
    							servedRadioBearer = srb-Identity = 2
    							mac-LogicalChannelConfig
    								ul-SpecificParameters
    									priority = 3
    									prioritisedBitRate = infinity
    									bucketSizeDuration = ms50
    									logicalChannelGroup = 0
    									schedulingRequestID = 0
    									logicalChannelSR-Mask = FALSE
    									logicalChannelSR-DelayTimerApplied = FALSE
    						RLC-BearerConfig(2)
    							logicalChannelIdentity = 4
    							servedRadioBearer = drb-Identity = 1
    							rlc-Config = am =
    								ul-AM-RLC
    									sn-FieldLength = size18
    									t-PollRetransmit = ms80
    									pollPDU = p32768
    									pollByte = kB750
    									maxRetxThreshold = t8
    								dl-AM-RLC
    									sn-FieldLength = size18
    									t-Reassembly = ms80
    									t-StatusProhibit = ms30
    							mac-LogicalChannelConfig
    								ul-SpecificParameters
    									priority = 1
    									prioritisedBitRate = infinity
    									bucketSizeDuration = ms50
    									logicalChannelGroup = 1
    									schedulingRequestID = 0
    									logicalChannelSR-Mask = FALSE
    									logicalChannelSR-DelayTimerApplied = FALSE
    				dedicatedNAS-MessageList = SEQUENCE OF DedicatedNAS-Message
    					DedicatedNAS-Message(1) = 7E028B63FFFC07D50F27

    rrcReconfiguration

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcReconfiguration
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcReconfiguration
    								radioBearerConfig
    									srb_ToAddModList
    										SRB_ToAddMod
    											srb_Identity = 2
    											reestablishPDCP = Omit
    											discardOnPDCP = Omit
    											pdcp_Config = Omit
    									srb3_ToRelease = Omit
    									drb_ToAddModList
    										DRB_ToAddMod
    											cnAssociation
    												sdap_Config
    													pdu_Session = 1
    													sdap_HeaderDL = absent (1)
    													sdap_HeaderUL = present_ (0)
    													defaultDRB = True
    													mappedQoS_FlowsToAdd
    														IntegerType = 2
    													mappedQoS_FlowsToRelease = Omit
    											drb_Identity = 1
    											reestablishPDCP = Omit
    											recoverPDCP = Omit
    											pdcp_Config
    												drb
    													discardTimer = infinity_ (15)
    													pdcp_SN_SizeUL = len18bits (1)
    													pdcp_SN_SizeDL = len18bits (1)
    													headerCompression
    														notUsed = Null
    													integrityProtection = Omit
    													statusReportRequired = true_ (0)
    													outOfOrderDelivery = Omit
    												moreThanOneRLC = Omit
    												t_Reordering = Omit
    												cipheringDisabled = Omit
    												discardTimerExt_r16 = Omit
    												moreThanTwoRLC_DRB_r16 = Omit
    												ethernetHeaderCompression_r16 = Omit
    											daps_Config_r16 = Omit
    									drb_ToReleaseList = Omit
    									securityConfig
    										securityAlgorithmConfig
    											cipheringAlgorithm = nea1 (1)
    											integrityProtAlgorithm = nia1 (1)
    										keyToUse = master (0)
    								secondaryCellGroup = Omit
    								measConfig = Omit
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension
    									masterCellGroup = '400290941979802C700CF91D780C830F3200'O
    									fullConfig = Omit
    									dedicatedNAS_MessageList
    										NG_NAS_Message = '7E028B63FFFC07D50F27'O
    									masterKeyUpdate = Omit
    									dedicatedSIB1_Delivery = Omit
    									dedicatedSystemInformationDelivery = Omit
    									otherConfig = Omit
    									nonCriticalExtension = Omit

    Sent from port: NASEMU_NRNG:SYS_SRB

    UL-DCCH-Message
    	message = c1 = rrcReconfigurationComplete =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcReconfigurationComplete =

    rrcReconfigurationComplete

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 407
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcReconfigurationComplete
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcReconfigurationComplete
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Received on port: NASEMU_NRNG:SYS_SRB

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 407
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcReconfigurationComplete
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcReconfigurationComplete
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: SRB -> NR5GC:SRB

    SipMessage
    	Message Header = REGISTER sip:test.3gpp.com SIP/2.0
    From: ;tag=1584742388
    To:
    CSeq: 510079899 REGISTER
    Call-ID: 1583821721_207195148@3000::2:6c61:18ff:fe5d:9f1e
    Via: SIP/2.0/TCP [3000::2:6c61:18ff:fe5d:9f1e]:44724;branch=z9hG4bK35466275
    Max-Forwards: 70
    Contact: ;+g.3gpp.accesstype="cellular2";+sip.instance="";+g.3gpp.ps-data-off="active";audio;+g.3gpp.nw-init-ussi;+g.3gpp.smsip;+g.3gpp.icsi-ref="urn%3Aurn-7%3A3gpp-service.ims.icsi.mmtel"
    P-Access-Network-Info: 3GPP-NR-TDD;utran-cell-id-3gpp=00101000001000000400
    Security-Verify: ipsec-3gpp;alg=hmac-md5-96;spi-c=260;spi-s=256;port-c=5061;port-s=5062;q=0.9,ipsec-3gpp;alg=hmac-sha-1-96;spi-c=260;spi-s=256;port-c=5061;port-s=5062;q=0.7
    Expires: 0
    Supported: path,sec-agree
    Authorization: Digest username="001010123456789@test.3gpp.com",realm="test.3gpp.com",uri="sip:test.3gpp.com",qop=auth,nonce="o94MbTY+MMNkpAePG/jVd24yOzbEbIAAo98ObjI7tsQ=",nc=00000002,cnonce="1583821701",algorithm=AKAv1-MD5,response="4568eca91539397ec44846917be51656",opaque="5ccc069c403ebaf9f0171e9517f40e41"
    User-Agent: qti_Lahaina for arm64_RKQ1.210107.001
    Require: sec-agree
    Proxy-Require: sec-agree
    Allow: INVITE,BYE,CANCEL,ACK,NOTIFY,UPDATE,PRACK,INFO,MESSAGE,OPTIONS
    Security-Client: ipsec-3gpp; alg=hmac-md5-96; ealg=des-ede3-cbc; spi-c=1298788414; spi-s=2838622844; port-c=41015; port-s=44724,ipsec-3gpp; alg=hmac-md5-96; ealg=aes-cbc; spi-c=1298788414; spi-s=2838622844; port-c=41015; port-s=44724,ipsec-3gpp; alg=hmac-md5-96; ealg=null; spi-c=1298788414; spi-s=2838622844; port-c=41015; port-s=44724,ipsec-3gpp; alg=hmac-sha-1-96; ealg=des-ede3-cbc; spi-c=1298788414; spi-s=2838622844; port-c=41015; port-s=44724,ipsec-3gpp; alg=hmac-sha-1-96; ealg=aes-cbc; spi-c=1298788414; spi-s=2838622844; port-c=41015; port-s=44724,ipsec-3gpp; alg=hmac-sha-1-96; ealg=null; spi-c=1298788414; spi-s=2838622844; port-c=41015; port-s=44724
    Content-Length: 0

    Request:REGISTER sip:test.3gpp.com SIP/2.0

    IP_SOCKET_IND
    	DATA
    		ConnectionId
    			Protocol = tcp (1)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 5062
    			Remote
    				IpAddr
    					V6
    						Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    						ScopeId = Omit
    				Port = 43642
    		Ind
    			TCP
    				Recv = '[encoded data, 4216 characters]'O

    Received on port: IPMUX:IP_SOCK

    summary = Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol
    		DATA
    			ConnectionId
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5062
    				Remote
    					IpAddr
    						V6
    							Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    							ScopeId = Omit
    					Port = 43642
    			Ind
    				TCP
    					Recv = '[encoded data, 4216 characters]'O

    Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol

    summary = Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol
    		DATA
    			ConnectionId
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5062
    				Remote
    					IpAddr
    						V6
    							Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    							ScopeId = Omit
    					Port = 43642
    			Ind
    				TCP
    					Recv = '[encoded data, 4216 characters]'O

    Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol

    summary = Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol
    		DATA
    			ConnectionId
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5062
    				Remote
    					IpAddr
    						V6
    							Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    							ScopeId = Omit
    					Port = 43642
    			Ind
    				TCP
    					Recv = '[encoded data, 4216 characters]'O

    Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol

    summary = Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol
    		DATA
    			ConnectionId
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5062
    				Remote
    					IpAddr
    						V6
    							Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    							ScopeId = Omit
    					Port = 43642
    			Ind
    				TCP
    					Recv = '[encoded data, 4216 characters]'O

    Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol

    IP_SOCKET_IND
    	DATA
    		ConnectionId
    			Protocol = tcp (1)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 5062
    			Remote
    				IpAddr
    					V6
    						Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    						ScopeId = Omit
    				Port = 43642
    		Ind
    			TCP
    				Recv = '[encoded data, 4216 characters]'O

    Inter-component message: IP_SOCK_DATA -> IP:IP_SOCK_DATA

    ConstraintMismatch::Received:
    summary = Message Mismatch: IMS_DATA_REQ.Request
    MESSAGE_MISMATCH
    	Message Mismatch: IMS_DATA_REQ.Request
    		RoutingInfo
    			Protocol = tcp (1)
    			Security = protectedContext1 (1)
    			UE_Address
    				V6
    					Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    					ScopeId = Omit
    			NW_Address
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    		Request
    			Register
    				requestLine
    					method = REGISTER_E (5)
    					requestUri
    						scheme = 'sip'
    						components
    							sip
    								userInfo = Omit
    								hostPort
    									host = 'test.3gpp.com'
    									portField = Omit
    						urlParameters = Omit
    						headers = Omit
    					sipVersion = 'SIP/2.0'
    				msgHeader
    					accept = Omit
    					acceptContact = Omit
    					acceptEncoding = Omit
    					acceptLanguage = Omit
    					alertInfo = Omit
    					allow
    						fieldName = ALLOW_E (4)
    						methods
    							CharacterStringType = 'INVITE'
    							CharacterStringType = 'BYE'
    							CharacterStringType = 'CANCEL'
    							CharacterStringType = 'ACK'
    							CharacterStringType = 'NOTIFY'
    							CharacterStringType = 'UPDATE'
    							CharacterStringType = 'PRACK'
    							CharacterStringType = 'INFO'
    							CharacterStringType = 'MESSAGE'
    							CharacterStringType = 'OPTIONS'
    					allowEvents = Omit
    					authenticationInfo = Omit
    					authorization
    						fieldName = AUTHORIZATION_E (6)
    						body
    							Credentials
    								digestResponse
    									GenericParam
    										id = 'username'
    										paramValue
    											quotedString = '001010123456789@test.3gpp.com'
    									GenericParam
    										id = 'realm'
    										paramValue
    											quotedString = 'test.3gpp.com'
    									GenericParam
    										id = 'qop'
    										paramValue
    											tokenOrHost = 'auth'
    									GenericParam
    										id = 'cnonce'
    										paramValue
    											quotedString = '1583821701'
    									GenericParam
    										id = 'opaque'
    										paramValue
    											quotedString = '5ccc069c403ebaf9f0171e9517f40e41'
    									GenericParam
    										id = 'algorithm'
    										paramValue
    											tokenOrHost = 'AKAv1-MD5'
    									GenericParam
    										id = 'nonce'
    										paramValue
    											quotedString = 'o94MbTY+MMNkpAePG/jVd24yOzbEbIAAo98ObjI7tsQ='
    									GenericParam
    										id = 'uri'
    										paramValue
    											quotedString = 'sip:test.3gpp.com'
    									GenericParam
    										id = 'response'
    										paramValue
    											quotedString = '4568eca91539397ec44846917be51656'
    									GenericParam
    										id = 'nc'
    										paramValue
    											tokenOrHost = '00000002'
    					callId
    						fieldName = CALL_ID_E (7)
    						callid = '1583821721_207195148@3000::2:6c61:18ff:fe5d:9f1e'
    					callInfo = Omit
    					contact
    						fieldName = CONTACT_E (9)
    						contactBody
    							contactAddresses
    								ContactAddress
    									addressField
    										nameAddr
    											displayName = Omit
    											addrSpec
    												scheme = 'sip'
    												components
    													sip
    														userInfo
    															userOrTelephoneSubscriber = '7d50dd18-5ee3-4eaf-a145-d31d84987cb9'
    															password = Omit
    														hostPort
    															host = '3000::2:6c61:18ff:fe5d:9f1e'
    															portField = 44724
    												urlParameters = Omit
    												headers = Omit
    									contactParams
    										GenericParam
    											id = '+g.3gpp.accesstype'
    											paramValue
    												quotedString = 'cellular2'
    										GenericParam
    											id = '+sip.instance'
    											paramValue
    												quotedString = ''
    										GenericParam
    											id = '+g.3gpp.ps-data-off'
    											paramValue
    												quotedString = 'active'
    										GenericParam
    											id = 'audio'
    											paramValue = Omit
    										GenericParam
    											id = '+g.3gpp.nw-init-ussi'
    											paramValue = Omit
    										GenericParam
    											id = '+g.3gpp.smsip'
    											paramValue = Omit
    										GenericParam
    											id = '+g.3gpp.icsi-ref'
    											paramValue
    												quotedString = 'urn%3Aurn-7%3A3gpp-service.ims.icsi.mmtel'
    					contentDisposition = Omit
    					contentEncoding = Omit
    					contentLanguage = Omit
    					contentLength
    						fieldName = CONTENT_LENGTH_E (13)
    						len = 0
    					contentType = Omit
    					cSeq
    						fieldName = CSEQ_E (15)
    						seqNumber = 510079899
    						method = 'REGISTER'
    					date = Omit
    					errorInfo = Omit
    					event = Omit
    						fieldName = EVENT_E (47)

    					expires
    						fieldName = EXPIRES_E (18)
    						deltaSec = '0'
    					featureCaps = Omit
    					fromField
    						fieldName = FROM_E (19)
    						addressField
    							nameAddr
    								displayName = Omit
    								addrSpec
    									scheme = 'sip'
    									components
    										sip
    											userInfo
    												userOrTelephoneSubscriber = '001010123456789'
    												password = Omit
    											hostPort
    												host = 'ims.mnc001.mcc001.3gppnetwork.org'
    												portField = Omit
    									urlParameters = Omit
    									headers = Omit

    						fromParams
    							GenericParam
    								id = 'tag'
    								paramValue
    									tokenOrHost = '1584742388'

    					geolocation = Omit
    					geolocationRouting = Omit
    					historyInfo = Omit
    					infoPackage = Omit
    					inReplyTo = Omit
    					maxForwards
    						fieldName = MAX_FORWARDS_E (21)
    						forwards = 70
    					mimeVersion = Omit
    					minExpires = Omit
    					minSE = Omit
    					organization = Omit
    					pAccessNetworkInfo
    						fieldName = P_ACCESS_NETWORK_INFO_E (65)
    						accessType = '3GPP-NR-TDD'
    						genericParams
    							GenericParam
    								id = 'utran-cell-id-3gpp'
    								paramValue
    									tokenOrHost = '00101000001000000400'
    					pAssertedID = Omit
    					pAssertedService = Omit
    					pAssociatedURI = Omit
    					path = Omit
    					pCalledPartyID = Omit
    					pChargingFunctionAddresses = Omit
    					pChargingVector = Omit
    					pEarlyMedia = Omit
    					pMediaAuthorization = Omit
    					pPreferredID = Omit
    					pPreferredService = Omit
    					priority = Omit
    					privacy = Omit
    					proxyAuthenticate = Omit
    					proxyAuthorization = Omit
    					proxyRequire
    						fieldName = PROXY_REQUIRE_E (28)
    						optionsTags
    							CharacterStringType = 'sec-agree'
    					pVisitedNetworkID = Omit
    					rAck = Omit
    					rSeq = Omit
    					reason = Omit
    					recordRoute = Omit
    					recvInfo = Omit
    					requestDisposition = Omit
    					referredBy = Omit
    					referTo = Omit
    					referSub = Omit
    					replaces = Omit
    					replyTo = Omit
    					require
    						fieldName = REQUIRE_E (31)
    						optionsTags
    							CharacterStringType = 'sec-agree'
    					retryAfter = Omit
    					route = Omit
    					securityClient
    						fieldName = SECURITY_CLIENT_E (62)
    						securityMech
    							SecurityMechanism
    								mechName = 'ipsec-3gpp'
    								mechParams
    									GenericParam
    										id = 'alg'
    										paramValue
    											tokenOrHost = 'hmac-md5-96'
    									GenericParam
    										id = 'ealg'
    										paramValue
    											tokenOrHost = 'des-ede3-cbc'
    									GenericParam
    										id = 'spi-c'
    										paramValue
    											tokenOrHost = '1298788414'
    									GenericParam
    										id = 'spi-s'
    										paramValue
    											tokenOrHost = '2838622844'
    									GenericParam
    										id = 'port-c'
    										paramValue
    											tokenOrHost = '41015'
    									GenericParam
    										id = 'port-s'
    										paramValue
    											tokenOrHost = '44724'
    							SecurityMechanism
    								mechName = 'ipsec-3gpp'
    								mechParams
    									GenericParam
    										id = 'alg'
    										paramValue
    											tokenOrHost = 'hmac-md5-96'
    									GenericParam
    										id = 'ealg'
    										paramValue
    											tokenOrHost = 'aes-cbc'
    									GenericParam
    										id = 'spi-c'
    										paramValue
    											tokenOrHost = '1298788414'
    									GenericParam
    										id = 'spi-s'
    										paramValue
    											tokenOrHost = '2838622844'
    									GenericParam
    										id = 'port-c'
    										paramValue
    											tokenOrHost = '41015'
    									GenericParam
    										id = 'port-s'
    										paramValue
    											tokenOrHost = '44724'
    							SecurityMechanism
    								mechName = 'ipsec-3gpp'
    								mechParams
    									GenericParam
    										id = 'alg'
    										paramValue
    											tokenOrHost = 'hmac-md5-96'
    									GenericParam
    										id = 'ealg'
    										paramValue
    											tokenOrHost = 'null'
    									GenericParam
    										id = 'spi-c'
    										paramValue
    											tokenOrHost = '1298788414'
    									GenericParam
    										id = 'spi-s'
    										paramValue
    											tokenOrHost = '2838622844'
    									GenericParam
    										id = 'port-c'
    										paramValue
    											tokenOrHost = '41015'
    									GenericParam
    										id = 'port-s'
    										paramValue
    											tokenOrHost = '44724'
    							SecurityMechanism
    								mechName = 'ipsec-3gpp'
    								mechParams
    									GenericParam
    										id = 'alg'
    										paramValue
    											tokenOrHost = 'hmac-sha-1-96'
    									GenericParam
    										id = 'ealg'
    										paramValue
    											tokenOrHost = 'des-ede3-cbc'
    									GenericParam
    										id = 'spi-c'
    										paramValue
    											tokenOrHost = '1298788414'
    									GenericParam
    										id = 'spi-s'
    										paramValue
    											tokenOrHost = '2838622844'
    									GenericParam
    										id = 'port-c'
    										paramValue
    											tokenOrHost = '41015'
    									GenericParam
    										id = 'port-s'
    										paramValue
    											tokenOrHost = '44724'
    							SecurityMechanism
    								mechName = 'ipsec-3gpp'
    								mechParams
    									GenericParam
    										id = 'alg'
    										paramValue
    											tokenOrHost = 'hmac-sha-1-96'
    									GenericParam
    										id = 'ealg'
    										paramValue
    											tokenOrHost = 'aes-cbc'
    									GenericParam
    										id = 'spi-c'
    										paramValue
    											tokenOrHost = '1298788414'
    									GenericParam
    										id = 'spi-s'
    										paramValue
    											tokenOrHost = '2838622844'
    									GenericParam
    										id = 'port-c'
    										paramValue
    											tokenOrHost = '41015'
    									GenericParam
    										id = 'port-s'
    										paramValue
    											tokenOrHost = '44724'
    							SecurityMechanism
    								mechName = 'ipsec-3gpp'
    								mechParams
    									GenericParam
    										id = 'alg'
    										paramValue
    											tokenOrHost = 'hmac-sha-1-96'
    									GenericParam
    										id = 'ealg'
    										paramValue
    											tokenOrHost = 'null'
    									GenericParam
    										id = 'spi-c'
    										paramValue
    											tokenOrHost = '1298788414'
    									GenericParam
    										id = 'spi-s'
    										paramValue
    											tokenOrHost = '2838622844'
    									GenericParam
    										id = 'port-c'
    										paramValue
    											tokenOrHost = '41015'
    									GenericParam
    										id = 'port-s'
    										paramValue
    											tokenOrHost = '44724'
    					securityServer = Omit
    					securityVerify
    						fieldName = SECURITY_VERIFY_E (64)
    						securityMech
    							SecurityMechanism
    								mechName = 'ipsec-3gpp'
    								mechParams
    									GenericParam
    										id = 'alg'
    										paramValue
    											tokenOrHost = 'hmac-md5-96'
    									GenericParam
    										id = 'spi-c'
    										paramValue
    											tokenOrHost = '260'
    									GenericParam
    										id = 'spi-s'
    										paramValue
    											tokenOrHost = '256'
    									GenericParam
    										id = 'port-c'
    										paramValue
    											tokenOrHost = '5061'
    									GenericParam
    										id = 'port-s'
    										paramValue
    											tokenOrHost = '5062'
    									GenericParam
    										id = 'q'
    										paramValue
    											tokenOrHost = '0.9'
    							SecurityMechanism
    								mechName = 'ipsec-3gpp'
    								mechParams
    									GenericParam
    										id = 'alg'
    										paramValue
    											tokenOrHost = 'hmac-sha-1-96'
    									GenericParam
    										id = 'spi-c'
    										paramValue
    											tokenOrHost = '260'
    									GenericParam
    										id = 'spi-s'
    										paramValue
    											tokenOrHost = '256'
    									GenericParam
    										id = 'port-c'
    										paramValue
    											tokenOrHost = '5061'
    									GenericParam
    										id = 'port-s'
    										paramValue
    											tokenOrHost = '5062'
    									GenericParam
    										id = 'q'
    										paramValue
    											tokenOrHost = '0.7'
    					server = Omit
    					serviceRoute = Omit
    					sessionExpires = Omit
    					sessionId = Omit
    					sipETag = Omit
    					sipIfMatch = Omit
    					subject = Omit
    					subscriptionState = Omit
    					supported
    						fieldName = SUPPORTED_E (36)
    						optionsTags
    							CharacterStringType = 'path'
    							CharacterStringType = 'sec-agree'
    					timestamp = Omit
    					toField
    						fieldName = TO_E (38)
    						addressField
    							nameAddr
    								displayName = Omit
    								addrSpec
    									scheme = 'sip'
    									components
    										sip
    											userInfo
    												userOrTelephoneSubscriber = '001010123456789'
    												password = Omit
    											hostPort
    												host = 'ims.mnc001.mcc001.3gppnetwork.org'
    												portField = Omit
    									urlParameters = Omit
    									headers = Omit

    						toParams = Omit
    							GenericParam
    								id = 'tag'
    								paramValue
    									tokenOrHost = 'abc-SUBSCRIBE-to-reg-package-5-Totag'
    									quotedString = 'abc-SUBSCRIBE-to-reg-package-5-Totag'
    					unsupported = Omit
    					userToUser = Omit
    					userAgent
    						fieldName = USER_AGENT_E (40)
    						userAgentBody
    							CharacterStringType = 'qti_Lahaina for arm64_RKQ1.210107.001'
    					via
    						fieldName = VIA_E (41)
    						viaBody
    							ViaBody
    								sentProtocol
    									protocolName = 'SIP'
    									protocolVersion = '2.0'
    									transport = 'TCP'
    								sentBy
    									host = '3000::2:6c61:18ff:fe5d:9f1e'
    									portField = 44724
    								viaParams
    									GenericParam
    										id = 'branch'
    										paramValue
    											tokenOrHost = 'z9hG4bK35466275'
    					warning = Omit
    					wwwAuthenticate = Omit
    					resourcePriority = Omit
    					answerMode = Omit
    					privAnswerMode = Omit
    					targetDialog = Omit
    					pAnswerState = Omit
    					undefinedHeader_List = Omit
    				messageBody = Omit
    				payload = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IMS_DATA_REQ.Request
    MESSAGE_MISMATCH
    	Message Mismatch: IMS_DATA_REQ.Request
    		RoutingInfo
    			Protocol = AnyValue
    			Security = AnyOrOmit
    			UE_Address
    				V6
    					Addr
    					ScopeId
    			NW_Address
    				V6
    					Addr
    					ScopeId
    		Request
    			Register
    				requestLine
    					method = SUBSCRIBE_E (7)
    					requestUri
    						scheme
    						components
    							sip
    								userInfo
    								hostPort
    									host
    									portField
    						urlParameters
    						headers
    					sipVersion = 'SIP/2.0'
    				msgHeader
    					accept = AnyOrOmit
    					acceptContact = AnyOrOmit
    					acceptEncoding = AnyOrOmit
    					acceptLanguage = AnyOrOmit
    					alertInfo = AnyOrOmit
    					allow
    						fieldName
    						methods
    							CharacterStringType
    							CharacterStringType
    							CharacterStringType
    							CharacterStringType
    							CharacterStringType
    							CharacterStringType
    							CharacterStringType
    							CharacterStringType
    							CharacterStringType
    							CharacterStringType
    					allowEvents = AnyOrOmit
    					authenticationInfo = AnyOrOmit
    					authorization
    						fieldName
    						body
    							Credentials
    								digestResponse
    									GenericParam
    										id
    										paramValue
    											quotedString
    									GenericParam
    										id
    										paramValue
    											quotedString
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											quotedString
    									GenericParam
    										id
    										paramValue
    											quotedString
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											quotedString
    									GenericParam
    										id
    										paramValue
    											quotedString
    									GenericParam
    										id
    										paramValue
    											quotedString
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    					callId
    						fieldName = CALL_ID_E (7)
    						callid = '1583823794_207321852@3000::2:6c61:18ff:fe5d:9f1e'
    					callInfo = AnyOrOmit
    					contact
    						fieldName
    						contactBody
    							contactAddresses
    								ContactAddress
    									addressField
    										nameAddr
    											displayName
    											addrSpec
    												scheme
    												components
    													sip
    														userInfo
    															userOrTelephoneSubscriber
    															password
    														hostPort
    															host
    															portField
    												urlParameters
    												headers
    									contactParams
    										GenericParam
    											id
    											paramValue
    												quotedString
    										GenericParam
    											id
    											paramValue
    												quotedString
    										GenericParam
    											id
    											paramValue
    												quotedString
    										GenericParam
    											id
    											paramValue
    										GenericParam
    											id
    											paramValue
    										GenericParam
    											id
    											paramValue
    										GenericParam
    											id
    											paramValue
    												quotedString
    					contentDisposition = AnyOrOmit
    					contentEncoding = AnyOrOmit
    					contentLanguage = AnyOrOmit
    					contentLength
    						fieldName
    						len
    					contentType = AnyOrOmit
    					cSeq
    						fieldName = CSEQ_E (15)
    						seqNumber = AnyValue
    						method = 'SUBSCRIBE'
    					date = AnyOrOmit
    					errorInfo = AnyOrOmit
    					event = Omit
    						fieldName = 'reg'
    						eventParams = Omit
    					expires
    						fieldName = EXPIRES_E (18)
    						deltaSec = '0'
    					featureCaps = AnyOrOmit
    					fromField
    						fieldName = FROM_E (19)
    						addressField
    							nameAddr
    								displayName = AnyOrOmit
    								addrSpec
    									scheme = 'sip'
    									components
    										sip
    											userInfo
    												userOrTelephoneSubscriber = '001010123456789'
    												password = Omit
    											hostPort
    												host = 'ims.mnc001.mcc001.3gppnetwork.org'
    												portField = Omit
    									urlParameters = Omit
    									headers = Omit
    							addrSpecUnion
    								scheme = 'sip'
    								components
    									sip
    										userInfo
    											userOrTelephoneSubscriber = '001010123456789'
    											password = Omit
    										hostPort
    											host = 'ims.mnc001.mcc001.3gppnetwork.org'
    											portField = Omit
    								urlParameters = Omit
    								headers = Omit
    						fromParams
    							GenericParam
    								id = 'tag'
    								paramValue
    									tokenOrHost = '1583823796'
    									quotedString = '1583823796'
    							GenericParam = AnyOrOmit
    					geolocation = AnyOrOmit
    					geolocationRouting = AnyOrOmit
    					historyInfo = AnyOrOmit
    					infoPackage = AnyOrOmit
    					inReplyTo = AnyOrOmit
    					maxForwards
    						fieldName
    						forwards
    					mimeVersion = AnyOrOmit
    					minExpires = AnyOrOmit
    					minSE = AnyOrOmit
    					organization = AnyOrOmit
    					pAccessNetworkInfo
    						fieldName
    						accessType
    						genericParams
    							GenericParam
    								id
    								paramValue
    									tokenOrHost
    					pAssertedID = AnyOrOmit
    					pAssertedService = AnyOrOmit
    					pAssociatedURI = AnyOrOmit
    					path = AnyOrOmit
    					pCalledPartyID = AnyOrOmit
    					pChargingFunctionAddresses = AnyOrOmit
    					pChargingVector = AnyOrOmit
    					pEarlyMedia = AnyOrOmit
    					pMediaAuthorization = AnyOrOmit
    					pPreferredID = AnyOrOmit
    					pPreferredService = AnyOrOmit
    					priority = AnyOrOmit
    					privacy = AnyOrOmit
    					proxyAuthenticate = AnyOrOmit
    					proxyAuthorization = AnyOrOmit
    					proxyRequire
    						fieldName
    						optionsTags
    							CharacterStringType
    					pVisitedNetworkID = AnyOrOmit
    					rAck = AnyOrOmit
    					rSeq = AnyOrOmit
    					reason = AnyOrOmit
    					recordRoute = AnyOrOmit
    					recvInfo = AnyOrOmit
    					requestDisposition = AnyOrOmit
    					referredBy = AnyOrOmit
    					referTo = AnyOrOmit
    					referSub = AnyOrOmit
    					replaces = AnyOrOmit
    					replyTo = AnyOrOmit
    					require
    						fieldName
    						optionsTags
    							CharacterStringType
    					retryAfter = AnyOrOmit
    					route = AnyOrOmit
    					securityClient
    						fieldName
    						securityMech
    							SecurityMechanism
    								mechName
    								mechParams
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    							SecurityMechanism
    								mechName
    								mechParams
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    							SecurityMechanism
    								mechName
    								mechParams
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    							SecurityMechanism
    								mechName
    								mechParams
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    							SecurityMechanism
    								mechName
    								mechParams
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    							SecurityMechanism
    								mechName
    								mechParams
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    					securityServer = AnyOrOmit
    					securityVerify
    						fieldName
    						securityMech
    							SecurityMechanism
    								mechName
    								mechParams
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    							SecurityMechanism
    								mechName
    								mechParams
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    					server = AnyOrOmit
    					serviceRoute = AnyOrOmit
    					sessionExpires = AnyOrOmit
    					sessionId = AnyOrOmit
    					sipETag = AnyOrOmit
    					sipIfMatch = AnyOrOmit
    					subject = AnyOrOmit
    					subscriptionState = AnyOrOmit
    					supported
    						fieldName
    						optionsTags
    							CharacterStringType
    							CharacterStringType
    					timestamp = AnyOrOmit
    					toField
    						fieldName = TO_E (38)
    						addressField
    							nameAddr
    								displayName = AnyOrOmit
    								addrSpec
    									scheme = 'sip'
    									components
    										sip
    											userInfo
    												userOrTelephoneSubscriber = '001010123456789'
    												password = Omit
    											hostPort
    												host = 'ims.mnc001.mcc001.3gppnetwork.org'
    												portField = Omit
    									urlParameters = Omit
    									headers = Omit
    							addrSpecUnion
    								scheme = 'sip'
    								components
    									sip
    										userInfo
    											userOrTelephoneSubscriber = '001010123456789'
    											password = Omit
    										hostPort
    											host = 'ims.mnc001.mcc001.3gppnetwork.org'
    											portField = Omit
    								urlParameters = Omit
    								headers = Omit
    						toParams = Omit
    							GenericParam
    								id
    								paramValue
    									tokenOrHost
    									quotedString
    					unsupported = AnyOrOmit
    					userToUser = AnyOrOmit
    					userAgent
    						fieldName
    						userAgentBody
    							CharacterStringType
    					via
    						fieldName
    						viaBody
    							ViaBody
    								sentProtocol
    									protocolName
    									protocolVersion
    									transport
    								sentBy
    									host
    									portField
    								viaParams
    									GenericParam
    										id
    										paramValue
    											tokenOrHost
    					warning = AnyOrOmit
    					wwwAuthenticate = AnyOrOmit
    					resourcePriority = AnyOrOmit
    					answerMode = AnyOrOmit
    					privAnswerMode = AnyOrOmit
    					targetDialog = AnyOrOmit
    					pAnswerState = AnyOrOmit
    					undefinedHeader_List = AnyOrOmit
    				messageBody = Omit
    				payload = Omit

    Message Mismatch: IMS_DATA_REQ.Request

    IMS_DATA_REQ
    	RoutingInfo
    		Protocol = tcp (1)
    		Security = protectedContext1 (1)
    		UE_Address
    			V6
    				Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    				ScopeId = Omit
    		NW_Address
    			V6
    				Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    				ScopeId = Omit
    	Request
    		Register
    			requestLine
    				method = REGISTER_E (5)
    				requestUri
    					scheme = 'sip'
    					components
    						sip
    							userInfo = Omit
    							hostPort
    								host = 'test.3gpp.com'
    								portField = Omit
    					urlParameters = Omit
    					headers = Omit
    				sipVersion = 'SIP/2.0'
    			msgHeader
    				accept = Omit
    				acceptContact = Omit
    				acceptEncoding = Omit
    				acceptLanguage = Omit
    				alertInfo = Omit
    				allow
    					fieldName = ALLOW_E (4)
    					methods
    						CharacterStringType = 'INVITE'
    						CharacterStringType = 'BYE'
    						CharacterStringType = 'CANCEL'
    						CharacterStringType = 'ACK'
    						CharacterStringType = 'NOTIFY'
    						CharacterStringType = 'UPDATE'
    						CharacterStringType = 'PRACK'
    						CharacterStringType = 'INFO'
    						CharacterStringType = 'MESSAGE'
    						CharacterStringType = 'OPTIONS'
    				allowEvents = Omit
    				authenticationInfo = Omit
    				authorization
    					fieldName = AUTHORIZATION_E (6)
    					body
    						Credentials
    							digestResponse
    								GenericParam
    									id = 'username'
    									paramValue
    										quotedString = '001010123456789@test.3gpp.com'
    								GenericParam
    									id = 'realm'
    									paramValue
    										quotedString = 'test.3gpp.com'
    								GenericParam
    									id = 'qop'
    									paramValue
    										tokenOrHost = 'auth'
    								GenericParam
    									id = 'cnonce'
    									paramValue
    										quotedString = '1583821701'
    								GenericParam
    									id = 'opaque'
    									paramValue
    										quotedString = '5ccc069c403ebaf9f0171e9517f40e41'
    								GenericParam
    									id = 'algorithm'
    									paramValue
    										tokenOrHost = 'AKAv1-MD5'
    								GenericParam
    									id = 'nonce'
    									paramValue
    										quotedString = 'o94MbTY+MMNkpAePG/jVd24yOzbEbIAAo98ObjI7tsQ='
    								GenericParam
    									id = 'uri'
    									paramValue
    										quotedString = 'sip:test.3gpp.com'
    								GenericParam
    									id = 'response'
    									paramValue
    										quotedString = '4568eca91539397ec44846917be51656'
    								GenericParam
    									id = 'nc'
    									paramValue
    										tokenOrHost = '00000002'
    				callId
    					fieldName = CALL_ID_E (7)
    					callid = '1583821721_207195148@3000::2:6c61:18ff:fe5d:9f1e'
    				callInfo = Omit
    				contact
    					fieldName = CONTACT_E (9)
    					contactBody
    						contactAddresses
    							ContactAddress
    								addressField
    									nameAddr
    										displayName = Omit
    										addrSpec
    											scheme = 'sip'
    											components
    												sip
    													userInfo
    														userOrTelephoneSubscriber = '7d50dd18-5ee3-4eaf-a145-d31d84987cb9'
    														password = Omit
    													hostPort
    														host = '3000::2:6c61:18ff:fe5d:9f1e'
    														portField = 44724
    											urlParameters = Omit
    											headers = Omit
    								contactParams
    									GenericParam
    										id = '+g.3gpp.accesstype'
    										paramValue
    											quotedString = 'cellular2'
    									GenericParam
    										id = '+sip.instance'
    										paramValue
    											quotedString = ''
    									GenericParam
    										id = '+g.3gpp.ps-data-off'
    										paramValue
    											quotedString = 'active'
    									GenericParam
    										id = 'audio'
    										paramValue = Omit
    									GenericParam
    										id = '+g.3gpp.nw-init-ussi'
    										paramValue = Omit
    									GenericParam
    										id = '+g.3gpp.smsip'
    										paramValue = Omit
    									GenericParam
    										id = '+g.3gpp.icsi-ref'
    										paramValue
    											quotedString = 'urn%3Aurn-7%3A3gpp-service.ims.icsi.mmtel'
    				contentDisposition = Omit
    				contentEncoding = Omit
    				contentLanguage = Omit
    				contentLength
    					fieldName = CONTENT_LENGTH_E (13)
    					len = 0
    				contentType = Omit
    				cSeq
    					fieldName = CSEQ_E (15)
    					seqNumber = 510079899
    					method = 'REGISTER'
    				date = Omit
    				errorInfo = Omit
    				event = Omit
    				expires
    					fieldName = EXPIRES_E (18)
    					deltaSec = '0'
    				featureCaps = Omit
    				fromField
    					fieldName = FROM_E (19)
    					addressField
    						nameAddr
    							displayName = Omit
    							addrSpec
    								scheme = 'sip'
    								components
    									sip
    										userInfo
    											userOrTelephoneSubscriber = '001010123456789'
    											password = Omit
    										hostPort
    											host = 'ims.mnc001.mcc001.3gppnetwork.org'
    											portField = Omit
    								urlParameters = Omit
    								headers = Omit
    					fromParams
    						GenericParam
    							id = 'tag'
    							paramValue
    								tokenOrHost = '1584742388'
    				geolocation = Omit
    				geolocationRouting = Omit
    				historyInfo = Omit
    				infoPackage = Omit
    				inReplyTo = Omit
    				maxForwards
    					fieldName = MAX_FORWARDS_E (21)
    					forwards = 70
    				mimeVersion = Omit
    				minExpires = Omit
    				minSE = Omit
    				organization = Omit
    				pAccessNetworkInfo
    					fieldName = P_ACCESS_NETWORK_INFO_E (65)
    					accessType = '3GPP-NR-TDD'
    					genericParams
    						GenericParam
    							id = 'utran-cell-id-3gpp'
    							paramValue
    								tokenOrHost = '00101000001000000400'
    				pAssertedID = Omit
    				pAssertedService = Omit
    				pAssociatedURI = Omit
    				path = Omit
    				pCalledPartyID = Omit
    				pChargingFunctionAddresses = Omit
    				pChargingVector = Omit
    				pEarlyMedia = Omit
    				pMediaAuthorization = Omit
    				pPreferredID = Omit
    				pPreferredService = Omit
    				priority = Omit
    				privacy = Omit
    				proxyAuthenticate = Omit
    				proxyAuthorization = Omit
    				proxyRequire
    					fieldName = PROXY_REQUIRE_E (28)
    					optionsTags
    						CharacterStringType = 'sec-agree'
    				pVisitedNetworkID = Omit
    				rAck = Omit
    				rSeq = Omit
    				reason = Omit
    				recordRoute = Omit
    				recvInfo = Omit
    				requestDisposition = Omit
    				referredBy = Omit
    				referTo = Omit
    				referSub = Omit
    				replaces = Omit
    				replyTo = Omit
    				require
    					fieldName = REQUIRE_E (31)
    					optionsTags
    						CharacterStringType = 'sec-agree'
    				retryAfter = Omit
    				route = Omit
    				securityClient
    					fieldName = SECURITY_CLIENT_E (62)
    					securityMech
    						SecurityMechanism
    							mechName = 'ipsec-3gpp'
    							mechParams
    								GenericParam
    									id = 'alg'
    									paramValue
    										tokenOrHost = 'hmac-md5-96'
    								GenericParam
    									id = 'ealg'
    									paramValue
    										tokenOrHost = 'des-ede3-cbc'
    								GenericParam
    									id = 'spi-c'
    									paramValue
    										tokenOrHost = '1298788414'
    								GenericParam
    									id = 'spi-s'
    									paramValue
    										tokenOrHost = '2838622844'
    								GenericParam
    									id = 'port-c'
    									paramValue
    										tokenOrHost = '41015'
    								GenericParam
    									id = 'port-s'
    									paramValue
    										tokenOrHost = '44724'
    						SecurityMechanism
    							mechName = 'ipsec-3gpp'
    							mechParams
    								GenericParam
    									id = 'alg'
    									paramValue
    										tokenOrHost = 'hmac-md5-96'
    								GenericParam
    									id = 'ealg'
    									paramValue
    										tokenOrHost = 'aes-cbc'
    								GenericParam
    									id = 'spi-c'
    									paramValue
    										tokenOrHost = '1298788414'
    								GenericParam
    									id = 'spi-s'
    									paramValue
    										tokenOrHost = '2838622844'
    								GenericParam
    									id = 'port-c'
    									paramValue
    										tokenOrHost = '41015'
    								GenericParam
    									id = 'port-s'
    									paramValue
    										tokenOrHost = '44724'
    						SecurityMechanism
    							mechName = 'ipsec-3gpp'
    							mechParams
    								GenericParam
    									id = 'alg'
    									paramValue
    										tokenOrHost = 'hmac-md5-96'
    								GenericParam
    									id = 'ealg'
    									paramValue
    										tokenOrHost = 'null'
    								GenericParam
    									id = 'spi-c'
    									paramValue
    										tokenOrHost = '1298788414'
    								GenericParam
    									id = 'spi-s'
    									paramValue
    										tokenOrHost = '2838622844'
    								GenericParam
    									id = 'port-c'
    									paramValue
    										tokenOrHost = '41015'
    								GenericParam
    									id = 'port-s'
    									paramValue
    										tokenOrHost = '44724'
    						SecurityMechanism
    							mechName = 'ipsec-3gpp'
    							mechParams
    								GenericParam
    									id = 'alg'
    									paramValue
    										tokenOrHost = 'hmac-sha-1-96'
    								GenericParam
    									id = 'ealg'
    									paramValue
    										tokenOrHost = 'des-ede3-cbc'
    								GenericParam
    									id = 'spi-c'
    									paramValue
    										tokenOrHost = '1298788414'
    								GenericParam
    									id = 'spi-s'
    									paramValue
    										tokenOrHost = '2838622844'
    								GenericParam
    									id = 'port-c'
    									paramValue
    										tokenOrHost = '41015'
    								GenericParam
    									id = 'port-s'
    									paramValue
    										tokenOrHost = '44724'
    						SecurityMechanism
    							mechName = 'ipsec-3gpp'
    							mechParams
    								GenericParam
    									id = 'alg'
    									paramValue
    										tokenOrHost = 'hmac-sha-1-96'
    								GenericParam
    									id = 'ealg'
    									paramValue
    										tokenOrHost = 'aes-cbc'
    								GenericParam
    									id = 'spi-c'
    									paramValue
    										tokenOrHost = '1298788414'
    								GenericParam
    									id = 'spi-s'
    									paramValue
    										tokenOrHost = '2838622844'
    								GenericParam
    									id = 'port-c'
    									paramValue
    										tokenOrHost = '41015'
    								GenericParam
    									id = 'port-s'
    									paramValue
    										tokenOrHost = '44724'
    						SecurityMechanism
    							mechName = 'ipsec-3gpp'
    							mechParams
    								GenericParam
    									id = 'alg'
    									paramValue
    										tokenOrHost = 'hmac-sha-1-96'
    								GenericParam
    									id = 'ealg'
    									paramValue
    										tokenOrHost = 'null'
    								GenericParam
    									id = 'spi-c'
    									paramValue
    										tokenOrHost = '1298788414'
    								GenericParam
    									id = 'spi-s'
    									paramValue
    										tokenOrHost = '2838622844'
    								GenericParam
    									id = 'port-c'
    									paramValue
    										tokenOrHost = '41015'
    								GenericParam
    									id = 'port-s'
    									paramValue
    										tokenOrHost = '44724'
    				securityServer = Omit
    				securityVerify
    					fieldName = SECURITY_VERIFY_E (64)
    					securityMech
    						SecurityMechanism
    							mechName = 'ipsec-3gpp'
    							mechParams
    								GenericParam
    									id = 'alg'
    									paramValue
    										tokenOrHost = 'hmac-md5-96'
    								GenericParam
    									id = 'spi-c'
    									paramValue
    										tokenOrHost = '260'
    								GenericParam
    									id = 'spi-s'
    									paramValue
    										tokenOrHost = '256'
    								GenericParam
    									id = 'port-c'
    									paramValue
    										tokenOrHost = '5061'
    								GenericParam
    									id = 'port-s'
    									paramValue
    										tokenOrHost = '5062'
    								GenericParam
    									id = 'q'
    									paramValue
    										tokenOrHost = '0.9'
    						SecurityMechanism
    							mechName = 'ipsec-3gpp'
    							mechParams
    								GenericParam
    									id = 'alg'
    									paramValue
    										tokenOrHost = 'hmac-sha-1-96'
    								GenericParam
    									id = 'spi-c'
    									paramValue
    										tokenOrHost = '260'
    								GenericParam
    									id = 'spi-s'
    									paramValue
    										tokenOrHost = '256'
    								GenericParam
    									id = 'port-c'
    									paramValue
    										tokenOrHost = '5061'
    								GenericParam
    									id = 'port-s'
    									paramValue
    										tokenOrHost = '5062'
    								GenericParam
    									id = 'q'
    									paramValue
    										tokenOrHost = '0.7'
    				server = Omit
    				serviceRoute = Omit
    				sessionExpires = Omit
    				sessionId = Omit
    				sipETag = Omit
    				sipIfMatch = Omit
    				subject = Omit
    				subscriptionState = Omit
    				supported
    					fieldName = SUPPORTED_E (36)
    					optionsTags
    						CharacterStringType = 'path'
    						CharacterStringType = 'sec-agree'
    				timestamp = Omit
    				toField
    					fieldName = TO_E (38)
    					addressField
    						nameAddr
    							displayName = Omit
    							addrSpec
    								scheme = 'sip'
    								components
    									sip
    										userInfo
    											userOrTelephoneSubscriber = '001010123456789'
    											password = Omit
    										hostPort
    											host = 'ims.mnc001.mcc001.3gppnetwork.org'
    											portField = Omit
    								urlParameters = Omit
    								headers = Omit
    					toParams = Omit
    				unsupported = Omit
    				userToUser = Omit
    				userAgent
    					fieldName = USER_AGENT_E (40)
    					userAgentBody
    						CharacterStringType = 'qti_Lahaina for arm64_RKQ1.210107.001'
    				via
    					fieldName = VIA_E (41)
    					viaBody
    						ViaBody
    							sentProtocol
    								protocolName = 'SIP'
    								protocolVersion = '2.0'
    								transport = 'TCP'
    							sentBy
    								host = '3000::2:6c61:18ff:fe5d:9f1e'
    								portField = 44724
    							viaParams
    								GenericParam
    									id = 'branch'
    									paramValue
    										tokenOrHost = 'z9hG4bK35466275'
    				warning = Omit
    				wwwAuthenticate = Omit
    				resourcePriority = Omit
    				answerMode = Omit
    				privAnswerMode = Omit
    				targetDialog = Omit
    				pAnswerState = Omit
    				undefinedHeader_List = Omit
    			messageBody = Omit
    			payload = Omit

    Inter-component message: IMS_Server -> IMS1:IMS_Server

    summary = Message Mismatch: Expires.deltaSec
    MATCH_MISMATCH
    	Message Mismatch: Expires.deltaSec
    		fieldName = EXPIRES_E (18)
    		deltaSec = '0'

    Message Mismatch: Expires.deltaSec

    summary = Message Mismatch: GenericParam.paramValue
    MATCH_MISMATCH
    	Message Mismatch: GenericParam.paramValue
    		host = '3000::2:6c61:18ff:fe5d:9f1e'
    		portField = 44724

    Message Mismatch: GenericParam.paramValue

    summary = Message Mismatch: Contact.contactBody
    MATCH_MISMATCH
    	Message Mismatch: Contact.contactBody
    		fieldName = CONTACT_E (9)
    		contactBody
    			contactAddresses
    				ContactAddress
    					addressField
    						nameAddr
    							displayName = Omit
    							addrSpec
    								scheme = 'sip'
    								components
    									sip
    										userInfo
    											userOrTelephoneSubscriber = '7d50dd18-5ee3-4eaf-a145-d31d84987cb9'
    											password = Omit
    										hostPort
    											host = '3000::2:6c61:18ff:fe5d:9f1e'
    											portField = 44724
    								urlParameters = Omit
    								headers = Omit
    					contactParams
    						GenericParam
    							id = '+g.3gpp.accesstype'
    							paramValue
    								quotedString = 'cellular2'
    						GenericParam
    							id = '+sip.instance'
    							paramValue
    								quotedString = ''
    						GenericParam
    							id = '+g.3gpp.ps-data-off'
    							paramValue
    								quotedString = 'active'
    						GenericParam
    							id = 'audio'
    							paramValue = Omit
    						GenericParam
    							id = '+g.3gpp.nw-init-ussi'
    							paramValue = Omit
    						GenericParam
    							id = '+g.3gpp.smsip'
    							paramValue = Omit
    						GenericParam
    							id = '+g.3gpp.icsi-ref'
    							paramValue
    								quotedString = 'urn%3Aurn-7%3A3gpp-service.ims.icsi.mmtel'

    Message Mismatch: Contact.contactBody

    summary = Message Mismatch: HostPort.host
    MATCH_MISMATCH
    	Message Mismatch: HostPort.host
    		host = '3000::2:6c61:18ff:fe5d:9f1e'
    		portField = 44724

    Message Mismatch: HostPort.host

    ConstraintMismatch::Received:
    summary = Message Mismatch: SemicolonParam_List
    MATCH_MISMATCH
    	Message Mismatch: SemicolonParam_List

    ConstraintMismatch::Expected:
    summary = Message Mismatch: SemicolonParam_List
    MATCH_MISMATCH
    	Message Mismatch: SemicolonParam_List
    		GenericParam
    			id = 'tag'
    			paramValue = AnyOrOmit
    		GenericParam = AnyOrOmit

    Message Mismatch: SemicolonParam_List

    summary = Message Mismatch: GenericParam.paramValue.tokenOrHost
    MATCH_MISMATCH
    	Message Mismatch: GenericParam.paramValue.tokenOrHost
    		fieldName = SECURITY_CLIENT_E (62)
    		securityMech
    			SecurityMechanism
    				mechName = 'ipsec-3gpp'
    				mechParams
    					GenericParam
    						id = 'alg'
    						paramValue
    							tokenOrHost = 'hmac-md5-96'
    					GenericParam
    						id = 'ealg'
    						paramValue
    							tokenOrHost = 'des-ede3-cbc'
    					GenericParam
    						id = 'spi-c'
    						paramValue
    							tokenOrHost = '1298788414'
    					GenericParam
    						id = 'spi-s'
    						paramValue
    							tokenOrHost = '2838622844'
    					GenericParam
    						id = 'port-c'
    						paramValue
    							tokenOrHost = '41015'
    					GenericParam
    						id = 'port-s'
    						paramValue
    							tokenOrHost = '44724'
    			SecurityMechanism
    				mechName = 'ipsec-3gpp'
    				mechParams
    					GenericParam
    						id = 'alg'
    						paramValue
    							tokenOrHost = 'hmac-md5-96'
    					GenericParam
    						id = 'ealg'
    						paramValue
    							tokenOrHost = 'aes-cbc'
    					GenericParam
    						id = 'spi-c'
    						paramValue
    							tokenOrHost = '1298788414'
    					GenericParam
    						id = 'spi-s'
    						paramValue
    							tokenOrHost = '2838622844'
    					GenericParam
    						id = 'port-c'
    						paramValue
    							tokenOrHost = '41015'
    					GenericParam
    						id = 'port-s'
    						paramValue
    							tokenOrHost = '44724'
    			SecurityMechanism
    				mechName = 'ipsec-3gpp'
    				mechParams
    					GenericParam
    						id = 'alg'
    						paramValue
    							tokenOrHost = 'hmac-md5-96'
    					GenericParam
    						id = 'ealg'
    						paramValue
    							tokenOrHost = 'null'
    					GenericParam
    						id = 'spi-c'
    						paramValue
    							tokenOrHost = '1298788414'
    					GenericParam
    						id = 'spi-s'
    						paramValue
    							tokenOrHost = '2838622844'
    					GenericParam
    						id = 'port-c'
    						paramValue
    							tokenOrHost = '41015'
    					GenericParam
    						id = 'port-s'
    						paramValue
    							tokenOrHost = '44724'
    			SecurityMechanism
    				mechName = 'ipsec-3gpp'
    				mechParams
    					GenericParam
    						id = 'alg'
    						paramValue
    							tokenOrHost = 'hmac-sha-1-96'
    					GenericParam
    						id = 'ealg'
    						paramValue
    							tokenOrHost = 'des-ede3-cbc'
    					GenericParam
    						id = 'spi-c'
    						paramValue
    							tokenOrHost = '1298788414'
    					GenericParam
    						id = 'spi-s'
    						paramValue
    							tokenOrHost = '2838622844'
    					GenericParam
    						id = 'port-c'
    						paramValue
    							tokenOrHost = '41015'
    					GenericParam
    						id = 'port-s'
    						paramValue
    							tokenOrHost = '44724'
    			SecurityMechanism
    				mechName = 'ipsec-3gpp'
    				mechParams
    					GenericParam
    						id = 'alg'
    						paramValue
    							tokenOrHost = 'hmac-sha-1-96'
    					GenericParam
    						id = 'ealg'
    						paramValue
    							tokenOrHost = 'aes-cbc'
    					GenericParam
    						id = 'spi-c'
    						paramValue
    							tokenOrHost = '1298788414'
    					GenericParam
    						id = 'spi-s'
    						paramValue
    							tokenOrHost = '2838622844'
    					GenericParam
    						id = 'port-c'
    						paramValue
    							tokenOrHost = '41015'
    					GenericParam
    						id = 'port-s'
    						paramValue
    							tokenOrHost = '44724'
    			SecurityMechanism
    				mechName = 'ipsec-3gpp'
    				mechParams
    					GenericParam
    						id = 'alg'
    						paramValue
    							tokenOrHost = 'hmac-sha-1-96'
    					GenericParam
    						id = 'ealg'
    						paramValue
    							tokenOrHost = 'null'
    					GenericParam
    						id = 'spi-c'
    						paramValue
    							tokenOrHost = '1298788414'
    					GenericParam
    						id = 'spi-s'
    						paramValue
    							tokenOrHost = '2838622844'
    					GenericParam
    						id = 'port-c'
    						paramValue
    							tokenOrHost = '41015'
    					GenericParam
    						id = 'port-s'
    						paramValue
    							tokenOrHost = '44724'

    Message Mismatch: GenericParam.paramValue.tokenOrHost

    summary = Message Mismatch: GenericParam.id
    MATCH_MISMATCH
    	Message Mismatch: GenericParam.id
    		fieldName = SECURITY_CLIENT_E (62)
    		securityMech
    			SecurityMechanism
    				mechName = 'ipsec-3gpp'
    				mechParams
    					GenericParam
    						id = 'alg'
    						paramValue
    							tokenOrHost = 'hmac-md5-96'
    					GenericParam
    						id = 'ealg'
    						paramValue
    							tokenOrHost = 'des-ede3-cbc'
    					GenericParam
    						id = 'spi-c'
    						paramValue
    							tokenOrHost = '1298788414'
    					GenericParam
    						id = 'spi-s'
    						paramValue
    							tokenOrHost = '2838622844'
    					GenericParam
    						id = 'port-c'
    						paramValue
    							tokenOrHost = '41015'
    					GenericParam
    						id = 'port-s'
    						paramValue
    							tokenOrHost = '44724'
    			SecurityMechanism
    				mechName = 'ipsec-3gpp'
    				mechParams
    					GenericParam
    						id = 'alg'
    						paramValue
    							tokenOrHost = 'hmac-md5-96'
    					GenericParam
    						id = 'ealg'
    						paramValue
    							tokenOrHost = 'aes-cbc'
    					GenericParam
    						id = 'spi-c'
    						paramValue
    							tokenOrHost = '1298788414'
    					GenericParam
    						id = 'spi-s'
    						paramValue
    							tokenOrHost = '2838622844'
    					GenericParam
    						id = 'port-c'
    						paramValue
    							tokenOrHost = '41015'
    					GenericParam
    						id = 'port-s'
    						paramValue
    							tokenOrHost = '44724'
    			SecurityMechanism
    				mechName = 'ipsec-3gpp'
    				mechParams
    					GenericParam
    						id = 'alg'
    						paramValue
    							tokenOrHost = 'hmac-md5-96'
    					GenericParam
    						id = 'ealg'
    						paramValue
    							tokenOrHost = 'null'
    					GenericParam
    						id = 'spi-c'
    						paramValue
    							tokenOrHost = '1298788414'
    					GenericParam
    						id = 'spi-s'
    						paramValue
    							tokenOrHost = '2838622844'
    					GenericParam
    						id = 'port-c'
    						paramValue
    							tokenOrHost = '41015'
    					GenericParam
    						id = 'port-s'
    						paramValue
    							tokenOrHost = '44724'
    			SecurityMechanism
    				mechName = 'ipsec-3gpp'
    				mechParams
    					GenericParam
    						id = 'alg'
    						paramValue
    							tokenOrHost = 'hmac-sha-1-96'
    					GenericParam
    						id = 'ealg'
    						paramValue
    							tokenOrHost = 'des-ede3-cbc'
    					GenericParam
    						id = 'spi-c'
    						paramValue
    							tokenOrHost = '1298788414'
    					GenericParam
    						id = 'spi-s'
    						paramValue
    							tokenOrHost = '2838622844'
    					GenericParam
    						id = 'port-c'
    						paramValue
    							tokenOrHost = '41015'
    					GenericParam
    						id = 'port-s'
    						paramValue
    							tokenOrHost = '44724'
    			SecurityMechanism
    				mechName = 'ipsec-3gpp'
    				mechParams
    					GenericParam
    						id = 'alg'
    						paramValue
    							tokenOrHost = 'hmac-sha-1-96'
    					GenericParam
    						id = 'ealg'
    						paramValue
    							tokenOrHost = 'aes-cbc'
    					GenericParam
    						id = 'spi-c'
    						paramValue
    							tokenOrHost = '1298788414'
    					GenericParam
    						id = 'spi-s'
    						paramValue
    							tokenOrHost = '2838622844'
    					GenericParam
    						id = 'port-c'
    						paramValue
    							tokenOrHost = '41015'
    					GenericParam
    						id = 'port-s'
    						paramValue
    							tokenOrHost = '44724'
    			SecurityMechanism
    				mechName = 'ipsec-3gpp'
    				mechParams
    					GenericParam
    						id = 'alg'
    						paramValue
    							tokenOrHost = 'hmac-sha-1-96'
    					GenericParam
    						id = 'ealg'
    						paramValue
    							tokenOrHost = 'null'
    					GenericParam
    						id = 'spi-c'
    						paramValue
    							tokenOrHost = '1298788414'
    					GenericParam
    						id = 'spi-s'
    						paramValue
    							tokenOrHost = '2838622844'
    					GenericParam
    						id = 'port-c'
    						paramValue
    							tokenOrHost = '41015'
    					GenericParam
    						id = 'port-s'
    						paramValue
    							tokenOrHost = '44724'

    Message Mismatch: GenericParam.id

    summary = Message Mismatch: GenericParam.id
    MATCH_MISMATCH
    	Message Mismatch: GenericParam.id
    		CharacterStringType = '3000::2:6c61:18ff:fe5d:9f1e'

    Message Mismatch: GenericParam.id

    ConstraintMismatch::Received:
    summary = Message Mismatch: GenericParam.id
    MATCH_MISMATCH
    	Message Mismatch: GenericParam.id
    		GenericParam
    			id = '+g.3gpp.accesstype'
    			paramValue
    				quotedString = 'cellular2'

    		GenericParam
    			id = '+sip.instance'
    			paramValue
    				quotedString = ''
    		GenericParam
    			id = '+g.3gpp.ps-data-off'
    			paramValue
    				quotedString = 'active'
    		GenericParam
    			id = 'audio'
    			paramValue = Omit
    		GenericParam
    			id = '+g.3gpp.nw-init-ussi'
    			paramValue = Omit
    		GenericParam
    			id = '+g.3gpp.smsip'
    			paramValue = Omit
    		GenericParam
    			id = '+g.3gpp.icsi-ref'
    			paramValue
    				quotedString = 'urn%3Aurn-7%3A3gpp-service.ims.icsi.mmtel'
    ConstraintMismatch::Expected:
    summary = Message Mismatch: GenericParam.id
    MATCH_MISMATCH
    	Message Mismatch: GenericParam.id
    		GenericParam
    			id = 'expires'
    			paramValue
    				quotedString = AnyValue
    				quotedString = AnyValue
    		GenericParam
    			id
    			paramValue
    				quotedString
    		GenericParam
    			id
    			paramValue
    				quotedString
    		GenericParam
    			id
    			paramValue
    		GenericParam
    			id
    			paramValue
    		GenericParam
    			id
    			paramValue
    		GenericParam
    			id
    			paramValue
    				quotedString

    Message Mismatch: GenericParam.id

    summary = Message Mismatch: Contact
    MATCH_MISMATCH
    	Message Mismatch: Contact
    		fieldName = CONTACT_E (9)
    		contactBody
    			contactAddresses
    				ContactAddress
    					addressField
    						nameAddr
    							displayName = Omit
    							addrSpec
    								scheme = 'sip'
    								components
    									sip
    										userInfo
    											userOrTelephoneSubscriber = '7d50dd18-5ee3-4eaf-a145-d31d84987cb9'
    											password = Omit
    										hostPort
    											host = '3000::2:6c61:18ff:fe5d:9f1e'
    											portField = 44724
    								urlParameters = Omit
    								headers = Omit
    					contactParams
    						GenericParam
    							id = '+g.3gpp.accesstype'
    							paramValue
    								quotedString = 'cellular2'
    						GenericParam
    							id = '+sip.instance'
    							paramValue
    								quotedString = ''
    						GenericParam
    							id = '+g.3gpp.ps-data-off'
    							paramValue
    								quotedString = 'active'
    						GenericParam
    							id = 'audio'
    							paramValue = Omit
    						GenericParam
    							id = '+g.3gpp.nw-init-ussi'
    							paramValue = Omit
    						GenericParam
    							id = '+g.3gpp.smsip'
    							paramValue = Omit
    						GenericParam
    							id = '+g.3gpp.icsi-ref'
    							paramValue
    								quotedString = 'urn%3Aurn-7%3A3gpp-service.ims.icsi.mmtel'

    Message Mismatch: Contact

    timerEvent = 6
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\Common\CommonDefs.ttcn
    testName = TC_7_34_NR5GC
    lineNo = 592
    outStr = Timer: t_Delay, Duration: 3s, Started: 06:16:54

    Timer: t_Delay, Duration: 3s, Started: 06:16:54

    IMS_DATA_RSP
    	RoutingInfo
    		Protocol = tcp (1)
    		Security = protectedContext1 (1)
    		UE_Address
    			V6
    				Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    				ScopeId = Omit
    		NW_Address
    			V6
    				Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    				ScopeId = Omit
    	Response
    		statusLine
    			sipVersion = 'SIP/2.0'
    			statusCode = 200
    			reasonPhrase = 'OK'
    		msgHeader
    			accept = Omit
    			acceptContact = Omit
    			acceptEncoding = Omit
    			acceptLanguage = Omit
    			alertInfo = Omit
    			allow = Omit
    			allowEvents = Omit
    			authenticationInfo = Omit
    			authorization = Omit
    			callId
    				fieldName = CALL_ID_E (7)
    				callid = '1583821721_207195148@3000::2:6c61:18ff:fe5d:9f1e'
    			callInfo = Omit
    			contact
    				fieldName = CONTACT_E (9)
    				contactBody
    					contactAddresses
    						ContactAddress
    							addressField
    								nameAddr
    									displayName = Omit
    									addrSpec
    										scheme = 'sip'
    										components
    											sip
    												userInfo
    													userOrTelephoneSubscriber = '7d50dd18-5ee3-4eaf-a145-d31d84987cb9'
    													password = Omit
    												hostPort
    													host = '3000::2:6c61:18ff:fe5d:9f1e'
    													portField = 44724
    										urlParameters = Omit
    										headers = Omit
    							contactParams
    								GenericParam
    									id = 'expires'
    									paramValue
    										tokenOrHost = '0'
    			contentDisposition = Omit
    			contentEncoding = Omit
    			contentLanguage = Omit
    			contentLength
    				fieldName = CONTENT_LENGTH_E (13)
    				len = 0
    			contentType = Omit
    			cSeq
    				fieldName = CSEQ_E (15)
    				seqNumber = 510079899
    				method = 'REGISTER'
    			date = Omit
    			errorInfo = Omit
    			event = Omit
    			expires = Omit
    			featureCaps = Omit
    			fromField
    				fieldName = FROM_E (19)
    				addressField
    					nameAddr
    						displayName = Omit
    						addrSpec
    							scheme = 'sip'
    							components
    								sip
    									userInfo
    										userOrTelephoneSubscriber = '001010123456789'
    										password = Omit
    									hostPort
    										host = 'ims.mnc001.mcc001.3gppnetwork.org'
    										portField = Omit
    							urlParameters = Omit
    							headers = Omit
    				fromParams
    					GenericParam
    						id = 'tag'
    						paramValue
    							tokenOrHost = '1584742388'
    			geolocation = Omit
    			geolocationRouting = Omit
    			historyInfo = Omit
    			infoPackage = Omit
    			inReplyTo = Omit
    			maxForwards = Omit
    			mimeVersion = Omit
    			minExpires = Omit
    			minSE = Omit
    			organization = Omit
    			pAccessNetworkInfo = Omit
    			pAssertedID = Omit
    			pAssertedService = Omit
    			pAssociatedURI
    				fieldName = P_ASSOCIATED_URI_E (66)
    				nameAddrList
    					NameAddrParam
    						nameAddr
    							displayName = Omit
    							addrSpec
    								scheme = 'sip'
    								components
    									sip
    										userInfo
    											userOrTelephoneSubscriber = '001010123456789'
    											password = Omit
    										hostPort
    											host = 'ims.mnc001.mcc001.3gppnetwork.org'
    											portField = Omit
    								urlParameters = Omit
    								headers = Omit
    						genericParams = Omit
    					NameAddrParam
    						nameAddr
    							displayName = Omit
    							addrSpec
    								scheme = 'sip'
    								components
    									sip
    										userInfo
    											userOrTelephoneSubscriber = '+11234567890'
    											password = Omit
    										hostPort
    											host = 'test.3gpp.com'
    											portField = Omit
    								urlParameters = Omit
    								headers = Omit
    						genericParams = Omit
    					NameAddrParam
    						nameAddr
    							displayName = Omit
    							addrSpec
    								scheme = 'sip'
    								components
    									sip
    										userInfo
    											userOrTelephoneSubscriber = 'user'
    											password = Omit
    										hostPort
    											host = 'test.3gpp.com'
    											portField = Omit
    								urlParameters = Omit
    								headers = Omit
    						genericParams = Omit
    					NameAddrParam
    						nameAddr
    							displayName = Omit
    							addrSpec
    								scheme = 'tel'
    								components
    									tel
    										subscriber = '+4989364072'
    								urlParameters = Omit
    								headers = Omit
    						genericParams = Omit
    			path
    				fieldName = PATH_E (61)
    				pathValues
    					PathValue
    						nameAddr
    							displayName = Omit
    							addrSpec
    								scheme = 'sip'
    								components
    									sip
    										userInfo = Omit
    										hostPort
    											host = 'fd29:cc43:7fb9:2:20c:29ff:fe66:b4c7'
    											portField = Omit
    								urlParameters
    									GenericParam
    										id = 'lr'
    										paramValue = Omit
    								headers = Omit
    						rrParam = Omit
    			pCalledPartyID = Omit
    			pChargingFunctionAddresses = Omit
    			pChargingVector = Omit
    			pEarlyMedia = Omit
    			pMediaAuthorization = Omit
    			pPreferredID = Omit
    			pPreferredService = Omit
    			priority = Omit
    			privacy = Omit
    			proxyAuthenticate = Omit
    			proxyAuthorization = Omit
    			proxyRequire = Omit
    			pVisitedNetworkID = Omit
    			rAck = Omit
    			rSeq = Omit
    			reason = Omit
    			recordRoute = Omit
    			recvInfo = Omit
    			requestDisposition = Omit
    			referredBy = Omit
    			referTo = Omit
    			referSub = Omit
    			replaces = Omit
    			replyTo = Omit
    			require = Omit
    			retryAfter = Omit
    			route = Omit
    			securityClient = Omit
    			securityServer = Omit
    			securityVerify = Omit
    			server = Omit
    			serviceRoute
    				fieldName = SERVICE_ROUTE_E (71)
    				routeBody
    					RouteBody
    						nameAddr
    							displayName = Omit
    							addrSpec
    								scheme = 'sip'
    								components
    									sip
    										userInfo = Omit
    										hostPort
    											host = 'scscf.3gpp.org'
    											portField = Omit
    								urlParameters
    									GenericParam
    										id = 'lr'
    										paramValue = Omit
    								headers = Omit
    						rrParam = Omit
    			sessionExpires = Omit
    			sessionId = Omit
    			sipETag = Omit
    			sipIfMatch = Omit
    			subject = Omit
    			subscriptionState = Omit
    			supported = Omit
    			timestamp = Omit
    			toField
    				fieldName = TO_E (38)
    				addressField
    					nameAddr
    						displayName = Omit
    						addrSpec
    							scheme = 'sip'
    							components
    								sip
    									userInfo
    										userOrTelephoneSubscriber = '001010123456789'
    										password = Omit
    									hostPort
    										host = 'ims.mnc001.mcc001.3gppnetwork.org'
    										portField = Omit
    							urlParameters = Omit
    							headers = Omit
    				toParams
    					GenericParam
    						id = 'tag'
    						paramValue
    							tokenOrHost = 'abc-REGISTER-Totag'
    			unsupported = Omit
    			userToUser = Omit
    			userAgent = Omit
    			via
    				fieldName = VIA_E (41)
    				viaBody
    					ViaBody
    						sentProtocol
    							protocolName = 'SIP'
    							protocolVersion = '2.0'
    							transport = 'TCP'
    						sentBy
    							host = '3000::2:6c61:18ff:fe5d:9f1e'
    							portField = 44724
    						viaParams
    							GenericParam
    								id = 'branch'
    								paramValue
    									tokenOrHost = 'z9hG4bK35466275'
    			warning = Omit
    			wwwAuthenticate = Omit
    			resourcePriority = Omit
    			answerMode = Omit
    			privAnswerMode = Omit
    			targetDialog = Omit
    			pAnswerState = Omit
    			undefinedHeader_List = Omit
    		messageBody = Omit
    		payload = Omit

    Inter-component message: IMS_Server -> IP:IMS_Server

    IP_SOCKET_REQ
    	DATA
    		ConnectionId
    			Protocol = tcp (1)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 5062
    			Remote
    				IpAddr
    					V6
    						Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    						ScopeId = Omit
    				Port = 43642
    		Req
    			TCP
    				Send = '5349502F322E3020323030204F4B0D0A5669613A205349502F322E302F544350205B333030303A3A323A366336313A313866663A666535643A396631655D3A34343732343B6272616E63683D7A39684734624B33353436363237350D0A46726F6D3A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E3B7461673D313538343734323338380D0A546F3A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E3B7461673D6162632D52454749535445522D546F7461670D0A43616C6C2D49443A20313538333832313732315F32303731393531343840333030303A3A323A366336313A313866663A666535643A396631650D0A435365713A203531303037393839392052454749535445520D0A436F6E746163743A203C7369703A37643530646431382D356565332D346561662D613134352D643331643834393837636239405B333030303A3A323A366336313A313866663A666535643A396631655D3A34343732343E3B657870697265733D300D0A502D4173736F6369617465642D5552493A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E2C3C7369703A2B313132333435363738393040746573742E336770702E636F6D3E2C3C7369703A7573657240746573742E336770702E636F6D3E2C3C74656C3A2B343938393336343037323E0D0A506174683A203C7369703A5B666432393A636334333A376662393A323A3230633A323966663A666536363A623463375D3B6C723E0D0A536572766963652D526F7574653A203C7369703A73637363662E336770702E6F72673B6C723E0D0A436F6E74656E742D4C656E6774683A20300D0A0D0A'O

    Inter-component message: IP_SOCK_DATA -> IPMUX:IP_SOCK_DATA

    SipMessage
    	Message Header = SIP/2.0 200 OK
    Via: SIP/2.0/TCP [3000::2:6c61:18ff:fe5d:9f1e]:44724;branch=z9hG4bK35466275
    From: ;tag=1584742388
    To: ;tag=abc-REGISTER-Totag
    Call-ID: 1583821721_207195148@3000::2:6c61:18ff:fe5d:9f1e
    CSeq: 510079899 REGISTER
    Contact: ;expires=0
    P-Associated-URI: ,,,
    Path:
    Service-Route:
    Content-Length: 0

    Status:SIP/2.0 200 OK

    IP_SOCKET_REQ
    	DATA
    		ConnectionId
    			Protocol = tcp (1)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 5062
    			Remote
    				IpAddr
    					V6
    						Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    						ScopeId = Omit
    				Port = 43642
    		Req
    			TCP
    				Send = '5349502F322E3020323030204F4B0D0A5669613A205349502F322E302F544350205B333030303A3A323A366336313A313866663A666535643A396631655D3A34343732343B6272616E63683D7A39684734624B33353436363237350D0A46726F6D3A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E3B7461673D313538343734323338380D0A546F3A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E3B7461673D6162632D52454749535445522D546F7461670D0A43616C6C2D49443A20313538333832313732315F32303731393531343840333030303A3A323A366336313A313866663A666535643A396631650D0A435365713A203531303037393839392052454749535445520D0A436F6E746163743A203C7369703A37643530646431382D356565332D346561662D613134352D643331643834393837636239405B333030303A3A323A366336313A313866663A666535643A396631655D3A34343732343E3B657870697265733D300D0A502D4173736F6369617465642D5552493A203C7369703A30303130313031323334353637383940696D732E6D6E633030312E6D63633030312E336770706E6574776F726B2E6F72673E2C3C7369703A2B313132333435363738393040746573742E336770702E636F6D3E2C3C7369703A7573657240746573742E336770702E636F6D3E2C3C74656C3A2B343938393336343037323E0D0A506174683A203C7369703A5B666432393A636334333A376662393A323A3230633A323966663A666536363A623463375D3B6C723E0D0A536572766963652D526F7574653A203C7369703A73637363662E336770702E6F72673B6C723E0D0A436F6E74656E742D4C656E6774683A20300D0A0D0A'O

    Sent from port: IPMUX:IP_SOCK

    UL-DCCH-Message
    	message = c1 = ulInformationTransfer =
    		criticalExtensions = ulInformationTransfer =
    			dedicatedNAS-Message = 7E0290C8101008ABE56482D4D726B7FD761F76E37C2974D0

    ulInformationTransfer

    NR_RRC_PDU_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 2
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 444
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ulInformationTransfer
    						criticalExtensions
    							ulInformationTransfer
    								dedicatedNAS_Message = '7E0290C8101008ABE56482D4D726B7FD761F76E37C2974D0'O
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Received on port: NASEMU_NRNG:SYS_SRB

    DEREGISTRATION REQUEST ORIGINATED
    	Extended protocol discriminator = 0x7E [ 126 ]
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Spare half octet [4 bits] = 0x0 [ 0 ]
    	dereg_req_mt [8 bits] = 0x45 [ 69 ]
    	de_reg_tp
    		switch_off [1 bit] = 0x0 [ 0 ]
    		re_reg_req [1 bit] = 0x0 [ 0 ]
    		Access_typ [2 bits] = 0x0 [ 0 ]
    	ngksi
    		Type of security context flag [1 bit] = 0x1 [ 1 ]
    		nas_key_set_identi [3 bits] = 0x1 [ 1 ]
    	fivegs_mob_id
    		iel [16 bits] = 0xB [ 11 ]
    		id_dig [4 bits] = 0xF [ 15 ]
    		Spare bits [1 bit] = 0x0 [ 0 ]
    		typ_id [3 bits] = 0x2 [ 2 ]
    		mcc_dig_2 [4 bits] = 0x0 [ 0 ]
    		mcc_dig_1 [4 bits] = 0x0 [ 0 ]
    		Mobile network code digit 3 [4 bits] = 0xF [ 15 ]
    		Mobile country code digit 3 [4 bits] = 0x1 [ 1 ]
    		mnc_dig_2 [4 bits] = 0x1 [ 1 ]
    		mnc_dig_1 [4 bits] = 0x0 [ 0 ]
    		amf_reg_id = 0xFE [ 254 ]
    		amf_set_id = 0x00 [ 0 ]
    		amf_set_id_conti [2 bits] = 0x1 [ 1 ]
    		amf_pntr [6 bits] = 0x1 [ 1 ]
    		fiveg_tmsi = 0xC2345678 [ 3258209912 ]

    DEREGISTRATION REQUEST ORIGINATED PDU

    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		CTRL
    			ConnectionId
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5062
    				Remote
    					IpAddr
    						V6
    							Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    							ScopeId = Omit
    					Port = 43642
    			Ind
    				TCP
    					Close = True

    Message Mismatch: IP_SOCKET_IND

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = tcp (1)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 5062
    			Remote
    				IpAddr
    					V6
    						Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    						ScopeId = Omit
    				Port = 43642
    		Ind
    			TCP
    				Close = True

    Received on port: IPMUX:IP_SOCK

    summary = Message Mismatch: IP_SOCKET_IND.CTRL.Ind.TCP
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND.CTRL.Ind.TCP
    		CTRL
    			ConnectionId
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5062
    				Remote
    					IpAddr
    						V6
    							Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    							ScopeId = Omit
    					Port = 43642
    			Ind
    				TCP
    					Close = True

    Message Mismatch: IP_SOCKET_IND.CTRL.Ind.TCP

    summary = Message Mismatch: IP_SOCKET_IND.CTRL.ConnectionId.Local.Port
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND.CTRL.ConnectionId.Local.Port
    		CTRL
    			ConnectionId
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5062
    				Remote
    					IpAddr
    						V6
    							Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    							ScopeId = Omit
    					Port = 43642
    			Ind
    				TCP
    					Close = True

    Message Mismatch: IP_SOCKET_IND.CTRL.ConnectionId.Local.Port

    summary = Message Mismatch: IP_SOCKET_IND.CTRL.Ind.TCP
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND.CTRL.Ind.TCP
    		CTRL
    			ConnectionId
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5062
    				Remote
    					IpAddr
    						V6
    							Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    							ScopeId = Omit
    					Port = 43642
    			Ind
    				TCP
    					Close = True

    Message Mismatch: IP_SOCKET_IND.CTRL.Ind.TCP

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = tcp (1)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 5062
    			Remote
    				IpAddr
    					V6
    						Addr = '3000:0000:0000:0002:6c61:18ff:fe5d:9f1e'
    						ScopeId = Omit
    				Port = 43642
    		Ind
    			TCP
    				Close = True

    Inter-component message: IP_SOCK_CTRL -> IP:IP_SOCK_CTRL

    NR_SRB_COMMON_IND
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 2
    		RoutingInfoSUL = Omit
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 444
    				Subframe
    					Number = 9
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    	Signalling
    		Rrc = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0010'B
    					NasCount = '00000008'O
    				Pdu
    					Msg
    						deregistration_RequestMO
    							protocolDiscriminator = 01111110'B
    							spareHalfOctet = '0'H
    							securityHeaderType = 0000'B
    							messageType = 01000101'B
    							ngKSI
    								iei = Omit
    								tsc = 0'B
    								nasKeySetId = 000'B
    							deregistrationType
    								switchOff = 1'B
    								reRegistration = 0'B
    								accessType = 01'B
    							ngMobileId
    								iei = Omit
    								iel = '000B'O
    								idDigit1 = 1111'B
    								oddEvenInd = 0'B
    								typeOfId = 010'B
    								otherDigits = '00F110FE0041C2345678'O
    					PiggybackedPduList = Omit

    Inter-component message: SRB -> NR5GC:SRB

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		EnquireTiming = True

    Sent from port: NR5GC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 448
    				Subframe
    					Number = 4
    				HSFN
    					Number = 92
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		Result
    			Success = True
    	Confirm
    		EnquireTiming = True

    Received on port: NR5GC:SYS

    timerEvent = 6
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\NR5GC\NR5GC_RRCSteps.ttcn
    testName = TC_7_34_NR5GC
    lineNo = 326
    outStr = Timer: t_Timer, Duration: 1.22s, Started: 06:16:54

    Timer: t_Timer, Duration: 1.22s, Started: 06:16:54

    NR_SRB_COMMON_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 478
    				Subframe
    					Number = 7
    				HSFN
    					Number = 92
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcRelease
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcRelease
    									redirectedCarrierInfo = Omit
    									cellReselectionPriorities = Omit
    									suspendConfig = Omit
    									deprioritisationReq = Omit
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: TC_SRB -> NASEMU_NRNG:TC_SRB

    DL-DCCH-Message
    	message = c1 = rrcRelease =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcRelease =

    rrcRelease

    NR_RRC_PDU_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		RlcBearerRouting
    			NR = nr_Cell1 (1)
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 478
    				Subframe
    					Number = 7
    				HSFN
    					Number = 92
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcRelease
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcRelease
    								redirectedCarrierInfo = Omit
    								cellReselectionPriorities = Omit
    								suspendConfig = Omit
    								deprioritisationReq = Omit
    								lateNonCriticalExtension = Omit
    								nonCriticalExtension = Omit

    Sent from port: NASEMU_NRNG:SYS_SRB

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		PdcpCount
    			Get
    				AllRBs = True

    Sent from port: NR5GC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		PdcpCount
    			Get
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 1
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000011'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000010'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 2
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000001'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    				NR_PdcpCountInfo_Type
    					RadioBearerId
    						Drb = 1
    					UL
    						Format = PdcpCount_DrbSQN18 (2)
    						Value = 00000000000000000000000000000110'B
    					DL
    						Format = PdcpCount_DrbSQN18 (2)
    						Value = 00000000000000000000000000000101'B

    Received on port: NR5GC:SYS

    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 478
    			Subframe
    				Number = 7
    			HSFN
    				Number = 92
    			Slot
    				SlotOffset
    					Numerology1 = 0

    Message Mismatch: TimingInfo_Type

    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 478
    			Subframe
    				Number = 7
    			HSFN
    				Number = 92
    			Slot
    				SlotOffset
    					Numerology1 = 0

    Message Mismatch: TimingInfo_Type

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 478
    				Subframe
    					Number = 7
    				HSFN
    					Number = 92
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		Cell
    			AddOrReconfigure
    				StaticResourceConfig = Omit
    				CellConfigCommon = Omit
    				PhysicalLayer = Omit
    				BcchConfig = Omit
    				PcchConfig = Omit
    				RachProcedureConfig = Omit
    				DcchDtchConfig
    					DL = Omit
    					UL
    						SearchSpaceAndDci
    							AssignedBWPs = Omit
    							SearchSpaceType = Omit
    							DciInfo = Omit
    						PUCCH_Synch
    							None = True
    						GrantConfig
    							None = True
    					DrxCtrl = Omit
    					MeasGapCtrl = Omit
    				ServingCellConfig = Omit

    Sent from port: NR5GC:SYS

    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 479
    			Subframe
    				Number = 2
    			HSFN
    				Number = 92
    			Slot
    				SlotOffset
    					Numerology1 = 0

    Message Mismatch: TimingInfo_Type

    Sender = RequestServer
    Text = Received OK from Device Under Test

    RequestServer:Received OK from Device Under Test

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 479
    				Subframe
    					Number = 2
    				HSFN
    					Number = 92
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		AS_Security
    			Release = True

    Sent from port: NR5GC:SYS

    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 484
    			Subframe
    				Number = 2
    			HSFN
    				Number = 92
    			Slot
    				SlotOffset
    					Numerology1 = 0

    Message Mismatch: TimingInfo_Type

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 484
    				Subframe
    					Number = 2
    				HSFN
    					Number = 92
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		RadioBearerList
    			NR_RadioBearer_Type
    				Id
    					Srb = 1
    				Config
    					Release = True
    			NR_RadioBearer_Type
    				Id
    					Srb = 2
    				Config
    					Release = True
    			NR_RadioBearer_Type
    				Id
    					Drb = 1
    				Config
    					Release = True

    Sent from port: NR5GC:SYS

    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 484
    			Subframe
    				Number = 7
    			HSFN
    				Number = 92
    			Slot
    				SlotOffset
    					Numerology1 = 0

    Message Mismatch: TimingInfo_Type

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 484
    				Subframe
    					Number = 7
    				HSFN
    					Number = 92
    				Slot
    					SlotOffset
    						Numerology1 = 0
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		RadioBearerList
    			NR_RadioBearer_Type
    				Id
    					Srb = 1
    				Config
    					AddOrReconfigure
    						Sdap
    							None = True
    						Pdcp
    							RBTerminating
    								RbConfig
    									Params
    										Rb
    											Srb = True
    								LinkToOtherCellGroup
    									None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										AM
    											Tx
    												R15
    													sn_FieldLength = size12 (0)
    													t_PollRetransmit = ms45 (8)
    													pollPDU = infinity_ (23)
    													pollByte = infinity_ (43)
    													maxRetxThreshold = t8 (5)
    											Rx
    												R15
    													sn_FieldLength = size12 (0)
    													t_Reassembly = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    									TestMode
    										None = True
    								LogicalChannelId = 1
    								Mac
    									LogicalChannel
    										Priority = 1
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit
    			NR_RadioBearer_Type
    				Id
    					Srb = 2
    				Config
    					AddOrReconfigure
    						Sdap
    							None = True
    						Pdcp
    							RBTerminating
    								RbConfig
    									Params
    										Rb
    											Srb = True
    								LinkToOtherCellGroup
    									None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										AM
    											Tx
    												R15
    													sn_FieldLength = size12 (0)
    													t_PollRetransmit = ms45 (8)
    													pollPDU = infinity_ (23)
    													pollByte = infinity_ (43)
    													maxRetxThreshold = t8 (5)
    											Rx
    												R15
    													sn_FieldLength = size12 (0)
    													t_Reassembly = ms35 (7)
    													t_StatusProhibit = ms0 (0)
    									TestMode
    										None = True
    								LogicalChannelId = 2
    								Mac
    									LogicalChannel
    										Priority = 3
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit

    Sent from port: NR5GC:SYS

    timerEvent = 9
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\NR5GC\NR5GC_RRCSteps.ttcn
    testName = TC_7_34_NR5GC
    lineNo = 334
    outStr = Timer: t_Timer, Expired: 06:16:56

    Timer: t_Timer, Expired: 06:16:56

    Sender = RequestServer
    Text = [!SWITCH_OFF] Complete

    RequestServer:[!SWITCH_OFF] Complete

    Sender = !SWITCH_OFF
    Text = Stopping and Starting Serial Device Device Under Test

    !SWITCH_OFF:Stopping and Starting Serial Device Device Under Test

    Sender = RequestServer
    Text = Device Device Under Test Disconnected

    RequestServer:Device Device Under Test Disconnected

    Sender = Device Under Test
    Text = Opening RS232 Port COM17,9600,None,8,One,None,Timeout:25000 ms

    Device Under Test:Opening RS232 Port COM17,9600,None,8,One,None,Timeout:25000 ms

    Sender = RequestServer
    Text = Device Device Under Test Connected

    RequestServer:Device Device Under Test Connected

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		Cell
    			Release = True

    Sent from port: NR5GC:SYS

    recordType = 24
    summary = Postamble

    Postamble

    IntermediateVerdict = (None)
    summary = Intermediate verdict: (NONE)

    Intermediate verdict: (NONE)

    timerEvent = 9
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\Common\CommonDefs.ttcn
    testName = TC_7_34_NR5GC
    lineNo = 593
    outStr = Timer: t_Delay, Expired: 06:16:57

    Timer: t_Delay, Expired: 06:16:57

    summary = Message Mismatch: IMS_CONFIG_REQ
    MESSAGE_MISMATCH
    	Message Mismatch: IMS_CONFIG_REQ
    		CloseTCP = True

    Message Mismatch: IMS_CONFIG_REQ

    summary = Message Mismatch: IMS_CONFIG_REQ
    MESSAGE_MISMATCH
    	Message Mismatch: IMS_CONFIG_REQ
    		CloseTCP = True

    Message Mismatch: IMS_CONFIG_REQ

    summary = Message Mismatch: IMS_CONFIG_REQ
    MESSAGE_MISMATCH
    	Message Mismatch: IMS_CONFIG_REQ
    		CloseTCP = True

    Message Mismatch: IMS_CONFIG_REQ

    IMS_CONFIG_REQ
    	CloseTCP = True

    Inter-component message: IMS_CTRL -> IP:IMS_CTRL

    IMS_CONFIG_CNF
    	CloseTCP = True

    Inter-component message: IMS_CTRL -> IMS1:IMS_CTRL

    IMS_IPCAN_Coordination_MSG
    	TriggerEvent = True

    Inter-component message: IPCAN -> IMS1:IPCAN

    IntermediateVerdict = (Pass)
    summary = Intermediate verdict: (PASS)

    Intermediate verdict: (PASS)

    IntermediateVerdict = (Pass)
    summary = Intermediate verdict: (PASS)

    Intermediate verdict: (PASS)

    verdict = PASS
    summary = Test case ended: TC_7_34_NR5GC, Verdict: PASS

    Test case ended: TC_7_34_NR5GC, Verdict: PASS

    IntermediateVerdict = (None)
    summary = Intermediate verdict: (NONE)

    Intermediate verdict: (NONE)

    IntermediateVerdict = (None)
    summary = Intermediate verdict: (NONE)

    Intermediate verdict: (NONE)

    IntermediateVerdict = (None)
    summary = Intermediate verdict: (NONE)

    Intermediate verdict: (NONE)

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 149
    text = Unmapping port "MTC_IMS:Ut" from port "SYSTEM_IMS:Ut"

    Unmapping port "MTC_IMS:Ut" from port "SYSTEM_IMS:Ut"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 149
    text = Unmapping port "IP:IP_CTRL" from port "SYSTEM_IMS:IP_CTRL"

    Unmapping port "IP:IP_CTRL" from port "SYSTEM_IMS:IP_CTRL"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 149
    text = Unmapping port "IP:IPSEC_CTRL" from port "SYSTEM_IMS:IPSEC_CTRL"

    Unmapping port "IP:IPSEC_CTRL" from port "SYSTEM_IMS:IPSEC_CTRL"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 149
    text = Unmapping port "IPMUX:IP_SOCK" from port "SYSTEM_IMS:IP_SOCK"

    Unmapping port "IPMUX:IP_SOCK" from port "SYSTEM_IMS:IP_SOCK"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 149
    text = Unmapping port "NR5GC:SYS" from port "SYSTEM_IMS:NR_SYS"

    Unmapping port "NR5GC:SYS" from port "SYSTEM_IMS:NR_SYS"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 149
    text = Unmapping port "NR5GC:SYSIND" from port "SYSTEM_IMS:NR_SYSIND"

    Unmapping port "NR5GC:SYSIND" from port "SYSTEM_IMS:NR_SYSIND"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 149
    text = Unmapping port "NR5GC:DRB" from port "SYSTEM_IMS:NR_DRB"

    Unmapping port "NR5GC:DRB" from port "SYSTEM_IMS:NR_DRB"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 149
    text = Unmapping port "NASEMU_NRNG:SYS_SRB" from port "SYSTEM_IMS:NR_SRB"

    Unmapping port "NASEMU_NRNG:SYS_SRB" from port "SYSTEM_IMS:NR_SRB"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 149
    text = Disconnecting port "MTC_IMS:PTC_Ut" from port "IMS1:MMI"

    Disconnecting port "MTC_IMS:PTC_Ut" from port "IMS1:MMI"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 149
    text = Disconnecting port "MTC_IMS:PTC_Ut" from port "NR5GC:UT"

    Disconnecting port "MTC_IMS:PTC_Ut" from port "NR5GC:UT"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 149
    text = Disconnecting port "IMS1:IMS_CTRL" from port "IP:IMS_CTRL"

    Disconnecting port "IMS1:IMS_CTRL" from port "IP:IMS_CTRL"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 149
    text = Disconnecting port "IMS1:IMS_Client" from port "IP:IMS_Client"

    Disconnecting port "IMS1:IMS_Client" from port "IP:IMS_Client"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 149
    text = Disconnecting port "IMS1:IMS_Server" from port "IP:IMS_Server"

    Disconnecting port "IMS1:IMS_Server" from port "IP:IMS_Server"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 149
    text = Disconnecting port "IMS1:IPCAN" from port "NR5GC:IMS"

    Disconnecting port "IMS1:IPCAN" from port "NR5GC:IMS"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 149
    text = Disconnecting port "IP:IP_SOCK_DATA" from port "IPMUX:IP_SOCK_DATA"

    Disconnecting port "IP:IP_SOCK_DATA" from port "IPMUX:IP_SOCK_DATA"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 149
    text = Disconnecting port "IP:IP_SOCK_CTRL" from port "IPMUX:IP_SOCK_CTRL"

    Disconnecting port "IP:IP_SOCK_CTRL" from port "IPMUX:IP_SOCK_CTRL"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 149
    text = Disconnecting port "IP:NR_CTRL" from port "NR5GC:IP"

    Disconnecting port "IP:NR_CTRL" from port "NR5GC:IP"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 149
    text = Disconnecting port "NR5GC:NASCTRL" from port "NASEMU_NRNG:CTRL"

    Disconnecting port "NR5GC:NASCTRL" from port "NASEMU_NRNG:CTRL"

    recordType = 24
    fileName = C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v66.0\IMS_Testsuite_NR5GC\Common\MTC\MTC_Base.ttcn
    descriptionId = TC_7_34_NR5GC
    lineNo = 149
    text = Disconnecting port "NR5GC:SRB" from port "NASEMU_NRNG:TC_SRB"

    Disconnecting port "NR5GC:SRB" from port "NASEMU_NRNG:TC_SRB"

    Sender = RequestServer
    Text = Received !Stop, PASS from SAT Controller PC

    RequestServer:Received !Stop, PASS from SAT Controller PC

    Sender = RequestServer
    Text = Request received [!Stop, PASS]

    RequestServer:Request received [!Stop, PASS]

    Sender = RequestServer
    Text = Request [!Stop, PASS] not found in message file, does not meet Pass Through criteria

    RequestServer:Request [!Stop, PASS] not found in message file, does not meet Pass Through criteria

    Sender = RequestServer
    Text = Acknowledgment to SAT Contoller PC !OK

    RequestServer:Acknowledgment to SAT Contoller PC !OK

    Sender = SAT Controller PC
    Text = Sent "!OK"

    SAT Controller PC:Sent "!OK"

    recordType = 24
    fileName
    descriptionId = TC_7_34_NR5GC
    lineNo = 0
    text = Test Procedure: Final Verdict

    Test Procedure: Final Verdict

    recordType = 24
    summary = Final Verdict

    Final Verdict

    verdict = PASS
    summary = TEST CASE ENDED: TC_7_34_NR5GC

    TEST CASE ENDED: TC_7_34_NR5GC

    Sender = RequestServer
    Text = Disconnected event from Controller SAT Controller PC Received

    RequestServer:Disconnected event from Controller SAT Controller PC Received

    Sender = RequestServer
    Text = State changed from RunningConnected to RunningNotConnected

    RequestServer:State changed from RunningConnected to RunningNotConnected

    Sender = SAT Controller PC
    Text = Binding TCP Server to port 6667

    SAT Controller PC:Binding TCP Server to port 6667

    Sender = SAT Controller PC
    Text = Listening TCP Server to port 6667

    SAT Controller PC:Listening TCP Server to port 6667

    Server State Change to RunningNotConnected