MSG #80 2021-09-06 13:32:30.712
NAS

     EMM: EMM information
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x2 (Integrity protected and ciphered)
    Auth code = 0x91e050f9
    Sequence number = 0x03
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x0 (Plain NAS message, not security protected)
    Message type = 0x61 (EMM information)
    Full name for network:
      Length = 12
      Data = 84 cd e1 14 44 0d 87 a7 f4 b4 fb 0c
    Short name for network:
      Length = 8
      Data = 80 d4 70 78 4a 4f bb cf
    Local time zone = 128
    Universal time and local time zone:
      Data = 12 90 60 11 23 03 80
    Network daylight saving time:
      Length = 1
      Data = 01