ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 13:30:56.673 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 13:30:56.677 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 13:30:56.677 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 13:30:56.679 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 13:30:56.680 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 13:30:56.680 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:805: IMS UDP port 192.168.2.3:5060 configured
7 | 13:30:56.682 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:755: IMS TCP port 192.168.2.3:5060 configured!
8 | 13:30:56.684 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:776: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 13:30:56.684 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:787: IdM port 192.168.2.3:8080 configured!
10 | 13:30:56.686 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 13:30:57.888 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 13:30:57.890 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 13:30:59.740 |  | ←RRC BCCH SIB |  |  |
14 | 13:30:59.745 |  | ←RRC BCCH SIB1 |  |  |
15 | 13:30:59.760 |  | ←RRC BCCH SIB |  |  |
16 | 13:30:59.780 |  | ←RRC BCCH SIB |  |  |
17 | 13:30:59.825 |  | ←RRC BCCH SIB1 |  |  |
18 | 13:32:30.349 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 13:32:30.349 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 13:32:30.349 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 13:32:30.349 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 13:32:30.400 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 13:32:30.400 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 13:32:30.400 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 13:32:30.400 |  |  |  | →NAS EMM Attach request |  |
26 | 13:32:30.400 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 13:32:30.400 |  |  |  | NAS K-asme f4f0b6c9fb0f3ed0ce270058f59d8a8a... |  |
28 | 13:32:30.400 |  |  |  | NAS ← EMM Authentication request |  |
29 | 13:32:30.401 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 13:32:30.401 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 13:32:30.402 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 13:32:30.472 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 13:32:30.472 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 13:32:30.472 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 13:32:30.472 |  |  |  | →NAS EMM Authentication response |  |
36 | 13:32:30.472 |  |  |  | NAS UE auth OK |  |
37 | 13:32:30.472 |  |  |  | NAS K-nas-cip 6f2af8d847257e5d99c901908d894... |  |
38 | 13:32:30.472 |  |  |  | NAS K-nas-int 6ac852ea8461540b305560d1b07f4... |  |
39 | 13:32:30.472 |  |  |  | NAS ← EMM Security mode command |  |
40 | 13:32:30.473 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 13:32:30.473 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 13:32:30.474 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 13:32:30.512 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
44 | 13:32:30.512 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 13:32:30.512 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xb) |  |  |
46 | 13:32:30.512 |  |  |  | →NAS EMM Security mode complete |  |
47 | 13:32:30.512 |  |  |  | NAS ← ESM ESM information request |  |
48 | 13:32:30.513 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xc) |  |  |
49 | 13:32:30.513 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 13:32:30.514 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
51 | 13:32:30.522 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
52 | 13:32:30.560 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
53 | 13:32:30.560 |  | →RRC DCCH UL Information Transfer |  |  |
54 | 13:32:30.560 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x9) |  |  |
55 | 13:32:30.560 |  |  |  | →NAS ESM ESM information response |  |
56 | 13:32:30.560 |  |  |  | NAS ← EMM Attach accept |  |
57 | 13:32:30.560 |  |  |  | NAS K-enb 165b91a5ba01b24c4d4f53a15524431fa... |  |
58 | 13:32:30.561 |  | ←RRC DCCH Security Mode Command |  |  |
59 | 13:32:30.561 |  |  | RRC K-enb 165b91a5ba01b24c4d4f53a15524431fa... |  |  |
60 | 13:32:30.561 |  |  | RRC rrc-cip 3912024cd440c8463116f2a78226ab1... |  |  |
61 | 13:32:30.561 |  |  | RRC rrc-int fcbbc6f22f1a164248761dc0373d2b6... |  |  |
62 | 13:32:30.561 |  |  | RRC up-cip 887eb362a638bbf4ca342a5ec1a4310d... |  |  |
63 | 13:32:30.561 |  |  | RRC up-int 37d026fe78028906f5a131ae0f763fc0... |  |  |
64 | 13:32:30.562 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
65 | 13:32:30.592 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
66 | 13:32:30.592 |  | →RRC DCCH Security Mode Complete |  |  |
67 | 13:32:30.592 |  | ←RRC DCCH UE Capability Enquiry |  |  |
68 | 13:32:30.592 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
69 | 13:32:30.642 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
70 | 13:32:30.642 |  | →RRC DCCH UE Capability Information |  |  |
71 | 13:32:30.643 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x4) |  |  |
72 | 13:32:30.643 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
73 | 13:32:30.643 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
74 | 13:32:30.672 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
75 | 13:32:30.672 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
76 | 13:32:30.712 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
77 | 13:32:30.712 |  | →RRC DCCH UL Information Transfer |  |  |
78 | 13:32:30.712 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x9) |  |  |
79 | 13:32:30.712 |  |  |  | →NAS EMM Attach complete |  |
80 | 13:32:30.712 |  |  |  | NAS ← EMM EMM information |  |
81 | 13:32:30.713 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x9) |  |  |
82 | 13:32:30.713 |  | ←RRC DCCH DL Information Transfer |  |  |
83 | 13:32:30.714 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
84 | 13:32:35.153 |  | ←RRC DCCH RRC Connection Release |  |  |
85 | 13:32:35.154 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
86 | 13:32:36.419 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
87 | 13:32:36.419 |  | →RRC CCCH RRC Connection Request |  |  |
88 | 13:32:36.419 |  | ←RRC CCCH RRC Connection Setup |  |  |
89 | 13:32:36.419 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
90 | 13:32:36.472 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
91 | 13:32:36.472 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
92 | 13:32:36.472 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
93 | 13:32:36.472 |  |  |  | →NAS EMM Service request |  |
94 | 13:32:36.472 |  |  |  | NAS K-enb af0c8c908b0037d932ff402fddb3aa490... |  |
95 | 13:32:36.473 |  | ←RRC DCCH Security Mode Command |  |  |
96 | 13:32:36.473 |  |  | RRC K-enb af0c8c908b0037d932ff402fddb3aa490... |  |  |
97 | 13:32:36.473 |  |  | RRC rrc-cip a2d9a050040bc6deb481dc6c2d8e35c... |  |  |
98 | 13:32:36.473 |  |  | RRC rrc-int 2a8cabb60bdaf65a88ab177d71915c7... |  |  |
99 | 13:32:36.473 |  |  | RRC up-cip 7d715e68fa3d4751bb845967b7d22c94... |  |  |
100 | 13:32:36.473 |  |  | RRC up-int bad9d3b970a80e2b18f06dbae1c66856... |  |  |
101 | 13:32:36.474 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
102 | 13:32:36.512 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
103 | 13:32:36.512 |  | →RRC DCCH Security Mode Complete |  |  |
104 | 13:32:36.512 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
105 | 13:32:36.512 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
106 | 13:32:36.552 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
107 | 13:32:36.552 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
108 | 13:32:51.152 | →enobeB PCAP frame→ TCP |  |  |  |
109 | 13:32:51.155 |  | ←enobeB PCAP frame← TCP |  |  |
110 | 13:32:51.192 | →enobeB PCAP frame→ TCP |  |  |  |
111 | 13:32:51.280 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
112 | 13:32:51.283 |  | ←enobeB PCAP frame← TCP |  |  |
113 | 13:32:51.289 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
114 | 13:32:51.312 | →enobeB PCAP frame→ TCP |  |  |  |
115 | 13:32:51.440 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
116 | 13:32:51.443 |  | ←enobeB PCAP frame← TCP |  |  |
117 | 13:32:51.443 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 16)
118 | 13:32:51.444 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
119 | 13:32:51.472 | →enobeB PCAP frame→ TCP |  |  |  |
120 | 13:32:51.520 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
121 | 13:32:51.523 |  | ←enobeB PCAP frame← TCP |  |  |
122 | 13:32:51.523 |  |  |  |  | →HTTP GET | HTTP-Proxy
123 | 13:32:51.529 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:288: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
124 | 13:32:51.548 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
125 | 13:32:51.552 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
126 | 13:32:51.592 | →enobeB PCAP frame→ TCP |  |  |  |
127 | 13:32:53.432 | →enobeB PCAP frame→ TCP |  |  |  |
128 | 13:32:53.435 |  | ←enobeB PCAP frame← TCP |  |  |
129 | 13:32:53.472 | →enobeB PCAP frame→ TCP |  |  |  |
130 | 13:32:53.480 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
131 | 13:32:53.483 |  | ←enobeB PCAP frame← TCP |  |  |
132 | 13:32:53.488 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
133 | 13:32:53.512 | →enobeB PCAP frame→ TCP |  |  |  |
134 | 13:32:53.840 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
135 | 13:32:53.842 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:642: Client connected to IdM port (id 18)
136 | 13:32:53.843 |  | ←enobeB PCAP frame← TCP |  |  |
137 | 13:32:53.844 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
138 | 13:32:53.872 | →enobeB PCAP frame→ TCP |  |  |  |
139 | 13:32:53.880 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
140 | 13:32:53.884 |  |  |  |  | →HTTP GET | IDMS-Endpoint
141 | 13:32:53.885 |  | ←enobeB PCAP frame← TCP |  |  |
142 | 13:32:53.911 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
143 | 13:32:53.913 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
144 | 13:32:53.915 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:511: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
145 | 13:32:53.915 |  |  |  |  | MMICmd: Please provide user credentials: username and password
146 | 13:32:53.992 | →enobeB PCAP frame→ TCP |  |  |  |
147 | 13:33:14.840 | →enobeB PCAP frame→ HTTPS: POST /idms/userauth HTTP/1.1 |  |  |  |
148 | 13:33:14.843 |  | ←enobeB PCAP frame← TCP |  |  |
149 | 13:33:14.844 |  |  |  |  | →HTTP POST | IDMS-Endpoint
150 | 13:33:14.859 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
151 | 13:33:14.862 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
152 | 13:33:14.862 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:516: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
153 | 13:33:14.912 | →enobeB PCAP frame→ TCP |  |  |  |
154 | 13:33:14.920 | →enobeB PCAP frame→ TCP |  |  |  |
155 | 13:33:14.921 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:677: IdM port - Client closed the connection (id 18)
156 | 13:33:14.923 |  | ←enobeB PCAP frame← TCP |  |  |
157 | 13:33:14.952 | →enobeB PCAP frame→ TCP |  |  |  |
158 | 13:33:15.392 | →enobeB PCAP frame→ TCP |  |  |  |
159 | 13:33:15.395 |  | ←enobeB PCAP frame← TCP |  |  |
160 | 13:33:15.432 | →enobeB PCAP frame→ TCP |  |  |  |
161 | 13:33:15.440 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
162 | 13:33:15.443 |  | ←enobeB PCAP frame← TCP |  |  |
163 | 13:33:15.444 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
164 | 13:33:15.472 | →enobeB PCAP frame→ TCP |  |  |  |
165 | 13:33:15.560 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
166 | 13:33:15.562 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:642: Client connected to IdM port (id 18)
167 | 13:33:15.563 |  | ←enobeB PCAP frame← TCP |  |  |
168 | 13:33:15.564 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
169 | 13:33:15.592 | →enobeB PCAP frame→ TCP |  |  |  |
170 | 13:33:15.600 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
171 | 13:33:15.602 |  |  |  |  | →HTTP POST | IDMS-Endpoint
172 | 13:33:15.606 |  | ←enobeB PCAP frame← TCP |  |  |
173 | 13:33:15.619 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
174 | 13:33:15.621 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
175 | 13:33:15.621 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:521: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
176 | 13:33:15.672 | →enobeB PCAP frame→ TCP |  |  |  |
177 | 13:33:15.952 | →enobeB PCAP frame→ TCP |  |  |  |
178 | 13:33:15.955 |  | ←enobeB PCAP frame← TCP |  |  |
179 | 13:33:15.992 | →enobeB PCAP frame→ TCP |  |  |  |
180 | 13:33:16.000 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
181 | 13:33:16.003 |  | ←enobeB PCAP frame← TCP |  |  |
182 | 13:33:16.006 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
183 | 13:33:16.032 | →enobeB PCAP frame→ TCP |  |  |  |
184 | 13:33:16.080 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
185 | 13:33:16.083 |  | ←enobeB PCAP frame← TCP |  |  |
186 | 13:33:16.083 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 19)
187 | 13:33:16.084 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
188 | 13:33:16.160 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
189 | 13:33:16.164 |  | ←enobeB PCAP frame← TCP |  |  |
190 | 13:33:16.164 |  |  |  |  | →HTTP POST | HTTP-Proxy
191 | 13:33:16.190 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:541: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
192 | 13:33:16.197 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
193 | 13:33:16.201 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
194 | 13:33:16.232 | →enobeB PCAP frame→ TCP |  |  |  |
195 | 13:33:16.272 | →enobeB PCAP frame→ TCP |  |  |  |
196 | 13:33:16.275 |  | ←enobeB PCAP frame← TCP |  |  |
197 | 13:33:16.312 | →enobeB PCAP frame→ TCP |  |  |  |
198 | 13:33:16.320 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
199 | 13:33:16.323 |  | ←enobeB PCAP frame← TCP |  |  |
200 | 13:33:16.327 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
201 | 13:33:16.392 | →enobeB PCAP frame→ TCP |  |  |  |
202 | 13:33:16.400 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
203 | 13:33:16.403 |  | ←enobeB PCAP frame← TCP |  |  |
204 | 13:33:16.403 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 20)
205 | 13:33:16.404 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
206 | 13:33:16.440 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
207 | 13:33:16.443 |  | ←enobeB PCAP frame← TCP |  |  |
208 | 13:33:16.443 |  |  |  |  | →HTTP POST | HTTP-Proxy
209 | 13:33:16.506 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
210 | 13:33:16.506 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:545: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
211 | 13:33:16.508 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
212 | 13:33:16.552 | →enobeB PCAP frame→ TCP |  |  |  |
213 | 13:33:16.640 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
214 | 13:33:16.644 |  |  |  |  | →SIP REGISTER | P-CSCF
215 | 13:33:16.665 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:814: IMS UDP_s port 192.168.2.3:5062 configured
216 | 13:33:16.693 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:765: IMS TCP_s port 192.168.2.3:5062 configured!
217 | 13:33:16.695 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:823: IMS UDP_c port 192.168.2.3:5061 configured
218 | 13:33:16.701 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
219 | 13:33:17.280 | →enobeB PCAP frame→ SIP over IPSEC: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
220 | 13:33:17.285 |  |  |  |  | →SIP REGISTER | P-CSCF
221 | 13:33:17.309 |  |  |  |  | ←SIP 200 OK | P-CSCF
222 | 13:33:17.312 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
223 | 13:33:17.640 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
224 | 13:33:17.641 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
225 | 13:33:17.642 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 SIP over IPSEC: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 |  |  |  |
226 | 13:33:17.655 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
227 | 13:33:17.714 |  |  |  |  | ←SIP 200 OK | P-CSCF
228 | 13:33:17.714 |  |  |  |  | MIKEY | Media-Server
229 | 13:33:17.716 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
230 | 13:33:17.935 |  |  |  |  | XML→ | Media-Server
231 | 13:33:17.936 |  |  |  |  | XML→ | Media-Server
232 | 13:33:17.940 |  |  |  |  | ←XML | Media-Server
233 | 13:33:17.943 |  |  |  |  | ←SIP NOTIFY | P-CSCF
234 | 13:33:17.946 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:44436;transp... |  |  |
235 | 13:33:18.000 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
236 | 13:33:18.003 |  |  |  |  | →SIP 200 OK | P-CSCF
237 | 13:33:18.272 | →enobeB PCAP frame→ TCP |  |  |  |
238 | 13:33:18.275 |  | ←enobeB PCAP frame← TCP |  |  |
239 | 13:33:18.312 | →enobeB PCAP frame→ TCP |  |  |  |
240 | 13:33:18.320 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
241 | 13:33:18.323 |  | ←enobeB PCAP frame← TCP |  |  |
242 | 13:33:18.328 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
243 | 13:33:18.352 | →enobeB PCAP frame→ TCP |  |  |  |
244 | 13:33:18.440 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
245 | 13:33:18.442 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
246 | 13:33:18.443 |  | ←enobeB PCAP frame← TCP |  |  |
247 | 13:33:18.444 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
248 | 13:33:18.472 | →enobeB PCAP frame→ TCP |  |  |  |
249 | 13:33:18.480 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-co... |  |  |  |
250 | 13:33:18.482 |  |  |  |  | →HTTP GET | HTTP-Proxy
251 | 13:33:18.483 |  | ←enobeB PCAP frame← TCP |  |  |
252 | 13:33:18.488 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:642: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcptt-ue-configuration.xml
253 | 13:33:18.494 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
254 | 13:33:18.496 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
255 | 13:33:18.552 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
256 | 13:33:18.554 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
257 | 13:33:18.555 |  | ←enobeB PCAP frame← TCP |  |  |
258 | 13:33:18.560 | →enobeB PCAP frame→ TCP |  |  |  |
259 | 13:33:18.563 |  | ←enobeB PCAP frame← TCP |  |  |
260 | 13:33:18.592 | →enobeB PCAP frame→ TCP |  |  |  |
261 | 13:33:18.712 | →enobeB PCAP frame→ TCP |  |  |  |
262 | 13:33:18.715 |  | ←enobeB PCAP frame← TCP |  |  |
263 | 13:33:18.752 | →enobeB PCAP frame→ TCP |  |  |  |
264 | 13:33:18.760 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
265 | 13:33:18.763 |  | ←enobeB PCAP frame← TCP |  |  |
266 | 13:33:18.766 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
267 | 13:33:18.792 | →enobeB PCAP frame→ TCP |  |  |  |
268 | 13:33:18.880 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
269 | 13:33:18.883 |  | ←enobeB PCAP frame← TCP |  |  |
270 | 13:33:18.883 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
271 | 13:33:18.884 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
272 | 13:33:18.912 | →enobeB PCAP frame→ TCP |  |  |  |
273 | 13:33:18.920 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-... |  |  |  |
274 | 13:33:18.923 |  | ←enobeB PCAP frame← TCP |  |  |
275 | 13:33:18.923 |  |  |  |  | →HTTP GET | HTTP-Proxy
276 | 13:33:18.934 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:647: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcptt-user-profile-49.xml
277 | 13:33:18.973 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
278 | 13:33:18.981 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
279 | 13:33:18.982 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
280 | 13:33:19.032 | →enobeB PCAP frame→ TCP |  |  |  |
281 | 13:33:19.040 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
282 | 13:33:19.042 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
283 | 13:33:19.043 |  | ←enobeB PCAP frame← TCP |  |  |
284 | 13:33:19.072 | →enobeB PCAP frame→ TCP |  |  |  |
285 | 13:33:19.680 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
286 | 13:33:19.681 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
287 | 13:33:19.695 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
288 | 13:33:19.753 |  |  |  |  | ←SIP 200 OK | P-CSCF
289 | 13:33:19.753 |  |  |  |  | MIKEY | Media-Server
290 | 13:33:19.755 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
291 | 13:33:19.803 |  | ←enobeB PCAP frame← TCP |  |  |
292 | 13:33:19.883 |  | ←enobeB PCAP frame← TCP |  |  |
293 | 13:33:19.884 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
294 | 13:33:19.912 | →enobeB PCAP frame→ TCP |  |  |  |
295 | 13:33:19.960 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
296 | 13:33:19.961 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
297 | 13:33:19.963 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
298 | 13:33:19.970 |  |  |  |  | XML→ | Media-Server
299 | 13:33:19.972 |  |  |  |  | XML→ | Media-Server
300 | 13:33:19.976 |  |  |  |  | ←XML | Media-Server
301 | 13:33:19.978 |  |  |  |  | ←SIP NOTIFY | P-CSCF
302 | 13:33:19.981 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:44436;transp... |  |  |
303 | 13:33:19.992 | →enobeB PCAP frame→ TCP |  |  |  |
304 | 13:33:20.000 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
305 | 13:33:20.001 |  |  |  |  | →HTTP GET | HTTP-Proxy
306 | 13:33:20.003 |  | ←enobeB PCAP frame← TCP |  |  |
307 | 13:33:20.004 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:652: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
308 | 13:33:20.009 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
309 | 13:33:20.012 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
310 | 13:33:20.013 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
311 | 13:33:20.024 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
312 | 13:33:20.027 |  |  |  |  | →SIP 200 OK | P-CSCF
313 | 13:33:20.072 | →enobeB PCAP frame→ TCP |  |  |  |
314 | 13:33:20.080 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
315 | 13:33:20.082 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
316 | 13:33:20.083 |  | ←enobeB PCAP frame← TCP |  |  |
317 | 13:33:20.112 | →enobeB PCAP frame→ TCP |  |  |  |
318 | 13:33:20.152 | →enobeB PCAP frame→ TCP |  |  |  |
319 | 13:33:20.156 |  | ←enobeB PCAP frame← TCP |  |  |
320 | 13:33:20.192 | →enobeB PCAP frame→ TCP |  |  |  |
321 | 13:33:20.200 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
322 | 13:33:20.203 |  | ←enobeB PCAP frame← TCP |  |  |
323 | 13:33:20.206 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
324 | 13:33:20.232 | →enobeB PCAP frame→ TCP |  |  |  |
325 | 13:33:20.320 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
326 | 13:33:20.323 |  | ←enobeB PCAP frame← TCP |  |  |
327 | 13:33:20.323 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
328 | 13:33:20.324 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
329 | 13:33:20.352 | →enobeB PCAP frame→ TCP |  |  |  |
330 | 13:33:20.360 | →enobeB PCAP frame→ HTTPS: GET /xcap.gms.mcstaasting.com/org.openmobileallian... |  |  |  |
331 | 13:33:20.362 |  |  |  |  | →HTTP GET | HTTP-Proxy
332 | 13:33:20.363 |  | ←enobeB PCAP frame← TCP |  |  |
333 | 13:33:20.372 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:657: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at /xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
334 | 13:33:20.396 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
335 | 13:33:20.401 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
336 | 13:33:20.402 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
337 | 13:33:20.432 | →enobeB PCAP frame→ TCP |  |  |  |
338 | 13:33:20.440 | →enobeB PCAP frame→ TCP |  |  |  |
339 | 13:33:20.472 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
340 | 13:33:20.474 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
341 | 13:33:20.475 |  | ←enobeB PCAP frame← TCP |  |  |
342 | 13:33:20.480 | →enobeB PCAP frame→ TCP |  |  |  |
343 | 13:33:20.483 |  | ←enobeB PCAP frame← TCP |  |  |
344 | 13:33:20.512 | →enobeB PCAP frame→ TCP |  |  |  |
345 | 13:33:20.680 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
346 | 13:33:20.681 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
347 | 13:33:20.682 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
348 | 13:33:20.695 |  |  |  |  | →SIP PUBLISH | P-CSCF
349 | 13:33:20.742 |  |  |  |  | MIKEY | Media-Server
350 | 13:33:20.800 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
351 | 13:33:20.801 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
352 | 13:33:20.805 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
353 | 13:33:20.970 |  |  |  |  | XML→ | Media-Server
354 | 13:33:20.974 |  |  |  |  | ←SIP 200 OK | P-CSCF
355 | 13:33:20.976 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
356 | 13:33:20.977 |  |  |  |  | ←SIP 200 OK | P-CSCF
357 | 13:33:20.977 |  |  |  |  | MIKEY | Media-Server
358 | 13:33:20.979 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
359 | 13:33:21.182 |  |  |  |  | XML→ | Media-Server
360 | 13:33:21.183 |  |  |  |  | XML→ | Media-Server
361 | 13:33:21.218 |  |  |  |  | ←XML | Media-Server
362 | 13:33:21.223 |  |  |  |  | ←SIP NOTIFY | P-CSCF
363 | 13:33:21.225 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:44436;transp... |  |  |
364 | 13:33:21.280 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
365 | 13:33:21.282 |  |  |  |  | →SIP 200 OK | P-CSCF
366 | 13:33:21.286 |  |  |  |  | ←XML | Media-Server
367 | 13:33:21.297 |  |  |  |  | ←SIP MESSAGE | P-CSCF
368 | 13:33:21.300 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
369 | 13:33:22.120 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
370 | 13:33:22.123 |  |  |  |  | →SIP 200 OK | P-CSCF
371 | 13:33:22.129 |  |  |  |  | Info: MCX_IMS_CommonProcedures.ttcn:155: MESSAGE/200OK Table 5.3.2.3-2 Steps 7-8 Done
372 | 13:33:22.133 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
373 | 13:33:22.152 | →enobeB PCAP frame→ TCP |  |  |  |
374 | 13:33:22.192 | →enobeB PCAP frame→ TCP |  |  |  |
375 | 13:33:24.132 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
376 | 13:33:24.169 |  | ←RRC DCCH RRC Connection Release |  |  |
377 | 13:33:24.170 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
378 | 13:33:24.189 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
379 | 13:33:24.202 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:735: SRTP config: Master Key: 838CB72A2F04D91EC5F9711AFA4B0FBF, Master Salt: 3A62F5F143305C04942523CE, MKI: 2C22C0FA
380 | 13:33:24.202 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
381 | 13:33:24.205 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
382 | 13:33:24.207 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
383 | 13:33:24.223 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
384 | 13:33:24.223 |  |  |  |  | ←XML | Media-Server
385 | 13:33:24.249 |  |  |  |  | ←SIP INVITE | P-CSCF
386 | 13:33:24.599 |  | ←enobeB PCAP frame← LTE RRC PCCH Paging (1 PagingRecord) |  |  |
387 | 13:33:24.599 |  | ←RRC PCCH Paging |  |  |
388 | 13:33:24.639 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
389 | 13:33:24.639 |  | →RRC CCCH RRC Connection Request |  |  |
390 | 13:33:24.639 |  | ←RRC CCCH RRC Connection Setup |  |  |
391 | 13:33:24.639 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
392 | 13:33:24.672 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
393 | 13:33:24.672 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
394 | 13:33:24.672 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
395 | 13:33:24.672 |  |  |  | →NAS EMM Service request |  |
396 | 13:33:24.672 |  |  |  | NAS K-enb eaa06ba6893b15d3bcaf792b03927f5cb... |  |
397 | 13:33:24.673 |  | ←RRC DCCH Security Mode Command |  |  |
398 | 13:33:24.673 |  |  | RRC K-enb eaa06ba6893b15d3bcaf792b03927f5cb... |  |  |
399 | 13:33:24.673 |  |  | RRC rrc-cip c8a4ac3caca3b72e3eeda90202718bd... |  |  |
400 | 13:33:24.673 |  |  | RRC rrc-int 30b8b71380e06a85031509ccc49eff1... |  |  |
401 | 13:33:24.673 |  |  | RRC up-cip 472fa947fd08f441e8635c798c86e500... |  |  |
402 | 13:33:24.673 |  |  | RRC up-int 78bb0b8dd7a02ab91057ca15e4017424... |  |  |
403 | 13:33:24.674 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
404 | 13:33:24.712 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
405 | 13:33:24.712 |  | →RRC DCCH Security Mode Complete |  |  |
406 | 13:33:24.712 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
407 | 13:33:24.712 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
408 | 13:33:24.752 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
409 | 13:33:24.752 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
410 | 13:33:24.754 |  | ←enobeB PCAP frame← SIP over IPSEC: INVITE sip:PublicUserId-A@192.168.3.2:44436;transp... |  |  |
411 | 13:33:24.800 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 100 Trying |  |  |  |
412 | 13:33:24.803 |  |  |  |  | →SIP 100 Trying | P-CSCF
413 | 13:33:24.840 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
414 | 13:33:24.841 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
415 | 13:33:24.848 |  |  |  |  | →SIP 200 OK | P-CSCF
416 | 13:33:24.878 |  |  |  |  | XML→ | Media-Server
417 | 13:33:24.886 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:612: 200 OK Verdict: Pass
418 | 13:33:24.887 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:538: Step 1 Verdict: Pass
419 | 13:33:24.891 |  |  |  |  | ←SIP ACK | P-CSCF
420 | 13:33:24.892 |  |  |  |  | ←Floor Taken | Media-Server
421 | 13:33:24.893 |  | ←enobeB PCAP frame← SIP over IPSEC: ACK sip:PublicUserId-A@192.168.3.2:44436;transport... |  |  |
422 | 13:33:25.174 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
423 | 13:33:25.175 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x1) |  |  |
424 | 13:33:25.175 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
425 | 13:33:25.176 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
426 | 13:33:25.232 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
427 | 13:33:25.232 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
428 | 13:33:25.232 |  | →RRC DCCH UL Information Transfer |  |  |
429 | 13:33:25.232 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x3) |  |  |
430 | 13:33:25.232 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
431 | 13:33:25.299 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
432 | 13:33:25.312 | →enobeB PCAP frame→ |  |  |  |
433 | 13:33:25.314 |  |  |  |  | Floor ACK→ | Media-Server
434 | 13:33:25.317 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Ack Verdict: Pass
435 | 13:33:25.326 |  |  |  |  | ←SIP BYE | P-CSCF
436 | 13:33:25.328 |  | ←enobeB PCAP frame← SIP over IPSEC: BYE sip:PublicUserId-A@192.168.3.2:44436;transport... |  |  |
437 | 13:33:25.360 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
438 | 13:33:25.362 |  |  |  |  | →SIP 200 OK | P-CSCF
439 | 13:33:26.952 | →enobeB PCAP frame→ |  |  |  |
440 | 13:33:27.372 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
441 | 13:33:27.394 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
442 | 13:33:27.394 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xa) |  |  |
443 | 13:33:27.394 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
444 | 13:33:27.395 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
445 | 13:33:27.440 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
446 | 13:33:27.440 |  | →RRC DCCH UL Information Transfer |  |  |
447 | 13:33:27.440 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x8) |  |  |
448 | 13:33:27.440 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
449 | 13:33:27.507 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
450 | 13:33:27.508 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
451 | 13:33:27.543 |  | ←RRC DCCH RRC Connection Release |  |  |
452 | 13:33:27.544 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
453 | 13:33:27.563 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
454 | 13:33:27.564 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
455 | 13:33:27.566 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
456 | 13:33:28.315 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.