ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 13:41:53.475 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 13:41:53.478 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 13:41:53.478 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 13:41:53.480 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 13:41:53.481 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 13:41:53.482 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:805: IMS UDP port 192.168.2.3:5060 configured
7 | 13:41:53.484 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:755: IMS TCP port 192.168.2.3:5060 configured!
8 | 13:41:53.486 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:776: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 13:41:53.487 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:787: IdM port 192.168.2.3:8080 configured!
10 | 13:41:53.488 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 13:41:54.690 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 13:41:54.692 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 13:41:57.905 |  | ←RRC BCCH SIB1 |  |  |
14 | 13:41:57.980 |  | ←RRC BCCH SIB |  |  |
15 | 13:41:57.986 |  | ←RRC BCCH SIB1 |  |  |
16 | 13:41:58.001 |  | ←RRC BCCH SIB |  |  |
17 | 13:41:58.021 |  | ←RRC BCCH SIB |  |  |
18 | 13:43:11.099 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 13:43:11.099 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 13:43:11.099 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 13:43:11.099 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 13:43:11.160 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 13:43:11.161 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 13:43:11.161 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 13:43:11.161 |  |  |  | →NAS EMM Attach request |  |
26 | 13:43:11.161 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 13:43:11.161 |  |  |  | NAS K-asme 9b8b93141147869434f04356c608a9c6... |  |
28 | 13:43:11.161 |  |  |  | NAS ← EMM Authentication request |  |
29 | 13:43:11.161 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 13:43:11.162 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 13:43:11.163 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 13:43:11.232 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 13:43:11.232 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 13:43:11.232 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 13:43:11.233 |  |  |  | →NAS EMM Authentication response |  |
36 | 13:43:11.233 |  |  |  | NAS UE auth OK |  |
37 | 13:43:11.233 |  |  |  | NAS K-nas-cip c13fa1aed59ef191085864779976d... |  |
38 | 13:43:11.233 |  |  |  | NAS K-nas-int 99c2656ad47a5ece45d9b40e07dd9... |  |
39 | 13:43:11.233 |  |  |  | NAS ← EMM Security mode command |  |
40 | 13:43:11.234 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 13:43:11.234 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 13:43:11.234 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 13:43:11.243 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
44 | 13:43:11.273 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
45 | 13:43:11.273 |  | →RRC DCCH UL Information Transfer |  |  |
46 | 13:43:11.273 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xd) |  |  |
47 | 13:43:11.273 |  |  |  | →NAS EMM Security mode complete |  |
48 | 13:43:11.273 |  |  |  | NAS ← ESM ESM information request |  |
49 | 13:43:11.274 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x8) |  |  |
50 | 13:43:11.274 |  | ←RRC DCCH DL Information Transfer |  |  |
51 | 13:43:11.274 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
52 | 13:43:11.282 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
53 | 13:43:11.321 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
54 | 13:43:11.321 |  | →RRC DCCH UL Information Transfer |  |  |
55 | 13:43:11.321 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x5) |  |  |
56 | 13:43:11.321 |  |  |  | →NAS ESM ESM information response |  |
57 | 13:43:11.321 |  |  |  | NAS ← EMM Attach accept |  |
58 | 13:43:11.321 |  |  |  | NAS K-enb 63e87652339888be3aa02d02c36e8bc96... |  |
59 | 13:43:11.322 |  | ←RRC DCCH Security Mode Command |  |  |
60 | 13:43:11.322 |  |  | RRC K-enb 63e87652339888be3aa02d02c36e8bc96... |  |  |
61 | 13:43:11.322 |  |  | RRC rrc-cip d0a3f585c359d5f824175fcd61f03ba... |  |  |
62 | 13:43:11.322 |  |  | RRC rrc-int ec04943f3b17926c4cba94e06661eca... |  |  |
63 | 13:43:11.322 |  |  | RRC up-cip be7b0c96120cbfc91ce180b7d67a4142... |  |  |
64 | 13:43:11.322 |  |  | RRC up-int 2d163c9df1845dc9f0452fcdcb711298... |  |  |
65 | 13:43:11.323 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
66 | 13:43:11.352 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
67 | 13:43:11.352 |  | →RRC DCCH Security Mode Complete |  |  |
68 | 13:43:11.352 |  | ←RRC DCCH UE Capability Enquiry |  |  |
69 | 13:43:11.352 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
70 | 13:43:11.403 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
71 | 13:43:11.403 |  | →RRC DCCH UE Capability Information |  |  |
72 | 13:43:11.403 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x9) |  |  |
73 | 13:43:11.403 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
74 | 13:43:11.403 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
75 | 13:43:11.433 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
76 | 13:43:11.433 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
77 | 13:43:11.473 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
78 | 13:43:11.473 |  | →RRC DCCH UL Information Transfer |  |  |
79 | 13:43:11.473 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xd) |  |  |
80 | 13:43:11.473 |  |  |  | →NAS EMM Attach complete |  |
81 | 13:43:11.473 |  |  |  | NAS ← EMM EMM information |  |
82 | 13:43:11.474 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xae) |  |  |
83 | 13:43:11.474 |  | ←RRC DCCH DL Information Transfer |  |  |
84 | 13:43:11.475 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
85 | 13:43:16.885 |  | ←RRC DCCH RRC Connection Release |  |  |
86 | 13:43:16.885 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
87 | 13:43:18.190 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
88 | 13:43:18.190 |  | →RRC CCCH RRC Connection Request |  |  |
89 | 13:43:18.190 |  | ←RRC CCCH RRC Connection Setup |  |  |
90 | 13:43:18.190 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
91 | 13:43:18.233 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
92 | 13:43:18.233 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
93 | 13:43:18.233 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
94 | 13:43:18.233 |  |  |  | →NAS EMM Service request |  |
95 | 13:43:18.233 |  |  |  | NAS K-enb 176e61d89db53c4b8364aab8c3106e2c1... |  |
96 | 13:43:18.234 |  | ←RRC DCCH Security Mode Command |  |  |
97 | 13:43:18.234 |  |  | RRC K-enb 176e61d89db53c4b8364aab8c3106e2c1... |  |  |
98 | 13:43:18.234 |  |  | RRC rrc-cip afba60c75681f50cad1e823b20e8bdb... |  |  |
99 | 13:43:18.234 |  |  | RRC rrc-int 337dbd813990c820d98d87159459c2d... |  |  |
100 | 13:43:18.234 |  |  | RRC up-cip dab5d5de9dc7eaf025e1e5d41b5a6cf1... |  |  |
101 | 13:43:18.234 |  |  | RRC up-int 7463b353d5e78ace50a0af271a791545... |  |  |
102 | 13:43:18.235 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
103 | 13:43:18.273 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
104 | 13:43:18.273 |  | →RRC DCCH Security Mode Complete |  |  |
105 | 13:43:18.273 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
106 | 13:43:18.273 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
107 | 13:43:18.312 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
108 | 13:43:18.312 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
109 | 13:43:33.072 | →enobeB PCAP frame→ TCP |  |  |  |
110 | 13:43:33.076 |  | ←enobeB PCAP frame← TCP |  |  |
111 | 13:43:33.113 | →enobeB PCAP frame→ TCP |  |  |  |
112 | 13:43:33.200 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
113 | 13:43:33.203 |  | ←enobeB PCAP frame← TCP |  |  |
114 | 13:43:33.210 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
115 | 13:43:33.233 | →enobeB PCAP frame→ TCP |  |  |  |
116 | 13:43:33.361 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
117 | 13:43:33.363 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 16)
118 | 13:43:33.364 |  | ←enobeB PCAP frame← TCP |  |  |
119 | 13:43:33.365 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
120 | 13:43:33.393 | →enobeB PCAP frame→ TCP |  |  |  |
121 | 13:43:33.480 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
122 | 13:43:33.483 |  |  |  |  | →HTTP GET | HTTP-Proxy
123 | 13:43:33.484 |  | ←enobeB PCAP frame← TCP |  |  |
124 | 13:43:33.491 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:288: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
125 | 13:43:33.510 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
126 | 13:43:33.513 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
127 | 13:43:33.515 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
128 | 13:43:33.553 | →enobeB PCAP frame→ TCP |  |  |  |
129 | 13:43:33.560 | →enobeB PCAP frame→ TCP |  |  |  |
130 | 13:43:35.472 | →enobeB PCAP frame→ TCP |  |  |  |
131 | 13:43:35.475 |  | ←enobeB PCAP frame← TCP |  |  |
132 | 13:43:35.512 | →enobeB PCAP frame→ TCP |  |  |  |
133 | 13:43:35.521 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
134 | 13:43:35.523 |  | ←enobeB PCAP frame← TCP |  |  |
135 | 13:43:35.530 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
136 | 13:43:35.553 | →enobeB PCAP frame→ TCP |  |  |  |
137 | 13:43:35.801 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
138 | 13:43:35.803 |  | ←enobeB PCAP frame← TCP |  |  |
139 | 13:43:35.803 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:642: Client connected to IdM port (id 18)
140 | 13:43:35.804 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
141 | 13:43:35.833 | →enobeB PCAP frame→ TCP |  |  |  |
142 | 13:43:35.841 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
143 | 13:43:35.844 |  | ←enobeB PCAP frame← TCP |  |  |
144 | 13:43:35.844 |  |  |  |  | →HTTP GET | IDMS-Endpoint
145 | 13:43:35.875 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
146 | 13:43:35.878 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
147 | 13:43:35.879 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:511: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
148 | 13:43:35.879 |  |  |  |  | MMICmd: Please provide user credentials: username and password
149 | 13:43:35.953 | →enobeB PCAP frame→ TCP |  |  |  |
150 | 13:43:42.921 | →enobeB PCAP frame→ HTTPS: POST /idms/userauth HTTP/1.1 |  |  |  |
151 | 13:43:42.923 |  | ←enobeB PCAP frame← TCP |  |  |
152 | 13:43:42.925 |  |  |  |  | →HTTP POST | IDMS-Endpoint
153 | 13:43:42.939 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
154 | 13:43:42.941 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:516: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
155 | 13:43:42.942 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
156 | 13:43:42.992 | →enobeB PCAP frame→ TCP |  |  |  |
157 | 13:43:43.001 | →enobeB PCAP frame→ TCP |  |  |  |
158 | 13:43:43.002 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:677: IdM port - Client closed the connection (id 18)
159 | 13:43:43.004 |  | ←enobeB PCAP frame← TCP |  |  |
160 | 13:43:43.033 | →enobeB PCAP frame→ TCP |  |  |  |
161 | 13:43:43.873 | →enobeB PCAP frame→ TCP |  |  |  |
162 | 13:43:43.876 |  | ←enobeB PCAP frame← TCP |  |  |
163 | 13:43:43.913 | →enobeB PCAP frame→ TCP |  |  |  |
164 | 13:43:43.961 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
165 | 13:43:43.963 |  | ←enobeB PCAP frame← TCP |  |  |
166 | 13:43:43.966 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
167 | 13:43:43.993 | →enobeB PCAP frame→ TCP |  |  |  |
168 | 13:43:44.081 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
169 | 13:43:44.082 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:642: Client connected to IdM port (id 18)
170 | 13:43:44.083 |  | ←enobeB PCAP frame← TCP |  |  |
171 | 13:43:44.085 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
172 | 13:43:44.113 | →enobeB PCAP frame→ TCP |  |  |  |
173 | 13:43:44.121 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
174 | 13:43:44.123 |  |  |  |  | →HTTP POST | IDMS-Endpoint
175 | 13:43:44.124 |  | ←enobeB PCAP frame← TCP |  |  |
176 | 13:43:44.168 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:521: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
177 | 13:43:44.169 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
178 | 13:43:44.172 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
179 | 13:43:44.233 | →enobeB PCAP frame→ TCP |  |  |  |
180 | 13:43:44.513 | →enobeB PCAP frame→ TCP |  |  |  |
181 | 13:43:44.516 |  | ←enobeB PCAP frame← TCP |  |  |
182 | 13:43:44.553 | →enobeB PCAP frame→ TCP |  |  |  |
183 | 13:43:44.561 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
184 | 13:43:44.563 |  | ←enobeB PCAP frame← TCP |  |  |
185 | 13:43:44.568 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
186 | 13:43:44.592 | →enobeB PCAP frame→ TCP |  |  |  |
187 | 13:43:44.601 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
188 | 13:43:44.603 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 19)
189 | 13:43:44.604 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
190 | 13:43:44.641 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
191 | 13:43:44.644 |  | ←enobeB PCAP frame← TCP |  |  |
192 | 13:43:44.644 |  |  |  |  | →HTTP POST | HTTP-Proxy
193 | 13:43:44.668 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:541: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
194 | 13:43:44.674 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
195 | 13:43:44.678 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
196 | 13:43:44.713 | →enobeB PCAP frame→ TCP |  |  |  |
197 | 13:43:44.753 | →enobeB PCAP frame→ TCP |  |  |  |
198 | 13:43:44.756 |  | ←enobeB PCAP frame← TCP |  |  |
199 | 13:43:44.793 | →enobeB PCAP frame→ TCP |  |  |  |
200 | 13:43:44.801 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
201 | 13:43:44.803 |  | ←enobeB PCAP frame← TCP |  |  |
202 | 13:43:44.806 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
203 | 13:43:44.833 | →enobeB PCAP frame→ TCP |  |  |  |
204 | 13:43:44.841 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
205 | 13:43:44.843 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 20)
206 | 13:43:44.844 |  | ←enobeB PCAP frame← TCP |  |  |
207 | 13:43:44.845 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
208 | 13:43:44.881 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
209 | 13:43:44.884 |  | ←enobeB PCAP frame← TCP |  |  |
210 | 13:43:44.884 |  |  |  |  | →HTTP POST | HTTP-Proxy
211 | 13:43:44.946 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
212 | 13:43:44.947 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:545: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
213 | 13:43:44.949 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
214 | 13:43:44.993 | →enobeB PCAP frame→ TCP |  |  |  |
215 | 13:43:45.041 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
216 | 13:43:45.045 |  |  |  |  | →SIP REGISTER | P-CSCF
217 | 13:43:45.068 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:814: IMS UDP_s port 192.168.2.3:5062 configured
218 | 13:43:45.094 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:765: IMS TCP_s port 192.168.2.3:5062 configured!
219 | 13:43:45.095 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:823: IMS UDP_c port 192.168.2.3:5061 configured
220 | 13:43:45.101 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
221 | 13:43:45.841 | →enobeB PCAP frame→ SIP over IPSEC: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
222 | 13:43:45.845 |  |  |  |  | →SIP REGISTER | P-CSCF
223 | 13:43:45.870 |  |  |  |  | ←SIP 200 OK | P-CSCF
224 | 13:43:45.874 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
225 | 13:43:46.201 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
226 | 13:43:46.202 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
227 | 13:43:46.203 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 SIP over IPSEC: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 |  |  |  |
228 | 13:43:46.216 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
229 | 13:43:46.257 |  |  |  |  | ←SIP 200 OK | P-CSCF
230 | 13:43:46.257 |  |  |  |  | MIKEY | Media-Server
231 | 13:43:46.259 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
232 | 13:43:46.473 |  |  |  |  | XML→ | Media-Server
233 | 13:43:46.474 |  |  |  |  | XML→ | Media-Server
234 | 13:43:46.477 |  |  |  |  | ←XML | Media-Server
235 | 13:43:46.481 |  |  |  |  | ←SIP NOTIFY | P-CSCF
236 | 13:43:46.483 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:38084;transp... |  |  |
237 | 13:43:46.521 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
238 | 13:43:46.522 |  |  |  |  | →SIP 200 OK | P-CSCF
239 | 13:43:46.952 | →enobeB PCAP frame→ TCP |  |  |  |
240 | 13:43:46.956 |  | ←enobeB PCAP frame← TCP |  |  |
241 | 13:43:46.993 | →enobeB PCAP frame→ TCP |  |  |  |
242 | 13:43:47.000 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
243 | 13:43:47.004 |  | ←enobeB PCAP frame← TCP |  |  |
244 | 13:43:47.007 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
245 | 13:43:47.033 | →enobeB PCAP frame→ TCP |  |  |  |
246 | 13:43:47.081 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
247 | 13:43:47.083 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
248 | 13:43:47.084 |  | ←enobeB PCAP frame← TCP |  |  |
249 | 13:43:47.085 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
250 | 13:43:47.112 | →enobeB PCAP frame→ TCP |  |  |  |
251 | 13:43:47.121 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-co... |  |  |  |
252 | 13:43:47.124 |  | ←enobeB PCAP frame← TCP |  |  |
253 | 13:43:47.124 |  |  |  |  | →HTTP GET | HTTP-Proxy
254 | 13:43:47.132 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:642: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcptt-ue-configuration.xml
255 | 13:43:47.141 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
256 | 13:43:47.143 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
257 | 13:43:47.193 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
258 | 13:43:47.194 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
259 | 13:43:47.196 |  | ←enobeB PCAP frame← TCP |  |  |
260 | 13:43:47.201 | →enobeB PCAP frame→ TCP |  |  |  |
261 | 13:43:47.203 |  | ←enobeB PCAP frame← TCP |  |  |
262 | 13:43:47.233 | →enobeB PCAP frame→ TCP |  |  |  |
263 | 13:43:47.353 | →enobeB PCAP frame→ TCP |  |  |  |
264 | 13:43:47.356 |  | ←enobeB PCAP frame← TCP |  |  |
265 | 13:43:47.393 | →enobeB PCAP frame→ TCP |  |  |  |
266 | 13:43:47.401 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
267 | 13:43:47.404 |  | ←enobeB PCAP frame← TCP |  |  |
268 | 13:43:47.408 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
269 | 13:43:47.433 | →enobeB PCAP frame→ TCP |  |  |  |
270 | 13:43:47.521 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
271 | 13:43:47.523 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
272 | 13:43:47.524 |  | ←enobeB PCAP frame← TCP |  |  |
273 | 13:43:47.525 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
274 | 13:43:47.553 | →enobeB PCAP frame→ TCP |  |  |  |
275 | 13:43:47.561 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-... |  |  |  |
276 | 13:43:47.563 |  |  |  |  | →HTTP GET | HTTP-Proxy
277 | 13:43:47.564 |  | ←enobeB PCAP frame← TCP |  |  |
278 | 13:43:47.575 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:647: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcptt-user-profile-49.xml
279 | 13:43:47.615 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
280 | 13:43:47.623 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
281 | 13:43:47.624 |  | ←enobeB PCAP frame← TCP |  |  |
282 | 13:43:47.625 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
283 | 13:43:47.673 | →enobeB PCAP frame→ TCP |  |  |  |
284 | 13:43:47.681 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
285 | 13:43:47.682 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
286 | 13:43:47.684 |  | ←enobeB PCAP frame← TCP |  |  |
287 | 13:43:47.685 |  | ←enobeB PCAP frame← TCP |  |  |
288 | 13:43:47.713 | →enobeB PCAP frame→ TCP |  |  |  |
289 | 13:43:48.281 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
290 | 13:43:48.282 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
291 | 13:43:48.295 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
292 | 13:43:48.353 |  |  |  |  | ←SIP 200 OK | P-CSCF
293 | 13:43:48.353 |  |  |  |  | MIKEY | Media-Server
294 | 13:43:48.356 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
295 | 13:43:48.393 | →enobeB PCAP frame→ TCP |  |  |  |
296 | 13:43:48.396 |  | ←enobeB PCAP frame← TCP |  |  |
297 | 13:43:48.433 | →enobeB PCAP frame→ TCP |  |  |  |
298 | 13:43:48.441 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
299 | 13:43:48.444 |  | ←enobeB PCAP frame← TCP |  |  |
300 | 13:43:48.445 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
301 | 13:43:48.473 | →enobeB PCAP frame→ TCP |  |  |  |
302 | 13:43:48.561 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
303 | 13:43:48.562 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
304 | 13:43:48.564 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
305 | 13:43:48.571 |  |  |  |  | XML→ | Media-Server
306 | 13:43:48.572 |  |  |  |  | XML→ | Media-Server
307 | 13:43:48.575 |  |  |  |  | ←XML | Media-Server
308 | 13:43:48.578 |  |  |  |  | ←SIP NOTIFY | P-CSCF
309 | 13:43:48.581 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:38084;transp... |  |  |
310 | 13:43:48.593 | →enobeB PCAP frame→ TCP |  |  |  |
311 | 13:43:48.601 | →enobeB PCAP frame→ HTTPS: GET /xcap.cms.mcstaasting.com/org.3gpp.mcptt.servi... |  |  |  |
312 | 13:43:48.602 |  |  |  |  | →HTTP GET | HTTP-Proxy
313 | 13:43:48.604 |  | ←enobeB PCAP frame← TCP |  |  |
314 | 13:43:48.604 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:652: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at /xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
315 | 13:43:48.610 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
316 | 13:43:48.613 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
317 | 13:43:48.613 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
318 | 13:43:48.625 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
319 | 13:43:48.627 |  |  |  |  | →SIP 200 OK | P-CSCF
320 | 13:43:48.673 | →enobeB PCAP frame→ TCP |  |  |  |
321 | 13:43:48.681 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
322 | 13:43:48.682 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
323 | 13:43:48.684 |  | ←enobeB PCAP frame← TCP |  |  |
324 | 13:43:48.713 | →enobeB PCAP frame→ TCP |  |  |  |
325 | 13:43:48.753 | →enobeB PCAP frame→ TCP |  |  |  |
326 | 13:43:48.756 |  | ←enobeB PCAP frame← TCP |  |  |
327 | 13:43:48.793 | →enobeB PCAP frame→ TCP |  |  |  |
328 | 13:43:48.801 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
329 | 13:43:48.804 |  | ←enobeB PCAP frame← TCP |  |  |
330 | 13:43:48.808 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
331 | 13:43:48.833 | →enobeB PCAP frame→ TCP |  |  |  |
332 | 13:43:48.961 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
333 | 13:43:48.963 |  | ←enobeB PCAP frame← TCP |  |  |
334 | 13:43:48.963 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:636: Client connected to Http Proxy port (id 25)
335 | 13:43:48.965 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
336 | 13:43:48.993 | →enobeB PCAP frame→ TCP |  |  |  |
337 | 13:43:49.001 | →enobeB PCAP frame→ HTTPS: GET /xcap.gms.mcstaasting.com/org.openmobileallian... |  |  |  |
338 | 13:43:49.003 |  |  |  |  | →HTTP GET | HTTP-Proxy
339 | 13:43:49.004 |  | ←enobeB PCAP frame← TCP |  |  |
340 | 13:43:49.014 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:657: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at /xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
341 | 13:43:49.037 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
342 | 13:43:49.043 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
343 | 13:43:49.044 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
344 | 13:43:49.073 | →enobeB PCAP frame→ TCP |  |  |  |
345 | 13:43:49.081 | →enobeB PCAP frame→ TCP |  |  |  |
346 | 13:43:49.089 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
347 | 13:43:49.090 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:672: Http Proxy port - Client closed the connection (id 25)
348 | 13:43:49.092 |  | ←enobeB PCAP frame← TCP |  |  |
349 | 13:43:49.096 | →enobeB PCAP frame→ TCP |  |  |  |
350 | 13:43:49.100 |  | ←enobeB PCAP frame← TCP |  |  |
351 | 13:43:49.113 | →enobeB PCAP frame→ TCP |  |  |  |
352 | 13:43:49.201 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
353 | 13:43:49.202 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
354 | 13:43:49.215 |  |  |  |  | →SIP PUBLISH | P-CSCF
355 | 13:43:49.263 |  |  |  |  | MIKEY | Media-Server
356 | 13:43:49.321 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
357 | 13:43:49.322 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
358 | 13:43:49.325 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
359 | 13:43:49.486 |  |  |  |  | XML→ | Media-Server
360 | 13:43:49.490 |  |  |  |  | ←SIP 200 OK | P-CSCF
361 | 13:43:49.493 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
362 | 13:43:49.493 |  |  |  |  | ←SIP 200 OK | P-CSCF
363 | 13:43:49.494 |  |  |  |  | MIKEY | Media-Server
364 | 13:43:49.496 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
365 | 13:43:49.699 |  |  |  |  | XML→ | Media-Server
366 | 13:43:49.700 |  |  |  |  | XML→ | Media-Server
367 | 13:43:49.734 |  |  |  |  | ←XML | Media-Server
368 | 13:43:49.739 |  |  |  |  | ←SIP NOTIFY | P-CSCF
369 | 13:43:49.743 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:38084;transp... |  |  |
370 | 13:43:49.801 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
371 | 13:43:49.802 |  |  |  |  | →SIP 200 OK | P-CSCF
372 | 13:43:49.807 |  |  |  |  | ←XML | Media-Server
373 | 13:43:49.823 |  |  |  |  | ←SIP MESSAGE | P-CSCF
374 | 13:43:49.828 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
375 | 13:43:50.641 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
376 | 13:43:50.643 |  |  |  |  | →SIP 200 OK | P-CSCF
377 | 13:43:50.650 |  |  |  |  | Info: MCX_IMS_CommonProcedures.ttcn:155: MESSAGE/200OK Table 5.3.2.3-2 Steps 7-8 Done
378 | 13:43:50.653 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
379 | 13:43:52.652 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
380 | 13:43:52.688 |  | ←RRC DCCH RRC Connection Release |  |  |
381 | 13:43:52.689 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
382 | 13:43:52.708 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
383 | 13:43:52.710 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
384 | 13:43:52.710 |  |  |  |  | MMICmd: Make the MCPTT User request the establishment of an MCPTT On-demand chat group call with implicit floor control
385 | 13:44:17.040 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
386 | 13:44:17.040 |  | →RRC CCCH RRC Connection Request |  |  |
387 | 13:44:17.040 |  | ←RRC CCCH RRC Connection Setup |  |  |
388 | 13:44:17.040 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
389 | 13:44:17.073 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
390 | 13:44:17.073 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
391 | 13:44:17.073 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
392 | 13:44:17.073 |  |  |  | →NAS EMM Service request |  |
393 | 13:44:17.073 |  |  |  | NAS K-enb 3c67ae8646bd1736dfb9702a64cfeace5... |  |
394 | 13:44:17.074 |  | ←RRC DCCH Security Mode Command |  |  |
395 | 13:44:17.074 |  |  | RRC K-enb 3c67ae8646bd1736dfb9702a64cfeace5... |  |  |
396 | 13:44:17.074 |  |  | RRC rrc-cip f819c8f917e2376db3a43f9faaf27bd... |  |  |
397 | 13:44:17.074 |  |  | RRC rrc-int 418bf587f5f35a3a87641236e3b016c... |  |  |
398 | 13:44:17.074 |  |  | RRC up-cip 1d21c8e297ea790b58f9104bae2a75d1... |  |  |
399 | 13:44:17.074 |  |  | RRC up-int dcd0c15c531f3427f03df225952846c6... |  |  |
400 | 13:44:17.075 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
401 | 13:44:17.113 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
402 | 13:44:17.113 |  | →RRC DCCH Security Mode Complete |  |  |
403 | 13:44:17.113 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
404 | 13:44:17.113 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
405 | 13:44:17.153 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
406 | 13:44:17.153 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
407 | 13:44:17.161 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
408 | 13:44:17.162 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
409 | 13:44:17.169 |  |  |  |  | →SIP INVITE | P-CSCF
410 | 13:44:17.204 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:735: SRTP config: Master Key: 995CD330163F3CA1AB6C41F5AB1B5F69, Master Salt: 7A2A7ECB31573733E51E4C44, MKI: 235B797D
411 | 13:44:17.204 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
412 | 13:44:17.214 |  |  |  |  | XML→ | Media-Server
413 | 13:44:17.216 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
414 | 13:44:17.219 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1205: INVITE Verdict: Pass
415 | 13:44:17.221 |  |  |  |  | ←SIP 100 Trying | P-CSCF
416 | 13:44:17.223 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
417 | 13:44:17.227 |  |  |  |  | ←SIP 200 OK | P-CSCF
418 | 13:44:17.230 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
419 | 13:44:17.839 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
420 | 13:44:17.840 |  | [EMBEDDED NAS IN NEXT RRC] TP Unknown message (type=0x2f) |  |  |
421 | 13:44:17.840 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
422 | 13:44:17.841 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
423 | 13:44:17.873 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
424 | 13:44:17.873 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
425 | 13:44:17.873 |  | →RRC DCCH UL Information Transfer |  |  |
426 | 13:44:17.873 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x4) |  |  |
427 | 13:44:17.873 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
428 | 13:44:17.970 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
429 | 13:44:18.321 | →enobeB PCAP frame→ SIP over IPSEC: ACK sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
430 | 13:44:18.323 |  |  |  |  | →SIP ACK | P-CSCF
431 | 13:44:18.330 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1208: ACK Verdict: Pass
432 | 13:44:18.333 |  |  |  |  | ←Floor Granted | Media-Server
433 | 13:44:18.912 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
434 | 13:44:18.952 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
435 | 13:44:18.961 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
436 | 13:44:18.969 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
437 | 13:44:18.992 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
438 | 13:44:19.081 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:571: Step 7 Verdict: Pass
439 | 13:44:19.183 |  |  |  |  | MMICmd: Release PTT token
440 | 13:44:21.001 | →enobeB PCAP frame→ |  |  |  |
441 | 13:44:21.002 |  |  |  |  | Floor Release→ | Media-Server
442 | 13:44:21.006 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
443 | 13:44:21.009 |  |  |  |  | ←XML | Media-Server
444 | 13:44:21.010 |  |  |  |  | ←Floor Idle | Media-Server
445 | 13:44:21.046 |  |  |  |  | ←SIP INVITE | P-CSCF
446 | 13:44:21.050 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
447 | 13:44:21.051 |  | ←enobeB PCAP frame← SIP over IPSEC: INVITE sip:PublicUserId-A@192.168.3.2:38084;transp... |  |  |
448 | 13:44:21.121 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 100 Trying |  |  |  |
449 | 13:44:21.123 |  |  |  |  | →SIP 100 Trying | P-CSCF
450 | 13:44:21.632 | →enobeB PCAP frame→ |  |  |  |
451 | 13:44:21.841 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
452 | 13:44:21.848 |  |  |  |  | →SIP 200 OK | P-CSCF
454 | 13:44:21.882 |  |  |  |  | XML→ | Media-Server
455 | 13:44:21.891 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:685: 200 OK Verdict: Pass
456 | 13:44:21.892 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:581: Step 8 Verdict: Pass
457 | 13:44:21.895 |  |  |  |  | ←SIP ACK | P-CSCF
458 | 13:44:21.896 |  |  |  |  | ←Floor Taken | Media-Server
459 | 13:44:21.898 |  | ←enobeB PCAP frame← SIP over IPSEC: ACK sip:PublicUserId-A@192.168.3.2:38084;transport... |  |  |
460 | 13:44:21.953 | →enobeB PCAP frame→ |  |  |  |
461 | 13:44:21.954 |  |  |  |  | Floor ACK→ | Media-Server
462 | 13:44:21.957 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Ack Verdict: Pass
463 | 13:44:21.958 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:587: Step 11 Verdict: Pass
464 | 13:44:21.960 |  |  |  |  | ←XML | Media-Server
465 | 13:44:21.961 |  |  |  |  | ←Floor Idle | Media-Server
466 | 13:44:22.001 |  |  |  |  | ←SIP INVITE | P-CSCF
467 | 13:44:22.006 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
468 | 13:44:22.007 |  | ←enobeB PCAP frame← SIP over IPSEC: INVITE sip:PublicUserId-A@192.168.3.2:38084;transp... |  |  |
469 | 13:44:22.041 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 100 Trying |  |  |  |
470 | 13:44:22.042 |  |  |  |  | →SIP 100 Trying | P-CSCF
471 | 13:44:22.081 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
472 | 13:44:22.087 |  |  |  |  | →SIP 200 OK | P-CSCF
473 | 13:44:22.119 |  |  |  |  | XML→ | Media-Server
474 | 13:44:22.126 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:685: 200 OK Verdict: Pass
475 | 13:44:22.127 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:594: Step 13 Verdict: Pass
476 | 13:44:22.130 |  |  |  |  | ←SIP ACK | P-CSCF
477 | 13:44:22.131 |  |  |  |  | ←Floor Taken | Media-Server
478 | 13:44:22.133 |  | ←enobeB PCAP frame← SIP over IPSEC: ACK sip:PublicUserId-A@192.168.3.2:38084;transport... |  |  |
479 | 13:44:22.193 | →enobeB PCAP frame→ |  |  |  |
480 | 13:44:22.194 |  |  |  |  | Floor ACK→ | Media-Server
481 | 13:44:22.198 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Ack Verdict: Pass
482 | 13:44:22.200 |  |  |  |  | ←XML | Media-Server
483 | 13:44:22.201 |  |  |  |  | ←Floor Idle | Media-Server
484 | 13:44:22.235 |  |  |  |  | ←SIP INVITE | P-CSCF
485 | 13:44:22.239 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
486 | 13:44:22.240 |  | ←enobeB PCAP frame← SIP over IPSEC: INVITE sip:PublicUserId-A@192.168.3.2:38084;transp... |  |  |
487 | 13:44:22.281 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 100 Trying |  |  |  |
488 | 13:44:22.283 |  |  |  |  | →SIP 100 Trying | P-CSCF
489 | 13:44:22.305 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
490 | 13:44:22.306 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
491 | 13:44:22.312 |  |  |  |  | →SIP 200 OK | P-CSCF
492 | 13:44:22.314 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
493 | 13:44:22.342 |  |  |  |  | XML→ | Media-Server
494 | 13:44:22.350 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:685: 200 OK Verdict: Pass
495 | 13:44:22.350 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:606: Step 18 Verdict: Pass
496 | 13:44:22.353 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
497 | 13:44:22.353 |  |  |  |  | ←SIP ACK | P-CSCF
498 | 13:44:22.354 |  |  |  |  | ←Floor Taken | Media-Server
499 | 13:44:22.356 |  | ←enobeB PCAP frame← SIP over IPSEC: ACK sip:PublicUserId-A@192.168.3.2:38084;transport... SRTP frame: |  |  |
500 | 13:44:22.361 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
501 | 13:44:22.402 |  |  |  |  | Floor ACK→ | Media-Server
502 | 13:44:22.405 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Ack Verdict: Pass
503 | 13:44:22.405 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:610: Step 21 Verdict: Pass
504 | 13:44:22.407 |  |  |  |  | ←XML | Media-Server
505 | 13:44:22.408 |  |  |  |  | ←Floor Idle | Media-Server
506 | 13:44:22.439 |  |  |  |  | ←SIP INVITE | P-CSCF
507 | 13:44:22.443 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
508 | 13:44:22.444 |  | ←enobeB PCAP frame← SIP over IPSEC: INVITE sip:PublicUserId-A@192.168.3.2:38084;transp... SRTP frame: |  |  |
509 | 13:44:22.481 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 100 Trying |  |  |  |
510 | 13:44:22.483 |  |  |  |  | →SIP 100 Trying | P-CSCF
511 | 13:44:22.505 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK SRTP frame: |  |  |  |
512 | 13:44:22.509 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
513 | 13:44:22.512 |  |  |  |  | →SIP 200 OK | P-CSCF
514 | 13:44:22.515 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
515 | 13:44:22.544 |  |  |  |  | XML→ | Media-Server
516 | 13:44:22.551 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:685: 200 OK Verdict: Pass
517 | 13:44:22.551 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:617: Step 23 Verdict: Pass
518 | 13:44:22.553 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
519 | 13:44:22.554 |  |  |  |  | ←SIP ACK | P-CSCF
520 | 13:44:22.555 |  |  |  |  | ←Floor Taken | Media-Server
521 | 13:44:22.557 |  | ←enobeB PCAP frame← SIP over IPSEC: ACK sip:PublicUserId-A@192.168.3.2:38084;transport... SRTP frame: |  |  |
522 | 13:44:22.602 |  |  |  |  | Floor ACK→ | Media-Server
523 | 13:44:22.605 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Ack Verdict: Pass
524 | 13:44:22.608 |  |  |  |  | ←Floor Idle | Media-Server
525 | 13:44:22.614 |  |  |  |  | ←SIP BYE | P-CSCF
526 | 13:44:22.617 |  | ←enobeB PCAP frame← SIP over IPSEC: BYE sip:PublicUserId-A@192.168.3.2:38084;transport... |  |  |
527 | 13:44:22.641 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK SRTP frame: |  |  |  |
528 | 13:44:22.643 |  |  |  |  | →SIP 200 OK | P-CSCF
529 | 13:44:22.644 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
530 | 13:44:22.645 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
531 | 13:44:22.673 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
532 | 13:44:22.676 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
533 | 13:44:23.073 | →enobeB PCAP frame→ |  |  |  |
534 | 13:44:24.652 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
535 | 13:44:24.672 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
536 | 13:44:24.672 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xb) |  |  |
537 | 13:44:24.672 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
538 | 13:44:24.673 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
539 | 13:44:24.713 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
540 | 13:44:24.713 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
541 | 13:44:24.713 |  | →RRC DCCH UL Information Transfer |  |  |
542 | 13:44:24.713 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x1) |  |  |
543 | 13:44:24.713 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
544 | 13:44:24.787 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
545 | 13:44:24.788 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
546 | 13:44:24.835 |  | ←RRC DCCH RRC Connection Release |  |  |
547 | 13:44:24.836 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
548 | 13:44:24.854 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
549 | 13:44:24.855 |  |  |  |  | Verdict PASS: MCPTT_OnDemandGroupCallCT_MCX_IMS.ttcn:629: Step 28 Verdict: Pass
550 | 13:44:24.857 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
551 | 13:44:24.859 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
552 | 13:44:25.607 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.