ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 13:05:03.974 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 13:05:03.977 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 13:05:03.977 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 13:05:03.979 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 13:05:03.980 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 13:05:03.980 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:824: IMS UDP port 192.168.2.3:5060 configured
7 | 13:05:03.982 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:774: IMS TCP port 192.168.2.3:5060 configured!
8 | 13:05:03.984 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:795: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 13:05:03.985 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:806: IdM port 192.168.2.3:8080 configured!
10 | 13:05:03.987 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 13:05:05.188 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 13:05:05.190 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 13:05:07.257 |  | ←RRC BCCH SIB1 |  |  |
14 | 13:05:07.332 |  | ←RRC BCCH SIB |  |  |
15 | 13:05:07.337 |  | ←RRC BCCH SIB1 |  |  |
16 | 13:05:07.352 |  | ←RRC BCCH SIB |  |  |
17 | 13:05:07.372 |  | ←RRC BCCH SIB |  |  |
18 | 13:06:25.571 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 13:06:25.571 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 13:06:25.571 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 13:06:25.571 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 13:06:25.632 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 13:06:25.632 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 13:06:25.632 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 13:06:25.632 |  |  |  | →NAS EMM Attach request |  |
26 | 13:06:25.632 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 13:06:25.632 |  |  |  | NAS K-asme b75458cbd457457289db0722e1aea1e8... |  |
28 | 13:06:25.632 |  |  |  | NAS ← EMM Authentication request |  |
29 | 13:06:25.633 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 13:06:25.633 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 13:06:25.634 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 13:06:25.704 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 13:06:25.704 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 13:06:25.704 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 13:06:25.704 |  |  |  | →NAS EMM Authentication response |  |
36 | 13:06:25.704 |  |  |  | NAS UE auth OK |  |
37 | 13:06:25.704 |  |  |  | NAS K-nas-cip 4e36cc8b0f683b356e1c43c35a650... |  |
38 | 13:06:25.704 |  |  |  | NAS K-nas-int 258c31ea9c261241388cd2f078859... |  |
39 | 13:06:25.704 |  |  |  | NAS ← EMM Security mode command |  |
40 | 13:06:25.705 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 13:06:25.705 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 13:06:25.706 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 13:06:25.744 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
44 | 13:06:25.744 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 13:06:25.744 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xa) |  |  |
46 | 13:06:25.744 |  |  |  | →NAS EMM Security mode complete |  |
47 | 13:06:25.744 |  |  |  | NAS ← ESM ESM information request |  |
48 | 13:06:25.745 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xd) |  |  |
49 | 13:06:25.745 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 13:06:25.746 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
51 | 13:06:25.792 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
52 | 13:06:25.792 |  | →RRC DCCH UL Information Transfer |  |  |
53 | 13:06:25.792 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x9) |  |  |
54 | 13:06:25.792 |  |  |  | →NAS ESM ESM information response |  |
55 | 13:06:25.792 |  |  |  | NAS ← EMM Attach accept |  |
56 | 13:06:25.792 |  |  |  | NAS K-enb b6fb91addf4eb53a5dfae85650163528a... |  |
57 | 13:06:25.793 |  | ←RRC DCCH Security Mode Command |  |  |
58 | 13:06:25.793 |  |  | RRC K-enb b6fb91addf4eb53a5dfae85650163528a... |  |  |
59 | 13:06:25.793 |  |  | RRC rrc-cip bd72a5983e2a283e9577b904d5d6294... |  |  |
60 | 13:06:25.793 |  |  | RRC rrc-int 8852513b45cd2221393c82c37ac51ee... |  |  |
61 | 13:06:25.793 |  |  | RRC up-cip 271a0ceeced317753078fb0951e3077a... |  |  |
62 | 13:06:25.793 |  |  | RRC up-int d267a40fd6c5442f51d6fd80b618f50e... |  |  |
63 | 13:06:25.794 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
64 | 13:06:25.824 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
65 | 13:06:25.824 |  | →RRC DCCH Security Mode Complete |  |  |
66 | 13:06:25.824 |  | ←RRC DCCH UE Capability Enquiry |  |  |
67 | 13:06:25.824 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
68 | 13:06:25.874 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
69 | 13:06:25.874 |  | →RRC DCCH UE Capability Information |  |  |
70 | 13:06:25.874 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x9) |  |  |
71 | 13:06:25.874 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
72 | 13:06:25.874 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
73 | 13:06:25.904 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
74 | 13:06:25.904 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
75 | 13:06:25.944 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
76 | 13:06:25.944 |  | →RRC DCCH UL Information Transfer |  |  |
77 | 13:06:25.944 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xc) |  |  |
78 | 13:06:25.944 |  |  |  | →NAS EMM Attach complete |  |
79 | 13:06:25.944 |  |  |  | NAS ← EMM EMM information |  |
80 | 13:06:25.945 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x6) |  |  |
81 | 13:06:25.945 |  | ←RRC DCCH DL Information Transfer |  |  |
82 | 13:06:25.946 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
83 | 13:06:32.528 |  | ←RRC DCCH RRC Connection Release |  |  |
84 | 13:06:32.529 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
85 | 13:06:34.621 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
86 | 13:06:34.621 |  | →RRC CCCH RRC Connection Request |  |  |
87 | 13:06:34.621 |  | ←RRC CCCH RRC Connection Setup |  |  |
88 | 13:06:34.621 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
89 | 13:06:34.664 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
90 | 13:06:34.664 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
91 | 13:06:34.664 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
92 | 13:06:34.664 |  |  |  | →NAS EMM Service request |  |
93 | 13:06:34.664 |  |  |  | NAS K-enb 90b22e0e793449cf63f9890a596319589... |  |
94 | 13:06:34.665 |  | ←RRC DCCH Security Mode Command |  |  |
95 | 13:06:34.665 |  |  | RRC K-enb 90b22e0e793449cf63f9890a596319589... |  |  |
96 | 13:06:34.665 |  |  | RRC rrc-cip c905dce9a7d71f7ed7dc03f0abe318c... |  |  |
97 | 13:06:34.665 |  |  | RRC rrc-int 276fb9f4fe4b223495b0de8d8dd7695... |  |  |
98 | 13:06:34.665 |  |  | RRC up-cip 09afd1cfd5b458984b67172dbf26ed52... |  |  |
99 | 13:06:34.665 |  |  | RRC up-int fc452cb7c43a9320266cc690f5e307fc... |  |  |
100 | 13:06:34.666 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
101 | 13:06:34.704 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
102 | 13:06:34.704 |  | →RRC DCCH Security Mode Complete |  |  |
103 | 13:06:34.704 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
104 | 13:06:34.704 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
105 | 13:06:34.744 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
106 | 13:06:34.744 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
107 | 13:06:56.904 | →enobeB PCAP frame→ TCP |  |  |  |
108 | 13:06:56.907 |  | ←enobeB PCAP frame← TCP |  |  |
109 | 13:06:56.944 | →enobeB PCAP frame→ TCP |  |  |  |
110 | 13:06:56.992 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
111 | 13:06:56.995 |  | ←enobeB PCAP frame← TCP |  |  |
112 | 13:06:57.000 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
113 | 13:06:57.024 | →enobeB PCAP frame→ TCP |  |  |  |
114 | 13:06:57.150 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 16)
115 | 13:06:57.152 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
116 | 13:06:57.157 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
117 | 13:06:57.184 | →enobeB PCAP frame→ TCP |  |  |  |
118 | 13:06:57.229 |  |  |  |  | →HTTP GET | HTTP-Proxy
119 | 13:06:57.232 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
120 | 13:06:57.232 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:301: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
121 | 13:06:57.236 |  | ←enobeB PCAP frame← TCP |  |  |
122 | 13:06:57.239 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
123 | 13:06:57.247 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
124 | 13:06:57.264 | →enobeB PCAP frame→ TCP |  |  |  |
125 | 13:06:59.224 | →enobeB PCAP frame→ TCP |  |  |  |
126 | 13:06:59.229 |  | ←enobeB PCAP frame← TCP |  |  |
127 | 13:06:59.264 | →enobeB PCAP frame→ TCP |  |  |  |
128 | 13:06:59.272 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
129 | 13:06:59.275 |  | ←enobeB PCAP frame← TCP |  |  |
130 | 13:06:59.280 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
131 | 13:06:59.304 | →enobeB PCAP frame→ TCP |  |  |  |
132 | 13:06:59.757 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
133 | 13:06:59.760 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
134 | 13:06:59.763 |  | ←enobeB PCAP frame← TCP |  |  |
135 | 13:06:59.764 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
136 | 13:06:59.784 | →enobeB PCAP frame→ TCP |  |  |  |
137 | 13:06:59.791 |  |  |  |  | →HTTP GET | IDMS-Endpoint
138 | 13:06:59.792 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
139 | 13:06:59.795 |  | ←enobeB PCAP frame← TCP |  |  |
140 | 13:06:59.828 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
141 | 13:06:59.832 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:524: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
142 | 13:06:59.832 |  |  |  |  | MMICmd: Please provide user credentials: username and password
143 | 13:06:59.836 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
144 | 13:06:59.904 | →enobeB PCAP frame→ TCP |  |  |  |
145 | 13:07:04.391 |  |  |  |  | →HTTP POST | IDMS-Endpoint
146 | 13:07:04.392 | →enobeB PCAP frame→ HTTPS: POST /idms/userauth HTTP/1.1 |  |  |  |
147 | 13:07:04.395 |  | ←enobeB PCAP frame← TCP |  |  |
148 | 13:07:04.406 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
149 | 13:07:04.409 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:529: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
150 | 13:07:04.414 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
151 | 13:07:04.464 | →enobeB PCAP frame→ TCP |  |  |  |
152 | 13:07:04.468 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:693: IdM port - Client closed the connection (id 18)
153 | 13:07:04.472 | →enobeB PCAP frame→ TCP |  |  |  |
154 | 13:07:04.475 |  | ←enobeB PCAP frame← TCP |  |  |
155 | 13:07:04.504 | →enobeB PCAP frame→ TCP |  |  |  |
156 | 13:07:04.904 | →enobeB PCAP frame→ TCP |  |  |  |
157 | 13:07:04.907 |  | ←enobeB PCAP frame← TCP |  |  |
158 | 13:07:04.944 | →enobeB PCAP frame→ TCP |  |  |  |
159 | 13:07:04.963 |  | ←enobeB PCAP frame← TCP |  |  |
160 | 13:07:04.966 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
161 | 13:07:05.028 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
162 | 13:07:05.035 |  | ←enobeB PCAP frame← TCP |  |  |
163 | 13:07:05.036 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
164 | 13:07:05.068 |  |  |  |  | →HTTP POST | IDMS-Endpoint
165 | 13:07:05.072 | →enobeB PCAP frame→ TCP |  |  |  |
166 | 13:07:05.075 |  | ←enobeB PCAP frame← TCP |  |  |
167 | 13:07:05.078 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
168 | 13:07:05.082 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:534: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
169 | 13:07:05.099 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
170 | 13:07:05.184 | →enobeB PCAP frame→ TCP |  |  |  |
171 | 13:07:05.424 | →enobeB PCAP frame→ TCP |  |  |  |
172 | 13:07:05.427 |  | ←enobeB PCAP frame← TCP |  |  |
173 | 13:07:05.464 | →enobeB PCAP frame→ TCP |  |  |  |
174 | 13:07:05.472 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
175 | 13:07:05.477 |  | ←enobeB PCAP frame← TCP |  |  |
176 | 13:07:05.480 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
177 | 13:07:05.504 | →enobeB PCAP frame→ TCP |  |  |  |
178 | 13:07:05.549 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 19)
179 | 13:07:05.552 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
180 | 13:07:05.555 |  | ←enobeB PCAP frame← TCP |  |  |
181 | 13:07:05.559 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
182 | 13:07:05.591 |  |  |  |  | →HTTP POST | HTTP-Proxy
183 | 13:07:05.592 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
184 | 13:07:05.595 |  | ←enobeB PCAP frame← TCP |  |  |
185 | 13:07:05.616 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:554: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
186 | 13:07:05.623 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
187 | 13:07:05.631 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
188 | 13:07:05.664 | →enobeB PCAP frame→ TCP |  |  |  |
189 | 13:07:05.704 | →enobeB PCAP frame→ TCP |  |  |  |
190 | 13:07:05.710 |  | ←enobeB PCAP frame← TCP |  |  |
191 | 13:07:05.744 | →enobeB PCAP frame→ TCP |  |  |  |
192 | 13:07:05.752 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
193 | 13:07:05.755 |  | ←enobeB PCAP frame← TCP |  |  |
194 | 13:07:05.758 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
195 | 13:07:05.784 | →enobeB PCAP frame→ TCP |  |  |  |
196 | 13:07:05.789 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 20)
197 | 13:07:05.792 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
198 | 13:07:05.795 |  | ←enobeB PCAP frame← TCP |  |  |
199 | 13:07:05.796 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
200 | 13:07:05.830 |  |  |  |  | →HTTP POST | HTTP-Proxy
201 | 13:07:05.832 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
202 | 13:07:05.835 |  | ←enobeB PCAP frame← TCP |  |  |
203 | 13:07:05.898 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
204 | 13:07:05.898 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:558: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
205 | 13:07:05.906 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
206 | 13:07:05.944 | →enobeB PCAP frame→ TCP |  |  |  |
207 | 13:07:05.991 |  |  |  |  | →SIP REGISTER | P-CSCF
208 | 13:07:05.992 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
209 | 13:07:06.014 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:833: IMS UDP_s port 192.168.2.3:5062 configured
210 | 13:07:06.019 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:784: IMS TCP_s port 192.168.2.3:5062 configured!
211 | 13:07:06.022 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:842: IMS UDP_c port 192.168.2.3:5061 configured
212 | 13:07:06.033 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
213 | 13:07:06.720 |  |  |  |  | →SIP REGISTER | P-CSCF
214 | 13:07:06.745 |  |  |  |  | ←SIP 200 OK | P-CSCF
215 | 13:07:06.752 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
216 | 13:07:07.072 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
217 | 13:07:07.073 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
218 | 13:07:07.086 |  |  |  |  | ←SIP 200 OK | P-CSCF
219 | 13:07:07.086 |  |  |  |  | MIKEY | Media-Server
220 | 13:07:07.093 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
221 | 13:07:07.280 |  |  |  |  | XML→ | Media-Server
222 | 13:07:07.282 |  |  |  |  | XML→ | Media-Server
223 | 13:07:07.285 |  |  |  |  | ←XML | Media-Server
224 | 13:07:07.288 |  |  |  |  | ←SIP NOTIFY | P-CSCF
225 | 13:07:07.296 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
226 | 13:07:07.297 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:38570;transp... |  |  |
227 | 13:07:07.350 |  |  |  |  | →SIP 200 OK | P-CSCF
228 | 13:07:07.352 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
229 | 13:07:07.544 | →enobeB PCAP frame→ TCP |  |  |  |
230 | 13:07:07.547 |  | ←enobeB PCAP frame← TCP |  |  |
231 | 13:07:07.584 | →enobeB PCAP frame→ TCP |  |  |  |
232 | 13:07:07.592 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
233 | 13:07:07.598 |  | ←enobeB PCAP frame← TCP |  |  |
234 | 13:07:07.599 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
235 | 13:07:07.664 | →enobeB PCAP frame→ TCP |  |  |  |
236 | 13:07:07.709 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
237 | 13:07:07.712 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
238 | 13:07:07.715 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
239 | 13:07:07.744 | →enobeB PCAP frame→ TCP |  |  |  |
240 | 13:07:07.748 |  |  |  |  | →HTTP GET | HTTP-Proxy
241 | 13:07:07.751 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:655: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcptt-ue-configuration.xml
242 | 13:07:07.752 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
243 | 13:07:07.753 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
244 | 13:07:07.755 |  | ←enobeB PCAP frame← TCP |  |  |
245 | 13:07:07.760 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
246 | 13:07:07.821 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
247 | 13:07:07.824 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
248 | 13:07:07.827 |  | ←enobeB PCAP frame← TCP |  |  |
249 | 13:07:07.832 | →enobeB PCAP frame→ TCP |  |  |  |
250 | 13:07:07.835 |  | ←enobeB PCAP frame← TCP |  |  |
251 | 13:07:07.864 | →enobeB PCAP frame→ TCP |  |  |  |
252 | 13:07:07.904 | →enobeB PCAP frame→ TCP |  |  |  |
253 | 13:07:07.910 |  | ←enobeB PCAP frame← TCP |  |  |
254 | 13:07:07.944 | →enobeB PCAP frame→ TCP |  |  |  |
255 | 13:07:07.952 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
256 | 13:07:07.955 |  | ←enobeB PCAP frame← TCP |  |  |
257 | 13:07:07.959 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
258 | 13:07:07.984 | →enobeB PCAP frame→ TCP |  |  |  |
259 | 13:07:08.029 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
260 | 13:07:08.032 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
261 | 13:07:08.035 |  | ←enobeB PCAP frame← TCP |  |  |
262 | 13:07:08.036 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
263 | 13:07:08.069 |  |  |  |  | →HTTP GET | HTTP-Proxy
264 | 13:07:08.072 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
265 | 13:07:08.075 |  | ←enobeB PCAP frame← TCP |  |  |
266 | 13:07:08.082 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:660: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcptt-user-profile-49.xml
267 | 13:07:08.124 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
268 | 13:07:08.138 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
269 | 13:07:08.139 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
270 | 13:07:08.184 | →enobeB PCAP frame→ TCP |  |  |  |
271 | 13:07:08.189 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
272 | 13:07:08.192 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
273 | 13:07:08.195 |  | ←enobeB PCAP frame← TCP |  |  |
274 | 13:07:08.196 |  | ←enobeB PCAP frame← TCP |  |  |
275 | 13:07:08.224 | →enobeB PCAP frame→ TCP |  |  |  |
276 | 13:07:08.752 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
277 | 13:07:08.753 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
278 | 13:07:08.757 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
279 | 13:07:08.770 |  |  |  |  | ←SIP 200 OK | P-CSCF
280 | 13:07:08.770 |  |  |  |  | MIKEY | Media-Server
281 | 13:07:08.778 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
282 | 13:07:08.904 | →enobeB PCAP frame→ TCP |  |  |  |
283 | 13:07:08.907 |  | ←enobeB PCAP frame← TCP |  |  |
284 | 13:07:08.944 | →enobeB PCAP frame→ TCP |  |  |  |
285 | 13:07:08.952 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
286 | 13:07:08.955 |  | ←enobeB PCAP frame← TCP |  |  |
287 | 13:07:08.956 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
288 | 13:07:08.964 |  |  |  |  | XML→ | Media-Server
289 | 13:07:08.966 |  |  |  |  | XML→ | Media-Server
290 | 13:07:08.969 |  |  |  |  | ←XML | Media-Server
291 | 13:07:08.984 | →enobeB PCAP frame→ TCP |  |  |  |
292 | 13:07:09.028 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
293 | 13:07:09.029 |  |  |  |  | ←SIP NOTIFY | P-CSCF
294 | 13:07:09.032 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
295 | 13:07:09.035 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
296 | 13:07:09.036 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:38570;transp... |  |  |
297 | 13:07:09.064 | →enobeB PCAP frame→ TCP |  |  |  |
298 | 13:07:09.068 |  |  |  |  | →SIP 200 OK | P-CSCF
299 | 13:07:09.069 |  |  |  |  | →HTTP GET | HTTP-Proxy
300 | 13:07:09.071 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:665: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
301 | 13:07:09.072 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
302 | 13:07:09.075 |  | ←enobeB PCAP frame← TCP |  |  |
303 | 13:07:09.077 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
304 | 13:07:09.086 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
305 | 13:07:09.104 | →enobeB PCAP frame→ TCP |  |  |  |
306 | 13:07:09.141 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
307 | 13:07:09.144 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
308 | 13:07:09.148 |  | ←enobeB PCAP frame← TCP |  |  |
309 | 13:07:09.152 | →enobeB PCAP frame→ TCP |  |  |  |
310 | 13:07:09.155 |  | ←enobeB PCAP frame← TCP |  |  |
311 | 13:07:09.184 | →enobeB PCAP frame→ TCP |  |  |  |
312 | 13:07:09.264 | →enobeB PCAP frame→ TCP |  |  |  |
313 | 13:07:09.267 |  | ←enobeB PCAP frame← TCP |  |  |
314 | 13:07:09.304 | →enobeB PCAP frame→ TCP |  |  |  |
315 | 13:07:09.312 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
316 | 13:07:09.315 |  | ←enobeB PCAP frame← TCP |  |  |
317 | 13:07:09.319 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
318 | 13:07:09.344 | →enobeB PCAP frame→ TCP |  |  |  |
319 | 13:07:09.389 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
320 | 13:07:09.392 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
321 | 13:07:09.395 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
322 | 13:07:09.424 | →enobeB PCAP frame→ TCP |  |  |  |
323 | 13:07:09.437 |  |  |  |  | →HTTP GET | HTTP-Proxy
324 | 13:07:09.443 |  | ←enobeB PCAP frame← TCP |  |  |
325 | 13:07:09.449 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:670: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at http://xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
326 | 13:07:09.475 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
327 | 13:07:09.486 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
328 | 13:07:09.549 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
329 | 13:07:09.556 |  | ←enobeB PCAP frame← TCP |  |  |
330 | 13:07:09.584 | →enobeB PCAP frame→ TCP |  |  |  |
331 | 13:07:09.792 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
332 | 13:07:09.793 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
333 | 13:07:09.796 |  |  |  |  | →SIP PUBLISH | P-CSCF
334 | 13:07:09.806 |  |  |  |  | MIKEY | Media-Server
335 | 13:07:09.872 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
336 | 13:07:09.872 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
337 | 13:07:09.873 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
338 | 13:07:10.006 |  |  |  |  | XML→ | Media-Server
339 | 13:07:10.009 |  |  |  |  | ←SIP 200 OK | P-CSCF
340 | 13:07:10.012 |  |  |  |  | ←SIP 200 OK | P-CSCF
341 | 13:07:10.012 |  |  |  |  | MIKEY | Media-Server
342 | 13:07:10.016 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
343 | 13:07:10.020 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
344 | 13:07:10.207 |  |  |  |  | XML→ | Media-Server
345 | 13:07:10.209 |  |  |  |  | XML→ | Media-Server
346 | 13:07:10.245 |  |  |  |  | MIKEY | Media-Server
347 | 13:07:10.246 |  |  |  |  | ←XML | Media-Server
348 | 13:07:10.251 |  |  |  |  | ←SIP NOTIFY | P-CSCF
349 | 13:07:10.258 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:38570;transp... |  |  |
350 | 13:07:10.308 |  |  |  |  | →SIP 200 OK | P-CSCF
351 | 13:07:10.312 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
352 | 13:07:10.312 |  |  |  |  | ←XML | Media-Server
353 | 13:07:10.325 |  |  |  |  | ←SIP MESSAGE | P-CSCF
354 | 13:07:10.333 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
355 | 13:07:11.150 |  |  |  |  | →SIP 200 OK | P-CSCF
356 | 13:07:11.152 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
357 | 13:07:11.157 |  |  |  |  | Info: MCX_IMS_CommonProcedures.ttcn:228: MESSAGE/200OK Table 5.3.2.3-2 Steps 7-8 Done
358 | 13:07:13.159 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
359 | 13:07:13.209 |  | ←RRC DCCH RRC Connection Release |  |  |
360 | 13:07:13.210 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
361 | 13:07:13.224 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
362 | 13:07:13.227 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
363 | 13:07:13.227 |  |  |  |  | MMICmd: Make the MCPTT User request the establishment of an MCPTT private call, on-demand Automatic Commencement Mode, no Force of automatic commencement, applying End-to-end communication security with Floor Control
364 | 13:07:18.021 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
365 | 13:07:18.021 |  | →RRC CCCH RRC Connection Request |  |  |
366 | 13:07:18.021 |  | ←RRC CCCH RRC Connection Setup |  |  |
367 | 13:07:18.021 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
368 | 13:07:18.064 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
369 | 13:07:18.064 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
370 | 13:07:18.064 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
371 | 13:07:18.064 |  |  |  | →NAS EMM Service request |  |
372 | 13:07:18.064 |  |  |  | NAS K-enb c13c15c2048b9e39529d0c2225ff082c1... |  |
373 | 13:07:18.065 |  | ←RRC DCCH Security Mode Command |  |  |
374 | 13:07:18.065 |  |  | RRC K-enb c13c15c2048b9e39529d0c2225ff082c1... |  |  |
375 | 13:07:18.065 |  |  | RRC rrc-cip cfd703895095636daea4252b2a78666... |  |  |
376 | 13:07:18.065 |  |  | RRC rrc-int 5fe77d70f2a1df7d30e493403756f20... |  |  |
377 | 13:07:18.065 |  |  | RRC up-cip 39331acb6f9193eaa99b568ad5142e23... |  |  |
378 | 13:07:18.065 |  |  | RRC up-int e1597c1c15270955e171a872f2da1b6f... |  |  |
379 | 13:07:18.066 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
380 | 13:07:18.104 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
381 | 13:07:18.104 |  | →RRC DCCH Security Mode Complete |  |  |
382 | 13:07:18.104 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
383 | 13:07:18.104 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
384 | 13:07:18.144 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
385 | 13:07:18.144 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
386 | 13:07:18.152 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
387 | 13:07:18.153 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |  |
388 | 13:07:18.157 |  |  |  |  | →SIP INVITE | P-CSCF
389 | 13:07:18.169 |  |  |  |  | MIKEY | Media-Server
390 | 13:07:18.377 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:754: SRTP config: Master Key: 628F29DA9BB55EFF426AD18B9A045E2D, Master Salt: BCF80D2AAC9E6E09A56B7AB5, MKI: 23D874D9
391 | 13:07:18.377 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
392 | 13:07:18.380 |  |  |  |  | XML→ | Media-Server
393 | 13:07:18.381 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
394 | 13:07:18.381 |  |  |  |  | XML→ | Media-Server
395 | 13:07:18.384 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1233: INVITE Verdict: Pass
396 | 13:07:18.384 |  |  |  |  | ←SIP 100 Trying | P-CSCF
397 | 13:07:18.386 |  |  |  |  | ←SIP 200 OK | P-CSCF
398 | 13:07:18.392 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
399 | 13:07:18.394 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
400 | 13:07:19.011 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
401 | 13:07:19.011 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xc) |  |  |
402 | 13:07:19.011 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
403 | 13:07:19.012 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
404 | 13:07:19.064 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
405 | 13:07:19.064 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
406 | 13:07:19.064 |  | →RRC DCCH UL Information Transfer |  |  |
407 | 13:07:19.064 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x1) |  |  |
408 | 13:07:19.064 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
409 | 13:07:19.136 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
410 | 13:07:19.430 |  |  |  |  | →SIP ACK | P-CSCF
411 | 13:07:19.432 | →enobeB PCAP frame→ SIP over IPSEC: ACK sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
412 | 13:07:19.439 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1236: ACK Verdict: Pass
413 | 13:07:19.440 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:77: Step 2 Verdict: Pass
414 | 13:07:19.443 |  |  |  |  | ←Floor Granted | Media-Server
415 | 13:07:19.944 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
416 | 13:07:19.952 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
417 | 13:07:19.984 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
418 | 13:07:19.992 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
419 | 13:07:20.000 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
420 | 13:07:20.191 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:82: Step 5A Verdict: Pass
421 | 13:07:20.293 |  |  |  |  | MMICmd: Release PTT token
422 | 13:07:21.837 |  |  |  |  | Floor Release→ | Media-Server
423 | 13:07:21.840 | →enobeB PCAP frame→ |  |  |  |
424 | 13:07:21.840 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
425 | 13:07:21.841 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:89: Step 7 Verdict: Pass
426 | 13:07:21.844 |  |  |  |  | ←Floor Taken | Media-Server
427 | 13:07:21.848 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
428 | 13:07:21.851 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
429 | 13:07:21.942 |  |  |  |  | MMICmd: Request PTT token
430 | 13:07:23.381 |  |  |  |  | Floor Request→ | Media-Server
431 | 13:07:23.384 | →enobeB PCAP frame→ |  |  |  |
432 | 13:07:23.384 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Request Verdict: Pass
433 | 13:07:23.384 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:98: Step 11 Verdict: Pass
434 | 13:07:23.387 |  |  |  |  | ←Floor Deny | Media-Server
435 | 13:07:23.389 |  |  |  |  | ←Floor Idle | Media-Server
436 | 13:07:23.486 |  |  |  |  | MMICmd: Release PTT token
437 | 13:07:23.587 |  |  |  |  | MMICmd: Request PTT token
438 | 13:07:24.821 |  |  |  |  | Floor Request→ | Media-Server
439 | 13:07:24.824 | →enobeB PCAP frame→ |  |  |  |
440 | 13:07:24.824 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Request Verdict: Pass
441 | 13:07:24.827 |  |  |  |  | ←Floor Granted | Media-Server
442 | 13:07:24.860 |  |  |  |  | Floor ACK→ | Media-Server
443 | 13:07:24.864 | →enobeB PCAP frame→ |  |  |  |
444 | 13:07:24.864 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Ack Verdict: Pass
445 | 13:07:24.864 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:113: Step 16 Verdict: Pass
446 | 13:07:24.904 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
447 | 13:07:24.907 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
448 | 13:07:24.912 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
449 | 13:07:24.916 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
450 | 13:07:24.944 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
451 | 13:07:24.966 |  |  |  |  | MMICmd: Release PTT token
452 | 13:07:26.349 |  |  |  |  | Floor Release→ | Media-Server
453 | 13:07:26.353 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
454 | 13:07:26.353 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:122: Step 18A Verdict: Pass
455 | 13:07:26.354 |  |  |  |  | MMICmd: Make the UE (MCPTT User) request upgrade of the ongoing private call to MCPTT emergency private call
456 | 13:07:26.356 |  |  |  |  | ←Floor Idle | Media-Server
457 | 13:07:30.540 |  |  |  |  | →SIP INVITE | P-CSCF
458 | 13:07:30.566 |  |  |  |  | Info: IMS_SDP_Messages.ttcn:130: SDP media [0] match FAIL
459 | 13:07:30.568 |  |  |  |  | MIKEY | Media-Server
460 | 13:07:30.766 |  |  |  |  | XML→ | Media-Server
461 | 13:07:30.767 |  |  |  |  | XML→ | Media-Server
462 | 13:07:30.769 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1294: re-INVITE Verdict: Pass
463 | 13:07:30.771 |  |  |  |  | ←SIP 100 Trying | P-CSCF
464 | 13:07:30.772 |  |  |  |  | ←SIP 200 OK | P-CSCF
465 | 13:07:30.778 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
466 | 13:07:30.780 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
467 | 13:07:30.784 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
468 | 13:07:30.787 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
469 | 13:07:30.824 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
470 | 13:07:30.827 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
471 | 13:07:30.832 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
472 | 13:07:31.030 |  |  |  |  | →SIP ACK | P-CSCF
473 | 13:07:31.039 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1299: ACK Verdict: Pass
474 | 13:07:31.043 |  |  |  |  | ←Floor Granted | Media-Server
475 | 13:07:31.068 |  |  |  |  | Floor ACK→ | Media-Server
476 | 13:07:31.071 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Ack Verdict: Pass
477 | 13:07:31.072 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
478 | 13:07:31.072 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:129: Step 20 Verdict: Pass
479 | 13:07:31.075 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
480 | 13:07:31.104 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
481 | 13:07:31.107 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
482 | 13:07:31.112 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
483 | 13:07:31.115 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
484 | 13:07:31.173 |  |  |  |  | MMICmd: Release PTT token
485 | 13:07:32.708 |  |  |  |  | Floor Release→ | Media-Server
486 | 13:07:32.711 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
487 | 13:07:32.712 | →enobeB PCAP frame→ |  |  |  |
488 | 13:07:32.712 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:145: Step 24 Verdict: Pass
489 | 13:07:32.716 |  |  |  |  | ←Floor Taken | Media-Server
490 | 13:07:32.814 |  |  |  |  | MMICmd: Request PTT token
491 | 13:07:33.900 |  |  |  |  | Floor Request→ | Media-Server
492 | 13:07:33.904 | →enobeB PCAP frame→ |  |  |  |
493 | 13:07:33.904 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Request Verdict: Pass
494 | 13:07:33.907 |  |  |  |  | ←Floor Granted | Media-Server
495 | 13:07:33.940 |  |  |  |  | Floor ACK→ | Media-Server
496 | 13:07:33.944 | →enobeB PCAP frame→ |  |  |  |
497 | 13:07:33.944 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Ack Verdict: Pass
498 | 13:07:33.944 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:154: Step 28 Verdict: Pass
499 | 13:07:34.024 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
500 | 13:07:34.027 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
501 | 13:07:34.046 |  |  |  |  | MMICmd: Release PTT token
502 | 13:07:34.064 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
503 | 13:07:34.068 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
504 | 13:07:34.072 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
505 | 13:07:35.309 |  |  |  |  | Floor Release→ | Media-Server
506 | 13:07:35.312 | →enobeB PCAP frame→ |  |  |  |
507 | 13:07:35.312 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
508 | 13:07:35.312 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:163: Step 31 Verdict: Pass
509 | 13:07:35.313 |  |  |  |  | MMICmd: Make the UE (MCPTT User) request cancelling of MCPTT emergency private call
510 | 13:07:35.315 |  |  |  |  | ←Floor Idle | Media-Server
511 | 13:07:39.481 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
512 | 13:07:39.482 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
513 | 13:07:39.485 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
514 | 13:07:39.498 |  |  |  |  | →SIP INVITE | P-CSCF
515 | 13:07:39.504 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
516 | 13:07:39.507 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
517 | 13:07:39.553 |  |  |  |  | Info: IMS_SDP_Messages.ttcn:130: SDP media [0] match FAIL
518 | 13:07:39.562 |  |  |  |  | MIKEY | Media-Server
519 | 13:07:39.770 |  |  |  |  | XML→ | Media-Server
520 | 13:07:39.772 |  |  |  |  | XML→ | Media-Server
521 | 13:07:39.774 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1294: re-INVITE Verdict: Pass
522 | 13:07:39.775 |  |  |  |  | ←SIP 100 Trying | P-CSCF
523 | 13:07:39.777 |  |  |  |  | ←SIP 200 OK | P-CSCF
524 | 13:07:39.782 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
525 | 13:07:39.784 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
526 | 13:07:39.784 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
527 | 13:07:39.787 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
528 | 13:07:39.824 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
529 | 13:07:39.827 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
530 | 13:07:39.832 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
531 | 13:07:39.835 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
532 | 13:07:40.038 |  |  |  |  | →SIP ACK | P-CSCF
533 | 13:07:40.047 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1299: ACK Verdict: Pass
534 | 13:07:40.048 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:172: Step 34 Verdict: Pass
535 | 13:07:40.150 |  |  |  |  | MMICmd: Request PTT token
536 | 13:07:41.580 |  |  |  |  | Floor Request→ | Media-Server
537 | 13:07:41.583 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Request Verdict: Pass
538 | 13:07:41.584 | →enobeB PCAP frame→ |  |  |  |
539 | 13:07:41.587 |  |  |  |  | ←Floor Granted | Media-Server
540 | 13:07:41.620 |  |  |  |  | Floor ACK→ | Media-Server
541 | 13:07:41.622 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Ack Verdict: Pass
542 | 13:07:41.622 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:181: Step 36B Verdict: Pass
543 | 13:07:41.624 | →enobeB PCAP frame→ |  |  |  |
544 | 13:07:41.664 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
545 | 13:07:41.667 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
546 | 13:07:41.672 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
547 | 13:07:41.676 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
548 | 13:07:41.704 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
549 | 13:07:41.723 |  |  |  |  | MMICmd: Release PTT token
550 | 13:07:42.908 |  |  |  |  | Floor Release→ | Media-Server
551 | 13:07:42.911 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
552 | 13:07:42.912 | →enobeB PCAP frame→ |  |  |  |
553 | 13:07:42.912 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:188: Step 38 Verdict: Pass
554 | 13:07:42.915 |  |  |  |  | ←Floor Idle | Media-Server
555 | 13:07:43.017 |  |  |  |  | MMICmd: Release call (hang up the call)
556 | 13:07:44.591 |  |  |  |  | →SIP BYE | P-CSCF
557 | 13:07:44.606 |  |  |  |  | ←SIP 200 OK | P-CSCF
558 | 13:07:44.614 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
559 | 13:07:44.944 | →enobeB PCAP frame→ |  |  |  |
560 | 13:07:46.607 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
561 | 13:07:46.622 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
562 | 13:07:46.623 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xd) |  |  |
563 | 13:07:46.623 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
564 | 13:07:46.624 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
565 | 13:07:46.664 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
566 | 13:07:46.664 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
567 | 13:07:46.664 |  | →RRC DCCH UL Information Transfer |  |  |
568 | 13:07:46.664 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xc) |  |  |
569 | 13:07:46.664 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
570 | 13:07:46.734 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
571 | 13:07:46.735 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
572 | 13:07:46.775 |  | ←RRC DCCH RRC Connection Release |  |  |
573 | 13:07:46.776 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
574 | 13:07:46.790 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
575 | 13:07:46.791 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:194: Step 41 Verdict: Pass
576 | 13:07:46.792 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
577 | 13:07:46.795 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
578 | 13:07:47.542 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.