MSG #71 2021-09-28 15:28:43.478
RRC

     DCCH: RRC Connection Reconfiguration
    {
      message c1: rrcConnectionReconfiguration: {
        rrc-TransactionIdentifier 0,
        criticalExtensions c1: rrcConnectionReconfiguration-r8: {
          dedicatedInfoNASList {
            '275971705B02FB50CC4D9BA478E2B9F13AEEAD5F5FC1D1AFC6B6A813BA23571C8DF0597AB2015A8E94354E0CD2000CAE70E5C3126BBF432F4B09F0E0AB9044C2F624F6A33637A135BDB43359796EF9A5097BFAB69E953E13D20012A312C6DB79493CFAD3117B7095F03EBB44F0F6A80335414C1DD48ACA980811696391EFD8F161D704A5ED5A1989'H
          },
          radioResourceConfigDedicated {
            srb-ToAddModList {
              {
                srb-Identity 2,
                rlc-Config explicitValue: am: {
                  ul-AM-RLC {
                    t-PollRetransmit ms60,
                    pollPDU pInfinity,
                    pollByte kBinfinity,
                    maxRetxThreshold t32
                  },
                  dl-AM-RLC {
                    t-Reordering ms45,
                    t-StatusProhibit ms0
                  }
                },
                logicalChannelConfig defaultValue: NULL
              }
            },
            drb-ToAddModList {
              {
                eps-BearerIdentity 5,
                drb-Identity 1,
                pdcp-Config {
                  discardTimer infinity,
                  rlc-AM {
                    statusReportRequired TRUE
                  },
                  headerCompression notUsed: NULL
                },
                rlc-Config am: {
                  ul-AM-RLC {
                    t-PollRetransmit ms80,
                    pollPDU p128,
                    pollByte kB125,
                    maxRetxThreshold t4
                  },
                  dl-AM-RLC {
                    t-Reordering ms80,
                    t-StatusProhibit ms60
                  }
                },
                logicalChannelIdentity 3,
                logicalChannelConfig {
                  ul-SpecificParameters {
                    priority 4,
                    prioritisedBitRate kBps8,
                    bucketSizeDuration ms100,
                    logicalChannelGroup 1
                  }
                }
              }
            },
            physicalConfigDedicated {
              cqi-ReportConfig {
                nomPDSCH-RS-EPRE-Offset 0,
                cqi-ReportPeriodic setup: {
                  cqi-PUCCH-ResourceIndex 0,
                  cqi-pmi-ConfigIndex 38,
                  cqi-FormatIndicatorPeriodic widebandCQI: NULL,
                  simultaneousAckNackAndCQI TRUE
                }
              }
            }
          }
        }
      }
    }