ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 15:27:30.677 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 15:27:30.681 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 15:27:30.681 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 15:27:30.683 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 15:27:30.684 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 15:27:30.684 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:824: IMS UDP port 192.168.2.3:5060 configured
7 | 15:27:30.687 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:774: IMS TCP port 192.168.2.3:5060 configured!
8 | 15:27:30.689 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:795: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 15:27:30.690 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:806: IdM port 192.168.2.3:8080 configured!
10 | 15:27:30.693 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 15:27:31.894 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 15:27:31.896 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 15:27:36.941 |  | ←RRC BCCH SIB1 |  |  |
14 | 15:27:37.021 |  | ←RRC BCCH SIB1 |  |  |
15 | 15:27:37.096 |  | ←RRC BCCH SIB |  |  |
16 | 15:27:37.101 |  | ←RRC BCCH SIB1 |  |  |
17 | 15:27:37.116 |  | ←RRC BCCH SIB |  |  |
18 | 15:28:43.175 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 15:28:43.175 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 15:28:43.175 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 15:28:43.175 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 15:28:43.236 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 15:28:43.236 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 15:28:43.236 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 15:28:43.236 |  |  |  | →NAS EMM Attach request |  |
26 | 15:28:43.236 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 15:28:43.236 |  |  |  | NAS K-asme 2b2fa6609d01af71d6d42b1593dda4de... |  |
28 | 15:28:43.236 |  |  |  | NAS ← EMM Authentication request |  |
29 | 15:28:43.237 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 15:28:43.237 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 15:28:43.238 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 15:28:43.308 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 15:28:43.308 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 15:28:43.308 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 15:28:43.308 |  |  |  | →NAS EMM Authentication response |  |
36 | 15:28:43.308 |  |  |  | NAS UE auth OK |  |
37 | 15:28:43.308 |  |  |  | NAS K-nas-cip b3b15618f7ebd1c696a217c59ccf2... |  |
38 | 15:28:43.308 |  |  |  | NAS K-nas-int 79a2cba66c97028fdccbe8f0fd2f7... |  |
39 | 15:28:43.308 |  |  |  | NAS ← EMM Security mode command |  |
40 | 15:28:43.309 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 15:28:43.309 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 15:28:43.310 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 15:28:43.348 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
44 | 15:28:43.348 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 15:28:43.348 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x1) |  |  |
46 | 15:28:43.348 |  |  |  | →NAS EMM Security mode complete |  |
47 | 15:28:43.348 |  |  |  | NAS ← ESM ESM information request |  |
48 | 15:28:43.349 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x0) |  |  |
49 | 15:28:43.349 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 15:28:43.350 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
51 | 15:28:43.396 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
52 | 15:28:43.396 |  | →RRC DCCH UL Information Transfer |  |  |
53 | 15:28:43.396 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x8) |  |  |
54 | 15:28:43.396 |  |  |  | →NAS ESM ESM information response |  |
55 | 15:28:43.396 |  |  |  | NAS ← EMM Attach accept |  |
56 | 15:28:43.396 |  |  |  | NAS K-enb 1701ca59d0ee476f87eb09210c29c3c8d... |  |
57 | 15:28:43.397 |  | ←RRC DCCH Security Mode Command |  |  |
58 | 15:28:43.397 |  |  | RRC K-enb 1701ca59d0ee476f87eb09210c29c3c8d... |  |  |
59 | 15:28:43.397 |  |  | RRC rrc-cip 02de3a74cc3690d934e10420d556376... |  |  |
60 | 15:28:43.397 |  |  | RRC rrc-int ba52ec6c6779e9de1d87aff52aba0e2... |  |  |
61 | 15:28:43.397 |  |  | RRC up-cip a5c7dc4f41aa798a5c76d0b55e9ca613... |  |  |
62 | 15:28:43.397 |  |  | RRC up-int 72a0b3169cef8d35369a66f225dee043... |  |  |
63 | 15:28:43.398 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
64 | 15:28:43.428 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
65 | 15:28:43.428 |  | →RRC DCCH Security Mode Complete |  |  |
66 | 15:28:43.428 |  | ←RRC DCCH UE Capability Enquiry |  |  |
67 | 15:28:43.428 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
68 | 15:28:43.478 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
69 | 15:28:43.478 |  | →RRC DCCH UE Capability Information |  |  |
70 | 15:28:43.478 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xb) |  |  |
71 | 15:28:43.478 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
72 | 15:28:43.478 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
73 | 15:28:43.508 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
74 | 15:28:43.508 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
75 | 15:28:43.548 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
76 | 15:28:43.548 |  | →RRC DCCH UL Information Transfer |  |  |
77 | 15:28:43.548 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x0) |  |  |
78 | 15:28:43.548 |  |  |  | →NAS EMM Attach complete |  |
79 | 15:28:43.548 |  |  |  | NAS ← EMM EMM information |  |
80 | 15:28:43.549 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xc) |  |  |
81 | 15:28:43.549 |  | ←RRC DCCH DL Information Transfer |  |  |
82 | 15:28:43.550 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
83 | 15:28:49.066 |  | ←RRC DCCH RRC Connection Release |  |  |
84 | 15:28:49.067 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
85 | 15:28:49.195 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
86 | 15:28:49.195 |  | →RRC CCCH RRC Connection Request |  |  |
87 | 15:28:49.195 |  | ←RRC CCCH RRC Connection Setup |  |  |
88 | 15:28:49.195 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
89 | 15:28:49.228 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
90 | 15:28:49.228 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
91 | 15:28:49.228 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
92 | 15:28:49.228 |  |  |  | →NAS EMM Service request |  |
93 | 15:28:49.228 |  |  |  | NAS K-enb d5dae5a3cb42c4cd41ac99c9c46ab5049... |  |
94 | 15:28:49.229 |  | ←RRC DCCH Security Mode Command |  |  |
95 | 15:28:49.229 |  |  | RRC K-enb d5dae5a3cb42c4cd41ac99c9c46ab5049... |  |  |
96 | 15:28:49.229 |  |  | RRC rrc-cip 87afeabe272adeb231930138bcf0e0b... |  |  |
97 | 15:28:49.229 |  |  | RRC rrc-int f37aa4c229b26fa1235a70f2fd86166... |  |  |
98 | 15:28:49.229 |  |  | RRC up-cip 6ae3fefe32e732f156672e66428beaf4... |  |  |
99 | 15:28:49.229 |  |  | RRC up-int 30a5cb670f7c3d670a63fdcd9254f682... |  |  |
100 | 15:28:49.230 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
101 | 15:28:49.268 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
102 | 15:28:49.268 |  | →RRC DCCH Security Mode Complete |  |  |
103 | 15:28:49.268 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
104 | 15:28:49.268 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
105 | 15:28:49.308 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
106 | 15:28:49.308 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
107 | 15:29:24.508 | →enobeB PCAP frame→ TCP |  |  |  |
108 | 15:29:24.511 |  | ←enobeB PCAP frame← TCP |  |  |
109 | 15:29:24.548 | →enobeB PCAP frame→ TCP |  |  |  |
110 | 15:29:24.596 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
111 | 15:29:24.599 |  | ←enobeB PCAP frame← TCP |  |  |
112 | 15:29:24.604 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
113 | 15:29:24.628 | →enobeB PCAP frame→ TCP |  |  |  |
114 | 15:29:24.756 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
115 | 15:29:24.758 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 16)
116 | 15:29:24.759 |  | ←enobeB PCAP frame← TCP |  |  |
117 | 15:29:24.760 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
118 | 15:29:24.788 | →enobeB PCAP frame→ TCP |  |  |  |
119 | 15:29:24.836 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
120 | 15:29:24.838 |  |  |  |  | →HTTP GET | HTTP-Proxy
121 | 15:29:24.839 |  | ←enobeB PCAP frame← TCP |  |  |
122 | 15:29:24.846 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:301: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
123 | 15:29:24.866 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
124 | 15:29:24.870 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
125 | 15:29:24.908 | →enobeB PCAP frame→ TCP |  |  |  |
126 | 15:29:26.588 | →enobeB PCAP frame→ TCP |  |  |  |
127 | 15:29:26.591 |  | ←enobeB PCAP frame← TCP |  |  |
128 | 15:29:26.628 | →enobeB PCAP frame→ TCP |  |  |  |
129 | 15:29:26.636 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
130 | 15:29:26.639 |  | ←enobeB PCAP frame← TCP |  |  |
131 | 15:29:26.642 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
132 | 15:29:26.668 | →enobeB PCAP frame→ TCP |  |  |  |
133 | 15:29:27.076 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
134 | 15:29:27.190 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
135 | 15:29:27.192 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
136 | 15:29:27.228 | →enobeB PCAP frame→ TCP |  |  |  |
137 | 15:29:27.334 |  | ←enobeB PCAP frame← TCP |  |  |
138 | 15:29:27.334 |  |  |  |  | →HTTP GET | IDMS-Endpoint
139 | 15:29:27.374 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
140 | 15:29:27.378 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:524: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
141 | 15:29:27.378 |  |  |  |  | MMICmd: Please provide user credentials: username and password
142 | 15:29:27.478 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
143 | 15:29:32.927 |  | ←enobeB PCAP frame← TCP |  |  |
144 | 15:29:32.928 |  |  |  |  | →HTTP POST | IDMS-Endpoint
145 | 15:29:32.942 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
146 | 15:29:32.945 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
147 | 15:29:32.945 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:529: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
148 | 15:29:32.989 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:693: IdM port - Client closed the connection (id 18)
149 | 15:29:32.991 |  | ←enobeB PCAP frame← TCP |  |  |
150 | 15:29:33.508 | →enobeB PCAP frame→ TCP |  |  |  |
151 | 15:29:33.511 |  | ←enobeB PCAP frame← TCP |  |  |
152 | 15:29:33.548 | →enobeB PCAP frame→ TCP |  |  |  |
153 | 15:29:33.556 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
154 | 15:29:33.559 |  | ←enobeB PCAP frame← TCP |  |  |
155 | 15:29:33.562 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
156 | 15:29:33.588 | →enobeB PCAP frame→ TCP |  |  |  |
157 | 15:29:33.676 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
158 | 15:29:33.677 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
159 | 15:29:33.679 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
160 | 15:29:33.708 | →enobeB PCAP frame→ TCP |  |  |  |
161 | 15:29:33.716 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
162 | 15:29:33.718 |  |  |  |  | →HTTP POST | IDMS-Endpoint
163 | 15:29:33.719 |  | ←enobeB PCAP frame← TCP |  |  |
164 | 15:29:33.751 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
165 | 15:29:33.752 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:534: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
166 | 15:29:33.754 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
167 | 15:29:33.828 | →enobeB PCAP frame→ TCP |  |  |  |
168 | 15:29:34.228 | →enobeB PCAP frame→ TCP |  |  |  |
169 | 15:29:34.231 |  | ←enobeB PCAP frame← TCP |  |  |
170 | 15:29:34.268 | →enobeB PCAP frame→ TCP |  |  |  |
171 | 15:29:34.287 |  | ←enobeB PCAP frame← TCP |  |  |
172 | 15:29:34.290 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
173 | 15:29:34.358 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 19)
174 | 15:29:34.359 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
175 | 15:29:34.396 | →enobeB PCAP frame→ TCP |  |  |  |
176 | 15:29:34.398 |  |  |  |  | →HTTP POST | HTTP-Proxy
177 | 15:29:34.399 |  | ←enobeB PCAP frame← TCP |  |  |
178 | 15:29:34.404 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
179 | 15:29:34.407 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
180 | 15:29:34.407 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:554: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
181 | 15:29:34.428 | →enobeB PCAP frame→ TCP |  |  |  |
182 | 15:29:34.508 | →enobeB PCAP frame→ TCP |  |  |  |
183 | 15:29:34.511 |  | ←enobeB PCAP frame← TCP |  |  |
184 | 15:29:34.548 | →enobeB PCAP frame→ TCP |  |  |  |
185 | 15:29:34.556 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
186 | 15:29:34.559 |  | ←enobeB PCAP frame← TCP |  |  |
187 | 15:29:34.562 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
188 | 15:29:34.588 | →enobeB PCAP frame→ TCP |  |  |  |
189 | 15:29:34.596 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
190 | 15:29:34.598 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 20)
191 | 15:29:34.599 |  | ←enobeB PCAP frame← TCP |  |  |
192 | 15:29:34.600 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
193 | 15:29:34.636 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
194 | 15:29:34.639 |  | ←enobeB PCAP frame← TCP |  |  |
195 | 15:29:34.639 |  |  |  |  | →HTTP POST | HTTP-Proxy
196 | 15:29:34.700 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
197 | 15:29:34.700 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:558: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
198 | 15:29:34.703 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
199 | 15:29:34.748 | →enobeB PCAP frame→ TCP |  |  |  |
200 | 15:29:34.836 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
201 | 15:29:34.839 |  |  |  |  | →SIP REGISTER | P-CSCF
202 | 15:29:34.861 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:833: IMS UDP_s port 192.168.2.3:5062 configured
203 | 15:29:34.867 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:784: IMS TCP_s port 192.168.2.3:5062 configured!
204 | 15:29:34.869 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:842: IMS UDP_c port 192.168.2.3:5061 configured
205 | 15:29:34.880 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
206 | 15:29:35.676 | →enobeB PCAP frame→ SIP over IPSEC: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
207 | 15:29:35.747 |  |  |  |  | →SIP REGISTER | P-CSCF
208 | 15:29:35.758 |  |  |  |  | ←SIP 200 OK | P-CSCF
209 | 15:29:35.761 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
210 | 15:29:36.116 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
211 | 15:29:36.117 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 SIP over IPSEC: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 |  |  |  |
212 | 15:29:36.130 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
213 | 15:29:36.171 |  |  |  |  | ←SIP 200 OK | P-CSCF
214 | 15:29:36.171 |  |  |  |  | MIKEY | Media-Server
215 | 15:29:36.173 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
216 | 15:29:36.367 |  |  |  |  | XML→ | Media-Server
217 | 15:29:36.369 |  |  |  |  | XML→ | Media-Server
218 | 15:29:36.372 |  |  |  |  | ←XML | Media-Server
219 | 15:29:36.375 |  |  |  |  | ←SIP NOTIFY | P-CSCF
220 | 15:29:36.378 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:45784;transp... |  |  |
221 | 15:29:36.436 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
222 | 15:29:36.439 |  |  |  |  | →SIP 200 OK | P-CSCF
223 | 15:29:36.708 | →enobeB PCAP frame→ TCP |  |  |  |
224 | 15:29:36.711 |  | ←enobeB PCAP frame← TCP |  |  |
225 | 15:29:36.748 | →enobeB PCAP frame→ TCP |  |  |  |
226 | 15:29:36.756 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
227 | 15:29:36.760 |  | ←enobeB PCAP frame← TCP |  |  |
228 | 15:29:36.763 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
229 | 15:29:36.788 | →enobeB PCAP frame→ TCP |  |  |  |
230 | 15:29:36.836 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
231 | 15:29:36.838 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
232 | 15:29:36.839 |  | ←enobeB PCAP frame← TCP |  |  |
233 | 15:29:36.840 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
234 | 15:29:36.868 | →enobeB PCAP frame→ TCP |  |  |  |
235 | 15:29:36.876 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
236 | 15:29:36.879 |  | ←enobeB PCAP frame← TCP |  |  |
237 | 15:29:36.879 |  |  |  |  | →HTTP GET | HTTP-Proxy
238 | 15:29:36.889 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:655: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcptt-ue-configuration.xml
239 | 15:29:36.896 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
240 | 15:29:36.900 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
241 | 15:29:36.948 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
242 | 15:29:36.950 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
243 | 15:29:36.951 |  | ←enobeB PCAP frame← TCP |  |  |
244 | 15:29:36.988 | →enobeB PCAP frame→ TCP |  |  |  |
245 | 15:29:37.108 | →enobeB PCAP frame→ TCP |  |  |  |
246 | 15:29:37.111 |  | ←enobeB PCAP frame← TCP |  |  |
247 | 15:29:37.148 | →enobeB PCAP frame→ TCP |  |  |  |
248 | 15:29:37.156 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
249 | 15:29:37.159 |  | ←enobeB PCAP frame← TCP |  |  |
250 | 15:29:37.163 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
251 | 15:29:37.188 | →enobeB PCAP frame→ TCP |  |  |  |
252 | 15:29:37.236 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
253 | 15:29:37.239 |  | ←enobeB PCAP frame← TCP |  |  |
254 | 15:29:37.239 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
255 | 15:29:37.240 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
256 | 15:29:37.268 | →enobeB PCAP frame→ TCP |  |  |  |
257 | 15:29:37.276 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
258 | 15:29:37.279 |  | ←enobeB PCAP frame← TCP |  |  |
259 | 15:29:37.279 |  |  |  |  | →HTTP GET | HTTP-Proxy
260 | 15:29:37.293 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:660: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcptt-user-profile-49.xml
261 | 15:29:37.337 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
262 | 15:29:37.344 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
263 | 15:29:37.345 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
264 | 15:29:37.388 | →enobeB PCAP frame→ TCP |  |  |  |
265 | 15:29:37.396 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
266 | 15:29:37.398 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
267 | 15:29:37.399 |  | ←enobeB PCAP frame← TCP |  |  |
268 | 15:29:37.400 |  | ←enobeB PCAP frame← TCP |  |  |
269 | 15:29:37.428 | →enobeB PCAP frame→ TCP |  |  |  |
270 | 15:29:38.036 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
271 | 15:29:38.037 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
272 | 15:29:38.045 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
273 | 15:29:38.058 |  |  |  |  | ←SIP 200 OK | P-CSCF
274 | 15:29:38.058 |  |  |  |  | MIKEY | Media-Server
275 | 15:29:38.060 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
276 | 15:29:38.108 | →enobeB PCAP frame→ TCP |  |  |  |
277 | 15:29:38.111 |  | ←enobeB PCAP frame← TCP |  |  |
278 | 15:29:38.148 | →enobeB PCAP frame→ TCP |  |  |  |
279 | 15:29:38.156 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
280 | 15:29:38.159 |  | ←enobeB PCAP frame← TCP |  |  |
281 | 15:29:38.160 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
282 | 15:29:38.188 | →enobeB PCAP frame→ TCP |  |  |  |
283 | 15:29:38.236 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
284 | 15:29:38.238 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
285 | 15:29:38.240 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
286 | 15:29:38.256 |  |  |  |  | XML→ | Media-Server
287 | 15:29:38.257 |  |  |  |  | XML→ | Media-Server
288 | 15:29:38.260 |  |  |  |  | ←XML | Media-Server
289 | 15:29:38.264 |  |  |  |  | ←SIP NOTIFY | P-CSCF
290 | 15:29:38.267 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:45784;transp... |  |  |
291 | 15:29:38.268 | →enobeB PCAP frame→ TCP |  |  |  |
292 | 15:29:38.276 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
293 | 15:29:38.278 |  |  |  |  | →HTTP GET | HTTP-Proxy
294 | 15:29:38.279 |  | ←enobeB PCAP frame← TCP |  |  |
295 | 15:29:38.288 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:665: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
296 | 15:29:38.305 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
297 | 15:29:38.308 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
298 | 15:29:38.309 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
299 | 15:29:38.316 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
300 | 15:29:38.318 |  |  |  |  | →SIP 200 OK | P-CSCF
301 | 15:29:38.348 | →enobeB PCAP frame→ TCP |  |  |  |
302 | 15:29:38.388 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
303 | 15:29:38.390 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
304 | 15:29:38.391 |  | ←enobeB PCAP frame← TCP |  |  |
305 | 15:29:38.396 | →enobeB PCAP frame→ TCP |  |  |  |
306 | 15:29:38.399 |  | ←enobeB PCAP frame← TCP |  |  |
307 | 15:29:38.428 | →enobeB PCAP frame→ TCP |  |  |  |
308 | 15:29:38.508 | →enobeB PCAP frame→ TCP |  |  |  |
309 | 15:29:38.511 |  | ←enobeB PCAP frame← TCP |  |  |
310 | 15:29:38.548 | →enobeB PCAP frame→ TCP |  |  |  |
311 | 15:29:38.556 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
312 | 15:29:38.559 |  | ←enobeB PCAP frame← TCP |  |  |
313 | 15:29:38.562 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
314 | 15:29:38.588 | →enobeB PCAP frame→ TCP |  |  |  |
315 | 15:29:38.676 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
316 | 15:29:38.678 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
317 | 15:29:38.679 |  | ←enobeB PCAP frame← TCP |  |  |
318 | 15:29:38.680 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
319 | 15:29:38.708 | →enobeB PCAP frame→ TCP |  |  |  |
320 | 15:29:38.716 | →enobeB PCAP frame→ HTTPS: GET http://xcap.gms.mcstaasting.com/org.openmobile... |  |  |  |
321 | 15:29:38.718 |  |  |  |  | →HTTP GET | HTTP-Proxy
322 | 15:29:38.719 |  | ←enobeB PCAP frame← TCP |  |  |
323 | 15:29:38.730 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:670: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at http://xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
324 | 15:29:38.756 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
325 | 15:29:38.762 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
326 | 15:29:38.788 | →enobeB PCAP frame→ TCP |  |  |  |
327 | 15:29:38.828 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
328 | 15:29:38.830 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
329 | 15:29:38.831 |  | ←enobeB PCAP frame← TCP |  |  |
330 | 15:29:38.836 | →enobeB PCAP frame→ TCP |  |  |  |
331 | 15:29:38.839 |  | ←enobeB PCAP frame← TCP |  |  |
332 | 15:29:38.868 | →enobeB PCAP frame→ TCP |  |  |  |
333 | 15:29:39.036 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
334 | 15:29:39.037 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
335 | 15:29:39.047 |  |  |  |  | →SIP PUBLISH | P-CSCF
336 | 15:29:39.066 |  |  |  |  | MIKEY | Media-Server
337 | 15:29:39.116 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
338 | 15:29:39.117 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
339 | 15:29:39.121 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
340 | 15:29:39.271 |  |  |  |  | XML→ | Media-Server
341 | 15:29:39.274 |  |  |  |  | ←SIP 200 OK | P-CSCF
342 | 15:29:39.277 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
343 | 15:29:39.278 |  |  |  |  | ←SIP 200 OK | P-CSCF
344 | 15:29:39.279 |  |  |  |  | MIKEY | Media-Server
345 | 15:29:39.281 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
346 | 15:29:39.484 |  |  |  |  | XML→ | Media-Server
347 | 15:29:39.485 |  |  |  |  | XML→ | Media-Server
348 | 15:29:39.525 |  |  |  |  | MIKEY | Media-Server
349 | 15:29:39.526 |  |  |  |  | ←XML | Media-Server
350 | 15:29:39.531 |  |  |  |  | ←SIP NOTIFY | P-CSCF
351 | 15:29:39.534 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:45784;transp... |  |  |
352 | 15:29:39.606 |  |  |  |  | →SIP 200 OK | P-CSCF
353 | 15:29:39.611 |  |  |  |  | ←XML | Media-Server
354 | 15:29:39.621 |  |  |  |  | ←SIP MESSAGE | P-CSCF
355 | 15:29:39.624 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
356 | 15:29:40.478 |  |  |  |  | →SIP 200 OK | P-CSCF
357 | 15:29:40.486 |  |  |  |  | Info: MCX_IMS_CommonProcedures.ttcn:228: MESSAGE/200OK Table 5.3.2.3-2 Steps 7-8 Done
358 | 15:29:42.487 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
359 | 15:29:42.522 |  | ←RRC DCCH RRC Connection Release |  |  |
360 | 15:29:42.523 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
361 | 15:29:42.542 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
362 | 15:29:42.612 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:754: SRTP config: Master Key: A356A755C1EE5C81C836F3D97D12356F, Master Salt: 1BB6B430368D88FF9D91E03F, MKI: 270B0273
363 | 15:29:42.612 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
364 | 15:29:42.613 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
365 | 15:29:42.615 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
366 | 15:29:42.619 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
367 | 15:29:42.619 |  |  |  |  | ←XML | Media-Server
368 | 15:29:42.628 |  |  |  |  | ←SIP INVITE | P-CSCF
369 | 15:29:43.075 |  | ←enobeB PCAP frame← LTE RRC PCCH Paging (1 PagingRecord) |  |  |
370 | 15:29:43.075 |  | ←RRC PCCH Paging |  |  |
371 | 15:29:43.115 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
372 | 15:29:43.115 |  | →RRC CCCH RRC Connection Request |  |  |
373 | 15:29:43.115 |  | ←RRC CCCH RRC Connection Setup |  |  |
374 | 15:29:43.115 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
375 | 15:29:43.148 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
376 | 15:29:43.148 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
377 | 15:29:43.148 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
378 | 15:29:43.148 |  |  |  | →NAS EMM Service request |  |
379 | 15:29:43.148 |  |  |  | NAS K-enb d8e5c619ef428b2b2039757ac046c2729... |  |
380 | 15:29:43.149 |  | ←RRC DCCH Security Mode Command |  |  |
381 | 15:29:43.149 |  |  | RRC K-enb d8e5c619ef428b2b2039757ac046c2729... |  |  |
382 | 15:29:43.149 |  |  | RRC rrc-cip eaa3d12849a0cd3cba567766970aa4f... |  |  |
383 | 15:29:43.149 |  |  | RRC rrc-int 645bbfc1f30035728f82f376ca9e821... |  |  |
384 | 15:29:43.149 |  |  | RRC up-cip e49920ff181d6a68ffae12f00dc7d6f2... |  |  |
385 | 15:29:43.149 |  |  | RRC up-int 152782cda28835df53ef8e1afb35f686... |  |  |
386 | 15:29:43.150 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
387 | 15:29:43.188 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
388 | 15:29:43.188 |  | →RRC DCCH Security Mode Complete |  |  |
389 | 15:29:43.188 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
390 | 15:29:43.188 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
391 | 15:29:43.228 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
392 | 15:29:43.228 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
393 | 15:29:43.230 |  | ←enobeB PCAP frame← SIP over IPSEC: INVITE sip:PublicUserId-A@192.168.3.2:45784;transp... |  |  |
394 | 15:29:43.276 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 100 Trying |  |  |  |
395 | 15:29:43.277 |  |  |  |  | →SIP 100 Trying | P-CSCF
396 | 15:29:43.556 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
397 | 15:29:43.578 |  |  |  |  | →SIP 200 OK | P-CSCF
398 | 15:29:43.594 |  |  |  |  | XML→ | Media-Server
399 | 15:29:43.599 |  |  |  |  | ←SIP ACK | P-CSCF
400 | 15:29:43.599 |  |  |  |  | ←Floor Taken | Media-Server
401 | 15:29:43.602 |  | ←enobeB PCAP frame← SIP over IPSEC: ACK sip:PublicUserId-A@192.168.3.2:45784;transport... |  |  |
402 | 15:29:43.660 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
403 | 15:29:43.661 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x8) |  |  |
404 | 15:29:43.661 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
405 | 15:29:43.662 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
406 | 15:29:43.708 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
407 | 15:29:43.708 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
408 | 15:29:43.708 |  | →RRC DCCH UL Information Transfer |  |  |
409 | 15:29:43.708 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xb) |  |  |
410 | 15:29:43.708 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
411 | 15:29:43.797 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
412 | 15:29:44.347 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:1239: Step 3A Verdict: Pass
413 | 15:29:44.448 |  |  |  |  | MMICmd: Request PTT token
414 | 15:29:49.358 |  |  |  |  | ←SIP BYE | P-CSCF
415 | 15:29:49.362 |  | ←enobeB PCAP frame← SIP over IPSEC: BYE sip:PublicUserId-A@192.168.3.2:45784;transport... |  |  |
416 | 15:29:49.396 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
417 | 15:29:49.398 |  |  |  |  | →SIP 200 OK | P-CSCF
418 | 15:29:49.588 | →enobeB PCAP frame→ |  |  |  |
419 | 15:29:51.406 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
420 | 15:29:51.415 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
421 | 15:29:51.415 |  | [EMBEDDED NAS IN NEXT RRC] ESM Unknown message (type=0x72) |  |  |
422 | 15:29:51.415 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
423 | 15:29:51.416 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration |  |  |
424 | 15:29:51.468 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
425 | 15:29:51.468 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
426 | 15:29:51.468 |  | →RRC DCCH UL Information Transfer |  |  |
427 | 15:29:51.468 |  | [EMBEDDED NAS IN PREV RRC] Message too short (len=9) |  |  |
428 | 15:29:51.468 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
429 | 15:29:51.530 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
430 | 15:29:51.531 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
431 | 15:29:51.576 |  | ←RRC DCCH RRC Connection Release |  |  |
432 | 15:29:51.577 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
433 | 15:29:51.596 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
434 | 15:29:51.597 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:1249: Step 5 Verdict: Pass
435 | 15:29:51.598 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
436 | 15:29:51.600 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
437 | 15:29:52.348 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.