MSG #72 2021-10-26 11:51:56.098
RRC

     DCCH: RRC Connection Reconfiguration
    {
      message c1: rrcConnectionReconfiguration: {
        rrc-TransactionIdentifier 0,
        criticalExtensions c1: rrcConnectionReconfiguration-r8: {
          dedicatedInfoNASList {
            '272FFE14700206BBE73A7A472865C81C5B66A5407CB516ACBB8AFC0C4B1C7F588267004C786E2675DF28D3F5634691DAB91933F554EACA62AF7E6C16611158BC6D9F025F0E3ABE9EBA0765A7477B995A7528D1EB5773B41B36939FA07DB54CAA6037FFBB61426F4CEC4175A96ADB361C15BFCCA3AA3ECE0564A1FA9BA1A3B3FDDB1651836DC4EEDB'H
          },
          radioResourceConfigDedicated {
            srb-ToAddModList {
              {
                srb-Identity 2,
                rlc-Config explicitValue: am: {
                  ul-AM-RLC {
                    t-PollRetransmit ms60,
                    pollPDU pInfinity,
                    pollByte kBinfinity,
                    maxRetxThreshold t32
                  },
                  dl-AM-RLC {
                    t-Reordering ms45,
                    t-StatusProhibit ms0
                  }
                },
                logicalChannelConfig defaultValue: NULL
              }
            },
            drb-ToAddModList {
              {
                eps-BearerIdentity 5,
                drb-Identity 1,
                pdcp-Config {
                  discardTimer infinity,
                  rlc-AM {
                    statusReportRequired TRUE
                  },
                  headerCompression notUsed: NULL
                },
                rlc-Config am: {
                  ul-AM-RLC {
                    t-PollRetransmit ms80,
                    pollPDU p128,
                    pollByte kB125,
                    maxRetxThreshold t4
                  },
                  dl-AM-RLC {
                    t-Reordering ms80,
                    t-StatusProhibit ms60
                  }
                },
                logicalChannelIdentity 3,
                logicalChannelConfig {
                  ul-SpecificParameters {
                    priority 4,
                    prioritisedBitRate kBps8,
                    bucketSizeDuration ms100,
                    logicalChannelGroup 1
                  }
                }
              }
            },
            physicalConfigDedicated {
              cqi-ReportConfig {
                nomPDSCH-RS-EPRE-Offset 0,
                cqi-ReportPeriodic setup: {
                  cqi-PUCCH-ResourceIndex 0,
                  cqi-pmi-ConfigIndex 38,
                  cqi-FormatIndicatorPeriodic widebandCQI: NULL,
                  simultaneousAckNackAndCQI TRUE
                }
              }
            }
          }
        }
      }
    }