ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 11:50:23.717 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 11:50:23.722 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 11:50:23.723 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 11:50:23.725 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 11:50:23.726 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 11:50:23.727 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:824: IMS UDP port 192.168.2.3:5060 configured
7 | 11:50:23.732 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:774: IMS TCP port 192.168.2.3:5060 configured!
8 | 11:50:23.736 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:795: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 11:50:23.738 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:806: IdM port 192.168.2.3:8080 configured!
10 | 11:50:23.741 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 11:50:24.943 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 11:50:24.945 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 11:50:33.076 |  | ←RRC BCCH SIB |  |  |
14 | 11:50:33.081 |  | ←RRC BCCH SIB1 |  |  |
15 | 11:50:33.096 |  | ←RRC BCCH SIB |  |  |
16 | 11:50:33.116 |  | ←RRC BCCH SIB |  |  |
17 | 11:50:33.161 |  | ←RRC BCCH SIB1 |  |  |
18 | 11:51:55.795 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 11:51:55.795 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 11:51:55.795 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 11:51:55.795 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 11:51:55.856 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 11:51:55.856 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 11:51:55.856 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 11:51:55.856 |  |  |  | →NAS EMM Attach request |  |
26 | 11:51:55.856 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 11:51:55.856 |  |  |  | NAS K-asme 0f87eec55ba4268539a117589585abd7... |  |
28 | 11:51:55.856 |  |  |  | NAS ← EMM Authentication request |  |
29 | 11:51:55.857 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 11:51:55.857 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 11:51:55.858 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 11:51:55.928 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 11:51:55.928 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 11:51:55.928 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 11:51:55.928 |  |  |  | →NAS EMM Authentication response |  |
36 | 11:51:55.928 |  |  |  | NAS UE auth OK |  |
37 | 11:51:55.928 |  |  |  | NAS K-nas-cip d76eb75b2d421104a07774389b8b8... |  |
38 | 11:51:55.928 |  |  |  | NAS K-nas-int a7df112f537a03e4d324b8dcabc05... |  |
39 | 11:51:55.928 |  |  |  | NAS ← EMM Security mode command |  |
40 | 11:51:55.929 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 11:51:55.929 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 11:51:55.930 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 11:51:55.968 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
44 | 11:51:55.968 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 11:51:55.968 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x5) |  |  |
46 | 11:51:55.968 |  |  |  | →NAS EMM Security mode complete |  |
47 | 11:51:55.968 |  |  |  | NAS ← ESM ESM information request |  |
48 | 11:51:55.969 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xa) |  |  |
49 | 11:51:55.969 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 11:51:55.970 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
51 | 11:51:56.016 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
52 | 11:51:56.016 |  | →RRC DCCH UL Information Transfer |  |  |
53 | 11:51:56.016 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x9) |  |  |
54 | 11:51:56.016 |  |  |  | →NAS ESM ESM information response |  |
55 | 11:51:56.016 |  |  |  | NAS ← EMM Attach accept |  |
56 | 11:51:56.016 |  |  |  | NAS K-enb e47ff202ff580e693081e7ff59ba5c44c... |  |
57 | 11:51:56.017 |  | ←RRC DCCH Security Mode Command |  |  |
58 | 11:51:56.017 |  |  | RRC K-enb e47ff202ff580e693081e7ff59ba5c44c... |  |  |
59 | 11:51:56.017 |  |  | RRC rrc-cip 413aefcb4622016fad6487ced4fda4a... |  |  |
60 | 11:51:56.017 |  |  | RRC rrc-int 3a3261cbd4b183bceb174d634deb1c3... |  |  |
61 | 11:51:56.017 |  |  | RRC up-cip d56677b2d2f2e94b484883d9e0f67af7... |  |  |
62 | 11:51:56.017 |  |  | RRC up-int 285df6e7ef6b6271eb69ddf41b0c4f9c... |  |  |
63 | 11:51:56.018 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
64 | 11:51:56.026 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
65 | 11:51:56.048 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
66 | 11:51:56.048 |  | →RRC DCCH Security Mode Complete |  |  |
67 | 11:51:56.048 |  | ←RRC DCCH UE Capability Enquiry |  |  |
68 | 11:51:56.048 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
69 | 11:51:56.098 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
70 | 11:51:56.098 |  | →RRC DCCH UE Capability Information |  |  |
71 | 11:51:56.098 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x6) |  |  |
72 | 11:51:56.098 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
73 | 11:51:56.098 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
74 | 11:51:56.128 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
75 | 11:51:56.128 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
76 | 11:51:56.168 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
77 | 11:51:56.168 |  | →RRC DCCH UL Information Transfer |  |  |
78 | 11:51:56.168 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xc) |  |  |
79 | 11:51:56.168 |  |  |  | →NAS EMM Attach complete |  |
80 | 11:51:56.168 |  |  |  | NAS ← EMM EMM information |  |
81 | 11:51:56.169 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x8) |  |  |
82 | 11:51:56.169 |  | ←RRC DCCH DL Information Transfer |  |  |
83 | 11:51:56.170 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
84 | 11:52:02.254 |  | ←RRC DCCH RRC Connection Release |  |  |
85 | 11:52:02.255 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
86 | 11:52:04.235 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
87 | 11:52:04.235 |  | →RRC CCCH RRC Connection Request |  |  |
88 | 11:52:04.235 |  | ←RRC CCCH RRC Connection Setup |  |  |
89 | 11:52:04.235 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
90 | 11:52:04.288 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
91 | 11:52:04.288 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
92 | 11:52:04.288 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
93 | 11:52:04.288 |  |  |  | →NAS EMM Service request |  |
94 | 11:52:04.288 |  |  |  | NAS K-enb a815e5f5e16b9926afe46b5948f24e541... |  |
95 | 11:52:04.289 |  | ←RRC DCCH Security Mode Command |  |  |
96 | 11:52:04.289 |  |  | RRC K-enb a815e5f5e16b9926afe46b5948f24e541... |  |  |
97 | 11:52:04.289 |  |  | RRC rrc-cip 9f4cdf2b2ec7c18eb3034ba53294d50... |  |  |
98 | 11:52:04.289 |  |  | RRC rrc-int 7c267375a12452f39b3172d57601f33... |  |  |
99 | 11:52:04.289 |  |  | RRC up-cip 9df33a0297c2cd10bc0c3fc5db4c8a67... |  |  |
100 | 11:52:04.289 |  |  | RRC up-int 6adec0acd4ac464fea9232ce755e331d... |  |  |
101 | 11:52:04.290 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
102 | 11:52:04.328 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
103 | 11:52:04.328 |  | →RRC DCCH Security Mode Complete |  |  |
104 | 11:52:04.328 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
105 | 11:52:04.328 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
106 | 11:52:04.368 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
107 | 11:52:04.368 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
108 | 11:52:29.248 | →enobeB PCAP frame→ TCP |  |  |  |
109 | 11:52:29.251 |  | ←enobeB PCAP frame← TCP |  |  |
110 | 11:52:29.288 | →enobeB PCAP frame→ TCP |  |  |  |
111 | 11:52:29.376 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
112 | 11:52:29.380 |  | ←enobeB PCAP frame← TCP |  |  |
113 | 11:52:29.383 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
114 | 11:52:29.408 | →enobeB PCAP frame→ TCP |  |  |  |
115 | 11:52:29.496 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
116 | 11:52:29.496 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 16)
117 | 11:52:29.499 |  | ←enobeB PCAP frame← TCP |  |  |
118 | 11:52:29.500 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
119 | 11:52:29.528 | →enobeB PCAP frame→ TCP |  |  |  |
120 | 11:52:29.575 |  |  |  |  | →HTTP GET | HTTP-Proxy
121 | 11:52:29.576 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
122 | 11:52:29.578 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:302: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
123 | 11:52:29.579 |  | ←enobeB PCAP frame← TCP |  |  |
124 | 11:52:29.584 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
125 | 11:52:29.589 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
126 | 11:52:29.590 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
127 | 11:52:29.608 | →enobeB PCAP frame→ TCP |  |  |  |
128 | 11:52:29.648 | →enobeB PCAP frame→ TCP |  |  |  |
129 | 11:52:31.648 | →enobeB PCAP frame→ TCP |  |  |  |
130 | 11:52:31.651 |  | ←enobeB PCAP frame← TCP |  |  |
131 | 11:52:31.688 | →enobeB PCAP frame→ TCP |  |  |  |
132 | 11:52:31.696 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
133 | 11:52:31.699 |  | ←enobeB PCAP frame← TCP |  |  |
134 | 11:52:31.704 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
135 | 11:52:31.728 | →enobeB PCAP frame→ TCP |  |  |  |
136 | 11:52:32.016 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
137 | 11:52:32.016 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
138 | 11:52:32.019 |  | ←enobeB PCAP frame← TCP |  |  |
139 | 11:52:32.020 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
140 | 11:52:32.048 | →enobeB PCAP frame→ TCP |  |  |  |
141 | 11:52:32.056 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
142 | 11:52:32.057 |  |  |  |  | →HTTP GET | IDMS-Endpoint
143 | 11:52:32.060 |  | ←enobeB PCAP frame← TCP |  |  |
144 | 11:52:32.099 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
145 | 11:52:32.102 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:525: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
146 | 11:52:32.102 |  |  |  |  | MMICmd: Please provide user credentials: username and password
147 | 11:52:32.103 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
148 | 11:52:32.168 | →enobeB PCAP frame→ TCP |  |  |  |
149 | 11:52:36.856 | →enobeB PCAP frame→ HTTPS: POST /idms/userauth HTTP/1.1 |  |  |  |
150 | 11:52:36.858 |  |  |  |  | →HTTP POST | IDMS-Endpoint
151 | 11:52:36.860 |  | ←enobeB PCAP frame← TCP |  |  |
152 | 11:52:36.868 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
153 | 11:52:36.872 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
154 | 11:52:36.872 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:530: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
155 | 11:52:36.887 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:693: IdM port - Client closed the connection (id 18)
156 | 11:52:36.888 | →enobeB PCAP frame→ TCP |  |  |  |
157 | 11:52:36.891 |  | ←enobeB PCAP frame← TCP |  |  |
158 | 11:52:36.928 | →enobeB PCAP frame→ TCP |  |  |  |
159 | 11:52:37.488 | →enobeB PCAP frame→ TCP |  |  |  |
160 | 11:52:37.491 |  | ←enobeB PCAP frame← TCP |  |  |
161 | 11:52:37.528 | →enobeB PCAP frame→ TCP |  |  |  |
162 | 11:52:37.576 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
163 | 11:52:37.579 |  | ←enobeB PCAP frame← TCP |  |  |
164 | 11:52:37.580 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
165 | 11:52:37.608 | →enobeB PCAP frame→ TCP |  |  |  |
166 | 11:52:37.656 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
167 | 11:52:37.657 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
168 | 11:52:37.662 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
169 | 11:52:37.688 | →enobeB PCAP frame→ TCP |  |  |  |
170 | 11:52:37.735 |  |  |  |  | →HTTP POST | IDMS-Endpoint
171 | 11:52:37.736 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
172 | 11:52:37.739 |  | ←enobeB PCAP frame← TCP |  |  |
173 | 11:52:37.746 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
174 | 11:52:37.749 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:535: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
175 | 11:52:37.750 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
176 | 11:52:37.808 | →enobeB PCAP frame→ TCP |  |  |  |
177 | 11:52:38.168 | →enobeB PCAP frame→ TCP |  |  |  |
178 | 11:52:38.171 |  | ←enobeB PCAP frame← TCP |  |  |
179 | 11:52:38.208 | →enobeB PCAP frame→ TCP |  |  |  |
180 | 11:52:38.216 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
181 | 11:52:38.219 |  | ←enobeB PCAP frame← TCP |  |  |
182 | 11:52:38.221 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
183 | 11:52:38.248 | →enobeB PCAP frame→ TCP |  |  |  |
184 | 11:52:38.256 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
185 | 11:52:38.256 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 19)
186 | 11:52:38.259 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
187 | 11:52:38.296 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
188 | 11:52:38.298 |  |  |  |  | →HTTP POST | HTTP-Proxy
189 | 11:52:38.303 |  | ←enobeB PCAP frame← TCP |  |  |
190 | 11:52:38.321 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:555: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
191 | 11:52:38.328 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
192 | 11:52:38.334 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
193 | 11:52:38.335 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
194 | 11:52:38.368 | →enobeB PCAP frame→ TCP |  |  |  |
195 | 11:52:38.408 | →enobeB PCAP frame→ TCP |  |  |  |
196 | 11:52:38.411 |  | ←enobeB PCAP frame← TCP |  |  |
197 | 11:52:38.448 | →enobeB PCAP frame→ TCP |  |  |  |
198 | 11:52:38.456 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
199 | 11:52:38.459 |  | ←enobeB PCAP frame← TCP |  |  |
200 | 11:52:38.460 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
201 | 11:52:38.488 | →enobeB PCAP frame→ TCP |  |  |  |
202 | 11:52:38.495 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 20)
203 | 11:52:38.496 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
204 | 11:52:38.499 |  | ←enobeB PCAP frame← TCP |  |  |
205 | 11:52:38.500 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
206 | 11:52:38.536 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
207 | 11:52:38.538 |  |  |  |  | →HTTP POST | HTTP-Proxy
208 | 11:52:38.540 |  | ←enobeB PCAP frame← TCP |  |  |
209 | 11:52:38.598 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
210 | 11:52:38.599 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:559: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
211 | 11:52:38.603 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
212 | 11:52:38.604 |  | ←enobeB PCAP frame← TCP |  |  |
213 | 11:52:38.605 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
214 | 11:52:38.648 | →enobeB PCAP frame→ TCP |  |  |  |
215 | 11:52:38.688 | →enobeB PCAP frame→ TCP |  |  |  |
216 | 11:52:38.696 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
217 | 11:52:38.698 |  |  |  |  | →SIP REGISTER | P-CSCF
218 | 11:52:38.719 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:833: IMS UDP_s port 192.168.2.3:5062 configured
219 | 11:52:38.734 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:784: IMS TCP_s port 192.168.2.3:5062 configured!
220 | 11:52:38.735 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:842: IMS UDP_c port 192.168.2.3:5061 configured
221 | 11:52:38.739 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
222 | 11:52:38.743 |  | ←enobeB PCAP frame← SIP -cleartext-: SIP/2.0 401 Unauthorized |  |  |
223 | 11:52:39.376 | →enobeB PCAP frame→ SIP over IPSEC: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
224 | 11:52:39.380 |  |  |  |  | →SIP REGISTER | P-CSCF
225 | 11:52:39.401 |  |  |  |  | ←SIP 200 OK | P-CSCF
226 | 11:52:39.406 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
227 | 11:52:39.776 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
228 | 11:52:39.777 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 SIP over IPSEC: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 |  |  |  |
229 | 11:52:39.789 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
230 | 11:52:39.820 |  |  |  |  | ←SIP 200 OK | P-CSCF
231 | 11:52:39.821 |  |  |  |  | MIKEY | Media-Server
232 | 11:52:39.825 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
233 | 11:52:40.024 |  |  |  |  | XML→ | Media-Server
234 | 11:52:40.026 |  |  |  |  | XML→ | Media-Server
235 | 11:52:40.029 |  |  |  |  | ←XML | Media-Server
236 | 11:52:40.033 |  |  |  |  | ←SIP NOTIFY | P-CSCF
237 | 11:52:40.038 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
238 | 11:52:40.039 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:39146;transp... |  |  |
239 | 11:52:40.096 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
240 | 11:52:40.096 |  |  |  |  | →SIP 200 OK | P-CSCF
241 | 11:52:40.248 | →enobeB PCAP frame→ TCP |  |  |  |
242 | 11:52:40.251 |  | ←enobeB PCAP frame← TCP |  |  |
243 | 11:52:40.288 | →enobeB PCAP frame→ TCP |  |  |  |
244 | 11:52:40.296 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
245 | 11:52:40.299 |  | ←enobeB PCAP frame← TCP |  |  |
246 | 11:52:40.302 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
247 | 11:52:40.328 | →enobeB PCAP frame→ TCP |  |  |  |
248 | 11:52:40.376 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
249 | 11:52:40.376 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
250 | 11:52:40.379 |  | ←enobeB PCAP frame← TCP |  |  |
251 | 11:52:40.380 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
252 | 11:52:40.408 | →enobeB PCAP frame→ TCP |  |  |  |
253 | 11:52:40.416 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
254 | 11:52:40.417 |  |  |  |  | →HTTP GET | HTTP-Proxy
255 | 11:52:40.419 |  | ←enobeB PCAP frame← TCP |  |  |
256 | 11:52:40.426 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:656: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcptt-ue-configuration.xml
257 | 11:52:40.435 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
258 | 11:52:40.440 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
259 | 11:52:40.487 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
260 | 11:52:40.488 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
261 | 11:52:40.491 |  | ←enobeB PCAP frame← TCP |  |  |
262 | 11:52:40.497 | →enobeB PCAP frame→ TCP |  |  |  |
263 | 11:52:40.500 |  | ←enobeB PCAP frame← TCP |  |  |
264 | 11:52:40.528 | →enobeB PCAP frame→ TCP |  |  |  |
265 | 11:52:40.648 | →enobeB PCAP frame→ TCP |  |  |  |
266 | 11:52:40.651 |  | ←enobeB PCAP frame← TCP |  |  |
267 | 11:52:40.688 | →enobeB PCAP frame→ TCP |  |  |  |
268 | 11:52:40.696 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
269 | 11:52:40.700 |  | ←enobeB PCAP frame← TCP |  |  |
270 | 11:52:40.703 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
271 | 11:52:40.728 | →enobeB PCAP frame→ TCP |  |  |  |
272 | 11:52:40.816 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
273 | 11:52:40.816 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
274 | 11:52:40.819 |  | ←enobeB PCAP frame← TCP |  |  |
275 | 11:52:40.820 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
276 | 11:52:40.848 | →enobeB PCAP frame→ TCP |  |  |  |
277 | 11:52:40.856 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
278 | 11:52:40.857 |  |  |  |  | →HTTP GET | HTTP-Proxy
279 | 11:52:40.859 |  | ←enobeB PCAP frame← TCP |  |  |
280 | 11:52:40.869 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:661: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcptt-user-profile-49.xml
281 | 11:52:40.903 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
282 | 11:52:40.911 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
283 | 11:52:40.912 |  | ←enobeB PCAP frame← TCP |  |  |
284 | 11:52:40.913 |  | ←enobeB PCAP frame← TCP |  |  |
285 | 11:52:40.914 |  | ←enobeB PCAP frame← TCP |  |  |
286 | 11:52:40.915 |  | ←enobeB PCAP frame← TCP |  |  |
287 | 11:52:40.916 |  | ←enobeB PCAP frame← TCP |  |  |
288 | 11:52:40.917 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
289 | 11:52:40.928 | →enobeB PCAP frame→ TCP |  |  |  |
290 | 11:52:40.936 | →enobeB PCAP frame→ TCP |  |  |  |
291 | 11:52:40.944 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
292 | 11:52:40.944 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
293 | 11:52:40.947 |  | ←enobeB PCAP frame← TCP |  |  |
294 | 11:52:40.948 |  | ←enobeB PCAP frame← TCP |  |  |
295 | 11:52:40.952 | →enobeB PCAP frame→ TCP |  |  |  |
296 | 11:52:40.955 |  | ←enobeB PCAP frame← TCP |  |  |
297 | 11:52:40.968 | →enobeB PCAP frame→ TCP |  |  |  |
298 | 11:52:41.536 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
299 | 11:52:41.537 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
300 | 11:52:41.540 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
301 | 11:52:41.561 |  |  |  |  | ←SIP 200 OK | P-CSCF
302 | 11:52:41.561 |  |  |  |  | MIKEY | Media-Server
303 | 11:52:41.565 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
304 | 11:52:41.608 | →enobeB PCAP frame→ TCP |  |  |  |
305 | 11:52:41.611 |  | ←enobeB PCAP frame← TCP |  |  |
306 | 11:52:41.648 | →enobeB PCAP frame→ TCP |  |  |  |
307 | 11:52:41.656 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
308 | 11:52:41.659 |  | ←enobeB PCAP frame← TCP |  |  |
309 | 11:52:41.660 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
310 | 11:52:41.688 | →enobeB PCAP frame→ TCP |  |  |  |
311 | 11:52:41.771 |  |  |  |  | XML→ | Media-Server
312 | 11:52:41.772 |  |  |  |  | XML→ | Media-Server
313 | 11:52:41.775 |  |  |  |  | ←XML | Media-Server
314 | 11:52:41.775 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
315 | 11:52:41.776 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
316 | 11:52:41.778 |  |  |  |  | ←SIP NOTIFY | P-CSCF
317 | 11:52:41.779 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
318 | 11:52:41.783 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:39146;transp... |  |  |
319 | 11:52:41.808 | →enobeB PCAP frame→ TCP |  |  |  |
320 | 11:52:41.815 |  |  |  |  | →HTTP GET | HTTP-Proxy
321 | 11:52:41.816 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
322 | 11:52:41.816 |  |  |  |  | →SIP 200 OK | P-CSCF
323 | 11:52:41.818 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:666: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
324 | 11:52:41.819 |  | ←enobeB PCAP frame← TCP |  |  |
325 | 11:52:41.824 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
326 | 11:52:41.829 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
327 | 11:52:41.831 |  | ←enobeB PCAP frame← TCP |  |  |
328 | 11:52:41.832 |  | ←enobeB PCAP frame← TCP |  |  |
329 | 11:52:41.833 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
330 | 11:52:41.888 | →enobeB PCAP frame→ TCP |  |  |  |
331 | 11:52:41.896 | →enobeB PCAP frame→ TCP |  |  |  |
332 | 11:52:41.928 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
333 | 11:52:41.928 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
334 | 11:52:41.931 |  | ←enobeB PCAP frame← TCP |  |  |
335 | 11:52:41.936 | →enobeB PCAP frame→ TCP |  |  |  |
336 | 11:52:41.939 |  | ←enobeB PCAP frame← TCP |  |  |
337 | 11:52:41.968 | →enobeB PCAP frame→ TCP |  |  |  |
338 | 11:52:42.008 | →enobeB PCAP frame→ TCP |  |  |  |
339 | 11:52:42.011 |  | ←enobeB PCAP frame← TCP |  |  |
340 | 11:52:42.048 | →enobeB PCAP frame→ TCP |  |  |  |
341 | 11:52:42.056 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
342 | 11:52:42.059 |  | ←enobeB PCAP frame← TCP |  |  |
343 | 11:52:42.062 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
344 | 11:52:42.088 | →enobeB PCAP frame→ TCP |  |  |  |
345 | 11:52:42.176 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
346 | 11:52:42.176 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
347 | 11:52:42.179 |  | ←enobeB PCAP frame← TCP |  |  |
348 | 11:52:42.180 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
349 | 11:52:42.208 | →enobeB PCAP frame→ TCP |  |  |  |
350 | 11:52:42.216 | →enobeB PCAP frame→ HTTPS: GET http://xcap.gms.mcstaasting.com/org.openmobile... |  |  |  |
351 | 11:52:42.216 |  |  |  |  | →HTTP GET | HTTP-Proxy
352 | 11:52:42.219 |  | ←enobeB PCAP frame← TCP |  |  |
353 | 11:52:42.219 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:671: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at http://xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
354 | 11:52:42.226 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
355 | 11:52:42.232 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
356 | 11:52:42.233 |  | ←enobeB PCAP frame← TCP |  |  |
357 | 11:52:42.234 |  | ←enobeB PCAP frame← TCP |  |  |
358 | 11:52:42.235 |  | ←enobeB PCAP frame← TCP |  |  |
359 | 11:52:42.236 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
360 | 11:52:42.288 | →enobeB PCAP frame→ TCP |  |  |  |
361 | 11:52:42.295 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
362 | 11:52:42.296 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
363 | 11:52:42.299 |  | ←enobeB PCAP frame← TCP |  |  |
364 | 11:52:42.328 | →enobeB PCAP frame→ TCP |  |  |  |
365 | 11:52:42.576 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
366 | 11:52:42.577 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
367 | 11:52:42.584 |  |  |  |  | →SIP PUBLISH | P-CSCF
368 | 11:52:42.618 |  |  |  |  | MIKEY | Media-Server
369 | 11:52:42.656 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
370 | 11:52:42.657 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
371 | 11:52:42.659 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
372 | 11:52:42.837 |  |  |  |  | XML→ | Media-Server
373 | 11:52:42.840 |  |  |  |  | ←SIP 200 OK | P-CSCF
374 | 11:52:42.844 |  |  |  |  | ←SIP 200 OK | P-CSCF
375 | 11:52:42.844 |  |  |  |  | MIKEY | Media-Server
376 | 11:52:42.845 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
377 | 11:52:42.848 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
378 | 11:52:43.046 |  |  |  |  | XML→ | Media-Server
379 | 11:52:43.047 |  |  |  |  | XML→ | Media-Server
380 | 11:52:43.086 |  |  |  |  | MIKEY | Media-Server
381 | 11:52:43.086 |  |  |  |  | ←XML | Media-Server
382 | 11:52:43.091 |  |  |  |  | ←SIP NOTIFY | P-CSCF
383 | 11:52:43.096 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
384 | 11:52:43.097 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:39146;transp... |  |  |
385 | 11:52:43.136 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
386 | 11:52:43.137 |  |  |  |  | →SIP 200 OK | P-CSCF
387 | 11:52:43.149 |  |  |  |  | ←XML | Media-Server
388 | 11:52:43.184 |  |  |  |  | ←SIP MESSAGE | P-CSCF
389 | 11:52:43.191 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
390 | 11:52:43.192 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
391 | 11:52:43.193 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
392 | 11:52:44.016 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
393 | 11:52:44.016 |  |  |  |  | →SIP 200 OK | P-CSCF
394 | 11:52:44.020 |  |  |  |  | Info: MCX_IMS_CommonProcedures.ttcn:228: MESSAGE/200OK Table 5.3.2.3-2 Steps 7-8 Done
395 | 11:52:46.022 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
396 | 11:52:46.070 |  | ←RRC DCCH RRC Connection Release |  |  |
397 | 11:52:46.071 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
398 | 11:52:46.088 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
399 | 11:52:46.089 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:72: Test-Body Step 1
400 | 11:52:46.091 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
401 | 11:52:46.091 |  |  |  |  | MMICmd: Make the MCPTT User request the establishment of an MCPTT private call, on-demand Automatic Commencement Mode, no Force of automatic commencement, applying End-to-end communication security with Floor Control
402 | 11:52:46.092 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:75: Test-Body Step 2
403 | 11:52:50.235 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
404 | 11:52:50.235 |  | →RRC CCCH RRC Connection Request |  |  |
405 | 11:52:50.235 |  | ←RRC CCCH RRC Connection Setup |  |  |
406 | 11:52:50.235 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
407 | 11:52:50.288 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
408 | 11:52:50.288 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
409 | 11:52:50.288 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
410 | 11:52:50.288 |  |  |  | →NAS EMM Service request |  |
411 | 11:52:50.288 |  |  |  | NAS K-enb 560f16a10b4e63640e8975ab29862590e... |  |
412 | 11:52:50.289 |  | ←RRC DCCH Security Mode Command |  |  |
413 | 11:52:50.289 |  |  | RRC K-enb 560f16a10b4e63640e8975ab29862590e... |  |  |
414 | 11:52:50.289 |  |  | RRC rrc-cip 120fa8585fc8f6a47cf5c762c6e3973... |  |  |
415 | 11:52:50.289 |  |  | RRC rrc-int 685eed96198a66e845fa0a3e8ab9470... |  |  |
416 | 11:52:50.289 |  |  | RRC up-cip e93bf32c0e2a1af7148f2cc08fb99440... |  |  |
417 | 11:52:50.289 |  |  | RRC up-int 4e96546e28997d06c0ccef13b8ddf29b... |  |  |
418 | 11:52:50.290 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
419 | 11:52:50.328 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
420 | 11:52:50.328 |  | →RRC DCCH Security Mode Complete |  |  |
421 | 11:52:50.328 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
422 | 11:52:50.328 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
423 | 11:52:50.368 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
424 | 11:52:50.368 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
425 | 11:52:50.376 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
426 | 11:52:50.377 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |  |
427 | 11:52:50.385 |  |  |  |  | →SIP INVITE | P-CSCF
428 | 11:52:50.416 |  |  |  |  | MIKEY | Media-Server
429 | 11:52:50.626 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:754: SRTP config: Master Key: BCE69D051AE10611D3DCBA7A951AA7CE, Master Salt: 3983DABED7778606D28317DA, MKI: 295C295B
430 | 11:52:50.626 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
431 | 11:52:50.630 |  |  |  |  | XML→ | Media-Server
432 | 11:52:50.631 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
433 | 11:52:50.632 |  |  |  |  | XML→ | Media-Server
434 | 11:52:50.634 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1244: INVITE Verdict: Pass
435 | 11:52:50.635 |  |  |  |  | ←SIP 100 Trying | P-CSCF
436 | 11:52:50.637 |  |  |  |  | ←SIP 200 OK | P-CSCF
437 | 11:52:50.639 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
438 | 11:52:50.641 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
439 | 11:52:51.267 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
440 | 11:52:51.267 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x0) |  |  |
441 | 11:52:51.267 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
442 | 11:52:51.268 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
443 | 11:52:51.288 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
444 | 11:52:51.288 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
445 | 11:52:51.328 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
446 | 11:52:51.328 |  | →RRC DCCH UL Information Transfer |  |  |
447 | 11:52:51.328 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x6) |  |  |
448 | 11:52:51.328 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
449 | 11:52:51.398 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
450 | 11:52:51.656 | →enobeB PCAP frame→ SIP over IPSEC: ACK sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
451 | 11:52:51.657 |  |  |  |  | →SIP ACK | P-CSCF
452 | 11:52:51.666 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1247: ACK Verdict: Pass
453 | 11:52:51.667 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:77: Step 2 Verdict: Pass
454 | 11:52:51.667 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:81: Test-Body Step 5A
455 | 11:52:51.670 |  |  |  |  | ←Floor Granted | Media-Server
456 | 11:52:51.674 |  | ←enobeB PCAP frame← |  |  |
457 | 11:52:52.208 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
458 | 11:52:52.216 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
459 | 11:52:52.224 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
460 | 11:52:52.248 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
461 | 11:52:52.288 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
462 | 11:52:52.417 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:82: Step 5A Verdict: Pass
463 | 11:52:52.417 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:84: Test-Body Step 6
464 | 11:52:52.418 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:87: Test-Body Step 7
465 | 11:52:52.519 |  |  |  |  | MMICmd: Release PTT token
466 | 11:52:53.832 | →enobeB PCAP frame→ |  |  |  |
467 | 11:52:53.832 |  |  |  |  | Floor Release→ | Media-Server
468 | 11:52:53.835 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
469 | 11:52:53.836 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:89: Step 7 Verdict: Pass
470 | 11:52:53.836 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:93: Test-Body Step 10
471 | 11:52:53.836 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:96: Test-Body Step 11
472 | 11:52:53.839 |  |  |  |  | ←Floor Taken | Media-Server
473 | 11:52:53.843 |  | ←enobeB PCAP frame← |  |  |
474 | 11:52:53.937 |  |  |  |  | MMICmd: Request PTT token
475 | 11:52:54.968 | →enobeB PCAP frame→ |  |  |  |
476 | 11:52:54.968 |  |  |  |  | Floor Request→ | Media-Server
477 | 11:52:54.971 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Request Verdict: Pass
478 | 11:52:54.971 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:98: Step 11 Verdict: Pass
479 | 11:52:54.971 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:102: Test-Body Step 13
480 | 11:52:54.972 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:105: Test-Body Step 14
481 | 11:52:54.972 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:108: Test-Body Step 15
482 | 11:52:54.973 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:111: Test-Body Step 16
483 | 11:52:54.975 |  |  |  |  | ←Floor Deny | Media-Server
484 | 11:52:54.976 |  |  |  |  | ←Floor Idle | Media-Server
485 | 11:52:54.979 |  | ←enobeB PCAP frame← |  |  |
486 | 11:52:54.980 |  | ←enobeB PCAP frame← |  |  |
487 | 11:52:55.074 |  |  |  |  | MMICmd: Release PTT token
488 | 11:52:55.175 |  |  |  |  | MMICmd: Request PTT token
489 | 11:52:56.528 | →enobeB PCAP frame→ |  |  |  |
490 | 11:52:56.528 |  |  |  |  | Floor Request→ | Media-Server
491 | 11:52:56.531 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Request Verdict: Pass
492 | 11:52:56.534 |  |  |  |  | ←Floor Granted | Media-Server
493 | 11:52:56.539 |  | ←enobeB PCAP frame← |  |  |
494 | 11:52:56.568 | →enobeB PCAP frame→ |  |  |  |
495 | 11:52:56.568 |  |  |  |  | Floor ACK→ | Media-Server
496 | 11:52:56.571 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Ack Verdict: Pass
497 | 11:52:56.571 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:113: Step 16 Verdict: Pass
498 | 11:52:56.571 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:117: Test-Body Step 18
499 | 11:52:56.572 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:120: Test-Body Step 18A
500 | 11:52:56.648 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
501 | 11:52:56.652 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
502 | 11:52:56.656 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
503 | 11:52:56.660 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
504 | 11:52:56.664 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
505 | 11:52:56.673 |  |  |  |  | MMICmd: Release PTT token
506 | 11:52:57.936 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
507 | 11:52:57.936 |  |  |  |  | Floor Release→ | Media-Server
508 | 11:52:57.939 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
509 | 11:52:57.939 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
510 | 11:52:57.940 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:122: Step 18A Verdict: Pass
511 | 11:52:57.940 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:124: Test-Body Step 19
512 | 11:52:57.941 |  |  |  |  | MMICmd: Make the UE (MCPTT User) request upgrade of the ongoing private call to MCPTT emergency private call
513 | 11:52:57.942 |  |  |  |  | ←Floor Idle | Media-Server
514 | 11:52:57.942 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:127: Test-Body Step 20
515 | 11:52:57.947 |  | ←enobeB PCAP frame← |  |  |
516 | 11:53:02.656 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
517 | 11:53:02.657 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
518 | 11:53:02.658 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 SIP XML: application/vnd.3gpp.mcptt-signed+xml SRTP frame: |  |  |  |
519 | 11:53:02.668 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
520 | 11:53:02.674 |  |  |  |  | →SIP INVITE | P-CSCF
521 | 11:53:02.683 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
522 | 11:53:02.688 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
523 | 11:53:02.691 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
524 | 11:53:02.701 |  |  |  |  | MIKEY | Media-Server
525 | 11:53:02.912 |  |  |  |  | XML→ | Media-Server
526 | 11:53:02.980 |  |  |  |  | XML→ | Media-Server
527 | 11:53:02.984 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1305: re-INVITE Verdict: Pass
528 | 11:53:02.986 |  |  |  |  | ←SIP 100 Trying | P-CSCF
529 | 11:53:02.989 |  |  |  |  | ←SIP 200 OK | P-CSCF
530 | 11:53:02.991 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
531 | 11:53:02.994 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
532 | 11:53:03.008 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
533 | 11:53:03.011 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
534 | 11:53:03.048 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
535 | 11:53:03.051 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
536 | 11:53:03.056 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
537 | 11:53:03.257 |  |  |  |  | →SIP ACK | P-CSCF
538 | 11:53:03.266 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1310: ACK Verdict: Pass
539 | 11:53:03.270 |  |  |  |  | ←Floor Granted | Media-Server
540 | 11:53:03.274 |  | ←enobeB PCAP frame← |  |  |
541 | 11:53:03.288 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
542 | 11:53:03.291 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
543 | 11:53:03.295 |  |  |  |  | Floor ACK→ | Media-Server
544 | 11:53:03.296 | →enobeB PCAP frame→ |  |  |  |
545 | 11:53:03.300 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Ack Verdict: Pass
546 | 11:53:03.300 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:133: Test-Body Step 22A
547 | 11:53:03.300 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:140: Test-Body Step 23
548 | 11:53:03.300 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:143: Test-Body Step 24
549 | 11:53:03.328 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
550 | 11:53:03.331 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
551 | 11:53:03.336 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
552 | 11:53:03.339 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
553 | 11:53:03.344 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
554 | 11:53:03.402 |  |  |  |  | MMICmd: Release PTT token
555 | 11:53:04.736 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
556 | 11:53:04.736 |  |  |  |  | Floor Release→ | Media-Server
557 | 11:53:04.739 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
558 | 11:53:04.740 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
559 | 11:53:04.740 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:145: Step 24 Verdict: Pass
560 | 11:53:04.740 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:149: Test-Body Step 27
561 | 11:53:04.741 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:152: Test-Body Step 28
562 | 11:53:04.743 |  |  |  |  | ←Floor Taken | Media-Server
563 | 11:53:04.744 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
564 | 11:53:04.747 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
565 | 11:53:04.842 |  |  |  |  | MMICmd: Request PTT token
566 | 11:53:06.088 | →enobeB PCAP frame→ |  |  |  |
567 | 11:53:06.088 |  |  |  |  | Floor Request→ | Media-Server
568 | 11:53:06.091 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Request Verdict: Pass
569 | 11:53:06.094 |  |  |  |  | ←Floor Granted | Media-Server
570 | 11:53:06.101 |  | ←enobeB PCAP frame← |  |  |
571 | 11:53:06.128 | →enobeB PCAP frame→ |  |  |  |
572 | 11:53:06.128 |  |  |  |  | Floor ACK→ | Media-Server
573 | 11:53:06.131 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Ack Verdict: Pass
574 | 11:53:06.131 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:154: Step 28 Verdict: Pass
575 | 11:53:06.132 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:158: Test-Body Step 30
576 | 11:53:06.132 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:161: Test-Body Step 31
577 | 11:53:06.168 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
578 | 11:53:06.172 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
579 | 11:53:06.208 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
580 | 11:53:06.212 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
581 | 11:53:06.216 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
582 | 11:53:06.234 |  |  |  |  | MMICmd: Release PTT token
583 | 11:53:07.416 |  |  |  |  | Floor Release→ | Media-Server
584 | 11:53:07.420 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
585 | 11:53:07.420 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:163: Step 31 Verdict: Pass
586 | 11:53:07.420 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:167: Test-Body Step 33
587 | 11:53:07.422 |  |  |  |  | MMICmd: Make the UE (MCPTT User) request cancelling of MCPTT emergency private call
588 | 11:53:07.423 |  |  |  |  | ←Floor Idle | Media-Server
589 | 11:53:07.423 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:170: Test-Body Step 34
590 | 11:53:07.433 |  | ←enobeB PCAP frame← |  |  |
591 | 11:53:14.016 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
592 | 11:53:14.017 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
593 | 11:53:14.018 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
594 | 11:53:14.019 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 SIP XML: application/vnd.3gpp.mcptt-signed+xml SRTP frame: |  |  |  |
595 | 11:53:14.048 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
596 | 11:53:14.088 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
597 | 11:53:14.089 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
598 | 11:53:14.096 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
599 | 11:53:14.096 |  |  |  |  | →SIP INVITE | P-CSCF
600 | 11:53:14.130 |  |  |  |  | MIKEY | Media-Server
601 | 11:53:14.349 |  |  |  |  | XML→ | Media-Server
602 | 11:53:14.350 |  |  |  |  | XML→ | Media-Server
603 | 11:53:14.352 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1305: re-INVITE Verdict: Pass
604 | 11:53:14.354 |  |  |  |  | ←SIP 100 Trying | P-CSCF
605 | 11:53:14.356 |  |  |  |  | ←SIP 200 OK | P-CSCF
606 | 11:53:14.358 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
607 | 11:53:14.360 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
608 | 11:53:14.368 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
609 | 11:53:14.371 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
610 | 11:53:14.408 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
611 | 11:53:14.411 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
612 | 11:53:14.416 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
613 | 11:53:14.726 |  |  |  |  | →SIP ACK | P-CSCF
614 | 11:53:14.735 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl.ttcn:1310: ACK Verdict: Pass
615 | 11:53:14.735 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:172: Step 34 Verdict: Pass
616 | 11:53:14.736 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:176: Test-Body Step 36A
617 | 11:53:14.736 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:179: Test-Body Step 36B
618 | 11:53:14.837 |  |  |  |  | MMICmd: Request PTT token
619 | 11:53:16.368 | →enobeB PCAP frame→ |  |  |  |
620 | 11:53:16.368 |  |  |  |  | Floor Request→ | Media-Server
621 | 11:53:16.371 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Request Verdict: Pass
622 | 11:53:16.375 |  |  |  |  | ←Floor Granted | Media-Server
623 | 11:53:16.379 |  | ←enobeB PCAP frame← |  |  |
624 | 11:53:16.408 | →enobeB PCAP frame→ |  |  |  |
625 | 11:53:16.408 |  |  |  |  | Floor ACK→ | Media-Server
626 | 11:53:16.411 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Ack Verdict: Pass
627 | 11:53:16.412 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:181: Step 36B Verdict: Pass
628 | 11:53:16.412 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:183: Test-Body Step 37
629 | 11:53:16.412 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:186: Test-Body Step 38
630 | 11:53:16.448 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
631 | 11:53:16.452 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
632 | 11:53:16.488 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
633 | 11:53:16.495 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
634 | 11:53:16.496 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
635 | 11:53:16.513 |  |  |  |  | MMICmd: Release PTT token
636 | 11:53:17.744 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
637 | 11:53:17.744 |  |  |  |  | Floor Release→ | Media-Server
638 | 11:53:17.747 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:154: Floor Release Verdict: Pass
639 | 11:53:17.748 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
640 | 11:53:17.748 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:188: Step 38 Verdict: Pass
641 | 11:53:17.748 |  |  |  |  | Info: MCPTT_PrivateCall_MCX_IMS.ttcn:192: Test-Body Step 40 - 41
642 | 11:53:17.751 |  |  |  |  | ←Floor Idle | Media-Server
643 | 11:53:17.755 |  | ←enobeB PCAP frame← |  |  |
644 | 11:53:17.853 |  |  |  |  | MMICmd: Release call (hang up the call)
645 | 11:53:19.776 | →enobeB PCAP frame→ SIP over IPSEC: BYE sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
646 | 11:53:19.778 |  |  |  |  | →SIP BYE | P-CSCF
647 | 11:53:19.797 |  |  |  |  | ←SIP 200 OK | P-CSCF
648 | 11:53:19.802 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
649 | 11:53:20.168 | →enobeB PCAP frame→ |  |  |  |
650 | 11:53:21.796 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
651 | 11:53:21.808 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
652 | 11:53:21.809 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x0) |  |  |
653 | 11:53:21.809 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
654 | 11:53:21.810 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
655 | 11:53:21.848 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
656 | 11:53:21.848 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
657 | 11:53:21.848 |  | →RRC DCCH UL Information Transfer |  |  |
658 | 11:53:21.848 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x0) |  |  |
659 | 11:53:21.848 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
660 | 11:53:21.923 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
661 | 11:53:21.924 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
662 | 11:53:21.961 |  | ←RRC DCCH RRC Connection Release |  |  |
663 | 11:53:21.962 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
664 | 11:53:21.980 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
665 | 11:53:21.981 |  |  |  |  | Verdict PASS: MCPTT_PrivateCall_MCX_IMS.ttcn:194: Step 41 Verdict: Pass
666 | 11:53:21.982 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
667 | 11:53:21.986 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
668 | 11:53:22.732 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.