ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 08:33:50.129 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 08:33:50.132 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 08:33:50.132 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 08:33:50.134 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 08:33:50.134 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 08:33:50.135 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:824: IMS UDP port 192.168.2.3:5060 configured
7 | 08:33:50.137 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:774: IMS TCP port 192.168.2.3:5060 configured!
8 | 08:33:50.138 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:795: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 08:33:50.139 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:806: IdM port 192.168.2.3:8080 configured!
10 | 08:33:50.141 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 08:33:51.342 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 08:33:51.344 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 08:33:53.518 |  | ←RRC BCCH SIB1 |  |  |
14 | 08:33:53.598 |  | ←RRC BCCH SIB1 |  |  |
15 | 08:33:53.673 |  | ←RRC BCCH SIB |  |  |
16 | 08:33:53.678 |  | ←RRC BCCH SIB1 |  |  |
17 | 08:33:53.693 |  | ←RRC BCCH SIB |  |  |
18 | 08:34:28.392 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 08:34:28.392 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 08:34:28.392 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 08:34:28.392 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 08:34:28.453 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 08:34:28.453 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 08:34:28.453 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 08:34:28.453 |  |  |  | →NAS EMM Attach request |  |
26 | 08:34:28.453 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 08:34:28.453 |  |  |  | NAS K-asme e4a093625282ea02434297b6223541dd... |  |
28 | 08:34:28.453 |  |  |  | NAS ← EMM Authentication request |  |
29 | 08:34:28.454 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 08:34:28.454 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 08:34:28.455 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 08:34:28.525 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 08:34:28.525 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 08:34:28.525 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 08:34:28.525 |  |  |  | →NAS EMM Authentication response |  |
36 | 08:34:28.525 |  |  |  | NAS UE auth OK |  |
37 | 08:34:28.525 |  |  |  | NAS K-nas-cip 00000000000000000000000000000... |  |
38 | 08:34:28.525 |  |  |  | NAS K-nas-int 00488e4e9adc76469ac7a69f9db95... |  |
39 | 08:34:28.525 |  |  |  | NAS ← EMM Security mode command |  |
40 | 08:34:28.526 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 08:34:28.526 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 08:34:28.527 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 08:34:28.565 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Security mode complete |  |  |  |
44 | 08:34:28.565 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 08:34:28.565 |  | [EMBEDDED NAS IN PREV RRC] EMM Security mode complete |  |  |
46 | 08:34:28.565 |  |  |  | →NAS EMM Security mode complete |  |
47 | 08:34:28.565 |  |  |  | NAS ← ESM ESM information request |  |
48 | 08:34:28.566 |  | [EMBEDDED NAS IN NEXT RRC] ESM ESM information request |  |  |
49 | 08:34:28.566 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 08:34:28.567 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer ESM information request |  |  |
51 | 08:34:28.613 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer ESM information response |  |  |  |
52 | 08:34:28.613 |  | →RRC DCCH UL Information Transfer |  |  |
53 | 08:34:28.613 |  | [EMBEDDED NAS IN PREV RRC] ESM ESM information response |  |  |
54 | 08:34:28.613 |  |  |  | →NAS ESM ESM information response |  |
55 | 08:34:28.613 |  |  |  | NAS K-enb e4ba8d2930554bcf189ad273b8d4aa755... |  |
56 | 08:34:28.613 |  |  |  | NAS ← EMM Attach accept |  |
57 | 08:34:28.614 |  | ←RRC DCCH Security Mode Command |  |  |
58 | 08:34:28.614 |  |  | RRC K-enb e4ba8d2930554bcf189ad273b8d4aa755... |  |  |
59 | 08:34:28.614 |  |  | RRC rrc-cip 4f497740cb1c0eb8a5262ad8407da0d... |  |  |
60 | 08:34:28.614 |  |  | RRC rrc-int b8ae870bb7abff4d5b6701f3457b0a3... |  |  |
61 | 08:34:28.614 |  |  | RRC up-cip cca9392db1840c08b81a8d20c2bcf427... |  |  |
62 | 08:34:28.614 |  |  | RRC up-int 7944448d68482e92a865e4ab30717542... |  |  |
63 | 08:34:28.615 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
64 | 08:34:28.645 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
65 | 08:34:28.645 |  | →RRC DCCH Security Mode Complete |  |  |
66 | 08:34:28.645 |  | ←RRC DCCH UE Capability Enquiry |  |  |
67 | 08:34:28.645 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
68 | 08:34:28.695 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
69 | 08:34:28.695 |  | →RRC DCCH UE Capability Information |  |  |
70 | 08:34:28.696 |  | [EMBEDDED NAS IN NEXT RRC] EMM Attach accept |  |  |
71 | 08:34:28.696 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
72 | 08:34:28.696 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration Attach accept Activate default EPS bearer context request (PDN ... |  |  |
73 | 08:34:28.725 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
74 | 08:34:28.725 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
75 | 08:34:28.765 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Attach complete Activate default EPS bearer context accept |  |  |  |
76 | 08:34:28.765 |  | →RRC DCCH UL Information Transfer |  |  |
77 | 08:34:28.765 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach complete |  |  |
78 | 08:34:28.765 |  |  |  | →NAS EMM Attach complete |  |
79 | 08:34:28.765 |  |  |  | NAS ← EMM EMM information |  |
80 | 08:34:28.766 |  | [EMBEDDED NAS IN NEXT RRC] EMM EMM information |  |  |
81 | 08:34:28.766 |  | ←RRC DCCH DL Information Transfer |  |  |
82 | 08:34:28.767 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer EMM information |  |  |
83 | 08:34:33.464 |  | ←RRC DCCH RRC Connection Release |  |  |
84 | 08:34:33.465 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
85 | 08:34:35.902 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
86 | 08:34:35.902 |  | →RRC CCCH RRC Connection Request |  |  |
87 | 08:34:35.902 |  | ←RRC CCCH RRC Connection Setup |  |  |
88 | 08:34:35.902 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
89 | 08:34:35.965 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
90 | 08:34:35.965 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
91 | 08:34:35.965 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
92 | 08:34:35.965 |  |  |  | →NAS EMM Service request |  |
93 | 08:34:35.965 |  |  |  | NAS K-enb d51270ac32d1d94d7056cfb30752a906f... |  |
94 | 08:34:35.966 |  | ←RRC DCCH Security Mode Command |  |  |
95 | 08:34:35.966 |  |  | RRC K-enb d51270ac32d1d94d7056cfb30752a906f... |  |  |
96 | 08:34:35.966 |  |  | RRC rrc-cip f2023a7ff5a02c63c2a412a92dd7f42... |  |  |
97 | 08:34:35.966 |  |  | RRC rrc-int 1af59b8bcebce6574ae9f99dea9b495... |  |  |
98 | 08:34:35.966 |  |  | RRC up-cip 3a8548f42d10381da88eeb6fd3d317ed... |  |  |
99 | 08:34:35.966 |  |  | RRC up-int ba9126436e715672a367350507dc3723... |  |  |
100 | 08:34:35.967 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
101 | 08:34:36.005 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
102 | 08:34:36.005 |  | →RRC DCCH Security Mode Complete |  |  |
103 | 08:34:36.005 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
104 | 08:34:36.005 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
105 | 08:34:36.045 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
106 | 08:34:36.045 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
107 | 08:35:47.485 | →enobeB PCAP frame→ TCP |  |  |  |
108 | 08:35:47.489 |  | ←enobeB PCAP frame← TCP |  |  |
109 | 08:35:47.525 | →enobeB PCAP frame→ TCP |  |  |  |
110 | 08:35:47.653 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
111 | 08:35:47.657 |  | ←enobeB PCAP frame← TCP |  |  |
112 | 08:35:47.662 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
113 | 08:35:47.685 | →enobeB PCAP frame→ TCP |  |  |  |
114 | 08:35:47.853 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
115 | 08:35:47.857 |  | ←enobeB PCAP frame← TCP |  |  |
116 | 08:35:47.858 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
117 | 08:35:47.860 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 16)
118 | 08:35:47.885 | →enobeB PCAP frame→ TCP |  |  |  |
119 | 08:35:47.973 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
120 | 08:35:47.977 |  | ←enobeB PCAP frame← TCP |  |  |
121 | 08:35:47.986 |  |  |  |  | →HTTP GET | HTTP-Proxy
122 | 08:35:47.993 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:307: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
123 | 08:35:48.011 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
124 | 08:35:48.011 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
125 | 08:35:48.045 | →enobeB PCAP frame→ TCP |  |  |  |
126 | 08:35:48.053 | →enobeB PCAP frame→ TCP |  |  |  |
127 | 08:35:50.365 | →enobeB PCAP frame→ TCP |  |  |  |
128 | 08:35:50.369 |  | ←enobeB PCAP frame← TCP |  |  |
129 | 08:35:50.405 | →enobeB PCAP frame→ TCP |  |  |  |
130 | 08:35:50.413 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
131 | 08:35:50.417 |  | ←enobeB PCAP frame← TCP |  |  |
132 | 08:35:50.422 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
133 | 08:35:50.445 | →enobeB PCAP frame→ TCP |  |  |  |
134 | 08:35:50.813 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
135 | 08:35:50.817 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
136 | 08:35:50.820 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
137 | 08:35:50.845 | →enobeB PCAP frame→ TCP |  |  |  |
138 | 08:35:50.853 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
139 | 08:35:50.857 |  | ←enobeB PCAP frame← TCP |  |  |
140 | 08:35:50.858 |  | ←enobeB PCAP frame← TCP |  |  |
141 | 08:35:50.860 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
142 | 08:35:50.860 |  |  |  |  | →HTTP GET | IDMS-Endpoint
143 | 08:35:50.863 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
144 | 08:35:50.867 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:526: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
145 | 08:35:50.868 |  |  |  |  | MMICmd: Please provide user credentials: username and password
146 | 08:35:50.925 | →enobeB PCAP frame→ TCP |  |  |  |
147 | 08:35:55.973 | →enobeB PCAP frame→ HTTPS: POST /idms/userauth HTTP/1.1 |  |  |  |
148 | 08:35:55.977 |  | ←enobeB PCAP frame← TCP |  |  |
149 | 08:35:55.982 |  |  |  |  | →HTTP POST | IDMS-Endpoint
150 | 08:35:55.994 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
151 | 08:35:55.996 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
152 | 08:35:55.998 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:531: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
153 | 08:35:56.005 | →enobeB PCAP frame→ TCP |  |  |  |
154 | 08:35:56.045 | →enobeB PCAP frame→ TCP |  |  |  |
155 | 08:35:56.049 |  | ←enobeB PCAP frame← TCP |  |  |
156 | 08:35:56.051 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:693: IdM port - Client closed the connection (id 18)
157 | 08:35:56.085 | →enobeB PCAP frame→ TCP |  |  |  |
158 | 08:35:56.405 | →enobeB PCAP frame→ TCP |  |  |  |
159 | 08:35:56.408 |  | ←enobeB PCAP frame← TCP |  |  |
160 | 08:35:56.445 | →enobeB PCAP frame→ TCP |  |  |  |
161 | 08:35:56.453 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
162 | 08:35:56.456 |  | ←enobeB PCAP frame← TCP |  |  |
163 | 08:35:56.459 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
164 | 08:35:56.485 | →enobeB PCAP frame→ TCP |  |  |  |
165 | 08:35:56.533 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
166 | 08:35:56.539 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
167 | 08:35:56.540 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
168 | 08:35:56.565 | →enobeB PCAP frame→ TCP |  |  |  |
169 | 08:35:56.613 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
170 | 08:35:56.619 |  | ←enobeB PCAP frame← TCP |  |  |
171 | 08:35:56.620 |  |  |  |  | →HTTP POST | IDMS-Endpoint
172 | 08:35:56.623 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
173 | 08:35:56.625 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
174 | 08:35:56.629 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:536: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
175 | 08:35:56.685 | →enobeB PCAP frame→ TCP |  |  |  |
176 | 08:35:56.965 | →enobeB PCAP frame→ TCP |  |  |  |
177 | 08:35:56.968 |  | ←enobeB PCAP frame← TCP |  |  |
178 | 08:35:57.005 | →enobeB PCAP frame→ TCP |  |  |  |
179 | 08:35:57.013 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
180 | 08:35:57.016 |  | ←enobeB PCAP frame← TCP |  |  |
181 | 08:35:57.085 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
182 | 08:35:57.125 | →enobeB PCAP frame→ TCP |  |  |  |
183 | 08:35:57.133 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
184 | 08:35:57.136 |  | ←enobeB PCAP frame← TCP |  |  |
185 | 08:35:57.137 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
186 | 08:35:57.140 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 19)
187 | 08:35:57.173 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
188 | 08:35:57.177 |  | ←enobeB PCAP frame← TCP |  |  |
189 | 08:35:57.180 |  |  |  |  | →HTTP POST | HTTP-Proxy
190 | 08:35:57.204 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
191 | 08:35:57.204 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:554: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
192 | 08:35:57.205 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
193 | 08:35:57.245 | →enobeB PCAP frame→ TCP |  |  |  |
194 | 08:35:57.285 | →enobeB PCAP frame→ TCP |  |  |  |
195 | 08:35:57.289 |  | ←enobeB PCAP frame← TCP |  |  |
196 | 08:35:57.325 | →enobeB PCAP frame→ TCP |  |  |  |
197 | 08:35:57.333 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
198 | 08:35:57.337 |  | ←enobeB PCAP frame← TCP |  |  |
199 | 08:35:57.340 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
200 | 08:35:57.365 | →enobeB PCAP frame→ TCP |  |  |  |
201 | 08:35:57.373 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
202 | 08:35:57.377 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
203 | 08:35:57.381 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 20)
204 | 08:35:57.413 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
205 | 08:35:57.417 |  | ←enobeB PCAP frame← TCP |  |  |
206 | 08:35:57.422 |  |  |  |  | →HTTP POST | HTTP-Proxy
207 | 08:35:57.470 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
208 | 08:35:57.471 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
209 | 08:35:57.472 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:558: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
210 | 08:35:57.485 | →enobeB PCAP frame→ TCP |  |  |  |
211 | 08:35:57.613 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
212 | 08:35:57.622 |  |  |  |  | →SIP REGISTER | P-CSCF
213 | 08:35:57.704 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:833: IMS UDP_s port 192.168.2.3:5062 configured
214 | 08:35:57.733 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:784: IMS TCP_s port 192.168.2.3:5062 configured!
215 | 08:35:57.736 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:842: IMS UDP_c port 192.168.2.3:5061 configured
216 | 08:35:57.739 |  | ←enobeB PCAP frame← SIP -cleartext-: SIP/2.0 401 Unauthorized |  |  |
217 | 08:35:57.741 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
218 | 08:35:58.453 | →enobeB PCAP frame→ SIP over IPSEC: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
219 | 08:35:58.463 |  |  |  |  | →SIP REGISTER | P-CSCF
220 | 08:35:58.472 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
221 | 08:35:58.475 |  |  |  |  | ←SIP 200 OK | P-CSCF
222 | 08:35:58.808 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
223 | 08:35:58.863 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
224 | 08:35:58.865 |  |  |  |  | ←SIP 200 OK | P-CSCF
225 | 08:35:58.866 |  |  |  |  | MIKEY | Media-Server
226 | 08:35:59.071 |  |  |  |  | XML→ | Media-Server
227 | 08:35:59.073 |  |  |  |  | XML→ | Media-Server
228 | 08:35:59.076 |  |  |  |  | ←XML | Media-Server
229 | 08:35:59.078 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:39322;transp... |  |  |
230 | 08:35:59.080 |  |  |  |  | ←SIP NOTIFY | P-CSCF
231 | 08:35:59.140 |  |  |  |  | →SIP 200 OK | P-CSCF
232 | 08:35:59.368 |  | ←enobeB PCAP frame← TCP |  |  |
233 | 08:35:59.405 | →enobeB PCAP frame→ TCP |  |  |  |
234 | 08:35:59.413 | →enobeB PCAP frame→ TLS: Mix Info DNS |  |  |  |
235 | 08:35:59.416 |  | ←enobeB PCAP frame← TCP |  |  |
236 | 08:35:59.418 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
237 | 08:35:59.445 | →enobeB PCAP frame→ TCP |  |  |  |
238 | 08:35:59.493 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
239 | 08:35:59.497 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
240 | 08:35:59.500 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
241 | 08:35:59.525 | →enobeB PCAP frame→ TCP |  |  |  |
242 | 08:35:59.533 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
243 | 08:35:59.537 |  | ←enobeB PCAP frame← TCP |  |  |
244 | 08:35:59.540 |  |  |  |  | →HTTP GET | HTTP-Proxy
245 | 08:35:59.548 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:691: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcpttue-configuration.xml
246 | 08:35:59.554 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
247 | 08:35:59.556 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
248 | 08:35:59.645 | →enobeB PCAP frame→ TCP |  |  |  |
249 | 08:35:59.653 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
250 | 08:35:59.657 |  | ←enobeB PCAP frame← TCP |  |  |
251 | 08:35:59.659 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
252 | 08:35:59.685 | →enobeB PCAP frame→ TCP |  |  |  |
253 | 08:35:59.765 | →enobeB PCAP frame→ TCP |  |  |  |
254 | 08:35:59.769 |  | ←enobeB PCAP frame← TCP |  |  |
255 | 08:35:59.805 | →enobeB PCAP frame→ TCP |  |  |  |
256 | 08:35:59.813 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
257 | 08:35:59.817 |  | ←enobeB PCAP frame← TCP |  |  |
258 | 08:35:59.821 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
259 | 08:35:59.845 | →enobeB PCAP frame→ TCP |  |  |  |
260 | 08:35:59.893 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
261 | 08:35:59.897 |  | ←enobeB PCAP frame← TCP |  |  |
262 | 08:35:59.898 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
263 | 08:35:59.901 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
264 | 08:35:59.925 | →enobeB PCAP frame→ TCP |  |  |  |
265 | 08:35:59.933 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
266 | 08:35:59.936 |  | ←enobeB PCAP frame← TCP |  |  |
267 | 08:35:59.940 |  |  |  |  | →HTTP GET | HTTP-Proxy
268 | 08:35:59.951 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:696: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcpttuser-profile-49.xml
269 | 08:35:59.981 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
270 | 08:35:59.981 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
271 | 08:35:59.982 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
272 | 08:36:00.005 | →enobeB PCAP frame→ TCP |  |  |  |
273 | 08:36:00.021 | →enobeB PCAP frame→ TCP |  |  |  |
274 | 08:36:00.045 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
275 | 08:36:00.048 |  | ←enobeB PCAP frame← TCP |  |  |
276 | 08:36:00.051 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
277 | 08:36:00.053 | →enobeB PCAP frame→ TCP |  |  |  |
278 | 08:36:00.057 |  | ←enobeB PCAP frame← TCP |  |  |
279 | 08:36:00.085 | →enobeB PCAP frame→ TCP |  |  |  |
280 | 08:36:00.723 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
281 | 08:36:00.734 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
282 | 08:36:00.736 |  |  |  |  | ←SIP 200 OK | P-CSCF
283 | 08:36:00.736 |  |  |  |  | MIKEY | Media-Server
284 | 08:36:00.849 |  | ←enobeB PCAP frame← TCP |  |  |
285 | 08:36:00.929 |  |  |  |  | XML→ | Media-Server
286 | 08:36:00.930 |  |  |  |  | XML→ | Media-Server
287 | 08:36:00.933 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
288 | 08:36:00.933 |  |  |  |  | ←XML | Media-Server
289 | 08:36:00.936 |  | ←enobeB PCAP frame← TCP |  |  |
290 | 08:36:00.937 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
291 | 08:36:00.965 | →enobeB PCAP frame→ TCP |  |  |  |
292 | 08:36:01.053 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
293 | 08:36:01.056 |  | ←enobeB PCAP frame← TCP |  |  |
294 | 08:36:01.057 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
295 | 08:36:01.060 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
296 | 08:36:01.062 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:39322;transp... |  |  |
297 | 08:36:01.063 |  |  |  |  | ←SIP NOTIFY | P-CSCF
298 | 08:36:01.085 | →enobeB PCAP frame→ TCP |  |  |  |
299 | 08:36:01.105 |  | ←enobeB PCAP frame← TCP |  |  |
300 | 08:36:01.109 |  |  |  |  | →HTTP GET | HTTP-Proxy
301 | 08:36:01.111 |  |  |  |  | →SIP 200 OK | P-CSCF
302 | 08:36:01.118 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:701: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
303 | 08:36:01.135 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
304 | 08:36:01.137 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
305 | 08:36:01.185 |  | ←enobeB PCAP frame← TCP |  |  |
306 | 08:36:01.188 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
307 | 08:36:01.189 | →enobeB PCAP frame→ TCP |  |  |  |
308 | 08:36:01.192 |  | ←enobeB PCAP frame← TCP |  |  |
309 | 08:36:01.205 | →enobeB PCAP frame→ TCP |  |  |  |
310 | 08:36:01.245 | →enobeB PCAP frame→ TCP |  |  |  |
311 | 08:36:01.249 |  | ←enobeB PCAP frame← TCP |  |  |
312 | 08:36:01.285 | →enobeB PCAP frame→ TCP |  |  |  |
313 | 08:36:01.293 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
314 | 08:36:01.297 |  | ←enobeB PCAP frame← TCP |  |  |
315 | 08:36:01.300 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
316 | 08:36:01.325 | →enobeB PCAP frame→ TCP |  |  |  |
317 | 08:36:01.413 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
318 | 08:36:01.417 |  | ←enobeB PCAP frame← TCP |  |  |
319 | 08:36:01.418 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
320 | 08:36:01.421 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
321 | 08:36:01.445 | →enobeB PCAP frame→ TCP |  |  |  |
322 | 08:36:01.465 |  | ←enobeB PCAP frame← TCP |  |  |
323 | 08:36:01.468 |  |  |  |  | →HTTP GET | HTTP-Proxy
324 | 08:36:01.475 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:706: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at http://xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
325 | 08:36:01.483 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
326 | 08:36:01.484 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
327 | 08:36:01.485 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
328 | 08:36:01.533 | →enobeB PCAP frame→ TCP |  |  |  |
329 | 08:36:01.537 |  | ←enobeB PCAP frame← TCP |  |  |
330 | 08:36:01.540 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
331 | 08:36:01.565 | →enobeB PCAP frame→ TCP |  |  |  |
332 | 08:36:01.772 |  |  |  |  | →SIP PUBLISH | P-CSCF
333 | 08:36:01.806 |  |  |  |  | MIKEY | Media-Server
334 | 08:36:01.839 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
335 | 08:36:02.008 |  |  |  |  | XML→ | Media-Server
336 | 08:36:02.009 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
337 | 08:36:02.011 |  |  |  |  | ←SIP 200 OK | P-CSCF
338 | 08:36:02.012 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
339 | 08:36:02.015 |  |  |  |  | ←SIP 200 OK | P-CSCF
340 | 08:36:02.015 |  |  |  |  | MIKEY | Media-Server
341 | 08:36:02.218 |  |  |  |  | XML→ | Media-Server
342 | 08:36:02.219 |  |  |  |  | XML→ | Media-Server
343 | 08:36:02.254 |  |  |  |  | MIKEY | Media-Server
344 | 08:36:02.254 |  |  |  |  | ←XML | Media-Server
345 | 08:36:02.257 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:39322;transp... |  |  |
346 | 08:36:02.259 |  |  |  |  | ←SIP NOTIFY | P-CSCF
347 | 08:36:02.299 |  |  |  |  | →SIP 200 OK | P-CSCF
348 | 08:36:02.302 |  |  |  |  | ←XML | Media-Server
349 | 08:36:02.308 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
350 | 08:36:02.310 |  |  |  |  | ←SIP MESSAGE | P-CSCF
351 | 08:36:03.140 |  |  |  |  | →SIP 200 OK | P-CSCF
352 | 08:36:05.150 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
353 | 08:36:05.228 |  | ←RRC DCCH RRC Connection Release |  |  |
354 | 08:36:05.229 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
355 | 08:36:05.243 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
356 | 08:36:05.244 |  |  |  |  | Info: MCPTT_ClientConfiguration_MCX_IMS.ttcn:460: Test-Body Step 1 - 2
357 | 08:36:05.247 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
358 | 08:36:05.247 |  |  |  |  | MMICmd: Make the MCPTT User request the creation of a pre-established session
359 | 08:36:12.142 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
360 | 08:36:12.142 |  | →RRC CCCH RRC Connection Request |  |  |
361 | 08:36:12.142 |  | ←RRC CCCH RRC Connection Setup |  |  |
362 | 08:36:12.142 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
363 | 08:36:12.205 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
364 | 08:36:12.205 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
365 | 08:36:12.205 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
366 | 08:36:12.205 |  |  |  | →NAS EMM Service request |  |
367 | 08:36:12.205 |  |  |  | NAS K-enb 9db9444162d6edd86acbaf69d1bf2ff68... |  |
368 | 08:36:12.206 |  | ←RRC DCCH Security Mode Command |  |  |
369 | 08:36:12.206 |  |  | RRC K-enb 9db9444162d6edd86acbaf69d1bf2ff68... |  |  |
370 | 08:36:12.206 |  |  | RRC rrc-cip c3751d37b63c497abfb340f40d48e0b... |  |  |
371 | 08:36:12.206 |  |  | RRC rrc-int df04f7659504aedae13b75babadce2c... |  |  |
372 | 08:36:12.206 |  |  | RRC up-cip 07bc5f99209e44666bee2ae5caff21fa... |  |  |
373 | 08:36:12.206 |  |  | RRC up-int 2b83a9b4cd0af881db9f7e60e7b52160... |  |  |
374 | 08:36:12.207 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
375 | 08:36:12.245 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
376 | 08:36:12.245 |  | →RRC DCCH Security Mode Complete |  |  |
377 | 08:36:12.245 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
378 | 08:36:12.245 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
379 | 08:36:12.285 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
380 | 08:36:12.285 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
381 | 08:36:12.293 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
382 | 08:36:12.301 |  |  |  |  | →SIP INVITE | P-CSCF
383 | 08:36:12.386 |  |  |  |  | ←SIP 100 Trying | P-CSCF
384 | 08:36:12.388 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
385 | 08:36:12.394 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
386 | 08:36:12.399 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
387 | 08:36:12.399 |  |  |  |  | ←SIP 200 OK | P-CSCF
388 | 08:36:13.016 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
389 | 08:36:13.017 |  | [EMBEDDED NAS IN NEXT RRC] ESM Activate dedicated EPS bearer conte... |  |  |
390 | 08:36:13.017 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
391 | 08:36:13.018 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration Activate dedicated EPS bearer context request |  |  |
392 | 08:36:13.045 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Activate dedicated EPS bearer context accept |  |  |  |
393 | 08:36:13.045 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
394 | 08:36:13.045 |  | →RRC DCCH UL Information Transfer |  |  |
395 | 08:36:13.045 |  | [EMBEDDED NAS IN PREV RRC] ESM Activate dedicated EPS bearer conte... |  |  |
396 | 08:36:13.045 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
397 | 08:36:13.156 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
398 | 08:36:13.413 | →enobeB PCAP frame→ SIP over IPSEC: ACK sip:sessionB@cf.mcstaasting.com SIP/2.0 |  |  |  |
399 | 08:36:13.422 |  |  |  |  | →SIP ACK | P-CSCF
400 | 08:36:15.433 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
401 | 08:36:15.474 |  | ←RRC DCCH RRC Connection Release |  |  |
402 | 08:36:15.475 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
403 | 08:36:15.505 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
404 | 08:36:15.506 |  |  |  |  | Verdict PASS: MCPTT_ClientConfiguration_MCX_IMS.ttcn:464: Step 2 Verdict: Pass
405 | 08:36:15.507 |  |  |  |  | Info: MCPTT_ClientConfiguration_MCX_IMS.ttcn:468: Test-Body Step 4
406 | 08:36:15.507 |  |  |  |  | Info: MCPTT_ClientConfiguration_MCX_IMS.ttcn:493: Test-Body Step 6Aa1
407 | 08:36:15.508 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
408 | 08:36:15.510 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
409 | 08:36:15.511 |  |  |  |  | Info: MCPTT_ClientConfiguration_MCX_IMS.ttcn:497: Test-Body Steps 7 - 8
410 | 08:36:15.525 |  |  |  |  | ←SIP UPDATE | P-CSCF
411 | 08:36:15.652 |  | ←enobeB PCAP frame← LTE RRC PCCH Paging (1 PagingRecord) |  |  |
412 | 08:36:15.652 |  | ←RRC PCCH Paging |  |  |
413 | 08:36:15.682 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
414 | 08:36:15.682 |  | →RRC CCCH RRC Connection Request |  |  |
415 | 08:36:15.682 |  | ←RRC CCCH RRC Connection Setup |  |  |
416 | 08:36:15.682 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
417 | 08:36:15.725 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
418 | 08:36:15.725 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
419 | 08:36:15.725 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
420 | 08:36:15.725 |  |  |  | →NAS EMM Service request |  |
421 | 08:36:15.725 |  |  |  | NAS K-enb 4d598393f8dbbf02e5bcbb0410c4c6469... |  |
422 | 08:36:15.726 |  | ←RRC DCCH Security Mode Command |  |  |
423 | 08:36:15.726 |  |  | RRC K-enb 4d598393f8dbbf02e5bcbb0410c4c6469... |  |  |
424 | 08:36:15.726 |  |  | RRC rrc-cip a733407e7ab969a350130059ab227ba... |  |  |
425 | 08:36:15.726 |  |  | RRC rrc-int 8cb3d00154b1be4e5b80300e6bc74d8... |  |  |
426 | 08:36:15.726 |  |  | RRC up-cip c0d7dfbcae7df8126e28a67fe23a0d62... |  |  |
427 | 08:36:15.726 |  |  | RRC up-int eabc1930364b6b4f55d76d7123508c2e... |  |  |
428 | 08:36:15.727 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
429 | 08:36:15.765 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
430 | 08:36:15.765 |  | →RRC DCCH Security Mode Complete |  |  |
431 | 08:36:15.765 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
432 | 08:36:15.765 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
433 | 08:36:15.805 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
434 | 08:36:15.805 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
435 | 08:36:15.807 |  | ←enobeB PCAP frame← SIP over IPSEC: UPDATE sip:PublicUserId-A@192.168.3.2:39322;transp... |  |  |
436 | 08:36:15.853 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
437 | 08:36:15.863 |  |  |  |  | →SIP 200 OK | P-CSCF
438 | 08:36:15.880 |  |  |  |  | Verdict PASS: MCPTT_ClientConfiguration_MCX_IMS.ttcn:504: Step 8 Verdict: Pass
439 | 08:36:15.881 |  |  |  |  | Info: MCPTT_ClientConfiguration_MCX_IMS.ttcn:509: Test-Body Step 9
440 | 08:36:15.885 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
441 | 08:36:15.889 |  | ←enobeB PCAP frame← SRTP frame: |  |  |
442 | 08:36:15.893 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
443 | 08:36:15.893 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:754: SRTP config: Master Key: A34D37285D090E36106725E70027A45A, Master Salt: A2DD876EE13DE0DE9B1BFF12, MKI: 2BFB7EE1
444 | 08:36:15.893 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
445 | 08:36:15.911 |  | ←enobeB PCAP frame← SIP over IPSEC: INVITE sip:PublicUserId-A@192.168.3.2:39322;transp... |  |  |
446 | 08:36:15.912 |  |  |  |  | ←SIP INVITE | P-CSCF
447 | 08:36:15.933 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 100 Trying SRTP frame: |  |  |  |
448 | 08:36:15.940 |  |  |  |  | →SIP 100 Trying | P-CSCF
449 | 08:36:15.973 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK SRTP frame: |  |  |  |
450 | 08:36:15.983 |  |  |  |  | →SIP 200 OK | P-CSCF
451 | 08:36:16.005 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
452 | 08:36:16.005 |  |  |  |  | Verdict PASS: MCPTT_ClientConfiguration_MCX_IMS.ttcn:513: Step 9 Verdict: Pass
453 | 08:36:16.006 |  |  |  |  | Info: MCPTT_ClientConfiguration_MCX_IMS.ttcn:517: Test-Body Step 11 - 12
454 | 08:36:16.009 |  | ←enobeB PCAP frame← SIP over IPSEC: ACK sip:PublicUserId-A@192.168.3.2:39322;transport... |  |  |
455 | 08:36:16.011 |  |  |  |  | ←SIP ACK | P-CSCF
456 | 08:36:16.013 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
457 | 08:36:16.045 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
458 | 08:36:16.053 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
459 | 08:36:16.085 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
460 | 08:36:16.093 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
461 | 08:36:16.190 |  |  |  |  | MMICmd: Release call (hang up the call)
462 | 08:36:18.423 |  |  |  |  | →SIP BYE | P-CSCF
463 | 08:36:18.441 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
464 | 08:36:18.443 |  |  |  |  | ←SIP 200 OK | P-CSCF
465 | 08:36:19.005 | →enobeB PCAP frame→ |  |  |  |
466 | 08:36:20.441 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
467 | 08:36:20.454 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
468 | 08:36:20.455 |  | [EMBEDDED NAS IN NEXT RRC] ESM Deactivate EPS bearer context reque... |  |  |
469 | 08:36:20.455 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
470 | 08:36:20.456 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration Deactivate EPS bearer context request (Regular de... |  |  |
471 | 08:36:20.485 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Deactivate EPS bearer context accept |  |  |  |
472 | 08:36:20.485 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
473 | 08:36:20.485 |  | →RRC DCCH UL Information Transfer |  |  |
474 | 08:36:20.485 |  | [EMBEDDED NAS IN PREV RRC] ESM Deactivate EPS bearer context accep... |  |  |
475 | 08:36:20.485 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
476 | 08:36:20.581 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
477 | 08:36:20.582 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
478 | 08:36:20.611 |  | ←RRC DCCH RRC Connection Release |  |  |
479 | 08:36:20.612 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
480 | 08:36:20.637 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
481 | 08:36:20.639 |  |  |  |  | Verdict PASS: MCPTT_ClientConfiguration_MCX_IMS.ttcn:520: Step 11 Verdict: Pass
482 | 08:36:20.639 |  |  |  |  | Info: MCPTT_ClientConfiguration_MCX_IMS.ttcn:524: Test-Body Step 14 - 15
483 | 08:36:20.642 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
484 | 08:36:20.643 |  |  |  |  | MMICmd: Make the MCPTT User request the creation of a pre-established session
485 | 08:36:26.302 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
486 | 08:36:26.302 |  | →RRC CCCH RRC Connection Request |  |  |
487 | 08:36:26.302 |  | ←RRC CCCH RRC Connection Setup |  |  |
488 | 08:36:26.302 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
489 | 08:36:26.325 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
490 | 08:36:26.325 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
491 | 08:36:26.325 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
492 | 08:36:26.325 |  |  |  | →NAS EMM Service request |  |
493 | 08:36:26.325 |  |  |  | NAS K-enb 34f6bf985512429b1710782a78489f49e... |  |
494 | 08:36:26.326 |  |  | RRC K-enb 34f6bf985512429b1710782a78489f49e... |  |  |
495 | 08:36:26.327 |  |  | RRC rrc-cip 236b4a3779d08ea4062f466e4a77992... |  |  |
496 | 08:36:26.327 |  |  | RRC rrc-int fd90f41305334b4594d0bddd6ea6350... |  |  |
497 | 08:36:26.327 |  |  | RRC up-cip 3e914ef4bb29806f30363919b5030473... |  |  |
498 | 08:36:26.327 |  |  | RRC up-int 2a12e9cdd7f0e29a565d5fdba35f25cc... |  |  |
499 | 08:36:26.327 |  | ←RRC DCCH Security Mode Command |  |  |
500 | 08:36:26.327 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
501 | 08:36:26.365 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
502 | 08:36:26.365 |  | →RRC DCCH Security Mode Complete |  |  |
503 | 08:36:26.365 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
504 | 08:36:26.365 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
505 | 08:36:26.405 | →enobeB PCAP frame→ RLC-LTE RRCConnectionReconfigurationComplete |  |  |  |
506 | 08:36:26.405 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
507 | 08:36:26.413 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
508 | 08:36:26.423 |  |  |  |  | →SIP INVITE | P-CSCF
509 | 08:36:26.437 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
510 | 08:36:26.439 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
511 | 08:36:26.440 |  |  |  |  | ←SIP 100 Trying | P-CSCF
512 | 08:36:26.442 |  |  |  |  | ←SIP 200 OK | P-CSCF
513 | 08:36:26.443 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
514 | 08:36:27.053 | →enobeB PCAP frame→ SIP over IPSEC: ACK sip:sessionB@cf.mcstaasting.com SIP/2.0 |  |  |  |
515 | 08:36:27.062 |  |  |  |  | →SIP ACK | P-CSCF
516 | 08:36:27.081 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
517 | 08:36:27.081 |  | [EMBEDDED NAS IN NEXT RRC] ESM Activate dedicated EPS bearer conte... |  |  |
518 | 08:36:27.081 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
519 | 08:36:27.082 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration Activate dedicated EPS bearer context request |  |  |
520 | 08:36:27.125 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Activate dedicated EPS bearer context accept |  |  |  |
521 | 08:36:27.125 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
522 | 08:36:27.125 |  | →RRC DCCH UL Information Transfer |  |  |
523 | 08:36:27.125 |  | [EMBEDDED NAS IN PREV RRC] ESM Activate dedicated EPS bearer conte... |  |  |
524 | 08:36:27.125 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
525 | 08:36:27.219 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
526 | 08:36:29.133 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
527 | 08:36:29.173 |  | ←RRC DCCH RRC Connection Release |  |  |
528 | 08:36:29.174 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
529 | 08:36:29.198 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
530 | 08:36:29.199 |  |  |  |  | Verdict PASS: MCPTT_ClientConfiguration_MCX_IMS.ttcn:526: Step 15 Verdict: Pass
531 | 08:36:29.200 |  |  |  |  | Info: MCPTT_ClientConfiguration_MCX_IMS.ttcn:530: Test-Body Step 17
532 | 08:36:29.207 |  |  |  |  | ←SIP BYE | P-CSCF
533 | 08:36:29.732 |  | ←enobeB PCAP frame← LTE RRC PCCH Paging (1 PagingRecord) |  |  |
534 | 08:36:29.732 |  | ←RRC PCCH Paging |  |  |
535 | 08:36:29.762 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
536 | 08:36:29.762 |  | →RRC CCCH RRC Connection Request |  |  |
537 | 08:36:29.762 |  | ←RRC CCCH RRC Connection Setup |  |  |
538 | 08:36:29.762 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
539 | 08:36:29.805 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
540 | 08:36:29.805 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
541 | 08:36:29.805 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
542 | 08:36:29.805 |  |  |  | →NAS EMM Service request |  |
543 | 08:36:29.805 |  |  |  | NAS K-enb fe23ae365f134175775822ef8d5689cde... |  |
544 | 08:36:29.806 |  | ←RRC DCCH Security Mode Command |  |  |
545 | 08:36:29.806 |  |  | RRC K-enb fe23ae365f134175775822ef8d5689cde... |  |  |
546 | 08:36:29.806 |  |  | RRC rrc-cip 381019ab9d3967e7635b37295f5c80a... |  |  |
547 | 08:36:29.806 |  |  | RRC rrc-int dff827f41ccee5c2a8dfe195ec02195... |  |  |
548 | 08:36:29.806 |  |  | RRC up-cip 65ac95a99f70579668ad53ed59abdb62... |  |  |
549 | 08:36:29.806 |  |  | RRC up-int 9aa53fc8b2cdfd88f4aee088b818a01f... |  |  |
550 | 08:36:29.807 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
551 | 08:36:29.845 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
552 | 08:36:29.845 |  | →RRC DCCH Security Mode Complete |  |  |
553 | 08:36:29.845 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
554 | 08:36:29.845 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
555 | 08:36:29.885 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
556 | 08:36:29.885 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
557 | 08:36:29.887 |  | ←enobeB PCAP frame← SIP over IPSEC: BYE sip:PublicUserId-A@192.168.3.2:39322;transport... |  |  |
558 | 08:36:29.933 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
559 | 08:36:29.941 |  |  |  |  | →SIP 200 OK | P-CSCF
560 | 08:36:30.285 | →enobeB PCAP frame→ |  |  |  |
561 | 08:36:31.950 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
562 | 08:36:31.950 |  | [EMBEDDED NAS IN NEXT RRC] ESM Deactivate EPS bearer context reque... |  |  |
563 | 08:36:31.950 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
564 | 08:36:31.951 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration Deactivate EPS bearer context request (Regular de... |  |  |
565 | 08:36:31.951 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
566 | 08:36:32.005 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Deactivate EPS bearer context accept |  |  |  |
567 | 08:36:32.005 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
568 | 08:36:32.005 |  | →RRC DCCH UL Information Transfer |  |  |
569 | 08:36:32.005 |  | [EMBEDDED NAS IN PREV RRC] ESM Deactivate EPS bearer context accep... |  |  |
570 | 08:36:32.005 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
571 | 08:36:32.081 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
572 | 08:36:32.082 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
573 | 08:36:32.119 |  | ←RRC DCCH RRC Connection Release |  |  |
574 | 08:36:32.120 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
575 | 08:36:32.144 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
576 | 08:36:32.145 |  |  |  |  | Verdict PASS: MCPTT_ClientConfiguration_MCX_IMS.ttcn:532: Step 17 Verdict: Pass
577 | 08:36:32.147 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
578 | 08:36:32.149 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
579 | 08:36:32.897 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.