ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 09:14:13.347 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 09:14:13.349 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 09:14:13.350 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 09:14:13.352 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 09:14:13.353 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 09:14:13.354 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:824: IMS UDP port 192.168.2.3:5060 configured
7 | 09:14:13.357 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:774: IMS TCP port 192.168.2.3:5060 configured!
8 | 09:14:13.360 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:795: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 09:14:13.361 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:806: IdM port 192.168.2.3:8080 configured!
10 | 09:14:13.364 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 09:14:14.565 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 09:14:14.567 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 09:14:16.753 |  | ←RRC BCCH SIB |  |  |
14 | 09:14:16.798 |  | ←RRC BCCH SIB1 |  |  |
15 | 09:14:16.873 |  | ←RRC BCCH SIB |  |  |
16 | 09:14:16.878 |  | ←RRC BCCH SIB1 |  |  |
17 | 09:14:16.958 |  | ←RRC BCCH SIB1 |  |  |
18 | 09:15:26.202 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 09:15:26.202 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 09:15:26.202 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 09:15:26.202 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 09:15:26.253 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 09:15:26.253 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 09:15:26.253 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 09:15:26.253 |  |  |  | →NAS EMM Attach request |  |
26 | 09:15:26.253 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 09:15:26.253 |  |  |  | NAS K-asme 7d43cda15e5d140e1b936aeec37a07fb... |  |
28 | 09:15:26.253 |  |  |  | NAS ← EMM Authentication request |  |
29 | 09:15:26.254 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 09:15:26.254 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 09:15:26.255 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 09:15:26.325 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 09:15:26.325 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 09:15:26.325 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 09:15:26.325 |  |  |  | →NAS EMM Authentication response |  |
36 | 09:15:26.325 |  |  |  | NAS UE auth OK |  |
37 | 09:15:26.325 |  |  |  | NAS K-nas-cip 00000000000000000000000000000... |  |
38 | 09:15:26.325 |  |  |  | NAS K-nas-int 9337f92abef6a1dfb1f048eee820d... |  |
39 | 09:15:26.325 |  |  |  | NAS ← EMM Security mode command |  |
40 | 09:15:26.326 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 09:15:26.326 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 09:15:26.327 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 09:15:26.365 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Security mode complete |  |  |  |
44 | 09:15:26.365 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 09:15:26.365 |  | [EMBEDDED NAS IN PREV RRC] EMM Security mode complete |  |  |
46 | 09:15:26.365 |  |  |  | →NAS EMM Security mode complete |  |
47 | 09:15:26.365 |  |  |  | NAS ← ESM ESM information request |  |
48 | 09:15:26.366 |  | [EMBEDDED NAS IN NEXT RRC] ESM ESM information request |  |  |
49 | 09:15:26.366 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 09:15:26.367 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer ESM information request |  |  |
51 | 09:15:26.413 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer ESM information response |  |  |  |
52 | 09:15:26.413 |  | →RRC DCCH UL Information Transfer |  |  |
53 | 09:15:26.413 |  | [EMBEDDED NAS IN PREV RRC] ESM ESM information response |  |  |
54 | 09:15:26.413 |  |  |  | →NAS ESM ESM information response |  |
55 | 09:15:26.413 |  |  |  | NAS K-enb 50c741cd50d02bcf0905d411a97ea0268... |  |
56 | 09:15:26.413 |  |  |  | NAS ← EMM Attach accept |  |
57 | 09:15:26.414 |  | ←RRC DCCH Security Mode Command |  |  |
58 | 09:15:26.414 |  |  | RRC K-enb 50c741cd50d02bcf0905d411a97ea0268... |  |  |
59 | 09:15:26.414 |  |  | RRC rrc-cip ad871773d4ccb68312788f296108fa3... |  |  |
60 | 09:15:26.414 |  |  | RRC rrc-int 7e3c4e7eccb373b1d9224c01dabfb0c... |  |  |
61 | 09:15:26.414 |  |  | RRC up-cip 8f6b6a279079338fbc84486a2384b5ee... |  |  |
62 | 09:15:26.414 |  |  | RRC up-int 1552d2159c36e08839ef42e9949bc362... |  |  |
63 | 09:15:26.415 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
64 | 09:15:26.445 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
65 | 09:15:26.445 |  | →RRC DCCH Security Mode Complete |  |  |
66 | 09:15:26.445 |  | ←RRC DCCH UE Capability Enquiry |  |  |
67 | 09:15:26.445 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
68 | 09:15:26.495 | →enobeB PCAP frame→ LTE RRC UL_DCCH UECapabilityInformation |  |  |  |
69 | 09:15:26.495 |  | →RRC DCCH UE Capability Information |  |  |
70 | 09:15:26.495 |  | [EMBEDDED NAS IN NEXT RRC] EMM Attach accept |  |  |
71 | 09:15:26.495 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
72 | 09:15:26.495 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration Attach accept Activate default EPS bearer context request (PDN ... |  |  |
73 | 09:15:26.525 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
74 | 09:15:26.525 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
75 | 09:15:26.565 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Attach complete Activate default EPS bearer context accept |  |  |  |
76 | 09:15:26.565 |  | →RRC DCCH UL Information Transfer |  |  |
77 | 09:15:26.565 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach complete |  |  |
78 | 09:15:26.565 |  |  |  | →NAS EMM Attach complete |  |
79 | 09:15:26.565 |  |  |  | NAS ← EMM EMM information |  |
80 | 09:15:26.566 |  | [EMBEDDED NAS IN NEXT RRC] EMM EMM information |  |  |
81 | 09:15:26.566 |  | ←RRC DCCH DL Information Transfer |  |  |
82 | 09:15:26.567 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer EMM information |  |  |
83 | 09:15:31.857 |  | ←RRC DCCH RRC Connection Release |  |  |
84 | 09:15:31.858 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
85 | 09:15:32.022 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
86 | 09:15:32.022 |  | →RRC CCCH RRC Connection Request |  |  |
87 | 09:15:32.022 |  | ←RRC CCCH RRC Connection Setup |  |  |
88 | 09:15:32.022 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
89 | 09:15:32.045 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
90 | 09:15:32.045 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
91 | 09:15:32.045 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
92 | 09:15:32.045 |  |  |  | →NAS EMM Service request |  |
93 | 09:15:32.045 |  |  |  | NAS K-enb d3a07b37d6e60728f208ec1933253ac63... |  |
94 | 09:15:32.046 |  | ←RRC DCCH Security Mode Command |  |  |
95 | 09:15:32.046 |  |  | RRC K-enb d3a07b37d6e60728f208ec1933253ac63... |  |  |
96 | 09:15:32.046 |  |  | RRC rrc-cip 2a64832d7f8ef7a98a6f2e826045446... |  |  |
97 | 09:15:32.046 |  |  | RRC rrc-int 62616785b464b2bf41541d1b98ffcbf... |  |  |
98 | 09:15:32.046 |  |  | RRC up-cip f248c97edcb219a68c085a261c38d9da... |  |  |
99 | 09:15:32.046 |  |  | RRC up-int 8f3df81ff95c8988e41b833e3ddc496d... |  |  |
100 | 09:15:32.047 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
101 | 09:15:32.085 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
102 | 09:15:32.085 |  | →RRC DCCH Security Mode Complete |  |  |
103 | 09:15:32.085 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
104 | 09:15:32.085 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
105 | 09:15:32.125 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
106 | 09:15:32.125 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
107 | 09:16:00.925 | →enobeB PCAP frame→ TCP |  |  |  |
108 | 09:16:00.928 |  | ←enobeB PCAP frame← TCP |  |  |
109 | 09:16:00.965 | →enobeB PCAP frame→ TCP |  |  |  |
110 | 09:16:01.093 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
111 | 09:16:01.097 |  | ←enobeB PCAP frame← TCP |  |  |
112 | 09:16:01.102 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
113 | 09:16:01.125 | →enobeB PCAP frame→ TCP |  |  |  |
114 | 09:16:01.253 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
115 | 09:16:01.258 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
116 | 09:16:01.270 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 16)
117 | 09:16:01.285 | →enobeB PCAP frame→ TCP |  |  |  |
118 | 09:16:01.293 | →enobeB PCAP frame→ HTTPS: GET /xcap-root/org.3gpp.mcptt.ue-init-config/users... |  |  |  |
119 | 09:16:01.297 |  | ←enobeB PCAP frame← TCP |  |  |
120 | 09:16:01.310 |  |  |  |  | →HTTP GET | HTTP-Proxy
121 | 09:16:01.316 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:307: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
122 | 09:16:01.326 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
123 | 09:16:01.336 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
124 | 09:16:01.365 | →enobeB PCAP frame→ TCP |  |  |  |
125 | 09:16:03.205 | →enobeB PCAP frame→ TCP |  |  |  |
126 | 09:16:03.209 |  | ←enobeB PCAP frame← TCP |  |  |
127 | 09:16:03.245 | →enobeB PCAP frame→ TCP |  |  |  |
128 | 09:16:03.253 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
129 | 09:16:03.257 |  | ←enobeB PCAP frame← TCP |  |  |
130 | 09:16:03.262 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
131 | 09:16:03.285 | →enobeB PCAP frame→ TCP |  |  |  |
132 | 09:16:03.581 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
133 | 09:16:03.665 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
134 | 09:16:03.678 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
135 | 09:16:03.685 | →enobeB PCAP frame→ TCP |  |  |  |
136 | 09:16:03.693 | →enobeB PCAP frame→ HTTPS: GET /idms/auth?redirect_uri=https%3A%2F%2F192.168... |  |  |  |
137 | 09:16:03.697 |  | ←enobeB PCAP frame← TCP |  |  |
138 | 09:16:03.711 |  |  |  |  | →HTTP GET | IDMS-Endpoint
139 | 09:16:03.712 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
140 | 09:16:03.724 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
141 | 09:16:03.725 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:526: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
142 | 09:16:03.726 |  |  |  |  | MMICmd: Please provide user credentials: username and password
143 | 09:16:03.765 | →enobeB PCAP frame→ TCP |  |  |  |
144 | 09:16:08.173 | →enobeB PCAP frame→ HTTPS: POST /idms/userauth HTTP/1.1 |  |  |  |
145 | 09:16:08.177 |  | ←enobeB PCAP frame← TCP |  |  |
146 | 09:16:08.192 |  |  |  |  | →HTTP POST | IDMS-Endpoint
147 | 09:16:08.194 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
148 | 09:16:08.205 | →enobeB PCAP frame→ TCP |  |  |  |
149 | 09:16:08.207 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
150 | 09:16:08.209 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:531: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
151 | 09:16:08.245 | →enobeB PCAP frame→ TCP |  |  |  |
152 | 09:16:08.248 |  | ←enobeB PCAP frame← TCP |  |  |
153 | 09:16:08.261 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:693: IdM port - Client closed the connection (id 18)
154 | 09:16:08.285 | →enobeB PCAP frame→ TCP |  |  |  |
155 | 09:16:08.725 | →enobeB PCAP frame→ TCP |  |  |  |
156 | 09:16:08.729 |  | ←enobeB PCAP frame← TCP |  |  |
157 | 09:16:08.765 | →enobeB PCAP frame→ TCP |  |  |  |
158 | 09:16:08.813 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
159 | 09:16:08.817 |  | ←enobeB PCAP frame← TCP |  |  |
160 | 09:16:08.818 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
161 | 09:16:08.845 | →enobeB PCAP frame→ TCP |  |  |  |
162 | 09:16:08.933 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
163 | 09:16:08.937 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
164 | 09:16:08.949 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
165 | 09:16:08.965 | →enobeB PCAP frame→ TCP |  |  |  |
166 | 09:16:08.973 | →enobeB PCAP frame→ HTTPS: POST /idms/token HTTP/1.1 |  |  |  |
167 | 09:16:08.977 |  | ←enobeB PCAP frame← TCP |  |  |
168 | 09:16:08.984 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
169 | 09:16:08.990 |  |  |  |  | →HTTP POST | IDMS-Endpoint
170 | 09:16:08.996 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
171 | 09:16:09.000 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:536: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
172 | 09:16:09.045 | →enobeB PCAP frame→ TCP |  |  |  |
173 | 09:16:09.325 | →enobeB PCAP frame→ TCP |  |  |  |
174 | 09:16:09.329 |  | ←enobeB PCAP frame← TCP |  |  |
175 | 09:16:09.365 | →enobeB PCAP frame→ TCP |  |  |  |
176 | 09:16:09.373 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
177 | 09:16:09.377 |  | ←enobeB PCAP frame← TCP |  |  |
178 | 09:16:09.381 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
179 | 09:16:09.405 | →enobeB PCAP frame→ TCP |  |  |  |
180 | 09:16:09.453 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
181 | 09:16:09.456 |  | ←enobeB PCAP frame← TCP |  |  |
182 | 09:16:09.458 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
183 | 09:16:09.470 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 19)
184 | 09:16:09.493 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
185 | 09:16:09.497 |  | ←enobeB PCAP frame← TCP |  |  |
186 | 09:16:09.512 |  |  |  |  | →HTTP POST | HTTP-Proxy
187 | 09:16:09.534 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
188 | 09:16:09.536 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:554: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
189 | 09:16:09.545 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
190 | 09:16:09.565 | →enobeB PCAP frame→ TCP |  |  |  |
191 | 09:16:09.605 | →enobeB PCAP frame→ TCP |  |  |  |
192 | 09:16:09.608 |  | ←enobeB PCAP frame← TCP |  |  |
193 | 09:16:09.645 | →enobeB PCAP frame→ TCP |  |  |  |
194 | 09:16:09.653 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
195 | 09:16:09.656 |  | ←enobeB PCAP frame← TCP |  |  |
196 | 09:16:09.660 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
197 | 09:16:09.685 | →enobeB PCAP frame→ TCP |  |  |  |
198 | 09:16:09.693 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
199 | 09:16:09.696 |  | ←enobeB PCAP frame← TCP |  |  |
200 | 09:16:09.698 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
201 | 09:16:09.711 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 20)
202 | 09:16:09.733 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
203 | 09:16:09.737 |  | ←enobeB PCAP frame← TCP |  |  |
204 | 09:16:09.752 |  |  |  |  | →HTTP POST | HTTP-Proxy
205 | 09:16:09.802 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
206 | 09:16:09.814 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
207 | 09:16:09.815 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:558: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
208 | 09:16:09.845 | →enobeB PCAP frame→ TCP |  |  |  |
209 | 09:16:09.933 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
210 | 09:16:09.953 |  |  |  |  | →SIP REGISTER | P-CSCF
211 | 09:16:09.977 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:833: IMS UDP_s port 192.168.2.3:5062 configured
212 | 09:16:09.996 |  | ←enobeB PCAP frame← SIP -cleartext-: SIP/2.0 401 Unauthorized |  |  |
213 | 09:16:10.002 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:784: IMS TCP_s port 192.168.2.3:5062 configured!
214 | 09:16:10.003 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:842: IMS UDP_c port 192.168.2.3:5061 configured
215 | 09:16:10.008 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
216 | 09:16:10.653 | →enobeB PCAP frame→ SIP over IPSEC: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
217 | 09:16:10.675 |  |  |  |  | →SIP REGISTER | P-CSCF
218 | 09:16:10.692 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
219 | 09:16:10.701 |  |  |  |  | ←SIP 200 OK | P-CSCF
220 | 09:16:11.013 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
221 | 09:16:11.054 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
222 | 09:16:11.108 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
223 | 09:16:11.117 |  |  |  |  | ←SIP 200 OK | P-CSCF
224 | 09:16:11.118 |  |  |  |  | MIKEY | Media-Server
225 | 09:16:11.324 |  |  |  |  | XML→ | Media-Server
226 | 09:16:11.325 |  |  |  |  | XML→ | Media-Server
227 | 09:16:11.329 |  |  |  |  | ←XML | Media-Server
228 | 09:16:11.332 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:39473;transp... |  |  |
229 | 09:16:11.333 |  |  |  |  | ←SIP NOTIFY | P-CSCF
230 | 09:16:11.396 |  |  |  |  | →SIP 200 OK | P-CSCF
231 | 09:16:11.530 |  | ←enobeB PCAP frame← TCP |  |  |
232 | 09:16:11.565 | →enobeB PCAP frame→ TCP |  |  |  |
233 | 09:16:11.573 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
234 | 09:16:11.577 |  | ←enobeB PCAP frame← TCP |  |  |
235 | 09:16:11.581 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
236 | 09:16:11.605 | →enobeB PCAP frame→ TCP |  |  |  |
237 | 09:16:11.693 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
238 | 09:16:11.705 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
239 | 09:16:11.712 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
240 | 09:16:11.725 | →enobeB PCAP frame→ TCP |  |  |  |
241 | 09:16:11.773 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... DNS |  |  |  |
242 | 09:16:11.778 |  | ←enobeB PCAP frame← TCP |  |  |
243 | 09:16:11.792 |  |  |  |  | →HTTP GET | HTTP-Proxy
244 | 09:16:11.795 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
245 | 09:16:11.800 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:691: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/mcptt-userA-id@mcstaasting.com/urn:uuid:6421193d-7997-4256-bc9a-30f70e37cd0b/mcpttue-configuration.xml
246 | 09:16:11.805 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
247 | 09:16:11.845 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
248 | 09:16:11.849 |  | ←enobeB PCAP frame← TCP |  |  |
249 | 09:16:11.853 | →enobeB PCAP frame→ TCP |  |  |  |
250 | 09:16:11.862 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
251 | 09:16:11.865 |  | ←enobeB PCAP frame← TCP |  |  |
252 | 09:16:11.885 | →enobeB PCAP frame→ TCP |  |  |  |
253 | 09:16:12.045 | →enobeB PCAP frame→ TCP |  |  |  |
254 | 09:16:12.049 |  | ←enobeB PCAP frame← TCP |  |  |
255 | 09:16:12.085 | →enobeB PCAP frame→ TCP |  |  |  |
256 | 09:16:12.093 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
257 | 09:16:12.104 |  | ←enobeB PCAP frame← TCP |  |  |
258 | 09:16:12.105 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
259 | 09:16:12.125 | →enobeB PCAP frame→ TCP |  |  |  |
260 | 09:16:12.173 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
261 | 09:16:12.182 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
262 | 09:16:12.193 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
263 | 09:16:12.205 | →enobeB PCAP frame→ TCP |  |  |  |
264 | 09:16:12.213 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
265 | 09:16:12.236 |  |  |  |  | →HTTP GET | HTTP-Proxy
266 | 09:16:12.243 |  | ←enobeB PCAP frame← TCP |  |  |
267 | 09:16:12.249 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:696: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/mcptt-userA-id@mcstaasting.com/mcpttuser-profile-49.xml
268 | 09:16:12.287 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
269 | 09:16:12.288 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
270 | 09:16:12.290 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
271 | 09:16:12.325 | →enobeB PCAP frame→ TCP |  |  |  |
272 | 09:16:12.333 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
273 | 09:16:12.344 |  | ←enobeB PCAP frame← TCP |  |  |
274 | 09:16:12.356 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
275 | 09:16:12.365 | →enobeB PCAP frame→ TCP |  |  |  |
276 | 09:16:13.143 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
277 | 09:16:13.173 |  | ←enobeB PCAP frame← TCP |  |  |
278 | 09:16:13.182 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
279 | 09:16:13.194 |  |  |  |  | ←SIP 200 OK | P-CSCF
280 | 09:16:13.195 |  |  |  |  | MIKEY | Media-Server
281 | 09:16:13.253 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
282 | 09:16:13.257 |  | ←enobeB PCAP frame← TCP |  |  |
283 | 09:16:13.258 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
284 | 09:16:13.285 | →enobeB PCAP frame→ TCP |  |  |  |
285 | 09:16:13.333 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
286 | 09:16:13.339 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
287 | 09:16:13.352 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
288 | 09:16:13.373 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
289 | 09:16:13.380 |  | ←enobeB PCAP frame← TCP |  |  |
290 | 09:16:13.392 |  |  |  |  | →HTTP GET | HTTP-Proxy
291 | 09:16:13.394 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:701: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
292 | 09:16:13.395 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
293 | 09:16:13.400 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
294 | 09:16:13.416 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:39473;transp... |  |  |
295 | 09:16:13.416 |  |  |  |  | XML→ | Media-Server
296 | 09:16:13.417 |  |  |  |  | XML→ | Media-Server
297 | 09:16:13.420 |  |  |  |  | ←XML | Media-Server
298 | 09:16:13.423 |  |  |  |  | ←SIP NOTIFY | P-CSCF
299 | 09:16:13.445 | →enobeB PCAP frame→ TCP |  |  |  |
300 | 09:16:13.453 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK TLS: Mix Info |  |  |  |
301 | 09:16:13.457 |  | ←enobeB PCAP frame← TCP |  |  |
302 | 09:16:13.470 |  |  |  |  | →SIP 200 OK | P-CSCF
303 | 09:16:13.470 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
304 | 09:16:13.485 | →enobeB PCAP frame→ TCP |  |  |  |
305 | 09:16:13.525 | →enobeB PCAP frame→ TCP |  |  |  |
306 | 09:16:13.529 |  | ←enobeB PCAP frame← TCP |  |  |
307 | 09:16:13.565 | →enobeB PCAP frame→ TCP |  |  |  |
308 | 09:16:13.573 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
309 | 09:16:13.576 |  | ←enobeB PCAP frame← TCP |  |  |
310 | 09:16:13.592 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
311 | 09:16:13.605 | →enobeB PCAP frame→ TCP |  |  |  |
312 | 09:16:13.733 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
313 | 09:16:13.741 |  | ←enobeB PCAP frame← TCP |  |  |
314 | 09:16:13.745 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
315 | 09:16:13.754 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
316 | 09:16:13.765 | →enobeB PCAP frame→ TCP |  |  |  |
317 | 09:16:13.773 | →enobeB PCAP frame→ HTTPS: GET http://xcap.gms.mcstaasting.com/org.openmobile... |  |  |  |
318 | 09:16:13.792 |  |  |  |  | →HTTP GET | HTTP-Proxy
319 | 09:16:13.793 |  | ←enobeB PCAP frame← TCP |  |  |
320 | 09:16:13.803 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:706: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at http://xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
321 | 09:16:13.832 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
322 | 09:16:13.832 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
323 | 09:16:13.837 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
324 | 09:16:13.845 | →enobeB PCAP frame→ TCP |  |  |  |
325 | 09:16:13.885 | →enobeB PCAP frame→ TCP |  |  |  |
326 | 09:16:13.893 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
327 | 09:16:13.909 |  | ←enobeB PCAP frame← TCP |  |  |
328 | 09:16:13.919 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
329 | 09:16:13.925 | →enobeB PCAP frame→ TCP |  |  |  |
330 | 09:16:14.139 |  |  |  |  | →SIP PUBLISH | P-CSCF
331 | 09:16:14.183 |  |  |  |  | MIKEY | Media-Server
332 | 09:16:14.210 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
333 | 09:16:14.385 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
334 | 09:16:14.393 |  |  |  |  | XML→ | Media-Server
335 | 09:16:14.397 |  |  |  |  | ←SIP 200 OK | P-CSCF
336 | 09:16:14.400 |  |  |  |  | ←SIP 200 OK | P-CSCF
337 | 09:16:14.400 |  |  |  |  | MIKEY | Media-Server
338 | 09:16:14.401 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
339 | 09:16:14.595 |  |  |  |  | XML→ | Media-Server
340 | 09:16:14.596 |  |  |  |  | XML→ | Media-Server
341 | 09:16:14.624 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:39473;transp... |  |  |
342 | 09:16:14.630 |  |  |  |  | MIKEY | Media-Server
343 | 09:16:14.631 |  |  |  |  | ←XML | Media-Server
344 | 09:16:14.636 |  |  |  |  | ←SIP NOTIFY | P-CSCF
345 | 09:16:14.667 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
346 | 09:16:14.668 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
347 | 09:16:14.669 |  |  |  |  | →SIP 200 OK | P-CSCF
348 | 09:16:14.672 |  |  |  |  | ←XML | Media-Server
349 | 09:16:14.679 |  |  |  |  | ←SIP MESSAGE | P-CSCF
350 | 09:16:15.533 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
351 | 09:16:15.551 |  |  |  |  | →SIP 200 OK | P-CSCF
352 | 09:16:17.559 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
353 | 09:16:17.595 |  | ←RRC DCCH RRC Connection Release |  |  |
354 | 09:16:17.596 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
355 | 09:16:17.630 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
356 | 09:16:17.634 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
357 | 09:16:17.634 |  |  |  |  | MMICmd: Make the MCPTT User request the creation of a pre-established session
358 | 09:16:18.142 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
359 | 09:16:18.142 |  | →RRC CCCH RRC Connection Request |  |  |
360 | 09:16:18.142 |  | ←RRC CCCH RRC Connection Setup |  |  |
361 | 09:16:18.142 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
362 | 09:16:18.165 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
363 | 09:16:18.165 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
364 | 09:16:18.165 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
365 | 09:16:18.165 |  |  |  | →NAS EMM Service request |  |
366 | 09:16:18.165 |  |  |  | NAS K-enb 6f15082523871db62c024d057e0876e53... |  |
367 | 09:16:18.166 |  | ←RRC DCCH Security Mode Command |  |  |
368 | 09:16:18.166 |  |  | RRC K-enb 6f15082523871db62c024d057e0876e53... |  |  |
369 | 09:16:18.166 |  |  | RRC rrc-cip 351d64236f70e3a25edfdf5555ae5bf... |  |  |
370 | 09:16:18.166 |  |  | RRC rrc-int eb1bf32783fd9c79299765f734d6cb2... |  |  |
371 | 09:16:18.166 |  |  | RRC up-cip 792fff997c5407068ad2ff7f107523d2... |  |  |
372 | 09:16:18.166 |  |  | RRC up-int e724718dc195cc808f5e828d4edb0552... |  |  |
373 | 09:16:18.167 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
374 | 09:16:18.205 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
375 | 09:16:18.205 |  | →RRC DCCH Security Mode Complete |  |  |
376 | 09:16:18.205 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
377 | 09:16:18.205 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
378 | 09:16:18.245 | →enobeB PCAP frame→ DNS RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
379 | 09:16:18.245 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
380 | 09:16:23.053 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
381 | 09:16:23.075 |  |  |  |  | →SIP INVITE | P-CSCF
382 | 09:16:23.098 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
383 | 09:16:23.110 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
384 | 09:16:23.110 |  |  |  |  | ←SIP 100 Trying | P-CSCF
385 | 09:16:23.121 |  |  |  |  | ←SIP 200 OK | P-CSCF
386 | 09:16:23.123 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
387 | 09:16:23.744 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
388 | 09:16:23.744 |  | [EMBEDDED NAS IN NEXT RRC] ESM Activate dedicated EPS bearer conte... |  |  |
389 | 09:16:23.744 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
390 | 09:16:23.745 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration Activate dedicated EPS bearer context request |  |  |
391 | 09:16:23.765 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
392 | 09:16:23.765 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
393 | 09:16:23.805 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Activate dedicated EPS bearer context accept |  |  |  |
394 | 09:16:23.805 |  | →RRC DCCH UL Information Transfer |  |  |
395 | 09:16:23.805 |  | [EMBEDDED NAS IN PREV RRC] ESM Activate dedicated EPS bearer conte... |  |  |
396 | 09:16:23.805 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
397 | 09:16:23.907 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
398 | 09:16:24.093 | →enobeB PCAP frame→ SIP over IPSEC: ACK sip:sessionB@cf.mcstaasting.com SIP/2.0 |  |  |  |
399 | 09:16:24.111 |  |  |  |  | →SIP ACK | P-CSCF
400 | 09:16:26.122 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
401 | 09:16:26.163 |  | ←RRC DCCH RRC Connection Release |  |  |
402 | 09:16:26.164 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
403 | 09:16:26.188 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
404 | 09:16:26.189 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:1250: Test-Body Step 1
405 | 09:16:26.191 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
406 | 09:16:26.193 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
407 | 09:16:26.208 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:754: SRTP config: Master Key: 02D546D3783B5AC9D2E3C4B44351E826, Master Salt: 866F01480F39E6C4F8779F61, MKI: 20E914B0
408 | 09:16:26.208 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
409 | 09:16:26.214 |  |  |  |  | ←Connect | Media-Server
410 | 09:16:27.172 |  | ←enobeB PCAP frame← LTE RRC PCCH Paging (1 PagingRecord) |  |  |
411 | 09:16:27.172 |  | ←RRC PCCH Paging |  |  |
412 | 09:16:27.202 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
413 | 09:16:27.202 |  | →RRC CCCH RRC Connection Request |  |  |
414 | 09:16:27.202 |  | ←RRC CCCH RRC Connection Setup |  |  |
415 | 09:16:27.202 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
416 | 09:16:27.245 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
417 | 09:16:27.245 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
418 | 09:16:27.245 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
419 | 09:16:27.245 |  |  |  | →NAS EMM Service request |  |
420 | 09:16:27.245 |  |  |  | NAS K-enb be5662fada7a21a3669d82765881b3b16... |  |
421 | 09:16:27.246 |  | ←RRC DCCH Security Mode Command |  |  |
422 | 09:16:27.246 |  |  | RRC K-enb be5662fada7a21a3669d82765881b3b16... |  |  |
423 | 09:16:27.246 |  |  | RRC rrc-cip 51cf870ad7b43e3f041d52422a2ad55... |  |  |
424 | 09:16:27.246 |  |  | RRC rrc-int b7ff31a4abcadd9806aa9e3da17f548... |  |  |
425 | 09:16:27.246 |  |  | RRC up-cip ed365e43e3cf5df921a6e080ee25157a... |  |  |
426 | 09:16:27.246 |  |  | RRC up-int 506ac791300ba413d19501e3c8da81de... |  |  |
427 | 09:16:27.247 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
428 | 09:16:27.285 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
429 | 09:16:27.285 |  | →RRC DCCH Security Mode Complete |  |  |
430 | 09:16:27.285 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
431 | 09:16:27.285 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
432 | 09:16:27.325 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
433 | 09:16:27.325 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
434 | 09:16:27.327 |  | ←enobeB PCAP frame← |  |  |
435 | 09:16:27.365 | →enobeB PCAP frame→ |  |  |  |
436 | 09:16:27.376 |  | ←enobeB PCAP frame← |  |  |
437 | 09:16:27.382 |  |  |  |  | MCPC Acknowledgement→ | Media-Server
438 | 09:16:27.384 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:465: PreestablishedSessionAcknowledge Verdict: Pass
439 | 09:16:27.385 |  |  |  |  | Verdict PASS: MCPTT_GroupCall_MCX_IMS.ttcn:1252: Step 1 Verdict: Pass
440 | 09:16:27.385 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:1256: Test-Body Step 3
441 | 09:16:27.385 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:1259: Test-Body Step 4
442 | 09:16:27.388 |  |  |  |  | ←Floor Taken | Media-Server
443 | 09:16:28.126 |  | ←enobeB PCAP frame← |  |  |
444 | 09:16:28.136 |  |  |  |  | Info: MCPTT_GroupCall_MCX_IMS.ttcn:1262: Test-Body Step 5
445 | 09:16:28.139 |  |  |  |  | ←Disconnect | Media-Server
446 | 09:16:28.165 | →enobeB PCAP frame→ |  |  |  |
447 | 09:16:28.181 |  |  |  |  | MCPC Acknowledgement→ | Media-Server
448 | 09:16:28.184 |  |  |  |  | Verdict PASS: MCX_MediaControl_Procedures.ttcn:465: PreestablishedSessionAcknowledge Verdict: Pass
449 | 09:16:30.187 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
450 | 09:16:30.217 |  | ←RRC DCCH RRC Connection Release |  |  |
451 | 09:16:30.218 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
452 | 09:16:30.252 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
453 | 09:16:30.253 |  |  |  |  | Verdict PASS: MCPTT_GroupCall_MCX_IMS.ttcn:1264: Step 5 Verdict: Pass
454 | 09:16:30.255 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
455 | 09:16:30.257 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
456 | 09:16:30.266 |  |  |  |  | ←SIP BYE | P-CSCF
457 | 09:16:31.012 |  | ←enobeB PCAP frame← LTE RRC PCCH Paging (1 PagingRecord) |  |  |
458 | 09:16:31.012 |  | ←RRC PCCH Paging |  |  |
459 | 09:16:31.042 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
460 | 09:16:31.042 |  | →RRC CCCH RRC Connection Request |  |  |
461 | 09:16:31.042 |  | ←RRC CCCH RRC Connection Setup |  |  |
462 | 09:16:31.042 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
463 | 09:16:31.085 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
464 | 09:16:31.085 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
465 | 09:16:31.085 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
466 | 09:16:31.085 |  |  |  | →NAS EMM Service request |  |
467 | 09:16:31.085 |  |  |  | NAS K-enb f4363dddf9dab2a6461dac024510a0704... |  |
468 | 09:16:31.086 |  | ←RRC DCCH Security Mode Command |  |  |
469 | 09:16:31.086 |  |  | RRC K-enb f4363dddf9dab2a6461dac024510a0704... |  |  |
470 | 09:16:31.086 |  |  | RRC rrc-cip d8b33c09e4404939e498b0c4726e443... |  |  |
471 | 09:16:31.086 |  |  | RRC rrc-int 857ecdcc39e62c0f3a671029a4087dd... |  |  |
472 | 09:16:31.086 |  |  | RRC up-cip be921e113375c3590d862f33ce7d84da... |  |  |
473 | 09:16:31.086 |  |  | RRC up-int e305448a88eda97016ab69f109269656... |  |  |
474 | 09:16:31.087 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
475 | 09:16:31.125 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
476 | 09:16:31.125 |  | →RRC DCCH Security Mode Complete |  |  |
477 | 09:16:31.125 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
478 | 09:16:31.125 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
479 | 09:16:31.165 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
480 | 09:16:31.165 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
481 | 09:16:31.167 |  | ←enobeB PCAP frame← SIP over IPSEC: BYE sip:sessionB@cf.mcstaasting.com SIP/2.0 |  |  |
482 | 09:16:31.213 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
483 | 09:16:31.231 |  |  |  |  | →SIP 200 OK | P-CSCF
484 | 09:16:31.405 | →enobeB PCAP frame→ |  |  |  |
485 | 09:16:33.242 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
486 | 09:16:33.243 |  | [EMBEDDED NAS IN NEXT RRC] ESM Deactivate EPS bearer context reque... |  |  |
487 | 09:16:33.243 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
488 | 09:16:33.244 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration Deactivate EPS bearer context request (Regular de... |  |  |
489 | 09:16:33.250 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
490 | 09:16:33.285 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Deactivate EPS bearer context accept |  |  |  |
491 | 09:16:33.285 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
492 | 09:16:33.285 |  | →RRC DCCH UL Information Transfer |  |  |
493 | 09:16:33.285 |  | [EMBEDDED NAS IN PREV RRC] ESM Deactivate EPS bearer context accep... |  |  |
494 | 09:16:33.285 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
495 | 09:16:33.380 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
496 | 09:16:33.381 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
497 | 09:16:33.402 |  | ←RRC DCCH RRC Connection Release |  |  |
498 | 09:16:33.403 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
499 | 09:16:33.426 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
500 | 09:16:33.428 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
501 | 09:16:33.431 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
502 | 09:16:34.178 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.