MSG #201 2022-08-08 11:45:31.510

SIP REGISTER message at 11:45:31.510

    REGISTER sip:mcstaasting.com SIP/2.0
    Via: SIP/2.0/UDP 192.168.3.2:37559;branch=z9hG4bK-284222731;rport
    From: <sip:PublicUserId-A@mcstaasting.com>;tag=733155356
    To: <sip:PublicUserId-A@mcstaasting.com>
    Contact: <sip:PublicUserId-A@192.168.3.2:37559;transport=udp>;expires=600000;audio;+g.3gpp.icsi-ref="urn%3Aurn-7%3A3gpp-service.ims.icsi.mcptt";+g.3gpp.icsi-ref="urn%3Aurn-7%3A3gpp-service.ims.icsi.mcdata";+g.3gpp.icsi-ref="urn%3Aurn-7%3A3gpp-service.ims.icsi.mcdata.sds";+g.3gpp.cs-voice;+g.3gpp.mcptt;+g.3gpp.mcdata;+g.3gpp.mcdata.sds
    Call-ID: 07778ad9-2655-3350-0724-0555a88fcbbc
    CSeq: 1172732502 REGISTER
    Content-Length: 0
    Max-Forwards: 70
    Authorization: Digest username="PrivateUserId-A@mcstaasting.com",realm="mcstaasting.com",nonce="",uri="sip:mcstaasting.com",response=""
    Allow: INVITE, ACK, CANCEL, BYE, MESSAGE, OPTIONS, NOTIFY, PRACK, UPDATE, REFER
    Privacy: none
    P-Access-Network-Info: 3GPP-E-UTRAN-FDD;utran-cell-id-3gpp=0000000000000000
    User-Agent: MCS CLIENT SDK Nemergent 1.0 /v 7.2.6
    P-Preferred-Identity: <sip:PublicUserId-A@mcstaasting.com>
    Supported: path
    Supported: timer
    Security-Client: ipsec-3gpp;alg=hmac-sha-1-96;ealg=aes-cbc;prot=esp;mod=trans;spi-c=622426207;spi-s=390878626;port-c=40565;port-s=42058;q=0.9
    Require: sec-agree
    Proxy-Require: sec-agree