ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 11:43:01.059 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 11:43:01.061 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 11:43:01.062 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 11:43:01.064 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 11:43:01.066 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 11:43:01.068 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:824: IMS UDP port 192.168.2.3:5060 configured
7 | 11:43:01.075 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:774: IMS TCP port 192.168.2.3:5060 configured!
8 | 11:43:01.081 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:795: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 11:43:01.083 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:806: IdM port 192.168.2.3:8081 configured!
10 | 11:43:01.089 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 11:43:02.289 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 11:43:02.290 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 11:43:03.046 |  | ←RRC BCCH SIB |  |  |
14 | 11:43:03.051 |  | ←RRC BCCH SIB1 |  |  |
15 | 11:43:03.131 |  | ←RRC BCCH SIB1 |  |  |
16 | 11:43:03.206 |  | ←RRC BCCH SIB |  |  |
17 | 11:43:03.211 |  | ←RRC BCCH SIB1 |  |  |
18 | 11:43:39.525 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 11:43:39.525 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 11:43:39.525 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 11:43:39.525 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 11:43:39.594 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
23 | 11:43:39.594 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
24 | 11:43:39.594 |  |  |  | →NAS EMM Attach request |  |
25 | 11:43:39.594 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
26 | 11:43:39.594 |  |  |  | NAS K-asme 9011103d2f62be6cc8010d2d0aeed34d... |  |
27 | 11:43:39.594 |  |  |  | NAS ← EMM Authentication request |  |
28 | 11:43:39.595 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
29 | 11:43:39.595 |  | ←RRC DCCH DL Information Transfer |  |  |
30 | 11:43:39.596 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
31 | 11:43:39.658 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
32 | 11:43:39.658 |  | →RRC DCCH UL Information Transfer |  |  |
33 | 11:43:39.658 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
34 | 11:43:39.658 |  |  |  | →NAS EMM Authentication response |  |
35 | 11:43:39.658 |  |  |  | NAS UE auth OK |  |
36 | 11:43:39.658 |  |  |  | NAS K-nas-cip f745abbb6acfb4c20e4fdb3b8e9b3... |  |
37 | 11:43:39.658 |  |  |  | NAS K-nas-int 33901ad6717e1e58809079efca102... |  |
38 | 11:43:39.658 |  |  |  | NAS ← EMM Security mode command |  |
39 | 11:43:39.659 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
40 | 11:43:39.659 |  | ←RRC DCCH DL Information Transfer |  |  |
41 | 11:43:39.660 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
42 | 11:43:39.698 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
43 | 11:43:39.698 |  | →RRC DCCH UL Information Transfer |  |  |
44 | 11:43:39.698 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x8e) |  |  |
45 | 11:43:39.698 |  |  |  | →NAS EMM Security mode complete |  |
46 | 11:43:39.698 |  |  |  | NAS ← ESM ESM information request |  |
47 | 11:43:39.699 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xe) |  |  |
48 | 11:43:39.699 |  | ←RRC DCCH DL Information Transfer |  |  |
49 | 11:43:39.700 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
50 | 11:43:39.746 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer |  |  |  |
51 | 11:43:39.746 |  | →RRC DCCH UL Information Transfer |  |  |
52 | 11:43:39.746 |  | [EMBEDDED NAS IN PREV RRC] ESM Unknown message (type=0x2f) |  |  |
53 | 11:43:39.746 |  |  |  | →NAS ESM ESM information response |  |
54 | 11:43:39.746 |  |  |  | NAS K-enb dec1e15941a0ba1303b9c605123df942f... |  |
55 | 11:43:39.746 |  |  |  | NAS ← EMM Attach accept |  |
56 | 11:43:39.747 |  | ←RRC DCCH Security Mode Command |  |  |
57 | 11:43:39.747 |  |  | RRC K-enb dec1e15941a0ba1303b9c605123df942f... |  |  |
58 | 11:43:39.747 |  |  | RRC rrc-cip 5b1a0d4b8a9d3363b5e43d71f6cab85... |  |  |
59 | 11:43:39.747 |  |  | RRC rrc-int bf725d4972e5fcf2274cda2ede0d36b... |  |  |
60 | 11:43:39.747 |  |  | RRC up-cip 9d666c8210735b12686c492b8a5c4bfd... |  |  |
61 | 11:43:39.747 |  |  | RRC up-int f7f128eafa8ab34b0641ba5d9ff92918... |  |  |
62 | 11:43:39.748 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
63 | 11:43:39.756 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
64 | 11:43:39.778 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
65 | 11:43:39.778 |  | →RRC DCCH Security Mode Complete |  |  |
66 | 11:43:39.778 |  | ←RRC DCCH UE Capability Enquiry |  |  |
67 | 11:43:39.778 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
68 | 11:43:39.836 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS RRCConnectionReconfiguration(DTAP) (TP) |  |  |
69 | 11:43:39.836 |  | →RRC DCCH UE Capability Information |  |  |
70 | 11:43:39.836 |  | [EMBEDDED NAS IN NEXT RRC] TP Unknown message (type=0x15) |  |  |
71 | 11:43:39.836 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
72 | 11:43:39.858 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
73 | 11:43:39.898 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
74 | 11:43:39.898 |  | →RRC DCCH UL Information Transfer |  |  |
75 | 11:43:39.898 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xfe) |  |  |
76 | 11:43:39.898 |  |  |  | →NAS EMM Attach complete |  |
77 | 11:43:39.898 |  |  |  | NAS ← EMM EMM information |  |
78 | 11:43:39.899 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x6) |  |  |
79 | 11:43:39.899 |  | ←RRC DCCH DL Information Transfer |  |  |
80 | 11:43:39.900 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS DLInformationTransfer Ciphered message |  |  |
81 | 11:43:44.457 |  | ←RRC DCCH RRC Connection Release |  |  |
82 | 11:43:44.458 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
83 | 11:43:45.895 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
84 | 11:43:45.895 |  | →RRC CCCH RRC Connection Request |  |  |
85 | 11:43:45.895 |  | ←RRC CCCH RRC Connection Setup |  |  |
86 | 11:43:45.895 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
87 | 11:43:45.946 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
88 | 11:43:45.946 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
89 | 11:43:45.946 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
90 | 11:43:45.946 |  |  |  | →NAS EMM Service request |  |
91 | 11:43:45.946 |  |  |  | NAS K-enb 188a36f806bcadca69637989a48ef0999... |  |
92 | 11:43:45.947 |  | ←RRC DCCH Security Mode Command |  |  |
93 | 11:43:45.947 |  |  | RRC K-enb 188a36f806bcadca69637989a48ef0999... |  |  |
94 | 11:43:45.947 |  |  | RRC rrc-cip dc325235ab5d0b34c59bd72cac3b115... |  |  |
95 | 11:43:45.947 |  |  | RRC rrc-int 04c992b6c8f0ac0b49ecdf769b73f6c... |  |  |
96 | 11:43:45.947 |  |  | RRC up-cip 61aa828f08b6873a1e34299bdb73064a... |  |  |
97 | 11:43:45.947 |  |  | RRC up-int 44c0aa4f00641cb8181f3eff1e9212be... |  |  |
98 | 11:43:45.948 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
99 | 11:43:45.978 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
100 | 11:43:45.978 |  | →RRC DCCH Security Mode Complete |  |  |
101 | 11:43:45.978 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
102 | 11:43:45.978 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
103 | 11:43:46.018 | →enobeB PCAP frame→ TCP + LTE RRC RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
104 | 11:43:46.018 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
105 | 11:45:10.549 |  | ←enobeB PCAP frame← TCP |  |  |
106 | 11:45:10.717 |  | ←enobeB PCAP frame← TCP |  |  |
107 | 11:45:10.718 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
108 | 11:45:10.866 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
109 | 11:45:10.867 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 16)
110 | 11:45:10.869 |  | ←enobeB PCAP frame← TCP |  |  |
111 | 11:45:10.870 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
112 | 11:45:10.898 | →enobeB PCAP frame→ TCP |  |  |  |
113 | 11:45:10.946 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
114 | 11:45:10.948 |  |  |  |  | →HTTP GET | HTTP-Proxy
115 | 11:45:10.949 |  | ←enobeB PCAP frame← TCP |  |  |
116 | 11:45:10.955 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:323: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
117 | 11:45:10.976 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
118 | 11:45:10.980 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
119 | 11:45:10.981 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
120 | 11:45:11.018 | →enobeB PCAP frame→ TCP |  |  |  |
121 | 11:45:13.268 |  | ←enobeB PCAP frame← TCP |  |  |
122 | 11:45:13.309 |  | ←enobeB PCAP frame← TCP |  |  |
123 | 11:45:13.314 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
124 | 11:45:13.746 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
125 | 11:45:13.747 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
126 | 11:45:13.749 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
127 | 11:45:13.778 | →enobeB PCAP frame→ TCP |  |  |  |
128 | 11:45:13.786 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
129 | 11:45:13.787 |  |  |  |  | →HTTP GET | IDMS-Endpoint
130 | 11:45:13.789 |  | ←enobeB PCAP frame← TCP |  |  |
131 | 11:45:13.791 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
132 | 11:45:13.793 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
133 | 11:45:13.795 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:561: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
134 | 11:45:13.795 |  |  |  |  | MMICmd: Please provide user credentials: username and password
135 | 11:45:13.858 | →enobeB PCAP frame→ TCP |  |  |  |
136 | 11:45:29.626 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
137 | 11:45:29.627 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
138 | 11:45:29.630 |  | ←enobeB PCAP frame← TCP |  |  |
139 | 11:45:29.630 |  |  |  |  | →HTTP POST | IDMS-Endpoint
140 | 11:45:29.644 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
141 | 11:45:29.646 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
142 | 11:45:29.647 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:566: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
143 | 11:45:29.698 | →enobeB PCAP frame→ TCP |  |  |  |
144 | 11:45:29.699 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:693: IdM port - Client closed the connection (id 18)
145 | 11:45:29.700 |  | ←enobeB PCAP frame← TCP |  |  |
146 | 11:45:29.738 | →enobeB PCAP frame→ TCP |  |  |  |
147 | 11:45:30.058 | →enobeB PCAP frame→ TCP |  |  |  |
148 | 11:45:30.061 |  | ←enobeB PCAP frame← TCP |  |  |
149 | 11:45:30.098 | →enobeB PCAP frame→ TCP |  |  |  |
150 | 11:45:30.116 |  | ←enobeB PCAP frame← TCP |  |  |
151 | 11:45:30.119 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
152 | 11:45:30.267 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
153 | 11:45:30.269 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
154 | 11:45:30.298 | →enobeB PCAP frame→ TCP |  |  |  |
155 | 11:45:30.306 | →enobeB PCAP frame→ TCP |  |  |  |
156 | 11:45:30.308 |  |  |  |  | →HTTP POST | IDMS-Endpoint
157 | 11:45:30.309 |  | ←enobeB PCAP frame← TCP |  |  |
158 | 11:45:30.331 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:571: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
159 | 11:45:30.333 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
160 | 11:45:30.335 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
161 | 11:45:30.418 | →enobeB PCAP frame→ TCP |  |  |  |
162 | 11:45:30.858 | →enobeB PCAP frame→ TCP |  |  |  |
163 | 11:45:30.861 |  | ←enobeB PCAP frame← TCP |  |  |
164 | 11:45:30.898 | →enobeB PCAP frame→ TCP |  |  |  |
165 | 11:45:30.906 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
166 | 11:45:30.909 |  | ←enobeB PCAP frame← TCP |  |  |
167 | 11:45:30.912 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
168 | 11:45:30.938 | →enobeB PCAP frame→ TCP |  |  |  |
169 | 11:45:30.986 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
170 | 11:45:30.988 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 19)
171 | 11:45:30.989 |  | ←enobeB PCAP frame← TCP |  |  |
172 | 11:45:30.990 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
173 | 11:45:31.026 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/init HTTP/1.1 |  |  |  |
174 | 11:45:31.029 |  | ←enobeB PCAP frame← TCP |  |  |
175 | 11:45:31.030 |  |  |  |  | →HTTP POST | HTTP-Proxy
176 | 11:45:31.052 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:591: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
177 | 11:45:31.054 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
178 | 11:45:31.056 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
179 | 11:45:31.057 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
180 | 11:45:31.098 | →enobeB PCAP frame→ TCP |  |  |  |
181 | 11:45:31.138 | →enobeB PCAP frame→ TCP |  |  |  |
182 | 11:45:31.141 |  | ←enobeB PCAP frame← TCP |  |  |
183 | 11:45:31.178 | →enobeB PCAP frame→ TCP |  |  |  |
184 | 11:45:31.186 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
185 | 11:45:31.189 |  | ←enobeB PCAP frame← TCP |  |  |
186 | 11:45:31.193 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
187 | 11:45:31.218 | →enobeB PCAP frame→ TCP |  |  |  |
188 | 11:45:31.226 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
189 | 11:45:31.228 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 20)
190 | 11:45:31.229 |  | ←enobeB PCAP frame← TCP |  |  |
191 | 11:45:31.230 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
192 | 11:45:31.266 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
193 | 11:45:31.269 |  | ←enobeB PCAP frame← TCP |  |  |
194 | 11:45:31.269 |  |  |  |  | →HTTP POST | HTTP-Proxy
195 | 11:45:31.327 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
196 | 11:45:31.328 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:595: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
197 | 11:45:31.330 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
198 | 11:45:31.378 | →enobeB PCAP frame→ TCP |  |  |  |
199 | 11:45:31.418 | →enobeB PCAP frame→ TCP |  |  |  |
200 | 11:45:31.506 | →enobeB PCAP frame→ SIP -cleartext-: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
201 | 11:45:31.510 |  |  |  |  | →SIP REGISTER | P-CSCF
202 | 11:45:31.534 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:833: IMS UDP_s port 192.168.2.3:5062 configured
203 | 11:45:31.561 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:784: IMS TCP_s port 192.168.2.3:5062 configured!
204 | 11:45:31.563 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:842: IMS UDP_c port 192.168.2.3:5061 configured
205 | 11:45:31.569 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
206 | 11:45:31.571 |  | ←enobeB PCAP frame← SIP -cleartext-: SIP/2.0 401 Unauthorized |  |  |
207 | 11:45:32.346 | →enobeB PCAP frame→ SIP over IPSEC: REGISTER sip:mcstaasting.com SIP/2.0 |  |  |  |
208 | 11:45:32.351 |  |  |  |  | →SIP REGISTER | P-CSCF
209 | 11:45:32.376 |  |  |  |  | ←SIP 200 OK | P-CSCF
210 | 11:45:32.379 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
211 | 11:45:32.706 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
212 | 11:45:32.707 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
213 | 11:45:32.708 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
214 | 11:45:32.709 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 SIP over IPSEC: SUBSCRIBE sip:cms.mcstaasting.com SIP/2.0 |  |  |  |
215 | 11:45:32.723 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
216 | 11:45:32.782 |  |  |  |  | ←SIP 200 OK | P-CSCF
217 | 11:45:32.782 |  |  |  |  | MIKEY | Media-Server
218 | 11:45:32.784 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
219 | 11:45:33.002 |  |  |  |  | XML→ | Media-Server
220 | 11:45:33.003 |  |  |  |  | XML→ | Media-Server
221 | 11:45:33.006 |  |  |  |  | ←XML | Media-Server
222 | 11:45:33.010 |  |  |  |  | ←SIP NOTIFY | P-CSCF
223 | 11:45:33.012 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:42058;transp... |  |  |
224 | 11:45:33.066 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
225 | 11:45:33.067 |  |  |  |  | →SIP 200 OK | P-CSCF
226 | 11:45:33.258 | →enobeB PCAP frame→ TCP |  |  |  |
227 | 11:45:33.261 |  | ←enobeB PCAP frame← TCP |  |  |
228 | 11:45:33.298 | →enobeB PCAP frame→ TCP |  |  |  |
229 | 11:45:33.306 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
230 | 11:45:33.309 |  | ←enobeB PCAP frame← TCP |  |  |
231 | 11:45:33.313 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
232 | 11:45:33.338 | →enobeB PCAP frame→ TCP |  |  |  |
233 | 11:45:33.386 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
234 | 11:45:33.388 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
235 | 11:45:33.389 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
236 | 11:45:33.418 | →enobeB PCAP frame→ TCP |  |  |  |
237 | 11:45:33.426 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
238 | 11:45:33.428 |  |  |  |  | →HTTP GET | HTTP-Proxy
239 | 11:45:33.429 |  | ←enobeB PCAP frame← TCP |  |  |
240 | 11:45:33.436 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:731: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.ue-config/users/sip:mcptt-userA-id@mcstaasting.com/urn:gsma:imei:86740002-086650-0/mcpttue-configuration.xml
241 | 11:45:33.443 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
242 | 11:45:33.446 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
243 | 11:45:33.498 | →enobeB PCAP frame→ TCP |  |  |  |
244 | 11:45:33.506 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
245 | 11:45:33.507 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
246 | 11:45:33.509 |  | ←enobeB PCAP frame← TCP |  |  |
247 | 11:45:33.538 | →enobeB PCAP frame→ TCP |  |  |  |
248 | 11:45:33.698 | →enobeB PCAP frame→ TCP |  |  |  |
249 | 11:45:33.701 |  | ←enobeB PCAP frame← TCP |  |  |
250 | 11:45:33.738 | →enobeB PCAP frame→ TCP |  |  |  |
251 | 11:45:33.746 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
252 | 11:45:33.749 |  | ←enobeB PCAP frame← TCP |  |  |
253 | 11:45:33.753 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
254 | 11:45:33.778 | →enobeB PCAP frame→ TCP |  |  |  |
255 | 11:45:33.826 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
256 | 11:45:33.828 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
257 | 11:45:33.829 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
258 | 11:45:33.858 | →enobeB PCAP frame→ TCP |  |  |  |
259 | 11:45:33.866 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
260 | 11:45:33.868 |  |  |  |  | →HTTP GET | HTTP-Proxy
261 | 11:45:33.869 |  | ←enobeB PCAP frame← TCP |  |  |
262 | 11:45:33.880 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:736: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.user-profile/users/sip:mcptt-userA-id@mcstaasting.com/mcpttuser-profile-49.xml
263 | 11:45:33.922 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
264 | 11:45:33.927 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
265 | 11:45:33.928 |  | ←enobeB PCAP frame← TCP |  |  |
266 | 11:45:33.929 |  | ←enobeB PCAP frame← TCP |  |  |
267 | 11:45:33.930 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
268 | 11:45:33.978 | →enobeB PCAP frame→ TCP |  |  |  |
269 | 11:45:33.986 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
270 | 11:45:33.987 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
271 | 11:45:33.989 |  | ←enobeB PCAP frame← TCP |  |  |
272 | 11:45:34.667 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
273 | 11:45:34.668 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
274 | 11:45:34.669 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
275 | 11:45:34.683 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
276 | 11:45:34.698 | →enobeB PCAP frame→ TCP |  |  |  |
277 | 11:45:34.701 |  | ←enobeB PCAP frame← TCP |  |  |
278 | 11:45:34.738 | →enobeB PCAP frame→ TCP |  |  |  |
279 | 11:45:34.739 |  |  |  |  | ←SIP 200 OK | P-CSCF
280 | 11:45:34.740 |  |  |  |  | MIKEY | Media-Server
281 | 11:45:34.742 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
282 | 11:45:34.746 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
283 | 11:45:34.749 |  | ←enobeB PCAP frame← TCP |  |  |
284 | 11:45:34.751 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
285 | 11:45:34.778 | →enobeB PCAP frame→ TCP |  |  |  |
286 | 11:45:34.866 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
287 | 11:45:34.867 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
288 | 11:45:34.869 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
289 | 11:45:34.898 | →enobeB PCAP frame→ TCP |  |  |  |
290 | 11:45:34.906 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcptt... |  |  |  |
291 | 11:45:34.907 |  |  |  |  | →HTTP GET | HTTP-Proxy
292 | 11:45:34.909 |  | ←enobeB PCAP frame← TCP |  |  |
293 | 11:45:34.909 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:741: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcptt.service-config/global/service-config.xml
294 | 11:45:34.915 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
295 | 11:45:34.917 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
296 | 11:45:34.918 |  | ←enobeB PCAP frame← TCP |  |  |
297 | 11:45:34.919 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
298 | 11:45:34.938 | →enobeB PCAP frame→ TCP |  |  |  |
299 | 11:45:34.953 |  |  |  |  | XML→ | Media-Server
300 | 11:45:34.954 |  |  |  |  | XML→ | Media-Server
301 | 11:45:34.957 |  |  |  |  | ←XML | Media-Server
302 | 11:45:34.960 |  |  |  |  | ←SIP NOTIFY | P-CSCF
303 | 11:45:34.962 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:42058;transp... |  |  |
304 | 11:45:34.978 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
305 | 11:45:34.979 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
306 | 11:45:34.981 |  | ←enobeB PCAP frame← TCP |  |  |
307 | 11:45:34.986 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
308 | 11:45:34.987 |  |  |  |  | →SIP 200 OK | P-CSCF
309 | 11:45:34.989 |  | ←enobeB PCAP frame← TCP |  |  |
310 | 11:45:35.018 | →enobeB PCAP frame→ TCP |  |  |  |
311 | 11:45:35.746 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
312 | 11:45:35.747 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... SIP over IPSEC: PUBLISH sip:mcptt-server-A@mcstaasting.com SIP/2.0... |  |  |  |
313 | 11:45:35.750 |  | ←enobeB PCAP frame← TCP |  |  |
314 | 11:45:35.761 |  |  |  |  | →SIP PUBLISH | P-CSCF
315 | 11:45:35.778 | →enobeB PCAP frame→ TCP |  |  |  |
316 | 11:45:35.786 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
317 | 11:45:35.789 |  | ←enobeB PCAP frame← TCP |  |  |
318 | 11:45:35.792 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
319 | 11:45:35.807 |  |  |  |  | MIKEY | Media-Server
320 | 11:45:35.818 | →enobeB PCAP frame→ TCP |  |  |  |
321 | 11:45:35.906 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
322 | 11:45:35.907 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
323 | 11:45:35.909 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
324 | 11:45:35.938 | →enobeB PCAP frame→ TCP |  |  |  |
325 | 11:45:35.946 | →enobeB PCAP frame→ HTTPS: GET http://xcap.gms.mcstaasting.com/org.openmobile... |  |  |  |
326 | 11:45:35.947 |  |  |  |  | →HTTP GET | HTTP-Proxy
327 | 11:45:35.949 |  | ←enobeB PCAP frame← TCP |  |  |
328 | 11:45:35.949 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:746: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at http://xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
329 | 11:45:35.955 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
330 | 11:45:35.958 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
331 | 11:45:35.959 |  | ←enobeB PCAP frame← TCP |  |  |
332 | 11:45:35.960 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
333 | 11:45:35.978 | →enobeB PCAP frame→ TCP |  |  |  |
334 | 11:45:36.018 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
335 | 11:45:36.019 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
336 | 11:45:36.021 |  | ←enobeB PCAP frame← TCP |  |  |
337 | 11:45:36.026 | →enobeB PCAP frame→ TCP |  |  |  |
338 | 11:45:36.028 |  | ←enobeB PCAP frame← TCP |  |  |
339 | 11:45:36.029 |  |  |  |  | XML→ | Media-Server
340 | 11:45:36.032 |  |  |  |  | ←SIP 200 OK | P-CSCF
341 | 11:45:36.034 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
342 | 11:45:36.058 | →enobeB PCAP frame→ TCP |  |  |  |
343 | 11:45:36.146 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
344 | 11:45:36.147 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
345 | 11:45:36.148 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
346 | 11:45:36.149 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
347 | 11:45:36.162 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
348 | 11:45:36.210 |  |  |  |  | ←SIP 200 OK | P-CSCF
349 | 11:45:36.211 |  |  |  |  | MIKEY | Media-Server
350 | 11:45:36.213 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
351 | 11:45:36.428 |  |  |  |  | XML→ | Media-Server
352 | 11:45:36.429 |  |  |  |  | XML→ | Media-Server
354 | 11:45:36.463 |  |  |  |  | ←XML | Media-Server
355 | 11:45:36.468 |  |  |  |  | ←SIP NOTIFY | P-CSCF
356 | 11:45:36.471 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:42058;transp... |  |  |
357 | 11:45:36.506 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
358 | 11:45:36.507 |  |  |  |  | →SIP 200 OK | P-CSCF
359 | 11:45:36.510 |  |  |  |  | ←XML | Media-Server
360 | 11:45:36.517 |  |  |  |  | ←SIP MESSAGE | P-CSCF
361 | 11:45:36.521 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
362 | 11:45:36.522 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
363 | 11:45:37.436 |  |  |  |  | →SIP 200 OK | P-CSCF
364 | 11:45:39.445 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
365 | 11:45:39.537 |  | ←RRC DCCH RRC Connection Release |  |  |
366 | 11:45:39.538 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
367 | 11:45:39.551 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
368 | 11:45:39.623 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
369 | 11:45:39.625 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
370 | 11:45:39.625 |  |  |  |  | Info: MCPTT_ClientConfiguration_MCX_IMS.ttcn:300: Test-Body Step 1 - 2
371 | 11:45:39.629 |  |  |  |  | ←SIP MESSAGE | P-CSCF
372 | 11:45:40.225 |  | ←enobeB PCAP frame← LTE RRC PCCH Paging (1 PagingRecord) |  |  |
373 | 11:45:40.225 |  | ←RRC PCCH Paging |  |  |
374 | 11:45:40.265 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
375 | 11:45:40.265 |  | →RRC CCCH RRC Connection Request |  |  |
376 | 11:45:40.265 |  | ←RRC CCCH RRC Connection Setup |  |  |
377 | 11:45:40.265 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
378 | 11:45:40.306 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
379 | 11:45:40.306 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
380 | 11:45:40.306 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
381 | 11:45:40.306 |  |  |  | →NAS EMM Service request |  |
382 | 11:45:40.306 |  |  |  | NAS K-enb 2511ae65e6b643af687725f73f5604719... |  |
383 | 11:45:40.307 |  | ←RRC DCCH Security Mode Command |  |  |
384 | 11:45:40.307 |  |  | RRC K-enb 2511ae65e6b643af687725f73f5604719... |  |  |
385 | 11:45:40.307 |  |  | RRC rrc-cip cca762beb16846a1a60f68b365d9e08... |  |  |
386 | 11:45:40.307 |  |  | RRC rrc-int 8b3e14972d780a6c25d0afe6090cdb8... |  |  |
387 | 11:45:40.307 |  |  | RRC up-cip 5da455b5725f5f4854dd1b3c3a7c6a0e... |  |  |
388 | 11:45:40.307 |  |  | RRC up-int 02385bc535b348cd0ad13a5f7c6b8a13... |  |  |
389 | 11:45:40.308 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
390 | 11:45:40.338 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
391 | 11:45:40.338 |  | →RRC DCCH Security Mode Complete |  |  |
392 | 11:45:40.338 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
393 | 11:45:40.338 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
394 | 11:45:40.378 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
395 | 11:45:40.378 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
396 | 11:45:40.380 |  | ←enobeB PCAP frame← SIP MIKEY: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... |  |  |
397 | 11:45:41.186 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
398 | 11:45:41.188 |  |  |  |  | →SIP 200 OK | P-CSCF
399 | 11:45:41.195 |  |  |  |  | Verdict PASS: MCPTT_ClientConfiguration_MCX_IMS.ttcn:305: Step 2 Verdict: Pass
400 | 11:45:43.197 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
401 | 11:45:43.251 |  | ←RRC DCCH RRC Connection Release |  |  |
402 | 11:45:43.252 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
403 | 11:45:43.265 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
404 | 11:45:43.266 |  |  |  |  | Info: MCPTT_ClientConfiguration_MCX_IMS.ttcn:310: Test-Body Step 3
405 | 11:45:43.267 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
406 | 11:45:43.267 |  |  |  |  | MMICmd: Make the MCPTT User request the establishment of an MCPTT on-demand pre-arranged group call using Group A, automatic commencement mode, with implicit floor control
407 | 11:45:43.268 |  |  |  |  | Info: MCPTT_ClientConfiguration_MCX_IMS.ttcn:313: Test-Body Step 4
408 | 11:45:44.315 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
409 | 11:45:44.315 |  | →RRC CCCH RRC Connection Request |  |  |
410 | 11:45:44.315 |  | ←RRC CCCH RRC Connection Setup |  |  |
411 | 11:45:44.315 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
412 | 11:45:44.338 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
413 | 11:45:44.338 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
414 | 11:45:44.338 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
415 | 11:45:44.338 |  |  |  | →NAS EMM Service request |  |
416 | 11:45:44.338 |  |  |  | NAS K-enb ff8d0bfd89f4ab7917a9a0f65ecae6afe... |  |
417 | 11:45:44.339 |  | ←RRC DCCH Security Mode Command |  |  |
418 | 11:45:44.339 |  |  | RRC K-enb ff8d0bfd89f4ab7917a9a0f65ecae6afe... |  |  |
419 | 11:45:44.339 |  |  | RRC rrc-cip 8d66ad86ef7a2882f063ee683493789... |  |  |
420 | 11:45:44.339 |  |  | RRC rrc-int f1afa099566563f98f1d433be455d3d... |  |  |
421 | 11:45:44.339 |  |  | RRC up-cip 0be936f6f9badde9643ac4835e976749... |  |  |
422 | 11:45:44.339 |  |  | RRC up-int 3327bb096c00918cbc9baf87ce7bc1d9... |  |  |
423 | 11:45:44.340 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
424 | 11:45:44.378 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
425 | 11:45:44.378 |  | →RRC DCCH Security Mode Complete |  |  |
426 | 11:45:44.378 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
427 | 11:45:44.378 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
428 | 11:45:44.418 | →enobeB PCAP frame→ DNS RRCConnectionReconfigurationComplete [62-bytes] |  |  |  |
429 | 11:45:44.418 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
430 | 11:45:50.906 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
431 | 11:45:50.907 | →enobeB PCAP frame→ SIP over IPSEC: INVITE sip:mcptt-server-A@mcstaasting.com SIP/2.0 |  |  |  |
432 | 11:45:50.918 |  |  |  |  | →SIP INVITE | P-CSCF
433 | 11:45:50.971 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:754: SRTP config: Master Key: 412151304DF60441B2258FF08BFB28F0, Master Salt: F4DD66C81D3B3E59C20F812F, MKI: 20000102
434 | 11:45:50.971 |  |  |  |  | Info: TitanAdaptor_Functions.ttcn:184: RTP and FloorControl ports configured 192.168.2.3:60350:60351:60354
435 | 11:45:50.986 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
436 | 11:45:50.987 |  |  |  |  | XML→ | Media-Server
437 | 11:45:50.991 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl_MCPTT_MCVideo.ttcn:998: INVITE Verdict: Pass
438 | 11:45:50.992 |  |  |  |  | ←SIP 100 Trying | P-CSCF
439 | 11:45:50.995 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 100 Trying |  |  |
440 | 11:45:50.997 |  |  |  |  | ←SIP 200 OK | P-CSCF
441 | 11:45:50.999 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
442 | 11:45:51.639 |  |  |  | NAS ← ESM Activate dedicated EPS bearer conte... |  |
443 | 11:45:51.640 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0x5) |  |  |
444 | 11:45:51.640 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
445 | 11:45:51.641 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
446 | 11:45:51.658 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
447 | 11:45:51.658 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
448 | 11:45:51.698 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
449 | 11:45:51.698 |  | →RRC DCCH UL Information Transfer |  |  |
450 | 11:45:51.698 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0xc) |  |  |
451 | 11:45:51.698 |  |  |  | →NAS ESM Activate dedicated EPS bearer conte... |  |
452 | 11:45:51.765 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
453 | 11:45:51.877 |  |  |  |  | →SIP ACK | P-CSCF
454 | 11:45:51.885 |  |  |  |  | Verdict PASS: MCX_SIP_CallControl_MCPTT_MCVideo.ttcn:1001: ACK Verdict: Pass
455 | 11:45:51.886 |  |  |  |  | Verdict PASS: MCPTT_ClientConfiguration_MCX_IMS.ttcn:315: Step 4 Verdict: Pass
456 | 11:45:51.886 |  |  |  |  | Info: MCPTT_ClientConfiguration_MCX_IMS.ttcn:317: Test-Body Step 5
457 | 11:45:52.418 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
458 | 11:45:52.466 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
459 | 11:45:52.474 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
460 | 11:45:52.482 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
461 | 11:45:52.538 | →enobeB PCAP frame→ SRTP frame: |  |  |  |
462 | 11:45:52.637 |  |  |  |  | Info: MCPTT_ClientConfiguration_MCX_IMS.ttcn:320: Test-Body Step 6
463 | 11:45:52.637 |  |  |  |  | Info: MCPTT_ClientConfiguration_MCX_IMS.ttcn:323: Test-Body Step 7
464 | 11:45:52.738 |  |  |  |  | MMICmd: Release PTT token
465 | 11:45:54.426 | →enobeB PCAP frame→ |  |  |  |
466 | 11:45:54.427 |  |  |  |  | Floor Release→ | Media-Server
467 | 11:45:54.430 |  |  |  |  | Verdict PASS: MCPTT_MediaControl_Procedures.ttcn:95: Floor Release Verdict: Pass
468 | 11:45:54.431 |  |  |  |  | Verdict PASS: MCPTT_ClientConfiguration_MCX_IMS.ttcn:325: Step 7 Verdict: Pass
469 | 11:45:54.431 |  |  |  |  | Info: MCPTT_ClientConfiguration_MCX_IMS.ttcn:327: Test-Body Step 8 - 9
470 | 11:45:54.433 |  |  |  |  | ←Floor Idle | Media-Server
471 | 11:45:54.436 |  | ←enobeB PCAP frame← |  |  |
472 | 11:45:54.538 |  |  |  |  | MMICmd: Release call (hang up the call)
473 | 11:45:58.549 |  |  |  |  | →SIP BYE | P-CSCF
474 | 11:45:58.569 |  |  |  |  | ←SIP 200 OK | P-CSCF
475 | 11:45:58.571 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
476 | 11:45:59.058 | →enobeB PCAP frame→ |  |  |  |
477 | 11:46:00.567 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
478 | 11:46:00.586 |  |  |  | NAS ← ESM Deactivate EPS bearer context reque... |  |
479 | 11:46:00.587 |  | [EMBEDDED NAS IN NEXT RRC] TP Unknown message (type=0x94) |  |  |
480 | 11:46:00.587 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
481 | 11:46:00.588 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
482 | 11:46:00.618 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
483 | 11:46:00.618 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
484 | 11:46:00.618 |  | →RRC DCCH UL Information Transfer |  |  |
485 | 11:46:00.618 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x9) |  |  |
486 | 11:46:00.618 |  |  |  | →NAS ESM Deactivate EPS bearer context accep... |  |
487 | 11:46:00.706 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
488 | 11:46:00.708 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
489 | 11:46:00.760 |  | ←RRC DCCH RRC Connection Release |  |  |
490 | 11:46:00.761 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
491 | 11:46:00.784 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
492 | 11:46:00.785 |  |  |  |  | Verdict PASS: MCPTT_ClientConfiguration_MCX_IMS.ttcn:329: Step 9 Verdict: Pass
493 | 11:46:00.786 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
494 | 11:46:00.787 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
495 | 11:46:01.536 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.