ENB
MME
ENBMMEINFO
PCAP
SIP
HTTP
IPCAN
Info

# | Time | UE | Air | enodeB | MME | Tester | Component
--- | --- | --- | --- | --- | --- | --- | ---
1 | 08:52:45.948 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
2 | 08:52:45.951 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
3 | 08:52:45.952 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
4 | 08:52:45.953 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
5 | 08:52:45.956 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
6 | 08:52:45.957 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:824: IMS UDP port 192.168.2.3:5060 configured
7 | 08:52:45.964 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:774: IMS TCP port 192.168.2.3:5060 configured!
8 | 08:52:45.970 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:795: Http Proxy (CMS, KMS, GMS) at port 192.168.2.3:8100 configured!
9 | 08:52:45.972 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:806: IdM port 192.168.2.3:8081 configured!
10 | 08:52:45.978 |  |  |  |  | MMICmd: POWER_ON the UE
11 | 08:52:47.179 |  |  |  |  | MMICmd: Please initiate MCPTT authorisation/configuration
12 | 08:52:47.181 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
13 | 08:52:49.397 |  | ←RRC BCCH SIB |  |  |
14 | 08:52:49.402 |  | ←RRC BCCH SIB1 |  |  |
15 | 08:52:49.482 |  | ←RRC BCCH SIB1 |  |  |
16 | 08:52:49.557 |  | ←RRC BCCH SIB |  |  |
17 | 08:52:49.562 |  | ←RRC BCCH SIB1 |  |  |
18 | 08:54:17.286 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
19 | 08:54:17.286 |  | →RRC CCCH RRC Connection Request |  |  |
20 | 08:54:17.286 |  | ←RRC CCCH RRC Connection Setup |  |  |
21 | 08:54:17.286 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
22 | 08:54:17.337 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Attach request PDN connectivity request |  |  |  |
23 | 08:54:17.337 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
24 | 08:54:17.337 |  | [EMBEDDED NAS IN PREV RRC] EMM Attach request |  |  |
25 | 08:54:17.337 |  |  |  | →NAS EMM Attach request |  |
26 | 08:54:17.337 |  |  |  | NAS EPS encryption caps=0xf0 integrity caps=... |  |
27 | 08:54:17.337 |  |  |  | NAS K-asme 6a5599e0e286ae84c868810f180b6a43... |  |
28 | 08:54:17.337 |  |  |  | NAS ← EMM Authentication request |  |
29 | 08:54:17.338 |  | [EMBEDDED NAS IN NEXT RRC] EMM Authentication request |  |  |
30 | 08:54:17.338 |  | ←RRC DCCH DL Information Transfer |  |  |
31 | 08:54:17.339 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Authentication request |  |  |
32 | 08:54:17.409 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS ULInformationTransfer Authentication response |  |  |  |
33 | 08:54:17.409 |  | →RRC DCCH UL Information Transfer |  |  |
34 | 08:54:17.409 |  | [EMBEDDED NAS IN PREV RRC] EMM Authentication response |  |  |
35 | 08:54:17.409 |  |  |  | →NAS EMM Authentication response |  |
36 | 08:54:17.409 |  |  |  | NAS UE auth OK |  |
37 | 08:54:17.409 |  |  |  | NAS K-nas-cip 4599c401b6481b3e42c4faf36d6d9... |  |
38 | 08:54:17.409 |  |  |  | NAS K-nas-int 8bd5bdc9ebf7c4a7c435816b81a44... |  |
39 | 08:54:17.409 |  |  |  | NAS ← EMM Security mode command |  |
40 | 08:54:17.410 |  | [EMBEDDED NAS IN NEXT RRC] EMM Security mode command |  |  |
41 | 08:54:17.410 |  | ←RRC DCCH DL Information Transfer |  |  |
42 | 08:54:17.411 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer Security mode command |  |  |
43 | 08:54:17.449 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
44 | 08:54:17.449 |  | →RRC DCCH UL Information Transfer |  |  |
45 | 08:54:17.449 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x6) |  |  |
46 | 08:54:17.449 |  |  |  | →NAS EMM Security mode complete |  |
47 | 08:54:17.449 |  |  |  | NAS ← ESM ESM information request |  |
48 | 08:54:17.450 |  | [EMBEDDED NAS IN NEXT RRC] ESM Unknown message (type=0xdf) |  |  |
49 | 08:54:17.450 |  | ←RRC DCCH DL Information Transfer |  |  |
50 | 08:54:17.451 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer |  |  |
51 | 08:54:17.497 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
52 | 08:54:17.497 |  | →RRC DCCH UL Information Transfer |  |  |
53 | 08:54:17.497 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x1e) |  |  |
54 | 08:54:17.497 |  |  |  | →NAS ESM ESM information response |  |
55 | 08:54:17.497 |  |  |  | NAS ← EMM Attach accept |  |
56 | 08:54:17.497 |  |  |  | NAS K-enb 463e59a454cdbccf7f3c99a70ab10a0a7... |  |
57 | 08:54:17.498 |  | ←RRC DCCH Security Mode Command |  |  |
58 | 08:54:17.498 |  |  | RRC K-enb 463e59a454cdbccf7f3c99a70ab10a0a7... |  |  |
59 | 08:54:17.498 |  |  | RRC rrc-cip 4302853f6622b406784384eec42e637... |  |  |
60 | 08:54:17.498 |  |  | RRC rrc-int 11acc58d87d6261154ac08f5e9da6f5... |  |  |
61 | 08:54:17.498 |  |  | RRC up-cip 2da3363f358e8f3a2109f688657467c9... |  |  |
62 | 08:54:17.498 |  |  | RRC up-int 53409036bdbec9dd794a0a84caf352e1... |  |  |
63 | 08:54:17.499 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
64 | 08:54:17.529 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
65 | 08:54:17.529 |  | →RRC DCCH Security Mode Complete |  |  |
66 | 08:54:17.529 |  | ←RRC DCCH UE Capability Enquiry |  |  |
67 | 08:54:17.529 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH UECapabilityEnquiry |  |  |
68 | 08:54:17.594 |  | →RRC DCCH UE Capability Information |  |  |
69 | 08:54:17.595 |  | [EMBEDDED NAS IN NEXT RRC] Ciphered NAS Message (0xc) |  |  |
70 | 08:54:17.595 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
71 | 08:54:17.595 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS/NAS-EPS RRCConnectionReconfiguration Ciphered message |  |  |
72 | 08:54:17.649 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS/NAS-EPS ULInformationTransfer Ciphered message |  |  |  |
73 | 08:54:17.649 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
74 | 08:54:17.649 |  | →RRC DCCH UL Information Transfer |  |  |
75 | 08:54:17.649 |  | [EMBEDDED NAS IN PREV RRC] Ciphered NAS Message (0x0) |  |  |
76 | 08:54:17.649 |  |  |  | →NAS EMM Attach complete |  |
77 | 08:54:17.649 |  |  |  | NAS ← EMM EMM information |  |
78 | 08:54:17.650 |  | [EMBEDDED NAS IN NEXT RRC] ESM Unknown message (type=0xa9) |  |  |
79 | 08:54:17.650 |  | ←RRC DCCH DL Information Transfer |  |  |
80 | 08:54:17.651 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH/NAS-EPS DLInformationTransfer |  |  |
81 | 08:54:24.608 |  | ←RRC DCCH RRC Connection Release |  |  |
82 | 08:54:24.609 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
83 | 08:54:24.856 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
84 | 08:54:24.856 |  | →RRC CCCH RRC Connection Request |  |  |
85 | 08:54:24.856 |  | ←RRC CCCH RRC Connection Setup |  |  |
86 | 08:54:24.856 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
87 | 08:54:24.889 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
88 | 08:54:24.889 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
89 | 08:54:24.889 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
90 | 08:54:24.889 |  |  |  | →NAS EMM Service request |  |
91 | 08:54:24.889 |  |  |  | NAS K-enb b4f8bf6642a6a85076222421003a82967... |  |
92 | 08:54:24.890 |  |  | RRC K-enb b4f8bf6642a6a85076222421003a82967... |  |  |
93 | 08:54:24.891 |  |  | RRC rrc-cip c5954c574c3433f5a8b73fdef3625a5... |  |  |
94 | 08:54:24.891 |  |  | RRC rrc-int fe4151123cb70f0b014b7e79374804f... |  |  |
95 | 08:54:24.891 |  |  | RRC up-cip 89c0e7e9858378f4eb2c97cd528c56a1... |  |  |
96 | 08:54:24.891 |  |  | RRC up-int ea5752cfac4392c14a808db122b5cbf9... |  |  |
97 | 08:54:24.891 |  | ←RRC DCCH Security Mode Command |  |  |
98 | 08:54:24.891 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
99 | 08:54:24.945 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
100 | 08:54:24.945 |  | →RRC DCCH Security Mode Complete |  |  |
101 | 08:54:24.945 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
102 | 08:54:24.945 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
103 | 08:54:25.009 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
104 | 08:54:44.732 |  | ←enobeB PCAP frame← TCP |  |  |
105 | 08:54:44.820 |  | ←enobeB PCAP frame← TCP |  |  |
106 | 08:54:44.865 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
107 | 08:54:45.025 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 16)
108 | 08:54:45.028 |  | ←enobeB PCAP frame← TCP |  |  |
109 | 08:54:45.029 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
110 | 08:54:45.108 |  | ←enobeB PCAP frame← TCP |  |  |
111 | 08:54:45.109 |  |  |  |  | →HTTP GET | HTTP-Proxy
112 | 08:54:45.110 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:323: --- TS 36.579-1 Table 5.3.2.3-1A (Initial UE Configuration download) Step 1
113 | 08:54:45.114 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
114 | 08:54:45.119 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
115 | 08:54:47.332 |  | ←enobeB PCAP frame← TCP |  |  |
116 | 08:54:47.369 | →enobeB PCAP frame→ TCP |  |  |  |
117 | 08:54:47.377 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
118 | 08:54:47.380 |  | ←enobeB PCAP frame← TCP |  |  |
119 | 08:54:47.381 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
120 | 08:54:47.409 | →enobeB PCAP frame→ TCP |  |  |  |
121 | 08:54:47.744 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
122 | 08:54:47.748 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
123 | 08:54:47.776 |  |  |  |  | →HTTP GET | IDMS-Endpoint
124 | 08:54:47.780 |  | ←enobeB PCAP frame← TCP |  |  |
125 | 08:54:47.780 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
126 | 08:54:47.783 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
127 | 08:54:47.784 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:561: --- TS 36.579-1 Table 5.3.2.3-1 (User Authentication) Steps 3-4 DONE
128 | 08:54:47.784 |  |  |  |  | MMICmd: Please provide user credentials: username and password
129 | 08:54:47.849 | →enobeB PCAP frame→ TCP |  |  |  |
130 | 08:54:53.497 | →enobeB PCAP frame→ TCP |  |  |  |
131 | 08:54:53.499 |  |  |  |  | →HTTP POST | IDMS-Endpoint
132 | 08:54:53.500 |  | ←enobeB PCAP frame← TCP |  |  |
133 | 08:54:53.511 |  |  |  |  | ←HTTP 302 Found | IDMS-Endpoint
134 | 08:54:53.514 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:566: --- Table 5.3.2.3-1 (User Authentication) Steps 5-7 DONE
135 | 08:54:53.515 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
136 | 08:54:53.529 | →enobeB PCAP frame→ TCP |  |  |  |
137 | 08:54:53.576 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:693: IdM port - Client closed the connection (id 18)
138 | 08:54:53.580 |  | ←enobeB PCAP frame← TCP |  |  |
139 | 08:54:54.300 |  | ←enobeB PCAP frame← TCP |  |  |
140 | 08:54:54.388 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
141 | 08:54:54.536 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:649: Client connected to IdM port (id 18)
142 | 08:54:54.540 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
143 | 08:54:54.569 | →enobeB PCAP frame→ TCP |  |  |  |
144 | 08:54:54.584 |  |  |  |  | →HTTP POST | IDMS-Endpoint
145 | 08:54:54.588 |  | ←enobeB PCAP frame← TCP |  |  |
146 | 08:54:54.592 |  |  |  |  | ←HTTP 200 OK | IDMS-Endpoint
147 | 08:54:54.595 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:571: --- Table 5.3.2.3-1 (User Authentication) Steps 9-10 DONE
148 | 08:54:54.596 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
149 | 08:54:55.092 |  | ←enobeB PCAP frame← TCP |  |  |
150 | 08:54:55.129 | →enobeB PCAP frame→ TCP |  |  |  |
151 | 08:54:55.148 |  | ←enobeB PCAP frame← TCP |  |  |
152 | 08:54:55.217 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
153 | 08:54:55.265 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 19)
154 | 08:54:55.268 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
155 | 08:54:55.298 |  |  |  |  | →HTTP POST | HTTP-Proxy
156 | 08:54:55.300 |  | ←enobeB PCAP frame← TCP |  |  |
157 | 08:54:55.330 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:591: --- Table 5.3.2.3-1 (User Authentication) Steps 11-12 DONE
158 | 08:54:55.337 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
159 | 08:54:55.342 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
160 | 08:54:55.343 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
161 | 08:54:55.369 | →enobeB PCAP frame→ TCP |  |  |  |
162 | 08:54:55.409 | →enobeB PCAP frame→ TCP |  |  |  |
163 | 08:54:55.412 |  | ←enobeB PCAP frame← TCP |  |  |
164 | 08:54:55.449 | →enobeB PCAP frame→ TCP |  |  |  |
165 | 08:54:55.457 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
166 | 08:54:55.460 |  | ←enobeB PCAP frame← TCP |  |  |
167 | 08:54:55.463 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
168 | 08:54:55.489 | →enobeB PCAP frame→ TCP |  |  |  |
169 | 08:54:55.497 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
170 | 08:54:55.497 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 20)
171 | 08:54:55.500 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
172 | 08:54:55.537 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
173 | 08:54:55.537 |  |  |  |  | →HTTP POST | HTTP-Proxy
174 | 08:54:55.538 | →enobeB PCAP frame→ HTTPS: POST /keymanagement/identity/v1/keyprov HTTP/1.1 |  |  |  |
175 | 08:54:55.540 |  | ←enobeB PCAP frame← TCP |  |  |
176 | 08:54:55.559 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
177 | 08:54:55.560 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:595: --- Table 5.3.2.3-1 (User Authentication) Steps 13-14 DONE
178 | 08:54:55.563 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
179 | 08:54:55.609 | →enobeB PCAP frame→ TCP |  |  |  |
180 | 08:54:55.649 | →enobeB PCAP frame→ TCP |  |  |  |
181 | 08:54:55.819 |  |  |  |  | →SIP REGISTER | P-CSCF
182 | 08:54:55.909 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:833: IMS UDP_s port 192.168.2.3:5062 configured
183 | 08:54:55.935 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:784: IMS TCP_s port 192.168.2.3:5062 configured!
184 | 08:54:55.937 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:842: IMS UDP_c port 192.168.2.3:5061 configured
185 | 08:54:55.943 |  |  |  |  | ←SIP 401 Unauthorized | P-CSCF
186 | 08:54:55.947 |  | ←enobeB PCAP frame← SIP -cleartext-: SIP/2.0 401 Unauthorized |  |  |
187 | 08:54:56.860 |  |  |  |  | →SIP REGISTER | P-CSCF
188 | 08:54:56.877 |  |  |  |  | ←SIP 200 OK | P-CSCF
189 | 08:54:56.881 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
190 | 08:54:57.217 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
191 | 08:54:57.218 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
192 | 08:54:57.232 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
193 | 08:54:57.245 |  |  |  |  | ←SIP 200 OK | P-CSCF
194 | 08:54:57.245 |  |  |  |  | MIKEY | Media-Server
195 | 08:54:57.249 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
196 | 08:54:57.443 |  |  |  |  | XML→ | Media-Server
197 | 08:54:57.444 |  |  |  |  | XML→ | Media-Server
198 | 08:54:57.447 |  |  |  |  | ←XML | Media-Server
199 | 08:54:57.450 |  |  |  |  | ←SIP NOTIFY | P-CSCF
200 | 08:54:57.455 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
201 | 08:54:57.456 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:40250;transp... |  |  |
202 | 08:54:57.496 |  |  |  |  | →SIP 200 OK | P-CSCF
203 | 08:54:57.652 |  | ←enobeB PCAP frame← TCP |  |  |
204 | 08:54:57.689 | →enobeB PCAP frame→ TCP |  |  |  |
205 | 08:54:57.697 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
206 | 08:54:57.700 |  | ←enobeB PCAP frame← TCP |  |  |
207 | 08:54:57.701 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
208 | 08:54:57.729 | →enobeB PCAP frame→ TCP |  |  |  |
209 | 08:54:57.817 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
210 | 08:54:57.817 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
211 | 08:54:57.820 |  | ←enobeB PCAP frame← TCP |  |  |
212 | 08:54:57.821 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
213 | 08:54:57.849 | →enobeB PCAP frame→ TCP |  |  |  |
214 | 08:54:57.896 |  |  |  |  | →HTTP GET | HTTP-Proxy
215 | 08:54:57.897 | →enobeB PCAP frame→ HTTPS: GET http://xcap.cms.mcstaasting.com/org.3gpp.mcdat... |  |  |  |
216 | 08:54:57.898 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:731: --- TS 36.579-1 Table 5.3.2.3-2A: Step 5 Download UE Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcdata.ue-config/users/sip:mcdata-userA-id@mcstaasting.com/urn:gsma:imei:86740002-086650-0/mcdataue-configuration.xml
217 | 08:54:57.900 |  | ←enobeB PCAP frame← TCP |  |  |
218 | 08:54:57.901 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
219 | 08:54:57.906 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
220 | 08:54:57.929 | →enobeB PCAP frame→ TCP |  |  |  |
221 | 08:54:57.969 | →enobeB PCAP frame→ TCP |  |  |  |
222 | 08:54:57.976 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
223 | 08:54:57.977 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
224 | 08:54:57.980 |  | ←enobeB PCAP frame← TCP |  |  |
225 | 08:54:57.985 | →enobeB PCAP frame→ TCP |  |  |  |
226 | 08:54:57.988 |  | ←enobeB PCAP frame← TCP |  |  |
227 | 08:54:58.009 | →enobeB PCAP frame→ TCP |  |  |  |
228 | 08:54:58.409 | →enobeB PCAP frame→ TCP |  |  |  |
229 | 08:54:58.412 |  | ←enobeB PCAP frame← TCP |  |  |
230 | 08:54:58.449 | →enobeB PCAP frame→ TCP |  |  |  |
231 | 08:54:58.457 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
232 | 08:54:58.460 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
233 | 08:54:58.537 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
234 | 08:54:58.540 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
235 | 08:54:58.577 | →enobeB PCAP frame→ TCP |  |  |  |
236 | 08:54:58.577 |  |  |  |  | →HTTP GET | HTTP-Proxy
237 | 08:54:58.580 |  | ←enobeB PCAP frame← TCP |  |  |
238 | 08:54:58.580 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:736: --- TS 36.579-1 Table 5.3.2.3-2A: Step 7 Download User Profile at http://xcap.cms.mcstaasting.com/org.3gpp.mcdata.user-profile/users/sip:mcdata-userA-id@mcstaasting.com/mcdatauser-profile-49.xml
239 | 08:54:58.591 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
240 | 08:54:58.596 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
241 | 08:54:58.597 |  | ←enobeB PCAP frame← TCP |  |  |
242 | 08:54:58.598 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
243 | 08:54:58.609 | →enobeB PCAP frame→ TCP |  |  |  |
244 | 08:54:58.617 | →enobeB PCAP frame→ TCP |  |  |  |
245 | 08:54:58.649 | →enobeB PCAP frame→ TCP |  |  |  |
246 | 08:54:58.649 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
247 | 08:54:58.652 |  | ←enobeB PCAP frame← TCP |  |  |
248 | 08:54:58.657 | →enobeB PCAP frame→ TCP |  |  |  |
249 | 08:54:58.661 |  | ←enobeB PCAP frame← TCP |  |  |
250 | 08:54:58.689 | →enobeB PCAP frame→ TCP |  |  |  |
251 | 08:54:59.298 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
252 | 08:54:59.298 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
253 | 08:54:59.299 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
254 | 08:54:59.312 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
255 | 08:54:59.329 | →enobeB PCAP frame→ TCP |  |  |  |
256 | 08:54:59.332 |  | ←enobeB PCAP frame← TCP |  |  |
257 | 08:54:59.368 |  |  |  |  | ←SIP 200 OK | P-CSCF
258 | 08:54:59.369 | →enobeB PCAP frame→ TCP |  |  |  |
259 | 08:54:59.369 |  |  |  |  | MIKEY | Media-Server
260 | 08:54:59.372 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
261 | 08:54:59.404 |  | ←enobeB PCAP frame← TCP |  |  |
262 | 08:54:59.405 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
263 | 08:54:59.496 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
264 | 08:54:59.500 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
265 | 08:54:59.529 | →enobeB PCAP frame→ TCP |  |  |  |
266 | 08:54:59.537 |  |  |  |  | →HTTP GET | HTTP-Proxy
267 | 08:54:59.538 | →enobeB PCAP frame→ TCP |  |  |  |
268 | 08:54:59.539 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:741: --- TS 36.579-1 Table 5.3.2.3-2A: Step 9 Download Service Configuration at http://xcap.cms.mcstaasting.com/org.3gpp.mcdata.service-config/global/service-config.xml
269 | 08:54:59.541 |  | ←enobeB PCAP frame← TCP |  |  |
270 | 08:54:59.541 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
271 | 08:54:59.545 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
272 | 08:54:59.569 | →enobeB PCAP frame→ TCP |  |  |  |
273 | 08:54:59.580 |  |  |  |  | XML→ | Media-Server
274 | 08:54:59.581 |  |  |  |  | XML→ | Media-Server
275 | 08:54:59.584 |  |  |  |  | ←XML | Media-Server
276 | 08:54:59.587 |  |  |  |  | ←SIP NOTIFY | P-CSCF
277 | 08:54:59.591 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:40250;transp... |  |  |
278 | 08:54:59.616 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
279 | 08:54:59.620 |  | ←enobeB PCAP frame← TCP |  |  |
280 | 08:54:59.627 |  | ←enobeB PCAP frame← TCP |  |  |
281 | 08:54:59.627 |  |  |  |  | →SIP 200 OK | P-CSCF
282 | 08:54:59.977 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
283 | 08:54:59.978 | →enobeB PCAP frame→ SIP MIKEY: PUBLISH sip:mcdata-server-A@mcstaasting.com SIP/2.... SIP over IPSEC: PUBLISH sip:mcdata-server-A@mcstaasting.com SIP/2.... |  |  |  |
284 | 08:54:59.990 |  |  |  |  | →SIP PUBLISH | P-CSCF
285 | 08:55:00.004 |  |  |  |  | MIKEY | Media-Server
286 | 08:55:00.049 | →enobeB PCAP frame→ TCP |  |  |  |
287 | 08:55:00.052 |  | ←enobeB PCAP frame← TCP |  |  |
288 | 08:55:00.089 | →enobeB PCAP frame→ TCP |  |  |  |
289 | 08:55:00.097 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
290 | 08:55:00.100 |  | ←enobeB PCAP frame← TCP |  |  |
291 | 08:55:00.101 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
292 | 08:55:00.129 | →enobeB PCAP frame→ TCP |  |  |  |
293 | 08:55:00.176 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:640: Client connected to Http Proxy port (id 25)
294 | 08:55:00.177 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
295 | 08:55:00.180 |  | ←enobeB PCAP frame← TLS: Mix Info |  |  |
296 | 08:55:00.203 |  |  |  |  | XML→ | Media-Server
297 | 08:55:00.207 |  |  |  |  | ←SIP 200 OK | P-CSCF
298 | 08:55:00.211 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
299 | 08:55:00.260 | →enobeB PCAP frame→ HTTPS: GET http://xcap.gms.mcstaasting.com/org.openmobile... |  |  |  |
300 | 08:55:00.260 |  |  |  |  | →HTTP GET | HTTP-Proxy
301 | 08:55:00.262 |  |  |  |  | Info: MCX_HTTP_CommonFunctions.ttcn:746: --- TS 36.579-1 Table 5.3.2.3-2B: Step 5 Download Group Configuration at http://xcap.gms.mcstaasting.com/org.openmobilealliance.groups/global/byGroupID/sip:groupA@group.mcstaasting.com
302 | 08:55:00.263 |  | ←enobeB PCAP frame← TCP |  |  |
303 | 08:55:00.268 |  |  |  |  | ←HTTP 200 OK | HTTP-Proxy
304 | 08:55:00.272 |  | ←enobeB PCAP frame← HTTPS: HTTP/1.1 200 OK |  |  |
305 | 08:55:00.329 | →enobeB PCAP frame→ TCP |  |  |  |
306 | 08:55:00.336 |  |  |  |  | Info: TitanAdaptor_Main.ttcn:687: Http Proxy port - Client closed the connection (id 25)
307 | 08:55:00.337 | →enobeB PCAP frame→ TLS: Mix Info |  |  |  |
308 | 08:55:00.340 |  | ←enobeB PCAP frame← TCP |  |  |
309 | 08:55:00.369 | →enobeB PCAP frame→ TCP |  |  |  |
310 | 08:55:00.458 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
311 | 08:55:00.459 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
312 | 08:55:00.460 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
313 | 08:55:00.462 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
314 | 08:55:00.463 | →enobeB PCAP frame→ IP DATA: Info IPv4 |  |  |  |
315 | 08:55:00.464 | →enobeB PCAP frame→ SIP MIKEY: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... SIP over IPSEC: SUBSCRIBE sip:subscription-proxy.gms.mcstaasting.c... |  |  |  |
316 | 08:55:00.476 |  |  |  |  | →SIP SUBSCRIBE | P-CSCF
317 | 08:55:00.523 |  |  |  |  | ←SIP 200 OK | P-CSCF
318 | 08:55:00.524 |  |  |  |  | MIKEY | Media-Server
319 | 08:55:00.528 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 200 OK |  |  |
320 | 08:55:00.740 |  |  |  |  | XML→ | Media-Server
321 | 08:55:00.741 |  |  |  |  | XML→ | Media-Server
322 | 08:55:00.743 |  |  |  |  | Protected MCData Message | -
323 | 08:55:00.775 |  |  |  |  | ←XML | Media-Server
324 | 08:55:00.780 |  |  |  |  | ←SIP NOTIFY | P-CSCF
325 | 08:55:00.784 |  | ←enobeB PCAP frame← SIP over IPSEC: NOTIFY sip:PublicUserId-A@192.168.3.2:40250;transp... |  |  |
326 | 08:55:00.816 |  |  |  |  | →SIP 200 OK | P-CSCF
327 | 08:55:00.817 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
328 | 08:55:00.885 |  |  |  |  | ←XML | Media-Server
329 | 08:55:00.906 |  |  |  |  | ←SIP MESSAGE | P-CSCF
330 | 08:55:00.910 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcptt-signed+xml |  |  |
331 | 08:55:01.697 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
332 | 08:55:01.698 |  |  |  |  | →SIP 200 OK | P-CSCF
333 | 08:55:03.707 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
334 | 08:55:03.763 |  | ←RRC DCCH RRC Connection Release |  |  |
335 | 08:55:03.764 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
336 | 08:55:03.792 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
337 | 08:55:03.794 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
338 | 08:55:03.796 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
339 | 08:55:03.797 |  |  |  |  | Info: MCData_SDS_MCX_IMS.ttcn:399: Test-Body Step 1 - 1B
340 | 08:55:03.799 |  |  |  |  | ←XML | Media-Server
341 | 08:55:03.814 |  |  |  |  | MCData Message | -
342 | 08:55:03.814 |  |  |  |  | Protected MCData Message | -
343 | 08:55:03.814 |  |  |  |  | MCData Message | -
344 | 08:55:03.815 |  |  |  |  | Protected MCData Message | -
345 | 08:55:03.836 |  |  |  |  | ←SIP MESSAGE | P-CSCF
346 | 08:55:04.176 |  | ←enobeB PCAP frame← LTE RRC PCCH Paging (1 PagingRecord) |  |  |
347 | 08:55:04.176 |  | ←RRC PCCH Paging |  |  |
348 | 08:55:04.216 | →enobeB PCAP frame→ LTE RRC UL_CCCH RRCConnectionRequest |  |  |  |
349 | 08:55:04.216 |  | →RRC CCCH RRC Connection Request |  |  |
350 | 08:55:04.216 |  | ←RRC CCCH RRC Connection Setup |  |  |
351 | 08:55:04.216 |  | ←enobeB PCAP frame← LTE RRC DL_CCCH RRCConnectionSetup |  |  |
352 | 08:55:04.273 | →enobeB PCAP frame→ LTE RRC UL_DCCH/NAS-EPS RRCConnectionSetupComplete Service request |  |  |  |
353 | 08:55:04.273 |  | →RRC DCCH RRC Connection Setup Complete |  |  |
354 | 08:55:04.273 |  | [EMBEDDED NAS IN PREV RRC] EMM Service request |  |  |
355 | 08:55:04.273 |  |  |  | →NAS EMM Service request |  |
356 | 08:55:04.273 |  |  |  | NAS K-enb fb63e9e7b933556ae328bc7b49f1e8721... |  |
357 | 08:55:04.274 |  |  | RRC K-enb fb63e9e7b933556ae328bc7b49f1e8721... |  |  |
358 | 08:55:04.275 |  |  | RRC rrc-cip 57c08235ba32a624bce6435ac7cfdbe... |  |  |
359 | 08:55:04.275 |  |  | RRC rrc-int 8aa668238d65c895af596156484fb3f... |  |  |
360 | 08:55:04.275 |  |  | RRC up-cip a9487493e16e1db18542adae6e4cd69a... |  |  |
361 | 08:55:04.275 |  |  | RRC up-int 972d19d11adfdc65d920f3abdc4767b6... |  |  |
362 | 08:55:04.275 |  | ←RRC DCCH Security Mode Command |  |  |
363 | 08:55:04.275 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH SecurityModeCommand |  |  |
364 | 08:55:04.329 | →enobeB PCAP frame→ LTE RRC UL_DCCH SecurityModeComplete |  |  |  |
365 | 08:55:04.329 |  | →RRC DCCH Security Mode Complete |  |  |
366 | 08:55:04.329 |  | ←RRC DCCH RRC Connection Reconfiguration |  |  |
367 | 08:55:04.329 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionReconfiguration |  |  |
368 | 08:55:04.369 | →enobeB PCAP frame→ LTE RRC UL_DCCH RRCConnectionReconfigurationComplete |  |  |  |
369 | 08:55:04.369 |  | →RRC DCCH RRC Connection Reconfiguration Com... |  |  |
370 | 08:55:04.371 |  | ←enobeB PCAP frame← IP DATA: Info IPv4 |  |  |
371 | 08:55:04.372 |  | ←enobeB PCAP frame← SIP over IPSEC: MESSAGE sip:PublicUserId-A@mcstaasting.com SIP/2.0... SIP XML: application/vnd.3gpp.mcdata-payload |  |  |
372 | 08:55:04.497 | →enobeB PCAP frame→ SIP over IPSEC: SIP/2.0 200 OK |  |  |  |
373 | 08:55:04.497 |  |  |  |  | →SIP 200 OK | P-CSCF
374 | 08:55:04.505 |  |  |  |  | Verdict PASS: MCData_SDS_MCX_IMS.ttcn:402: Step 1 Verdict: Pass
375 | 08:55:04.505 |  |  |  |  | Info: MCData_SDS_MCX_IMS.ttcn:406: Test-Body Step 3
376 | 08:55:04.568 |  |  |  |  | →SIP MESSAGE | P-CSCF
377 | 08:55:04.596 |  |  |  |  | ←SIP 202 Accepted | P-CSCF
378 | 08:55:04.598 |  |  |  |  | XML→ | Media-Server
379 | 08:55:04.600 |  | ←enobeB PCAP frame← SIP over IPSEC: SIP/2.0 202 Accepted |  |  |
380 | 08:55:04.603 |  |  |  |  | XML→ | Media-Server
381 | 08:55:04.612 |  |  |  |  | Info: MCData_MCDataMessages.ttcn:734: MIME part application/vnd.3gpp.mcdata-signalling 450062F35648000000000001BBADB23CFEAEB83611F5379469251E9C2ECDE33D7800380251DD6885FD7677B186DCC786C0DEDADA984D02A3A00FCCCB69BEAEA4617959CC1DDDBCBC5A070579305A3A275D61B84319C8EF88195B6F
382 | 08:55:04.612 |  |  |  |  | Protected MCData Message | -
383 | 08:55:04.613 |  |  |  |  | Info: MCData_MCDataMessages.ttcn:617: Decrypted payload: 05020062F356480101010101010101010101010101010101010101010101010101010101010101
384 | 08:55:04.613 |  |  |  |  | MCData Message | -
385 | 08:55:04.613 |  |  |  |  | Verdict PASS: MCData_SDS_MCX_IMS.ttcn:410: Step 3 Verdict: Pass
386 | 08:55:06.616 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
387 | 08:55:06.673 |  | ←RRC DCCH RRC Connection Release |  |  |
388 | 08:55:06.674 |  | ←enobeB PCAP frame← LTE RRC DL_DCCH RRCConnectionRelease [cause=other] |  |  |
389 | 08:55:06.695 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
390 | 08:55:06.696 |  |  |  |  | Info: MCData_SDS_MCX_IMS.ttcn:416: Test-Body Step 5
391 | 08:55:07.447 |  |  |  |  | IPCAN-Config-Req → | IPCAN-Ctrl
392 | 08:55:07.450 |  |  |  |  | IPCAN-Config-Cnf ← | IPCAN-Ctrl
393 | 08:55:08.197 |  |  |  |  | Verdict PASS: Final verdict PASS

##### Description of the logs

- 1.- This webpage provides a graphical representation of combined information from different sources in the IPCAN model including a) enodeB, b) MME (RRC/NAS), c) pre-processed traces in the Uu interface -enodeB- (including deciphering of PDCP, NAS, IPSEC and TLS) and d) logs from different SS components. All the information is extracted from the included .json consolidated log file.
- 2.- Just first 5 SIB messages are included to avoid huge logs (traces from enodeB are filtered out completely from the processed pcap).
- 3.- The webpage was designed as static HTML standalone page to avoid the need for a backend/frontend but still allows syntax highlighting and basic filtering functions. By default SS logs and enodeB/mme are displayed only. Mark the checks in the upper part to show or hide the associated message types. Additionally, by clicking on any message and the content is displayed on a right panel with syntax highlighted. Every message can also be displayed in a separate tab/window. If you experience any GUI and scrolling issues try to zoom in/out (better usability proven in Mozilla Firefox and Google Chrome).
- 4.- NAS EEA2 ciphered messages are dumped in clear text in the MME and ciphered when transported in RRC in the enodeB (both are displayed). Furthermore, builtin pcap dissection in the webpage includes MCS TaaSting EEA2 NAS deciphering Wireshark dissector to include also the clear text NAS message later re-processed by Wireshark itself.
- 5.- The inherent complexity behind merging different information sources with different time sources with different granularity (SS and Uu traces microsec and enodeB and MME milisecond) may lead to some apparent packet disordering when several messages overlap in the same ms (i.e. packet arriving at SS before pcap frame in the uplink depicted). A tailored post-processing logic has been developed in the MCS TaaSting log processing engine to avoid as much as possible this overlapping issues. However, some disorder may still appear, please check carefully the timestamp to identify possible disordering problems. They are anyway safe to ignore.