MSG #54 2022-08-10 08:54:17.497
NAS

     ESM: ESM information response
    Protocol discriminator = 0x7 (EPS Mobility Management)
    Security header = 0x2 (Integrity protected and ciphered)
    Auth code = 0x2954b31a
    Sequence number = 0x01
    Protocol discriminator = 0x2 (EPS Session Management)
    EPS bearer identity = 0
    Procedure transaction identity = 1
    Message type = 0xda (ESM information response)
    Access point name = "MCSTaastingDefault"
    Protocol configuration options:
      Ext = 1
      Configuration protocol = 0
      Protocol ID = 0xc223 (CHAP)
      Data = 01 00 00 16 10 f4 17 90 90 f4 17 90 90 f4 17 90 90 f4 17 90 90 2a
      Protocol ID = 0xc223 (CHAP)
      Data = 02 00 00 16 10 ed 66 d3 b5 a2 2e 58 3a 4b be 96 2c 15 47 b8 6e 2a
      Protocol ID = 0x8021 (IPCP)
      Data = 01 00 00 10 81 06 00 00 00 00 83 06 00 00 00 00
      Protocol ID = 0x000d (DNS Server IPv4 Address Request)
      Data =
      Protocol ID = 0x0003 (DNS Server IPv6 Address Request)
      Data =
      Protocol ID = 0x000a (IP address allocation via NAS signalling)
      Data =
      Protocol ID = 0x0005 (MS Support of Network Requested Bearer Control indicator)
      Data =
      Protocol ID = 0x0011 (MS support of Local address in TFT indicator)
      Data =