#######################################################################

# Anritsu Generated PICS/PIXIT file

#

# Changes Applied: 3GPP_TS_34.123-3_AND_TestSequence-1921141576_AND_Test-1921141576/9_AND_TestSequence-1921141576_AND_Test-1921141576/9

#######################################################################

pc_1xCSfallback,                             BOOLEAN,       false   #-- @desc  Support of 1xCS fallback #-- @spec 36.523-2, A.4.2.1.1-1/3

pc_1xRTT,                                    BOOLEAN,       false   #-- @desc  UE supports CDMA2000 1xRTT band class #-- @spec 36.523-2, A.4.1-1/4

pc_4C_DBCC12,                                BOOLEAN,       FALSE   #-- @desc  Setting this ICS means that Dual band carrier combination (12) is supported for one or more of the supported 4C-HSDPA Dual band combinations (A-B) in table A.18a.0a.This ICS is set to true if UE supports Dual band Carrier Combination (12) (22) or ( #-- @spec 34.123-2 Table A.18a/53

pc_4C_DBCC22,                                BOOLEAN,       FALSE   #-- @desc  Setting this ICS means that Dual band carrier combination (22) is supported for one or more of the supported 4C-HSDPA Dual band combinations (A-B) in table A.18a.0a. #-- @spec 34.123-2 Table A.18a/57

pc_4C_DBCC31,                                BOOLEAN,       FALSE   #-- @desc  Setting this ICS means that Dual band carrier combination (31) is supported for one or more of the supported 4C-HSDPA Dual band combinations (A-B) in table A.18a.0a. #-- @spec 34.123-2 Table A.18a/55

pc_4Layer_spatial_muxDL,                     BOOLEAN,       false   #-- @desc  Support of 4 layer spatial multiplexing in DL #-- @spec 36.523-2 A.4.4-1/yy1

pc_4Layer_spatial_mux_tm3_tm4,               BOOLEAN,       false   #-- @desc  Support of 4 layer spatial multiplexing with transmission mode 3 and transmission mode 4 #-- @spec 36.523-2 A.4.4-1/159

pc_5GCN,                                     BOOLEAN,       false   #-- @desc  UE supports 5GS Core #-- @spec 38.508-2 Table A.4.1-5/1

pc_5GS_IMS_eCall_CEN17184,                   BOOLEAN,       false   #-- @desc  UE subjected to national regulations in CEN EN 17184:2024 [100] for IMS eCall over 5GS #-- @spec 34.229-2 A.12/68

pc_5GS_IMS_eCall_Capable,                    BOOLEAN,       false   #-- @desc  UE supports IMS eCall type of emergency services over 5GS #-- @spec 34.229-2 Table A.12/63

pc_5GS_IMS_eCall_Only,                       BOOLEAN,       false   #-- @desc  UE supports IMS eCall Only type of emergency services over 5GS #-- @spec 34.229-2 Table A.12/64

pc_A5_4_CS,                                  BOOLEAN,       false   #-- @desc  Support of A54 #-- @spec 51.010-2, A.2/87

pc_APN_Default_Configuration,                ENUM-APN_DefaultConfiguration_Type,None    #-- @desc  The DNNAPN configuration specified in TS 38.508-1 [2] Table 4.8.4-1 which is to be used for the default DNNAPN. #-- @spec 38.508-1, Table 4.8.4-1

pc_APN_ID_C2,                                CHARSTRING,            #-- @desc  APNDNN ID of type UAS C2 #-- @spec 38.508-2, Table A.4.4-2A

pc_APN_ID_Ethernet,                          CHARSTRING,            #-- @desc  APNDNN ID of type Ethernet #-- @spec 

pc_APN_ID_IMS,                               CHARSTRING,            #-- @desc  APNDNN ID of type IMS #-- @spec 38.508-1, Table 4.8.4-1

pc_APN_ID_Internet,                          CHARSTRING,            #-- @desc  APNDNN ID of type Internet #-- @spec 38.508-1, Table 4.8.4-1

pc_APN_ID_MCX,                               CHARSTRING,    false   #-- @desc  APN/DNN ID of type MCX The APN/DNN Network Identifier portion of the Access Point / Data Network Name, as defined in TS 23.003 [26], subclause 9.1 OR "none" if the UE will not establish PDN/PDU of type MCX If the provided value is different to "none" then for this APN/DNN the DNN/APN configuration of type "MCX" as specified in TS 38.508-1 [2], Table 4.8.4-3 applies. #-- @spec 38.508-2, Table A.4.4-2A

pc_APN_ID_MIOT,                              CHARSTRING,            #-- @desc  APNDNN ID of type MIOT #-- @spec 38.508-1, Table 4.8.4-2A

pc_APN_ID_URLLC,                             CHARSTRING,            #-- @desc  APNDNN ID of type URLLC #-- @spec 38.508-1, Table 4.8.4-2A

pc_APN_ID_USS,                               CHARSTRING,            #-- @desc  APNDNN ID of type UAS USS #-- @spec 38.508-2, Table A.4.4-2A

pc_APN_ID_V2X,                               CHARSTRING,            #-- @desc  APNDNN ID of type V2X #-- @spec 38.508-1, Table 4.8.4-2A

pc_APN_RateControl,                          BOOLEAN,       false   #-- @desc  The UE supports APN rate control #-- @spec 36.523-2 A.4.4-2/Z5

pc_A_BDS,                                    BOOLEAN,       false   #-- @desc  Support for A-BDS #-- @spec 37.571-3 Table A.4.3-2/18

pc_A_GLONASS,                                BOOLEAN,       false   #-- @desc  Support for A-GLONASS #-- @spec 37.571-3 Table A.4.3-2/7

pc_A_GPS_ADR,                                BOOLEAN,       false   #-- @desc  Support of ADR measurement reporting for Gps #-- @spec 37.571-3 Table A.4.3-6/1

pc_A_GPS_ADR_ENH,                            BOOLEAN,       false   #-- @desc  Support of ADR enhancements for Gps #-- @spec 37.571-3 Table A.4.3-6/13

pc_A_GPS_HA,                                 BOOLEAN,       false   #-- @desc  Support of High accuracy GNSS modes for Gps #-- @spec 37.571-3 Table A.4.3-6/19

pc_A_GPS_L1C,                                BOOLEAN,       false   #-- @desc  Support of A-GPS L1C signal #-- @spec 37.571-3 Table A.4.3-5/1

pc_A_GPS_L1C_A,                              BOOLEAN,       false   #-- @desc  Support for A-GPS L1CA #-- @spec 37.571-3 Table A.4.3-2/6

pc_A_GPS_L1C_A_MGPS,                         BOOLEAN,       false   #-- @desc  Support for A-GPS L1CA and Modernized GPS #-- @spec 37.571-3 Table A.4.3-2/8

pc_A_GPS_L2C,                                BOOLEAN,       false   #-- @desc  Support of A-GPS L2C signal #-- @spec 37.571-3 Table A.4.3-5/2

pc_A_GPS_L5,                                 BOOLEAN,       false   #-- @desc  Support of A-GPS L5 signal #-- @spec 37.571-3 Table A.4.3-5/3

pc_A_GPS_VelocityMeas,                       BOOLEAN,       false   #-- @desc  Support of Velocity measurement reporting for Gps #-- @spec 37.571-3 Table A.4.3-6/6

pc_A_Galileo,                                BOOLEAN,       false   #-- @desc  Support for A-Galileo #-- @spec 37.571-3 Table A.4.3-2/9

pc_A_QZSS,                                   BOOLEAN,       false   #-- @desc  Support of A-QZSS #-- @spec 37.571-3 Table A.4.3-2/14

pc_A_SBAS,                                   BOOLEAN,       false   #-- @desc  Support of A-SBAS #-- @spec 37.571-3 Table A.4.3-2/13

pc_Additional_APN_RateControl,               BOOLEAN,       false   #-- @desc  The UE supports additional APN rate control for exception data reporting #-- @spec 36.523-2 A.4.4-2/30

pc_Allowed_CSG_list,                         BOOLEAN,       false   #-- @desc  Support of Allowed CSG list #-- @spec 36.523-2 A.4.4-1/2

pc_Attach,                                   BOOLEAN,       FALSE   #-- @desc  Support EPS attach (with or without pre-configuration) #-- @spec 36.523-2 A.4.4-2/1

pc_AttachWithIMSI,                           BOOLEAN,       false   #-- @desc  Support of Attach With IMSI #-- @spec 34.123-2 A.10/34

pc_AttachWithPDN,                            BOOLEAN,       false   #-- @desc  Support of EMM-REGISTERED with PDN #-- @spec 36.523-2 A.4.4.1-1/X3

pc_AttachWithoutPDN,                         BOOLEAN,       false   #-- @desc  Support of EMM-REGISTERED without PDN #-- @spec 36.523-2 A.4.4.1-1/X2

pc_Auto_Attach_after_TAU_Reject,             BOOLEAN,       false   #-- @desc  Support of automatic re-activation of the EPS bearer(s) after the TAU Reject #-- @spec 

pc_Auto_PDN_Connectivity,                    BOOLEAN,       false   #-- @desc  Support of automatic PDN Connectivity in EUTRAN #-- @spec 36.523-2 A.4.4-1/68

pc_AutomaticAttachSwitchON,                  BOOLEAN,       true    #-- @desc  Support of automatic PS attach procedure at switch on. #-- @spec 34.123-2 A.20/38

pc_AutomaticHRPD_PDN_Connection,             BOOLEAN,       true    #-- @desc  Support of automatic PDN connection trigger on HRPD cell #-- @spec X.s0057, 6.4.1

pc_Automatic_EPS_Re_Attach,                  BOOLEAN,       false   #-- @desc  Support of automatic re-activation of the EPS bearer(s) #-- @spec 36.523-2 A.4.4-1/64

pc_Automatic_Re_Attach,                      BOOLEAN,       false   #-- @desc  Support of automatic re-activation of the EPS bearer(s) during Network Initiated Detach with detach type set to re-attach required #-- @spec 36.523-2 A.4.4-1/27

pc_Available_PLMNs_AcT_Ind,                  BOOLEAN,       false   #-- @desc  Support of AccessTechnology indication in available PLMNs list #-- @spec 36.523-2 A.4.4-1/78

pc_B41_UE_PC2,                               BOOLEAN,       false   #-- @desc  Support of TDD Band 41 Power class 2 operation #-- @spec 36.523-2 A.4.4-1/abc

pc_BDS,                                      BOOLEAN,       false   #-- @desc  Support for BDS #-- @spec 37.571-3 Table A.4.3-1/13

pc_BDS2_Only,                                BOOLEAN,       false   #-- @desc  Support for BDS-2 Only #-- @spec 37.571-3 Table A.4.3-2/52

pc_BDS_ADR,                                  BOOLEAN,       false   #-- @desc  Support of ADR measurement reporting for BDS #-- @spec 37.571-3 Table A.4.3-6/11

pc_BDS_ADR_ENH,                              BOOLEAN,       false   #-- @desc  Support of ADR enhancements for BDS #-- @spec 37.571-3 Table A.4.3-6/18

pc_BDS_B1C,                                  BOOLEAN,       false   #-- @desc  Support for A-BDS B1C #-- @spec 37.571-3 Table A.4.3-5/17

pc_BDS_B1I,                                  BOOLEAN,       false   #-- @desc  Support for A-BDS B1I #-- @spec 37.571-3 Table A.4.3-5/16

pc_BDS_B2a,                                  BOOLEAN,       false   #-- @desc  Support of B2a signal in BDS #-- @spec 37.571-3 Table A.4.3-5/18

pc_BDS_B3I,                                  BOOLEAN,       false   #-- @desc  Support of B3I signal in BDS #-- @spec 37.571-3 Table A.4.3-5/19

pc_BDS_DiffCorr,                             BOOLEAN,       false   #-- @desc  Gnss-AuxiliaryInformationSupport for BDS #-- @spec 37.571-3 Table A.4.3-7/59

pc_BDS_GridMod,                              BOOLEAN,       false   #-- @desc  Gnss-AuxiliaryInformationSupport for BDS #-- @spec 37.571-3 Table A.4.3-7/60

pc_BDS_HA,                                   BOOLEAN,       false   #-- @desc  Support of High accuracy GNSS modes for BDS #-- @spec 37.571-3 Table A.4.3-6/24

pc_BDS_VelocityMeas,                         BOOLEAN,       false   #-- @desc  Support of Velocity measurement reporting for BDS #-- @spec 37.571-3 Table A.4.3-6/12

pc_BI_UG,                                    BOOLEAN,       false   #--  #-- @spec 

pc_BSRVCC,                                   BOOLEAN,       false   #-- @desc  UE indicates g.3gpp.ps2cs-srvcc-orig-pre-alerting media feature tag in INVITE request #-- @spec 34.229-2 A.12/36

pc_Background,                               BOOLEAN,       false   #-- @desc  UE Supports Background QoS class #-- @spec 34.123-2 A.6/4

pc_Band10_Supp,                              BOOLEAN,       false   #-- @desc  UE supports Frequency Band 10 #-- @spec 34.123-2 A.15/22

pc_Band11_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 11 #-- @spec 34.123-2 Table A.15/23

pc_Band12_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 12 #-- @spec 34.123-2 Table A.15/24

pc_Band13_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 13 #-- @spec 34.123-2 Table A.15/25

pc_Band14_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 14 #-- @spec 34.123-2 Table A.15/26

pc_Band19_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 19 #-- @spec 34.123-2 Table A.15/27

pc_Band1_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 1 #-- @spec 34.123-2 A.15/2

pc_Band20_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 20 #-- @spec 34.123-2 Table A.15/30

pc_Band21_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 21 #-- @spec 34.123-2 Table A.15/28

pc_Band22_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 22 #-- @spec 34.123-2 Table A.15/29

pc_Band25_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 25 #-- @spec 34.123-2 Table A.15/31

pc_Band26_Supp,                              BOOLEAN,       false   #-- @desc  TRUE if UE supports Frequency Band 26 #-- @spec 34.123-2 Table A.15/32

pc_Band2_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 2 #-- @spec 34.123-2 A.15/3

pc_Band32_Supp,                              BOOLEAN,       false   #-- @desc  UE supports Frequency Band 32 #-- @spec 34.123-2 A.15/33

pc_Band3_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 3 #-- @spec 34.123-2 A.15/14

pc_Band4_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 4 #-- @spec 34.123-2 A.15/15

pc_Band5_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 5 #-- @spec 34.123-2 A.15/16

pc_Band6_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 6 #-- @spec 34.123-2 A.15/17

pc_Band7_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 7 #-- @spec 34.123-2 A.15/18

pc_Band8_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 8 #-- @spec 34.123-2 A.15/19

pc_Band9_Supp,                               BOOLEAN,       false   #-- @desc  UE supports Frequency Band 9 #-- @spec 34.123-2 A.15/20

pc_Bds_DiffCorr_B1C,                         BOOLEAN,       false   #-- @desc  Bds-DifferentialCorrectionsSupport for B1C #-- @spec 37.571-3 Table A.4.3-7/103

pc_BidirecVoiceOverIMS,                      BOOLEAN,       false   #-- @desc  UE capable of initiating a bidirectional voice session over IMS #-- @spec 34.229-2 Table A.12/12

pc_Bluetooth,                                BOOLEAN,       false   #-- @desc  Support for UE-Assisted Bluetooth #-- @spec 37.571-3 Table A.4.3-2/22

pc_CE_Measurements,                          BOOLEAN,       false   #-- @desc  Support of intra-frequency RSRQ measurements and inter-frequency RSRP and RSRQ measurements in RRC_CONNECTED #-- @spec 36.523-2 A.4.4-1A/16

pc_CEmodeA,                                  BOOLEAN,       false   #-- @desc  Support of CE mode A #-- @spec 36.523-2 A.4.4-1/122

pc_CEmodeB,                                  BOOLEAN,       false   #-- @desc  Support of CE mode B #-- @spec 36.523-2 A.4.4-1/123

pc_CMAS_Message,                             BOOLEAN,       false   #-- @desc  Support of CMAS message #-- @spec 36.523-2 A.4.4-1/58

pc_CRS_Interference_Handling,                BOOLEAN,       false   #-- @desc  Support of CRS interference handling #-- @spec 36.523-2 A.4.4-1A/7

pc_CS,                                       BOOLEAN,       false   #-- @desc  UE supports CS domain services #-- @spec 34.123-2 A.3/1

pc_CSI_RS_DS_Meas,                           BOOLEAN,       false   #-- @desc  Support of CSI-RS based discovery signals measurement #-- @spec 36.523-2 A.4.4.1/118

pc_CS_Em_Call_in_1xRTT,                      BOOLEAN,       false   #-- @desc  Support for establishing the emergency call using the CS domain in 1xRTT #-- @spec 36.523-2 A.4.4-1/37

pc_CS_Em_Call_in_GERAN,                      BOOLEAN,       false   #-- @desc  Support for establishing the emergency call using the CS domain in GERAN #-- @spec 36.523-2 A.4.4-1/36

pc_CS_Em_Call_in_UTRA,                       BOOLEAN,       false   #-- @desc  Support for establishing the emergency call using the CS domain in UTRA #-- @spec 36.523-2 A.4.4-1/35

pc_CS_Fallback,                              BOOLEAN,       false   #-- @desc  The UE supports CS fallback for voice calls. If true pc_CS and at least one of pc_FDD pc_TDD_HCR pc_TDD_LCR pc_TDD_VHCR or pc_UMTS_GSM is also true. #-- @spec 36.523-2, A.4.2.1.1-1/1

pc_CS_MO_LR_CSFallback,                      BOOLEAN,       false   #-- @desc  Support for CS-MO-LR with CS Fallback for a position estimate #-- @spec 37.571-3 Table A.4.3-3/4

pc_CS_PS_data_centric,                       BOOLEAN,       false   #-- @desc  Support of CSPS mode 2 #-- @spec 36.523-2 A.4.4-2/5

pc_CS_PS_voice_centric,                      BOOLEAN,       false   #-- @desc  Support of configuring the UE to voice centric #-- @spec 36.523-2 A.4.4-2/4

pc_CS_SMS_only,                              BOOLEAN,       false   #-- @desc  The UE supports registration for SMS only.  If true pc_CS_fallback is false and at least one of pc_SMS_SGs_MT and pc_SMS_SGs_MO is true. #-- @spec 

pc_Category_M1_voice,                        BOOLEAN,       false   #-- @desc  Support for GSMA PRD NG.108 "IMS Profile for Voice and SMS for UE Category M1" #-- @spec 36.523-2 A.4.4-1/nnn

pc_Combined_Attach,                          BOOLEAN,       TRUE    #-- @desc  Support combined EPSIMSI attach (with or without pre-configuration) #-- @spec 36.523-2 A.4.4-2/2

pc_CommunicationHold_DuringEmergencyCall,    BOOLEAN,       false   #-- @desc  UE supports Communication Hold during emergency call #-- @spec 34.229-2, Table A.12/33

pc_Concatenated_SMS_IP_MO,                   BOOLEAN,       false   #-- @desc  Concatenated SM-over-IP sender #-- @spec 34.229-2 Table A.3A/64

pc_Concatenated_SMS_IP_MT,                   BOOLEAN,       false   #-- @desc  Concatenated SM-over-IP receiver #-- @spec 34.229-2 Table A.3A/65

pc_Control_Plane_CIoT_Optimisation,          BOOLEAN,       false   #-- @desc  Support of Control Plane CIoT #-- @spec 36.523-2 A.4.4-1/nnn

pc_Conversational,                           BOOLEAN,       FALSE   #-- @desc  Support Conversational #-- @spec 34.123-2 Table A.6/1

pc_DC_SCG_DRB,                               BOOLEAN,       false   #-- @desc  Support of DC SCG DRB #-- @spec 36.523-2 A.4.2.1.1-1/10

pc_DC_Split_DRB,                             BOOLEAN,       false   #-- @desc  Support of DC Split DRB #-- @spec 36.523-2 A.4.2.1.1-1/9

pc_DL_256QAM,                                BOOLEAN,       false   #-- @desc  Support of downlink 256 QAM #-- @spec 36.523-2 A.4.4.1/xxx

pc_DL_AoD_periodicalReporting_UEA,           BOOLEAN,       false   #-- @desc  Support of periodicalReporting in UE-assisted mode #-- @spec 37.571-3 Table A.4.3-6E/7

pc_DL_AoD_periodicalReporting_UEB,           BOOLEAN,       false   #-- @desc  Support of periodicalReporting in UE-based mode #-- @spec 37.571-3 Table A.4.3-6E/6

pc_DL_AoD_periodicalReporting_standalone,    BOOLEAN,       false   #-- @desc  Support of periodicalReporting in standalone mode #-- @spec 37.571-3 Table A.4.3-6E/5

pc_DL_CA_2Carriers,                          BOOLEAN,       false   #-- @desc  DL CA with 2 carriers #-- @spec 36.523-2 A.4.3.3-1/1

pc_DL_CA_3Carriers,                          BOOLEAN,       false   #-- @desc  DL CA with 3 carriers #-- @spec 36.523-2 A.4.3.3-1/2

pc_DL_InterBand_CaBwClassComb_AA,            BOOLEAN,       false   #-- @desc  DL Inter-band contiguous CA BW class A-A #-- @spec 36.523-2 A.4.3.3.3-1/1

pc_DL_InterBand_CaBwclassA,                  BOOLEAN,       false   #-- @desc  DL Inter-band CA BW class A #-- @spec 

pc_DL_InterBand_CaBwclassB,                  BOOLEAN,       false   #-- @desc  DL Inter-band CA BW class B #-- @spec 

pc_DL_InterBand_CaBwclassC,                  BOOLEAN,       false   #-- @desc  DL Inter-band CA BW class C #-- @spec 

pc_DL_IntraBand_ContCaBWclassB,              BOOLEAN,       false   #-- @desc  DL Intra-band contiguous CA BW class B #-- @spec 36.523-2 A.4.3.3.1-1/1

pc_DL_IntraBand_ContCaBWclassC,              BOOLEAN,       false   #-- @desc  DL Intra-band contiguous CA BW class C #-- @spec 36.523-2 A.4.3.3.1-1/2

pc_DL_IntraBand_nonContCaBwClassComb_AA,     BOOLEAN,       false   #-- @desc  Support of DL intra-band non-contiguous CA BW Class Combination A-A #-- @spec 36.523-2 A.4.3.3.2-1/1

pc_DL_PRS_BWA_RRC_Connected_DL_TDOA,         BOOLEAN,       false   #-- @desc  Support DL-PRS bandwidth aggregation in RRC_CONNECTED for DL-TDOA positioning method #-- @spec 37.571-3 Table A.4.3-6F/13

pc_DL_PRS_BWA_RRC_Connected_Multi_RTT,       BOOLEAN,       false   #-- @desc  Support DL-PRS bandwidth aggregation in RRC_CONNECTED for Multi-RTT positioning method #-- @spec 37.571-3 Table A.4.3-6C/13

pc_DL_PRS_RSRP_MeasFR1,                      BOOLEAN,       false   #-- @desc  Support of DL-PRS-RSRP-MeasFR1 #-- @spec 37.571-3 Table A.4.3-6F/3

pc_DL_PRS_RSRP_MeasFR2,                      BOOLEAN,       false   #-- @desc  Support of DL-PRS-RSRP-MeasFR2 #-- @spec 37.571-3 Table A.4.3-6F/4

pc_DL_TC_FDD,                                BOOLEAN,       TRUE    #-- @desc  Support for turbo decoding for downlink - FDD #-- @spec 34.123-2 Table A.18a/1

pc_DL_TC_TDD,                                BOOLEAN,       FALSE   #-- @desc  Support for turbo decoding for downlink - TDD #-- @spec 34.123-2 Table A.18b/1

pc_DL_TDOA_additionalPathsReport,            BOOLEAN,       false   #-- @desc  Support of additionalPathsReport #-- @spec 37.571-3 Table A.4.3-6F/5

pc_DL_TDOA_periodicalReporting_UEA,          BOOLEAN,       false   #-- @desc  Support of periodicalReporting in UE-assisted mode #-- @spec 37.571-3 Table A.4.3-6F/8

pc_DL_TDOA_periodicalReporting_UEB,          BOOLEAN,       false   #-- @desc  Support of periodicalReporting in UE-based mode #-- @spec 37.571-3 Table A.4.3-6F/7

pc_DL_TDOA_periodicalReporting_standalone,   BOOLEAN,       false   #-- @desc  Support of periodicalReporting in standalone mode #-- @spec 37.571-3 Table A.4.3-6F/6

pc_DSMIPv6,                                  BOOLEAN,       false   #-- @desc  Support of Mobility management based on Dual-Stack Mobile IPv6 #-- @spec 36.523-2 A.4.4-1/6

pc_DaylightSavingTime,                       BOOLEAN,       false   #-- @desc  UE storesupdates the daylight saving time when receives information #-- @spec 36.523-2 A.4.4-1/93

pc_DualRM_Coding,                            BOOLEAN,       false   #-- @desc  Dual RM Coding #-- @spec 36.523/2 ????

pc_Dynamic_GERAN_Rel_downgrade,              BOOLEAN,       false   #-- @desc  Dynamically downgrades the GERAN release when the support of EPS is disabled #-- @spec 36.523-2, A.4.4-2/XYZ

pc_EAB,                                      BOOLEAN,       false   #-- @desc  Support of Extended Access Barring #-- @spec 36.523-2 A.4.4-1A/4

pc_EAB_override,                             BOOLEAN,       false   #-- @desc  Support of Extended Access Barring Override #-- @spec 36.523-2 A.4.4-1/91

pc_ECID,                                     BOOLEAN,       false   #-- @desc  Support of UE assisted ECID #-- @spec 37.571-3 Table A.4.3-2/5

pc_ECID_Rsrp,                                BOOLEAN,       false   #-- @desc  RSRP Supported #-- @spec 37.571-3 Table A.4.3-4/1

pc_ECID_Rsrq,                                BOOLEAN,       false   #-- @desc  RSRQ Supported #-- @spec 37.571-3 Table A.4.3-4/2

pc_ECID_UeRxTx,                              BOOLEAN,       false   #-- @desc  UE Rx-Tx Time Difference Supported #-- @spec 37.571-3 Table A.4.3-4/3

pc_ECID_idleStateForMeasurements,            BOOLEAN,       false   #-- @desc  Support of idleStateForMeasurements #-- @spec 37.571-3 Table A.4.3-2/7

pc_ECID_onNR,                                BOOLEAN,       false   #-- @desc  Support of UE assisted ECID (based on LTE signals) on NR #-- @spec 37.571-3 Table A.4.3-2/43

pc_ECID_periodicalReporting,                 BOOLEAN,       false   #-- @desc  Support of periodicalReporting #-- @spec 37.571-3 Table A.4.3-4/5

pc_ECID_triggeredReporting,                  BOOLEAN,       false   #-- @desc  Support of triggeredReporting #-- @spec 37.571-3 Table A.4.3-4/6

pc_ECID_ueRxTxSupTDD,                        BOOLEAN,       false   #-- @desc  Support of ueRxTxSupTDD #-- @spec 37.571-3 Table A.4.3-4/4

pc_EDCH_UE_Category_FDD,                     INTEGER,       1       #-- @desc  FDD E-DCH physical layer categories #-- @spec 34.123-2 Table A.18a.2

pc_EDCH_UE_Category_TDD,                     INTEGER,       1       #-- @desc  LCR TDD E-DCH physical layer categories #-- @spec 34.123-2 Table A.18b.2

pc_EDTM,                                     BOOLEAN,       false   #-- @desc  Support for EDTM #-- @spec 36.523-2 A.4.4-1/38

pc_EMM_Information,                          BOOLEAN,       false   #-- @desc  Support of EMM Information message #-- @spec 36.523-2 A.4.4-1/9

pc_EN_DC,                                    BOOLEAN,       false   #-- @desc  EN-DC (Option 3) #-- @spec 38.508-2 Table A.4.1-1/5

pc_EPC_AutomaticAttachSwitchOn,              BOOLEAN,       false   #-- @desc  Support of automatic re-activation oof the EPS bearers during network initiated detach even though UE has initiated a detach procedure with detach type set to EPS detach or combined EPSIMSI detach #-- @spec 

pc_EPC_MO_LR_RequestAssistanceData,          BOOLEAN,       false   #-- @desc  Support of EPC-MO-LR request for assistance data #-- @spec 37.571-3 Table A.4.3-3/1

pc_EPC_MO_LR_RequestPositionEstimate,        BOOLEAN,       false   #-- @desc  Support of EPC-MO-LR request for a position estimate #-- @spec 37.571-3 Table A.4.3-3/2

pc_EPC_RACS,                                 BOOLEAN,       false   #-- @desc  Support of RACS #-- @spec 36.523-2 A.4.4-1/III

pc_EPS_Disable,                              BOOLEAN,       false   #-- @desc  Support of disabling of EPS capability #-- @spec 

pc_EPS_IMS_EmergencyCall,                    BOOLEAN,       false   #-- @desc  Support of MS emergency call in EPS #-- @spec 36.523-2, A.4.2.1.1-1/4

pc_EPS_IMS_eCall_CEN17184,                   BOOLEAN,       false   #-- @desc  UE subjected to national regulations in CEN EN 17184:2024 [100] for IMS eCall over EPS #-- @spec 34.229-2 A.12/67

pc_EPS_IMS_eCall_Capable,                    BOOLEAN,       false   #-- @desc  UE supports IMS eCall type of emergency services over EPS #-- @spec 34.229-2 Table A.12/54

pc_EPS_IMS_eCall_Only,                       BOOLEAN,       false   #-- @desc  UE supports IMS eCall Only type of emergency services over EPS #-- @spec 34.229-2 Table A.12/55

pc_EPS_Services_Disable,                     BOOLEAN,       false   #-- @desc  Support of disabling of EPS services #-- @spec 36.523-2 A.4.4-1/26

pc_EPS_UAS,                                  BOOLEAN,       false   #-- @desc  Support of UAS Services #-- @spec 36.523-2 A.4.4-1/249

pc_EPS_UPIP,                                 BOOLEAN,       false   #-- @desc  Support of user plane integrity protection with EPS #-- @spec 38.508-2 Table A.4.3.7-1/50

pc_ESM_MO_Bearer_Allocation,                 BOOLEAN,       false   #-- @desc  Support of ESM UE requested bearer resource allocation procedure #-- @spec 36.523-2 A.4.4-1/10

pc_ESM_MO_Bearer_Modification,               BOOLEAN,       false   #-- @desc  Support of ESM UE requested bearer resource modification procedure #-- @spec 36.523-2 A.4.4-1/11

pc_ESM_Notification,                         BOOLEAN,       false   #-- @desc  Support of ESM Notification procedure #-- @spec 36.523-2 A.4.4.1-71

pc_ESM_UE_Modification_NW_TFT,               BOOLEAN,       false   #-- @desc  Support for UE requested modification of network allocated TFTs #-- @spec 36.523-2 A.4.4-1/54

pc_ETWS_message,                             BOOLEAN,       false   #-- @desc  Support of ETWS message #-- @spec 36.523-2 A.4.4-1/20

pc_ETWS_message_security,                    BOOLEAN,       false   #-- @desc  Support of ETWS message with security #-- @spec 

pc_EUTRAN_EHC,                               BOOLEAN,       false   #-- @desc UE supports Ethernet header compression and decompression using EHC protocol #-- @spec 36.523-2 A.4.4-1/213

pc_EUTRA_mpspriorityindication_r16,          BOOLEAN,       false   #-- @desc  Support of mpsPriorityIndication on RRC release with redirect #-- @spec 36.523-2 A.4.4-1/yyy

pc_E_UTRAN_2_GERAN_PSHO,                     BOOLEAN,       false   #-- @desc  Support for inter-RAT PS handover from E_UTRAN to GERAN #-- @spec 36.523-2 A.4.4-1/52

pc_E_UTRA_WLAN_offload,                      BOOLEAN,       false   #-- @desc  Support Offload tofrom WLAN and supports S2b #-- @spec 36.523-2 A.4.2.1.1-1/8

pc_EarlyMedia,                               BOOLEAN,       false   #-- @desc  UE supports early media #-- @spec 34.229-2 Table A.12/45

pc_EmergSpeech,                              BOOLEAN,       false   #-- @desc  Emergency Call #-- @spec 34.123-2 A.2/2

pc_Enable_Disable_SMSoverIMS,                BOOLEAN,       false   #-- @desc  UE supports enablingdisabling SMS over IMS #-- @spec 34.229-2 Table A.12/58

pc_Enhanced_1xCSfallback,                    BOOLEAN,       false   #-- @desc  Support of Enhanced 1xCS fallback #-- @spec 36.523-2, A.4.2.1.1-1/6

pc_FDD,                                      BOOLEAN,       false   #-- @desc  UE supports UTRA band as defined in TS 25.101 #-- @spec 34.123-2 A.1/1

pc_FDD_TypeB_HalfDuplex,                     BOOLEAN,       false   #-- @desc  Support of Type B Half duplex FDD operation #-- @spec 36.523-2 A.4.4.1/103

pc_FDPCH,                                    BOOLEAN,       false   #-- @desc  Full support of F-DPCH #-- @spec 34.123-2 Table A.18a/19

pc_Fast_First_HPPLMN_Search,                 BOOLEAN,       false   #-- @desc  Support of Fast First Higher Piority PLMN search #-- @spec 36.523-2 A.4.4-1/xxx

pc_FeatrGrp_1,                               BOOLEAN,       false   #-- @desc  Support of Intra-subframe frequency hopping for PUSCH scheduled by UL grant Extended cyclic prefix with f = 7.5kHz for DL resource block DCI format 3a (TPC commands for PUCCH and PUSCH with single bit power adjustments) Multi-user MIMO for PDSCH Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-0 - UE selected subband CQI without PMI Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2 - UE selected subband CQI with multiple PMI #-- @spec 36.523-2 A.4.5-1/1

pc_FeatrGrp_10,                              BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to GERAN (Packet_)Idle by Cell Change Order EUTRA RRC_CONNECTED to GERAN (Packet_)Idle by Cell Change Order with NACC (Network Assisted Cell Change) #-- @spec 36.523-2 A.4.5-1/10

pc_FeatrGrp_101,                             BOOLEAN,       false   #-- @desc  DMRS with OCC (orthogonal cover code) and SGH (sequence group hopping) disabling #-- @spec 36.523-2 A.4.5-3/1

pc_FeatrGrp_101_F,                           BOOLEAN,       false   #-- @desc  DMRS with OCC (orthogonal cover code) and SGH (sequence group hopping) disabling #-- @spec 36.523-2 A.4.5-3a/1

pc_FeatrGrp_101_T,                           BOOLEAN,       false   #-- @desc  DMRS with OCC (orthogonal cover code) and SGH (sequence group hopping) disabling #-- @spec 36.523-2 A.4.5-3b/1

pc_FeatrGrp_102,                             BOOLEAN,       false   #-- @desc  Trigger type 1 SRS (aperiodic SRS) transmission (Up to X ports) #-- @spec 36.523-2 A.4.5-3/2

pc_FeatrGrp_102_F,                           BOOLEAN,       false   #-- @desc  Trigger type 1 SRS (aperiodic SRS) transmission (Up to X ports) #-- @spec 36.523-2 A.4.5-3a/2

pc_FeatrGrp_102_T,                           BOOLEAN,       false   #-- @desc  Trigger type 1 SRS (aperiodic SRS) transmission (Up to X ports) #-- @spec 36.523-2 A.4.5-3b/2

pc_FeatrGrp_103,                             BOOLEAN,       false   #-- @desc  PDSCH transmission mode 9 when up to 4 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3/3

pc_FeatrGrp_103_F,                           BOOLEAN,       false   #-- @desc  PDSCH transmission mode 9 when up to 4 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3a/3

pc_FeatrGrp_103_T,                           BOOLEAN,       false   #-- @desc  PDSCH transmission mode 9 when up to 4 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3b/3

pc_FeatrGrp_104,                             BOOLEAN,       false   #-- @desc  PDSCH transmission mode 9 for TDD when 8 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3/4

pc_FeatrGrp_104_F,                           BOOLEAN,       false   #-- @desc  PDSCH transmission mode 9 for TDD when 8 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3a/4

pc_FeatrGrp_104_T,                           BOOLEAN,       false   #-- @desc  PDSCH transmission mode 9 for TDD when 8 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3b/4

pc_FeatrGrp_105,                             BOOLEAN,       false   #-- @desc  Periodic CQIPMIRI reporting on PUCCH: Mode 2-0:UE selected subband CQI without PMI when PDSCH transmission mode 9 is configured.Periodic CQIPMIRI reporting on PUCCH: Mode 2-1:UE selected subband CQI with single PMI when PDSCH transmission mode 9 and up to 4 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3/5

pc_FeatrGrp_105_F,                           BOOLEAN,       false   #-- @desc  Periodic CQIPMIRI reporting on PUCCH: Mode 2-0:UE selected subband CQI without PMI when PDSCH transmission mode 9 is configured.Periodic CQIPMIRI reporting on PUCCH: Mode 2-1:UE selected subband CQI with single PMI when PDSCH transmission mode 9 and up to 4 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3a/5

pc_FeatrGrp_105_T,                           BOOLEAN,       false   #-- @desc  Periodic CQIPMIRI reporting on PUCCH: Mode 2-0:UE selected subband CQI without PMI when PDSCH transmission mode 9 is configured.Periodic CQIPMIRI reporting on PUCCH: Mode 2-1:UE selected subband CQI with single PMI when PDSCH transmission mode 9 and up to 4 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3b/5

pc_FeatrGrp_106,                             BOOLEAN,       false   #-- @desc  Periodic CQIPMIRIPTI reporting on PUCCH: Mode 2-1: UE selected subband CQI with single PMI when PDSCH transmission mode 9 and 8 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3/6

pc_FeatrGrp_106_F,                           BOOLEAN,       false   #-- @desc  Periodic CQIPMIRIPTI reporting on PUCCH: Mode 2-1: UE selected subband CQI with single PMI when PDSCH transmission mode 9 and 8 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3a/6

pc_FeatrGrp_106_T,                           BOOLEAN,       false   #-- @desc  Periodic CQIPMIRIPTI reporting on PUCCH: Mode 2-1: UE selected subband CQI with single PMI when PDSCH transmission mode 9 and 8 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3b/6

pc_FeatrGrp_107,                             BOOLEAN,       false   #-- @desc  Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-0: UE selected subband CQI without PMI when PDSCH transmission mode 9 is configured. Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2: UE selected subband CQI with multiple PMI when PDSCH transmission mode 9 and up to 4 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3/7

pc_FeatrGrp_107_F,                           BOOLEAN,       false   #-- @desc  Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-0: UE selected subband CQI without PMI when PDSCH transmission mode 9 is configured. Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2: UE selected subband CQI with multiple PMI when PDSCH transmission mode 9 and up to 4 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3a/7

pc_FeatrGrp_107_T,                           BOOLEAN,       false   #-- @desc  Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-0: UE selected subband CQI without PMI when PDSCH transmission mode 9 is configured. Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2: UE selected subband CQI with multiple PMI when PDSCH transmission mode 9 and up to 4 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3b/7

pc_FeatrGrp_108,                             BOOLEAN,       false   #-- @desc  Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2: UE selected subband CQI with multiple PMI when PDSCH transmission mode 9 and 8 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3/8

pc_FeatrGrp_108_F,                           BOOLEAN,       false   #-- @desc  Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2: UE selected subband CQI with multiple PMI when PDSCH transmission mode 9 and 8 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3a/8

pc_FeatrGrp_108_T,                           BOOLEAN,       false   #-- @desc  Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2: UE selected subband CQI with multiple PMI when PDSCH transmission mode 9 and 8 CSI reference signal ports are configured #-- @spec 36.523-2 A.4.5-3b/8

pc_FeatrGrp_109,                             BOOLEAN,       false   #-- @desc  Periodic CQIPMIRI reporting on PUCCH Mode 1-1 submode 1 #-- @spec 36.523-2 A.4.5-3/9

pc_FeatrGrp_109_F,                           BOOLEAN,       false   #-- @desc  Periodic CQIPMIRI reporting on PUCCH Mode 1-1 submode 1 #-- @spec 36.523-2 A.4.5-3a/9

pc_FeatrGrp_109_T,                           BOOLEAN,       false   #-- @desc  Periodic CQIPMIRI reporting on PUCCH Mode 1-1 submode 1 #-- @spec 36.523-2 A.4.5-3b/9

pc_FeatrGrp_10_F,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to GERAN (Packet_)Idle by Cell Change Order EUTRA RRC_CONNECTED to GERAN (Packet_)Idle by Cell Change Order with NACC (Network Assisted Cell Change) #-- @spec 36.523-2 A.4.5-1a/10

pc_FeatrGrp_10_T,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to GERAN (Packet_)Idle by Cell Change Order EUTRA RRC_CONNECTED to GERAN (Packet_)Idle by Cell Change Order with NACC (Network Assisted Cell Change) #-- @spec 36.523-2 A.4.5-1b/10

pc_FeatrGrp_11,                              BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to 1xRTT CS Active handover #-- @spec 36.523-2 A.4.5-1/11

pc_FeatrGrp_110,                             BOOLEAN,       false   #-- @desc  Periodic CQIPMIRI reporting on PUCCH Mode 1-1 submode 2 #-- @spec 36.523-2 A.4.5-3/10

pc_FeatrGrp_110_F,                           BOOLEAN,       false   #-- @desc  Periodic CQIPMIRI reporting on PUCCH Mode 1-1 submode 2 #-- @spec 36.523-2 A.4.5-3a/10

pc_FeatrGrp_110_T,                           BOOLEAN,       false   #-- @desc  Periodic CQIPMIRI reporting on PUCCH Mode 1-1 submode 2 #-- @spec 36.523-2 A.4.5-3b/10

pc_FeatrGrp_111,                             BOOLEAN,       false   #-- @desc  Measurement reporting trigger Event A6 #-- @spec 36.523-2 A.4.5-3/11

pc_FeatrGrp_111_F,                           BOOLEAN,       false   #-- @desc  Measurement reporting trigger Event A6 #-- @spec 36.523-2 A.4.5-3a/11

pc_FeatrGrp_111_T,                           BOOLEAN,       false   #-- @desc  Measurement reporting trigger Event A6 #-- @spec 36.523-2 A.4.5-3b/11

pc_FeatrGrp_112,                             BOOLEAN,       false   #-- @desc  SCell addition within the Handover to EUTRA procedure #-- @spec 36.523-2 A.4.5-3/12

pc_FeatrGrp_112_F,                           BOOLEAN,       false   #-- @desc  SCell addition within the Handover to EUTRA procedure #-- @spec 36.523-2 A.4.5-3a/12

pc_FeatrGrp_112_T,                           BOOLEAN,       false   #-- @desc  SCell addition within the Handover to EUTRA procedure #-- @spec 36.523-2 A.4.5-3b/12

pc_FeatrGrp_113,                             BOOLEAN,       false   #-- @desc  Trigger type 0 SRS (periodic SRS) transmission on X Serving Cells #-- @spec 36.523-2 A.4.5-3/13

pc_FeatrGrp_113_F,                           BOOLEAN,       false   #-- @desc  Trigger type 0 SRS (periodic SRS) transmission on X Serving Cells #-- @spec 36.523-2 A.4.5-3a/13

pc_FeatrGrp_113_T,                           BOOLEAN,       false   #-- @desc  Trigger type 0 SRS (periodic SRS) transmission on X Serving Cells #-- @spec 36.523-2 A.4.5-3b/13

pc_FeatrGrp_114,                             BOOLEAN,       false   #-- @desc  Reporting of both UTRA CPICH RSCP and EcN0 in a Measurement Report #-- @spec 36.523-2 A.4.5-3/14

pc_FeatrGrp_114_F,                           BOOLEAN,       false   #-- @desc  Reporting of both UTRA CPICH RSCP and EcN0 in a Measurement Report #-- @spec 36.523-2 A.4.5-3a/14

pc_FeatrGrp_114_T,                           BOOLEAN,       false   #-- @desc  Reporting of both UTRA CPICH RSCP and EcN0 in a Measurement Report #-- @spec 36.523-2 A.4.5-3b/14

pc_FeatrGrp_115,                             BOOLEAN,       false   #-- @desc  time domain ICIC RLMRRM measurement subframe restriction for the serving cell. time domain ICIC RRM measurement subframe restriction for neighbour cells. time domain ICIC CSI measurement subframe restriction #-- @spec 36.523-2 A.4.5-3/15

pc_FeatrGrp_115_F,                           BOOLEAN,       false   #-- @desc  time domain ICIC RLMRRM measurement subframe restriction for the serving cell. time domain ICIC RRM measurement subframe restriction for neighbour cells. time domain ICIC CSI measurement subframe restriction #-- @spec 36.523-2 A.4.5-3a/15

pc_FeatrGrp_115_T,                           BOOLEAN,       false   #-- @desc  time domain ICIC RLMRRM measurement subframe restriction for the serving cell. time domain ICIC RRM measurement subframe restriction for neighbour cells. time domain ICIC CSI measurement subframe restriction #-- @spec 36.523-2 A.4.5-3b/15

pc_FeatrGrp_116,                             BOOLEAN,       false   #-- @desc  Relative transmit phase continuity for spatial multiplexing in UL #-- @spec 36.523-2 A.4.5-3/16

pc_FeatrGrp_116_F,                           BOOLEAN,       false   #-- @desc  Relative transmit phase continuity for spatial multiplexing in UL #-- @spec 36.523-2 A.4.5-3a/16

pc_FeatrGrp_116_T,                           BOOLEAN,       false   #-- @desc  Relative transmit phase continuity for spatial multiplexing in UL #-- @spec 36.523-2 A.4.5-3b/16

pc_FeatrGrp_11_F,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to 1xRTT CS Active handover #-- @spec 36.523-2 A.4.5-1a/11

pc_FeatrGrp_11_T,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to 1xRTT CS Active handover #-- @spec 36.523-2 A.4.5-1b/11

pc_FeatrGrp_12,                              BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to HRPD Active handover #-- @spec 36.523-2 A.4.5-1/12

pc_FeatrGrp_12_F,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to HRPD Active handover #-- @spec 36.523-2 A.4.5-1a/12

pc_FeatrGrp_12_T,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to HRPD Active handover #-- @spec 36.523-2 A.4.5-1b/12

pc_FeatrGrp_13,                              BOOLEAN,       false   #-- @desc  Support of Inter-frequency handover (within FDD or TDD) #-- @spec 36.523-2 A.4.5-1/13

pc_FeatrGrp_13_F,                            BOOLEAN,       false   #-- @desc  Support of Inter-frequency handover (within FDD or TDD) #-- @spec 36.523-2 A.4.5-1a/13

pc_FeatrGrp_13_T,                            BOOLEAN,       false   #-- @desc  Support of Inter-frequency handover (within FDD or TDD) #-- @spec 36.523-2 A.4.5-1b/13

pc_FeatrGrp_14,                              BOOLEAN,       false   #-- @desc  Support of Measurement reporting event: Event A4 - Neighbour > threshold Measurement reporting event: Event A5 - Serving < threshold1 & Neighbour > threshold2 #-- @spec 36.523-2 A.4.5-1/14

pc_FeatrGrp_14_F,                            BOOLEAN,       false   #-- @desc  Support of Measurement reporting event: Event A4 - Neighbour > threshold Measurement reporting event: Event A5 - Serving < threshold1 & Neighbour > threshold2 #-- @spec 36.523-2 A.4.5-1a/14

pc_FeatrGrp_14_T,                            BOOLEAN,       false   #-- @desc  Support of Measurement reporting event: Event A4 - Neighbour > threshold Measurement reporting event: Event A5 - Serving < threshold1 & Neighbour > threshold2 #-- @spec 36.523-2 A.4.5-1b/14

pc_FeatrGrp_15,                              BOOLEAN,       false   #-- @desc  Support of Measurement reporting event: Event B1 - Neighbour > threshold #-- @spec 36.523-2 A.4.5-1/15

pc_FeatrGrp_15_F,                            BOOLEAN,       false   #-- @desc  Support of Measurement reporting event: Event B1 - Neighbour > threshold #-- @spec 36.523-2 A.4.5-1a/15

pc_FeatrGrp_15_T,                            BOOLEAN,       false   #-- @desc  Support of Measurement reporting event: Event B1 - Neighbour > threshold #-- @spec 36.523-2 A.4.5-1b/15

pc_FeatrGrp_16,                              BOOLEAN,       false   #-- @desc  Support of Periodical measurement reporting for non-ANR related measurements #-- @spec 36.523-2 A.4.5-1/16

pc_FeatrGrp_16_F,                            BOOLEAN,       false   #-- @desc  Support of Periodical measurement reporting for non-ANR related measurements #-- @spec 36.523-2 A.4.5-1a/16

pc_FeatrGrp_16_T,                            BOOLEAN,       false   #-- @desc  Support of Periodical measurement reporting for non-ANR related measurements #-- @spec 36.523-2 A.4.5-1b/16

pc_FeatrGrp_17,                              BOOLEAN,       false   #-- @desc  Support of Periodical measurement reporting for SON  ANR and ANR related intra-frequency measurement reporting events #-- @spec 36.523-2 A.4.5-1/17

pc_FeatrGrp_17_F,                            BOOLEAN,       false   #-- @desc  Support of Periodical measurement reporting for SON  ANR and ANR related intra-frequency measurement reporting events #-- @spec 36.523-2 A.4.5-1a/17

pc_FeatrGrp_17_T,                            BOOLEAN,       false   #-- @desc  Support of Periodical measurement reporting for SON  ANR and ANR related intra-frequency measurement reporting events #-- @spec 36.523-2 A.4.5-1b/17

pc_FeatrGrp_18,                              BOOLEAN,       false   #-- @desc  Support of ANR related inter-frequency measurement reporting events #-- @spec 36.523-2 A.4.5-1/18

pc_FeatrGrp_18_F,                            BOOLEAN,       false   #-- @desc  Support of ANR related inter-frequency measurement reporting events #-- @spec 36.523-2 A.4.5-1a/18

pc_FeatrGrp_18_T,                            BOOLEAN,       false   #-- @desc  Support of ANR related inter-frequency measurement reporting events #-- @spec 36.523-2 A.4.5-1b/18

pc_FeatrGrp_19,                              BOOLEAN,       false   #-- @desc  Support of ANR related inter-RAT measurement reporting events #-- @spec 36.523-2 A.4.5-1/19

pc_FeatrGrp_19_F,                            BOOLEAN,       false   #-- @desc  Support of ANR related inter-RAT measurement reporting events #-- @spec 36.523-2 A.4.5-1a/19

pc_FeatrGrp_19_T,                            BOOLEAN,       false   #-- @desc  Support of ANR related inter-RAT measurement reporting events #-- @spec 36.523-2 A.4.5-1b/19

pc_FeatrGrp_1_F,                             BOOLEAN,       false   #-- @desc  Support of Intra-subframe frequency hopping for PUSCH scheduled by UL grant Extended cyclic prefix with f = 7.5kHz for DL resource block DCI format 3a (TPC commands for PUCCH and PUSCH with single bit power adjustments) Multi-user MIMO for PDSCH Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-0 - UE selected subband CQI without PMI Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2 - UE selected subband CQI with multiple PMI #-- @spec 36.523-2 A.4.5-1a/1

pc_FeatrGrp_1_T,                             BOOLEAN,       false   #-- @desc  Support of Intra-subframe frequency hopping for PUSCH scheduled by UL grant Extended cyclic prefix with f = 7.5kHz for DL resource block DCI format 3a (TPC commands for PUCCH and PUSCH with single bit power adjustments) Multi-user MIMO for PDSCH Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-0 - UE selected subband CQI without PMI Aperiodic CQIPMIRI reporting on PUSCH: Mode 2-2 - UE selected subband CQI with multiple PMI #-- @spec 36.523-2 A.4.5-1b/1

pc_FeatrGrp_2,                               BOOLEAN,       false   #-- @desc  Support of Simultaneous CQI and ACKNACK on PUCCH i.e. PUCCH format 2a and 2b Absolute TPC command for PUSCH Resource allocation type 1 for PDSCH Periodic CQIPMIRI reporting on PUCCH: Mode 2- 0 - UE selected subband CQI without PMI Periodic CQIPMIRI reporting on PUCCH: Mode 2-1 - UE selected subband CQI with single PMI #-- @spec 36.523-2 A.4.5-1/2

pc_FeatrGrp_20,                              BOOLEAN,       false   #-- @desc  Support of RB combination: SRB1 and SRB2 for DCCH + x AM DRB + x UM DRB #-- @spec 36.523-2 A.4.5-1/20

pc_FeatrGrp_20_F,                            BOOLEAN,       false   #-- @desc  Support of RB combination: SRB1 and SRB2 for DCCH + x AM DRB + x UM DRB #-- @spec 36.523-2 A.4.5-1a/20

pc_FeatrGrp_20_T,                            BOOLEAN,       false   #-- @desc  Support of RB combination: SRB1 and SRB2 for DCCH + x AM DRB + x UM DRB #-- @spec 36.523-2 A.4.5-1b/20

pc_FeatrGrp_21,                              BOOLEAN,       false   #-- @desc  Support of Predefined intra-subframe frequency hopping for PUSCH with N_sb > 1 Predefined inter-subframe frequency hopping for PUSCH with N_sb > 1 #-- @spec 36.523-2 A.4.5-1/21

pc_FeatrGrp_21_F,                            BOOLEAN,       false   #-- @desc  Support of Predefined intra-subframe frequency hopping for PUSCH with N_sb > 1 Predefined inter-subframe frequency hopping for PUSCH with N_sb > 1 #-- @spec 36.523-2 A.4.5-1a/21

pc_FeatrGrp_21_T,                            BOOLEAN,       false   #-- @desc  Support of Predefined intra-subframe frequency hopping for PUSCH with N_sb > 1 Predefined inter-subframe frequency hopping for PUSCH with N_sb > 1 #-- @spec 36.523-2 A.4.5-1b/21

pc_FeatrGrp_22,                              BOOLEAN,       false   #-- @desc  Support of UTRAN measurements and reporting in E-UTRA connected mode #-- @spec 36.523-2 A.4.5-1/22

pc_FeatrGrp_22_F,                            BOOLEAN,       false   #-- @desc  Support of UTRAN measurements and reporting in E-UTRA connected mode #-- @spec 36.523-2 A.4.5-1a/22

pc_FeatrGrp_22_T,                            BOOLEAN,       false   #-- @desc  Support of UTRAN measurements and reporting in E-UTRA connected mode #-- @spec 36.523-2 A.4.5-1b/22

pc_FeatrGrp_23,                              BOOLEAN,       false   #-- @desc  Support of GERAN measurements and reporting in E-UTRA connected mode #-- @spec 36.523-2 A.4.5-1/23

pc_FeatrGrp_23_F,                            BOOLEAN,       false   #-- @desc  Support of GERAN measurements and reporting in E-UTRA connected mode #-- @spec 36.523-2 A.4.5-1a/23

pc_FeatrGrp_23_T,                            BOOLEAN,       false   #-- @desc  Support of GERAN measurements and reporting in E-UTRA connected mode #-- @spec 36.523-2 A.4.5-1b/23

pc_FeatrGrp_24,                              BOOLEAN,       false   #-- @desc  Support of cdma2000 measurements and reporting in E-UTRA connected mode #-- @spec 36.523-2 A.4.5-1/24

pc_FeatrGrp_24_F,                            BOOLEAN,       false   #-- @desc  Support of cdma2000 measurements and reporting in E-UTRA connected mode #-- @spec 36.523-2 A.4.5-1a/24

pc_FeatrGrp_24_T,                            BOOLEAN,       false   #-- @desc  Support of cdma2000 measurements and reporting in E-UTRA connected mode #-- @spec 36.523-2 A.4.5-1b/24

pc_FeatrGrp_25,                              BOOLEAN,       false   #-- @desc  Support of Inter-frequency measurements and reporting in E-UTRA connected mode #-- @spec 36.523-2 A.4.5-1/25

pc_FeatrGrp_25_F,                            BOOLEAN,       false   #-- @desc  Support of Inter-frequency measurements and reporting in E-UTRA connected mode #-- @spec 36.523-2 A.4.5-1a/25

pc_FeatrGrp_25_T,                            BOOLEAN,       false   #-- @desc  Support of Inter-frequency measurements and reporting in E-UTRA connected mode #-- @spec 36.523-2 A.4.5-1b/25

pc_FeatrGrp_26,                              BOOLEAN,       false   #-- @desc  Support of HRPD measurements reporting and measurement reporting event B2 in E-UTRA connected mode #-- @spec 36.523-2 A.4.5-1/26

pc_FeatrGrp_26_F,                            BOOLEAN,       false   #-- @desc  Support of HRPD measurements reporting and measurement reporting event B2 in E-UTRA connected mode #-- @spec 36.523-2 A.4.5-1a/26

pc_FeatrGrp_26_T,                            BOOLEAN,       false   #-- @desc  Support of HRPD measurements reporting and measurement reporting event B2 in E-UTRA connected mode #-- @spec 36.523-2 A.4.5-1b/26

pc_FeatrGrp_27,                              BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to UTRA CELL_DCH CS handover #-- @spec 36.523-2 A.4.5-1/27

pc_FeatrGrp_27_F,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to UTRA CELL_DCH CS handover #-- @spec 36.523-2 A.4.5-1a/27

pc_FeatrGrp_27_T,                            BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to UTRA CELL_DCH CS handover #-- @spec 36.523-2 A.4.5-1b/27

pc_FeatrGrp_28,                              BOOLEAN,       false   #-- @desc  Support of TTI bundling #-- @spec 36.523-2 A.4.5-1/28

pc_FeatrGrp_28_F,                            BOOLEAN,       false   #-- @desc  Support of TTI bundling #-- @spec 36.523-2 A.4.5-1a/28

pc_FeatrGrp_28_T,                            BOOLEAN,       false   #-- @desc  Support of TTI bundling #-- @spec 36.523-2 A.4.5-1b/28

pc_FeatrGrp_29,                              BOOLEAN,       false   #-- @desc  Support of Semi-Persistent Scheduling #-- @spec 36.523-2 A.4.5-1/29

pc_FeatrGrp_29_F,                            BOOLEAN,       false   #-- @desc  Support of Semi-Persistent Scheduling #-- @spec 36.523-2 A.4.5-1a/29

pc_FeatrGrp_29_T,                            BOOLEAN,       false   #-- @desc  Support of Semi-Persistent Scheduling #-- @spec 36.523-2 A.4.5-1b/29

pc_FeatrGrp_2_F,                             BOOLEAN,       false   #-- @desc  Support of Simultaneous CQI and ACKNACK on PUCCH i.e. PUCCH format 2a and 2b Absolute TPC command for PUSCH Resource allocation type 1 for PDSCH Periodic CQIPMIRI reporting on PUCCH: Mode 2- 0 - UE selected subband CQI without PMI Periodic CQIPMIRI reporting on PUCCH: Mode 2-1 - UE selected subband CQI with single PMI #-- @spec 36.523-2 A.4.5-1a/2

pc_FeatrGrp_2_T,                             BOOLEAN,       false   #-- @desc  Support of Simultaneous CQI and ACKNACK on PUCCH i.e. PUCCH format 2a and 2b Absolute TPC command for PUSCH Resource allocation type 1 for PDSCH Periodic CQIPMIRI reporting on PUCCH: Mode 2- 0 - UE selected subband CQI without PMI Periodic CQIPMIRI reporting on PUCCH: Mode 2-1 - UE selected subband CQI with single PMI #-- @spec 36.523-2 A.4.5-1b/2

pc_FeatrGrp_3,                               BOOLEAN,       false   #-- @desc  Support of Semi-persistent scheduling TTI bundling 5bit RLC UM SN 7bit PDCP SN #-- @spec 36.523-2 A.4.5-1/3

pc_FeatrGrp_30,                              BOOLEAN,       false   #-- @desc  Support of Handover between FDD and TDD #-- @spec 36.523-2 A.4.5-1/30

pc_FeatrGrp_30_F,                            BOOLEAN,       false   #-- @desc  Support of Handover between FDD and TDD #-- @spec 36.523-2 A.4.5-1a/30

pc_FeatrGrp_30_T,                            BOOLEAN,       false   #-- @desc  Support of Handover between FDD and TDD #-- @spec 36.523-2 A.4.5-1b/30

pc_FeatrGrp_31,                              BOOLEAN,       false   #-- @desc  Support of the mechanisms defined for cells broadcasting multi band information i.e. comprehending multiBandInfoList #-- @spec 36.523-2 A.4.5-1/31

pc_FeatrGrp_31_F,                            BOOLEAN,       false   #-- @desc  Support of the mechanisms defined for cells broadcasting multi band information i.e. comprehending multiBandInfoList #-- @spec 36.523-2 A.4.5-1a/31

pc_FeatrGrp_31_T,                            BOOLEAN,       false   #-- @desc  Support of the mechanisms defined for cells broadcasting multi band information i.e. comprehending multiBandInfoList #-- @spec 36.523-2 A.4.5-1b/31

pc_FeatrGrp_33,                              BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for UTRAN including: #-- @spec 36.523-2 A.4.5-1c/1

pc_FeatrGrp_33_F,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for UTRAN including:  Inter-RAT periodical measurement reporting where triggerType is set to periodical and purpose is set to reportStrongestCellsForSON #-- @spec 36.523-2 A.4.5-1d/1

pc_FeatrGrp_33_T,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for UTRAN including: #-- @spec 36.523-2 A.4.5-1e/1

pc_FeatrGrp_34,                              BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for GERAN including: #-- @spec 36.523-2 A.4.5-1c/2

pc_FeatrGrp_34_F,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for GERAN including: #-- @spec 36.523-2 A.4.5-1d/2

pc_FeatrGrp_34_T,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for GERAN including: #-- @spec 36.523-2 A.4.5-1e/2

pc_FeatrGrp_35,                              BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for 1xRTT including: #-- @spec 36.523-2 A.4.5-1c/3

pc_FeatrGrp_35_F,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for 1xRTT including: #-- @spec 36.523-2 A.4.5-1d/3

pc_FeatrGrp_35_T,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for 1xRTT including: #-- @spec 36.523-2 A.4.5-1e/3

pc_FeatrGrp_36,                              BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for HRPD including: #-- @spec 36.523-2 A.4.5-1c/4

pc_FeatrGrp_36_F,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for HRPD including: #-- @spec 36.523-2 A.4.5-1d/4

pc_FeatrGrp_36_T,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for HRPD including:  Inter-RAT periodical measurement reporting where triggerType is set to periodical and purpose is set to portStrongestCellsForSON #-- @spec 36.523-2 A.4.5-1e/4

pc_FeatrGrp_37,                              BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for UTRAN TDD including: #-- @spec 36.523-2 A.4.5-1c/5

pc_FeatrGrp_37_F,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for UTRAN TDD including: #-- @spec 36.523-2 A.4.5-1d/5

pc_FeatrGrp_37_T,                            BOOLEAN,       false   #-- @desc  Inter-RAT ANR features for UTRAN TDD including: #-- @spec 36.523-2 A.4.5-1e/5

pc_FeatrGrp_38,                              BOOLEAN,       false   #-- @desc  EUTRA RRC_CONNECTED to UTRA TDD CELL_DCH PS handover if the UE supports both UTRAN FDD and UTRAN TDD #-- @spec 36.523-2 A.4.5-1c/6

pc_FeatrGrp_38_F,                            BOOLEAN,       false   #-- @desc  EUTRA RRC_CONNECTED to UTRA TDD CELL_DCH PS handover if the UE supports both UTRAN FDD and UTRAN TDD #-- @spec 36.523-2 A.4.5-1d/6

pc_FeatrGrp_38_T,                            BOOLEAN,       false   #-- @desc  EUTRA RRC_CONNECTED to UTRA TDD CELL_DCH PS handover if the UE supports both UTRAN FDD and UTRAN TDD #-- @spec 36.523-2 A.4.5-1e/6

pc_FeatrGrp_39,                              BOOLEAN,       false   #-- @desc  UTRAN TDD measurements reporting and measurement reporting event B2 in E-UTRA connected mode if the UE supports both UTRAN FDD and UTRAN TDD #-- @spec 36.523-2 A.4.5-1c/7

pc_FeatrGrp_39_F,                            BOOLEAN,       false   #-- @desc  UTRAN TDD measurements reporting and measurement reporting event B2 in E-UTRA connected mode if the UE supports both UTRAN FDD and UTRAN TDD #-- @spec 36.523-2 A.4.5-1d/7

pc_FeatrGrp_39_T,                            BOOLEAN,       false   #-- @desc  UTRAN TDD measurements reporting and measurement reporting event B2 in E-UTRA connected mode if the UE supports both UTRAN FDD and UTRAN TDD #-- @spec 36.523-2 A.4.5-1e/7

pc_FeatrGrp_3_F,                             BOOLEAN,       false   #-- @desc  Support of Semi-persistent scheduling TTI bundling 5bit RLC UM SN 7bit PDCP SN #-- @spec 36.523-2 A.4.5-1a/3

pc_FeatrGrp_3_T,                             BOOLEAN,       false   #-- @desc  Support of Semi-persistent scheduling TTI bundling 5bit RLC UM SN 7bit PDCP SN #-- @spec 36.523-2 A.4.5-1b/3

pc_FeatrGrp_4,                               BOOLEAN,       false   #-- @desc  Support of Short DRX cycle #-- @spec 36.523-2 A.4.5-1/4

pc_FeatrGrp_40,                              BOOLEAN,       false   #-- @desc  EUTRA RRC_CONNECTED to UTRA TDD  CELL_DCH  CS handover if the UE supports both UTRAN FDD and UTRAN TDD #-- @spec 36.523-2 A.4.5-1c/8

pc_FeatrGrp_40_F,                            BOOLEAN,       false   #-- @desc  EUTRA RRC_CONNECTED to UTRA TDD  CELL_DCH  CS handover if the UE supports both UTRAN FDD and UTRAN TDD #-- @spec 36.523-2 A.4.5-1d/8

pc_FeatrGrp_40_T,                            BOOLEAN,       false   #-- @desc  EUTRA RRC_CONNECTED to UTRA TDD  CELL_DCH  CS handover if the UE supports both UTRAN FDD and UTRAN TDD #-- @spec 36.523-2 A.4.5-1e/8

pc_FeatrGrp_41,                              BOOLEAN,       false   #-- @desc  Measurement reporting event: Event B1 û Neighbour > threshold for UTRAN FDD if the UE supports UTRAN FDD and has set bit number 22 to 1 #-- @spec 36.523-2 A.4.5-1c/9

pc_FeatrGrp_41_F,                            BOOLEAN,       false   #-- @desc  Measurement reporting event: Event B1 Neighbour > threshold for UTRAN FDD if the UE supports UTRAN FDD and has set bit number 22 to 1 #-- @spec 36.523-2 A.4.5-1d/9

pc_FeatrGrp_41_T,                            BOOLEAN,       false   #-- @desc  Measurement reporting event: Event B1 Neighbour > threshold for UTRAN FDD if the UE supports UTRAN FDD and has set bit number 22 to 1 #-- @spec 36.523-2 A.4.5-1e/9

pc_FeatrGrp_42_F,                            BOOLEAN,       false   #-- @desc  DCI format 3a (TPC commands for PUCCH and PUSCH with single bit power adjustments) #-- @spec 36.523-2 A.4.5-1d/10

pc_FeatrGrp_42_T,                            BOOLEAN,       false   #-- @desc  DCI format 3a (TPC commands for PUCCH and PUSCH with single bit power adjustments) #-- @spec 36.523-2 A.4.5-1e/10

pc_FeatrGrp_4_F,                             BOOLEAN,       false   #-- @desc  Support of Short DRX cycle #-- @spec 36.523-2 A.4.5-1a/4

pc_FeatrGrp_4_T,                             BOOLEAN,       false   #-- @desc  Support of Short DRX cycle #-- @spec 36.523-2 A.4.5-1b/4

pc_FeatrGrp_5,                               BOOLEAN,       false   #-- @desc  Support of Long DRX cycle DRX command MAC control element #-- @spec 36.523-2 A.4.5-1/5

pc_FeatrGrp_5_F,                             BOOLEAN,       false   #-- @desc  Support of Long DRX cycle DRX command MAC control element #-- @spec 36.523-2 A.4.5-1a/5

pc_FeatrGrp_5_T,                             BOOLEAN,       false   #-- @desc  Support of Long DRX cycle DRX command MAC control element #-- @spec 36.523-2 A.4.5-1b/5

pc_FeatrGrp_6,                               BOOLEAN,       false   #-- @desc  Support of Piroritized bit rate #-- @spec 36.523-2 A.4.5-1/6

pc_FeatrGrp_6_F,                             BOOLEAN,       false   #-- @desc  Support of Piroritized bit rate #-- @spec 36.523-2 A.4.5-1a/6

pc_FeatrGrp_6_T,                             BOOLEAN,       false   #-- @desc  Support of Piroritized bit rate #-- @spec 36.523-2 A.4.5-1b/6

pc_FeatrGrp_7,                               BOOLEAN,       false   #-- @desc  Support of RLC UM #-- @spec 36.523-2 A.4.5-1/7

pc_FeatrGrp_7_F,                             BOOLEAN,       false   #-- @desc  Support of RLC UM #-- @spec 36.523-2 A.4.5-1a/7

pc_FeatrGrp_7_T,                             BOOLEAN,       false   #-- @desc  Support of RLC UM #-- @spec 36.523-2 A.4.5-1b/7

pc_FeatrGrp_8,                               BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to UTRA CELL_DCH PS handover #-- @spec 36.523-2 A.4.5-1/8

pc_FeatrGrp_8_F,                             BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to UTRA CELL_DCH PS handover #-- @spec 36.523-2 A.4.5-1a/8

pc_FeatrGrp_8_T,                             BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to UTRA CELL_DCH PS handover #-- @spec 36.523-2 A.4.5-1b/8

pc_FeatrGrp_9,                               BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to GERAN GSM_Dedicated handover #-- @spec 36.523-2 A.4.5-1/9

pc_FeatrGrp_9_F,                             BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to GERAN GSM_Dedicated handover #-- @spec 36.523-2 A.4.5-1a/9

pc_FeatrGrp_9_T,                             BOOLEAN,       false   #-- @desc  Support of EUTRA RRC_CONNECTED to GERAN GSM_Dedicated handover #-- @spec 36.523-2 A.4.5-1b/9

pc_FixedBroadband,                           BOOLEAN,       false   #-- @desc  UE supports Fixed Broadband #-- @spec 34.229-2 Table A.18/3

pc_FlexibleStartPRB_PDSCH,                   BOOLEAN,       false   #-- @desc  Support of flexible starting PRB for PDSCH #-- @spec 36.523-2 A.4.4-1/222

pc_FlexibleStartPRB_PUSCH,                   BOOLEAN,       false   #-- @desc  Support of flexible starting PRB for PUSCH #-- @spec 36.523-2 A.4.4-1/223

pc_FlightPathPlan,                           BOOLEAN,       false   #-- @desc  Support of GNSS for height measurement #-- @spec 36.523-2 A.4.4-1/kkj

pc_FourCell,                                 BOOLEAN,       FALSE   #-- @desc  Support of Four cell #-- @spec 34.123-2 Table A.18a/51

pc_FourCellMIMO,                             BOOLEAN,       FALSE   #-- @desc  Support of Four cell MIMO #-- @spec 34.123-2 Table A.18a/49

pc_FullNameNetwork,                          BOOLEAN,       false   #-- @desc  Support of storage of the network full name #-- @spec 36.523-2 A.4.4-1/12

pc_Full_FDPCH,                               BOOLEAN,       false   #-- @desc  Full support of F-DPCH #-- @spec 34.123-2 Table A.18a/19

pc_GALILEO,                                  BOOLEAN,       false   #-- @desc  Support for Galileo #-- @spec 37.571-3 Table A.4.3-1/9

pc_GALILEO_ADR,                              BOOLEAN,       false   #-- @desc  Support of ADR measurement reporting for Galileo #-- @spec 37.571-3 Table A.4.3-6/4

pc_GALILEO_ADR_ENH,                          BOOLEAN,       false   #-- @desc  Support of ADR enhancements for Galileo #-- @spec 37.571-3 Table A.4.3-6/5

pc_GALILEO_E1,                               BOOLEAN,       false   #-- @desc  Support of E1 signal in Galileo #-- @spec 37.571-3 Table A.4.3-5/11

pc_GALILEO_E5a,                              BOOLEAN,       false   #-- @desc  Support of E5a signal in Galileo #-- @spec 37.571-3 Table A.4.3-5/12

pc_GALILEO_E5aE5b,                           BOOLEAN,       false   #-- @desc  Support of E5a+E5b signal in Galileo #-- @spec 37.571-3 Table A.4.3-5/15

pc_GALILEO_E5b,                              BOOLEAN,       false   #-- @desc  Support of E5b signal in Galileo #-- @spec 37.571-3 Table A.4.3-5/13

pc_GALILEO_E6,                               BOOLEAN,       false   #-- @desc  Support of E6 signal in Galileo #-- @spec 37.571-3 Table A.4.3-5/14

pc_GALILEO_HA,                               BOOLEAN,       false   #-- @desc  Support of High accuracy GNSS modes for Galileo #-- @spec 37.571-3 Table A.4.3-6/22

pc_GALILEO_VelocityMeas,                     BOOLEAN,       false   #-- @desc  Support of Velocity measurement reporting for Galileo #-- @spec 37.571-3 Table A.4.3-6/9

pc_GBAForXCAPAuthentication,                 BOOLEAN,       false   #-- @desc  UE supports and uses GBA for XCAP authentication #-- @spec 34.229-2 Table A.12/xx

pc_GERAN,                                    BOOLEAN,       false   #-- @desc  UE Supports GSM andor GPRS #-- @spec 36.523-2 A.4.1-1/7

pc_GERAN_2_E_UTRAN_PSHO,                     BOOLEAN,       false   #-- @desc  Support of GERAN to E-UTRAN PS Handover #-- @spec 36.523-2 A.4.4-1/29

pc_GERAN_2_E_UTRAN_meas,                     BOOLEAN,       false   #-- @desc  Supports Neighbour Cell measurements and Network controlled & autonomous cell reselection to E-UTRAN #-- @spec 36.523-2 A.4.4-1/21

pc_GERAN_2_E_UTRAN_measreporting_CCN,        BOOLEAN,       false   #-- @desc  Supports CCN towards E-UTRAN E-UTRAN Neighbour cell measurement reporting and Network controlled cell reselection to E-UTRAN #-- @spec 36.523-2 A.4.4-1/39

pc_GLONASS,                                  BOOLEAN,       false   #-- @desc  Support for GLONASS #-- @spec 37.571-3 Table A.4.3-1/7

pc_GLONASS_ADR,                              BOOLEAN,       false   #-- @desc  Support of ADR measurement reporting for Glonass #-- @spec 37.571-3 Table A.4.3-6/5

pc_GLONASS_ADR_ENH,                          BOOLEAN,       false   #-- @desc  Support of ADR enhancements for Glonass #-- @spec 37.571-3 Table A.4.3-6/17

pc_GLONASS_G1,                               BOOLEAN,       false   #-- @desc  Support of G1 signal in Glonass #-- @spec 37.571-3 Table A.4.3-5/8

pc_GLONASS_G2,                               BOOLEAN,       false   #-- @desc  Support of G2 signal in Glonass #-- @spec 37.571-3 Table A.4.3-5/9

pc_GLONASS_G3,                               BOOLEAN,       false   #-- @desc  Support of G3 signal in Glonass #-- @spec 37.571-3 Table A.4.3-5/10

pc_GLONASS_HA,                               BOOLEAN,       false   #-- @desc  Support of High accuracy GNSS modes for Glonass #-- @spec 37.571-3 Table A.4.3-6/23

pc_GLONASS_VelocityMeas,                     BOOLEAN,       false   #-- @desc  Support of Velocity measurement reporting for Glonass #-- @spec 37.571-3 Table A.4.3-6/10

pc_GNSS_AA,                                  BOOLEAN,       false   #-- @desc  Support of GNSS Acquisition Assistance #-- @spec 37.571-3 Table A.4.3-2/12

pc_GNSS_AcquAssistSup_BDS,                   BOOLEAN,       false   #-- @desc  Gnss-AcquisitionAssistanceSupport for BDS #-- @spec 37.571-3 Table A.4.3-7/55

pc_GNSS_AcquAssistSup_Galileo,               BOOLEAN,       false   #-- @desc  Gnss-AcquisitionAssistanceSupport for galileo #-- @spec 37.571-3 Table A.4.3-7/33

pc_GNSS_AcquAssistSup_Glonass,               BOOLEAN,       false   #-- @desc  Gnss-AcquisitionAssistanceSupport for glonass #-- @spec 37.571-3 Table A.4.3-7/34

pc_GNSS_AcquAssistSup_Gps,                   BOOLEAN,       false   #-- @desc  Gnss-AcquisitionAssistanceSupport for gps #-- @spec 37.571-3 Table A.4.3-7/30

pc_GNSS_AcquAssistSup_Qzss,                  BOOLEAN,       false   #-- @desc  Gnss-AcquisitionAssistanceSupport for qzss #-- @spec 37.571-3 Table A.4.3-7/32

pc_GNSS_AcquAssistSup_Sbas,                  BOOLEAN,       false   #-- @desc  Gnss-AcquisitionAssistanceSupport for sbas #-- @spec 37.571-3 Table A.4.3-7/31

pc_GNSS_AcquAssist_BDS_B1C,                  BOOLEAN,       false   #-- @desc  Support of GNSS-AcquisitionAssistance for BDS B1C #-- @spec 37.571-3 Table A.4.3-7/99

pc_GNSS_AcquAssist_BDS_B1I,                  BOOLEAN,       false   #-- @desc  Support of GNSS-AcquisitionAssistance for BDS B1I #-- @spec 37.571-3 Table A.4.3-7/98

pc_GNSS_AcquAssist_BDS_B2a,                  BOOLEAN,       false   #-- @desc  Support of GNSS-AcquisitionAssistance for BDS B2a #-- @spec 37.571-3 Table A.4.3-7/135

pc_GNSS_AcquAssist_BDS_B3I,                  BOOLEAN,       false   #-- @desc  Support of GNSS-AcquisitionAssistance for BDS B3I #-- @spec 37.571-3 Table A.4.3-7/136

pc_GNSS_AcquAssist_GPS_L1CA,                 BOOLEAN,       false   #-- @desc  Support of GNSS-AcquisitionAssistance for GPS L1 CA #-- @spec 37.571-3 Table A.4.3-7/61

pc_GNSS_AcquAssist_GPS_L5,                   BOOLEAN,       false   #-- @desc  Support of GNSS-AcquisitionAssistance for GPS L5 #-- @spec 37.571-3 Table A.4.3-7/62

pc_GNSS_AcquAssist_Galileo_E1,               BOOLEAN,       false   #-- @desc  Support of GNSS-AcquisitionAssistance for Galileo E1 #-- @spec 37.571-3 Table A.4.3-7/63

pc_GNSS_AcquAssist_Galileo_E5A,              BOOLEAN,       false   #-- @desc  Support of GNSS-AcquisitionAssistance for Galileo E5A #-- @spec 37.571-3 Table A.4.3-7/64

pc_GNSS_AlmanacSup_BDS,                      BOOLEAN,       false   #-- @desc  Gnss-AlmanacSupport for BDS #-- @spec 37.571-3 Table A.4.3-7/56

pc_GNSS_AlmanacSup_Galileo,                  BOOLEAN,       false   #-- @desc  Gnss-AlmanacSupport for galileo #-- @spec 37.571-3 Table A.4.3-7/38

pc_GNSS_AlmanacSup_Glonass,                  BOOLEAN,       false   #-- @desc  Gnss-AlmanacSupport for glonass #-- @spec 37.571-3 Table A.4.3-7/39

pc_GNSS_AlmanacSup_Gps,                      BOOLEAN,       false   #-- @desc  Gnss-AlmanacSupport for gps #-- @spec 37.571-3 Table A.4.3-7/35

pc_GNSS_AlmanacSup_Qzss,                     BOOLEAN,       false   #-- @desc  Gnss-AlmanacSupport for qzss #-- @spec 37.571-3 Table A.4.3-7/37

pc_GNSS_AlmanacSup_Sbas,                     BOOLEAN,       false   #-- @desc  Gnss-AlmanacSupport for sbas #-- @spec 37.571-3 Table A.4.3-7/36

pc_GNSS_AuxInfoSup_BDS,                      BOOLEAN,       false   #-- @desc  Gnss-AuxiliaryInformationSupport for BDS #-- @spec 37.571-3 Table A.4.3-7/58

pc_GNSS_AuxInfoSup_Galileo,                  BOOLEAN,       false   #-- @desc  Gnss-AuxiliaryInformationSupport for galileo #-- @spec 37.571-3 Table A.4.3-7/48

pc_GNSS_AuxInfoSup_Glonass,                  BOOLEAN,       false   #-- @desc  Gnss-AuxiliaryInformationSupport for glonass #-- @spec 37.571-3 Table A.4.3-7/49

pc_GNSS_AuxInfoSup_Gps,                      BOOLEAN,       false   #-- @desc  Gnss-AuxiliaryInformationSupport for gps #-- @spec 37.571-3 Table A.4.3-7/45

pc_GNSS_AuxInfoSup_Qzss,                     BOOLEAN,       false   #-- @desc  Gnss-AuxiliaryInformationSupport for qzss #-- @spec 37.571-3 Table A.4.3-7/47

pc_GNSS_AuxInfoSup_Sbas,                     BOOLEAN,       false   #-- @desc  Gnss-AuxiliaryInformationSupport for sbas #-- @spec 37.571-3 Table A.4.3-7/46

pc_GNSS_DGNSS_Sup_BDS,                       BOOLEAN,       false   #-- @desc  Gnss-DifferentialCorrectionsSupport for BDS #-- @spec 37.571-3 Table A.4.3-7/51

pc_GNSS_DGNSS_Sup_Bds_B1C,                   BOOLEAN,       false   #-- @desc  Gnss-DifferentialCorrectionsSupport for BDS B1C #-- @spec 37.571-3 Table A.4.3-7/102

pc_GNSS_DGNSS_Sup_Galileo,                   BOOLEAN,       false   #-- @desc  Gnss-DifferentialCorrectionsSupport for galileo #-- @spec 37.571-3 Table A.4.3-7/13

pc_GNSS_DGNSS_Sup_Galileo_E5A,               BOOLEAN,       false   #-- @desc  Gnss-DifferentialCorrectionsSupport for Galileo E5A #-- @spec 37.571-3 Table A.4.3-7/101

pc_GNSS_DGNSS_Sup_Glonass,                   BOOLEAN,       false   #-- @desc  Gnss-DifferentialCorrectionsSupport for glonass #-- @spec 37.571-3 Table A.4.3-7/14

pc_GNSS_DGNSS_Sup_Gps,                       BOOLEAN,       false   #-- @desc  Gnss-DifferentialCorrectionsSupport for gps #-- @spec 37.571-3 Table A.4.3-7/10

pc_GNSS_DGNSS_Sup_Gps_L5,                    BOOLEAN,       false   #-- @desc  Gnss-DifferentialCorrectionsSupport for GPS L5 #-- @spec 37.571-3 Table A.4.3-7/100

pc_GNSS_DGNSS_Sup_Qzss,                      BOOLEAN,       false   #-- @desc  Gnss-DifferentialCorrectionsSupport for qzss #-- @spec 37.571-3 Table A.4.3-7/12

pc_GNSS_DGNSS_Sup_Sbas,                      BOOLEAN,       false   #-- @desc  Gnss-DifferentialCorrectionsSupport for sbas #-- @spec 37.571-3 Table A.4.3-7/11

pc_GNSS_DataBitsSup_BDS,                     BOOLEAN,       false   #-- @desc  Gnss-DataBitAssistanceSupport for BDS #-- @spec 37.571-3 Table A.4.3-7/54

pc_GNSS_DataBitsSup_Galileo,                 BOOLEAN,       false   #-- @desc  Gnss-DataBitAssistanceSupport for galileo #-- @spec 37.571-3 Table A.4.3-7/28

pc_GNSS_DataBitsSup_Glonass,                 BOOLEAN,       false   #-- @desc  Gnss-DataBitAssistanceSupport for glonass #-- @spec 37.571-3 Table A.4.3-7/29

pc_GNSS_DataBitsSup_Gps,                     BOOLEAN,       false   #-- @desc  Gnss-DataBitAssistanceSupport for gps #-- @spec 37.571-3 Table A.4.3-7/25

pc_GNSS_DataBitsSup_Qzss,                    BOOLEAN,       false   #-- @desc  Gnss-DataBitAssistanceSupport for qzss #-- @spec 37.571-3 Table A.4.3-7/27

pc_GNSS_DataBitsSup_Sbas,                    BOOLEAN,       false   #-- @desc  Gnss-DataBitAssistanceSupport for sbas #-- @spec 37.571-3 Table A.4.3-7/26

pc_GNSS_EOPSup,                              BOOLEAN,       false   #-- @desc  Gnss-EarthOrientationParametersSupport (Common Assistance Data) #-- @spec 37.571-3 Table A.4.3-7/4

pc_GNSS_EllipArc,                            BOOLEAN,       false   #-- @desc  Ellipsoid Arc Support #-- @spec 37.571-3 Table A.4.3-8/7

pc_GNSS_EllipPoint,                          BOOLEAN,       false   #-- @desc  Ellipsoid Point Support #-- @spec 37.571-3 Table A.4.3-8/1

pc_GNSS_EllipPointAlt,                       BOOLEAN,       false   #-- @desc  Ellipsoid Point With Altitude Support #-- @spec 37.571-3 Table A.4.3-8/5

pc_GNSS_EllipPointAltUncertEllip,            BOOLEAN,       false   #-- @desc  Ellipsoid Point With Altitude And Uncertainty Ellipsoid Support #-- @spec 37.571-3 Table A.4.3-8/6

pc_GNSS_EllipPointUncertCircle,              BOOLEAN,       false   #-- @desc  Ellipsoid Point With Uncertainty Circle Support #-- @spec 37.571-3 Table A.4.3-8/2

pc_GNSS_EllipPointUncertEllip,               BOOLEAN,       false   #-- @desc  Ellipsoid Point With Uncertainty Ellipse Support #-- @spec 37.571-3 Table A.4.3-8/3

pc_GNSS_FTA,                                 BOOLEAN,       false   #-- @desc  Support of GNSS Fine Time Assistance #-- @spec 37.571-3 Table A.4.3-2/3

pc_GNSS_FTA_UEA,                             BOOLEAN,       false   #-- @desc  Support of UE Fine Time Assistance measurements for UE-assisted Assisted-GNSS #-- @spec 37.571-3 Table A.4.3-2/11

pc_GNSS_FTA_UEB,                             BOOLEAN,       false   #-- @desc  Support of UE Fine Time Assistance measurements for UE-based Assisted-GNSS #-- @spec 37.571-3 Table A.4.3-2/10

pc_GNSS_HA_EllipPointAltUncertEllip,         BOOLEAN,       false   #-- @desc  High Accuracy Ellipsoid Point With Altitude And Uncertainty Ellipsoid-r15 #-- @spec 37.571-3 Table A.4.3-8/9

pc_GNSS_HA_EllipPointUncertCircle,           BOOLEAN,       false   #-- @desc  High Accuracy Ellipsoid Point With Uncertainty Ellipse-r15 #-- @spec 37.571-3 Table A.4.3-8/8

pc_GNSS_HVVel,                               BOOLEAN,       false   #-- @desc  Horizontal With Vertical Velocity Support #-- @spec 37.571-3 Table A.4.3-9/2

pc_GNSS_HVVelUncert,                         BOOLEAN,       false   #-- @desc  Horizontal With Vertical Velocity And Uncertainty Support #-- @spec 37.571-3 Table A.4.3-9/4

pc_GNSS_HVel,                                BOOLEAN,       false   #-- @desc  Horizontal Velocity Support #-- @spec 37.571-3 Table A.4.3-9/1

pc_GNSS_HVelUncert,                          BOOLEAN,       false   #-- @desc  Horizontal Velocity With Uncertainty Support #-- @spec 37.571-3 Table A.4.3-9/3

pc_GNSS_IonoModSup,                          BOOLEAN,       false   #-- @desc  Gnss-IonosphericModelSupport (Common Assistance Data) #-- @spec 37.571-3 Table A.4.3-7/3

pc_GNSS_NavModSup_BDS,                       BOOLEAN,       false   #-- @desc  Gnss-NavigationModelSupport for BDS #-- @spec 37.571-3 Table A.4.3-7/52

pc_GNSS_NavModSup_Galileo,                   BOOLEAN,       false   #-- @desc  Gnss-NavigationModelSupport for galileo #-- @spec 37.571-3 Table A.4.3-7/18

pc_GNSS_NavModSup_Glonass,                   BOOLEAN,       false   #-- @desc  Gnss-NavigationModelSupport for glonass #-- @spec 37.571-3 Table A.4.3-7/19

pc_GNSS_NavModSup_Gps,                       BOOLEAN,       false   #-- @desc  Gnss-NavigationModelSupport for gps #-- @spec 37.571-3 Table A.4.3-7/15

pc_GNSS_NavModSup_Qzss,                      BOOLEAN,       false   #-- @desc  Gnss-NavigationModelSupport for qzss #-- @spec 37.571-3 Table A.4.3-7/17

pc_GNSS_NavModSup_Sbas,                      BOOLEAN,       false   #-- @desc  Gnss-NavigationModelSupport for sbas #-- @spec 37.571-3 Table A.4.3-7/16

pc_GNSS_Polygon,                             BOOLEAN,       false   #-- @desc  Polygon Support #-- @spec 37.571-3 Table A.4.3-8/4

pc_GNSS_RTISup_BDS,                          BOOLEAN,       false   #-- @desc  Gnss-RealTimeIntegritySupport for BDS #-- @spec 37.571-3 Table A.4.3-7/53

pc_GNSS_RTISup_Galileo,                      BOOLEAN,       false   #-- @desc  Gnss-RealTimeIntegritySupport for galileo #-- @spec 37.571-3 Table A.4.3-7/23

pc_GNSS_RTISup_Glonass,                      BOOLEAN,       false   #-- @desc  Gnss-RealTimeIntegritySupport for glonass #-- @spec 37.571-3 Table A.4.3-7/24

pc_GNSS_RTISup_Gps,                          BOOLEAN,       false   #-- @desc  Gnss-RealTimeIntegritySupport for gps #-- @spec 37.571-3 Table A.4.3-7/20

pc_GNSS_RTISup_Qzss,                         BOOLEAN,       false   #-- @desc  Gnss-RealTimeIntegritySupport for qzss #-- @spec 37.571-3 Table A.4.3-7/22

pc_GNSS_RTISup_Sbas,                         BOOLEAN,       false   #-- @desc  Gnss-RealTimeIntegritySupport for sbas #-- @spec 37.571-3 Table A.4.3-7/21

pc_GNSS_RTK_AuxStationInfo,                  BOOLEAN,       false   #-- @desc  Gnss-RTK-AuxiliaryStationDataSupport-r15 (Common assistance data) #-- @spec 37.571-3 Table A.4.3-7/66

pc_GNSS_RTK_BiasInfo_Glonass,                BOOLEAN,       false   #-- @desc  Glo-RTK-BiasInformationSupport-r15 #-- @spec 37.571-3 Table A.4.3-7/74

pc_GNSS_RTK_FKP_Gradients_Bds,               BOOLEAN,       false   #-- @desc  Gnss-RTK-FKP-GradientsSupport-r15 for BDS #-- @spec 37.571-3 Table A.4.3-7/92

pc_GNSS_RTK_FKP_Gradients_Galileo,           BOOLEAN,       false   #-- @desc  Gnss-RTK-FKP-GradientsSupport-r15 for GALILEO #-- @spec 37.571-3 Table A.4.3-7/85

pc_GNSS_RTK_FKP_Gradients_Glonass,           BOOLEAN,       false   #-- @desc  Gnss-RTK-FKP-GradientsSupport-r15 for GLONASS #-- @spec 37.571-3 Table A.4.3-7/78

pc_GNSS_RTK_FKP_Gradients_Gps,               BOOLEAN,       false   #-- @desc  Gnss-RTK-FKP-GradientsSupport-r15 for GPS #-- @spec 37.571-3 Table A.4.3-7/70

pc_GNSS_RTK_MAC_CorrectionDifferences_Bds,   BOOLEAN,       false   #-- @desc  Gnss-RTK-MAC-CorrectionDifferencesSupport-r15 for BDS #-- @spec 37.571-3 Table A.4.3-7/90

pc_GNSS_RTK_MAC_CorrectionDifferences_Galileo,BOOLEAN,       false   #-- @desc  Gnss-RTK-MAC-CorrectionDifferencesSupport-r15 for GALILEO #-- @spec 37.571-3 Table A.4.3-7/83

pc_GNSS_RTK_MAC_CorrectionDifferences_Glonass,BOOLEAN,       false   #-- @desc  Gnss-RTK-MAC-CorrectionDifferencesSupport-r15 for GLONASS #-- @spec 37.571-3 Table A.4.3-7/76

pc_GNSS_RTK_MAC_CorrectionDifferences_Gps,   BOOLEAN,       false   #-- @desc  Gnss-RTK-MAC-CorrectionDifferencesSupport-r15 for GPS #-- @spec 37.571-3 Table A.4.3-7/68

pc_GNSS_RTK_OBS_Bds,                         BOOLEAN,       false   #-- @desc  Gnss-RTK-ObservationsSupport-r15 for BDS #-- @spec 37.571-3 Table A.4.3-7/89

pc_GNSS_RTK_OBS_Bds_B1C,                     BOOLEAN,       false   #-- @desc  Gnss-RTK-ObservationsSupport-r15 for BDS B1C #-- @spec 37.571-3 Table A.4.3-7/106

pc_GNSS_RTK_OBS_Galileo,                     BOOLEAN,       false   #-- @desc  Gnss-RTK-ObservationsSupport-r15 for GALILEO #-- @spec 37.571-3 Table A.4.3-7/82

pc_GNSS_RTK_OBS_Galileo_E5A,                 BOOLEAN,       false   #-- @desc  Gnss-RTK-ObservationsSupport-r15 for Galileo E5A #-- @spec 37.571-3 Table A.4.3-7/105

pc_GNSS_RTK_OBS_Glonass,                     BOOLEAN,       false   #-- @desc  gnss-RTK-ObservationsSupport-r15 for GLONASS #-- @spec 37.571-3 Table A.4.3-7/75

pc_GNSS_RTK_OBS_Gps,                         BOOLEAN,       false   #-- @desc  Gnss-RTK-ObservationsSupport-r15 for GPS #-- @spec 37.571-3 Table A.4.3-7/67

pc_GNSS_RTK_OBS_Gps_L5,                      BOOLEAN,       false   #-- @desc  Gnss-RTK-ObservationsSupport-r15 for GPS L5 #-- @spec 37.571-3 Table A.4.3-7/104

pc_GNSS_RTK_RefStationInfo,                  BOOLEAN,       false   #-- @desc  Gnss-RTK-ReferenceStationInfoSupport-r15 (Common assistance data) #-- @spec 37.571-3 Table A.4.3-7/65

pc_GNSS_RTK_Residuals_Bds,                   BOOLEAN,       false   #-- @desc  Gnss-RTK-ResidualsSupport-r15 for BDS #-- @spec 37.571-3 Table A.4.3-7/91

pc_GNSS_RTK_Residuals_Galileo,               BOOLEAN,       false   #-- @desc  Gnss-RTK-ResidualsSupport-r15 for GALILEO #-- @spec 37.571-3 Table A.4.3-7/84

pc_GNSS_RTK_Residuals_Glonass,               BOOLEAN,       false   #-- @desc  Gnss-RTK-ResidualsSupport-r15 for GLONASS #-- @spec 37.571-3 Table A.4.3-7/77

pc_GNSS_RTK_Residuals_Gps,                   BOOLEAN,       false   #-- @desc  Gnss-RTK-ResidualsSupport-r15 for GPS #-- @spec 37.571-3 Table A.4.3-7/69

pc_GNSS_RTK_SSR_ClockCorrections_Bds,        BOOLEAN,       false   #-- @desc  Gnss-SSR-ClockCorrectionsSupport-r15 for BDS #-- @spec 37.571-3 Table A.4.3-7/94

pc_GNSS_RTK_SSR_ClockCorrections_Galileo,    BOOLEAN,       false   #-- @desc  Gnss-SSR-ClockCorrectionsSupport-r15 for GALILEO #-- @spec 37.571-3 Table A.4.3-7/87

pc_GNSS_RTK_SSR_ClockCorrections_Glonass,    BOOLEAN,       false   #-- @desc  Gnss-SSR-ClockCorrectionsSupport-r15 for GLONASS #-- @spec 37.571-3 Table A.4.3-7/80

pc_GNSS_RTK_SSR_ClockCorrections_Gps,        BOOLEAN,       false   #-- @desc  Gnss-SSR-ClockCorrectionsSupport-r15 for GPS #-- @spec 37.571-3 Table A.4.3-7/72

pc_GNSS_RTK_SSR_CodeBias_Bds,                BOOLEAN,       false   #-- @desc  Gnss-SSR-CodeBiasSupport-r15 for BDS #-- @spec 37.571-3 Table A.4.3-7/95

pc_GNSS_RTK_SSR_CodeBias_Bds_B1C,            BOOLEAN,       false   #-- @desc  Gnss-SSR-CodeBiasSupport-r15 for BDS B1C #-- @spec 37.571-3 Table A.4.3-7/109

pc_GNSS_RTK_SSR_CodeBias_Galileo,            BOOLEAN,       false   #-- @desc  Gnss-SSR-CodeBiasSupport-r15 for GALILEO #-- @spec 37.571-3 Table A.4.3-7/88

pc_GNSS_RTK_SSR_CodeBias_Galileo_E5A,        BOOLEAN,       false   #-- @desc  Gnss-SSR-CodeBiasSupport-r15 for Galileo E5A #-- @spec 37.571-3 Table A.4.3-7/108

pc_GNSS_RTK_SSR_CodeBias_Glonass,            BOOLEAN,       false   #-- @desc  Gnss-SSR-CodeBiasSupport-r15 for GLONASS #-- @spec 37.571-3 Table A.4.3-7/81

pc_GNSS_RTK_SSR_CodeBias_Gps,                BOOLEAN,       false   #-- @desc  Gnss-SSR-CodeBiasSupport-r15 for GPS #-- @spec 37.571-3 Table A.4.3-7/73

pc_GNSS_RTK_SSR_CodeBias_Gps_L5,             BOOLEAN,       false   #-- @desc  Gnss-SSR-CodeBiasSupport-r15 for GPS L5 #-- @spec 37.571-3 Table A.4.3-7/107

pc_GNSS_RTK_SSR_OrbitCorrections_Bds,        BOOLEAN,       false   #-- @desc  Gnss-SSR-OrbitCorrectionsSupport-r15 for BDS #-- @spec 37.571-3 Table A.4.3-7/93

pc_GNSS_RTK_SSR_OrbitCorrections_Galileo,    BOOLEAN,       false   #-- @desc  Gnss-SSR-OrbitCorrectionsSupport-r15 for GALILEO #-- @spec 37.571-3 Table A.4.3-7/86

pc_GNSS_RTK_SSR_OrbitCorrections_Glonass,    BOOLEAN,       false   #-- @desc  Gnss-SSR-OrbitCorrectionsSupport-r15 for GLONASS #-- @spec 37.571-3 Table A.4.3-7/79

pc_GNSS_RTK_SSR_OrbitCorrections_Gps,        BOOLEAN,       false   #-- @desc  Gnss-SSR-OrbitCorrectionsSupport-r15 for GPS #-- @spec 37.571-3 Table A.4.3-7/71

pc_GNSS_RefLocSup,                           BOOLEAN,       false   #-- @desc  Gnss-ReferenceLocationSupport (Common Assistance Data) #-- @spec 37.571-3 Table A.4.3-7/2

pc_GNSS_RefTimeSup,                          BOOLEAN,       false   #-- @desc  Gnss-ReferenceTimeSupport (Common Assistance Data) #-- @spec 37.571-3 Table A.4.3-7/1

pc_GNSS_SSR_GridCorrSupp_Bds,                BOOLEAN,       false   #-- @desc  Gnss-SSR-GriddedCorrectionSupport-r16 for BDS #-- @spec 37.571-3 Table A.4.3-7/132

pc_GNSS_SSR_GridCorrSupp_Galileo,            BOOLEAN,       false   #-- @desc  Gnss-SSR-GriddedCorrectionSupport-r16 for Galileo #-- @spec 37.571-3 Table A.4.3-7/130

pc_GNSS_SSR_GridCorrSupp_Glonass,            BOOLEAN,       false   #-- @desc  Gnss-SSR-GriddedCorrectionSupport-r16 for GLONASS #-- @spec 37.571-3 Table A.4.3-7/131

pc_GNSS_SSR_GridCorrSupp_Gps,                BOOLEAN,       false   #-- @desc  Gnss-SSR-GriddedCorrectionSupport-r16 for GPS #-- @spec 37.571-3 Table A.4.3-7/128

pc_GNSS_SSR_GridCorrSupp_Qzss,               BOOLEAN,       false   #-- @desc  Gnss-SSR-GriddedCorrectionSupport-r16 for QZSS #-- @spec 37.571-3 Table A.4.3-7/129

pc_GNSS_SSR_PhaseBias_Bds_B1C,               BOOLEAN,       false   #-- @desc  Gnss-SSR-PhaseBiasSupport-r16 for BDS B1C #-- @spec 37.571-3 Table A.4.3-7/122

pc_GNSS_SSR_PhaseBias_Bds_B1I,               BOOLEAN,       false   #-- @desc  Gnss-SSR-PhaseBiasSupport-r16 for BDS B1I #-- @spec 37.571-3 Table A.4.3-7/121

pc_GNSS_SSR_PhaseBias_Galileo_E1,            BOOLEAN,       false   #-- @desc  Gnss-SSR-PhaseBiasSupport-r16 for Galileo E1 #-- @spec 37.571-3 Table A.4.3-7/118

pc_GNSS_SSR_PhaseBias_Galileo_E5A,           BOOLEAN,       false   #-- @desc  Gnss-SSR-PhaseBiasSupport-r16 for Galileo E5A #-- @spec 37.571-3 Table A.4.3-7/119

pc_GNSS_SSR_PhaseBias_Glonass,               BOOLEAN,       false   #-- @desc  Gnss-SSR-PhaseBiasSupport-r16 for GLONASS #-- @spec 37.571-3 Table A.4.3-7/120

pc_GNSS_SSR_PhaseBias_Gps_L1CA,              BOOLEAN,       false   #-- @desc  Gnss-SSR-PhaseBiasSupport-r16 for GPS L1 CA #-- @spec 37.571-3 Table A.4.3-7/115

pc_GNSS_SSR_PhaseBias_Gps_L5,                BOOLEAN,       false   #-- @desc  Gnss-SSR-PhaseBiasSupport-r16 for GPS L5 #-- @spec 37.571-3 Table A.4.3-7/116

pc_GNSS_SSR_PhaseBias_Qzss,                  BOOLEAN,       false   #-- @desc  Gnss-SSR-PhaseBiasSupport-r16 for QZSS #-- @spec 37.571-3 Table A.4.3-7/117

pc_GNSS_SSR_STEC_CorrSupp_Bds,               BOOLEAN,       false   #-- @desc  Gnss-SSR-STEC-CorrectionSupport-r16 for BDS #-- @spec 37.571-3 Table A.4.3-7/127

pc_GNSS_SSR_STEC_CorrSupp_Galileo,           BOOLEAN,       false   #-- @desc  Gnss-SSR-STEC-CorrectionSupport-r16 for Galileo #-- @spec 37.571-3 Table A.4.3-7/125

pc_GNSS_SSR_STEC_CorrSupp_Glonass,           BOOLEAN,       false   #-- @desc  Gnss-SSR-STEC-CorrectionSupport-r16 for GLONASS #-- @spec 37.571-3 Table A.4.3-7/126

pc_GNSS_SSR_STEC_CorrSupp_Gps,               BOOLEAN,       false   #-- @desc  Gnss-SSR-STEC-CorrectionSupport-r16 for GPS #-- @spec 37.571-3 Table A.4.3-7/123

pc_GNSS_SSR_STEC_CorrSupp_Qzss,              BOOLEAN,       false   #-- @desc  Gnss-SSR-STEC-CorrectionSupport-r16 for QZSS #-- @spec 37.571-3 Table A.4.3-7/124

pc_GNSS_SSR_URA_Bds,                         BOOLEAN,       false   #-- @desc  Gnss-SSR-URA-Support-r16 for BDS #-- @spec 37.571-3 Table A.4.3-7/114

pc_GNSS_SSR_URA_Galileo,                     BOOLEAN,       false   #-- @desc  Gnss-SSR-URA-Support-r16 for Galileo #-- @spec 37.571-3 Table A.4.3-7/112

pc_GNSS_SSR_URA_Glonass,                     BOOLEAN,       false   #-- @desc  Gnss-SSR-URA-Support-r16 for GLONASS #-- @spec 37.571-3 Table A.4.3-7/113

pc_GNSS_SSR_URA_Gps,                         BOOLEAN,       false   #-- @desc  Gnss-SSR-URA-Support-r16 for GPS #-- @spec 37.571-3 Table A.4.3-7/110

pc_GNSS_SSR_URA_Qzss,                        BOOLEAN,       false   #-- @desc  Gnss-SSR-URA-Support-r16 for QZSS #-- @spec 37.571-3 Table A.4.3-7/111

pc_GNSS_TimeModSup_BDS,                      BOOLEAN,       false   #-- @desc  Gnss-TimeModelsSupport for BDS #-- @spec 37.571-3 Table A.4.3-7/50

pc_GNSS_TimeModSup_Galileo,                  BOOLEAN,       false   #-- @desc  Gnss-TimeModelsSupport for galileo #-- @spec 37.571-3 Table A.4.3-7/8

pc_GNSS_TimeModSup_Glonass,                  BOOLEAN,       false   #-- @desc  Gnss-TimeModelsSupport for glonass #-- @spec 37.571-3 Table A.4.3-7/9

pc_GNSS_TimeModSup_Gps,                      BOOLEAN,       false   #-- @desc  Gnss-TimeModelsSupport for gps #-- @spec 37.571-3 Table A.4.3-7/5

pc_GNSS_TimeModSup_Qzss,                     BOOLEAN,       false   #-- @desc  Gnss-TimeModelsSupport for qzss #-- @spec 37.571-3 Table A.4.3-7/7

pc_GNSS_TimeModSup_Sbas,                     BOOLEAN,       false   #-- @desc  Gnss-TimeModelsSupport for sbas #-- @spec 37.571-3 Table A.4.3-7/6

pc_GNSS_UTCModSup_BDS,                       BOOLEAN,       false   #-- @desc  Gnss-UTC-ModelSupport for BDS #-- @spec 37.571-3 Table A.4.3-7/57

pc_GNSS_UTCModSup_Galileo,                   BOOLEAN,       false   #-- @desc  Gnss-UTC-ModelSupport for galileo #-- @spec 37.571-3 Table A.4.3-7/43

pc_GNSS_UTCModSup_Glonass,                   BOOLEAN,       false   #-- @desc  Gnss-UTC-ModelSupport for glonass #-- @spec 37.571-3 Table A.4.3-7/44

pc_GNSS_UTCModSup_Gps,                       BOOLEAN,       false   #-- @desc  Gnss-UTC-ModelSupport for gps #-- @spec 37.571-3 Table A.4.3-7/40

pc_GNSS_UTCModSup_Qzss,                      BOOLEAN,       false   #-- @desc  Gnss-UTC-ModelSupport for qzss #-- @spec 37.571-3 Table A.4.3-7/42

pc_GNSS_UTCModSup_Sbas,                      BOOLEAN,       false   #-- @desc  Gnss-UTC-ModelSupport for sbas #-- @spec 37.571-3 Table A.4.3-7/41

pc_GPRS,                                     BOOLEAN,       true    #-- @desc  Support of GPRS #-- @spec 51.010-2, A.2/41

pc_G_operation_mode_C,                       BOOLEAN,       false   #-- @desc  GERAN UE Operation Mode C #-- @spec 51.010-2, A.2/49

pc_HCCPCIoT,                                 BOOLEAN,       false   #-- @desc  The UE supports Header compression for control plane CIoT EPS optimisation #-- @spec 36.523-2 A.4.4-2/Z6

pc_HO_from_UTRA,                             BOOLEAN,       false   #-- @desc  Support of Inter-RAT PS handover to E-UTRA from UTRA #-- @spec 

pc_HO_from_UTRA_to_eFDD,                     BOOLEAN,       false   #-- @desc  Support of Inter-RAT PS handover to E-UTRA from UTRA (FDD) #-- @spec 36.523-2 A.4.4-1/8

pc_HO_from_UTRA_to_eTDD,                     BOOLEAN,       false   #-- @desc  Support of Inter-RAT PS handover to E-UTRA from UTRA (TDD) #-- @spec 36.523-2 A.4.4-1/53

pc_HRPD,                                     BOOLEAN,       false   #-- @desc  UE supports CDMA2000 HRPD band class #-- @spec 36.523-2, A.4.1-1/3

pc_HSDPA,                                    BOOLEAN,       false   #-- @desc  UE Supports HSDPA #-- @spec 34.123-2 A.18a/14

pc_HSDPA_FDD,                                BOOLEAN,       false   #-- @desc  UE Supports HSDPA - FDD #-- @spec 34.123-2 A.18a/14

pc_HSDPA_TDD,                                BOOLEAN,       false   #-- @desc  UE Supports HSDPA - TDD #-- @spec 34.123-2 A.18b/10

pc_HSDSCH_UE_Category_Extension4,            INTEGER,       29      #-- @desc  FDD HS-DSCH physical layer category 4 Multi Cell withwithout MIMO extensions #-- @spec 34.123-2 Table A.18a.1d

pc_HSDSCH_UE_Category_Extension4_FDD,        INTEGER,       29      #-- @desc  FDD HS-DSCH physical layer category 4 Multi Cell withwithout MIMO extensions #-- @spec 34.123-2 Table A.18a.1d

pc_HSDSCH_UE_Category_Extension5,            INTEGER,       31      #-- @desc  FDD HS-DSCH physical layer category 5 Multi Cell withwithout MIMO extensions #-- @spec 34.123-2 Table A.18a.1d

pc_HSDSCH_UE_Category_Extension5_FDD,        INTEGER,       31      #-- @desc  FDD HS-DSCH physical layer category 5 Multi Cell withwithout MIMO extensions #-- @spec 34.123-2 Table A.18a.1d

pc_HSDSCH_UE_Category_Extension_FDD,         INTEGER,       5       #-- @desc  FDD HS-DSCH physical layer category extensions #-- @spec 34.123-2 Table A.18a.1a

pc_HSDSCH_UE_Category_FDD,                   INTEGER,       5       #-- @desc  FDD HS-DSCH physical layer categories #-- @spec 34.123-2 Table A.18a.1

pc_HSDSCH_UE_Category_TDD,                   INTEGER,       5       #-- @desc  LCR TDD HS-DSCH physical layer categories #-- @spec 34.123-2 Table A.18b.1

pc_HSUPA,                                    BOOLEAN,       false   #-- @desc  UE Supports HSUPA #-- @spec 34.123-2 A.18a/18

pc_HSUPA_FDD,                                BOOLEAN,       false   #-- @desc  UE Supports HSUPA - FDD #-- @spec 34.123-2 A.18a/18

pc_HSUPA_TDD,                                BOOLEAN,       false   #-- @desc  UE Supports HSUPA - TDD #-- @spec 34.123-2 A.18b/14

pc_Highspeed_Enh_Prach,                      BOOLEAN,       false   #-- @desc  Support high speed enhancement for random access preambles generated from restricted set type B in high speed scenario as specifed in TS 36.211 #-- @spec 36.523-2 A.4.4-1/164

pc_HttpDigestAuthentication,                 BOOLEAN,       false   #-- @desc  HTTP Digest XCAP Authentication #-- @spec 34.229-2, Table A.6a/4

pc_HttpGAAAuthentication,                    BOOLEAN,       false   #-- @desc  GAA XCAP Authentication #-- @spec 34.229-2, Table A.6a/3

pc_HttpGBAAuthentication,                    BOOLEAN,       false   #-- @desc  GBA XCAP Authentication #-- @spec 34.229-2, Table A.6a/3

pc_IMS,                                      BOOLEAN,       false   #-- @desc  Support of IMS #-- @spec 36.523-2 A.4.4-1/25

pc_IMSDataChannel,                           BOOLEAN,       false   #-- @desc  IMS data channel #-- @spec 34.229-2 Table A.15/yy

pc_IMSI_Detach,                              BOOLEAN,       false   #-- @desc  Support of detach for non-EPS services #-- @spec 36.523-2 A.4.4-1/34

pc_IMS_APN_default,                          BOOLEAN,       false   #-- @desc  Configured with IMS APN as default APN #-- @spec 36.523-2 A.4.4-2/11

pc_IMS_Audio_FeatureTag,                     BOOLEAN,       false   #-- @desc  UE supports audio media feature tag #-- @spec 34.229-2 Table A.12/xx

pc_IMS_CS_PS_SRVCC,                          BOOLEAN,       false   #-- @desc  UE Supports CS to PS SRVCC #-- @spec 34.229-2 A.12/40

pc_IMS_CS_PS_SRVCCAlert,                     BOOLEAN,       false   #-- @desc  UE Supports CS to PS SRVCC in alerting state #-- @spec 34.229-2 A.12/41

pc_IMS_CS_PS_SRVCCMidCall,                   BOOLEAN,       false   #-- @desc  UE Supports CS to PS SRVCC and the MSC server assisted mid-call feature #-- @spec 34.229-2 A.12/42

pc_IMS_Deregistration,                       BOOLEAN,       false   #-- @desc  UE has the method that supports IMS deregistration #-- @spec 34.229-2 Table A.12/39

pc_IMS_Disable_Preconditions,                BOOLEAN,       false   #-- @desc  UE supports disabling preconditions #-- @spec 34.229-2 Table A.12/59

pc_IMS_E2ae,                                 BOOLEAN,       false   #-- @desc  UE supports end-to-access-edge media security using SDES #-- @spec 34.229-2 Table A.12/31

pc_IMS_EmergencyCall,                        BOOLEAN,       false   #-- @desc  UE supports IMS emergency services #-- @spec 34.229-2 Table A.12/26

pc_IMS_ExplicitConsultativeTransfer,         BOOLEAN,       false   #-- @desc  Explicit Communication Transfer - consultative transfer #-- @spec 34.229-2 Table A.16/11

pc_IMS_GIBA_Sec,                             BOOLEAN,       false   #-- @desc  UE supports GIBA security only #-- @spec 34.229-2 Table A.6a/1

pc_IMS_GRUUsInSIP,                           BOOLEAN,       false   #-- @desc  UE supports obtaining and using GRUUs in the Session Initiation Protocol (SIP) #-- @spec 34.229-2 Table A.4/53

pc_IMS_Geolocation,                          BOOLEAN,       false   #-- @desc  UE is capable of obtaining location information #-- @spec 34.229-2 Table A.12/27

pc_IMS_RtcpDuringVoiceSession,               BOOLEAN,       false   #-- @desc  RTCP used during voice session #-- @spec 34.229 ???

pc_IMS_SRVCCAlert,                           BOOLEAN,       false   #-- @desc  UE indicates g.3gpp.srvcc-alerting media feature tag in INVITE request or 180 response #-- @spec 34.229-2 A.12/34

pc_IMS_Sec,                                  BOOLEAN,       true    #-- @desc  UE supports full IMS security #-- @spec 34.229-2 Table A.6a/2

pc_IMS_SessionIdSupported,                   BOOLEAN,       false   #-- @desc  UE supports session id #-- @spec 34.229-2 Table A.12/30

pc_IMS_Session_Timer,                        BOOLEAN,       false   #-- @desc  UE supports Session Timer #-- @spec 34.229-2 Table A.12/57

pc_IMS_Session_Timer_own_benefit,            BOOLEAN,       false   #-- @desc  UE uses Session Timer for its benefit alone #-- @spec 34.229-2 Table A.12/60

pc_IMS_Session_Timer_reINVITE,               BOOLEAN,       false   #-- @desc  UE supports usage of re-INVITE for session refresh #-- @spec 34.229-2 Table A.12/61

pc_IMS_TWS,                                  BOOLEAN,       false   #-- @desc  Three way session #-- @spec 34.229-2, Table A.16/14

pc_IMS_Video_FeatureTag,                     BOOLEAN,       false   #-- @desc  UE indicates video media feature tag in REGISTER and INVITE request #-- @spec 34.229-2 Table A.12/32

pc_IMS_after_EmReg_rejection,                BOOLEAN,       false   #-- @desc  UE reattempts IMS emergency service without registration after rejection of emergency registration #-- @spec 34.229-2 Table A.12/zz

pc_IMS_eCall_Capable,                        BOOLEAN,       false   #-- @desc  UE supports IMS eCall type of emergency services #-- @spec 34.229-2 Table A.12/54

pc_IMS_eCall_Only,                           BOOLEAN,       false   #-- @desc  UE supports IMS eCall Only type of emergency services #-- @spec 34.229-2 Table A.12/55

pc_IMS_emergency_call,                       BOOLEAN,       false   #-- @desc  Support of MS emergency call #-- @spec 36.523-2, A.4.2.1.1-1/4

pc_IP_PDN,                                   BOOLEAN,       false   #-- @desc  UE capable of requesting PDN of type "IP" #-- @spec 36.523-2 A.4.4-2/Z2

pc_IP_Ping,                                  BOOLEAN,       false   #-- @desc  Support of ICMP or ICMP IPv6 #-- @spec 38.508-2 Table A.4.4-1/1

pc_IPv4,                                     BOOLEAN,       true    #-- @desc  UE supports IPv4 (used IMS PICS as currently not defined in LTE) #-- @spec 34.229-2 A.7/1

pc_IPv4_Link_MTU_Parameter,                  BOOLEAN,       false   #-- @desc  UE supports IPv4 Link MTU parameter #-- @spec 36.523-2 A.4.4-2/Z4

pc_IPv6,                                     BOOLEAN,       TRUE    #-- @desc  UE supports IPv6 (used IMS PICS as currently not defined in LTE) #-- @spec 34.229-2 A.7/2

pc_IR_92,                                    BOOLEAN,       false   #-- @desc  Support of IR.92 #-- @spec 

pc_ISR,                                      BOOLEAN,       false   #-- @desc  Support of ISR #-- @spec 36.523-2 A.4.4-1/5

pc_ImmConnect,                               BOOLEAN,       false   #-- @desc  Immediate connection supported for all circuit switched basic services #-- @spec 34.123-2 A.20/6

pc_IndicateSigcomp,                          BOOLEAN,       false   #-- @desc  Indicate the willingness to receive the responses and requests compressed from initial REGISTER onwards by using the "comp=sigcomp" parameter #-- @spec 34.229-2 Table A.8/5

pc_InitiateP_CSCFDiscovery_viaDHCPv4,        BOOLEAN,       false   #-- @desc  UE capable of being configured to initiate P-CSCF discovery via DHCPv4 #-- @spec 34.229-2 Table A.13/1

pc_InitiateP_CSCFDiscovery_viaDHCPv6,        BOOLEAN,       false   #-- @desc  UE capable of being configured to initiate P-CSCF discovery via DHCPv6 #-- @spec 34.229-2 Table A.12/7

pc_InitiateP_CSCFDiscovery_viaPCO,           BOOLEAN,       false   #-- @desc  UE capable of being configured to initiate P-CSCF discovery via PCO #-- @spec 34.229-2 Table A.12/5

pc_InitiateSession,                          BOOLEAN,       false   #-- @desc  Initiating a session #-- @spec 34.229-2 Table A.4/2B

pc_InitiatesDedicatedPDPContext,             BOOLEAN,       false   #-- @desc  UE capable of being configured to initiate Dedicated PDP Context #-- @spec 34.229-2 Table A.12/4

pc_InterBand_ENDC_IncludingFR1_FR2,          BOOLEAN,       false   #-- @desc  Inter-Band EN-DC including both FR1 and FR2 #-- @spec 38.508-2 Table A.4.1-4/5

pc_InterBand_ENDC_IncludingFR2,              BOOLEAN,       false   #-- @desc  Inter-Band EN-DC including FR2 #-- @spec 38.508-2 Table A.4.1-4/4

pc_InterBand_ENDC_WithinFR1,                 BOOLEAN,       false   #-- @desc  Inter-Band EN-DC within FR1 #-- @spec 38.508-2 Table A.4.1-4/3

pc_InterBand_NRDC_BetweenFR1_FR2,            BOOLEAN,       false   #-- @desc  Inter-Band EN-DC bewtween FR1 and FR2 #-- @spec 38.508-2 Table A.4.1-4/6

pc_InterFreq_ProximityIndication,            BOOLEAN,       false   #-- @desc  Support of Inter Frequency Proximity Indication #-- @spec 36.523-2 A.4.4.1-b

pc_InterFreq_RSTD_WithGaps,                  BOOLEAN,       false   #-- @desc  Support of inter-frequency RSTD measurements that require measurement gaps #-- @spec 37.571-3 Table A.4.3-2/16

pc_InterFreq_RSTD_withGaps,                  BOOLEAN,       false   #-- @desc  Support of inter-frequency RSTD measurements that require measurement gaps #-- @spec 37.571-3 Table A.4.3-2/16

pc_InterRAT_DL_CompressedModeRequired,       BOOLEAN,       true    #-- @desc  UE supports DL DPCH compressed mode #-- @spec 34.123-2 A.18a/9a

pc_InterRAT_UL_CompressedModeRequired,       BOOLEAN,       true    #-- @desc  UE supports UL DPCH compressed mode #-- @spec 34.123-2 A.18a/8a

pc_Interactive,                              BOOLEAN,       false   #-- @desc  UE Supports Interactive QoS class #-- @spec 34.123-2 A.6/3

pc_IntraBand_Contiguous_ENDC,                BOOLEAN,       false   #-- @desc  Intra-Band Contiguous EN-DC #-- @spec 38.508-2 Table A.4.1-4/1

pc_IntraBand_NonContiguous_ENDC,             BOOLEAN,       false   #-- @desc  Intra-Band Non-Contiguous EN-DC #-- @spec 38.508-2 Table A.4.1-4/2

pc_IntraFreqA3_CE_ModeA,                     BOOLEAN,       false   #-- @desc  Support of eventA3 for intra-frequency neighbouring cells in normal coverage and CE Mode A #-- @spec 36.523-2 A.4.4-1/1xx1

pc_IntraFreqHO_CE_ModeA,                     BOOLEAN,       false   #-- @desc  Support of intra-frequency handover to target cell in normal coverage and CE Mode A #-- @spec 36.523-2 A.4.4-1/1xx2

pc_IntraFreq_ProximityIndication,            BOOLEAN,       false   #-- @desc  Support of Intra Frequency Proximity Indication #-- @spec 36.523-2 A.4.4.1-a

pc_KeepEpsBearerParametersAfterNormalDetach, BOOLEAN,       false   #-- @desc  If the UE supports this then the next ATTACH after DETACH shall be done using AT command AT+CGATT=1. #-- @spec 36.523-2 A.4.4.2-10

pc_LAP,                                      BOOLEAN,       false   #-- @desc  Support of Low Access Priority Indication. Also defined in 36.523-2 A4.4-183 #-- @spec 34.123-2 A.10/31

pc_LAP_override,                             BOOLEAN,       false   #-- @desc  Support of Low Access Prioirty Override #-- @spec 36.523-2 A.4.4-1/90

pc_LPP,                                      BOOLEAN,       false   #-- @desc  LTE Positioning Protocol (LPP) #-- @spec 37.571-3 Table A.4.2-1/1

pc_LPP_MsgSegmentation,                      BOOLEAN,       false   #-- @desc  Support of LPP message segmentation #-- @spec 37.571-3 Table A.4.4-1/5

pc_LPP_SendingACK_ProvideCapabilities,       BOOLEAN,       false   #-- @desc  Support of sending of acknowledgement request in LPP Provide Capabilities message #-- @spec 37.571-3 Table A.4.4-1/1

pc_LTE_UL_Segmentation,                      BOOLEAN,       false   #-- @desc  Support of RRC message Segmentation in the UL #-- @spec 36.523-2 A.4.4-1/216

pc_LocalTimeZone,                            BOOLEAN,       false   #-- @desc  Support of storage of the local time zone #-- @spec 36.523-2 A.4.4-1/14

pc_LoggedMeasurementsIdle,                   BOOLEAN,       false   #-- @desc  Support of logged measurements in RRC_IDLE #-- @spec 36.523-2 A.4.4-1/62

pc_Loggedmeasurements_Idle_PCH,              BOOLEAN,       FALSE   #-- @desc  Support of logged measurements in Idle mode and PCH States #-- @spec 34.123-2 Table A.20/85

pc_LosslessSRNS_Reloc,                       BOOLEAN,       FALSE   #-- @desc  Lossless SRNS Relocation is supported #-- @spec 34.123-2 Table A.19a/2

pc_MBS_AcquisitionAssist,                    BOOLEAN,       false   #-- @desc  Support of mbs-AcquisitionAssistance #-- @spec 37.571-3 Table A.4.3-7A/2

pc_MBS_AlmanacAssist,                        BOOLEAN,       false   #-- @desc  Support of mbs-AlmanacAssistance #-- @spec 37.571-3 Table A.4.3-7A/1

pc_MFBI_FrequencyBand1,                      INTEGER,       5       #-- Anritsu TTCN CR required for MFBI #-- @spec 

pc_MFBI_FrequencyBand2,                      INTEGER,       18      #-- Anritsu TTCN CR required for MFBI #-- @spec 

pc_MFBI_FrequencyBand3,                      INTEGER,       19      #-- Anritsu TTCN CR required for MFBI #-- @spec 

pc_MFBI_FrequencyBand4,                      INTEGER,       26      #-- Anritsu TTCN CR required for MFBI #-- @spec 

pc_MFBI_FrequencyBand5,                      INTEGER,       27      #-- Anritsu TTCN CR required for MFBI #-- @spec 

pc_MFBI_FrequencyBand6,                      INTEGER,       33      #-- Anritsu TTCN CR required for MFBI #-- @spec 

pc_MFBI_FrequencyBand7,                      INTEGER,       38      #-- Anritsu TTCN CR required for MFBI #-- @spec 

pc_MFBI_FrequencyBand8,                      INTEGER,       41      #-- Anritsu TTCN CR required for MFBI #-- @spec 

pc_MGPS,                                     BOOLEAN,       false   #-- @desc  Support for Modernized GPS #-- @spec 37.571-3 Table A.4.3-1/8

pc_MICO_Mode,                                BOOLEAN,       false   #-- @desc  Support of MICO mode #-- @spec 38.508-2 Table A.4.3.7-1/59

pc_MTSI_ACR,                                 BOOLEAN,       false   #-- @desc  MTSI supplementary services - Anonymous Communication Rejection #-- @spec 34.229-2 Table A.16/12

pc_MTSI_CB,                                  BOOLEAN,       false   #-- @desc  MTSI supplementary services - Communication Barring #-- @spec 34.229-2 Table A.16/7

pc_MTSI_CommDivert,                          BOOLEAN,       false   #-- @desc  MTSI supplementary services - Communication Diversion #-- @spec 34.229-2 Table A.16/5

pc_MTSI_CommHold,                            BOOLEAN,       false   #-- @desc  Communication Hold #-- @spec 34.229-2 Table A.16/6

pc_MTSI_CommWaiting,                         BOOLEAN,       false   #-- @desc  MTSI supplementary services - Communication Waiting #-- @spec 34.229-2 Table A.16/13

pc_MTSI_Conference,                          BOOLEAN,       false   #-- @desc  MTSI supplementary services - Conference #-- @spec 34.229-2 Table A.16/9

pc_MTSI_Incoming_CB,                         BOOLEAN,       false   #-- @desc  MTSI supplementary services - Incoming Communication Barring #-- @spec 34.229-2 Table A.16/7

pc_MTSI_MessageWait,                         BOOLEAN,       false   #-- @desc  MTSI supplementary services - Message Waiting Indication #-- @spec 34.229-2 Table A.16/8

pc_MTSI_NetworkInvitationToConference,       BOOLEAN,       false   #-- @desc  MTSI supplementary services - Network Invitation to Conference #-- @spec 34.229-2 Table A.16/16

pc_MTSI_OIP,                                 BOOLEAN,       false   #-- @desc  MTSI supplementary services - Originating Identification Presentation #-- @spec 34.229-2 Table A.16/1

pc_MTSI_OIR,                                 BOOLEAN,       false   #-- @desc  MTSI supplementary services - Originating Identification Restriction #-- @spec 34.229-2 Table A.16/2

pc_MTSI_OIR_C,                               BOOLEAN,       false   #-- @desc  MTSI supplementary services - Originating Identification Restriction - Configuration #-- @spec 34.229-2 Table A.16/2A

pc_MTSI_OOD_REFER,                           BOOLEAN,       false   #-- @desc  UE supports Fixed Out of Dialog REFER #-- @spec 34.229-2 Table A.16/17

pc_MTSI_Outgoing_CB,                         BOOLEAN,       false   #-- @desc  MTSI supplementary services - Outgoing Communication Barring #-- @spec 34.229-2 Table A.16/15

pc_MTSI_Speech,                              BOOLEAN,       false   #-- @desc  MTSI media - Speech #-- @spec 34.229-2 Table A.15/1

pc_MTSI_Speech_AMRWB,                        BOOLEAN,       false   #-- @desc  MTSI media - Speech AMR wideband #-- @spec 34.229-2 Table A.15/2

pc_MTSI_Speech_EVS,                          BOOLEAN,       false   #-- @desc  MTSI media - Speech EVS #-- @spec 34.229-2 Table A.15/10

pc_MTSI_TIP,                                 BOOLEAN,       false   #-- @desc  MTSI supplementary services - Terminating Identification Presentation #-- @spec 34.229-2 Table A.16/3

pc_MTSI_TIR,                                 BOOLEAN,       false   #-- @desc  MTSI supplementary services - Terminating Identification Restriction #-- @spec 34.229-2 Table A.16/4

pc_MTSI_TIR_C,                               BOOLEAN,       false   #-- @desc  MTSI supplementary services - Terminating Identification Restriction - Configuration #-- @spec 34.229-2 Table A.16/4A

pc_MTSI_Text_RTP,                            BOOLEAN,       false   #-- @desc  MTSI media - Text RTP #-- @spec 34.229-2 Table A.15/7

pc_MTSI_Video,                               BOOLEAN,       false   #-- @desc   MTSI media - Video #-- @spec 34.229-2 Table A.15/3

pc_MTSI_rtt,                                 BOOLEAN,       false   #-- @desc  Real-time text #-- @spec 34.229-2 Table A.15/15

pc_MT_LR,                                    BOOLEAN,       false   #-- @desc  Support of Mobile Terminated location request #-- @spec 37.571-3 tabel A.4.3-3/8

pc_MT_LR_loc_notif,                          BOOLEAN,       false   #-- @desc  Support of EPC-MT-LR Location Notification #-- @spec 37.571-3 Table A.4.3-3/3

pc_Manual_CSG_Selection,                     BOOLEAN,       false   #-- @desc  Support of Manual CSG selection #-- @spec 36.523-2 A.4.4-1/49

pc_MinimumPeriodicSearchTimer,               BOOLEAN,       false   #-- @desc  Support of Minimum Periodic Search Timer #-- @spec 34.123-2 A.10/32

pc_More_Than_128_CAbandComb,                 BOOLEAN,       false   #-- @desc  Support of more than 128 CA Band Combinations #-- @spec 36.523-2 A.4.4.1/102

pc_Multi_RTT,                                BOOLEAN,       false   #-- @desc  Support for UE-Assisted Multi-RTT #-- @spec 37.571-3 Table A.4.3-2/29

pc_Multi_RTT_additionalPathsReport,          BOOLEAN,       false   #-- @desc  Support of additionalPathsReport #-- @spec 37.571-3 Table A.4.3-6C/7

pc_Multi_RTT_periodicalReporting,            BOOLEAN,       false   #-- @desc  Support of periodicalReporting #-- @spec 37.571-3 Table A.4.3-6C/8

pc_MultimediaTelephonyService,               BOOLEAN,       false   #-- @desc  Multimedia telephony service participant #-- @spec 34.229-2 Table A.3A/50

pc_MultipleIMPU,                             BOOLEAN,       false   #-- @desc  UE supports multiple IMPU #-- @spec 34.229-2 Table A.12/48

pc_Multiple_Cells_Meas_Ext,                  BOOLEAN,       false   #-- @desc  Support of measurement reporting triggered based on a number of cells #-- @spec 36.523-2 A.4.4-1/kkk

pc_Multiple_PDN,                             BOOLEAN,       false   #-- @desc  Support for multiple PDN connections #-- @spec 36.523-2 A.4.4-1/30

pc_NB,                                       BOOLEAN,       false   #-- @desc  NB-IoT #-- @spec 36.523-2 A.4.1-1/8

pc_NB_Control_Plane_CIoT_Optimisation_EDT,   BOOLEAN,       false   #-- @desc  Support of Control Plane CIoT Optimization Early Data Transmission over NB-IoT #-- @spec 36.523-2 A.4.4-1/255

pc_NB_Control_Plane_data_backoff,            BOOLEAN,       false   #-- @desc  Support of control plane data back-off timer T3448 #-- @spec 36.523-2 A.4.4-1/kkk

pc_NB_FDD,                                   BOOLEAN,       false   #-- @desc  NB-IoT FDD #-- @spec 36.523-2 A.4.1-1/8

pc_NB_InterferenceRandomisation,             BOOLEAN,       false   #-- @desc  Support of interference randomisation in connected mode in NB-IoT #-- @spec 36.523-2 A.4.4-1A/Y3

pc_NB_MultiCarrier,                          BOOLEAN,       false   #-- @desc  Support of multi-carrier operation in NB-IoT #-- @spec 36.523-2 A.4.4-1/X5

pc_NB_MultiCarrier_NPRACH,                   BOOLEAN,       false   #-- @desc  Support of PRACH on non-anchor carrier in NB-IoT #-- @spec 36.523-2 A.4.4-1A/Y1

pc_NB_MultiCarrier_Paging,                   BOOLEAN,       false   #-- @desc  Support of paging on non-anchor carrier in NB-IoT #-- @spec 36.523-2 A.4.4-1A/12

pc_NB_MultiCarrier_Paging_TDD,               BOOLEAN,       false   #-- @desc  Support of paging on non-anchor carriers for TDD in NB-IoT #-- @spec 36.523-2 A.4.4-1A/17

pc_NB_MultiDRB,                              BOOLEAN,       false   #-- @desc  Support of multiple DRBs in NB-IoT #-- @spec 36.523-2 A.4.4-1/X6

pc_NB_MultiTone,                             BOOLEAN,       false   #-- @desc  Support of UL multi-tone transmissions on NPUSCH in NB-IoT #-- @spec 36.523-2 A.4.4-1/X4

pc_NB_RLC_UM,                                BOOLEAN,       false   #-- @desc  Support of RLC UM mode in NB-IoT #-- @spec 36.523-2 A.4.4-1/202

pc_NB_Rai_Support,                           BOOLEAN,       false   #-- @desc  Support of 2 Release Assistance Indication (RAI) in NB-IoT #-- @spec 36.523-2 A.4.4-1/X2

pc_NB_Report_Coarse_Location_Information_NAS,BOOLEAN,       false   #-- @desc  Support of reporting coarse location information via NAS #-- @spec 36.523-2 A.4.4-1/aaa

pc_NB_S1_only,                               BOOLEAN,       false   #-- @desc  UE supports only NB-S1 mode (i.e. NB-IoT) #-- @spec 36.523-2 A.4.4-2/Z0

pc_NB_TDD,                                   BOOLEAN,       false   #-- @desc  NB-IoT TDD #-- @spec 36.523-2 A.4.1-1/9

pc_NB_TwoHARQ_Processes,                     BOOLEAN,       false   #-- @desc  Support of 2 HARQ processes in DL and UL in NB-IoT #-- @spec 36.523-2 A.4.4-1/X1

pc_NB_User_Plane_CIoT_Optimisation,          BOOLEAN,       false   #-- @desc  Support of User Plane CIoT in NB-S1 mode #-- @spec 36.523-2 A.4.4-1/199

pc_NB_User_Plane_CIoT_Optimisation_EDT,      BOOLEAN,       false   #-- @desc  Support of User Plane CIoT Optimization Early Data Transmission over NB-IoT #-- @spec 36.523-2 A.4.4-1/256

pc_NB_earlyContentionResolution_r14,         BOOLEAN,       false   #-- @desc  Support of Early contention resolution in NB-IoT #-- @spec 36.523-2 A.4.4-1A/18

pc_NB_mixedOperationMode,                    BOOLEAN,       false   #-- @desc  Support of Mixed Operation Mode in NB-IoT #-- @spec 36.523-2 A.4.4-1/218

pc_NB_multiCarrier_Paging,                   BOOLEAN,       false   #-- @desc  Support of paging on non-anchor carrier in NB-IoT #-- @spec 36.523-2 A.4.4-1A/Y2

pc_NB_nprach_Format2,                        BOOLEAN,       false   #-- @desc  Support of NPRACH resources using preamble format 2 for FDD in NB-IoT #-- @spec 36.523-2 A.4.4-1/219

pc_NB_ntn_Connectivity_EPC,                  BOOLEAN,       false   #-- @desc  Support of NTN access in NB-IoT #-- @spec 36.523-2 A.4.4-1/230

pc_NB_ntn_DL_HARQ_disable_RRC_singleTB,      BOOLEAN,       false   #-- @desc Support for disabling HARQ feedback for a single TB per HARQ process in downlink transmission through RRC configuration #-- @spec 36.523-2 A.4.4-1/253

pc_NB_ntn_DiscontinuousCoverage,             BOOLEAN,       false   #-- @desc  Support of Discontinuous coverage #-- @spec 36.523-2 A.4.4-1/260

pc_NB_ntn_GSO_ScenarioSupport,               BOOLEAN,       false   #-- @desc  Support of NTN features in GSO scenario in NB-IoT #-- @spec 36.523-2 A.4.4-1/234

pc_NB_ntn_NGSO_ScenarioSupport,              BOOLEAN,       false   #-- @desc  Support of NTN features in NGSO scenario in NB-IoT #-- @spec 36.523-2 A.4.4-1/237

pc_NB_ntn_OffsetTimingEnh,                   BOOLEAN,       false   #-- @desc  Support of timing relationship enhancements using Differential Koffset in NB-IoT #-- @spec 36.523-2 A.4.4-1/233

pc_NB_ntn_PUR_TimerEnhancement,              BOOLEAN,       false   #-- @desc  Support of modified timer value for PUR operation required for NTN operation in NB-IoT #-- @spec 36.523-2 A.4.4-1/232

pc_NB_ntn_TA_Report,                         BOOLEAN,       false   #-- @desc  Support of Timing advance reporting in NTN cell in NB-IoT #-- @spec 36.523-2 A.4.4-1/231

pc_NB_ntn_UL_HARQ_MODE_B_singleTB,           BOOLEAN,       false   #-- @desc Support of uplink HARQ mode B for a single TB per HARQ process #-- @spec 36.523-2 A.4.4-1/254

pc_NB_ntn_Uplink_Tx_Extension,               BOOLEAN,       false   #-- @desc  Support of NTN features in NGSO scenario in NB-IoT #-- @spec 36.523-2 A.4.4-1/237

pc_NB_ntn_autonomous_GNSS_position_fix,      BOOLEAN,       false   #-- @desc  Support of autonomous GNSS position fix #-- @spec 36.523-2 A.4.4-1/264

pc_NB_ntn_only_Connectivity_EPC,             BOOLEAN,       false   #-- @desc  Support of NTN only access in NB-IoT #-- @spec 36.523-2 A.4.4-1/KKK

pc_NB_ntn_triggered_GNSS_position_fix,       BOOLEAN,       false   #-- @desc  Support of network triggered GNSS position fix #-- @spec 36.523-2 A.4.4-1/258

pc_NG102_Call_Combined_Registration_EUTRA,   BOOLEAN,       false   #-- @desc  Voice call after combined Registration E-UTRA #-- @spec 34.229-2 Table A.20/5

pc_NG102_Call_Combined_Registration_WLAN,    BOOLEAN,       false   #-- @desc  Voice call after combined Registration WLAN #-- @spec 34.229-2 Table A.20/7

pc_NG102_Combined_Registration_EUTRA,        BOOLEAN,       false   #-- @desc  Combined Registration E-UTRA #-- @spec 34.229-2 Table A.20/1

pc_NG102_Combined_Registration_WLAN,         BOOLEAN,       false   #-- @desc  Combined Registration WLAN #-- @spec 34.229-2 Table A.20/3

pc_NG102_Dual_Registration_EUTRA,            BOOLEAN,       false   #-- @desc  Dual Registration E-UTRA #-- @spec 34.229-2 Table A.20/2

pc_NG114,                                    BOOLEAN,       false   #-- @desc  GSMA PRD NG.114 #-- @spec 34.229-2 A.21/3

pc_NG114_v1_0,                               BOOLEAN,       false   #-- @desc  Version 1.0 as of 07 August 2020 #-- @spec 34.229-2 Table A.21/1

pc_NG114_v1_0_EVS_A1,                        BOOLEAN,       false   #-- @desc  EVS Configuration A1 #-- @spec 34.229-2 Table A.22/mm

pc_NG114_v1_0_EVS_B0,                        BOOLEAN,       false   #-- @desc  EVS Configuration B0 #-- @spec 34.229-2 Table A.22/nn

pc_NG114_v1_0_audio,                         BOOLEAN,       false   #-- @desc  audio feature tag #-- @spec 34.229-2 Table A.22/

pc_NG114_v1_0_default_config_evs_br,         BOOLEAN,       false   #-- @desc  Annex C.3 default configuration for EVSBr #-- @spec 34.229-2 Table A.22/10

pc_NG114_v1_0_default_config_evs_bw,         BOOLEAN,       false   #-- @desc  Annex C.3 default configuration for EVSBw #-- @spec 34.229-2 Table A.22/11

pc_NG114_v1_0_default_config_voice_exempt,   BOOLEAN,       false   #-- @desc  Annex C.3 default configuration for voice exempt #-- @spec 34.229-2 Table A.22/8

pc_NG114_v1_0_final_SDP_offer,               BOOLEAN,       false   #-- @desc  final codec selection #-- @spec 34.229-2 Table A.22/

pc_NG114_v1_0_first_SDP_answer,              BOOLEAN,       false   #-- @desc  Codecs and attributes in answer to initial SDP offer #-- @spec 34.229-2 Table A.22/12

pc_NG114_v1_0_forking,                       BOOLEAN,       false   #-- @desc  Forking behavior #-- @spec 34.229-2 Table A.22/14

pc_NG114_v1_0_initial_SDP_offer,             BOOLEAN,       false   #-- @desc  Codecs and attributes in initial SDP offer #-- @spec 34.229-2 Table A.22/

pc_NG114_v1_0_mmtel,                         BOOLEAN,       false   #-- @desc  mmtel ICSI value #-- @spec 34.229-2 Table A.22/

pc_NG114_v1_0_second_SDP_answer,             BOOLEAN,       false   #-- @desc  Codecs and attributes in answer to second SDP offer #-- @spec 34.229-2 Table A.22/13

pc_NG114_v1_0_video,                         BOOLEAN,       false   #-- @desc  video feature tag #-- @spec 34.229-2 Table A.22/

pc_NG114_v2_0,                               BOOLEAN,       false   #-- @desc  Version 2.0 as of 07 August 2021 #-- @spec 34.229-2 Table A.21/2

pc_NG114_v2_0_default_config_video_exempt,   BOOLEAN,       false   #-- @desc  Annex C.3 default configuration for video exempt #-- @spec 34.229-2 Table A.22/9

pc_NG_RAN_NR,                                BOOLEAN,       false   #-- @desc  NG-RAN NR (Option 2) #-- @spec 38.508-2 Table A.4.1-3/1

pc_NMO_I_Behaviour,                          BOOLEAN,       false   #-- @desc  Support of the extended NMO I system information #-- @spec 34.123-2 A.10/33

pc_NR_5GC_EmergencyServices,                 BOOLEAN,       false   #-- @desc  Support of emergency services in NR connected to 5GCN #-- @spec 38.508-2 Table A.4.3.7-1/14

pc_NR_ECID,                                  BOOLEAN,       false   #-- @desc  Support for UE-Assisted NR E-CID #-- @spec 37.571-3 Table A.4.3-2/34

pc_NR_ECID_CSIRsrp,                          BOOLEAN,       false   #-- @desc  Support of CSI RSRP #-- @spec 37.571-3 Table A.4.3-6A/3

pc_NR_ECID_CSIRsrq,                          BOOLEAN,       false   #-- @desc  Support of CSI RSRQ #-- @spec 37.571-3 Table A.4.3-6A/4

pc_NR_ECID_SSRsrp,                           BOOLEAN,       false   #-- @desc  Support of SS RSRP #-- @spec 37.571-3 Table A.4.3-6A/1

pc_NR_ECID_SSRsrq,                           BOOLEAN,       false   #-- @desc  Support of SS RSRQ #-- @spec 37.571-3 Table A.4.3-6A/2

pc_NR_ECID_periodicalReporting,              BOOLEAN,       false   #-- @desc  Support of periodicalReporting #-- @spec 37.571-3 Table A.4.3-6A/5

pc_NR_ECID_triggeredReporting,               BOOLEAN,       false   #-- @desc  Support of triggeredReporting #-- @spec 37.571-3 Table A.4.3-6A/6

pc_NR_UL_SRS_Capability,                     BOOLEAN,       false   #-- @desc  Support for NR UL-SRS-Capability #-- @spec 37.571-3 Table A.4.3-2/35

pc_NR_mpsPriorityIndication_r16,             BOOLEAN,       false   #-- @desc  Support of mpsPriorityIndication on RRC release with redirect #-- @spec 38.508-2 Table A.4.4-1/26

pc_Navic_DGNSS_Sup,                          BOOLEAN,       false   #-- @desc  Navic-DifferentialCorrectionsSupport-r16 for #-- @spec 37.571-3 Table A.4.3-7/133

pc_Navic_GridModelSupp,                      BOOLEAN,       false   #-- @desc  Navic-GridModelSupport-r16 #-- @spec 37.571-3 Table A.4.3-7/134

pc_No_USIM_TestExecution,                    BOOLEAN,       false   #-- @desc  Support of test execution with no USIM #-- @spec 34.123-2 A.20/90

pc_NonCallRelSS,                             BOOLEAN,       FALSE   #-- @desc  At least one non-call related Supplementary Service supported #-- @spec 34.123-2 Table A.7/30

pc_NonIP_Link_MTU_Parameter,                 BOOLEAN,       false   #-- @desc  UE supports Non-IP Link MTU parameter #-- @spec 36.523-2 A.4.4-2/Z3

pc_NonIP_PDN,                                BOOLEAN,       false   #-- @desc  UE capable of requesting PDN of type "Non-IP" #-- @spec 36.523-2 A.4.4-2/Z1

pc_NumberOfTriggeringCells_meas,             BOOLEAN,       false   #-- @desc  Support of measurement triggering based on number of cells above a threshold #-- @spec 36.523-2 A.4.4-1/kkk

pc_OMA_LPPe,                                 BOOLEAN,       false   #-- @desc  Support for OMA LPPe #-- @spec 37.571-3 Table A.4.2-1/2

pc_OTDOA,                                    BOOLEAN,       false   #-- @desc  Support of UE assisted OTDOA #-- @spec 37.571-3 Table A.4.3-2/4

pc_OTDOA_additionalNeighbourCellInfoList,    BOOLEAN,       false   #-- @desc  Support of additionalNeighbourCellInfoList #-- @spec 37.571-3 Table A.4.3-3A/2

pc_OTDOA_additionalPathsReport,              BOOLEAN,       false   #-- @desc  Support of additionalPathsReport #-- @spec 37.571-3 Table A.4.3-3A/7

pc_OTDOA_additional_prs_config,              BOOLEAN,       false   #-- @desc  Support of additional-prs-config #-- @spec 37.571-3 Table A.4.3-3A/5

pc_OTDOA_densePrsConfig,                     BOOLEAN,       false   #-- @desc  Support of densePrsConfig #-- @spec 37.571-3 Table A.4.3-3A/8

pc_OTDOA_idleStateForMeasurements,           BOOLEAN,       false   #-- @desc  Support of idleStateForMeasurements #-- @spec 37.571-3 Table A.4.3-3A/15

pc_OTDOA_interFreqRSTDmeasurement,           BOOLEAN,       false   #-- @desc  Support of interFreqRSTDmeasurement #-- @spec 37.571-3 Table A.4.3-3A/1

pc_OTDOA_interRAT_RSTDmeasurement,           BOOLEAN,       false   #-- @desc  Support of interRAT-RSTDmeasurement #-- @spec 37.571-3 Table A.4.3-3A/18

pc_OTDOA_maxSupportedPrsBandwidth,           BOOLEAN,       false   #-- @desc  Support of maxSupportedPrsBandwidth #-- @spec 37.571-3 Table A.4.3-3A/9

pc_OTDOA_maxSupportedPrsBandwidth_r14,       ENUM-OTDOA_ProvideCapabilities.maxSupportedPrsBandwidth_r14,n6      #-- @desc  maxSupportedPrsBandwidth #-- @spec 37.571-3 Table A.4.3-3A/9

pc_OTDOA_maxSupportedPrsConfigs,             BOOLEAN,       false   #-- @desc  Support of maxSupportedPrsConfigs #-- @spec 37.571-3 Table A.4.3-3A/12

pc_OTDOA_maxSupportedPrsConfigs_r14,         ENUM-OTDOA_ProvideCapabilities.maxSupportedPrsConfigs_r14,c2      #-- @desc  maxSupportedPrsConfigs #-- @spec 37.571-3 Table A.4.3-3A/12

pc_OTDOA_motionMeasurements,                 BOOLEAN,       false   #-- @desc  Support of motionMeasurements #-- @spec 37.571-3 Table A.4.3-3A/17

pc_OTDOA_multiPrbNprs,                       BOOLEAN,       false   #-- @desc  Support of multiPrbNprs #-- @spec 37.571-3 Table A.4.3-3A/14

pc_OTDOA_numberOfRXantennas,                 BOOLEAN,       false   #-- @desc  Support of numberOfRXantennas #-- @spec 37.571-3 Table A.4.3-3A/16

pc_OTDOA_numberOfRXantennas_r14,             ENUM-OTDOA_ProvideCapabilities.numberOfRXantennas_r14,rx1     #-- @desc  Support of numberOfRXantennas #-- @spec 37.571-3 Table A.4.3-3A/16

pc_OTDOA_onNR,                               BOOLEAN,       false   #-- @desc  Support of UE assisted OTDOA (based on LTE signals) on NR #-- @spec 37.571-3 Table A.4.3-2/42

pc_OTDOA_periodicalReporting,                BOOLEAN,       false   #-- @desc  Support of periodicalReporting #-- @spec 37.571-3 Table A.4.3-3A/13

pc_OTDOA_prsFrequencyHopping,                BOOLEAN,       false   #-- @desc  Support of prsFrequencyHopping #-- @spec 37.571-3 Table A.4.3-3A/11

pc_OTDOA_prsOccGroup,                        BOOLEAN,       false   #-- @desc  Support of prsOccGroup #-- @spec 37.571-3 Table A.4.3-3A/10

pc_OTDOA_prs_based_tbs,                      BOOLEAN,       false   #-- @desc  Support of prs-based-tbs #-- @spec 37.571-3 Table A.4.3-3A/6

pc_OTDOA_prs_id,                             BOOLEAN,       false   #-- @desc  Support of prs-id #-- @spec 37.571-3 Table A.4.3-3A/3

pc_OTDOA_tp_separation_via_muting,           BOOLEAN,       false   #-- @desc  Support of tp-separation-via-muting #-- @spec 37.571-3 Table A.4.3-3A/4

pc_P2X_UE,                                   BOOLEAN,       false   #-- @desc  Support of V2X communicatin as Pedestrian UE #-- @spec 36.523-2 A.4.4-1/XXX

pc_PDCP_PktDelay,                            BOOLEAN,       false   #-- @desc  Support for PDCP Packet Delay per QCI #-- @spec 36.523-2 A.4.4-1/140

pc_PLMN_EF_LRPLMNSI_Automatic_Mode_Exception,BOOLEAN,       false   #-- @desc  Support of Automatic Mode EF_LRPLMSI PLMN Selection Expression #-- @spec 36.523-2 A.4.4-1/97

pc_PLMN_Manual_Mode_Exception,               BOOLEAN,       false   #-- @desc  Support of Manual Mode PLMN Selection Expression #-- @spec 36.523-2 A.4.4-1/98

pc_PPI_Support,                              BOOLEAN,       false   #-- @desc  Support of Power Preference Indication #-- @spec 36.523-2 A.4.4.1/86

pc_PRS_ProcessingSymbolsInEveryTms,          ENUM-PRS_ProcessingCapabilityPerBand_r16.durationOfPRS_Processing_r16.durationOfPRS_ProcessingSymbolsInEveryTms_r16,n8      #-- @desc  PRS-ProcessingSymbolsInEveryTms for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/17

pc_PS,                                       BOOLEAN,       true    #-- @desc  Packet Switched #-- @spec 34.123-2 A.3/2

pc_PS_data_centric,                          BOOLEAN,       false   #-- @desc  Support of configuring the UE to PS data centric #-- @spec 36.523-2 A.4.4-2/8

pc_PS_data_off,                              BOOLEAN,       false   #-- @desc  UE supports PS data off #-- @spec 34.229-2 Table A.12/62

pc_PS_voice_centric,                         BOOLEAN,       false   #-- @desc  Support of configuring the UE to PS voice centric #-- @spec 36.523-2 A.4.4-2/7

pc_PUSCH_Ehn_MMTEL,                          BOOLEAN,       false   #-- @desc  Support of PUSCH enhancement for MMTEL voice and video enhancements mode #-- @spec 36.523-2 A.4.4-1/161

pc_PWS_UpperLayer,                           BOOLEAN,       false   #-- @desc  Presence of PWS upper layer for functions like duplicate definition #-- @spec 36.523-2 A.4.4-1/67

pc_P_CSCFDiscovery_viaDHCP,                  BOOLEAN,       true    #-- @desc  UE supports P-CSCF Discovery via DHCP #-- @spec 34.229-2 Table A.12/9

pc_P_CSCFDiscovery_viaDHCPv4,                BOOLEAN,       false   #-- @desc  UE supports P-CSCF discovery via DHCPv4 #-- @spec 34.229-2 Table A.13/2

pc_P_CSCFDiscovery_viaDHCPv6,                BOOLEAN,       false   #-- @desc  UE supports P-CSCF discovery via DHCPv6 #-- @spec 34.229-2 Table A.12/10

pc_P_CSCFDiscovery_viaPCO,                   BOOLEAN,       true    #-- @desc  UE supports P-CSCF Discovery via PCO #-- @spec 34.229-2 Table A.12/8

pc_ParamGpsAssisData,                        BOOLEAN,       false   #-- @desc  Support of MO-LR request for assistance data #-- @spec 37.571-3 table A.4.3-3/5

pc_ParamPosEstimate,                         BOOLEAN,       false   #-- @desc  Support of MO-LR request for a position estimate #-- @spec 37.571-3 table A.4.3-3/6

pc_Preconditions,                            BOOLEAN,       false   #-- @desc  Integration of resource management and SIP? (use of preconditions) #-- @spec 34.229-2 Table A.4/16

pc_ProvideDST_inUse,                         BOOLEAN,       false   #-- @desc  UE supports a mechanism to provide daylight saving time #-- @spec 36.523-2 A.4.4-2/xxx

pc_Provide_IMS_APN,                          BOOLEAN,       false   #-- @desc  Configured to provide IMS APN during initial attach #-- @spec 36.523-2 A.4.4-2/13

pc_Provide_IMS_as_second_APN,                BOOLEAN,       false   #-- @desc  Configured to provide IMS APN as the 2nd PDN connection #-- @spec 36.523-2 A.4.4-2/14

pc_Provide_Internet_as_second_APN,           BOOLEAN,       false   #-- @desc  Configured to provide Internet APN as the 2nd PDN connection #-- @spec 36.523-2 A.4.4-2/15

pc_QZSS_ADR,                                 BOOLEAN,       false   #-- @desc  Support of ADR measurement reporting for Qzss #-- @spec 37.571-3 Table A.4.3-6/3

pc_QZSS_ADR_ENH,                             BOOLEAN,       false   #-- @desc  Support of ADR enhancements for Qzss #-- @spec 37.571-3 Table A.4.3-6/15

pc_QZSS_HA,                                  BOOLEAN,       false   #-- @desc  Support of High accuracy GNSS modes for Qzss #-- @spec 37.571-3 Table A.4.3-6/21

pc_QZSS_QZS_L1,                              BOOLEAN,       false   #-- @desc  Support of QZS-L1 signal in QZSS #-- @spec 37.571-3 Table A.4.3-5/4

pc_QZSS_QZS_L1C,                             BOOLEAN,       false   #-- @desc  Support of QZS-L1C signal in QZSS #-- @spec 37.571-3 Table A.4.3-5/5

pc_QZSS_QZS_L2C,                             BOOLEAN,       false   #-- @desc  Support of QZS-L2C signal in QZSS #-- @spec 37.571-3 Table A.4.3-5/6

pc_QZSS_QZS_L5,                              BOOLEAN,       false   #-- @desc  Support of QZS-L5 signal in QZSS #-- @spec 37.571-3 Table A.4.3-5/7

pc_QZSS_VelocityMeas,                        BOOLEAN,       false   #-- @desc  Support of Velocity measurement reporting for Qzss #-- @spec 37.571-3 Table A.4.3-6/8

pc_RFC2507,                                  BOOLEAN,       TRUE    #-- @desc  IP header compression protocol RFC 2507 is supported #-- @spec 34.123-2 Table A.19a/1

pc_RLF_ReportForInterRAT_MRO,                BOOLEAN,       false   #-- @desc  Support of Radio Link Failure Report for InterRAT MRO #-- @spec 36.523-2 A.4.4-1/94

pc_ROHC_profile0x0001,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0001 #-- @spec 36.523-2 A.4.4-1/40

pc_ROHC_profile0x0002,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0002 #-- @spec 36.523-2 A.4.4-1/41

pc_ROHC_profile0x0003,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0003 #-- @spec 36.523-2 A.4.4-1/42

pc_ROHC_profile0x0004,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0004 #-- @spec 36.523-2 A.4.4-1/43

pc_ROHC_profile0x0006,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0006 #-- @spec 36.523-2 A.4.4-1/44

pc_ROHC_profile0x0101,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0101 #-- @spec 36.523-2 A.4.4-1/45

pc_ROHC_profile0x0102,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0102 #-- @spec 36.523-2 A.4.4-1/46

pc_ROHC_profile0x0103,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0103 #-- @spec 36.523-2 A.4.4-1/47

pc_ROHC_profile0x0104,                       BOOLEAN,       false   #-- @desc  Support for ROHC profile0x0104 #-- @spec 36.523-2 A.4.4-1/48

pc_RRC_re_establishment_CP_CIoT,             BOOLEAN,       false   #-- @desc  Support of RRC connection re-establishment #-- @spec 36.523-2 A.4.4-1/165

pc_RSRP_MeasFR1,                             BOOLEAN,       false   #-- @desc  Support of RSRP-MeasFR1 #-- @spec 37.571-3 Table A.4.3-6C/3

pc_RSRP_MeasFR2,                             BOOLEAN,       false   #-- @desc  Support of RSRP-MeasFR2 #-- @spec 37.571-3 Table A.4.3-6C/4

pc_RS_SINR_MeasEUTRA,                        BOOLEAN,       false   #-- @desc  Support of E-UTRA RS-SINR measurements #-- @spec 38.508-2 Table A.4.3.6-1/42

pc_Rach_Report,                              BOOLEAN,       false   #-- @desc  Support of delivery of rachReport upon request from the network #-- @spec 36.523-2 A.4.4-1/85

pc_Re_Attach_AfterDetachColl,                BOOLEAN,       false   #-- @desc  Support of automatic re-activation of the EPS bearers during network initiated detach even though UE has initiated a detach procedure with detach type set to EPS detach or combined EPSIMSI detach #-- @spec 36.523-2 A.4.4-1/55

pc_RequestIPv4HAAddress_DuringAttach,        BOOLEAN,       false   #-- @desc  Support for being configured to request the IPv4 address of the Home Agent during Attach procedure #-- @spec 36.523-2 A.4.4-1/23

pc_RequestIPv6HAAddress_DuringAttach,        BOOLEAN,       false   #-- @desc  Support for being configured to request the IPv6 address of the Home Agent during Attach procedure #-- @spec 36.523-2 A.4.4-1/22

pc_S1_U_DataTransfer,                        BOOLEAN,       false   #-- @desc  Support of S1-U data transfer #-- @spec 36.523-2 A.4.4-1/Xyz

pc_SBAS_ADR,                                 BOOLEAN,       false   #-- @desc  Support of ADR measurement reporting for Sbas #-- @spec 37.571-3 Table A.4.3-6/2

pc_SBAS_ADR_ENH,                             BOOLEAN,       false   #-- @desc  Support of ADR enhancements for Sbas #-- @spec 37.571-3 Table A.4.3-6/14

pc_SBAS_HA,                                  BOOLEAN,       false   #-- @desc  Support of High accuracy GNSS modes for Sbas #-- @spec 37.571-3 Table A.4.3-6/20

pc_SBAS_VelocityMeas,                        BOOLEAN,       false   #-- @desc  Support of Velocity measurement reporting for Sbas #-- @spec 37.571-3 Table A.4.3-6/7

pc_SCPTM,                                    BOOLEAN,       false   #-- @desc  The UE supports SC-PTM #-- @spec 36.523-2 A.4.2.1.1-1/11

pc_SCPTM_IDLE,                               BOOLEAN,       false   #-- @desc  The UE supports SC-PTM in idle mode #-- @spec 36.523-2 A.4.2.1.1-1/15

pc_SIP_Based_UserConfiguration,              BOOLEAN,       false   #-- @desc  SIP based user configuration #-- @spec 34.229-2 Table A.16/18

pc_SIP_Digest,                               BOOLEAN,       false   #-- @desc  SIP Digest without TLS #-- @spec 34.229-2 Table A.6a/5

pc_SIP_DigestWithoutTLS,                     BOOLEAN,       false   #-- @desc  SIP Digest without TLS #-- @spec 34.229-2 Table A.6a/5

pc_SI_Neighbour_UMTS_Autonomous_Gaps,        BOOLEAN,       false   #-- @desc  Upon configuration of si-RequestForHO by the network supports acquistion of relevant information from a neighbouring UMTS cell by reading the SI of the neighbouring cell using autonomous gaps and reporting #-- @spec 36.523-2, A.4.4-1/100

pc_SI_Neighbour_interFreq_Autonomous_Gaps,   BOOLEAN,       false   #-- @desc  Supports upon configuration of si-requestForHO by the network acquisition of relevant information from a neighbouring intrer-frequency cell by reading the SI of the neighouring cell using autonomous gaps and reporting #-- @spec 36.523-2, A.4.4-1/104

pc_SI_Neighbour_intraFreq_Autonomous_Gaps,   BOOLEAN,       false   #-- @desc  Supports upon configuration of si-requestForHO by the network acquisition of relevant information from a neighbouring intra-frequency cell by reading the SI of the neighouring cell using autonomous gaps and reporting #-- @spec 36.523-2, A.4.4-1/103

pc_SMS_CS_MO,                                BOOLEAN,       FALSE   #-- @desc  Short Message Service (SMS) MO over CS #-- @spec 34.123-2 Table A.2/4

pc_SMS_IP_MO,                                BOOLEAN,       false   #-- @desc  UE supports SM-over-IP sender #-- @spec 34.229-2 Table A.3A/61

pc_SMS_IP_MT,                                BOOLEAN,       false   #-- @desc  UE supports SM-over-IP receiver #-- @spec 34.229-2 Table A.3A/62

pc_SMS_IP_MT_emergency,                      BOOLEAN,       false   #-- @desc  UE supports SM-over-IP receiver on emergency PDN #-- @spec 34.229-2 Table A.3A/63

pc_SMS_MO,                                   BOOLEAN,       true    #-- @desc  UE supports SM-over-IP sender #-- @spec 34.229-2 Table A.3A/61

pc_SMS_MT,                                   BOOLEAN,       true    #-- @desc  UE supports SM-over-IP receiver #-- @spec 34.229-2 Table A.3A/62

pc_SMS_SGs,                                  BOOLEAN,       false   #-- @desc  The UE supports SMS over SGs and is configured for SMS over SGs.  If true at least one of pc_SMS_SGs_MT and pc_SMS_SGs_MO is true. If it is set to true pc_combined_attach shall be set to true #-- @spec 36.523-2, A.4.2.1.1-1/2

pc_SMS_SGs_MO,                               BOOLEAN,       false   #-- @desc  Support of Short Message Service (SMS) MO over SGs #-- @spec 36.523-2 A.4.4-1/4

pc_SMS_SGs_MT,                               BOOLEAN,       false   #-- @desc  Support of Short Message Service (SMS) MT over SGs #-- @spec 36.523-2 A.4.4-1/3

pc_SMS_SGs_Multi_MO,                         BOOLEAN,       false   #-- @desc  Support of sending concatenated multiple short message over SGs #-- @spec 36.523-2 A.4.4.1-72

pc_SRS_switching,                            BOOLEAN,       false   #-- @desc  Support of SRS switching between a band pair #-- @spec 36.523-2 A.4.4-1/166

pc_SRVCC_GERAN_UTRAN,                        BOOLEAN,       false   #-- @desc  Support for SRVCC from E-UTRAN to GERANUTRAN #-- @spec 36.523-2 A.4.4-1/32

pc_SR_WithHARQ_ACK,                          BOOLEAN,       false   #-- @desc  Support of physical layer SR with HARQ ACK #-- @spec 36.523-2 A.4.4-1/211

pc_SR_WithoutHARQ_ACK,                       BOOLEAN,       false   #-- @desc  Support of physical layer SR without HARQ ACK #-- @spec 36.523-2 A.4.4-1/212

pc_Semi_Persistence_Scheduling,              BOOLEAN,       false   #-- @desc  Support of semi persistance scheduling #-- @spec 36.523-2 A.4.4-1/50

pc_SendRTCPOnlyOnHold,                       BOOLEAN,       true    #-- @desc  UE supports sending RTCP only while call is put on hold #-- @spec 34.229-2 Table A.12/23

pc_Sens,                                     BOOLEAN,       false   #-- @desc  Support for UE-Assisted Sensor #-- @spec 37.571-3 Table A.4.3-2/23

pc_Set_UE_Cap_Info_LTE,                      BOOLEAN,       false   #-- @desc  Support of test function SET UL MESSAGE for using a preconfigured UE capability container over LTE #-- @spec 36.523-2 A.4.4-1/221

pc_ShortNameNetwork,                         BOOLEAN,       false   #-- @desc  Support of storage of the network short name #-- @spec 36.523-2 A.4.4-1/13

pc_Speech,                                   BOOLEAN,       false   #-- @desc  UE supports Speech #-- @spec 34.123-2 A.2/1

pc_Squal_based_CellReselection_between_E_UTRAN_and_GERAN,BOOLEAN,       false   #-- @desc  Support of Squal based cell reselection to E-UTRAN from GERAN #-- @spec 36.523-2 A.4.4-1/79

pc_Squal_based_CellReselection_to_E_UTRAN_from_UTRAN,BOOLEAN,       false   #-- @desc  Support of Squal based cell reselection to E-UTRAN from UTRAN #-- @spec 36.523-2 A.4.4-1/57

pc_Squal_based_CellReselection_to_UTRAN_from_E_UTRAN,BOOLEAN,       false   #-- @desc  Support of Squal based cell reselection to UTRAN from E-UTRAN #-- @spec 36.523-2 A.4.4-1/56

pc_StandaloneGNSS_Location,                  BOOLEAN,       false   #-- @desc  Support of standalone GNSS receiver to provide detailed location information in RRC measurement report and logged measurements in RRC_IDLE #-- @spec 36.523-2 A.4.4-1/63

pc_Streaming,                                BOOLEAN,       false   #-- @desc  UE Supports Streaming QoS class #-- @spec 34.123-2 A.6/2

pc_SubscribeConferenceEvent_OutsideINVITEDialog,BOOLEAN,       false   #-- @desc  UE supports subscription to conference event package outside INVITE dialog #-- @spec 34.229-2 Table A.12/xx

pc_Subscribed,                               BOOLEAN,       false   #-- Anritsu Prose CR R5-121434 #-- @spec 

pc_SupportForSF_512,                         BOOLEAN,       FALSE   #-- @desc  Downlink support. Part of DL_PhysChCapabilityFDD. #-- @spec 34.123-2 Table A.18a/3

pc_SupportOfMultiCarrier,                    BOOLEAN,       FALSE   #-- @desc  Multi carrier supported #-- @spec 34.123-2 Table A.1/6

pc_SupportOpModeA,                           BOOLEAN,       false   #-- @desc  UE supports Operation Mode A #-- @spec 34.123-2 A.3/3

pc_SwitchOnOff,                              BOOLEAN,       true    #-- @desc  switch onoff supported #-- @spec 36.523-2, A4.4-1/10

pc_T3412Extended,                            BOOLEAN,       false   #-- @desc  Support of T3412 extended value IE #-- @spec 36.523-2 A.4.4.1/81

pc_TAU_connected,                            BOOLEAN,       false   #-- @desc  Support of TAU in connected mode. Applicable when configured to pc_voice_PS_1_CS_2 and pc_Attach #-- @spec 

pc_TAU_connected_in_IMS,                     BOOLEAN,       false   #-- @desc  Support of TAU in connected mode. Applicable when configured to pc_voice_PS_1_CS_2 and pc_Attach #-- @spec 36.523-2 A.4.4.1-73

pc_TAU_idle,                                 BOOLEAN,       false   #-- @desc  Support of TAU in idle mode. Applicable when configured to pc_voice_PS_1_CS_2 and pc_Attach #-- @spec 

pc_TAU_idle_in_IMS,                          BOOLEAN,       false   #-- @desc  Support of TAU in idle mode. Applicable when configured to pc_voice_PS_1_CS_2 and pc_Attach #-- @spec 36.523-2 A.4.4.1-74

pc_TDD_HCR,                                  BOOLEAN,       false   #-- @desc  UE supports UTRA band as defined in TS 25.102 #-- @spec 34.123-2 A.1/2

pc_TDD_LCR,                                  BOOLEAN,       false   #-- @desc  UE supports UTRA band as defined in TS 25.102 #-- @spec 34.123-2 A.1/3

pc_TDD_SpecialSubframe,                      BOOLEAN,       false   #-- @desc  Support of TDD special subframe #-- @spec 36.523-2 A.4.4.1A/2

pc_TDD_VHCR,                                 BOOLEAN,       false   #-- @desc  UE supports UTRA band as defined in TS 25.102 #-- @spec 34.123-2 A.1/8

pc_TDD_band_UE_PC2,                          BOOLEAN,       false   #-- @desc  Support of TDD Bands 38 40 41 and 42 Power class 2 operation #-- @spec 36.523-2 A.4.4-1/139

pc_TMPI_forGBA,                              BOOLEAN,       false   #-- @desc  UE uses TMPI in HTTP request for GBA #-- @spec 34.229-2 Table A.12/44

pc_TTI_Bundling,                             BOOLEAN,       false   #-- @desc  Support of TTI Bundling #-- @spec 36.523-2 A.4.4-1/51

pc_TestModeforCSGproximity,                  BOOLEAN,       false   #-- @desc  Support of UE radio bearer test mode for CSG proximity testing #-- @spec 36.523-2 A.4.4-1/92

pc_ThreeCell,                                BOOLEAN,       FALSE   #-- @desc  Support of Three cell #-- @spec 34.123-2 Table A.18a/50

pc_ThreeCellMIMO,                            BOOLEAN,       FALSE   #-- @desc  Support of Three cell MIMO #-- @spec 34.123-2 Table A.18a/48

pc_UAS,                                      BOOLEAN,       false   #-- @desc  A UE supporting UAS services #-- @spec 38.508-2 Table A.4.3.7-1/51

pc_UDC,                                      BOOLEAN,       false   #-- @desc  Support of the uplink data compression operation #-- @spec 36.523-2 A.4.4-1/179

pc_UDC_SIP,                                  BOOLEAN,       false   #-- @desc  Support of UL data compression with SIP static dictionary #-- @spec 36.523-2 A.4.4-1/180

pc_UEA2_UIA2,                                BOOLEAN,       TRUE    #-- @desc  Set UEA2UIA2 to FALSE if not fully IOT tested #-- @spec 34.123-2 Table A.18a/35

pc_UEA_AGNSS,                                BOOLEAN,       false   #-- @desc  Support of UE assisted Assisted-GNSS #-- @spec 37.571-3 Table A.4.3-2/2

pc_UEA_A_GANSS,                              BOOLEAN,       false   #-- @desc  Support of UE-Assisted A-GANSS #-- @spec 37.571-3 Table A.4.3-1/6

pc_UEA_DL_AoD,                               BOOLEAN,       false   #-- @desc  Support for UE-Assisted DL-AoD #-- @spec 37.571-3 Table A.4.3-2/30

pc_UEA_DL_TDOA,                              BOOLEAN,       false   #-- @desc  Support for UE-Assisted DL-TDOA #-- @spec 37.571-3 Table A.4.3-2/32

pc_UEA_MBS,                                  BOOLEAN,       false   #-- @desc  Support for UE-Assisted MBS #-- @spec 37.571-3 Table A.4.3-2/20

pc_UEA_UL_TDOA,                              BOOLEAN,       false   #-- @desc  Support for UE-Assisted UL-TDOA #-- @spec 37.571-3 Table A.4.3-2/44

pc_UEB_AGNSS,                                BOOLEAN,       false   #-- @desc  Support of UE based Assisted-GNSS #-- @spec 37.571-3 Table A.4.3-2/1

pc_UEB_A_GANSS,                              BOOLEAN,       false   #-- @desc  Support of UE-Based A-GANSS #-- @spec 37.571-3 Table A.4.3-1/5

pc_UEB_DL_AoD,                               BOOLEAN,       false   #-- @desc  Support for UE-Based DL-AoD #-- @spec 37.571-3 Table A.4.3-2/31

pc_UEB_DL_TDOA,                              BOOLEAN,       false   #-- @desc  Support for UE-Based DL-TDOA #-- @spec 37.571-3 Table A.4.3-2/33

pc_UEB_MBS,                                  BOOLEAN,       false   #-- @desc  Support for UE-Based MBS #-- @spec 37.571-3 Table A.4.3-2/26

pc_UEB_Sens,                                 BOOLEAN,       false   #-- @desc  Support for UE-Based Sensor #-- @spec 37.571-3 Table A.4.3-2/28

pc_UEB_WLAN,                                 BOOLEAN,       false   #-- @desc  Support for UE-Based WLAN #-- @spec 37.571-3 Table A.4.3-2/27

pc_UE_NoRegIMS_IMSVoPS_0,                    BOOLEAN,       false   #-- @desc  The UE does not request IMS PDN connection when IMS VoPS set to '0' #-- @spec 36.523-2 A.4.4-2/xx

pc_UE_NoReqIMS_IMSVoPS_0,                    BOOLEAN,       false   #-- @desc  The UE does not request IMS PDN connection when IMS VoPS set to '0' #-- @spec 36.523-2 A.4.4-2/xx

pc_UE_PositioningBasedOTDOA_Sup,             BOOLEAN,       FALSE   #-- @desc  UE positioning capability: the Based OTDOA is supporting by UE #-- @spec 34.123-2 Table A.8a/3

pc_UE_PositioningGPS_TimingOfCellFramesSup,  BOOLEAN,       FALSE   #-- @desc  UE positioning capability: the UE supports the GPS timing of cell frames #-- @spec 34.123-2 Table A.8a/2

pc_UE_PositioningIPDL_Sup,                   BOOLEAN,       FALSE   #-- @desc  UE positioning capability: support for IPDL #-- @spec 34.123-2 Table A.8a/1

pc_UE_PositioningStandaloneLocMethodsSup,    BOOLEAN,       FALSE   #-- @desc  UE positioning capability: the standalone location method is supporting by UE - Refer to 3GPP TS 37.571-3 [57] Table A.4.3-14 #-- @spec 34.123-2 Table A.8a/4

pc_UE_supports_user_initiated_PDN_disconnect,BOOLEAN,       false   #-- @desc  UE supports user initiated PDN disconnect #-- @spec 36.523-2 A.4.4-2/16

pc_UL_256QAM,                                BOOLEAN,       false   #-- @desc  Support of uplink 256 QAM #-- @spec 36.523-2 A.4.4-1/183

pc_UL_64QAM,                                 BOOLEAN,       false   #-- @desc  Support of uplink 64 QAM #-- @spec 36.523-2 A.4.4.1/xxx

pc_UL_CA,                                    BOOLEAN,       false   #-- @desc  Support of UL CA #-- @spec 36.523-2, ???

pc_UL_CA_2Carriers,                          BOOLEAN,       false   #-- @desc  UL CA with 2 carriers #-- @spec 36.523-2 A.4.3.3-2/1

pc_UL_CA_3Carriers,                          BOOLEAN,       false   #-- @desc  UL CA with 3 carriers #-- @spec 36.523-2 A.4.3.3-2/2

pc_UL_CoMP,                                  BOOLEAN,       false   #-- @desc  Support of UL co-ordinated multi-point operation #-- @spec 36.523-2 A.4.4-1A/1

pc_UL_CoordinatedMultiPointOperation,        BOOLEAN,       false   #-- @desc  Support of UL co-ordinated multi-point operation #-- @spec 36.523-2 A.4.4-1A/xx

pc_UL_InterBand_CaAA,                        BOOLEAN,       false   #-- @desc  Support of UL inter-band CA _ A-A #-- @spec 36.523-2 A.4.3.3.3-2A/1

pc_UL_InterBand_CaBwClassComb_AA,            BOOLEAN,       false   #-- @desc  UL Inter-band contiguous CA BW class A-A #-- @spec 36.523-2 A.4.3.3.3-2/1

pc_UL_IntraBand_ContCaBWclassB,              BOOLEAN,       false   #-- @desc  UL Intra-band contiguous CA BW class B #-- @spec 36.523-2 A.4.3.3.1-2/1

pc_UL_IntraBand_ContCaBWclassC,              BOOLEAN,       false   #-- @desc  UL Intra-band contiguous CA BW class C #-- @spec 36.523-2 A.4.3.3.1-2/2

pc_UL_IntraBand_contCaTypeB,                 BOOLEAN,       false   #-- @desc  UL Intra-band contiguous CA Type B #-- @spec 36.523-2 A.4.3.3.1-2A/1

pc_UL_IntraBand_contCaTypeC,                 BOOLEAN,       false   #-- @desc  UL Intra-band contiguous CA Type C #-- @spec 36.523-2 A.4.3.3.1-2A/2

pc_UL_IntraBand_nonContCaAA,                 BOOLEAN,       false   #-- @desc  Support of UL intra-band non-contiguous CA _ A-A #-- @spec 36.523-2 A.4.3.3.2-2A/1

pc_UL_IntraBand_nonContCaBwClassComb_AA,     BOOLEAN,       false   #-- @desc  Support of UL intra-band non-contiguous CA BW Class Combination A-A #-- @spec 36.523-2 A.4.3.3.2-2/1

pc_UL_MIMO,                                  BOOLEAN,       false   #-- @desc  Support of UL MIMO #-- @spec 36.523-2 A.4.4-170

pc_UL_SupportedInAllBandsInCAComb,           BOOLEAN,       false   #-- @desc  UL (Pcell) supported in each band of Inter-band CA combination under test #-- @spec 36.523-2 A.4.3.3.3-2/2

pc_UL_TC_FDD,                                BOOLEAN,       TRUE    #-- @desc  Support for turbo encoding for uplink - FDD #-- @spec 34.123-2 Table A.18a/2

pc_UL_TC_TDD,                                BOOLEAN,       FALSE   #-- @desc  Support for turbo encoding for uplink - TDD #-- @spec 34.123-2 Table A.18b/2

pc_UMI_ProcNeeded_DuringCSFB,                BOOLEAN,       false   #-- @desc  Requiring UMI proceeding to paging response #-- @spec 36.523-2 A.4.4-2/6

pc_UMI_ProcNeeded_DuringSRVCC,               BOOLEAN,       false   #-- @desc  Requiring UMI proceeding to paging response #-- @spec 

pc_UMTS_GSM,                                 BOOLEAN,       false   #-- @desc  UE supports GSM as defined in 21.904 #-- @spec 34.123-2 A.1/4

pc_USIM_Removal,                             BOOLEAN,       false   #-- @desc  USIM removable without power down supported #-- @spec 36.523-2, A4.4-1/1

pc_USSI,                                     BOOLEAN,       false   #-- @desc  USSI #-- @spec 34.229-2 Table A.16/19

pc_UTRA,                                     BOOLEAN,       false   #-- @desc  UE supports UTRA #-- @spec 36.523-2 A.4.1-1/6

pc_UTRAN_ANR,                                BOOLEAN,       false   #-- @desc  Support of UTRAN ANR #-- @spec 36.523-2 A.4.4-1/65

pc_UTRAN_ProximityIndication,                BOOLEAN,       false   #-- @desc  Support of UTRAN Proximity Indication #-- @spec 36.523-2 A.4.4.1/77

pc_UTRAN_TO_GAN_CS_Handover,                 BOOLEAN,       false   #-- @desc  Support of UTRAN to GAN CS Handover #-- @spec 51.010-2 Table A.2/80

pc_UTRAN_WLAN_offload,                       BOOLEAN,       false   #-- @desc  Supports WLAN supports Offload tofrom WLAN and supports S2b #-- @spec 34.123-2 Table A.10/40

pc_UTRA_CSG_CellsReport,                     BOOLEAN,       false   #-- @desc  UTRA CSG cells report - Used in Classmark 3 #-- @spec 51.010-2 Table A.2/133

pc_UTRA_CompressedModeRequired,              BOOLEAN,       false   #-- @desc  Support of Compressed Mode #-- @spec 36.523-2 A.4.4-1/28

pc_UTRA_FeatrGrp_1,                          BOOLEAN,       false   #-- @desc  Support of UTRA CELL_PCH and URA_PCH to RRC_IDLE cell reselection #-- @spec 36.523-2 A.4.5-2/1

pc_UTRA_FeatrGrp_2,                          BOOLEAN,       false   #-- @desc  Support of EUTRAN measurements and reporting in connected mode #-- @spec 36.523-2 A.4.5-2/2

pc_UTRA_FeatrGrp_3,                          BOOLEAN,       false   #-- @desc  Support of UTRA CELL_FACH absolute priority cell reselection for high priority layers #-- @spec 36.523-2 A.4.5-2/3

pc_UTRA_FeatrGrp_4,                          BOOLEAN,       false   #-- @desc  Support of UTRA CELL_FACH absolute priority cell reselection for all layers #-- @spec 36.523-2 A.4.5-2/4

pc_UeAssistedAgps,                           BOOLEAN,       false   #-- @desc  Support of UE assisted Network Assisted GPS L1 CA #-- @spec 37.571-3 A.4.3-1/11

pc_UeBasedAgps,                              BOOLEAN,       false   #-- @desc  Support of UE based Network Assisted GPS L1 CA #-- @spec 37.571-3 A.4.3-1/10

pc_UniversalAndLocalTimeZone,                BOOLEAN,       false   #-- @desc  Support of storage of the universal time and local time zone #-- @spec 36.523-2 A.4.4-1/15

pc_UpdateUE_LocationInformation,             BOOLEAN,       false   #-- @desc  Update UE Location Information #-- @spec 36.523-2 A.4.3-2/3

pc_UpperLayer_PDU_Start_Ind,                 BITSTRING,     0       #-- @desc  Support of Indication of Upper Layer PDU Start Capability for RLC UM #-- @spec 51.010-2 Table A.2/118

pc_Use_QCI_66,                               BOOLEAN,       false   #-- @desc  The UE supports a bearer with QCI 66 #-- @spec 36.523-2 A.4.4-2/33

pc_Use_SMS_over_IP,                          BOOLEAN,       false   #-- @desc  The UE is configured to use SMS over IP #-- @spec 36.523-2 A.4.4-2/32

pc_UserInitiatedPLMN_Reselection,            BOOLEAN,       false   #-- @desc  Support user initiated PLMN reselection in automatic mode #-- @spec 36.523-2 A.4.4-1/69

pc_UserInitiated_SNPN_Reselection,           BOOLEAN,       false   #-- @desc  Support of autonomous search function to detect CAG cells on serving and non-serving frequencies #-- @spec 38.508-2 Table A.4.3.7-1/30

pc_UserRequestedPS_Detach,                   BOOLEAN,       false   #-- @desc User requested PS detach without powering off #-- @spec 34.123-2 A.4.4 A.20/63

pc_User_Plane_CIoT_Optimisation,             BOOLEAN,       false   #-- @desc  Support of User Plane CIoT #-- @spec 36.523-2 A.4.4.1-1/X1

pc_V2XCNPC5,                                 BOOLEAN,       false   #-- @desc  Support of V2X communication over NR-PC5 #-- @spec 38.508-2 Table A.4.3.7-1/34

pc_VAMOS_Type1,                              BOOLEAN,       false   #-- @desc  VAMOS type 1 - Used in Classmark 3 #-- @spec 51.010-2 Table A.2/121

pc_VAMOS_Type2,                              BOOLEAN,       false   #-- @desc  VAMOS type 2 - Used in Classmark 3 #-- @spec 51.010-2 Table A.2/122

pc_VAMOS_Type3,                              BOOLEAN,       false   #-- @desc  VAMOS type 2 - Used in Classmark 3 #-- @spec 51.010-2 Table A.2/123

pc_VideoCodecH264CBP,                        BOOLEAN,       false   #-- @desc  MTSI media - Video codec H.264 CBP Level 1.2 #-- @spec 34.229-2 Table A.15/9

pc_VideoCodecH264CBPLv31,                    BOOLEAN,       false   #-- @desc  Video codec H.264 (AVC) CBP Level 3.1 #-- @spec 34.229-2 Table A.15/13

pc_VideoCodecH264CHPLv31,                    BOOLEAN,       false   #-- @desc  Video codec H.264 (AVC) CHP Level 3.1 #-- @spec 34.229-2 Table A.15/12

pc_VideoCodecH265Lv31,                       BOOLEAN,       false   #-- @desc  Reference: 34.229-2 Table A.1511 #-- @spec 34.229-2 Table A.15/11

pc_VoLTE,                                    BOOLEAN,       false   #-- @desc  Support of VoLTE in GSMA PRD IR.92: "IMS profile for Voice and SMS" #-- @spec 36.523-2 A.4.4-1/33

pc_WLAN,                                     BOOLEAN,       false   #-- @desc  UE supports WLAN #-- @spec 34.229-2 Table A.18/4

pc_WLAN_APId,                                BOOLEAN,       false   #-- @desc  Support of wlan-AP-Identifier #-- @spec 37.571-3 Table A.4.3-7B/1

pc_WLAN_APLocinfo,                           BOOLEAN,       false   #-- @desc  Support of wlan-AP-Location #-- @spec 37.571-3 Table A.4.3-7B/2

pc_WLAN_IMS_EmergencyCall,                   BOOLEAN,       false   #-- @desc  UE supports IMS emergency call over WLAN #-- @spec 34.229-2 Table A.12/65

pc_WLAN_Meas_Imm_MDT,                        BOOLEAN,       false   #-- @desc  Support of WLAN Measurement Collection in Immediate MDT #-- @spec 36.523-2, A.4.4-1/187

pc_WLAN_Meas_logged_MDT,                     BOOLEAN,       false   #-- @desc  Support of WLAN Measurement Collection in logged MDT #-- @spec 36.523-2, A.4.4-1/185

pc_WLAN_XCAP_without_PDN,                    BOOLEAN,       false   #-- @desc  If PICS is true Wi-Fi access without PDN connection applies.  Otherwise EPC-integrated WLAN applies #-- @spec 34.229-2 a.12/49

pc_WLAN_voice,                               BOOLEAN,       false   #-- @desc  Support for IR.51 #-- @spec 36.523-2, A.4.4-1/nnn

pc_XCAP_UsernameIsConfiguredInUE,            BOOLEAN,       false   #-- @desc  UE indicated OMA-TS-XDM_MO-V1_1-20080627-A.doc section 5.2.8 "Node: <X>AAUTHNAME" is configured #-- @spec 34.229-2 Table A.12/37

pc_XCAP_XUIisDefaultPublicUserId,            BOOLEAN,       false   #-- @desc  UE uses the default public user id received in P-Associated-URI header in 200 OK for REGISTER as XCAP User Identity (XUI) #-- @spec 34.229-2 Table A.12/38

pc_XCAP_only_APN,                            BOOLEAN,       false   #-- @desc  Configured with an APN for XCAP only usage #-- @spec 36.523-2 A.4.4-2/12

pc_XCAP_over_Internet_APN,                   BOOLEAN,       false   #-- @desc  Configured to use Internet APN for XCAP signalling #-- @spec 36.523-2 A.4.4-2/17

pc_Xtd_Ctrl_Message_Segmentation,            BITSTRING,     0       #-- @desc  Support of Extended RLCMAC control message segmentation #-- @spec 51.010-2 Table A.2/108

pc_ZUC,                                      BOOLEAN,       false   #-- @desc  Support of ZUC algorithm #-- @spec 36.523-2 A.4.4.1/99

pc_aggregated_prs_MeasureAndReport,          BOOLEAN,       false   #-- @desc  Support of PRS bandwidth aggregation measurement and report nr-MeasBasedOnAggregatedResources-r18 after reception of nr-DL-PRS-JointMeasurementRequest-r18 #-- @spec 37.571-3 Table A.4.3-2/54

pc_ce_HARQ_AckBundling,                      BOOLEAN,       false   #-- @desc  Support of HARQ-ACK bundling #-- @spec 36.523-2 A.4.4-1/y

pc_ce_PUSCH_NB_MaxTBS,                       BOOLEAN,       false   #-- @desc  Support of ce-PUSCH-NB-MaxTBS-r14 #-- @spec 36.523-2 A.4.4-1/x

pc_cellReselectionMeasurements_locationBased_earthMovingCell,BOOLEAN,       false   #-- @desc Support of cell reselection measurements triggering based on location for earth moving cell #-- @spec 36.523-2 A.4.4-1/252

pc_cellReselectionMeasurements_locationBased_fixedCell,BOOLEAN,       false   #-- @desc Support of cell reselection measurements triggering based on location for (quasi-)fixed cell #-- @spec 36.523-2 A.4.4-1/251

pc_commSimultaneousTx,                       BOOLEAN,       false   #-- @desc  Support of simultaneous transmission of EUTRA and sidelink communication (on different carriers) in all bands for which the UE indicated simultaneous sidelink and EUTRA support in a band combination (using commSupportedBandsPerBC) #-- @spec 36.523-2 A.4.4.1/119

pc_commSupportedBands,                       BOOLEAN,       false   #-- @desc  Support of ProSe direct communication #-- @spec 36.523-2 A.4.4.1-1/111

pc_configuredUL_GrantType1,                  BOOLEAN,       false   #-- @desc  Support Type 1 PUSCH transmissions with configured grant #-- @spec 38.508-2 Table A.4.3.2-1/10

pc_configuredUL_GrantType2,                  BOOLEAN,       false   #-- @desc  Support Type 2 PUSCH transmissions with configured grant #-- @spec 38.508-2 Table A.4.3.2-1/11

pc_csi_RS_CFRA_ForHO,                        BOOLEAN,       false   #-- @desc  Support reconfiguration with sync using a contention free random access on PRACH resources that are associated with CSI-RS resources of the target cell #-- @spec 38.508-2 Table A.4.3.2-1/9

pc_dataInactMon,                             BOOLEAN,       false   #-- @desc  Support of data inactivity monitoring #-- @spec 36.523-2 A.4.2.1.1-1/yy

pc_data_centric,                             BOOLEAN,       false   #-- @desc  Support of CSPS mode 2 #-- @spec 

pc_discSLSS,                                 BOOLEAN,       false   #-- @desc  Support of ProSe discovery SLSS transmission and reception #-- @spec 36.523-2 A.4.4.1/113

pc_discScheduledResourceAlloc,               BOOLEAN,       false   #-- @desc  Support of transmission of discovery announcements based on network scheduled resource allocation #-- @spec 36.523-2 A.4.4-1A/5

pc_discSupportedBands,                       BOOLEAN,       false   #-- @desc  Support of ProSe direct discovery #-- @spec 36.523-2 A.4.4.1-1/112

pc_discUESelectedResourceAlloc,              BOOLEAN,       false   #-- @desc  Support of transmission of discovery announcements based on autonomous resource selection #-- @spec 36.523-2 A.4.4-1A/6

pc_disc_public_safety,                       BOOLEAN,       false   #-- @desc  ProSe discovery for Public Safety Supported #-- @spec 36.523-2 A.4.4.1-1/x1x

pc_dl_PRS_BufferType,                        ENUM-PRS_ProcessingCapabilityPerBand_r16.dl_PRS_BufferType_r16,type1   #-- @desc  dl-PRS-BufferType for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/15

pc_dl_RSTD_MeasurementPerPairOfTRP_FR1,      INTEGER,       1       #-- @desc  dl-RSTD-MeasurementPerPairOfTRP-FR1 #-- @spec 37.571-3 Table A.4.3-6F/1

pc_dl_RSTD_MeasurementPerPairOfTRP_FR2,      INTEGER,       1       #-- @desc  dl-RSTD-MeasurementPerPairOfTRP-FR2 #-- @spec 37.571-3 Table A.4.3-6F/2

pc_downlink_LAA,                             BOOLEAN,       false   #-- @desc  Supports downlink LAA operation #-- @spec 36.523-2 A.4.4-1/YY

pc_durationOfPRS_ProcessingSymbols,          ENUM-PRS_ProcessingCapabilityPerBand_r16.durationOfPRS_Processing_r16.durationOfPRS_ProcessingSymbols_r16,nDot125 #-- @desc  durationOfPRS-ProcessingSymbols for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/16

pc_dynamicPowerSharing,                      BOOLEAN,       false   #-- @desc  UE supports 5GS Core #-- @spec 38.508-2 Table A.4.3.2-1/17

pc_dynamicPowerSharingENDC,                  BOOLEAN,       false   #-- @desc  Support dynamic EN-DC power sharing for at least one EN-DC band combination_FR1 only #-- @spec 38.508-2 Table A.4.3.2-1/17

pc_dynamicSwitchRA_Type0_1_PDSCH,            BOOLEAN,       false   #-- @desc  Support dynamic switching between resource allocation Types 0 and 1 for PDSCH #-- @spec 38.508-2 Table A.4.3.2-1/26

pc_dynamicSwitchRA_Type0_1_PUSCH,            BOOLEAN,       false   #-- @desc  Support dynamic switching between resource allocation Types 0 and 1 for PUSCH #-- @spec 38.508-2 Table A.4.3.2-1/27

pc_eAttachWithIMSI,                          BOOLEAN,       false   #-- @desc  Support of Attach With IMSI #-- @spec 36.523-2 A.4.4.1/80

pc_eBand103_Supp,                            BOOLEAN,       false   #-- @desc  Support of Band 103 #-- @spec 36.523-2 A.4.3.1-1/103

pc_eBand10_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 10 #-- @spec 36.523-2 A.4.3.1-1/10

pc_eBand11_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 11 #-- @spec 36.523-2 A.4.3.1-1/11

pc_eBand12_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 12 #-- @spec 36.523-2 A.4.3.1-1/12

pc_eBand13_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 13 #-- @spec 36.523-2 A.4.3.1-1/13

pc_eBand14_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 14 #-- @spec 36.523-2 A.4.3.1-1/14

pc_eBand17_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 17 #-- @spec 36.523-2 A.4.3.1-1/17

pc_eBand18_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 18 #-- @spec 36.523-2 A.4.3.1-1/18

pc_eBand19_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 19 #-- @spec 36.523-2 A.4.3.1-1/19

pc_eBand1_Supp,                              BOOLEAN,       TRUE    #-- @desc  Support of Band 1 #-- @spec 36.523-2 A.4.3.1-1/1

pc_eBand20_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 20 #-- @spec 36.523-2 A.4.3.1-1/20

pc_eBand21_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 21 #-- @spec 36.523-2 A.4.3.1-1/21

pc_eBand22_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 22 #-- @spec 36.523-2 A.4.3.1-1/22

pc_eBand23_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 23 #-- @spec 36.523-2 A.4.3.1-1/23

pc_eBand24_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 24 #-- @spec 36.523-2 A.4.3.1-1/24

pc_eBand253_Supp,                            BOOLEAN,       false   #-- @desc  Support of Band 253 #-- @spec 36.523-2 A.4.3.1-1/253

pc_eBand254_Supp,                            BOOLEAN,       false   #-- @desc Support of Band 254 #-- @spec 36.523-2 A.4.3.1-1/254

pc_eBand255_Supp,                            BOOLEAN,       false   #-- @desc  Support of Band 255 #-- @spec 36.523-2 A.4.3.1-1/255

pc_eBand256_Supp,                            BOOLEAN,       false   #-- @desc  Support of Band 256 #-- @spec 36.523-2 A.4.3.1-1/256

pc_eBand25_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 25 #-- @spec 36.523-2 A.4.3.1-1/25

pc_eBand26_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 26 #-- @spec 36.523-2 A.4.3.1-1/26

pc_eBand27_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 27 #-- @spec 36.523-2 A.4.3.1-1/27

pc_eBand28_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 28 #-- @spec 36.523-2 A.4.3.1-1/28

pc_eBand29_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 29 #-- @spec 36.523-2 A.4.3.1-1/29

pc_eBand2_Supp,                              BOOLEAN,       false   #-- @desc  Support of Band 2 #-- @spec 36.523-2 A.4.3.1-1/2

pc_eBand30_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 30 #-- @spec 36.523-2 A.4.3.1-1/30

pc_eBand31_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 31 #-- @spec 36.523-2 A.4.3.1-1/31

pc_eBand32_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 32 #-- @spec 36.523-2 A.4.3.1-1/32

pc_eBand33_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 33 #-- @spec 36.523-2 A.4.3.1-2/1

pc_eBand34_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 34 #-- @spec 36.523-2 A.4.3.1-2/2

pc_eBand35_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 35 #-- @spec 36.523-2 A.4.3.1-2/3

pc_eBand36_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 36 #-- @spec 36.523-2 A.4.3.1-2/4

pc_eBand37_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 37 #-- @spec 36.523-2 A.4.3.1-2/5

pc_eBand38_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 38 #-- @spec 36.523-2 A.4.3.1-2/6

pc_eBand39_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 39 #-- @spec 36.523-2 A.4.3.1-2/7

pc_eBand3_Supp,                              BOOLEAN,       false   #-- @desc  Support of Band 3 #-- @spec 36.523-2 A.4.3.1-1/3

pc_eBand40_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 40 #-- @spec 36.523-2 A.4.3.1-2/8

pc_eBand41_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 41 #-- @spec 36.523-2 A.4.3.1-2/9

pc_eBand42_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 42 #-- @spec 36.523-2 A.4.3.1-2/10

pc_eBand43_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 43 #-- @spec 36.523-2 A.4.3.1-2/11

pc_eBand44_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 44 #-- @spec 36.523-2 A.4.3.1-2/12

pc_eBand45_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 45 #-- @spec 36.523-2 A.4.3.1-2/13

pc_eBand46_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 46 #-- @spec 36.523-2 A.4.3.1-2/14

pc_eBand47_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 47 #-- @spec 36.523-2 A.4.3.1-2/15

pc_eBand48_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 48 #-- @spec 36.523-2 A.4.3.1-2/16

pc_eBand4_Supp,                              BOOLEAN,       false   #-- @desc  Support of Band 4 #-- @spec 36.523-2 A.4.3.1-1/4

pc_eBand53_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 53 #-- @spec 36.523-2 A.4.3.1-2/17

pc_eBand54_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 54 #-- @spec 36.523-2 A.4.3.1-2/18

pc_eBand5_Supp,                              BOOLEAN,       false   #-- @desc  Support of Band 5 #-- @spec 36.523-2 A.4.3.1-1/5

pc_eBand65_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 65 #-- @spec 36.523-2 A.4.3.1-1/33

pc_eBand66_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 66 #-- @spec 36.523-2 A.4.3.1-1/34

pc_eBand67_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 67 #-- @spec 36.523-2 A.4.3.1-1/35

pc_eBand68_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 68 #-- @spec 36.523-2 A.4.3.1-1/36

pc_eBand69_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 69 #-- @spec 36.523-2 A.4.3.1-1/37

pc_eBand6_Supp,                              BOOLEAN,       false   #-- @desc  Support of Band 6 #-- @spec 36.523-2 A.4.3.1-1/6

pc_eBand70_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 70 #-- @spec 36.523-2 A.4.3.1-1/38

pc_eBand71_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 71 #-- @spec 36.523-2 A.4.3.1-1/39

pc_eBand72_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 72 #-- @spec 36.523-2 A.4.3.1-1/40

pc_eBand73_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 73 #-- @spec 36.523-2 A.4.3.1-1/41

pc_eBand74_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 74 #-- @spec 36.523-2 A.4.3.1-1/42

pc_eBand7_Supp,                              BOOLEAN,       false   #-- @desc  Support of Band 7 #-- @spec 36.523-2 A.4.3.1-1/7

pc_eBand85_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 85 #-- @spec 36.523-2 A.4.3.1-1/xx

pc_eBand87_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 87 #-- @spec 36.523-2 A.4.3.1-1/87

pc_eBand88_Supp,                             BOOLEAN,       false   #-- @desc  Support of Band 88 #-- @spec 36.523-2 A.4.3.1-1/88

pc_eBand8_Supp,                              BOOLEAN,       false   #-- @desc  Support of Band 8 #-- @spec 36.523-2 A.4.3.1-1/8

pc_eBand9_Supp,                              BOOLEAN,       false   #-- @desc  Support of Band 9 #-- @spec 36.523-2 A.4.3.1-1/9

pc_eCall_Test_Call,                          BOOLEAN,       false   #-- @desc  Capability to trigger a Test eCall #-- @spec 34.123-2 A.10/19

pc_eCall_automatic_Initiated,                BOOLEAN,       false   #-- @desc  Capability to initiate Automatic eCall #-- @spec 34.123-2 Table A.10/17

pc_eCall_manual_Initiated,                   BOOLEAN,       false   #-- @desc  Capability to initiate a Manual eCall #-- @spec 34.123-2 Table A.10/16

pc_eFDD,                                     BOOLEAN,       TRUE    #-- @desc  UE supports EUTRA FDD #-- @spec 36.523-2 A.4.1-1/1

pc_eFDD_MultiBand,                           BOOLEAN,       TRUE    #-- @desc  Support of multiple E-UTRA FDD bands #-- @spec 36.523-2 A.4.1-2/1

pc_eHARQ_Pattern_for_TTI_bundling,           BOOLEAN,       false   #-- @desc  Support of enhanced HARQ pattern for TTI bundling operation for FDD #-- @spec 36.523-2 A.4.4.1/107

pc_eIMTA_TDD,                                BOOLEAN,       false   #-- @desc  Support of TDD ULDL reconfiguration for TDD serving cell(s) via monitoring PDCCH with eIMTA-RNTI on a TDD Pcell #-- @spec 36.523-2 A.4.4-1/124

pc_eLAP,                                     BOOLEAN,       false   #-- @desc  Support of Low Access Priority Indication #-- @spec 36.523-2 A.4.4.1-x1

pc_eMBMS,                                    BOOLEAN,       false   #-- @desc  Support of eMBMS #-- @spec 36.523-2 A.4.2.1.1.-1/5

pc_eMBMS_SC,                                 BOOLEAN,       false   #-- @desc  Support of eMBMS service continuity #-- @spec 36.523-2 A.4.2.1.1.-1/7

pc_eMinimumPeriodicSearchTimer,              BOOLEAN,       false   #-- @desc  Support of Minimum Periodic Search Timer #-- @spec 36.523-2 A.4.4.1/84

pc_ePDCCH,                                   BOOLEAN,       false   #-- @desc  Support of ePDCCH #-- @spec 36.523-2 A.4.4.1/87

pc_ePSM,                                     BOOLEAN,       false   #-- @desc  Support of Power Saving Mode (in EUTRA) #-- @spec 36.523-2 A.4.4.1/YY

pc_eRedirectionUTRA,                         BOOLEAN,       false   #-- @desc  Support of use of the UTRA system information provided by RRCConnectionRelease upon redirection #-- @spec 36.523-2 A.4.4-1/31

pc_eTDD,                                     BOOLEAN,       false   #-- @desc  UE supports EUTRA TDD #-- @spec 36.523-2 A.4.1-1/2

pc_eTDD_MultiBand,                           BOOLEAN,       false   #-- @desc  Support of multiple E-UTRA TDD bands #-- @spec 36.523-2 A.4.1-2/2

pc_eWLAN,                                    BOOLEAN,       false   #-- @desc  WLAN #-- @spec 36.523-2 A.4.1-1/5

pc_edrx,                                     BOOLEAN,       false   #-- @desc  Support of extended DRX #-- @spec 36.523-2 A.4.4-1/121

pc_extendedLongDRX,                          BOOLEAN,       false   #-- @desc  Support of extended Long DRX cycle #-- @spec 36.523-2 A.4.4.1/abc

pc_fixed_broadband_XCAP,                     BOOLEAN,       false   #-- @desc  The UE uses XCAP in fixed broadband access #-- @spec 34.229-2 Table A.12/50

pc_freqBandPriorityAdjustment,               BOOLEAN,       false   #-- @desc  Support of prioritization of the frequency bands in multiBandInfoList over the band in freqBandIndicator as defined by freqBandIndicatorPriority-r12 #-- @spec 36.523-2 A.4.4-1/125

pc_gnss_heightMeas,                          BOOLEAN,       false   #-- @desc  Support of GNSS for height measurement #-- @spec 36.523-2 A.4.4-1/yyy

pc_gp10_en_dc,                               BOOLEAN,       false   #-- @desc Support NR supports gap pattern 10 for independent measurement gap configuration on FR1 and per-UE gap in (NG) EN-DC #-- @spec 38.508-2 A.4.3.6-1/17

pc_gp11_en_dc,                               BOOLEAN,       false   #-- @desc Support NR supports gap pattern 1 for independent measurement gap configuration on FR1 and per-UE gap in (NG) EN-DC #-- @spec 38.508-2 A.4.3.6-1/18

pc_gp13_en_dc,                               BOOLEAN,       false   #-- @desc Support of measurement gap pattern 13 configured by NR RRC when in (NG)EN-DC #-- @spec 38.508-2 A.4.3.6-1/92

pc_gp14_en_dc,                               BOOLEAN,       false   #-- @desc Support of measurement gap pattern 14 configured by NR RRC when in (NG)EN-DC #-- @spec 38.508-2 A.4.3.6-1/93

pc_gp2_gp3_en_dc,                            BOOLEAN,       false   #-- @desc Support shorter measurement gap length (i.e. gp2 and gp3) for independent measurement gap configuration on FR1 and per-UE gap in (NG)EN-DC. #-- @spec 38.508-2 A.4.3.6-1/10

pc_gp4_en_dc,                                BOOLEAN,       false   #-- @desc Support NR supports gap pattern 4 for independent measurement gap configuration on FR1 and per-UE gap in (NG) EN-DC #-- @spec 38.508-2 A.4.3.6-1/11

pc_gp5_en_dc,                                BOOLEAN,       false   #-- @desc Support NR supports gap pattern 5 for independent measurement gap configuration on FR1 and per-UE gap in (NG) EN-DC #-- @spec 38.508-2 A.4.3.6-1/12

pc_gp6_en_dc,                                BOOLEAN,       false   #-- @desc Support NR supports gap pattern 6 for independent measurement gap configuration on FR1 and per-UE gap in (NG) EN-DC #-- @spec 38.508-2 A.4.3.6-1/13

pc_gp7_en_dc,                                BOOLEAN,       false   #-- @desc Support NR supports gap pattern 7 for independent measurement gap configuration on FR1 and per-UE gap in (NG) EN-DC #-- @spec 38.508-2 A.4.3.6-1/14

pc_gp8_en_dc,                                BOOLEAN,       false   #-- @desc Support NR supports gap pattern 8 for independent measurement gap configuration on FR1 and per-UE gap in (NG) EN-DC #-- @spec 38.508-2 A.4.3.6-1/15

pc_gp9_en_dc,                                BOOLEAN,       false   #-- @desc Support NR supports gap pattern 9 for independent measurement gap configuration on FR1 and per-UE gap in (NG) EN-DC #-- @spec 38.508-2 A.4.3.6-1/16

pc_heightMeas,                               BOOLEAN,       false   #-- @desc  Support of height-based measurement reporting #-- @spec 36.523-2 A.4.4-1/xxx

pc_idleInactiveEUTRA_MeasReport,             BOOLEAN,       false   #-- @desc  Support configuration of E-UTRA measurements in RRC_IDLERRC_INACTIVE and reporting of the corresponding results upon network request as specified in TS 38.331 #-- @spec 38.508-2 Table A.4.3.6.1/55

pc_inactiveState,                            BOOLEAN,       false   #-- @desc  Support of RRC_INACTIVE as specified in TS 38.331 #-- @spec 38.508-2 Table A.4.3.7-1/19

pc_interRAT_NR_ToENDC,                       BOOLEAN,       false   #-- @desc  Support inter-RAT Handover from NR to EN-DC #-- @spec 38.508-2 Table A.4.3.8-1/10

pc_intraFreq_CE_NeedForGaps,                 BOOLEAN,       false   #-- @desc  Require intra-frequency measurement gaps for operating in CE Mode A or CE Mode B #-- @spec 36.523-2 A.4.4-1/xx1

pc_maxDL_PRS_RSRP_MeasurementFR1,            INTEGER,       1       #-- @desc  maxDL-PRS-RSRP-MeasurementFR1 #-- @spec 37.571-3 Table A.4.3-6E/1

pc_maxDL_PRS_RSRP_MeasurementFR2,            INTEGER,       1       #-- @desc  maxDL-PRS-RSRP-MeasurementFR2 #-- @spec 37.571-3 Table A.4.3-6E/2

pc_maxNrOfDL_PRS_ResourceSetPerTrpPerFrequencyLayer,INTEGER,       1       #-- @desc  maxNrOfDL-PRS-ResourceSetPerTrpPerFrequencyLayer #-- @spec 37.571-3 Table A.4.3-6B/1

pc_maxNrOfDL_PRS_ResourcesAcrossAllFL_TRP_ResourceSet_fr1_FR2Mix_fr1,ENUM-DL_PRS_ResourcesBandCombination_r16.maxNrOfDL_PRS_ResourcesAcrossAllFL_TRP_ResourceSet_r16.fr1_FR2Mix_r16.fr1_r16,n6      #-- @desc  maxNrOfDL-PRS-ResourcesAcrossAllFL-TRP-ResourceSet-fr1-FR2Mix-fr1 #-- @spec 37.571-3 Table A.4.3-6B/8

pc_maxNrOfDL_PRS_ResourcesAcrossAllFL_TRP_ResourceSet_fr1_FR2Mix_fr2,ENUM-DL_PRS_ResourcesBandCombination_r16.maxNrOfDL_PRS_ResourcesAcrossAllFL_TRP_ResourceSet_r16.fr1_FR2Mix_r16.fr2_r16,n24     #-- @desc  maxNrOfDL-PRS-ResourcesAcrossAllFL-TRP-ResourceSet-fr1-FR2Mix-fr2 #-- @spec 37.571-3 Table A.4.3-6B/22

pc_maxNrOfDL_PRS_ResourcesAcrossAllFL_TRP_ResourceSet_fr1_Only,ENUM-DL_PRS_ResourcesBandCombination_r16.maxNrOfDL_PRS_ResourcesAcrossAllFL_TRP_ResourceSet_r16.fr1_Only_r16,n6      #-- @desc  maxNrOfDL-PRS-ResourcesAcrossAllFL-TRP-ResourceSet-fr1-Only #-- @spec 37.571-3 Table A.4.3-6B/6

pc_maxNrOfDL_PRS_ResourcesAcrossAllFL_TRP_ResourceSet_fr2_Only,ENUM-DL_PRS_ResourcesBandCombination_r16.maxNrOfDL_PRS_ResourcesAcrossAllFL_TRP_ResourceSet_r16.fr2_Only_r16,n24     #-- @desc  maxNrOfDL-PRS-ResourcesAcrossAllFL-TRP-ResourceSet-fr2-Only #-- @spec 37.571-3 Table A.4.3-6B/7

pc_maxNrOfDL_PRS_ResourcesPerPositioningFrequencylayer,ENUM-DL_PRS_ResourcesCapabilityPerBand_r16.maxNrOfDL_PRS_ResourcesPerPositioningFrequencylayer_r16,n6      #-- @desc  maxNrOfDL-PRS-ResourcesPerPositioningFrequencylayer for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/5

pc_maxNrOfDL_PRS_ResourcesPerResourceSet,    ENUM-DL_PRS_ResourcesCapabilityPerBand_r16.maxNrOfDL_PRS_ResourcesPerResourceSet_r16,n1      #-- @desc  maxNrOfDL-PRS-ResourcesPerResourceSet for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/4

pc_maxNrOfPosLayer,                          INTEGER,       1       #-- @desc  maxNrOfPosLayer #-- @spec 37.571-3 Table A.4.3-6B/3

pc_maxNrOfRx_TX_MeasFR1,                     INTEGER,       1       #-- @desc  maxNrOfRx-TX-MeasFR1 #-- @spec 37.571-3 Table A.4.3-6C/1

pc_maxNrOfRx_TX_MeasFR2,                     INTEGER,       1       #-- @desc  maxNrOfRx-TX-MeasFR2 #-- @spec 37.571-3 Table A.4.3-6C/2

pc_maxNrOfTRP_AcrossFreqs,                   ENUM-NR_DL_PRS_ResourcesCapability_r16.maxNrOfTRP_AcrossFreqs_r16,n4      #-- @desc  maxNrOfTRP-AcrossFreqs #-- @spec 37.571-3 Table A.4.3-6B/2

pc_maxNumOfDL_PRS_ResProcessedPerSlot_SCS120,ENUM-PRS_ProcessingCapabilityPerBand_r16.maxNumOfDL_PRS_ResProcessedPerSlot_r16.scs120_r16,n1      #-- @desc  maxNumOfDL-PRS-ResProcessedPerSlot in 120kHz SCS for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/21

pc_maxNumOfDL_PRS_ResProcessedPerSlot_SCS15, ENUM-PRS_ProcessingCapabilityPerBand_r16.maxNumOfDL_PRS_ResProcessedPerSlot_r16.scs15_r16,n1      #-- @desc  maxNumOfDL-PRS-ResProcessedPerSlot in 15kHz SCS for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/18

pc_maxNumOfDL_PRS_ResProcessedPerSlot_SCS30, ENUM-PRS_ProcessingCapabilityPerBand_r16.maxNumOfDL_PRS_ResProcessedPerSlot_r16.scs30_r16,n1      #-- @desc  maxNumOfDL-PRS-ResProcessedPerSlot in 30kHz SCS for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/19

pc_maxNumOfDL_PRS_ResProcessedPerSlot_SCS60, ENUM-PRS_ProcessingCapabilityPerBand_r16.maxNumOfDL_PRS_ResProcessedPerSlot_r16.scs60_r16,n1      #-- @desc  maxNumOfDL-PRS-ResProcessedPerSlot in 60kHz SCS for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/20

pc_maxNumberAP_SRS_PosResourcesPerBWP,       ENUM-SRS_PosResourcesPerBand_r16.maxNumberAP_SRS_PosResourcesPerBWP_r16,n1      #-- @desc  maxNumberAP-SRS-PosResourcesPerBWP #-- @spec 37.571-3 Table A.4.3-6D/16

pc_maxNumberCSI_RS_BFD,                      BOOLEAN,       false   #-- @desc Support of CSI-RS based BFD #-- @spec 38.508-2 A.4.3.2-1/64

pc_maxNumberCSI_RS_SSB_CBD,                  BOOLEAN,       false   #-- @desc Support of SSB and/or CSI-RS based Link Recovery #-- @spec 38.508-2 A.4.3.2-1/65

pc_maxNumberPathLossEstimatePerServing,      ENUM-OLPC_SRS_Pos_r16.maxNumberPathLossEstimatePerServing_r16,n1      #-- @desc  maxNumberPathLossEstimatePerServing for at least one NR band #-- @spec 37.571-3 Table A.4.3-6D/6

pc_maxNumberPeriodicSRS_PosResourcesPerBWP,  ENUM-SRS_PosResourcesPerBand_r16.maxNumberPeriodicSRS_PosResourcesPerBWP_r16,n1      #-- @desc  maxNumberPeriodicSRS-PosResourcesPerBWP #-- @spec 37.571-3 Table A.4.3-6D/15

pc_maxNumberSP_SRS_PosResourcesPerBWP,       ENUM-SRS_PosResourcesPerBand_r16.maxNumberSP_SRS_PosResourcesPerBWP_r16,n1      #-- @desc  maxNumberSP-SRS-PosResourcesPerBWP #-- @spec 37.571-3 Table A.4.3-6D/17

pc_maxNumberSRS_PosPathLossEstimateAllServingCells,ENUM-NR_UL_SRS_Capability_r16.maxNumberSRS_PosPathLossEstimateAllServingCells_r16,n1      #-- @desc  maxNumberSRS-PosPathLossEstimateAllServingCells #-- @spec 37.571-3 Table A.4.3-6D/1

pc_maxNumberSRS_PosResourceSetsPerBWP,       ENUM-SRS_PosResourcesPerBand_r16.maxNumberSRS_PosResourceSetsPerBWP_r16,n1      #-- @desc  maxNumberSRS-PosResourceSetsPerBWP #-- @spec 37.571-3 Table A.4.3-6D/13

pc_maxNumberSRS_PosResourcesPerBWP,          ENUM-SRS_PosResourcesPerBand_r16.maxNumberSRS_PosResourcesPerBWP_r16,n1      #-- @desc  maxNumberSRS-PosResourcesPerBWP #-- @spec 37.571-3 Table A.4.3-6D/14

pc_maxNumberSRS_PosSpatialRelationsAllServingCell,ENUM-NR_UL_SRS_Capability_r16.maxNumberSRS_PosSpatialRelationsAllServingCells_r16,n0      #-- @desc  maxNumberSRS-PosSpatialRelationsAllServingCells #-- @spec 37.571-3 Table A.4.3-6D/2

pc_maxSupportedFreqLayers,                   INTEGER,       1       #-- @desc  maxSupportedFreqLayers-r16 #-- @spec 37.571-3 Table A.4.3-6B/11

pc_maximumPRS_BandwidthAcrossAllHopsFR1,     BOOLEAN,       false   #-- @desc  Supporting one of maximum DL-PRS bandwidth mhz40, mhz50, mhz80 and mhz100 across all hops  for FR1 for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/37

pc_maximumPRS_BandwidthAcrossAllHopsFR1_value,ENUM-DL_PRS_MeasurementWithRxFH_RRC_Connected_r18.maximumPRS_BandwidthAcrossAllHopsFR1_r18,mhz40   #-- @desc  ppw-maxNumOfDL-Bandwidth in FR1 for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/34

pc_maximumPRS_BandwidthAcrossAllHopsFR2,     BOOLEAN,       false   #-- @desc  Supporting one of maximum DL-PRS bandwidth mhz100, mhz200 and mhz400 across all hops  for FR2 for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/38

pc_maximumPRS_BandwidthAcrossAllHopsFR2_value,ENUM-DL_PRS_MeasurementWithRxFH_RRC_Connected_r18.maximumPRS_BandwidthAcrossAllHopsFR1_r18,mhz100  #-- @desc  ppw-maxNumOfDL-Bandwidth in FR1 for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/34

pc_measureSameDL_PRS_ResourceWithDifferentRxTEGs,ENUM-NR_UE_TEG_ID_CapabilityPerBand_r17.measureSameDL_PRS_ResourceWithDifferentRxTEGs_r17,n2      #-- @desc  measureSameDL-PRS-ResourceWithDifferentRxTEGs for at least one NR band #-- @spec 37.571-3 Table A.4.3-6G/4

pc_measureSameDL_PRS_ResourceWithDifferentRxTEGsSimul,ENUM-NR_UE_TEG_ID_CapabilityPerBand_r17.measureSameDL_PRS_ResourceWithDifferentRxTEGsSimul_r17,n1      #-- @desc  measureSameDL-PRS-ResourceWithDifferentRxTEGsSimul for at least one NR band #-- @spec 37.571-3 Table A.4.3-6G/5

pc_mg_ActivationCommPRS_Meas,                BOOLEAN,       false   #-- @desc  Support for preconfiguration of MGs in RRC signalling for PRS measurements and the use of DL MAC CE from the gNB to activatedeactivate the preconfigured MG for PRS measurements. #-- @spec 37.571-3 Table A.4.3-2/46

pc_mg_ActivationRequest,                     BOOLEAN,       false   #-- @desc  Support for low latency measurement gap activation request for DL-PRS measurements. #-- @spec 37.571-3 Table A.4.3-2/45

pc_mg_ActivationRequestPRS_Meas,             BOOLEAN,       false   #-- @desc  Support for preconfiguration of MGs in RRC signalling for PRS measurements and supports the use of UL MAC CE to request the activationdeactivation of the preconfigured MG for PRS measurements. #-- @spec 37.571-3 Table A.4.3-2/47

pc_mg_ActivationRequest_DL_AoD,              BOOLEAN,       false   #-- @desc  Support of mg-ActivationRequest for DL-AoD positioning method #-- @spec 37.571-3 Table A.4.3-6E/8

pc_mg_ActivationRequest_DL_TDOA,             BOOLEAN,       false   #-- @desc  Support of mg-ActivationRequest for DL-TDOA positioning method #-- @spec 37.571-3 Table A.4.3-6F/9

pc_mg_ActivationRequest_Multi_RTT,           BOOLEAN,       false   #-- @desc  Support of mg-ActivationRequest for Multi-RTT positioning method #-- @spec 37.571-3 Table A.4.3-6C/9

pc_mtrpPuschCyclicMapping_r17,               BOOLEAN,       false   #-- @desc  Indicates whether UE supports cyclic mapping when the number of repetitions is larger than 2 with repetition type. #-- @spec 38.508-2 Table A.4.3.2-1/145

pc_multipleTimingAdvance,                    BOOLEAN,       false   #-- @desc  Support of multiple timing advances #-- @spec 36.523-2 A.4.4-1A/3

pc_multipleUplinkSPS,                        BOOLEAN,       false   #-- @desc  Support of multiple uplink SPS and reporting SPS assistance information #-- @spec 36.523-2 A.4.4-1/177

pc_noOf_PDNsSameConnection,                  INTEGER,       1       #-- @desc  Number of UE requested PDN connection establishments after ATTACH during the same signaling connection #-- @spec 38.508-2 Table A.4.4-2/5

pc_no_eutra_disable_5GS,                     BOOLEAN,       false   #-- @desc  Support of being configured for No E-UTRA Disabling In 5GS #-- @spec 38.508-2 Table A.4.3.7-1/58

pc_not_SMS_only,                             BOOLEAN,       false   #-- @desc  Supports not sending SMS only in the Additional update type IE #-- @spec 

pc_nr_DL_PRS_RSCPD_ReportingRRC_Connected_DL_TDOA,BOOLEAN,       false   #-- @desc  Support of reporting RSCPD in RRC CONNECTED for DL-TDOA positioning method #-- @spec 37.571-3 Table A.4.3-6F/12

pc_nr_DL_PRS_RSCP_ReportingRRC_Connected_Multi_RTT,BOOLEAN,       false   #-- @desc  Support of reporting RSCP in RRC CONNECTED for Multi-RTT positioning method #-- @spec 37.571-3 Table A.4.3-6C/12

pc_nr_UE_RxTEG_ID_MaxSupport,                ENUM-NR_UE_TEG_ID_CapabilityPerBand_r17.nr_UE_RxTEG_ID_MaxSupport_r17,n1      #-- @desc  Support at least one UE-RxTEG for at least one NR band #-- @spec 37.571-3 Table A.4.3-6G/1

pc_nr_UE_RxTxTEG_ID_MaxSupport,              ENUM-NR_UE_TEG_ID_CapabilityPerBand_r17.nr_UE_RxTxTEG_ID_MaxSupport_r17,n1      #-- @desc  nr-UE-RxTxTEG-ID-MaxSupport for at least one NR band #-- @spec 37.571-3 Table A.4.3-6G/3

pc_nr_UE_TxTEG_ID,                           BOOLEAN,       false   #-- @desc  Support at least one UE-TxTEG for at least one NR band #-- @spec 37.571-3 Table A.4.3-6G/6

pc_nr_UE_TxTEG_ID_MaxSupport,                ENUM-NR_UE_TEG_ID_CapabilityPerBand_r17.nr_UE_TxTEG_ID_MaxSupport_r17,n1      #-- @desc  nr-UE-TxTEG-ID-MaxSupport for at least one NR band #-- @spec 37.571-3 Table A.4.3-6G/2

pc_ntn_SegmentedPrecompensationGaps,         BOOLEAN,       false   #-- @desc  Support of gap length between segments for PUSCH and PUCCH required by a UE supporting ce-ModeA-r13 or for NPUSCH required by a UE supporting ue-category-NB for TA pre-compensation #-- @spec 36.523-2 A.4.4-1/238

pc_olpc_SRS_PosBasedOnPRS_Neigh,             BOOLEAN,       false   #-- @desc  Support of olpc-SRS-PosBasedOnPRS-Neigh for at least one NR band #-- @spec 37.571-3 Table A.4.3-6D/5

pc_olpc_SRS_PosBasedOnPRS_Serving,           BOOLEAN,       false   #-- @desc  Support of olpc-SRS-PosBasedOnPRS-Serving for at least one NR band #-- @spec 37.571-3 Table A.4.3-6D/3

pc_olpc_SRS_PosBasedOnSSB_Neigh,             BOOLEAN,       false   #-- @desc  Support of olpc-SRS-PosBasedOnSSB-Neigh for at least one NR band #-- @spec 37.571-3 Table A.4.3-6D/4

pc_operator_controlled_signal_threshold_per_access_technology,BOOLEAN,       false   #-- @desc  Support of operator controlled signal threshold per access technology #-- @spec 36.523-2 A.4.4-1/zzz

pc_posMeasGapSupport_DL_AoD,                 BOOLEAN,       false   #-- @desc  posMeasGapSupport for DL-AoD positioning method #-- @spec 37.571-3 Table A.4.3-6E/9

pc_posMeasGapSupport_DL_TDOA,                BOOLEAN,       false   #-- @desc  posMeasGapSupport for DL-TDOA positioning method #-- @spec 37.571-3 Table A.4.3-6F/10

pc_posMeasGapSupport_Multi_RTT,              BOOLEAN,       false   #-- @desc  posMeasGapSupport for Multi-RTT positioning method #-- @spec 37.571-3 Table A.4.3-6C/10

pc_posSRS_ValidityAreaRRC_InactiveInitialUL_BWP,BOOLEAN,       false   #-- @desc  posSRS-ValidityAreaRRC-InactiveInitialUL-BWP for at least one NR band #-- @spec 37.571-3 Table A.4.3-6D/18

pc_ppw_dl_PRS_BufferType,                    ENUM-PRS_ProcessingCapabilityOutsideMGinPPWperType_r17.,type1   #-- @desc  ppw-dl-PRS-BufferType for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/25

pc_ppw_durationOfPRS_ProcessingSymbolsN,     ENUM-PRS_ProcessingCapabilityOutsideMGinPPWperType_r17.,msDot125 #-- @desc  ppw-durationOfPRS-ProcessingSymbolsN for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/26

pc_ppw_durationOfPRS_ProcessingSymbolsN2,    ENUM-PRS_ProcessingCapabilityOutsideMGinPPWperType_r17.,msDot125 #-- @desc  ppw-durationOfPRS-ProcessingSymbolsN2 for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/28

pc_ppw_durationOfPRS_ProcessingSymbolsT,     ENUM-PRS_ProcessingCapabilityOutsideMGinPPWperType_r17.,ms1     #-- @desc  ppw-durationOfPRS-ProcessingSymbolsT for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/27

pc_ppw_durationOfPRS_ProcessingSymbolsT2,    ENUM-PRS_ProcessingCapabilityOutsideMGinPPWperType_r17.,ms4     #-- @desc  ppw-durationOfPRS-ProcessingSymbolsT2 for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/29

pc_ppw_maxNumOfDL_Bandwidth_FR1,             ENUM-PRS_ProcessingCapabilityOutsideMGinPPWperType_r17.,mhz5    #-- @desc  ppw-maxNumOfDL-Bandwidth in FR1 for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/34

pc_ppw_maxNumOfDL_Bandwidth_FR2,             ENUM-PRS_ProcessingCapabilityOutsideMGinPPWperType_r17.,mhz50   #-- @desc  ppw-maxNumOfDL-Bandwidth in FR2 for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/35

pc_ppw_maxNumOfDL_PRS_ResProcessedPerSlot_SCS120,ENUM-PRS_ProcessingCapabilityOutsideMGinPPWperType_r17.,n1      #-- @desc  ppw-maxNumOfDL-PRS-ResProcessedPerSlot in 120kHz SCS for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/33

pc_ppw_maxNumOfDL_PRS_ResProcessedPerSlot_SCS15,ENUM-PRS_ProcessingCapabilityOutsideMGinPPWperType_r17.,n1      #-- @desc  ppw-maxNumOfDL-PRS-ResProcessedPerSlot in 15kHz SCS for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/30

pc_ppw_maxNumOfDL_PRS_ResProcessedPerSlot_SCS30,ENUM-PRS_ProcessingCapabilityOutsideMGinPPWperType_r17.,n1      #-- @desc  ppw-maxNumOfDL-PRS-ResProcessedPerSlot in 30kHz SCS for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/31

pc_ppw_maxNumOfDL_PRS_ResProcessedPerSlot_SCS60,ENUM-PRS_ProcessingCapabilityOutsideMGinPPWperType_r17.,n1      #-- @desc  ppw-maxNumOfDL-PRS-ResProcessedPerSlot in 60kHz SCS for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/32

pc_protection_against_improperReselection_to_GERAN_UTRAN,BOOLEAN,       false   #-- @desc  Support of protection against improper reselection to GERAN/UTRAN #-- @spec 36.523-2 A.4.4-1/266

pc_prsProcessingType,                        ENUM-PRS_ProcessingCapabilityOutsideMGinPPWperType_r17.,type1A  #-- @desc  prsProcessingType for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/24

pc_prs_FromServNeighCellAsQCL,               BOOLEAN,       false   #-- @desc  Support of prs-FromServNeighCellAsQCL for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/10

pc_prs_ProcessingCapabilityOutsideMGinPPW,   BOOLEAN,       false   #-- @desc  Support for DL-PRS Processing Capability outside MG #-- @spec 37.571-3 Table A.4.3-2/48

pc_prs_ProcessingWindowType1A,               BOOLEAN,       false   #-- @desc  Support one of option1 option2 or option3 priority options of prs-ProcessingWindowType1A #-- @spec 37.571-3 Table A.4.3-2/49

pc_prs_ProcessingWindowType1B,               BOOLEAN,       false   #-- @desc  Support one of option1 option2 or option3 priority options of prs-ProcessingWindowType1B #-- @spec 37.571-3 Table A.4.3-2/50

pc_prs_ProcessingWindowType2,                BOOLEAN,       false   #-- @desc  Support one of option1 option2 or option3 priority options of prs-ProcessingWindowType2 #-- @spec 37.571-3 Table A.4.3-2/51

pc_prs_frequencyhopping_MeasureAndReport,    BOOLEAN,       false   #-- @desc  Support of PRS receiver frequency hopping measurement and report the nr-ReportDL-PRS-MeasBasedOnSingleOrMultiHopRx-r18 after reception of nr-DL-PRS-RxHoppingRequest-r18 #-- @spec 37.571-3 Table A.4.3-2/53

pc_pusch_RepetitionMsg3_r17,                 BOOLEAN,       false   #-- @desc  Support of repetition of PUSCH transmission scheduled by RAR UL grant and DCI format 0_0 with CRC scrambled by TC-RNTI. #-- @spec 38.508-2 Table A.4.3.2-1/85

pc_qci1Indication_inRLF,                     BOOLEAN,       false   #-- @desc  Support of QCI1 indication in Radio Link Failure Report #-- @spec 36.523-2 A.4.4-1/131

pc_qoe_MTSI_MeasReport,                      BOOLEAN,       false   #-- @desc  Support of QoE Measurement collection for MTSI Service #-- @spec 36.523-2 A.4.4-1/182

pc_qoe_MeasReport,                           BOOLEAN,       false   #-- @desc  Support of QoE Measurement collection for Streaming Service #-- @spec 36.523-2 A.4.4-1/181

pc_ra_Type0_PUSCH,                           BOOLEAN,       false   #-- @desc  Support resource allocation Type 0 for PUSCH #-- @spec 38.508-2 Table A.4.3.2-1/7

pc_reqFreqBands,                             BOOLEAN,       false   #-- @desc  Support of reception of requested Frequency Bands #-- @spec 36.523-2 A.4.4.1/101

pc_rssiAndChannelOccupancyReporting,         BOOLEAN,       false   #-- @desc  Supports measurement and reporting for RSSI and channel occupancy #-- @spec 36.523-2 A.4.4-1/ZZ

pc_scptm_NonServingCell,                     BOOLEAN,       false   #-- @desc  Support of MBMS reception via SC-PTM on a cell that may be additionally configured as an Scell #-- @spec 36.523-2 A.4.4-1/127

pc_scptm_SCell,                              BOOLEAN,       false   #-- @desc  Support of MBMS reception via SC-PTM on configured SCell #-- @spec 36.523-2 A.4.4-1/126

pc_shortSPS_intervalFDD,                     BOOLEAN,       false   #-- @desc  Support of SPS interval shorter than 10 subfranes in FDD mode #-- @spec 36.523-2 A.4.4-1/170

pc_shortSPS_intervalTDD,                     BOOLEAN,       false   #-- @desc  Support of SPS interval shorter than 10 subfranes in TDD mode #-- @spec 36.523-2 A.4.4-1/171

pc_simulLTE_NR_PRS,                          BOOLEAN,       false   #-- @desc  Support of simulLTE-NR-PRS #-- @spec 37.571-3 Table A.4.3-6B/12

pc_simul_NR_DL_AoD_DL_TDOA,                  BOOLEAN,       false   #-- @desc  Support of simul-NR-DL-AoD-DL-TDOA for at least one NR band #-- @spec 37.571-3 Table A.4.3-6E/3

pc_simul_NR_DL_AoD_Multi_RTT,                BOOLEAN,       false   #-- @desc  Support of simul-NR-DL-AoD-Multi-RTT for at least one NR band #-- @spec 37.571-3 Table A.4.3-6E/4

pc_skipUplinkDynamic,                        BOOLEAN,       false   #-- @desc  Support of skipping UL transmissions if no data is available #-- @spec 36.523-2 A.4.4-1/173

pc_skipUplinkSPS,                            BOOLEAN,       false   #-- @desc  Support of skipping SPS UL transmissions if no data is available #-- @spec 36.523-2 A.4.4-1/172

pc_spatialRelation_SRS_PosBasedOnCSI_RS_Serving,BOOLEAN,       false   #-- @desc  Support of spatialRelation-SRS-PosBasedOnCSI-RS-Serving for at least one NR band #-- @spec 37.571-3 Table A.4.3-6D/8

pc_spatialRelation_SRS_PosBasedOnPRS_Neigh,  BOOLEAN,       false   #-- @desc  Support of spatialRelation-SRS-PosBasedOnPRS-Neigh for at least one NR band #-- @spec 37.571-3 Table A.4.3-6D/12

pc_spatialRelation_SRS_PosBasedOnPRS_Serving,BOOLEAN,       false   #-- @desc  Support of spatialRelation-SRS-PosBasedOnPRS-Serving for at least one NR band #-- @spec 37.571-3 Table A.4.3-6D/9

pc_spatialRelation_SRS_PosBasedOnSRS,        BOOLEAN,       false   #-- @desc  Support of spatialRelation-SRS-PosBasedOnSRS for at least one NR band #-- @spec 37.571-3 Table A.4.3-6D/10

pc_spatialRelation_SRS_PosBasedOnSSB_Neigh,  BOOLEAN,       false   #-- @desc  Support of spatialRelation-SRS-PosBasedOnSSB-Neigh for at least one NR band #-- @spec 37.571-3 Table A.4.3-6D/11

pc_spatialRelation_SRS_PosBasedOnSSB_Serving,BOOLEAN,       false   #-- @desc  Support of spatialRelation-SRS-PosBasedOnSSB-Serving for at least one NR band #-- @spec 37.571-3 Table A.4.3-6D/7

pc_srb3,                                     BOOLEAN,       false   #-- @desc  Support direct SRB between the SN and the UE #-- @spec 38.508-2 Table A.4.3.7-1/3

pc_srs_AssocPRS_MultiLayersFR1,              BOOLEAN,       false   #-- @desc  Support of srs-AssocPRS-MultiLayersFR1 #-- @spec 37.571-3 Table A.4.3-6C/5

pc_srs_AssocPRS_MultiLayersFR2,              BOOLEAN,       false   #-- @desc  Support of srs-AssocPRS-MultiLayersFR2 #-- @spec 37.571-3 Table A.4.3-6C/6

pc_ss_CCH_Interference_Handling,             BOOLEAN,       false   #-- @desc  Support of Synchronisation signal and common channel interference handling #-- @spec 36.523-2 A.4.4-1A/8

pc_ss_SINR_Meas,                             BOOLEAN,       false   #-- @desc  Support SS-SINR measurements #-- @spec 38.508-2 Table A.4.3.6-1/6

pc_ssb_FromNeighCellAsQCL,                   BOOLEAN,       false   #-- @desc  Support of ssb-FromNeighCellAsQCL for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/9

pc_supportedBandwidthPRS_FR1,                ENUM-PRS_ProcessingCapabilityPerBand_r16.supportedBandwidthPRS_r16.fr1,mhz5    #-- @desc  supportedBandwidthPRS in FR1 for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/13

pc_supportedBandwidthPRS_FR2,                ENUM-PRS_ProcessingCapabilityPerBand_r16.supportedBandwidthPRS_r16.fr2,mhz50   #-- @desc  supportedBandwidthPRS in FR2 for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/14

pc_supportedDL_PRS_ProcessingSamples_RRC_CONNECTED,BOOLEAN,       false   #-- @desc  supportedDL-PRS-ProcessingSamples-RRC-CONNECTED for at least one NR band #-- @spec 37.571-3 Table A.4.3-6B/23

pc_survivalTime_r17,                         BOOLEAN,       false   #-- @desc  Support services with survival time requirement using configured grant resource and PDCP duplication as specified in TS 38.321. #-- @spec 38.508-2 Table A.4.3.5-1/16

pc_tdd_FDD_CA_FDD_PCell,                     BOOLEAN,       false   #-- @desc  Support of tdd-FDD-CA-PCellDuplex-r12 with the second bit setting to 1 #-- @spec 36.523-2 A.4.4.1/109

pc_tdd_FDD_CA_TDD_PCell,                     BOOLEAN,       false   #-- @desc  Support of tdd-FDD-CA-PCellDuplex-r12 with the first bit setting to 1 #-- @spec 36.523-2 A.4.4.1/108

pc_twoStepScheduling_uplink_LAA,             BOOLEAN,       false   #-- @desc  Supports two step uplink scheduling using PUSCH trigger A and PUSCH trigger B #-- @spec 36.523-2 A.4.4-1/176

pc_ue_CategoryDL_0,                          BOOLEAN,       false   #-- @desc  UE Category DL 0 #-- @spec 36.523-2 A.4.3.2-2/1

pc_ue_CategoryDL_10,                         BOOLEAN,       false   #-- @desc  UE Category DL 10 #-- @spec 36.523-2 A.4.3.2-2/5

pc_ue_CategoryDL_11,                         BOOLEAN,       false   #-- @desc  UE Category DL 11 #-- @spec 36.523-2 A.4.3.2-2/6

pc_ue_CategoryDL_12,                         BOOLEAN,       false   #-- @desc  UE Category DL 12 #-- @spec 36.523-2 A.4.3.2-2/7

pc_ue_CategoryDL_13,                         BOOLEAN,       false   #-- @desc  UE Category DL 13 #-- @spec 36.523-2 A.4.3.2-2/8

pc_ue_CategoryDL_14,                         BOOLEAN,       false   #-- @desc  UE Category DL 14 #-- @spec 36.523-2 A.4.3.2-2/9

pc_ue_CategoryDL_15,                         BOOLEAN,       false   #-- @desc  UE Category DL 15 #-- @spec 36.523-2 A.4.3.2-2/10

pc_ue_CategoryDL_16,                         BOOLEAN,       false   #-- @desc  UE Category DL 16 #-- @spec 36.523-2 A.4.3.2-2/11

pc_ue_CategoryDL_17,                         BOOLEAN,       false   #-- @desc  UE Category DL 17 #-- @spec 36.523-2 A.4.3.2-2/12

pc_ue_CategoryDL_18,                         BOOLEAN,       false   #-- @desc  UE Category DL 18 #-- @spec 36.523-2 A.4.3.2-2/13

pc_ue_CategoryDL_19,                         BOOLEAN,       false   #-- @desc  UE Category DL 19 #-- @spec 36.523-2 A.4.3.2-2/14

pc_ue_CategoryDL_1bis,                       BOOLEAN,       false   #-- @desc  Only in combination with Category UL 1bis and Category 1 UE #-- @spec 36.523-2 A.4.3.2-2A/2

pc_ue_CategoryDL_20,                         BOOLEAN,       false   #-- @desc  UE Category DL 20 #-- @spec 36.523-2 A.4.3.2-2/15

pc_ue_CategoryDL_21,                         BOOLEAN,       false   #-- @desc  UE Category DL 21 #-- @spec 36.523-2 A.4.3.2-2/16

pc_ue_CategoryDL_22,                         BOOLEAN,       false   #-- @desc  UE Category DL 22 #-- @spec 36.523-2 A.4.3.2-2/17

pc_ue_CategoryDL_23,                         BOOLEAN,       false   #-- @desc  UE Category DL 23 #-- @spec 36.523-2 A.4.3.2-2/18

pc_ue_CategoryDL_24,                         BOOLEAN,       false   #-- @desc  UE Category DL 24 #-- @spec 36.523-2 A.4.3.2-2/19

pc_ue_CategoryDL_25,                         BOOLEAN,       false   #-- @desc  UE Category DL 25 #-- @spec 36.523-2 A.4.3.2-2/20

pc_ue_CategoryDL_26,                         BOOLEAN,       false   #-- @desc  UE Category DL 26 #-- @spec 36.523-2 A.4.3.2-2/21

pc_ue_CategoryDL_4,                          BOOLEAN,       false   #-- @desc  UE Category DL 4 #-- @spec 36.523-2 A.4.3.2-2/1A

pc_ue_CategoryDL_6,                          BOOLEAN,       false   #-- @desc  UE Category DL 6 #-- @spec 36.523-2 A.4.3.2-2/2

pc_ue_CategoryDL_7,                          BOOLEAN,       false   #-- @desc  UE Category DL 7 #-- @spec 36.523-2 A.4.3.2-2/3

pc_ue_CategoryDL_9,                          BOOLEAN,       false   #-- @desc  UE Category DL 9 #-- @spec 36.523-2 A.4.3.2-2/4

pc_ue_CategoryDL_M1,                         BOOLEAN,       false   #-- @desc  Only in combination with Category UL M0 #-- @spec 36.523-2 A.4.3.2-2A/1

pc_ue_CategoryDL_M2,                         BOOLEAN,       false   #-- @desc  Only in combination with Category UL M2 #-- @spec 36.523-2 A.4.3.2-2A/3

pc_ue_CategoryUL_0,                          BOOLEAN,       false   #-- @desc  UE Category UL 0 #-- @spec 36.523-2 A.4.3.2-3/1

pc_ue_CategoryUL_13,                         BOOLEAN,       false   #-- @desc  UE Category UL 13 #-- @spec 36.523-2 A.4.3.2-3/6

pc_ue_CategoryUL_14,                         BOOLEAN,       false   #-- @desc  UE Category UL 14 #-- @spec 36.523-2 A.4.3.2-3/7

pc_ue_CategoryUL_15,                         BOOLEAN,       false   #-- @desc  UE Category UL 15 #-- @spec 36.523-2 A.4.3.2-3/8

pc_ue_CategoryUL_16,                         BOOLEAN,       false   #-- @desc  UE Category UL 16 #-- @spec 36.523-2 A.4.3.2-3/9

pc_ue_CategoryUL_17,                         BOOLEAN,       false   #-- @desc  UE Category UL 17 #-- @spec 36.523-2 A.4.3.2-3/10

pc_ue_CategoryUL_18,                         BOOLEAN,       false   #-- @desc  UE Category UL 18 #-- @spec 36.523-2 A.4.3.2-3/11

pc_ue_CategoryUL_19,                         BOOLEAN,       false   #-- @desc  UE Category UL 19 #-- @spec 36.523-2 A.4.3.2-3/12

pc_ue_CategoryUL_1bis,                       BOOLEAN,       false   #-- @desc  Only in combination with Category DL 1bis #-- @spec 36.523-2 A.4.3.2-3A/2

pc_ue_CategoryUL_20,                         BOOLEAN,       false   #-- @desc  UE Category UL 20 #-- @spec 36.523-2 A.4.3.2-3/13

pc_ue_CategoryUL_21,                         BOOLEAN,       false   #-- @desc  UE Category UL 21 #-- @spec 36.523-2 A.4.3.2-3/14

pc_ue_CategoryUL_22,                         BOOLEAN,       false   #-- @desc  UE Category UL 22 #-- @spec 36.523-2 A.4.3.2-3/15

pc_ue_CategoryUL_23,                         BOOLEAN,       false   #-- @desc  UE Category UL 23 #-- @spec 36.523-2 A.4.3.2-3/16

pc_ue_CategoryUL_24,                         BOOLEAN,       false   #-- @desc  UE Category UL 24 #-- @spec 36.523-2 A.4.3.2-3/17

pc_ue_CategoryUL_25,                         BOOLEAN,       false   #-- @desc  UE Category UL 25 #-- @spec 36.523-2 A.4.3.2-3/18

pc_ue_CategoryUL_26,                         BOOLEAN,       false   #-- @desc  UE Category UL 26 #-- @spec 36.523-2 A.4.3.2-3/19

pc_ue_CategoryUL_3,                          BOOLEAN,       false   #-- @desc  UE Category UL 3 #-- @spec 36.523-2 A.4.3.2-3/2

pc_ue_CategoryUL_5,                          BOOLEAN,       false   #-- @desc  UE Category UL 5 #-- @spec 36.523-2 A.4.3.2-3/3

pc_ue_CategoryUL_7,                          BOOLEAN,       false   #-- @desc  UE Category UL 7 #-- @spec 36.523-2 A.4.3.2-3/4

pc_ue_CategoryUL_8,                          BOOLEAN,       false   #-- @desc  UE Category UL 8 #-- @spec 36.523-2 A.4.3.2-3/5

pc_ue_CategoryUL_M1,                         BOOLEAN,       false   #-- @desc  Only in combination with Category DL M1 #-- @spec 36.523-2 A.4.3.2-3A/1

pc_ue_CategoryUL_M2,                         BOOLEAN,       false   #-- @desc  Only in combination with Category DL M2 #-- @spec 36.523-2 A.4.3.2-3A/3

pc_ue_Category_1,                            BOOLEAN,       false   #-- @desc  UE Category 1 #-- @spec 36.523-2 A.4.3.2-1/1

pc_ue_Category_10,                           BOOLEAN,       false   #-- @desc  UE Category 10 #-- @spec 36.523-2 A.4.3.2-1/10

pc_ue_Category_11,                           BOOLEAN,       false   #-- @desc  UE Category 11 #-- @spec 36.523-2 A.4.3.2-1/11

pc_ue_Category_12,                           BOOLEAN,       false   #-- @desc  UE Category 12 #-- @spec 36.523-2 A.4.3.2-1/12

pc_ue_Category_2,                            BOOLEAN,       false   #-- @desc  UE Category 2 #-- @spec 36.523-2 A.4.3.2-1/2

pc_ue_Category_3,                            BOOLEAN,       false   #-- @desc  UE Category 3 #-- @spec 36.523-2 A.4.3.2-1/3

pc_ue_Category_4,                            BOOLEAN,       false   #-- @desc  UE Category 4 #-- @spec 36.523-2 A.4.3.2-1/4

pc_ue_Category_5,                            BOOLEAN,       false   #-- @desc  UE Category 5 #-- @spec 36.523-2 A.4.3.2-1/5

pc_ue_Category_6,                            BOOLEAN,       false   #-- @desc  UE Category 6 #-- @spec 36.523-2 A.4.3.2-1/6

pc_ue_Category_7,                            BOOLEAN,       false   #-- @desc  UE Category 7 #-- @spec 36.523-2 A.4.3.2-1/7

pc_ue_Category_8,                            BOOLEAN,       false   #-- @desc  UE Category 8 #-- @spec 36.523-2 A.4.3.2-1/8

pc_ue_Category_9,                            BOOLEAN,       false   #-- @desc  UE Category 9 #-- @spec 36.523-2 A.4.3.2-1/9

pc_ue_Category_NB1,                          BOOLEAN,       false   #-- @desc  Category NB1 #-- @spec 36.523-2 A.4.3.2.-1A/1

pc_ue_Category_NB2,                          BOOLEAN,       false   #-- @desc  Category NB2 #-- @spec 36.523-2 A.4.3.2.-1A/2

pc_uplink_LAA,                               BOOLEAN,       false   #-- @desc  Supports uplink LAA operation #-- @spec 36.523-2 A.4.4-1/174

pc_v2xCBRMeas,                               BOOLEAN,       false   #-- @desc  Support of CBR measurement and reporting #-- @spec 36.523-2 A.4.4-1/156

pc_v2xCommSidelink,                          BOOLEAN,       false   #-- @desc  Support of V2X sidelink communication #-- @spec 36.523-2 A.4.4-1/148

pc_v2xCommUu,                                BOOLEAN,       false   #-- @desc  Support of V2X communication Via Uu #-- @spec 36.523-2 A.4.4-1/149

pc_v2xFullSensing,                           BOOLEAN,       false   #-- @desc  Support of transmitting PSCCHPSSCH using UE autonomous resource selection mode with full sensing #-- @spec 36.523-2 A.4.4-1/153

pc_v2xPartialSensing,                        BOOLEAN,       false   #-- @desc  Support of transmitting PSCCHPSSCH using UE autonomous resource selection mode with partial sensing #-- @spec 36.523-2 A.4.4-1/154

pc_v2xSLSS,                                  BOOLEAN,       false   #-- @desc  Support of SLSS transmission and reception for V2X sidelink communication #-- @spec 36.523-2 A.4.4-1/155

pc_v2xScheduling,                            BOOLEAN,       false   #-- @desc  Support of transmitting PSCCHPSSCH using dynamic scheduling #-- @spec 36.523-2 A.4.4-1/152

pc_v2xZoneBasedPoolSelection,                BOOLEAN,       false   #-- @desc  Support of zone based transmission resource pool selection for V2X sidelink communication #-- @spec 36.523-2 A.4.4-1/157

pc_voiceOverNR,                              BOOLEAN,       false   #-- @desc  Support IMS voice over NR #-- @spec 38.508-2 Table A.4.3.7-1/32

pc_voice_PS_1_CS_2,                          BOOLEAN,       false   #-- @desc  Configured voice domain preference #-- @spec 36.523-2 A.4.4.2-n

pc_voice_centric,                            BOOLEAN,       false   #-- @desc  Support of configuring the UE to voice centric #-- @spec 

pc_wakeUpSignal,                             BOOLEAN,       false   #-- @desc  Support of Wake Up Signal #-- @spec 36.523-2 A.4.4-1/210

px_1XRTT_BandClass,                          INTEGER,       1       #-- @desc  Band Class; Table 1.5-1 of C.S0057_D. Default value corresponds to 1.8 to 2.0 GHz PCS band #-- @spec 

px_1XRTT_BaseId_Cell19,                      BITSTRING,     0000000000100111 #-- @desc  Base Id of Cell 19 #-- @spec 

px_1XRTT_BaseId_Cell20,                      BITSTRING,     0000000000101000 #-- @desc  Base Id of Cell 20 #-- @spec 

px_1XRTT_BaseId_Cell21,                      BITSTRING,     0000000000101001 #-- @desc  Base Id of Cell 21 #-- @spec 

px_1XRTT_BaseId_Cell22,                      BITSTRING,     0000000000101010 #-- @desc  Base Id of Cell 22 #-- @spec 

px_1XRTT_CS_PagingMessage_Cell19,            OCTETSTRING,   123456  #-- @desc  Encoded PDU of CS paging message  to be sent in DLInformationTransfer; The message is encapsulated in a GCSNA1xCircuitService defined in C.S0097 clause 2.4.1 #-- @spec 

px_1XRTT_HandoffDirectionCell19,             OCTETSTRING,   123456  #-- @desc  Encoded PDU of Handoff Direction Assignment to be sent in MobilityFromEUTRACommand #-- @spec 

px_1XRTT_MinProtRev,                         INTEGER,       0       #-- @desc  Minimum protocol revision support by Base Station #-- @spec 

px_1XRTT_MobilityParametersCell19,           OCTETSTRING,   123456  #-- @desc  Encoded PDU of mobility parameters to be sent in HandoverfromEUTRAPreparationRequest #-- @spec 

px_1XRTT_MobilityParametersCell21,           OCTETSTRING,   123456  #-- @desc  Encoded PDU of mobility parameters to be sent in HandoverfromEUTRAPreparationRequest #-- @spec 

px_1XRTT_NID,                                BITSTRING,     0000000001100100 #-- @desc  default Network ID of 1xRTT Cells #-- @spec 

px_1XRTT_SID,                                BITSTRING,     000000011001000 #-- @desc  default System ID of 1xRTT Cells #-- @spec 

px_1XRTT_Sig_EncMode,                        INTEGER,       2       #-- @desc  Rijndael algorithm #-- @spec 

px_1XRTT_TMSI_Def,                           OCTETSTRING,   1234ABCD #-- @desc  TMSI to be used in 1xRTT #-- @spec 

px_1XRTT_UserInfo_EncMode,                   INTEGER,       2       #-- @desc  Rijndael algorithm #-- @spec 

px_1XRTT_Zone_Timer,                         BITSTRING,     000     #-- @desc  Zone timer sent in 'System Parameters Message' overhead message #-- @spec 

px_8PSK_PowerCap,                            BITSTRING,     00      #-- @desc  Power Class used for8SK with the indicated Access Technology see 24.008 10.5.5.12a #-- @spec 34.123-3 Table B.1.17.2

px_AccessPointName,                          OCTETSTRING,   03696D73 #-- @desc  Access Point Name #-- @spec 

px_AnrForUtranMeasLogWaitTime,               INTEGER,       15      #-- @desc  Time required by UE to measure detect and log an ANR cell in idle mode CELL_PCH and URA_PCH. Value in seconds in the range of 1 to 60 seconds #-- @spec 34.123-3 Table B.1.20

px_AquireGNSS_MaxTime,                       INTEGER,       60      #-- @desc  The maximume time (in seconds) taken for the UE to acquire GNSS and derive UTC time (and normally position) and then start to transit or receive as appropriate #-- @spec 

px_AttachTypeTested,                         ENUM-EUTRA_ATTACH_TESTED_Type,COMBINED_ATTACH #-- @desc  Attach Type to be tested if UE supports both pc_Attach and pc_Combined_Attach #-- @spec 

px_AuthAMF,                                  BITSTRING,     1001000100010001 #-- @desc  Authentication Management Field (16 bits). The value shall be different from '1111 1111 1111 111'B (AMFresynch). #-- @spec 34.123-3, Table B.1

px_AuthK,                                    BITSTRING,     00000000000000010000001000000011000001000000010100000110000001110000100000001001000010100000101100001100000011010000111000001111 #-- @desc  Authentication Key #-- @spec 34.123-3, Table B.1

px_AuthN,                                    INTEGER,       127     #-- @desc  value of n to initialize tcv_AuthN (length of extended response) #-- @spec 34.123-3, B.1.1

px_BI_deviation,                             BOOLEAN,       false   #--  #-- @spec 

px_BI_deviation_dummy,                       INTEGER,       1       #--  #-- @spec 

px_BcapDataCompression,                      BITSTRING,     0       #-- @desc  Data compression supported (used in the Bearer Capability).Default value: Default IMSI #-- @spec 34.123-3, Table B.2

px_BcapFNUR,                                 BITSTRING,     00001   #-- @desc  Fixed Network User rate supported: '00001'B: FNUR 9.6 kbits '00010'B: FNUR 14.4 kbits '00011'B: FNUR 19.2 kbits '00100'B: FNUR 28.8 kbits '00101'B: FNUR 38.4 kbits '00110'B: FNUR 48.0 kbits '00111'B: FNUR 56.0 kbits '01000'B: FNUR 64.0 kbits '01001'B: FNUR 33.6 kbits '01010'B: FNUR 32.0 kbits. #-- @spec 34.123-3, Table B.2

px_CN_DomainTested,                          ENUM-CN_DomainIdentity,ps_domain #-- @desc  CN domain to be tested. This parameter is used in test cases that handle both PS and CS domains. #-- @spec 34.123-3 Table B.1.1

px_CipherAlg,                                BITSTRING,     010     #-- Anritsu ttCN CR required px_CipherAlg type @desc  NAS Ciphering Algorithm Default value: (GEA2) #-- @spec 

px_CipherKey,                                BITSTRING,     0101111001001010101100110101100010010001001101110101110100101010 #-- @desc   Cipher Key #-- @spec 51.010-5, Table B.1

px_CipherKey128,                             BITSTRING,     01011110010010101011001101011000100100010011011101011101001010100101111001001010101100110101100010010001001101110101110100101010 #-- @desc  Cipher key (128 bits) to be used e.g. for A54 and GEA4 #-- @spec 34.123-3, Table B.1.11

px_ColorCode,                                INTEGER,       64      #-- @desc  Color code of the subnet to which the sectors belong; Same for all HRPD cells #-- @spec 

px_ColorCodeDiff,                            INTEGER,       128     #-- @desc  Color code of the subnet to which the sectors belong; A different colour code than default #-- @spec 

px_D2D_SimulatedUE_Layer2Id,                 BITSTRING,     000100000000000000000000 #-- @desc  Simulated UE 1 layer 2 Id #-- @spec 

px_D2D_UE_Layer2Id,                          BITSTRING,     000100000000000000000000 #-- @desc  SideLink UE under test layer 2 Id #-- @spec 

px_DHCPServer_IPAddr,                        CHARSTRING,    10.122.11.24 #-- @desc  DHCP Server address #-- @spec 34.229-3

px_DL_MaxCCTrCH,                             INTEGER,       1       #-- @desc  Maximum number of Simultaneous CCTrCH for downlink #-- @spec 34.123-3 Table B.1.1

px_DL_MaxCC_TB_Bits,                         ENUM-MaxNoBits,b640    #-- @desc  Maximum sum of number of bits of all convolutionally coded transport blocks being received at an arbitrary time instant. #-- @spec 34.123-3 Table B.1.1

px_DL_MaxTB_Bits,                            ENUM-MaxNoBits,b6400   #-- @desc  Maximum sum of number of bits of all transport blocks being received at an arbitrary time instant #-- @spec 34.123-3 Table B.1.1

px_DL_MaxTC_TB_Bits,                         ENUM-MaxNoBits,b6400   #-- @desc  Maximum sum of number of bits of all turbo coded transport blocks being received at an arbitrary time instant. #-- @spec 34.123-3 Table B.1.5

px_DL_MaxTF,                                 ENUM-MaxNumberOfTF,tf64    #-- @desc  Maximum number of TF for downlink #-- @spec 34.123-3 Table B.1.1

px_DL_MaxTFS,                                ENUM-MaxNumberOfTFC_DL,tfc128  #-- @desc  Maximum number of TFC in the TFCS for downlink #-- @spec 34.123-3 Table B.1.1

px_DL_MaxTTI_TB,                             ENUM-MaxTransportBlocksDL,tb32    #-- @desc  Maximum total number of transport blocks received within TTIs that end within the same 10 ms interval. #-- @spec 34.123-3 Table B.1.1

px_DL_MaxTrCHs,                              ENUM-MaxSimultaneousTransChsDL,e8      #-- @desc  Maximum number of simultaneous transport channels for downlink #-- @spec 34.123-3 Table B.1.1

px_DNSServer_IPAddr,                         CHARSTRING,    10.122.11.23 #-- @desc  DNS Server address #-- @spec 34.229-3

px_DelayBeforeIntraCellHO,                   INTEGER,       300     #-- @desc  Temporary PIXIT used to define the delay before an intra cell handover #-- @spec 

px_DigestPasswordForSIP,                     CHARSTRING,    SIP-Password #-- @desc  SIP password #-- @spec 34.229-4

px_DigestPasswordForXCAP,                    CHARSTRING,    XCAP-Password #-- @desc  XCAP password #-- @spec 34.229-3

px_DoAttachWithoutPDN,                       BOOLEAN,       false   #-- @desc  UE is configured to do Attach without PDN if the value is FALSE it is assumed that the UE is configured to do Attach with PDN #-- @spec 

px_EDCH_UE_Category_FDD,                     INTEGER,       1       #-- @desc  Reference to other Spec: 34.123-2 Table A.18a.2 #-- @spec 34.123-2, Table A.18a.2

px_EDCH_UE_Category_TDD,                     INTEGER,       1       #-- @desc  Reference to other Spec: 34.123-2 Table A.18b.2 #-- @spec 34.123-2, Table A.18b.2

px_ENDC_BandCombination,                     ENUM-ENDC_BandCombination_Type,DC_25A_n41A #-- @desc  Band combination for EN-DC test cases #-- @spec 

px_ENDC_CA_BandCombination,                  ENUM-ENDC_CA_BandCombination_Type,DC_1A_n28A_n78A #-- @desc  EN-DC CA Band Combination #-- @spec 

px_ENDC_SecondaryBandCombination,            ENUM-ENDC_BandCombination_Type,DC_1A_n77A #-- @desc  Secondary band combination for EN-DC test cases #-- @spec 

px_ETWS_CB_DataPage1,                        CHARSTRING,    warning #-- @desc  ETWS Page 1 warning data message #-- @spec 

px_ETWS_CB_DataPage2,                        CHARSTRING,    warning #-- @desc  ETWS Page 2 warning data message #-- @spec 

px_ETWS_DigitalSignature,                    OCTETSTRING,   00000000000000000000000000000000000000000000000000000000000000000000000000000000000000 #-- @desc  ETWS Digital Signature #-- @spec 

px_EUTRA_CA_BandCombination,                 ENUM-CA_BandCombination_Type,CA_1C   #-- @desc  CA band combination applied in CA test cases #-- @spec 

px_EUTRA_DC_BandCombination,                 ENUM-DC_BandCombination_Type,DC_1A_3A #-- @desc  DC band combination applied in DC test cases #-- @spec 

px_EllipsoidPointWithAltitude,               OCTETSTRING,   1234560000000000 #-- @desc  Ellipsoid Point With Altitude value to be provided in Update UE location information (see 36.509 cl 6.12) #-- @spec 

px_EllipsoidPointWithAltitudeNotProSe,       OCTETSTRING,   1234560000000000 #-- @desc  Ellipsoid Point With Altitude value not corresponding to geographical area provided in EF PROSE RADIO COM to be provided in Update UE location information (see 36.509 cl 6.12) #-- @spec 

px_EllipsoidPointWithAltitudeProSe,          OCTETSTRING,   1234560000000000 #-- @desc  Ellipsoid Point With Altitude value corresponding to geographical area provided in EF PROSE RADIO COM to be provided in Update UE location information (see 36.509 cl 6.12) #-- @spec 

px_EllipsoidPointWithAltitude_NotProSe,      OCTETSTRING,   1234560000000000 #-- @desc  Ellipsoid Point With Altitude value not corresponding to geographical area provided in EFPROSE_RADIO_COM to be provided in Update UE location information (see 36.509 cl. 6.12) #-- @spec 

px_EllipsoidPointWithAltitude_ProSe_Area1,   OCTETSTRING,   1234560000000000 #-- @desc  Ellipsoid Point With Altitude value corresponding to geographical area 1 provided in EFPROSE_RADIO_COM to be provided in Update UE location information (see 36.509 cl. 6.12) #-- @spec 

px_EllipsoidPointWithAltitude_ProSe_Area2,   OCTETSTRING,   1234560000000000 #-- @desc  Ellipsoid Point With Altitude value corresponding to geographical area 2 provided in EFPROSE_RADIO_COM to be provided in Update UE location information (see 36.509 cl. 6.12) #-- @spec 

px_EmergencyCallNumber,                      CHARSTRING,    112     #-- @desc  Emergency Number used by UE to initiate an emergency call #-- @spec 34.123-3, Table B.1.2

px_EpsQosBitrateForVideo,                    INTEGER,       432     #-- @desc  Bitrate in kbps used by Reference Dedicated EPS Bearer#3 in 36.508 Table 6.6.2-1 #-- @spec 

px_FDD_OperationBand,                        INTEGER,       1       #-- @desc  The operation band under test as defined in 34.108 clause 5.1.1. Value 1 means Band 1 2 means Band 2 etc.This pixit shall be set in synchronisation with the values that are being set to 6 other Pixits viz: px_UARFCN_D_High px_UARFCN_D_Midpx_UARFCN_L_Mid #-- @spec 34.123-3, Table B.1

px_FRESH,                                    BITSTRING,     00001111000011110000111100001111 #-- @desc  no default value can be proposed #-- @spec 34.123-3, Table B.1

px_GERAN_BandUnderTest,                      ENUM-GERAN_BandUnderTestType,GSM_P900 #-- @desc  Indicates which band is under test.  The type is different to the parameter defined in 34.123-3 #-- @spec 

px_GPRS_CipheringAlgorithm,                  ENUM-GPRS_CipheringAlgorithm_Type,gea3    #-- @desc  NAS Ciphering Algorithm Default value: (GEA2) #-- @spec 34.123-3, Table B.1

px_GSM_CipherAlg,                            BITSTRING,     000     #-- @desc  GSM Cipher algorithm. #-- @spec 51.010-5, Table B.1

px_GSM_CipheringOnOff,                       BITSTRING,     1       #-- @desc  GSM Ciphering to be started or not #-- @spec 51.010-5, Table B.1

px_GeoInfo,                                  OCTETSTRING,   9032B9D66360B600323C3C006544 #-- @desc  Geographical information to be sent as Location Estimate in FACILITY message from the System Simulator. #-- @spec 37.571-4 Table B.1.13

px_GnssScenario2012,                         BOOLEAN,       false   #-- @desc  Usage of GNSS scenarios with date in 2012 from 3GPP TS 37.571-5 #-- @spec 37.571-4 Table 8.2-1

px_HRPD_BandClass,                           INTEGER,       1       #-- @desc  Band Class; Table 1.5-1 of C.S0057_D. Default value corresponds to 1.8 to 2.0 GHz PCS band #-- @spec 

px_HRPD_OpenLoopParametersCell15,            OCTETSTRING,   123456  #-- @desc  The HRPD Open Loop parameters for cell 15 message to be sent; it also includes the Tunneled Header as per C.S0087 clause 5.1.6.3 (default value needs updating FFS) #-- @spec 

px_HRPD_SectorID_Cell15,                     BITSTRING,     11111110101000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000001 #-- @desc  Sector ID of Cell 15; Clause 13.9 of C.S0024_B #-- @spec 

px_HRPD_SectorID_Cell16,                     BITSTRING,     11111110101000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000010 #-- @desc  Sector ID of Cell 16; Clause 13.9 of C.S0024_B #-- @spec 

px_HRPD_SectorID_Cell17,                     BITSTRING,     11111110101000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000011 #-- @desc  Sector ID of Cell 17; Clause 13.9 of C.S0024_B #-- @spec 

px_HRPD_SectorID_Cell18,                     BITSTRING,     11111110101000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000100 #-- @desc  Sector ID of Cell 18; Clause 13.9 of C.S0024_B #-- @spec 

px_HRPD_SilenceParametersCell15,             OCTETSTRING,   123456  #-- @desc  The HRPD Silence parameters for cell 15 message to be sent; it also includes the Tunneled Header as per C.S0087 clause 5.1.6.3 (default value needs updating FFS) #-- @spec 

px_HRPD_TrafficChannelAssignmentCell15,      OCTETSTRING,   123456  #--  #-- @spec 

px_HSDSCH_UE_Category_FDD,                   INTEGER,       5       #-- @desc  Reference to other Spec: 34.123-2 Table A.18a.1 #-- @spec 34.123-2, Table A.18a.1

px_HSDSCH_UE_Category_TDD,                   INTEGER,       5       #-- @desc  Reference to other Spec: 34.123-2 Table A.18b.1 #-- @spec 34.123-2, Table A.18b.1

px_HorizontalVelocity,                       OCTETSTRING,   123456  #-- @desc  Horizontal Velocity to be provided in Update UE location information (see 36.509 cl 6.12) #-- @spec 

px_IMEISV_Def,                               HEXSTRING,     123456789012345 #-- @desc  Default IMEISV value.  No default can be proposed as this is a manufacturer defined value #-- @spec 34.123-3, Table B.1

px_IMEI_Def,                                 HEXSTRING,     123456789012345 #-- @desc  Default IMEI value transmitted by UE.  According to TS 23.003 Annex B.1 the last digit is a Spare Digit to be set to '0' #-- @spec 34.123-3, Table B.1

px_IMSI_Def,                                 HEXSTRING,     001010000000333 #-- @desc  Default IMSI #-- @spec 34.123-3, Table B.1

px_IMSI_Diff,                                HEXSTRING,     001010654321063 #-- @desc  Different IMSI from the IMSI stored in the USIM #-- @spec 34.123-3, Table B.1

px_IMS_AssociatedTelUri,                     CHARSTRING,    tel:+4989364072 #-- @desc  Set as record 3 in EFIMPU as defined in TS 34.229-1[5] #-- @spec 34.229-3

px_IMS_CalleeContactUri,                     CHARSTRING,    sip:User-B-Contact@3gpp.org #-- @desc  URI provided by the remote side (i.e. by SS) to be used by the UE as contact address in further SIP signalling of the dialog #-- @spec 34.229-3

px_IMS_CalleeContactUri2,                    CHARSTRING,    sip:User-C-Contact@3gpp.org #-- @desc  URI provided by the remote side (i.e. by SS) to be used by the UE as contact address in further SIP signalling of the dialog #-- @spec 34.229-3

px_IMS_CalleeUri,                            CHARSTRING,    sip:1234@test.3gpp.com #-- @desc  URI of Callee sent by the UE in INVITE (MO call establishment) to address the remote UE #-- @spec 34.229-3

px_IMS_CalleeUri2,                           CHARSTRING,    sip:User-C@3gpp.org #-- @desc  URI of Callee sent by the UE in INVITE (MO call establishment) to address the remote UE #-- @spec 34.229-3

px_IMS_CiphAlgo_Def,                         ENUM-IPsec_CipheringAlgorithm_Type,des_ede3_cbc #-- @desc  Ciphering Algorithm #-- @spec 34.229-3

px_IMS_ConferenceFactoryUri,                 CHARSTRING,    sip:mmtel@conf-factory.3gpp.org #-- @desc  conference factory URI as used by the UE for IMS conferencing #-- @spec 

px_IMS_FinalConferenceUri,                   CHARSTRING,    sip:final@conf-factory.3gpp.org #-- @desc  final conference URI as sent to the UE during MTSI conference creation #-- @spec 

px_IMS_HomeDomainName,                       CHARSTRING,    test.3gpp.com #-- @desc  Home Domain Name. #-- @spec 34.229-3

px_IMS_HomeDomainName_Refreshed,             CHARSTRING,    refreshed3gpp.org #-- @desc  Used in 8.15 #-- @spec 

px_IMS_IPSecAlgorithm,                       ENUM-IPsec_IntegrityAlgorithm_Type,hmac_md5_96 #-- @desc  Integrity Algorithm #-- @spec 34.229-3

px_IMS_MessageAccountIdentity,               CHARSTRING,    testaccountidentity #-- @desc  message accout identity configured at the UE as used for subscription to message-summary event package #-- @spec 

px_IMS_Pcscf,                                CHARSTRING,    pcscf.3gpp.org #-- @desc  P-CSCF fully qualified domain name that resolves to the IP address of SS #-- @spec 34.229-3

px_IMS_Pcscf_Emg,                            CHARSTRING,    pcscfemg.3gpp.org #-- @desc  P-CSCF fully qualified domain name that resolves to the IP address of SS for emergency calls #-- @spec 34.229-3

px_IMS_Private_UserId,                       CHARSTRING,    001010123456789@test.3gpp.com #-- @desc  Private User Identity.When usingan ISIM this is set to the same value as EFIMPI.When ISIM is not used just USIM the private user identity is derived from px_IMSI. #-- @spec 34.229-3

px_IMS_Private_UserId_Refreshed,             CHARSTRING,    privateuser@refreshed3gpp.org #-- @desc  Used in 8.15 #-- @spec 

px_IMS_PublicUserIdentity1,                  CHARSTRING,    sip:001010123456789@ims.mnc001.mcc001.3gppnetwork.org #-- @desc  Public User Identity. It is set to the same value as the first record in EFIMPU. #-- @spec 34.229-3

px_IMS_PublicUserIdentity1_Refreshed,        CHARSTRING,    sip:PublicId1@refreshed3gpp.org #-- @desc  Used in 8.15 #-- @spec 

px_IMS_PublicUserIdentity2,                  CHARSTRING,    sip:+11234567890@test.3gpp.com #-- @desc  Public User Identity. It is set to the same value as the second record in EFIMPU. #-- @spec 34.229-3

px_IMS_PublicUserIdentity3,                  CHARSTRING,    sip:user@test.3gpp.com #-- @desc  Public User Identity. It is set to the same value as the third record in EFIMPU. #-- @spec 34.229-3

px_IMS_SPI_MinimumValue,                     INTEGER,       256     #-- @desc  lowest value for the SPI value #-- @spec 34.229-3

px_IMS_SPI_ValidValueList_PDN1,              CHARSTRING,    256,258,264,266 #-- @desc  list of comma separated integer values that can be used as SPI values for IMS security on PDN1; each value shall be greater than or equal to 256 #-- @spec 34.229-3

px_IMS_SPI_ValidValueList_PDN2,              CHARSTRING,    260,262,268,270 #-- @desc  list of comma separated integer values that can be used as SPI values for IMS security on PDN2; each value shall be greater than or equal to 256 #-- @spec 34.229-3

px_IMS_Scscf,                                CHARSTRING,    scscf.3gpp.org #-- @desc  S-CSCF fully qualified domain name that resolves to the IP address of SS #-- @spec 34.229-3

px_IMS_TemporaryConferenceUri,               CHARSTRING,    sip:temporary@conf-factory.3gpp.org #-- @desc  temporary conference URI as sent to the UE during MTSI conference creation #-- @spec 

px_IMS_ePcscf,                               CHARSTRING,    epcscf.3gpp.org #-- @desc  P-CSCF fully qualified domain name that resolves to the IP address of SS for emergency calls #-- @spec 

px_IP_MTU_Size,                              INTEGER,       1300    #-- @desc  MTU size. This value is specific to the SS. #-- @spec 

px_IPv4_Address,                             CHARSTRING,    192.168.0.1 #-- @desc  IPv4 Address #-- @spec 

px_IPv4_Address1_NW,                         CHARSTRING,    192.168.0.3 #-- @desc  IPv4 Gateway Address in PDN1 #-- @spec 

px_IPv4_Address1_RemoteUE,                   CHARSTRING,    192.168.0.6 #-- @desc  IPv4 Address of remote UE connected to PDN1 #-- @spec 

px_IPv4_Address1_UE,                         CHARSTRING,    192.168.0.1 #-- @desc  IPv4 Address connected to PDN1 #-- @spec 

px_IPv4_Address2,                            CHARSTRING,    192.168.1.2 #-- @desc  2nd IPv4 Address @sic R5s110011 sic@ #-- @spec 

px_IPv4_Address2_NW,                         CHARSTRING,    192.168.1.4 #-- @desc  IPv4 Gateway Address in PDN2 #-- @spec 

px_IPv4_Address2_RemoteUE,                   CHARSTRING,    192.168.1.6 #-- @desc  IPv4 Address of remote UE connected to PDN2 #-- @spec 

px_IPv4_Address2_UE,                         CHARSTRING,    192.168.1.2 #-- @desc  IPv4 Address connected to PDN2 #-- @spec 

px_IPv4_Address2a_UE,                        CHARSTRING,    192.168.1.3 #-- @desc  IPv4 Address connected to PDN2a #-- @spec 

px_IPv4_Address3_NW,                         CHARSTRING,            #-- @desc  IPv4 Gateway Address in PDN3 #-- @spec 

px_IPv4_Address3_RemoteUE,                   CHARSTRING,            #-- @desc  IPv4 Address of remote UE connected to PDN3 #-- @spec 

px_IPv4_Address3_UE,                         CHARSTRING,            #-- @desc  IPv4 Address connected to PDN3 #-- @spec 

px_IPv4_Address4_NW,                         CHARSTRING,            #-- @desc  IPv4 Gateway Address in PDN4 #-- @spec 

px_IPv4_Address4_UE,                         CHARSTRING,            #-- @desc  IPv4 Address connected to PDN4 #-- @spec 

px_IPv4_Address5_NW,                         CHARSTRING,            #-- @desc  IPv4 Gateway Address in PDN5 #-- @spec 

px_IPv4_Address5_UE,                         CHARSTRING,            #-- @desc  IPv4 Address connected to PDN5 #-- @spec 

px_IPv4_Address6_NW,                         CHARSTRING,            #-- @desc  IPv4 Gateway Address in PDN6 #-- @spec 

px_IPv4_Address6_UE,                         CHARSTRING,            #-- @desc  IPv4 Address connected to PDN6 #-- @spec 

px_IPv4_Address_BSF,                         CHARSTRING,            #-- @desc  IPv4 BSF address #-- @spec 

px_IPv4_Address_HomeAgent,                   CHARSTRING,    192.168.0.5 #-- @desc  IPv4 Home Address Agent #-- @spec 

px_IPv4_Address_Other,                       CHARSTRING,            #-- @desc  Other IPv4 Address #-- @spec 

px_IPv4viaNAS_TestMode,                      BOOLEAN,       false   #-- @desc  This parameter can be set to TRUE so as to force allocation of IPv4 only PDN connection and IP address allocation via NAS signalling in the preamble of test cases using test mode (see TS 36.508 [3] clause 4.5.2A). #-- @spec 

px_IPv6_Address,                             CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:1111 #-- @desc  IPv6 Address #-- @spec 

px_IPv6_Address1_NW,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:3333 #-- @desc  IPv6 Gateway Address in PDN1 #-- @spec 

px_IPv6_Address1_RemoteUE,                   CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:6666 #-- @desc  IPv6 Address of remote UE in PDN1 #-- @spec 

px_IPv6_Address1_UE,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:1111 #-- @desc  IPv6 Address in PDN1 #-- @spec 

px_IPv6_Address2,                            CHARSTRING,    1111:2222:3333:5555:5555:6666:7777:2222 #-- @desc  2nd IPv6 Address  @sic R5s110011 sic@ #-- @spec 

px_IPv6_Address2_NW,                         CHARSTRING,    1111:2222:3333:5555:5555:6666:7777:4444 #-- @desc  IPv6 Gateway Address in PDN2 #-- @spec 

px_IPv6_Address2_RemoteUE,                   CHARSTRING,    1111:2222:3333:5555:5555:6666:7777:6666 #-- @desc  IPv6 Address of remote UE in PDN2 #-- @spec 

px_IPv6_Address2_UE,                         CHARSTRING,    1111:2222:3333:5555:5555:6666:7777:2222 #-- @desc  IPv6 Address in PDN2 #-- @spec 

px_IPv6_Address2a_UE,                        CHARSTRING,    1111:2222:3333:5555:5555:6666:7777:5555 #-- @desc  IPv6 Address in PDN2a #-- @spec 

px_IPv6_Address3_NW,                         CHARSTRING,            #-- @desc  IPv6 Gateway Address in PDN3 #-- @spec 

px_IPv6_Address3_RemoteUE,                   CHARSTRING,            #-- @desc  IPv6 Address of remote UE in PDN3 #-- @spec 

px_IPv6_Address3_UE,                         CHARSTRING,            #-- @desc  IPv6 Address in PDN3 #-- @spec 

px_IPv6_Address4_NW,                         CHARSTRING,            #-- @desc  IPv6 Gateway Address in PDN4 #-- @spec 

px_IPv6_Address4_UE,                         CHARSTRING,            #-- @desc  IPv6 Address in PDN4 #-- @spec 

px_IPv6_Address5_NW,                         CHARSTRING,            #-- @desc  IPv6 Gateway Address in PDN5 #-- @spec 

px_IPv6_Address5_UE,                         CHARSTRING,            #-- @desc  IPv6 Address in PDN5 #-- @spec 

px_IPv6_Address6_NW,                         CHARSTRING,            #-- @desc  IPv6 Gateway Address in PDN6 #-- @spec 

px_IPv6_Address6_UE,                         CHARSTRING,            #-- @desc  IPv6 Address in PDN6 #-- @spec 

px_IPv6_Address_BSF,                         CHARSTRING,    1111:2222:3333:4444:5555:6666:7777:3333 #-- @desc  IPv6 BSF address #-- @spec 

px_IPv6_Address_HomeAgent,                   CHARSTRING,    1111:2222:3333:5555:5555:6666:7777:5555 #-- @desc  IPv6 Home Address Agent #-- @spec 

px_IPv6_Address_Other,                       CHARSTRING,            #-- @desc  Other IPv6 Address #-- @spec 

px_LcsClientAddressDigits,                   CHARSTRING,    0123456 #-- @desc  LCS Client external address Digits #-- @spec 37.571-4 Table B.1.13

px_LcsClientAddressNPI,                      BITSTRING,     0001    #-- @desc  LCS Client external address NPI #-- @spec 37.571-4 Table B.1.13

px_LcsClientAddressTOA,                      BITSTRING,     1001    #-- @desc  LCS Client external address TOA #-- @spec 37.571-4 Table B.1.13

px_LcsClientName,                            CHARSTRING,    OPERATOR #-- @desc  LCS Client name #-- @spec 37.571-4 Table B.1.13

px_MACIndex,                                 INTEGER,       15      #-- @desc  Reverse link MAC index to be used. C.S0024 clause 12.4.1.3.2.2.  Supported values 0..383 #-- @spec 

px_MFBI_BandChannelBandwidth,                ENUM-Dl_Bandwidth_Type,n25     #-- @desc  MFBI E-UTRAN Channel Bandwidth #-- @spec 

px_MFBI_FrequencyBand,                       INTEGER,       26      #-- @desc  a supported E-UTRA MFBI frequency band #-- @spec 

px_MFBI_UTRAN_FrequencyBand,                 INTEGER,       26      #-- @desc  A supported UTRAN MFBI frequency band. #-- @spec 34.123-3, Table B.1.20

px_MS_ClsmkESIND,                            BITSTRING,     0       #-- @desc  Default Early Sending Indication #-- @spec 34.123-3, Table B.1

px_MS_ClsmkRevLvl,                           BITSTRING,     10      #-- @desc  Default Revision Level #-- @spec 34.123-3, Table B.1

px_MS_TXPWR_MAX_CCH,                         BITSTRING,     01010   #-- @desc  MS_TXPWR_MAX_CCH #-- @spec 51.010-5, Table B.1

px_MaxAM_EntityNumberRLC_Cap,                ENUM-MaximumAM_EntityNumberRLC_Cap,am8     #-- @desc  Maximum AM Entity Number for RLC. #-- @spec 34.123-3 Table B.1.1

px_MaxHcContextSpace,                        ENUM-MaxHcContextSpace,by8192  #-- @desc  MaxHcContextSpace if RFC 2507 is supported. #-- @spec 34.123-3 Table B.1.5

px_MaxNoDPCH_PDSCH_Codes,                    INTEGER,       3       #-- @desc  Part of DL_PhysChCapabilityFDD. INTEGER (1..8 ). #-- @spec 34.123-3 Table B.1.1

px_MaxNoDPDCH_BitsTransmitted,               ENUM-MaxNoDPDCH_BitsTransmitted,b9600   #-- @desc  Part of UL_PhysChCapabilityFDD. #-- @spec 34.123-3 Table B.1.1

px_MaxNoPhysChBitsReceived,                  ENUM-MaxNoPhysChBitsReceived,b19200  #-- @desc  Part of DL_PhysChCapabilityFDD. #-- @spec 34.123-3 Table B.1.1

px_MaxNumberROHC_ContextSessions,            ENUM-MaxNumberROHC_ContextSessions_Type,cs16    #-- @desc  Maximum number of ROHC context sessions #-- @spec 

px_MaxRLC_WindowSize,                        ENUM-MaximumRLC_WindowSize,mws2047 #-- @desc  Maximum RLC window size. #-- @spec 34.123-3 Table B.1.1

px_MobileDataOn,                             BOOLEAN,       true    #-- @desc  Specifies whether mobile data associated with Internet PDN is enabled on the DUT #-- @spec 

px_ModifyBearerResources,                    BOOLEAN,       false   #-- @desc  NB-IoT UE configured to handle modification of bearer resources including dedicated bearers (PDN of type "IP") #-- @spec 

px_NAS_CipheringAlgorithm,                   BITSTRING,     001     #-- @desc  NAS Ciphering Algorithm (eea1) #-- @spec 

px_NAS_IntegrityProtAlgorithm,               BITSTRING,     001     #-- @desc  NAS Integrity Algorithm (eia1) #-- @spec 

px_NB_OperationMode,                         ENUM-NB_OperationMode_Type,standalone #-- @desc  NB-IoT Operation Mode #-- @spec 

px_NEDC_BandCombination,                     ENUM-NEDC_BandCombination_Type,DC_n28A_3A #-- @desc  NE-DC Band Combination #-- @spec 

px_NR_DC_CA_BandCombination,                 ENUM-NR_DC_CA_BandCombination_Type,DC_n78A_n257G #-- @desc  NR DC CA Band Combination #-- @spec 

px_NR_PrimaryBand,                           INTEGER,       1       #-- @desc  NR primary band #-- @spec 

px_NS_Value,                                 INTEGER,       1       #-- @desc  Network Signalling value as defined in TS 36.101 [34] clause 6.2.4F and used in TS 36.508 [3] clause 8.1.3.1 to select the NB-IoT frequencies #-- @spec 

px_NTN_ScenarioUnderTest,                    ENUM-NTN_ScenarioUnderTest,GSO     #-- @desc  NTN satellite scenario under test if UE supports NTN. #-- @spec 

px_NoTDD_LCR_onLTE,                          BOOLEAN,       false   #-- @desc  Only applicable to UE supporting (at least) LTE and LCR TDD.  If set to true the UE is configured not to report support of LCR TDD (IE utraTDD128 in UECapabilityInformation) when being camped on an LTE cell with no detectable LCR TDD cell in the environment. #-- @spec 

px_OpenLoopAdjust,                           INTEGER,       10      #-- @desc  The value of open loop adjust to be used by access terminals in the open loop power estimate expressed as an unsigned value in units of 1 dB. The value  used by the access terminal is -1 times the value of this field #-- @spec 

px_OverlappingNotSupportedFrequencyBand_MFBI,INTEGER,       27      #-- @desc  a not supported E-UTRA frequency band that is overlapping with a supported MFBI band #-- @spec 

px_OverlappingSupportedFrequencyBand_MFBI,   INTEGER,       26      #-- @desc  a not supported E-UTRA frequency band that is overlapping with a supported MFBI band #-- @spec 

px_PSI_SMSC,                                 CHARSTRING,    sip:psi_smsc@3gpp.org #-- @desc  The public service identity of the SMSC set to the same value as the first record in EFPSISMSC #-- @spec 

px_PTMSI_Def,                                OCTETSTRING,   C2345678 #-- @desc  Default PTMSI #-- @spec 34.123-3, Table B.1

px_PTMSI_SigDef,                             OCTETSTRING,   AB1234  #-- @desc  Default PTMSI signature (3 octets 3GPP 24.008   10.5.5.8). #-- @spec 34.123-3, Table B.1

px_PWS_CB_DataCodingScheme,                  BITSTRING,     1010    #-- @desc  CMAS or ETWS data coding scheme of the alphabetcodingand the applied language (see TS 23.401) #-- @spec 

px_PWS_CB_DataPage1,                         CHARSTRING,    warning #-- @desc  ETWS or CMAS Page 1 warning data message #-- @spec 

px_PWS_CB_DataPage2,                         CHARSTRING,    warning #-- @desc  ETWS or CMAS Page 2 warning data message #-- @spec 

px_PWS_CB_DataPage3,                         CHARSTRING,    warning #-- @desc  CMAS or ETWS Page 3 warning data message #-- @spec 

px_PWS_CB_DataPage4,                         CHARSTRING,    warning #-- @desc  CMAS or ETWS Page 4 warning data message #-- @spec 

px_P_CSCF_IPAddr,                            CHARSTRING,    10.122.11.22 #-- @desc  P-CSCF address #-- @spec 34.229-3

px_PeerUE_IPAddr,                            CHARSTRING,    10.122.11.25 #-- @desc  Peer UE address #-- @spec 34.229-3

px_PowerDownRegEnabled,                      BOOLEAN,       true    #-- @desc  Parameter for power down req in 1xRTT #-- @spec 

px_PowerLevel,                               BITSTRING,     00000   #-- @desc  power level value for L1 header #-- @spec 51.010-5, Table B.1

px_PriScrmCode,                              INTEGER,       100     #-- @desc  Primary scrambling code. #-- @spec 34.123-3 Table B.1.1

px_ProSeAnnApplicationIdentity1,             CHARSTRING,    mcc345.mnc012.ProSeApp.Food.Restaurants.Italian #-- @desc  A ProSe Application ID with which data structure the UE is preconfigured and for which the UE can request and perform Direct Discovery Announcing.  TS23.003 section 24.2 #-- @spec 

px_ProSeMonApplicationIdentity1,             CHARSTRING,    mcc300.mnc165.ProSeApp.*.Sports.Surfing #-- @desc  A ProSe Application ID with which data structure the UE is preconfigured and for which the UE can request and perform Direct Discovery Monitoring  TS23.003 section 24.2 #-- @spec 

px_ProSeMonApplicationIdentityNot1,          CHARSTRING,    mcc208.mnc*.ProSeApp.*.Shops.Food.Wine #-- @desc  A ProSe Application ID with which data structure the UE is NOT preconfigured to request and perform Direct Discovery Monitoring  TS23.003 section 24.2 #-- @spec 

px_ProSe_TLS_CipherSuite,                    ENUM-TLS_CIPHER_Type,TLS_PSK_WITH_3DES_EDE_CBC_SHA #-- @desc  TLS cipher suite to be used for ProSe communication #-- @spec 

px_RAND,                                     BITSTRING,     00001111000011110000111100001111 #-- @desc  Random challenge data to be included along with mobility parameters in CSFBParametersResponseCDMA2000 or HandoverFromEUTRAPreparationRequest #-- @spec 

px_RAND2,                                    BITSTRING,     00001111000011110000111100001111 #-- @desc  Random challenge data to be included along with mobility parameters in CSFBParametersResponseCDMA2000 or HandoverFromEUTRAPreparationRequest #-- @spec 

px_RAND_Cell19,                              BITSTRING,     00001111000011110000111100001111 #--  #-- @spec 

px_RAND_Cell21,                              BITSTRING,     00001111000011110000111100001111 #--  #-- @spec 

px_RANTech,                                  ENUM-RANTech,  EUTRA_FDD #-- @desc  Technology to be used #-- @spec 34.229-3

px_RATComb_Tested,                           ENUM-RATComb_Tested_Type,EUTRA_UTRA #-- @desc  This parameter represents the network RAT capabilitypreference and indicates which if any is supported RAT combination is to be tested #-- @spec 

px_RRC_CipheringAlgorithm,                   ENUM-CipheringAlgorithm_Type,eea1    #-- @desc  Ciphering Algorithm #-- @spec 

px_RRC_CipheringAlgorithm_r12,               ENUM-CipheringAlgorithm_r12,eea1    #-- @desc  Ciphering Algorithm  Anritsu TTCN WA for px_RRC_CipheringAlgorithm backward compatibility #-- @spec 

px_RRC_IntegrityProtAlgorithm,               ENUM-IntegrityProtAlgorithm_Type,eia1    #-- @desc  Integrity Algorithm #-- @spec 

px_RRC_PS_ServTested,                        ENUM-RRC_ServTested,ps_Interactive #-- @desc  PS Service to be tested #-- @spec 34.123-3, Table B.1

px_RXLEV_ACCESS_MIN,                         BITSTRING,     000000  #-- @desc   minimum received signal level at MS #-- @spec 51.010-5, Table B.1

px_Release,                                  ENUM-AccessStratumRelease,rel8    #-- @desc  Release the UE supports #-- @spec 

px_Release_check_in_eMBMS_TCs,               BOOLEAN,       true    #-- Anritsu TTCN WA for release check in MBMS #-- @spec 

px_ReportUTRA_RAT,                           ENUM-ReportUTRA_RAT_Type,both    #-- @desc  Specifies which UTRA RATs a UE reports on #-- @spec 

px_ResetStoredInfo,                          BOOLEAN,       false   #-- @desc  Support of RESETUEPOSITIONINGSTOREDINFORMATION command as defined in 3GPP TS 34.109 cl. 6.10 #-- @spec 34.109 cl. 6.10

px_SL_AdditionalSupportedBandwidth,          ENUM-Ul_Bandwidth_Type,n25     #-- @desc  Supported sidelink bandwidth different from px_ePrimaryBandChannelBandwidth #-- @spec 

px_SMSTransport_CP_CIoT,                     BOOLEAN,       false   #-- @desc  NB-IoT UE configured to utilise the SMS service as transport mechanism for user data for Control Plane CIoT Optimisation #-- @spec 

px_SMS_ChkMsgReceived,                       BOOLEAN,       true    #-- @desc  Whether the operator can check an MT Short Message received #-- @spec 

px_SMS_IndexOffset,                          INTEGER,       0       #-- @desc  Memory location index at UE for SMS storage used in +CMSS command #-- @spec 34.123-3, Table B.1.2

px_SMS_MsgFrmt,                              CHARSTRING,    1       #-- @desc  SMS message format <mode> (see TS 27.005 cl.3.2.). NOTE: Default value is for text mode. Change value to 0 to execute tests with PDU mode #-- @spec 

px_SMS_PrefMem1,                             CHARSTRING,    SM      #-- @desc  SMS Preferred Memory 1 <mem1> of TS 27.005 [31] clause 3.2.2 #-- @spec 34.123-3, Table B.1.2

px_SMS_PrefMem2,                             CHARSTRING,    SM      #-- @desc  SMS Preferred Memory 2 <mem2> of TS 27.005 [31] clause 3.2.2 #-- @spec 34.123-3, Table B.1.2

px_SMS_PrefMem3,                             CHARSTRING,    MT      #-- @desc  SMS Preferred Memory 3 <mem3> of TS 27.005 [31] clause 3.2.2 #-- @spec 34.123-3, Table B.1.2

px_SMS_SMSC_InternationalNumber,             CHARSTRING,    112233445566778 #-- @desc  international number of the SMSC: #-- @spec 34.229-3

px_SMS_Service,                              CHARSTRING,    0       #-- @desc  SMS Service <service> of TS 27.005 [31] clause 3.2.1 #-- @spec 34.123-3, Table B.1.2

px_SPI_pc,                                   INTEGER,       5000    #-- Anritsu TTCN WA for SPI #-- @spec 

px_SPI_ps,                                   INTEGER,       1000    #-- Anritsu TTCN WA for SPI #-- @spec 

px_SRNC_Id,                                  BITSTRING,     000000000001 #-- @desc  SRNC Id #-- @spec 34.123-3, Table B.1

px_SRNTI,                                    BITSTRING,     00000000000000000001 #-- @desc  S RNTI #-- @spec 34.123-3, Table B.1

px_SVN_Def,                                  HEXSTRING,     00      #-- Anritsu TTCN-CR required (ProseCR R5-131832) #-- @spec 

px_SinglePLMN_Tested,                        ENUM-SinglePLMN_TestedType,MultiPLMN #-- @desc  This parameter represents the network capabilitypreference to support multi PLMNs on the same test Band and indicates the preference of multi PLMNs or single PLMN test environment. This PIXIT shall be set to SinglePLMN when only one frequency is defined for the test band #-- @spec 

px_SplitOnCCCH,                              BITSTRING,     0       #-- @desc  Split pg cycle on CCCH supported indication #-- @spec 51.010-5, Table B.1

px_StartStop,                                BOOLEAN,       TRUE    #-- Anritsu TTCN WA for Automation EnableDisable #-- @spec 

px_StartString,                              CHARSTRING,    StartTest: #-- Anritsu TTCN WA for Automation Starting test cases string e.g.: StartTest:TC_7_1_2_1 #-- @spec 

px_StopString,                               CHARSTRING,    EndTest: #-- Anritsu TTCN WA for Automation Stopping test cases string e.g.: StopTest:Passed #-- @spec 

px_TCellA,                                   INTEGER,       256     #-- @desc  TCell value for cell A or 1. Except for the first created cell the value 0 applied in ts_SS_CellCfg. #-- @spec 34.123-3 Table B.1.1

px_TCellB,                                   INTEGER,       512     #-- @desc  TCell value for cell B or 2. Except for the first created cell the value 0 applied in ts_SS_CellCfg. #-- @spec 34.123-3 Table B.1.1

px_TCellC,                                   INTEGER,       1536    #-- @desc  TCell value for cell C or 3. Except  the  first created cell the value 0 applied in ts_SS_CellCfg. #-- @spec 34.123-3 Table B.1.1

px_TCellD,                                   INTEGER,       321     #-- @desc  TCell value for cell D or 4. Except the first created cell the value 0 applied in ts_SS_CellCfg. #-- @spec 34.123-3 Table B.1.1

px_TCellE,                                   INTEGER,       833     #-- @desc  TCell value for cell E or 5. Except the  first created cell the value 0 applied in ts_SS_CellCfg. #-- @spec 34.123-3 Table B.1.1

px_TCellF,                                   INTEGER,       6577    #-- @desc  TCell value for cell F or 6. Except the first created cell the value 0 applied in ts_SS_CellCfg. #-- @spec 34.123-3 Table B.1.1

px_TCellG,                                   INTEGER,       7253    #-- @desc  TCell value for cell G or 7. Except the first created cell the value 0 applied in ts_SS_CellCfg. #-- @spec 34.123-3 Table B.1.1

px_TCellH,                                   INTEGER,       4351    #-- @desc  TCell value for cell H or 8. Except the first created cell the value 0 applied in ts_SS_CellCfg. #-- @spec 34.123-3 Table B.1.1

px_TDD_OperationBand,                        CHARSTRING,    33      #-- @desc  LCR TDD Operation Band #-- @spec 

px_TDD_OperationBandCharstring,              CHARSTRING,    a       #-- @desc  Applicable for TDD. The operation band under test as defined in 34.108 clause 5.1.2 #-- @spec 

px_TDD_Sync_cells,                           BOOLEAN,       true    #-- @desc  Used for configuring synchronous TDD cells             Anrisu TTCN CR for TDD Tcell #-- @spec 

px_TMSI_Def,                                 OCTETSTRING,   11223344 #-- @desc  Default TMSI #-- @spec 34.123-3, Table B.1

px_TSC,                                      BITSTRING,     011     #-- @desc  Training sequence code for traffic channels. #-- @spec 51.010-5, Table B.1

px_TestLoopModeB_Delay,                      OCTETSTRING,   5A      #-- @desc  This parameter represents the IP PDU delay to be used for UE test loop mode B intest cases where long delay may be needed e.g. because of user interaction. #-- @spec 

px_TimingAdvance,                            BITSTRING,     0000000 #-- @desc  Timing advance value for L1 header #-- @spec 51.010-5, Table B.1

px_TotalRLC_AM_BufferSize,                   ENUM-TotalRLC_AM_BufferSize,kb500   #-- @desc  Total RLC AM buffer size for R99. The values are according to TotalRLC-AM-BufferSize defined in 3GPP TS 25.331 #-- @spec 34.123-3 Table B.1.1

px_UARFCN_D_High,                            INTEGER,       10837   #-- @desc  High Range downlink UARFCN value #-- @spec 34.123-3, Table B.1

px_UARFCN_D_Low,                             INTEGER,       10563   #-- @desc  Low Range downlink UARFCN value #-- @spec 34.123-3, Table B.1

px_UARFCN_D_Mid,                             INTEGER,       10700   #-- @desc  Mid Range downlink UARFCN value #-- @spec 34.123-3, Table B.1

px_UARFCN_High,                              INTEGER,       9596    #-- @desc  High Range UARFCN value for LCR TDD #-- @spec 

px_UARFCN_High_TDD,                          INTEGER,       9596    #-- @desc  High Range downlink UARFCN value for LCR TDD #-- @spec 

px_UARFCN_Low,                               INTEGER,       9504    #-- @desc  Low Range UARFCN value for LCR TDD #-- @spec 

px_UARFCN_Low_TDD,                           INTEGER,       9504    #-- @desc  Low Range downlink UARFCN value for LCR TDD #-- @spec 

px_UARFCN_Mid,                               INTEGER,       9550    #-- @desc  Mid Range UARFCN value for LCR TDD #-- @spec 

px_UARFCN_Mid_TDD,                           INTEGER,       9550    #-- @desc  Mid Range downlink UARFCN value for LCR TDD #-- @spec 

px_UARFCN_TDD_D_High,                        INTEGER,       10837   #-- @desc  High Range downlink UARFCN value for LCR TDD #-- @spec 

px_UARFCN_TDD_D_Low,                         INTEGER,       10563   #-- @desc  Low Range downlink UARFCN value for LCR TDD #-- @spec 

px_UARFCN_TDD_D_Mid,                         INTEGER,       10700   #-- @desc  Mid Range downlink UARFCN value for LCR TDD #-- @spec 

px_UATI24,                                   OCTETSTRING,   123456  #-- @desc  UATI to be allocated to the UE.  C.S0024 clause 6.3.7.2.2 #-- @spec 

px_UE_CS_PS_UsageSetting_Tested,             ENUM-CS_PS_MODE,VOICE_CENTRIC #-- @desc  specifies which CSPS mode is under test @sic R5s120274 sic@ #-- @spec 

px_UE_IPAddr,                                CHARSTRING,    10.122.11.21 #-- @desc  IP address assigned to UE (in v4 or v6 format) #-- @spec 34.229-3

px_UE_IPAddr2,                               CHARSTRING,    10.122.11.31 #-- @desc  2nd IP address assigned to UE (in v4 or v6 format) #-- @spec 34.229-3

px_UE_OpModeDef,                             ENUM-UE_OperationMode,opModeA #-- @desc  Default UE operation mode (either opModeA or opModeC). (For most Ues this corresponds class-A or class-C and can not be changed by the user). #-- @spec 34.123-3 Table B.1.1

px_UE_PS_UsageSetting_Tested,                ENUM-PS_MODE,  VOICE_CENTRIC #-- @desc  specifies which PS mode is under test @sic R5s120274 sic@ #-- @spec 

px_UE_PositioningNetworkAssistedGPS_Sup,     ENUM-NetworkAssistedGPS_Supported,noNetworkAssistedGPS #-- @desc  UE positioning capability: supports the network assisted GPS. #-- @spec 34.123-3 Table B.1.1

px_UE_Release,                               INTEGER,       8       #-- @desc  Required for 34.229 model only #-- @spec 

px_UE_UsageSetting_Tested,                   ENUM-CS_PS_MODE,VOICE_CENTRIC #-- @desc  specifies which CS/PS mode is under test #-- @spec 

px_UEwithISIM,                               BOOLEAN,       true    #-- @desc  true - UE has ISIM; false - UE has USIM only #-- @spec 34.229-3

px_UEwithSIM,                                BOOLEAN,       true    #-- @desc  UE has a SIM inserted #-- @spec 34.229-3

px_UL_MaxCC_TB_Bits,                         ENUM-MaxNoBits,b640    #-- @desc  Maximum sum of number of bits of all convolutionally coded transport blocks being transmitted at an arbitrary time instant. #-- @spec 34.123-3 Table B.1.1

px_UL_MaxTB_Bits,                            ENUM-MaxNoBits,b6400   #-- @desc  Maximum sum of number of bits of all transport blocks being transmitted at an arbitrary time instant. #-- @spec 34.123-3 Table B.1.1

px_UL_MaxTC_TB_Bits,                         ENUM-MaxNoBits,b6400   #-- @desc  Maximum sum of number of bits of all turbo coded transport blocks being transmitted at an arbitrary time instant. #-- @spec 34.123-3 Table B.1.5

px_UL_MaxTF,                                 ENUM-MaxNumberOfTF,tf32    #-- @desc  Maximum number of TF for uplink. #-- @spec 34.123-3 Table B.1.1

px_UL_MaxTFS,                                ENUM-MaxNumberOfTFC_UL,tfc64   #-- @desc  Maximum number of TFC in the TFCS for uplink. #-- @spec 34.123-3 Table B.1.1

px_UL_MaxTTI_TB,                             ENUM-MaxTransportBlocksUL,tb16    #-- @desc  Maximum total number of transport blocks transmitted within TTIs that start at the same time. #-- @spec 34.123-3 Table B.1.1

px_UL_MaxTrCHs,                              ENUM-MaxSimultaneousTransChsUL,e8      #-- @desc  Maximum number of simultaneous transport channels for uplink. #-- @spec 34.123-3 Table B.1.1

px_UL_ScramblingCode,                        INTEGER,       0       #-- @desc  UL scrambling code value to be used by UE. #-- @spec 34.123-3 Table B.1.1

px_UTRAN_CipheringAlgorithm,                 ENUM-CipheringAlgorithm_r7,uea1    #-- @desc  UTRAN Ciphering algorithm #-- @spec 

px_UTRAN_ModeUnderTest,                      ENUM-UTRAN_FDD_TDD_Type,UTRAN_FDD #-- @desc  specifies which radio access technology is being tested in UTRAN #-- @spec 

px_UTRAN_OverlappingNotSupportedFrequencyBandMFBI,INTEGER,       27      #-- @desc  A not supported UTRAN frequency band that is overlapping with a supported MFBI band (px_MFBI_UTRAN_FrequencyBand). This pixit shall be set also in accordance with the values of the 3 Pixits: px_UARFCN_D_High px_UARFCN_D_Midpx_UARFCN_L_Mid. #-- @spec 

px_UeLcsNotification,                        INTEGER,       20      #-- @desc  Value for UE LCS Notification timeout timer (in seconds) #-- @spec 37.571-4 Table B.1.13

px_WLANBand,                                 ENUM-WLAN_Band_Type,Band2_4Ghz #-- @desc  WLAN ISM Band #-- @spec 

px_WLAN_BeaconRSSI,                          INTEGER,       78      #-- @desc  Beacon RSSI value for IMS over WLAN test cases #-- @spec 

px_WLAN_NetworkAddrIPv4,                     CHARSTRING,    192.168.4.1 #-- @desc  IPv4 WLAN Network Address #-- @spec 

px_WLAN_NetworkAddrIPv6,                     CHARSTRING,    1111:2222:3333:8888:5555:6666:7777:1111 #-- @desc  IPv6 WLAN Network Address #-- @spec 

px_WLAN_PDN1_ToOffload,                      BOOLEAN,       true    #-- @desc  If set to true the first PDN connection is offloaded to WLAN. If set to false the second PDN connection is offloaded to WLAN. #-- @spec 

px_WLAN_RulesToBeTested,                     CHARSTRING,    ANDSF_Rules #-- @desc  Rules to be tested in WLAN test cases #-- @spec 

px_WLAN_UE_AddrIPv4,                         CHARSTRING,            #-- @desc  IPv4 WLAN UE Address #-- @spec 

px_WLAN_UE_AddrIPv6,                         CHARSTRING,            #-- @desc  IPv6 WLAN UE Address #-- @spec 

px_WLAN_UE_MAC_Address,                      CHARSTRING,            #-- @desc  UEDevice Wi-Fi MAC address (Format: aa-bb-cc-dd-ee-ff) #-- @spec 

px_XCAPServerAddress,                        CHARSTRING,    10.122.11.26 #-- @desc  XCAP Server address #-- @spec 34.229-3

px_XCAP_Password,                            CHARSTRING,    xcap    #-- @desc  XCAP password #-- @spec 34.229-3

px_XCAP_RootUri,                             CHARSTRING,    XCAP.3gpp.org #-- @desc  XCAP Root URI #-- @spec 

px_XCAP_TargetUri,                           CHARSTRING,    sip:user@domain.com #-- @desc  Target (SIP or TEL URI) where to forward to #-- @spec 

px_XCAP_Username,                            CHARSTRING,    0       #-- @desc  username to be used for HTTP authentication in case of pc_XCAP_UsernameIsConfiguredInUE==true #-- @spec 

px_eAuthRAND,                                BITSTRING,     10100011110111100000110001101101001101100011111000110000110000110110010010100100000001111000111100011011111110001101010101110111 #-- @desc  Random Challenge #-- @spec 

px_eJapanMCC_Band6,                          HEXSTRING,     442     #-- @desc  Japan MCC code to be used for Band 6. The same value will be used for E-UTRAN and Inter-RAT cells. Type is different to that defined in 34.123-3. #-- @spec 

px_eMaxNumberROHC_ContextSessions,           ENUM-MaxNumberROHC_ContextSessions_Type,cs16    #-- @desc  Maximum number of ROHC context sessions @sic R5s130329 sic@ #-- @spec 

px_ePDG_Ipsec_CipheringAlgorithm,            ENUM-IPsec_CipheringAlgorithm_Type,des_ede3_cbc #-- @desc  Ipsec Ciphering Algorithm used in ePDG #-- @spec 

px_ePDG_Ipsec_IntegrityAlgorithm,            ENUM-IPsec_IntegrityAlgorithm_Type,hmac_sha_1_96 #-- @desc  Ipsec Integrity Algorithm used in ePDG #-- @spec 

px_ePDG_OperatorProvisionedFQDN,             CHARSTRING,            #-- @desc  domain name of the ePDG to be considered to assign the IP addresses of the ePDG in responses to DNS queries #-- @spec 

px_ePrimaryBandChannelBandwidth,             ENUM-Dl_Bandwidth_Type,n25     #-- @desc  Channel bandwidth used on px_ePrimaryFrequencyBand #-- @spec 

px_ePrimaryFrequencyBand,                    INTEGER,       3       #-- @desc  E-UTRAN primary frequency band #-- @spec 

px_eSecondaryBandChannelBandwidth,           ENUM-Dl_Bandwidth_Type,n25     #-- @desc  Channel bandwidth used on px_eSecondaryFrequencyBand #-- @spec 

px_eSecondaryFrequencyBand,                  INTEGER,       2       #-- @desc  E-UTRAN secondary frequency band #-- @spec 

px_eTDDsubframeConfig,                       ENUM-TDD_SubframeAssignment_Type,sa1     #-- @desc  TDD uplink-downlink subframe configuration #-- @spec 

px_eUE_Category_Type,                        INTEGER,       3       #-- @desc  UE Category values 1..5 as defined in 36.306 clause 4.1 #-- @spec 

px_nonSMSTransport_CP_CIoT,                  BOOLEAN,       false   #-- @desc  NB-IoT UE configured to utilise non-SMS services as transport mechanism for user data for Control Plane CIoT Optimisation #-- @spec 

