# **[102-e-NR- 5G\_V2X\_NRSL-PHYprocedure-02] Email discussion/approval regarding the assumptions for the CSI reference resource for sidelink CSI**

[102-e-NR- 5G\_V2X\_NRSL-PHYprocedure-02] Email discussion/approval regarding the assumptions for the CSI reference resource for sidelink CSI by 8/21, followed by potential TPs by 8/26 – Hanbyul (LGE)

Q1: Do you agree following assumption?

* + For the sidelink CSI reference resource, UE assumes
		- First SL symbol is occupied by duplicated symbol of 2nd SL symbol within a SL slot
		- Numerology (CP length and SCS) of configured SL BWP is used

|  |  |  |
| --- | --- | --- |
| Company | Answer | Comment |
| NTT DOCOMO |  | For the first sub-bullet, the situation is always true, so the ‘assumption’ would not be necessary.Second sub-bullet is OK. |
| Sharp | Agree |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Q2: What is the assumption on RV for the sidelink CSI reference resource?

* + Option 1: RV0
	+ Option 2: RV indicated by SCI triggering the CSI report
	+ Option 3: Others (please specify)

|  |  |  |
| --- | --- | --- |
| Company | Preferred option | Comment |
| NTT DOCOMO | Option 1 | Reuse NR-Uu.For CSI report, self-decodable RV is feasible. RV0 should be OK. |
| Sharp | Option 1 | Reuse NR Uu. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Q3: What is the assumption on PSCCH overhead for the sidelink CSI reference resource?

* + Option 1: PSCCH occupies 2 OFDM symbols
	+ Option 2: PSCCH occupies timeResourcePSCCH OFDM symbols and frequencyResourcePSCCH PRBs in the resource pool
	+ Option 3: Others (please specify)

|  |  |  |
| --- | --- | --- |
| Company | Preferred option | Comment |
| NTT DOCOMO | Option 1 | Reuse Uu.UE receiving the CSI report would correct the information for actual transmission. As discussed before/after this question, there are some/many assumptions. Regardless of outcome of this question, the UE needs to do that. So it seems that option 2 has no benefit. |
| Sharp | Option 1 | Reuse NR Uu. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Q4: What is the assumption on the number of PSSCH and DM-RS symbols for the sidelink CSI reference resource?

* + Option 1: 10
	+ Option 2: sl-LengthSymbols ‒ 2
	+ Option 3: the number of PSSCH and DM-RS symbols in a slot where SCI triggering the CSI report is transmitted
	+ Option 4: sl-LengthSymbols ‒ 5 if periodPSFCHresource = 1. Otherwise, sl-LengthSymbols ‒ 2.
	+ Option 5: Others (please specify)

|  |  |  |
| --- | --- | --- |
| Company | Preferred option | Comment |
| NTT DOCOMO | Option 1 | Reuse NR-Uu, where assumption of the number of PDSCH and DM-RS is fixed as 12.Similar to our comment on Q3. |
| Sharp | Option 1 | Reuse NR Uu, where the assumption is (14-2-2)=10 |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Q5: What is the assumption on sidelink CSI-RS overhead for the sidelink CSI reference resource?

* + Option 1: No CSI-RS mapping REs
	+ Option 2: the number of CSI-RS REs in a PSSCH resource scheduled by SCI triggering the CSI report
	+ Option 3: Others (please specify)

|  |  |  |
| --- | --- | --- |
| Company | Preferred option | Comment |
| NTT DOCOMO | Option 1 | Reuse NR-Uu. |
| Sharp | Option 1 | Reuse NR Uu |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Q6: What is the assumption on 2nd SCI overhead for the sidelink CSI reference resource?

* + Option 1: No 2nd SCI mapping REs
	+ Option 2: Lowest overhead per (pre)configuration
	+ Option 3: : the number of REs for 2nd SCI triggering the CSI report
	+ Option 4: Others (please specify)

|  |  |  |
| --- | --- | --- |
| Company | Preferred option | Comment |
| NTT DOCOMO | Option 1 | Reuse NR-Uu.Similar to our comment on Q3. |
| Sharp | Option 1 | Reuse NR Uu |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Q7: What is the assumption on 2nd SCI overhead for the PSSCH DMRS ~~the sidelink CSI reference resource~~?

* + Option 1: Smallest number of PSSCH DMRS symbols per (pre)confiugraiton
	+ Option 2: the number of PSSCH DMRS symbols indicated by SCI associated with the triggered CSI report
	+ Option 3: Others (please specify)

|  |  |  |
| --- | --- | --- |
| Company | Preferred option | Comment |
| NTT DOCOMO | Option 1 | First of all, the question would be about DM-RS, not 2nd-stage SCI overhead.Regarding preferred option, reuse NR-Uu, where assumption of the number of DM-RS is based on the configurations. |
| Sharp | Option 3 | If the question refers to PSSCH DMRS overhead, then we propose to reuse NR Uu without containing DMRS, i.e. no overhead is assumed. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Q8: Do you think there are other aspects RAN1 needs to consider in defining assumptions for the sidelink CSI reference resource?

|  |  |  |
| --- | --- | --- |
| Company | Answer | Comment |
| Sharp |  | Assume the SL CSI reference resource does not contain SL PT-RS. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |