**3GPP TSG- RAN WG1 Meeting #104b-e R1-2xxxxxx**

**e-Meeting, April 12th – 20th, 2021**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **38.214** | **CR** | **DRAFT** | **rev** | **-** | **Current version:** | **16.5.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Draft CR on Beam Management  |
|  |  |
| ***Source to WG:*** | Moderator (Apple Inc), vivo |
| ***Source to TSG:*** | R1 |
|  |  |
| ***Work item code:*** | NR\_newRAT-Core |  | ***Date:*** | 2021-04-12 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | The name of RRC parameter *enableDefaultBeamPL-ForPUSCH0* is not aligned with what is defined in 38.331 |
|  |  |
| ***Summary of change:*** | Change *enableDefaultBeamPL-ForPUSCH0* into *enableDefaultBeamPL-ForPUSCH0-0* |
|  |  |
| ***Consequences if not approved:*** | RRC parameter name is not correct. |
|  |  |
| ***Clauses affected:*** | 6.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | Impac analysis: This is editorial correction . So no impact on legacy gNB and UE. |
|  |  |
| ***This CR's revision history:*** |  |

**6.1 UE procedure for transmitting the physical uplink shared channel**

< Unchanged parts are omitted >

For PUSCH scheduled by DCI format 0\_0 on a cell and if the higher layer parameter *enableDefaultBeamPL-ForPUSCH0-0* is set 'enabled', the UE is not configured with PUCCH resources on the active UL BWP and the UE is in RRC connected mode, the UE shall transmit PUSCH according to the spatial relation, if applicable, with a reference to the RS configured with *qcl-Type* set to 'typeD' corresponding to the QCL assumption of the CORESET with the lowest ID on the active DL BWP of the cell.

For PUSCH scheduled by DCI format 0\_0 on a cell and if the higher layer parameter *enableDefaultBeamPL-ForPUSCH0-0* is set 'enabled', the UE is configured with PUCCH resources on the active UL BWP where all the PUCCH resource(s) are not configured with any spatial relation and the UE is in RRC connected mode, the UE shall transmit PUSCH according to the spatial relation, if applicable, with a reference to the RS configured with *qcl-Type* set to 'typeD' corresponding to the QCL assumption of the CORESET with the lowest ID on the active DL BWP of the cell in case CORESET(s) are configured on the cell.

< Unchanged parts are omitted >