**3GPP TSG-RAN WG1 Meeting #105-e *R1-21xxxxx***

**E-meeting, May 10 – May 27, 2021**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **DRAFT CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.212** | **CR** |  | **rev** | **-** | **Current version:** | **16.5.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Alignment CR for TS 38.212 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei | | | | | | | | | |
| ***Source to TSG:*** | R1 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_L1enh\_URLLC-Core | | | | |  | ***Date:*** | | | 2021-5-26 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | RRC parameter *pdsch-HARQ-ACK-Codebook* in DCI formats is not applicable anymore for the case of two configured HARQ-ACK codebooks as discussed under issue #3 in [105-e-NR-L1enh-URLLC-01]. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Capture the correction on RRC parameter for the case of two configured HARQ-ACK codebooks as outcome of issue #3 in [105-e-NR-L1enh-URLLC-01]. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Specification is incorrect | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 7.3.1 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | |  | | |
| ***affected:*** | |  | **X** | Test specifications | | | |  | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | |  | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

7.3.1 DCI formats

The DCI formats defined in table 7.3.1-1 are supported.

**Table 7.3.1-1: DCI formats**

|  |  |
| --- | --- |
| **DCI format** | **Usage** |
| 0\_0 | Scheduling of PUSCH in one cell |
| 0\_1 | Scheduling of one or multiple PUSCH in one cell, or indicating downlink feedback information for configured grant PUSCH (CG-DFI) |
| 0\_2 | Scheduling of PUSCH in one cell |
| 1\_0 | Scheduling of PDSCH in one cell |
| 1\_1 | Scheduling of PDSCH in one cell, and/or triggering one shot HARQ-ACK codebook feedback |
| 1\_2 | Scheduling of PDSCH in one cell |
| 2\_0 | Notifying a group of UEs of the slot format, available RB sets, COT duration and search space set group switching |
| 2\_1 | Notifying a group of UEs of the PRB(s) and OFDM symbol(s) where UE may assume no transmission is intended for the UE |
| 2\_2 | Transmission of TPC commands for PUCCH and PUSCH |
| 2\_3 | Transmission of a group of TPC commands for SRS transmissions by one or more UEs |
| 2\_4 | Notifying a group of UEs of the PRB(s) and OFDM symbol(s) where UE cancels the corresponding UL transmission from the UE |
| 2\_5 | Notifying the availability of soft resources as defined in Clause 9.3.1 of [10, TS 38.473] |
| 2\_6 | Notifying the power saving information outside DRX Active Time for one or more UEs |
| 3\_0 | Scheduling of NR sidelink in one cell |
| 3\_1 | Scheduling of LTE sidelink in one cell |

The fields defined in the DCI formats below are mapped to the information bits  to  as follows.

Each field is mapped in the order in which it appears in the description, including the zero-padding bit(s), if any, with the first field mapped to the lowest order information bit  and each successive field mapped to higher order information bits. The most significant bit of each field is mapped to the lowest order information bit for that field, e.g. the most significant bit of the first field is mapped to .

If the number of information bits in a DCI format is less than 12 bits, zeros shall be appended to the DCI format until the payload size equals 12.

The size of each DCI format is determined by the configuration of the corresponding active bandwidth part of the scheduled cell and shall be adjusted as described in clause 7.3.1.0 if necessary.

If a UE is configured with *pdsch-HARQ-ACK-CodebookList-r16*, *pdsch-HARQ-ACK-Codebook* is replaced by the relevant entry in *pdsch-HARQ-ACK-CodebookList-r16* in this clause.