**3GPP TSG RAN WG1 #108-e R1-2202495**

**e-Meeting, February 21st – March 3rd, 2022**

**Title: FL Summary for Rel-17 RRC parameters for positioning enhancement**

**Source: Moderator (CATT)**

**Agenda item: 8.5**

**Document for:** **Discussion and Decision**

1. Introduction

This document provides a summary of the following email discussion for AI 8.5:

[108-e-R17-RRC-ePos] Email discussion on Rel-17 RRC parameters for positioning enhancement – Ren Da (CATT)

* 1st check point for first LS in [108-e-R17-RRC]: February 24
* Final check point for second LS in [108-e-R17-RRC] if necessary: March 3

The RRC parameters from the last meeting are included in R1-2110573[1].

The general recommendations from the R17-RRC-Moderator for RAN1 RRC parameter preparation are provided in *R1-2111193* [2]. Additional suggestion from the R17-RRC-Moderator includes:

* *use a different color (e.g. “blue”) than “black” for any change applied to a row that is currently “stable” with only-black color.*
* *do not change the content of “Status [106b-e]” and “Status [107bis-e]” columns.*
* *provide the status, i.e. “stable/unstable” for Column [108-e] for any row if the status is “unstable”, or the status is changed from “stable” to “unstable”.*
  + *If a row remains “stable”, or if a row hasn’t changed, no need to indicate the status. The previous status holds.*
* *Please continue considering the guidelines in R1-2111193 for RRC preparation.*

For Rel-17 ePOS most of the open issues are related to range values. Most of them are “FFS” and some of them are in the squared bracket []. In this meeting, we are targeting to complete the range values for all of the RRS parameters.

Note: We will need to remove the squared brackets “[]” for all agreeable range values, i.e., squared brackets will either be removed or replaced with round brackets “()” for all agreeable range values when submitting the RRC parameter list.

2. Accuracy improvements by mitigating UE Rx/Tx and/or gNB Rx/Tx timing delays

## (Round 1) FL Proposed Changes (marked in red in data Sheet “Positioning (Round 1)”)

­

* *Rows 2, 10: Change Value range FFS is changed to “[0, 1, …, 31]” based on Row 11*
* *Rows 4, 9: Change Value range FFS is changed to “[0, 1, …, 7]” based on Row 12.*
* *Row 5: Indicate srs-PosResourceSetId as “****removed”*** *in “Status [108-e]” based on the inputs from multiple companies to RAN2 LS*
* *Row 6: Remove the bracket for srs-PosResourceId*
* *Row 7: Change Value range FFS to N/A;*
* *Row 8: Change Value range FFS to “[0, 1., …, 255] based on previous agreement that the maximum number of Tx TEGs is 256*
* *Row 11: Correction. Change [8] to 32.*
* *Row 12: Change [8] to 8.*
* *Row 13, Change Value range FFS to [64], since the maximum number of SRS resource for positioning is 64. Change “unstable” to “new-stable”. And remove the bracket for the parameter name.*
* *Row 14, Change [256] to 256*
* *Rows 16, 17, 18, 19: Change Value range “FFS” to “~~FFS~~ BOOLEAN” for these simple requests. RAN2/RAN3 may decide whether it is “Yes” only, or has both “Yes” and “No”.*
* *Row 23, change Value range FFS to “FFS for RAN2”. It is up to RAN2 to use an existing format of the timestamp or a new format.*
* *Row 27 : Change Value range FFS to [0, 1, …,7]*
* *Row 30 : a) Change Value range FFS to N/A;*
* *Row 31 : Change Value range FFS to [0, 1, …,255]*
* *Row 32 : Change Value range FFS to [0, 1, …,7]*
* *Row 33 : Change Value range FFS to [0, 1, …,31]*
* *Row 34 : srs-PosResourceSetId as* ***removed*** *in status [#108e]. It seems no need to have the parameter.*
* *Row 35 : Change Value range FFS to [0, 1, …,63]*
* *Row 37 : Remove the bracket of the parameter name and change the Value range FFS to 32*
* *Row 38 : Remove the bracket of the parameter name and change the Value range FFS to 8*
* *Row 39 : Remove the bracket of the parameter name and change the Value range FFS to 64, add “new-stable” to in status [#108e].*
* *Row 40 : Remove the bracket of the parameter name and change the Value range FFS to 256*
* *Row 41 : Change the parameter name and description to match the agreement*
* *Row 42 : Change the parameter name and description to match the agreement, and replace the “agreement”.*
* *Row 43 : Change the parameter name and description to match the agreement*
* *Row 44, 45, 46: Change FFS to “FFS BOOLEAN” for a simple request*
* *Row 47: Add “Removed” in status [#108e], because of the duplication with Row 41, 42, 43.*
* *Row 48: Suggest to let RAN3 to define the timestamp value*

*Changes in Column M:*

* *Rows 11, 12, 14: Removed the bracket of “[per UE]”*
* *Rows 16, 17, 18, 19: Remove “FFS”, since it may not be meaningful to define “per UE, ..” for these parameters*
* *Rows 20, 21, 22: Change “FFS” tp “[per band]”*
* *Row 23: Removed “FFS”. since it may not be meaningful to define “per UE, ..” for the parameter*
* *Row 37 to Row 43: Removed the bracket of “[per TRP]”*

## (Round 1) Comments

|  |  |
| --- | --- |
| **Company** | **comments** |
|  |  |
|  |  |
|  |  |
|  |  |

***Question 1****: The the “FFS: A triplet of UE {RxTx TEG ID, Rx TEG ID, Tx TEG ID}” in Row 7, different companies may have different understanding on whether the reporting of the triplet of UE {RxTx TEG ID, Rx TEG ID, Tx TEG ID}” is supported based on the existing RAN1 agreement. Companies are invited to provide their views in the following table on:*

* *OP1 (YES): support the reporting of a triplet of UE {RxTx TEG ID, Rx TEG ID, Tx TEG ID}*
* *OP2 (NO): not support the reporting of a triplet of UE {RxTx TEG ID, Rx TEG ID, Tx TEG ID}*

## (Round 1) Comments for Q1

|  |  |  |
| --- | --- | --- |
| **Company** | **yes/NO** | **comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Question 2**: *RAN2 (R1-2200878) LS asks whether Row 15 “numOfUERxTEG-PerPRSResource” is a duplication of Row 20 “MeasPRSwithDiffRxTEGs\_Request\_RSTD”. Based on the contributions [12-20], it seems companies have different views. Companies are invited to provide their views on whether Row 15 “numOfUERxTEG-PerPRSResource” can be removed due to the duplication with Row 20 “MeasPRSwithDiffRxTEGs\_Request\_RSTD”.*

* *OP1 (YES): “numOfUERxTEG-PerPRSResource” can be removed*
* *OP2 (NO): Both “numOfUERxTEG-PerPRSResource” and “MeasPRSwithDiffRxTEGs\_Request\_RSTD” need to be kept.*

## (Round 1) Comments for Q2

|  |  |  |
| --- | --- | --- |
| **Company** | **yes/NO** | **comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

3. Accuracy improvements for UL-AoA positioning solutions

## (Round 1) FL Proposed Changes (marked in red in data Sheet “Positioning (Round 1)”)

* *Row 57: Change value range FFS to N/A*
* *Row 58, 59, 60,61, 62, 63, 64: changes are made according to approved RAN3 CR (R3-220072), and change “new-stable” in status [#108e]*
* *Row 65: Change “FFS” to “N/A”*
* *Row 66: Change the value FFS to “Defined in 9.2.38, TS 38.455”*
* *Row 69: Change the value rage to INTEGER(0..63) according to TS 38.455*
* *Row 70: Change the value rage to INTEGER(0..63) according to TS 38.455*

## (Round 1) Comments

|  |  |
| --- | --- |
| **Company** | **comments** |
|  |  |
|  |  |
|  |  |
|  |  |

4. Accuracy improvements for DL-AoD positioning solutions

## (1st Round) FL Proposed Changes (marked in red in Excel Sheet ePOS#v000)

* *Row 76: Change Value range “FFS” to “~~FFS~~ BOOLEAN” for the simple request. RAN2/3 may decide whether it is “Yes” only, or has both “Yes” and “No”.*
* *Row 77: Change FFS to N/A. No value range for an IE structure.*
* *Row 78: Change Value range “FFS” to “~~FFS~~ BOOLEAN” for the simple request. RAN2/3 may decide whether it is “Yes” only, or has both “Yes” and “No”.*
* *Row 79: Remove FFS. No value range for an IE structure. Also Remove FFS: The details of TRP beam/antenna information, since the details of trpBeamAntennaInformation are defined in Row 95 to 98,*
* *Row 80: Add the value range of PRS Resource ID based on the current range value defined e.g., in TS 38.355/455.*
* *Row 81: Add a new row for missing PRS Resource Set ID.*
* *Row 82, 83: The value ranges can be decided based on exiting range defined TS 38.455*
* *Row 85: Change Value range “FFS” to “~~FFS~~ BOOLEAN” for the simple request. RAN2/3 may decide whether it is “Yes” only, or has both “Yes” and “No”.*
* *Row 86: Change “FFS” to [Ref. TS38.133] and add RAN4 LS R4-2202780 “• PRS-RSRPP may be reported by reusing absolute and differential PRS-RSRP measurement report mapping tables in TS38.133 clause 10.1.24.3.1 and 10.1.24.3.2 respectively” in the comment column.*
* *Rows 90: Change “FFS” to “N/A”*
* *Rows 91: Change “FFS” to BOOLEAN*
* *Rows 92: Change “FFS” to BOOLEAN*
* *Rows 93 to 96: Suggest the values related to the expected DL-AOA values are defined in a similar way as expected UL-AOA values*
* *Rows 97 to 103: Making similar changes as Rows 90 to 96*
* *Row 104: Change “FFS” to “N/A”*
* *Row 105: Change FFS to INTEGER(0..63)*
* *Row 106: Change “FFS” to “N/A”*
* *Row 107, 108: Change FFS to the value range based on 38.455.*

## (Round 1) Comments

|  |  |
| --- | --- |
| **Company** | **comments** |
|  |  |
|  |  |
|  |  |
|  |  |

5. Latency improvements for both DL and DL+UL positioning

## (Round 1) FL Proposed Changes (marked in red in data Sheet “Positioning (Round 1)”)

* *Row 112: It seems the value range of a simple request can simply be a Boolean value decided by RAN2*
* *Row 118, It seems the value range of preconfigMG\_ID can be decided by RAN2*
* *Row 119: It seems the value range of a simple request can simply be a Boolean value decided by RAN2*
* *Row 120: Change the value range from FFS to [0, 1, 2] to represent the three options in the agreement*
* *Row 121: The value range should be “N/A”*
* *Row 122, 123: Change the value range from FFS to “[Ref. NR-DL-PRS-Periodicity-and-ResourceSetSlotOffset in TS 37.355”*
* *Row 124:*
* *Row 125: Change the value range from FFS to “[Ref. NR-PhysCellID and nr-CellGlobalID In TS 37.355”*
* *Row 126: Change the value range from FFS for [15, 30, 60, 120] kHz*
* *Row 127: The value of the request can simply be a Boolean value decided by RAN3.*

## (Round 1) Comments

|  |  |
| --- | --- |
| **Company** | **comments** |
|  |  |
|  |  |
|  |  |
|  |  |

6. Potential enhancements of information reporting from UE and gNB for multipath/NLOS mitigation

## (Round 1) FL Proposed Changes (marked in red in data Sheet “Positioning (Round 1)”)

* *Row 130: Added the agreements related to the reporting of the losNlosIndicator from UE*
* *Row 131: Added the agreements related to the reporting of the losNlosIndicator from TRP*
* *Row 132: Change FFS to the same value as row 131*
* *Row 135: Change the value range of FFS to [4, 8]*
* *Rows 137 to 143: Change Value range “FFS” to “~~FFS~~ BOOLEAN” for these simple requests. RAN2/RAN3 may decide whether it is “Yes” only, or has both “Yes” and “No”.*

## (Round 1) Comments

|  |  |
| --- | --- |
| **Company** | **comments** |
|  |  |
|  |  |
|  |  |
|  |  |

7. On-demand transmission and reception of DL PR

## (Round 1) FL Proposed Changes (marked in red in data Sheet “Positioning (Round 1)”)

* *Row 146: Change “FFS” to “[Ref. TS 37.355]”, assume all existing PRS periodicities are supported*
* *Row 168: Change “FFS” to “BOOLEAN” since the parameter is an ON/OFF indicator*

## 

## (Round 1) Comments

|  |  |
| --- | --- |
| **Company** | **comments** |
|  |  |
|  |  |
|  |  |
|  |  |

8. Support of positioning for UEs in RRC\_ INACTIVE state

## (Round 1) FL Proposed Changes (marked in red in data Sheet “Positioning (Round 1)”)

* *Row 175: Change “FFS” to “[Ref. TS 37.355]” based on RAN1’s agreement that “SRS for positioning for UEs in RRC\_INACTIVE state is configured using the SRS-PosResourceSet IE”.*

## (Round 1) Comments

|  |  |
| --- | --- |
| **Company** | **comments** |
|  |  |
|  |  |
|  |  |
|  |  |

9. Summary

TBD

10. References

1. R1-2111193 Recommendations for RAN1 RRC Parameter Preparation Moderator(Ericsson)
2. R1-2112979, Collection of updated higher layers parameter list for Rel-17 LTE and NR, Moderator (Ericsson)
3. R1-2200780, Updated RAN1 UE features list for Rel-17 NR after RAN1 #107bis-e, Moderators (AT&T, NTT RAN1 Chair’s Notes#104e.
4. R1-2112508, FL Summary for Rel-17 RRC parameters for positioning enhancement, Moderator (CATT)
5. R1-2200878 (R2-2201776), Response LS on the reporting of the Tx TEG association information, RAN2 (CATT)
6. RAN1 Chair’s Notes#104bis-e.
7. RAN1 Chair’s Notes#105e.
8. RAN1 Chair’s Notes#106e.
9. RAN1 Chair’s Notes#106bis-e.
10. RAN1 Chair’s Notes#107-e.
11. R1-2200878 Response LS on the reporting of the Tx TEG association information RAN2, CATT
12. R1-2201009 Draft reply LS on reporting of the Tx TEG association information Huawei
13. R1-2201054 Draft reply LS on reporting of the Tx TEG association information vivo
14. R1-2201207 Draft reply LS on the reporting of the Tx TEG association information ZTE
15. R1-2201247 Discussion on "Response LS on the reporting of the Tx TEG association information" OPPO
16. R1-2201317 Discussion on the reporting of the Tx TEG association information CATT
17. R1-2201318 Draft reply LS on the reporting of the Tx TEG association information CATT
18. R1-2202106 Draft Reply to RAN2 LS on the reporting of the Tx TEG association information Qualcomm Incorporated
19. R1-2202297 Draft Reply LS on the reporting of the Tx TEG association information LG Electronics
20. R1-2202327 Draft reply to Response LS on the reporting of the Tx TEG association information Ericsson