**3GPP TSG-RAN WG2 Meeting #113-eR2-21xxxxx**

**Online, 25th Jan – 5th Feb 2021**

**Agenda item: 8.1.1**

**Source: Chairman (Mediatek Inc)**

**Title: [Offline-038][MBS] UP Architecture Desicions**

**Document for: Discussion**

# 1 Introduction

This is to report the result of the following email discussion.

* [AT113-e][038][MBS] UP architecture decisions (Chairman)

 Scope: Gather comments to facilitate a CB to address two decisions: A) on L2 ARQ for PTM, B) for PTM PTP switch, which layer to be the anchor.

 Intended outcome: Report with collection of comments

 Deadline: Friday Jan 29 1200 UTC

The Discussion scope is to gather comments to facilitate a online CB discussion to address two decisions: A) on L2 ARQ for PTM, B) for PTM PTP switch, which layer to be the anchor.

Companies are strongly encouraged to voice their opinions here.

# 2 Contact Information

To make it easier to find the correct contact delegate in each company for potential follow-up questions, the rapporteur encourages the delegates who provide input to provide their contact information in this table:

|  |  |
| --- | --- |
| Company | Contact: Name (E-mail) |
| Chairman (Mediatek Inc.) | Johan.johansson@mediatek.com |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# 3 Discussion

## 3.1 Need for UP decisions

Chairman’s View:

First, pointing out the obvious: The MBS Work Item is large, there is a lot of functionality that need to be supported in RAN2, it impacts many specifications, has impact in all other group with need for work coordination. Both User Plane and Mobility is impacted which both are among the most difficult to progress topics in RAN2. Behind each alternative, also behind the seemingly “simple” alternatives, there is a lot of detailed issues that requires significant work and significant lead times to converge on.

The non-decided architecture blocks the possibility to progress many parts. Architecture = which functionality exists and where is it located (which protocol layer, which peer entity).

The current decision status is that there was a working assumption established last meeting that PTM will not support RLC-AM, and no further decision has been taken since to either overturn or confirm this. For the anchoring of PTP PTM switch there is no present decision.

It is important that RAN2 consolidates MBS user plane architectural decisions soon.

## 3.2 UP decisions

**The main two points that seems to need resolution/consolidation are the following**

*A. L2 ARQ for PTM for normal data transfer*

*B. Which layer anchors the PTM PTP switch, i.e. at PTM PTP switch which layer remains the same, (and might be responsible for service continuity).*

Both point A and B are included here because several companies indicate that they are inter-dependent,

**For A. there seems to be the following options on the table:**

A1. No L2 ARQ for PTM

A2. L2 ARQ by PDCP for PTM

A3. L2 ARQ by RLC-AM for PTM

**For B. There seems to be the following options on the table:**

B1. PDCP anchored PTM/PTP switch

B2. RLC anchored PTM/PTP Switch

Different combinations of Ax/Bx seems to be technically possible, but they seems to come with different complexity, different level of reuse and different characteristics.

## 3.3 This email discussion

The purpose of this discussion is to have opportunity to put on the table opinions and arguments of all interested companies with less time consumption.

As this is a controversial topic it seems there will not be sufficient on-line time to allow everyone to voice their opinions on-line on all these aspects. It is encouraged that companies voice their main opinions / suggestions and supporting arguments relating to the options and combination of A and B.

Similar to online debate It is furthermore encouraged that companies respond to other companies’ comments (not endlessly but maybe one round). Comments are numbered to facilitate this.

# 4 Discussion

**For A. there seems to be the following options on the table:**

A1. No L2 ARQ for PTM

A2. L2 ARQ by PDCP for PTM

A3. L2 ARQ by RLC-AM for PTM

**For B. There seems to be the following options on the table:**

B1. PDCP anchored PTM/PTP switch

B2. RLC anchored PTM/PTP Switch

|  |  |  |
| --- | --- | --- |
| **N** | **COMPANY** | **COMMENT** |
| 1 | Chairman | **My high level understanding of the proposals:** **A1:** No L2 ARQ for PTM, UNDERSTANDING: For normal data transfer, reliability is handled by L1, HARQ, and switching from PTM to PTP if the link gets bad and vice versa. PTP could be configured different to PTM, e.g. with RLC-AM. **A2:** L2 ARQ by PDCP for PTM, UNDERSTANDING: In addition to A1, there is possibility to have PDCP retransmission of SDUs across PTP at lost data, which could be triggered by a PDCP status report (other trigger FFS). **A3**: L2 ARQ by RLC-AM for PTM, UNDERSTANDING: RLC-AM is adapted such that dedicated protocol control and dedicated retransmissions uses the PTP leg. RLC-AM segments are retransmitted at lost data (as normal). It is assumed possible to keep current protocol including also e.g. Poll/Ack Nack supervision and retriggering mechanisms. Further It is proposed that both PTP and PTM is one single RLC-AM protocol instance (same SN, buffer status etc) and this would bring benefits at PTP PTM switching. However, this doesn’t seem to be a core part, so for a good discussion this point could be considered FFS. A1 or A2 could be supported in addition to A3 in order to support RLC-UM. **B1**: PDCP anchored PTM/PTP switch, UNDERSTANDING: Similar as Mobility, PDCP SN is the basis for service continuity. Receiver packet handling is anyway in PDCP, reordering duplicate handling, triggering of status report (FFS new triggers). When lost data at switch need to be recovered, transmitter can perform retransmissions of SDUs on PTP. B1 Can work with all of the alternatives of A1 A2 A3 and requires no particular interdependency from the lower protocols (e.g. RLC AM for PTP and RLC-UM for PTM would be ok).**B2:** RLC anchored PTM/PTP Switch, UNDERSTANDING: RLC anchored PTP PTM switch is intended for the case that both PTP and PTM is one single RLC-AM protocol instance where data lost at the switch is retransmitted as RLC-AM segments by the same protocol mechanisms as during normal data transfer. For RLC-UM cases, B2 would not be used, in particular if RLC-AM/PTP and RLC-UM/PTM shall be supported (my understanding). |
| 2 |  |  |
| 3 |  |  |
| 4 |  |  |
| 5 |  |  |
| 6 |  |  |
| 7 |  |  |
| 8 |  |  |
| 9 |  |  |
| 10 |  |  |
| 11 |  |  |
| 12 |  |  |
| 13 |  |  |
| 14 |  |  |
| 15 |  |  |
| 16 |  |  |
| 17 |  |  |
| 18 |  |  |
| 19 |  |  |
| 20 |  |  |
| 21 |  |  |
| 22 |  |  |
| 23 |  |  |
| 24 |  |  |
| 25 |  |  |
| 26 |  |  |
| 27 |  |  |
| 28 |  |  |
| 29 |  |  |
| 30 |  |  |
| 31 |  |  |
| 32 |  |  |
| 33 |  |  |
| 34 |  |  |
| 35 |  |  |
| 36 |  |  |
| 37 |  |  |
| 38 |  |  |
| 39 |  |  |
| 40 |  |  |
| 41 |  |  |
| 42 |  |  |
| 43 |  |  |
| 44 |  |  |
| 45 |  |  |
| 46 |  |  |
| 47 |  |  |
| 48 |  |  |
| 49 |  |  |
| 50 |  |  |
| 51 |  |  |
| 52 |  |  |
| 53 |  |  |
| 54 |  |  |
| 55 |  |  |
| 56 |  |  |
| 57 |  |  |
| 58 |  |  |
| 59 |  |  |
| 60 |  |  |