**3GPP TSG-RAN WG2 Meeting #117-e *R2-*** ***220XXX***

**Electronic Meeting, FEB 21 – MAR 03, 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **38.331** | **CR** | **2912** | **rev** | **1** | **Current version:** | **16.7.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Introduction of sidelink power class capability indication |
|  |  |
| ***Source to WG:*** | Xiaomi |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | 5G\_V2X\_NRSL-Core |  | ***Date:*** | 2022-3-2 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | RAN4 introduced two signalled capabilities for NR V2X as:1, NR V2X power class per band capability.2, NR V2X intra-band concurrent operation power class capability per band combinationUE can indicated PC2 and PC3. |
|  |  |
| ***Summary of change:*** | Introduce corresponding capability IEs**Impact Analysis**Impacted 5G architecture options: NR SAImpacted functionality:Capability reportInter-operability:1. If the network is implemented according to the CR and the UE is not, there is no inter-operability issue.2. If the UE is implemented according to the CR and the network is not, network can’t understand the introduced capability IEs. |
|  |  |
| ***Consequences if not approved:*** | UE can’t indicate supported power class on sidelink band and intra-band concurrent operation |
|  |  |
| ***Clauses affected:*** | 6.3.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

*Start Change*

### 6.3.3 UE capability information elements

#### – *BandCombinationList*

The IE *BandCombinationList* contains a list of NR CA, NR non-CA and/or MR-DC band combinations (also including DL only or UL only band).

*BandCombinationList* information element

-- ASN1START

-- TAG-BANDCOMBINATIONLIST-START

BandCombinationList ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination

BandCombinationList-v1540 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1540

BandCombinationList-v1550 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1550

BandCombinationList-v1560 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1560

BandCombinationList-v1570 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1570

BandCombinationList-v1580 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1580

BandCombinationList-v1590 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1590

BandCombinationList-v15g0 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v15g0

BandCombinationList-v1610 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1610

BandCombinationList-v1630 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1630

BandCombinationList-v1640 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1640

BandCombinationList-v1650 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1650

BandCombinationList-v16xy ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v16xy

BandCombinationList-UplinkTxSwitch-r16 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-r16

BandCombinationList-UplinkTxSwitch-v1630 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1630

BandCombinationList-UplinkTxSwitch-v1640 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1640

BandCombinationList-UplinkTxSwitch-v1650 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1650

BandCombinationList-UplinkTxSwitch-v1670 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-v1670

BandCombination ::= SEQUENCE {

 bandList SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParameters,

 featureSetCombination FeatureSetCombinationId,

 ca-ParametersEUTRA CA-ParametersEUTRA OPTIONAL,

 ca-ParametersNR CA-ParametersNR OPTIONAL,

 mrdc-Parameters MRDC-Parameters OPTIONAL,

 supportedBandwidthCombinationSet BIT STRING (SIZE (1..32)) OPTIONAL,

 powerClass-v1530 ENUMERATED {pc2} OPTIONAL

}

BandCombination-v1540::= SEQUENCE {

 bandList-v1540 SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParameters-v1540,

 ca-ParametersNR-v1540 CA-ParametersNR-v1540 OPTIONAL

}

BandCombination-v1550 ::= SEQUENCE {

 ca-ParametersNR-v1550 CA-ParametersNR-v1550

}

BandCombination-v1560::= SEQUENCE {

 ne-DC-BC ENUMERATED {supported} OPTIONAL,

 ca-ParametersNRDC CA-ParametersNRDC OPTIONAL,

 ca-ParametersEUTRA-v1560 CA-ParametersEUTRA-v1560 OPTIONAL,

 ca-ParametersNR-v1560 CA-ParametersNR-v1560 OPTIONAL

}

BandCombination-v1570 ::= SEQUENCE {

 ca-ParametersEUTRA-v1570 CA-ParametersEUTRA-v1570

}

BandCombination-v1580 ::= SEQUENCE {

 mrdc-Parameters-v1580 MRDC-Parameters-v1580

}

BandCombination-v1590::= SEQUENCE {

 supportedBandwidthCombinationSetIntraENDC BIT STRING (SIZE (1..32)) OPTIONAL,

 mrdc-Parameters-v1590 MRDC-Parameters-v1590

}

BandCombination-v15g0::= SEQUENCE {

 ca-ParametersNR-v15g0 CA-ParametersNR-v15g0 OPTIONAL,

 ca-ParametersNRDC-v15g0 CA-ParametersNRDC-v15g0 OPTIONAL,

 mrdc-Parameters-v15g0 MRDC-Parameters-v15g0 OPTIONAL

}

BandCombination-v1610 ::= SEQUENCE {

 bandList-v1610 SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParameters-v1610 OPTIONAL,

 ca-ParametersNR-v1610 CA-ParametersNR-v1610 OPTIONAL,

 ca-ParametersNRDC-v1610 CA-ParametersNRDC-v1610 OPTIONAL,

 powerClass-v1610 ENUMERATED {pc1dot5} OPTIONAL,

 powerClassNRPart-r16 ENUMERATED {pc1, pc2, pc3, pc5} OPTIONAL,

 featureSetCombinationDAPS-r16 FeatureSetCombinationId OPTIONAL,

 mrdc-Parameters-v1620 MRDC-Parameters-v1620 OPTIONAL

}

BandCombination-v1630 ::= SEQUENCE {

 ca-ParametersNR-v1630 CA-ParametersNR-v1630 OPTIONAL,

 ca-ParametersNRDC-v1630 CA-ParametersNRDC-v1630 OPTIONAL,

 mrdc-Parameters-v1630 MRDC-Parameters-v1630 OPTIONAL,

 supportedTxBandCombListPerBC-Sidelink-r16 BIT STRING (SIZE (1..maxBandComb)) OPTIONAL,

 supportedRxBandCombListPerBC-Sidelink-r16 BIT STRING (SIZE (1..maxBandComb)) OPTIONAL,

 scalingFactorTxSidelink-r16 SEQUENCE (SIZE (1..maxBandComb)) OF ScalingFactorSidelink-r16 OPTIONAL,

 scalingFactorRxSidelink-r16 SEQUENCE (SIZE (1..maxBandComb)) OF ScalingFactorSidelink-r16 OPTIONAL

}

BandCombination-v1640 ::= SEQUENCE {

 ca-ParametersNR-v1640 CA-ParametersNR-v1640 OPTIONAL,

 ca-ParametersNRDC-v1640 CA-ParametersNRDC-v1640 OPTIONAL

}

BandCombination-v1650 ::= SEQUENCE {

 ca-ParametersNRDC-v1650 CA-ParametersNRDC-v1650 OPTIONAL

}

BandCombination-v16xy ::= SEQUENCE {IntrabandConcurrentOperationPowerClass-r16 SEQUENCE (SIZE (1..maxBandComb)) OF IntraBandPowerClass-r16 OPTIONAL

}

BandCombination-UplinkTxSwitch-r16 ::= SEQUENCE {

 bandCombination-r16 BandCombination,

 bandCombination-v1540 BandCombination-v1540 OPTIONAL,

 bandCombination-v1560 BandCombination-v1560 OPTIONAL,

 bandCombination-v1570 BandCombination-v1570 OPTIONAL,

 bandCombination-v1580 BandCombination-v1580 OPTIONAL,

 bandCombination-v1590 BandCombination-v1590 OPTIONAL,

 bandCombination-v1610 BandCombination-v1610 OPTIONAL,

 supportedBandPairListNR-r16 SEQUENCE (SIZE (1..maxULTxSwitchingBandPairs)) OF ULTxSwitchingBandPair-r16,

 uplinkTxSwitching-OptionSupport-r16 ENUMERATED {switchedUL, dualUL, both} OPTIONAL,

 uplinkTxSwitching-PowerBoosting-r16 ENUMERATED {supported} OPTIONAL,

 ...

}

BandCombination-UplinkTxSwitch-v1630 ::= SEQUENCE {

 bandCombination-v1630 BandCombination-v1630 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1640 ::= SEQUENCE {

 bandCombination-v1640 BandCombination-v1640 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1650 ::= SEQUENCE {

 bandCombination-v1650 BandCombination-v1650 OPTIONAL

}

BandCombination-UplinkTxSwitch-v1670 ::= SEQUENCE {

 bandCombination-v15g0 BandCombination-v15g0 OPTIONAL

}

ULTxSwitchingBandPair-r16 ::= SEQUENCE {

 bandIndexUL1-r16 INTEGER(1..maxSimultaneousBands),

 bandIndexUL2-r16 INTEGER(1..maxSimultaneousBands),

 uplinkTxSwitchingPeriod-r16 ENUMERATED {n35us, n140us, n210us},

 uplinkTxSwitching-DL-Interruption-r16 BIT STRING (SIZE(1..maxSimultaneousBands)) OPTIONAL

}

BandParameters ::= CHOICE {

 eutra SEQUENCE {

 bandEUTRA FreqBandIndicatorEUTRA,

 ca-BandwidthClassDL-EUTRA CA-BandwidthClassEUTRA OPTIONAL,

 ca-BandwidthClassUL-EUTRA CA-BandwidthClassEUTRA OPTIONAL

 },

 nr SEQUENCE {

 bandNR FreqBandIndicatorNR,

 ca-BandwidthClassDL-NR CA-BandwidthClassNR OPTIONAL,

 ca-BandwidthClassUL-NR CA-BandwidthClassNR OPTIONAL

 }

}

BandParameters-v1540 ::= SEQUENCE {

 srs-CarrierSwitch CHOICE {

 nr SEQUENCE {

 srs-SwitchingTimesListNR SEQUENCE (SIZE (1..maxSimultaneousBands)) OF SRS-SwitchingTimeNR

 },

 eutra SEQUENCE {

 srs-SwitchingTimesListEUTRA SEQUENCE (SIZE (1..maxSimultaneousBands)) OF SRS-SwitchingTimeEUTRA

 }

 } OPTIONAL,

 srs-TxSwitch SEQUENCE {

 supportedSRS-TxPortSwitch ENUMERATED {t1r2, t1r4, t2r4, t1r4-t2r4, t1r1, t2r2, t4r4, notSupported},

 txSwitchImpactToRx INTEGER (1..32) OPTIONAL,

 txSwitchWithAnotherBand INTEGER (1..32) OPTIONAL

 } OPTIONAL

}

BandParameters-v1610 ::= SEQUENCE {

 srs-TxSwitch-v1610 SEQUENCE {

 supportedSRS-TxPortSwitch-v1610 ENUMERATED {t1r1-t1r2, t1r1-t1r2-t1r4, t1r1-t1r2-t2r2-t2r4, t1r1-t1r2-t2r2-t1r4-t2r4,

 t1r1-t2r2, t1r1-t2r2-t4r4}

 } OPTIONAL

}

ScalingFactorSidelink-r16 ::= ENUMERATED {f0p4, f0p75, f0p8, f1}

IntraBandPowerClass-r16 ::= ENUMERATED {PC2, PC3, spare6, spare5, spare4, spare3, spare2, spare1}

-- TAG-BANDCOMBINATIONLIST-STOP

-- ASN1STOP

|  |
| --- |
| *BandCombination* field descriptions |
| ***BandCombinationList-v1540, BandCombinationList-v1550, BandCombinationList-v1560, BandCombinationList-v1570, BandCombinationList-v1580, BandCombinationList-v1590, BandCombinationList-v15g0, BandCombinationList-r16，BandCombination-v16xy***The UE shall include the same number of entries, and listed in the same order, as in *BandCombinationList* (without suffix). If the field is included in *supportedBandCombinationListNEDC-Only-v1610*, the UE shall include the same number of entries, and listed in the same order, as in *BandCombinationList* of *supportedBandCombinationListNEDC-Only* (without suffix) field.If the field is included in *supportedBandCombinationListNEDC-Only-v15a0*, the UE shall include the same number of entries, and listed in the same order, as in *BandCombinationList* (without suffix) of *supportedBandCombinationListNEDC-Only* (without suffix) field. |
| ***ca-ParametersNRDC***If the field is included for a band combination in the NR capability container, the field indicates support of NR-DC. Otherwise, the field is absent. |
| ***featureSetCombinationDAPS***If this field is present for a band combination, it reports the feature set combination supported for the band combination when any DAPS bearer is configured. |
| ***ne-DC-BC***If the field is included for a band combination in the MR-DC capability container, the field indicates support of NE-DC. Otherwise, the field is absent. |
| ***srs-SwitchingTimesListNR***Indicates, for a particular pair of NR bands, the RF retuning time when switching between a NR carrier corresponding to this band entry and another (PUSCH-less) NR carrier corresponding to the band entry in the order indicated below:- For the first NR band, the UE shall include the same number of entries for NR bands as in *bandList*, i.e. first entry corresponds to first NR band in *bandList* and so on,- For the second NR band, the UE shall include one entry less, i.e. first entry corresponds to the second NR band in *bandList* and so on- And so on |
| ***srs-SwitchingTimesListEUTRA***Indicates, for a particular pair of E-UTRA bands, the RF retuning time when switching between an E-UTRA carrier corresponding to this band entry and another (PUSCH-less) E-UTRA carrier corresponding to the band entry in the order indicated below:- For the first E-UTRA band, the UE shall include the same number of entries for E-UTRA bands as in *bandList,* i.e. first entry corresponds to first E-UTRA band in *bandList* and so on,- For the second E-UTRA band, the UE shall include one entry less, i.e. first entry corresponds to the second E-UTRA band in *bandList* and so on - And so on |
| ***srs-TxSwitch***Indicates supported SRS antenna switch capability for the associated band. If the UE indicates support of *SRS-SwitchingTimeNR*, the UE is allowed to set this field for a band with associated *FeatureSetUplinkId* set to 0 for SRS carrier switching. |

*Nex Change*

#### – *SidelinkParameters*

The IE *SidelinkParameters* is used to convey capabilities related to NR and V2X sidelink communications.

*SidelinkParameters* information element

-- ASN1START

-- TAG-SIDELINKPARAMETERS-START

SidelinkParameters-r16 ::= SEQUENCE {

 sidelinkParametersNR-r16 SidelinkParametersNR-r16 OPTIONAL,

 sidelinkParametersEUTRA-r16 SidelinkParametersEUTRA-r16 OPTIONAL

}

SidelinkParametersNR-r16 ::= SEQUENCE {

 rlc-ParametersSidelink-r16 RLC-ParametersSidelink-r16 OPTIONAL,

 mac-ParametersSidelink-r16 MAC-ParametersSidelink-r16 OPTIONAL,

 fdd-Add-UE-Sidelink-Capabilities-r16 UE-SidelinkCapabilityAddXDD-Mode-r16 OPTIONAL,

 tdd-Add-UE-Sidelink-Capabilities-r16 UE-SidelinkCapabilityAddXDD-Mode-r16 OPTIONAL,

 supportedBandListSidelink-r16 SEQUENCE (SIZE (1..maxBands)) OF BandSidelink-r16 OPTIONAL,

 ...

}

SidelinkParametersEUTRA-r16 ::= SEQUENCE {

 sl-ParametersEUTRA1-r16 OCTET STRING OPTIONAL,

 sl-ParametersEUTRA2-r16 OCTET STRING OPTIONAL,

 sl-ParametersEUTRA3-r16 OCTET STRING OPTIONAL,

 supportedBandListSidelinkEUTRA-r16 SEQUENCE (SIZE (1..maxBandsEUTRA)) OF BandSidelinkEUTRA-r16 OPTIONAL,

 ...

}

RLC-ParametersSidelink-r16 ::= SEQUENCE {

 am-WithLongSN-Sidelink-r16 ENUMERATED {supported} OPTIONAL,

 um-WithLongSN-Sidelink-r16 ENUMERATED {supported} OPTIONAL,

 ...

}

MAC-ParametersSidelink-r16 ::= SEQUENCE {

 mac-ParametersSidelinkCommon-r16 MAC-ParametersSidelinkCommon-r16 OPTIONAL,

 mac-ParametersSidelinkXDD-Diff-r16 MAC-ParametersSidelinkXDD-Diff-r16 OPTIONAL,

 ...

}

UE-SidelinkCapabilityAddXDD-Mode-r16 ::= SEQUENCE {

 mac-ParametersSidelinkXDD-Diff-r16 MAC-ParametersSidelinkXDD-Diff-r16 OPTIONAL

}

MAC-ParametersSidelinkCommon-r16 ::= SEQUENCE {

 lcp-RestrictionSidelink-r16 ENUMERATED {supported} OPTIONAL,

 multipleConfiguredGrantsSidelink-r16 ENUMERATED {supported} OPTIONAL,

 ...

}

MAC-ParametersSidelinkXDD-Diff-r16 ::= SEQUENCE {

 multipleSR-ConfigurationsSidelink-r16 ENUMERATED {supported} OPTIONAL,

 logicalChannelSR-DelayTimerSidelink-r16 ENUMERATED {supported} OPTIONAL,

 ...

}

BandSidelinkEUTRA-r16 ::= SEQUENCE {

 freqBandSidelinkEUTRA-r16 FreqBandIndicatorEUTRA,

 -- R1 15-7: Transmitting LTE sidelink mode 3 scheduled by NR Uu

 gnb-ScheduledMode3SidelinkEUTRA-r16 SEQUENCE {

 gnb-ScheduledMode3DelaySidelinkEUTRA-r16 ENUMERATED {ms0, ms0dot25, ms0dot5, ms0dot625, ms0dot75, ms1,

 ms1dot25, ms1dot5, ms1dot75, ms2, ms2dot5, ms3, ms4,

 ms5, ms6, ms8, ms10, ms20}

 } OPTIONAL,

 -- R1 15-9: Transmitting LTE sidelink mode 4 configured by NR Uu

 gnb-ScheduledMode4SidelinkEUTRA-r16 ENUMERATED {supported} OPTIONAL

}

BandSidelink-r16 ::= SEQUENCE {

 freqBandSidelink-r16 FreqBandIndicatorNR,

 --15-1

 sl-Reception-r16 SEQUENCE {

 harq-RxProcessSidelink-r16 ENUMERATED {n16, n24, n32, n48, n64},

 pscch-RxSidelink-r16 ENUMERATED {value1, value2},

 scs-CP-PatternRxSidelink-r16 CHOICE {

 fr1-r16 SEQUENCE {

 scs-15kHz-r16 BIT STRING (SIZE (16)) OPTIONAL,

 scs-30kHz-r16 BIT STRING (SIZE (16)) OPTIONAL,

 scs-60kHz-r16 BIT STRING (SIZE (16)) OPTIONAL

 },

 fr2-r16 SEQUENCE {

 scs-60kHz-r16 BIT STRING (SIZE (16)) OPTIONAL,

 scs-120kHz-r16 BIT STRING (SIZE (16)) OPTIONAL

 }

 } OPTIONAL,

 extendedCP-RxSidelink-r16 ENUMERATED {supported} OPTIONAL

 } OPTIONAL,

 --15-2

 sl-TransmissionMode1-r16 SEQUENCE {

 harq-TxProcessModeOneSidelink-r16 ENUMERATED {n8, n16},

 scs-CP-PatternTxSidelinkModeOne-r16 CHOICE {

 fr1-r16 SEQUENCE {

 scs-15kHz-r16 BIT STRING (SIZE (16)) OPTIONAL,

 scs-30kHz-r16 BIT STRING (SIZE (16)) OPTIONAL,

 scs-60kHz-r16 BIT STRING (SIZE (16)) OPTIONAL

 },

 fr2-r16 SEQUENCE {

 scs-60kHz-r16 BIT STRING (SIZE (16)) OPTIONAL,

 scs-120kHz-r16 BIT STRING (SIZE (16)) OPTIONAL

 }

 },

 extendedCP-TxSidelink-r16 ENUMERATED {supported} OPTIONAL,

 harq-ReportOnPUCCH-r16 ENUMERATED {supported} OPTIONAL

 } OPTIONAL,

 --15-4

 sync-Sidelink-r16 SEQUENCE {

 gNB-Sync-r16 ENUMERATED {supported} OPTIONAL,

 gNB-GNSS-UE-SyncWithPriorityOnGNB-ENB-r16 ENUMERATED {supported} OPTIONAL,

 gNB-GNSS-UE-SyncWithPriorityOnGNSS-r16 ENUMERATED {supported} OPTIONAL

 } OPTIONAL,

 --15-10

 sl-Tx-256QAM-r16 ENUMERATED {supported} OPTIONAL,

 --15-11

 psfch-FormatZeroSidelink-r16 SEQUENCE {

 psfch-RxNumber ENUMERATED {n5, n15, n25, n32, n35, n45, n50, n64},

 psfch-TxNumber ENUMERATED {n4, n8, n16}

 } OPTIONAL,

 --15-12

 lowSE-64QAM-MCS-TableSidelink-r16 ENUMERATED {supported} OPTIONAL,

 --15-15

 enb-sync-Sidelink-r16 ENUMERATED {supported} OPTIONAL,

 ...,

 [[

 --15-3

 sl-TransmissionMode2-r16 SEQUENCE {

 harq-TxProcessModeTwoSidelink-r16 ENUMERATED {n8, n16},

 scs-CP-PatternTxSidelinkModeTwo-r16 ENUMERATED {supported} OPTIONAL,

 dl-openLoopPC-Sidelink-r16 ENUMERATED {supported} OPTIONAL

 } OPTIONAL,

 --15-5

 congestionControlSidelink-r16 SEQUENCE {

 cbr-ReportSidelink-r16 ENUMERATED {supported} OPTIONAL,

 cbr-CR-TimeLimitSidelink-r16 ENUMERATED {time1, time2}

 } OPTIONAL,

 --15-22

 fewerSymbolSlotSidelink-r16 ENUMERATED {supported} OPTIONAL,

 --15-23

 sl-openLoopPC-RSRP-ReportSidelink-r16 ENUMERATED {supported} OPTIONAL,

 --13-1

 sl-Rx-256QAM-r16 ENUMERATED {supported} OPTIONAL

 ]],

 [[

 ue-PowerClassSidelink-r16 ENUMERATED {PC2, PC3, spare6, spare5, spare4, spare3, spare2, spare1} OPTIONAL

 ]]

}

-- TAG-SIDELINKPARAMETERS-STOP

-- ASN1STOP

|  |
| --- |
| *SidelinkParametersEUTRA* field descriptions |
| ***sl-ParametersEUTRA1, sl-ParametersEUTRA2, sl-ParametersEUTRA3***This field includes IE of *SL-Parameters-v1430* (where *v2x-eNB-Scheduled-r14* and *V2X-SupportedBandCombination-r14* shall not be included), *SL-Parameters-v1530* (where *V2X-SupportedBandCombination-r1530* shall not be included) and *SL-Parameters-v1540* respectively defined in 36.331 [10]. It is used for reporting the per-UE capability for V2X sidelink communication. |

*End of Change*