**3GPP TSG-RAN WG2 Meeting #117e draftR2-2203160**

**Electronic, February, 2022**

**Agenda Item: 9.2.3.1**

**Source: OPPO**

**Title: Report of email discussion [Pre117-e][011][IoT-NTN] User plane Open Issues Input (OPPO)**

**Document for: Discussion and Decision**

# Introduction

This document is used to collect companies’ input to IoT NTN User Plane open issues identified after RAN2#116bis-e meeting and recommend proposals for RAN2#117e to discuss.

|  |  |
| --- | --- |
| Company | Delegate contact |
| COMPANY\_NAME | NAME ([email@address.com](mailto:email@address.com)) |
| ZTE | Ting Lu (lu.ting@zte.com.cn) |
| NEC | Yuhua Chen(yuhua.chen@emea.nec.com) |
| MediaTek | Abhishek Roy (Abhishek.Roy@mediatek.com) |
| Qualcomm | Bharat Shrestha (bshrestha@qti.qualcomm.com) |
| Nokia | Ping Yuan (Ping.1.Yuan@nokia-sbell.com) |
| Intel | Tangxun (xun.tang@intel.com) |
| Huawei, HiSilicon | Odile Rollinger (odile.rollinger@huawei.com) |
| Apple | Pavan Nuggehalli (pnuggehalli@apple.com) |
| Lenovo, Motorola Mobility | Min Xu (xumin13@lenovo.com) |
| CATT | Xiangdong Zhang ( [zhangxiangdong@catt.cn](mailto:zhangxiangdong@catt.cn) ) |
| OPPO | Haitao Li (lihaitao@oppo.com) |
| Xiaomi | Xiaowei jiang (jiangxiaowei@xiaomi.com) |
| Transsion Holdings | Wen Wu(wen.wu5@transsion.com) |
| InterDigital | Dylan Watts (dylan.watts@interdigital.com) |
| Ericsson | Robert.S.Karlsson AT ericsson.com |

# Discussion

For companies’ easy track, RAN2 agreements related to IoT NTN’s UP impact are copied below.

RAN2#115e:

|  |
| --- |
| * Start of ra-ResponseWindow is delayed by an offset. Postpone discussion on the offset value until further agreements regarding RACH are made in RAN1. * If the start of the RA Response window is accurately compensated by UE-eNB RTT and no extension of repetition is required, there is no need to extend the ra-ResponseWindowSize for IoT NTN. * Start of mac-ContentionResolutionTimer is delayed by an offset, (assumed equal to UE-eNB RTT). This can be revisited if RAN1 decides something that requires to change this. * If the start of mac-ContentionResolutionTimer is accurately compensated by UE-eNB RTT and no extension of repetition is required, there is no need to extend the mac-ContentionResolutionTimer for IoT NTN. * From RAN2 perspective, for UE with UE-specific pre-compensation as a baseline it is up to eNB implementation to ensure sufficient time on UE side for the Msg3 transmission for IoT NTN. * RAN2 assumes that TA information (FFS what) reporting by the UE on network enabling will be needed in IoT NTN. Expect RAN1 need to progress on this, and can maybe reuse NR NTN progress. FFS in which message this is provided. * UE-eNB RTT is taken into account when calculating the (UL) HARQ RTT timer. * RAN2 assumes that sr-ProhibitTimer need to be extended. Postpone treatment of sr-ProhibitTimer values until the NR NTN details have been decided. * From RAN2’s perspective, delayed start of pur-ResponseWindowTimer with UE-eNB RTT can be supported. This can be revised if RAN1 finds issues to support PUR that are not small. * pur-ResponseWindowSize is not extended for IoT NTN. * SPS is supported without modification for IoT NTN. * RAN2 confirm the SI agreement that the value range of the RLC t-Reordering timer will be extended to support IoT NTN. * Do not extend the PDCP discardTimer for NB-IoT over NTN. * FFS whether to extend the PDCP discardTimer for eMTC over NTN. * Do not extend PDCP t-Reordering for IoT NTN. |

RAN2#116e:

|  |
| --- |
| * The estimate of UE-eNB RTT is equal to the sum of UE’s TA and K\_mac, where the UE’s TA is given by , and K\_mac value is broadcasted by network. * RAN2 confirm that the start of mac-ContentionResolutionTimer is delayed by UE-eNB RTT in IoT NTN. * Any enhancements on (N)PRACH resource selection in IoT NTN will not be pursued in Rel-17. * An offset equal to UE-eNB RTT is added to the formula used for calculating the (UL) HARQ RTT timer in IoT NTN. * Support UE-specific TA reporting using MAC CE in Msg3/Msg5 for IoT NTN. * For IoT NTN, UE specific TA reporting during RACH procedure (MSG3/MSG5) in RRC IDLE is enabled/disabled by SI, similar with NR NTN. * Support TA reporting in RRC connected mode in IoT NTN. * UE-specific TA report uses MAC CE. * Support event-triggered for TA reporting in connected mode. Wait for NR NTN agreements for other triggers. * On how to extend RLC t-Reordering in IoT NTN, wait for NR NTN agreements and see if they can be reused. * Don’t change the L2 buffer requirement for IoT NTN (assume the network may need to limit the bit rate in order to not exceed L2 buffer). * The PDCP discardTimer should be extended to support eMTC over NTN. * If PDCP discardTimer is agreed to be extended to support eMTC over NTN, how to extend the timer value can wait for the conclusion for RLC t-reordering timer. * The ra window start offset is defined as sum (current offset, UE-eNB RTT) and current offset is defined in TS36.321 (FFS if applicable to NB-IoT 41ms offset) |

RAN2#116bis-e:

|  |
| --- |
| * Do not mandate Msg3 or Msg5 to include TA report MAC CE, and whether it can be included depends on the TB size of Msg3 or Msg5. * Reuse NR NTN’s TA reporting trigger event in IoT NTN, i.e., a TA offset threshold between current TA and the last successfully reported TA is used for event-triggered TA reporting. FFS for location used for TA reporting purpose. * Introduce a new MAC CE for provision of UE specific K\_offset and the size is fixed to 1 byte. FFS on the MAC CE’s name. * (Following NR NTN) Neither of the following options are supported “TA information requested by network”, “Periodical reporting of TA information” * (Following NR NTN) Upon reception of configuration or reconfiguration of TA reporting trigger event, if UE has not reported TA before, the UE triggers a TA reporting. FFS whether we need different behaviour for different re-configurations e.g. Handover. * On the RAR window’s start offset for the case of NB-IoT 41ms offset: The RA window start offset defined as sum (current offset, UE-eNB RTT) is applied to the case of NB-IoT 41ms offset. |

## 2.1 MAC

### 2.1.1 K\_Offset MAC CE

*MAC CE’s name:*

In the current running CRs of 38.321 and 36.321, the name of “Differential UE-Specific K\_Offset MAC CE” has been used for the MAC CE corresponding K\_Offset. Companies can comment if this is agreeable and if not, please indicate the suggested name.

**Question 1: Do companies agree to use the name of “Differential UE-Specific K\_Offset MAC CE”?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Additional comments** |
| ZTE | Agree |  |
| NEC | Agree |  |
| MediaTek | Agree | We believe it is better to align with NR-NTN whenever possible. |
| Qualcomm | Agree |  |
| Nokia | Agree |  |
| Spreadtrum | Agree |  |
| Intel | Agree |  |
| Huawei. HiSilicon | see comment | No strong opinion and fine with aligning with NR  Still, it is a bit strange to say ‘UE-specific’. What else could it be ? Could we just name it ‘Differential K\_Offset MAC CE’ |
| Apple | Agree | Agree to align with NR NTN |
| Lenovo, Motorola Mobility | Agree | Align with NR NTN |
| CATT | Agree |  |
| OPPO | Agree | Fine to align with NR NTN. |
| CMCC | Agree |  |
| Xiaomi | Agree |  |
| Transsion Holdings | Agree | Follow with the conclusion of the NR NTN |
| InterDigital | Agree | Can follow NR |
| Ericsson | Disagree, align with NR NTN | We agree with Huawei, “specific” shall be left out of the name and UE can be left out of the name too if we call it “Differential Koffset”. We do not agree with the use of underscore in K\_Offset, RAN1 uses just Koffset in the NR NTN spec.  We propose “Differential Koffset MAC CE” and to align this with NR NTN WI. |

**[Rapporteur summary]:**

Agree: 16 (including Huawei who are fine with aligning with NR)

Disagree: 1

Rapporteur assumes that “UE-specific” is to differentiate from “cell-specific” K\_Offset which is broadcasted in SIB. Regarding “K\_Offset” or “Koffset”, please note that in the current NR NTN RRC running CR, both “Koffset” and “K\_offset” are used. In any case, these wordings should be updated to be aligned. Given vast majority’s views, following proposal is made.

**Proposal 1: (16/17) Align with NR NTN and use the name of “Differential UE-Specific K\_Offset MAC CE”.**

*MAC CE’s contents:*

Regarding MAC CE’s contents, NR NTN running CR has captured the following contents.

- Differential UE-Specific K\_Offset: This field contains the differential UE-specific K\_Offset. The length of the field is 8 bits.

Rapporteur assumes 36.321 can follow the same text.

**Question 2: Do companies agree to follow the same text as 38.321 running CR for the contents of the MAC CE corresponding K\_Offset, i.e. “This field contains the differential UE-specific K\_Offset. The length of the field is 8 bits.”?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Additional comments** |
| ZTE | Agree |  |
| NEC | See comment | It is better to clarify that it is the differential UE-specific K\_offset to the cell-specific K\_offset |
| MediaTek | Agree | We believe it is better to align with NR-NTN whenever possible. |
| Nokia | Agree |  |
| Spreadtrum | Agree |  |
| Intel | Agree |  |
| Huawei. HiSilicon | Agree | Agree to follow NR and have a MAC CE size of 8 bits. Still not sure that 8 bits are needed for the value, so some bits could be eventually reserved. |
| Apple | Agree |  |
| Lenovo, Motorola Mobility | Agree |  |
| CATT | Agree |  |
| OPPO | Agree | Fine to align with NR NTN. |
| CMCC | Agree | Align with NR NTN. |
| Xiaomi | Agree |  |
| Transsion Holdings | Agree |  |
| InterDigital | Agree | Can follow NR |
| Ericsson | Agree but align with NR NTN | Align with NR NTN, the needed field length is only 6 bits:  **Agreement**  The value range of the differential UE specific K\_offset provided in MAC CE is 0 – 63 ms. |

**[Rapporteur summary]:**

Agree: 15

One company proposes to clarify in spec that it is the differential UE-specific K\_offset to the cell-specific K\_offset.

Two companies state that the needed field length is only 6 bits.

**Proposal 2: (15/16) Align with NR NTN and capture the contents of Differential UE-Specific K\_Offset MAC CE as “Differential UE-Specific K\_Offset: This field contains the differential UE-specific K\_Offset. The length of the field is 8 bits”. FFS on whether to change “8 bits” to “6 bits” for both 36.321 and 38.321.**

*MAC CE’s LCID:*

Regarding the LCID for the MAC CE corresponding K\_Offset, two options are mentioned in [6], i.e. using a reserved LCID or repurposing an existing LCID. Note that there are currently 4 reserved LCID for LTE.

**Question 3: Which option do companies prefer for the LCID used for the MAC CE corresponding K\_Offset?**

* **Option 1: use a reserved LCID**
* **Option 2: repurpose an existing LCID (and which one?)**

|  |  |  |
| --- | --- | --- |
| **Company** | **Option** | **Additional comments** |
| ZTE | Option 1 |  |
| NEC | Option1 | Option 2 is also acceptable.  But slightly prefer to have option1 and in future when we introduce new MAC CE which is not used in NTN, we can repurpose this LCID |
| MediaTek | Option 1 | Option 1 is simple and easy to implement in standards. |
| Qualcomm | Option 1 |  |
| Nokia | None | Since there are only 4 reserved LCID left for LTE DL-SCH, it is better leave it for common usage feature/function. In NR NTN, eLCID is agreed to be used for the MAC CE for differential UE-specific K\_offset. IoT NTN can follow NR NTN solution. |
| Spreadtrum | Option 1 |  |
| Intel | option 1 |  |
| Huawei. HiSilicon | Option 1 |  |
| Apple | Option 1 |  |
| Lenovo, Motorola Mobility | Option 1 |  |
| CATT | Option 1 |  |
| OPPO | Option 1 |  |
| CMCC | Option1 |  |
| Xiaomi | Option 1 |  |
| Transsion Holdings | Option1 |  |
| InterDigital | Option 1 |  |
| Ericsson | Disagree | We prefer to align with NR NTN where an eLCID was selected.  There is only 4 reserved LCIDs left.  This is not a frequent signalling (for Leo 600 km Earth fixed cells, approximately 35 or 36 changes to the Koffset are needed during the maximum connection time of about 500 seconds if Koffset is updated as soon as possible).  We propose to use a reserved eLCID instead of a LCID. For the UE, this can be seen as if the CE was two octets with a one octet LCID. |

**[Rapporteur summary]:**

Option 1: 15

Disagree: 2 companies prefer to align with NR NTN and use a reserved eLCID instead of a LCID.

Considering vast majority support of option 1, following proposal is given.

**Proposal 3: (15/17) A reserved LCID is used for the Differential UE-Specific K\_Offset MAC CE.**

### 2.1.2 TA reporting MAC CE

*MAC CE’s name:*

In the current running CRs of 38.321 and 36.321, the name of “UE-specific TA Report MAC CE” has been used for the TA reporting MAC CE. Companies can comment if this is agreeable and if not, please indicate the suggested name.

**Question 4: Do companies agree to use the name of “UE-specific TA Report MAC CE”?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Additional comments** |
| ZTE | Agree |  |
| NEC | Agree |  |
| MediaTek | Agree | We believe it is better to align with NR-NTN whenever possible. |
| Nokia | Agree |  |
| Spreadtrum | Agree |  |
| Intel | Agree |  |
| Huawei. HiSilicon | see comment | No strong opinion and fine with aligning with NR  Still, it is a bit strange to say ‘UE-specific’. What else could it be? The name in the RAN1 spreadsheet is ‘TA report’ |
| Apple | Agree |  |
| Lenovo, Motorola Mobility | Agree |  |
| CATT | Agree |  |
| OPPO | Agree | Fine to align with NR NTN. |
| CMCC | Agree |  |
| Xiaomi | Prefer to remove specific | In RAN1, UE specific TA refers to service link RTT. Full TA refers to UE’s TA. Thus, we prefer to use “UE’s TA” instead. |
| Transsion Holdings | Agree |  |
| InterDigital | Agree with comment | Note: MAC CE name has been revised to “**UE-specific TA MAC CE”** in latest “noted” version of running NR MAC CR |
| Ericsson | Disagree | Shall be aligned with NR NTN.  We propose to use “Timing Advance Report MAC CE” instead as RAN2/RAN1 decided to report the TA and not just the “UE specific” part of the TA. |

**[Rapporteur summary]:**

14 companies agree to align with NR NTN. 38.321’s rapporteur indicates that “UE-specific TA MAC CE” in the latest “noted” version of running NR MAC CR.

1 company prefers to use “UE’s TA”.

1 company proposes to use “Timing Advance Report MAC CE”.

**Proposal 4: (14/16) Align with NR NTN and use the name of “UE-specific TA MAC CE”.**

*MAC CE’s contents:*

Regarding TA reporting MAC CE’s contents, NR NTN running CR has captured the following contents.

- UE-specific TA: This field contains the UE estimate of the full UE-specific TA (i.e., T\_TA as defined in the UE’s TA formula). The length of the field is 16 bits.

Rapporteur assumes 36.321 can follow the same text.

**Question 5: Do companies agree to follow the same text as 38.321 running CR for the contents of the TA reporting MAC CE, i.e. “This field contains the UE estimate of the full UE-specific TA (i.e., T\_TA as defined in the UE’s TA formula). The length of the field is 16 bits.”?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Additional comments** |
| ZTE | Agree |  |
| NEC | Agree |  |
| MediaTek | Agree | We believe it is better to align with NR-NTN whenever possible. |
| Nokia | Agree |  |
| Spreadtrum | Agree |  |
| Intel | Agree |  |
| Huawei, HiSilicon | Agree | Agree to follow NR |
| Apple | Agree |  |
| Lenovo, Motorola Mobility | Agree |  |
| CATT | Agree |  |
| OPPO | Agree | Fine to align with NR NTN. |
| CMCC | Agree |  |
| Xiaomi | Agree |  |
| Transsion Holdings | Agree |  |
| InterDigital | Agree | Follow NR NTN |
| Ericsson | Disagree | Shall be aligned with NR NTN WI. Further, RAN1 have provided more information on how to round the TA.  We propose  - Timing Advance: The Timing Advance field indicates the least integer number of subframes greater than or equal to the Timing Advance value (see TS 36.2XX section Y.Y.Y). The length of the field is 16 bits. |

**[Rapporteur summary]:**

15 companies agree to align with NR NTN. 1 company provides some further detailed wording suggestions. Considering vast majority’s views, following proposal is given.

**Proposal 5: (15/16) Align with NR NTN and capture the contents of UE-specific TA MAC CE as “UE-specific TA: This field contains the UE estimate of the full UE-specific TA (i.e., T\_TA as defined in the UE’s TA formula). The length of the field is 16 bits”.**

*MAC CE’s LCID:*

Regarding the LCID for the TA reporting MAC CE, two options are proposed in [3][6][8], i.e. using a reserved LCID or repurposing an existing LCID. Note that there are currently 2 reserved LCID for LTE.

**Question 6: Which option do companies prefer for the LCID used for the TA reporting MAC CE?**

* **Option 1: use a reserved LCID**
* **Option 2: repurpose an existing LCID (and which one?)**

|  |  |  |
| --- | --- | --- |
| **Company** | **Option** | **Additional comments** |
| ZTE | Option 1 or Option 2 | Option 1 is simple.  As there are only two reserved LCID in uplink which are precious, we have sympathy with the analysis in [6] and are acceptable to Option 2. |
| NEC | Option1 | Option 2 is also acceptable.  But slightly prefer to have option1 and in future when we introduce new MAC CE which is not used in NTN, we can repurpose this LCID |
| MediaTek | Option 1 | Option 1 is simple and easy to implement in standards. |
| Qualcomm | Option 2 | Better not to use option 1 as only 2 codepoints are available. Will Dual Connectivity Power Headroom Report be ever applicable to IoT? |
| Nokia | None | Since there are only 2 reserved LCID left for LTE UL-SCH, it is better leave it for common usage feature/function. For Option2, repurpose an existing LCID can work but it makes the specification complex with many special cases which is related to system type detected by UE.  In our view, RAN2 may need to consider either using extended LCID or introduce a more general method to repurpose existing LCID (e.g. how to repurpose LCID for MAC CEs based on NW configuration). |
| Spreadtrum | Option 1 | Though the only two reserved LCID should be treated with caution, we may not need to worry too much as the extended LCID can be considered for some functionality in future. |
| Intel | option 1 |  |
| Huawei, HiSilicon | see comment. | If companies are fine to have only one reserved LCID left, then option 1 is simpler.  Otherwise, it should be possible to repurpose one, e.g. any of ‘10010’ (AUL confirmation), ‘10011’ (AUL confirmation), ‘10110’ (Truncated Sidelink BSR), ‘10111’ (Sidelink BSR) and ‘11000’ (Dual Connectivity Power Headroom Report) can be used for IOT NTN. |
| Apple | Option 1 | But if majority think option 2 is better, we can go with that too. |
| Lenovo, Motorola Mobility | Option 1 |  |
| CATT | Option 1 |  |
| OPPO | Option 1 | We slightly prefer option 1.  Option 2 is also acceptable. |
| CMCC | Option1 |  |
| Xiaomi | Option 1 |  |
| Transsion Holdings | Option1 |  |
| InterDigital | Option 1 |  |
| Ericsson | Option 1 | This new MAC CE for TA reports is of high importance as it may be included in the Msg3 during random access. The overhead is critical for the coverage, therefore it is better to use one of the two reserved LCIDs instead of the longer eLCIDs or repurposing an existing LCID.  We have however sympathy for the drawback leaving only one LCID for future functionality, but there are of course the eLCIDs and the possibility of future functionality to repurpose the LCID for TA report MAC CE… |

**[Rapporteur summary]:**

Option 1: 15

Option 2: 6 (including those companies who can also accept option 2)

Considering vast majority’s support for option 1, following proposal is given.

**Proposal 6: (15/17) A reserved LCID is used for the UE-specific TA MAC CE.**

*MAC CE’s logical channel priority:*

In NR NTN, logical channel priority of the TA reporting MAC CE has been agreed as below.

|  |
| --- |
| - C-RNTI MAC CE or data from UL-CCCH;  - Configured Grant Confirmation MAC CE or MAC CEs for BFR or Multiple Entry Configured Grant Confirmation MAC CE;  - Sidelink Configured Grant Confirmation MAC CE;  - LBT failure MAC CE;  - MAC CE for UE-Specific TA Report;  - MAC CE for SL-BSR prioritized according to clause 5.22.1.6;  - MAC CE for BSR, with exception of BSR included for padding;  - Single Entry PHR MAC CE or Multiple Entry PHR MAC CE;  - MAC CE for the number of Desired Guard Symbols;  - MAC CE for Pre-emptive BSR;  - MAC CE for SL-BSR, with exception of SL-BSR prioritized according to clause 5.22.1.6 and SL-BSR included for padding;  - data from any Logical Channel, except data from UL-CCCH;  - MAC CE for Recommended bit rate query;  - MAC CE for BSR included for padding;  - MAC CE for SL-BSR included for padding. |

Below is the list of MAC Ces in 36.321.

|  |
| --- |
| - MAC control element for C-RNTI or data from UL-CCCH;  - MAC control element for DPR;  - MAC control element for SPS confirmation;  - MAC control element for AUL confirmation;  - MAC control element for BSR, with exception of BSR included for padding;  - MAC control element for PHR, Extended PHR, or Dual Connectivity PHR;  - MAC control element for Sidelink BSR, with exception of Sidelink BSR included for padding;  - MAC control element for DCQR and AS RAI, with exception of when DCQR is to be included in Msg3;  - data from any Logical Channel, except data from UL-CCCH;  - MAC control element for DCQR and AS RAI, when DCQR is to be included in Msg3;  - MAC control element for Recommended bit rate query;  - MAC control element for BSR included for padding;  - MAC control element for Sidelink BSR included for padding. |

Rapporteur assumes LTE can follow the same priority as NR and propose that TA report MAC CE is put between “MAC control element for AUL confirmation” and “MAC control element for BSR, with exception of BSR included for padding”. Companies can comment if this is agreeable, and if not, please indicate the suggested order.

**Question 7: Do companies agree to put TA report MAC CE between “MAC control element for AUL confirmation” and “MAC control element for BSR, with exception of BSR included for padding”?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Additional comments** |
| ZTE | Agree | Even we slightly prefer that BSR/DCQR can have higher priority, the current suggested sequence is also acceptable to us (e.g., fine to follow NR NTN). |
| NEC | Agree |  |
| MediaTek | Agree |  |
| Qualcomm | Agree |  |
| Nokia | Agree |  |
| Spreadtrum | Agree |  |
| Intel | Agree |  |
| Huawei. HiSilicon | Agree |  |
| Apple | Agree |  |
| Lenovo, Motorola Mobility | Agree |  |
| CATT | Agree |  |
| OPPO | Agree |  |
| CMCC | Agree |  |
| Xiaomi | Agree |  |
| Transsion Holdings | Agree |  |
| InterDigital | Agree |  |
| Ericsson | Agree |  |

**[Rapporteur summary]:**

All companies agree to the proposed logical channel priority.

**Proposal 7: (17/17) On logical channel priority, put the UE-specific TA report MAC CE between “MAC control element for AUL confirmation” and “MAC control element for BSR, with exception of BSR included for padding”.**

### 2.1.3 Enable/disable indication applied for TA reporting in connected mode?

This is a common issue which is also being discussed in NR NTN. Note that the enable/disable indication in SI was initially introduced to control whether to trigger TA report during initial access (i.e. in Msg3/Msg5), and later RAN2 agreed to introduce event-triggered TA reporting in connected mode.

For connected mode UE TA reporting, we might need to look into following cases.

Case 1: re-establishment

During re-establishment procedure, the UE will read SIB from the target cell before initiating re-establishment request message and target cell’s SIB may include the enable/disable indication. If broadcasted and enabled, it seems reasonable for the UE to follow the indication in SI to trigger TA report during RACH in the re-establishment procedure. With this, network can configure the UE-specific K\_Offset at its earliest time.

**Question 8: Do companies agree that in re-establishment procedure, UE should follow the enable/disable indication broadcasted by the target cell’s SI to determine whether to trigger TA report during RACH?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Additional comments** |
| ZTE | Agree | After RLF, the UE would perform cell reselection and access to the target cell as that in idle state.  Therefore, it’s naturally that UE should follow the enable/disable indication broadcasted by the target cell’s SI to determine whether to trigger TA report during RACH. We assume no specification impacts for this part. |
| NEC | Agree |  |
| MediaTek | Agree | For NB-IoT this is more important, as there is no handover. |
| Qualcomm | Agree |  |
| Nokia | Agree | This seems reasonable to handle the case where UE re-establish in a new cell. |
| Spreadtrum | Agree |  |

|  |  |  |
| --- | --- | --- |
| Intel | Agree |  |
| Huawei, HiSilicon | Agree with comment | We should not mention RACH, if the report is in MSG5 which will be the case then this is no longer the RACH procedure. |
| Apple | Agree |  |
| Lenovo, Motorola Mobility | Agree |  |
| CATT | Agree |  |
| OPPO | Agree |  |
| CMCC | Agree |  |
| Xiaomi | Agree |  |
| InterDigital | Agree |  |
| Ericsson | Agree | Maybe the proposal can say:  **During RA procedure for RRC re-establishment procedure, the UE should trigger TA report if an indication is broadcasted by the target cell’s SI** |

**[Rapporteur summary]:**

All companies agree to the proposed UE behaviour. Wording suggestion from Ericsson looks good.

**Proposal 8: (17/17) During RA procedure for RRC re-establishment procedure, the UE should trigger TA report if an indication is broadcasted by the target cell’s SI.**

Case 2: handover

In the current handover procedure, handover command will include part of target cell’s essential system information for UE to perform handover access. In NTN, it can be assumed that some NTN specific system information would need to be provided in handover command, e.g. ephemeris, common TA, etc, for UE to do TA pre-compensation. Enable/disable indication could also be carried in handover command. Similar to initial access and re-establishment, it seems reasonable for the UE to follow that indication to trigger TA report or not during RACH. If enabled and TA report is triggered, target cell can provide the UE-specific K\_Offset at its earliest time.

**Question 9: Do companies agree that in handover procedure, UE should follow the target cell’s enable/disable indication carried in handover command to determine whether to trigger TA report during RACH?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Additional comments** |
| ZTE | Agree | For handover case, UE should follow the target cell’s enable/disable indication in SIB2 carried in handover command to determine whether to trigger TA report during RACH.  This is also aligned with the assumption that enable/disable indication in SIB is used to control whether to trigger TA report during RACH. |
| NEC | Agree |  |
| MediaTek | Agree for eMTC | There is no such handover in NB-IoT. |
| Qualcomm | Agree |  |
| Nokia | Agree |  |
| Spreadtrum | Agree |  |
| Intel | Agree |  |
| Huawei, HiSilicon | Agree with comment | We should not mention RACH, if the report is in MSG5 which will be the case, then this is no longer the RACH procedure |
| Apple | Agree |  |
| Lenovo, Motorola Mobility | Agree |  |
| CATT | Agree |  |
| OPPO | Agree |  |
| CMCC | Agree |  |
| Xiaomi | Agree |  |
| Transsion Holdings | Agree |  |
| InterDigital | Agree |  |
| Ericsson | Agree | We propose:  **During RA procedure for handover, the UE should trigger TA report if the target cell indicates this in the handover command** |

**[Rapporteur summary]:**

All companies agree to the proposed UE behaviour. Wording suggestion from Ericsson looks good.

**Proposal 9: (17/17) During RA procedure for handover, the UE should trigger TA report if the target cell indicates this in the handover command.**

Other than re-establishment and handover procedure, there seems no value to have extra control of TA reporting by checking enable/disable indication since network can have UE-specific TA reporting event configuration to control TA reporting in connected mode.

**Question 10: Do companies agree that other than re-establishment and handover procedure, TA reporting in connected mode is not controlled by enabling/disabling indication in SI?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Additional comments** |
| ZTE | Agree |  |
| NEC | Agree | It is better to have independent control of TA report at initial access (including handover and re-establishment if agreed) and at connected mode. This allows the implementation of no TA report at initial access stage but in connection mode, or vice versa |
| MediaTek | Agree |  |
| Qualcomm | Agree |  |
| Nokia | Agree with comment | For UE in connected mode, NW should anyway have the method to control whether UE should report the TA reporting. Other than re-establishment and handover procedure, if the SI flag is not pplicable then the TA reporting should be controlled in other means (e.g. configuration/re-configuration of TA reporting event in RRC) |
| Spreadtrum | Agree |  |
| Intel | Agree |  |
| Huawei. HiSilicon | Agree | For all other cases, the reporting is event triggered |
| Apple | Agree | Consistent with NR NTN, reporting should only be based on event triggering. |
| Lenovo, Motorola Mobility | Agree |  |
| CATT | Agree |  |
| OPPO | Agree |  |
| CMCC | Agree |  |
| Xiaomi | Agree |  |
| Transsion Holdings | Agree |  |
| InterDigital | Agree |  |
| Ericsson | Disagree | We think its fine to always send the TA report during RA if the target cell indicates in SI that it is wanted (the eNB anyway must make the Msg3 TBS sufficiently large as eNB cannot know if it is a UE in connected mode or idle mode doing RA, and the RA procedure is very seldom for each UE in a well-designed system).  It will be simpler to specify that all RA procedures triggers a TA report based on the target cells System Information. |

**[Rapporteur summary]:**

Agree: 16

Disagree: 1

**Proposal 10: (16/17) Other than re-establishment and handover procedure, TA reporting in connected mode is not controlled by enabling/disabling indication in SI.**

### 2.1.4 TA reporting upon configuration/reconfiguration

During RAN2#116bis-e online discussion, some comments are raised for the following proposal.

Proposal 5: Upon reception of configuration or reconfiguration of TA reporting trigger event, if UE has not reported TA before, the UE triggers a TA reporting.

Eventually proposal 5 is agreed with the following FFS added.

|  |
| --- |
| * (Following NR NTN) Upon reception of configuration or reconfiguration of TA reporting trigger event, if UE has not reported TA before, the UE triggers a TA reporting. FFS whether we need different behaviour for different re-configurations e.g. Handover. |

One issue related to handover seems to be that handover command may use delta-configuration and target cell may not provide explicit TA reporting event configuration in handover command. In such case, UE still has valid event configuration (i.e. the one used in the source cell), but based on above agreement, UE will not trigger TA report in the target cell (assuming target cell’s SI has disabled TA reporting during RACH) until the target cell reconfigures the triggering event.

Another issue is that UE may change cell during handover. Even if UE has reported TA to the source cell, the source cell TA may not be suitable to be compared to when evaluating the triggering condition in the target cell as it may lead to too late TA reporting. Before that late reporting, the target cell cannot know UE’s TA and thus cannot configure UE-specific K\_Offset properly.

Rapporteur understands that the above FFS may also apply to re-establishment and it can be resolved by adding explicit triggers in the spec that upon re-establishment or handover, UE triggers a TA reporting if the UE has a valid TA reporting event configuration. Companies please share views whether this is agreeable and if not, please indicate the suggested UE behaviours.

**Question 11: Do companies agree that upon re-establishment or handover, UE triggers a TA reporting if UE has a valid TA reporting event configuration? If you disagree, please indicate the suggested UE behaviours.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Additional comments** |
| ZTE | Disagree | For re-establishment case:  With reference to the summary from rapporteur, we can see the problematic case is that UE is configured event-trigger TA report in source cell while the TA report is disabled in SIB in target cell.  Considering the target cell may not need TA report in connected mode or may have different event configuration, we think the simpler or safer way may be that, only if the UE is (re)configured with new event by target cell via *RRCConnectionReestablishment* or *RRCConnectionReconfiguration*, UE can send TA report in connected mode. In other word, whether UE can send TA report after RRC reestablishment should follow explicit configuration in target cell and the event configuration in source cell cannot be reused.  We also agree with the rapporteur’s analysis and think the source cell TA is not suitable to be used as reference value for later comparison. Similar as that for UE in idle, no matter enable/disable in SIB, UE can record the TA value during RACH procedure in target cell as new reference.  One special sub-case may be that UE re-establish RRC connection in the same cell. It may be no issue even if UE continue to use the previous event-trigger configuration. But we prefer UE to have common process as that in re-establishing RRC connection in different cell case. We are open to discuss this.  For handover case (it’s only applicable to eMTC NTN):  We have similar thought as that for re-establishment, e.g., not to reuse the event configuration in source cell. Only if the UE is (re)configured with event by target cell via handover command, the UE can send TA report after handover. This may also related how to define the event configuration in reconfiguration message, e.g., use NEED OR or NEED ON.  Similarly, UE can record the TA value during RACH procedure in target cell as new reference for later comparison. |
| NEC | Disagree | we think we either agree that the TA report (trigger) upon HO and re-establishment follow the enable/disable bit, or we agree to follow the dedicated TA report event configuration, but not both |
| MediaTek | Disagree | We tend to agree with comments provided by ZTE, which is also aligned with our responses to Question 9 and Question 10. |
| Qualcomm | - | Not clear what is different from Q8, Q9 and Q10.  During RACH, the UE should follow SIB. But after that, if the UE has valid TA report configuration, the UE should follow it according to the event trigger. |
| Nokia | Disagree | In re-establishment or handover procedure, UE should follow the target cell’s SI enable/disable indication for TA reporting during RACH as discussed in Q8/Q9.  After UE enter RRC Connected state, whether UE triggers a TA reporting can follow below:   1. UE triggers a TA reporting upon reception of configuration or reconfiguration of TA reporting trigger event if the UE has not reported TA before. (i.e. new TA reporting trigger event should be indicated by target cell instead of using delta-configuration) 2. The update of TA reporting should be triggered by the TA update event. |
| Spreadtrum | Disagree | For the TA report in the target cell, it is only triggered by the enable/disable indication in SI or the new configured trigger event. |
| Intel | Disagree | same view as Nokia |
| Huawei, HiSilicon | Disagree | For these two cases, the UE follows the enabling/disabling indication in SI as per Q8/Q9. |
| Apple | Disagree | Same view as others above |
| Lenovo, Motorola Mobility | Disagree |  |
| CATT | Disagree | As discussed in Q8, UE will follow the indication in SI of target cell. |
| OPPO | Agree | Based on the comments from companies above, we clarify the difference between Q8/Q9 and Q11.  Q8/Q9 are related to TA reporting during RACH in re-establishment/handover. For initial access, RAN2 has agreed that TA reporting during RACH should follow the enable/disable indication. Then Q8/Q9 are just asking if re-establishment/handover should follow the same way as initial access with regards to TA reporting during RACH.  Q11 is related to TA reporting event configuration, i.e. how to trigger event-based reporting upon cell change (re-establishment or handover). RAN2 has agreed that “Upon reception of configuration or reconfiguration of TA reporting trigger event, if UE has not reported TA before, the UE triggers a TA reporting”, but it does not clearly state to which cell UE has not reported TA before. If UE has reported TA to the source cell, would UE still trigger TA reporting in the target cell if the UE knows it has a valid TA reporting event configuration on the target cell based on handover command?  For the question raised by ZTE on how to define the event configuration in reconfiguration message, e.g., use NEED OR or NEED ON. We think it is reasonable to define the TA event configuration as Need ON to support delta configuration. In this way, if a UE is configured with a TA reporting event in the source cell, and if the TA reporting event configuration is absent in the handover command, it means the UE is configured with the same TA reporting event in the target cell as that in the source cell. If the UE does not trigger a TA reporting, we may have the issue of TA report initiation, if unfortunately the target cell has set the indication in SI as “disabled”. In that case, UE may not trigger any TA report in the target cell. |
| CMCC | Disagree | Even if the TA reporting event configuration of the source cell is still valid, it is not suitable for the target cell. UE needs to obtain the enabling/disabling indication in SI as mentioned in above questions. |
| Xiaomi | Disagree | Should be based on the SI indication |
| InterDigital | Disagree | We understand the comments by OPPO and think it is probably worth clarifying the previous agreement to something like: *“Upon reception of configuration or reconfiguration of TA reporting trigger event, if UE has not reported TA to current serving cell before, the UE triggers a TA reporting”*. In this case if the UE receives a re-configuration in the target cell after completing handover then it would trigger a TA report. We note that most of the time the target cell will originate from the same satellite as the source cell, so the offset configuration will likely still be valid.  However, for the reporting during RACH we think we can just follow the SI indication. |
| Ericsson | Disagree | Simpler to always trigger a TA report during RA procedures if the target cells system information requests this, regardless of if there is any triggered TA reporting configured or not. |

**[Rapporteur summary]:**

Firstly, Q11 may not have been set very precisely and companies have some misunderstanding. The intention is not to repeat asking what is asked in Q8/Q9 (i.e. control by SI enable/disable), but is related to event-based TA reporting. As some companies understand, for cell change case, the source cell TA is not suitable to be used as reference value for later comparison. Clarification from IntelDigital on the previous agreement seems to work.

**Proposal 11a: RAN2 to clarify the previous agreement as: Upon reception of configuration or reconfiguration of TA reporting trigger event, if UE has not reported TA to current serving cell before, the UE triggers a TA reporting.**

Then the only left issue is: how should the UE trigger TA during handover, when handover command uses delta configuration. Some open issues are like:

1. Whether the event configuration in reconfiguration message uses NEED OR or NEED ON?
2. Whether target cell can use delta configuration for the event configuration in handover command?
3. If event configuration is absent in handover command and if target cell’s SI disables TA reporting during RACH, how should the UE trigger TA reporting after handover?

As these open issues are still not resolved, rapporteur suggests to have further discussion.

**Proposal 11b: RAN2 to further discuss below open issues.**

1. **Whether the TA reporting event configuration in reconfiguration message uses NEED OR or NEED ON?**
2. **Whether target cell can use delta configuration for the TA reporting event configuration in handover command?**
3. **If TA reporting event configuration is absent in handover command which supports delta configuration and if target cell’s SI disables TA reporting during RACH, how should the UE trigger TA reporting after handover?**

### 2.1.5 TA reporting aligned with NR NTN?

With the above RAN2#116bis-e agreements “Reuse NR NTN’s TA reporting trigger event in IoT NTN, i.e., a TA offset threshold between current TA and the last successfully reported TA is used for event-triggered TA reporting.”, the current running CR for 36.321 basically reused the formatting and progress of NR-NTN in Section “5.4.X UE-Specific TA Reporting”. During running CR discussion, some companies provided the following comments.

“We think that most of what is described below has not been fully agreed or even discussed. We suggest to remove the description and capture all the related agreements in Editor’s Notes. We suggest to add a MAC open issue on UE-specific TA reporting, covering e.g.:

* scope of enableTA-Report indication (only RACH during initial access, also Re-establishment, Handover, MAC triggered RACH)
* configuration of event-triggered reporting
* triggering during reconfiguration
* RRC-MAC interaction”

Rapporteur is not sure whether the intention of the above comments is to deviate anywhere from NR NTN, but it might be good to check companies’ views whether alignment with NR NTN should be targeted or any deviation would be favoured. If deviation is favoured, please indicate which part should be deviated from NR NTN.

**Question 12: Do companies agree that the threshold-based TA-Trigger needs to align with NR-NTN?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Additional comments** |
| ZTE | Agree | We are fine to reuse NR NTN agreements/description as much as possible.  The contents should also be aligned with our own agreements in IoT NTN. |
| NEC | Agree |  |
| MediaTek | Agree | We believe it is better to align with NR-NTN whenever possible. |
| Qualcomm | Agree |  |
| Nokia | Agree | No matter UE specific TA reporting or UE location reporting for TA purpose, we agree the threshold-based TA-trigger should be followed in IoT NTN. |
| Spreadtrum | Agree |  |
| Intel | Agree |  |
| Huawei, HiSilicon | Agree with comments | In principle, we agree with following NR agreements, Still, we need to check if there are applicable to IOT NTN. |
| Apple | Agree |  |
| Lenovo, Motorola Mobility | Agree |  |
| CATT | Agree |  |
| OPPO | Agree |  |
| CMCC | Agree only for TA value reporting | If reporting UE location information for TA reporting purpose in connected mode can be agreed(it is still FFS now in the chairman’s minutes), there are two options for the trigger condition:   * Option 1: Reuse the TA-based trigger condition * Option 2: Introduce location-based trigger condition   Although the majority’s view for this issue in NR NTN is that if reporting UE location information for TA reporting purpose in connected mode can be agreed, reuse the TA-based trigger condition.However, compared to the option 2, the frequency of TA value reporting will higher than that of option 1, which will cost higher uplink signalling load and power consumption than location reporting, especially considering the most IoT devices are stationery UEs, and large UL resource utilization for TA value reporting due to the repetition. Hence, we prefer to a solution which deviates from the NR NTN, i.e., introduce location-based trigger condition. |
| Xiaomi | Agree |  |
| Transsion Holdings | Agree |  |
| InterDigital | Agree |  |
| Ericsson | Agree |  |

**[Rapporteur summary]:**

All companies agree. For CMCC’s comments, we can of course discuss it after location reporting for TA reporting purpose is officially agreed.

**Proposal 12: (17/17) Threshold-based TA-Trigger will align with NR-NTN.**

### 2.1.6 Extension of *sr-ProhibitTimer*

How to extend *sr-ProhibitTimer* was discussed in [6]. It states that in NR, sr-ProhibitTimer is signalled as a value in the unit of ms so it is straightforward to extend the value range to take into account the RTT in NTN. In NB-IoT and eMTC, sr-ProhibitTimer is signalled as a value in number of SR period(s). The length of a SR period can take very different values depending on the configuration, i.e. 1ms, 2ms, 5ms, 10ms, 20ms, 40ms and 80ms for eMTC and 40ms, 80ms, 160ms, 240ms, 320ms, 640ms, 1280ms, 2560 ms, 5120 ms for NB-IoT. Thus it seems better to add an offset to the signalled value of the timer length.

**Question 13: Which option do companies prefer to extend *sr-ProhibitTimer* in IoT NTN?**

* **Option 1: add an offset to the legacy value**
* **Option 2: follow NR NTN and add more extended values (in number of SR periods)**

|  |  |  |
| --- | --- | --- |
| **Company** | **Option** | **Additional comments** |
| ZTE | Option 2 | It seems NR NTN still allow smaller value than RTT to be configured (technically, we think small value may be useless). Then maybe Option 1 is not so flexible.  Generally, the *sr-ProhibitTimer* is used to avoid UE frequently sending SR, e.g., after UE send the first SR, it should wait for some time and then send another SR. Some factors needs to be taken into account for setting this SR prohibit time, e.g., transmission RTT, the possible delay of UL grant scheduling for BSR in eNB side, e.g., due to resource congestion, and the loss of BSR and/or UL grant scheduling for BSR.  Yes, different from NR NTN, In NB-IoT and eMTC, sr-ProhibitTimer is signalled as a value in number of SR period(s).  If we only consider the possible delay of UL grant scheduling for BSR in eNB side, Option 1 may be ok. That is, the maximal time duration of the *sr-ProhibitTimer* in NTN could be UE-eNB RTT + 7 \* SR period.  But if also the loss of BSR and/or UL grant scheduling for BSR are considered, we think SR should be avoided during the possible multiple UL grant scheduling for BSR. Then the maximal time duration of the *sr-ProhibitTimer* may need to be multiple UE-eNB RTT. Following the legacy, such multiple factor can be with maximal value of 7, e.g., maximal time duration of the SR prohibit time can be 7 \* UE-eNB RTT.  Furthermore, with unit of SR period, when determine the value range of *sr-ProhibitTimer*, we need to do some conversion. We think we need to ensure the required maximum SR prohibit time can be achieved in the case of minimum SR period (1ms for eMTC and 40ms for NB-IoT). So the value range is calculated as follows:   * For eMTC:   + For LEO NTN, the maximum required SR prohibit time can be 32 (i.e., 4ms\*7/1ms=28, and ceiling to a value with 2^n=32) and minimum is 4ms. For LEO NTN, the maximum required SR prohibit time can be 4096 (i.e., 541ms\*7/1ms=3787, and ceiling to a value with 2^n=4096) and minimum is 541ms. After merge, we propose the value of *sr-ProhibitTimer* is extended to INTEGER (1...4096) * For NB-IoT:   + Mainly considering GEO NTN case, the maximum required SR prohibit time can be 128 (i.e., 541ms\*7/40ms=94.675, and ceiling a value with 2^n =128). We propose the value of *sr-ProhibitTimer* is extended to INTEGER (1...128)   With Option 2, we think the legacy configure rules which may take into account the network scheduling flexibility and tolerable UL/DL transmission loss can be kept as much as possible. |
| NEC | Option 2 | The motivation of having value less than RTT for NR is also valid for IoT NTN |
| MediaTek | Option 1 |  |
| Qualcomm | Option 2 |  |
| Nokia | Option 2 | Follow NR NTN is simple. E.g. introduce a new sr-ProhibitTimerExt-r17 IE to add more extended values. |
| Spreadtrum | Option 2 |  |
| Intel | option 2 |  |
| Huawei, HiSilicon | Option 1 | Option 2 does not make sense in IOT NTN, i.e. in NB-IoT IOT, it means extending the current range (1..8) to (1..4096) which seems ridiculous  The simplest approach is to signal an offset in addition to the existing value. This leaves every flexibility to the NW. |
| Apple | Option 2 | Seems to be the simpler and more flexible option. |
| Lenovo, Motorola Mobility | Option 2 |  |
| CATT | Option 2 |  |
| OPPO | Option 1 | The offset value should be in unit of SR periods. |
| CMCC | Option2 | Just follow NR NTN. |
| Xiaomi | Option 2 |  |
| Transsion Holdings | Option2 | Option2 seems have minimum effect on specification, and we think the actual added value will be in unit of SR periods(i.e. **extended value\* SR period**) |
| InterDigital | Option 2 |  |
| Ericsson | Option 1 | Option 1 and 2 are on the table for NR NTN |

**[Rapporteur summary]:**

Option 1: 4

Option 2: 13

Considering majority companies’ support for option 2, following proposal is given.

**Proposal 13: (13/17)** **Regarding how to extend sr-ProhibitTimer in IoT NTN, follow NR NTN and add more extended values (in number of SR periods).**

If option 1 is preferred, the next question is whether the offset is fixed (e.g. equal to UE-eNB RTT) or signalled by the network.

**Question 14: If option 1 is preferred in Q13, how to decide the offset?**

* **Option 1: the offset is fixed (e.g. equal to UE-eNB RTT)**
* **Option 2: the offset is signalled by the network**

|  |  |  |
| --- | --- | --- |
| **Company** | **Option** | **Additional comments** |
| ZTE | Option 2 | Even we prefer Option 2 in Q13, here we just give our opinion for Option 1. For simplicity, UE can just add a fixed offset (e.g. UE-eNB RTT) to the configured SR prohibit time by UE itself.  But network may want a smaller or larger value than RTT, then it may be better to let network configure this value. |
| MediaTek | Option 1 | A fixed offset of UE-eNB RTT should work fine. |
| Huawei, HiSilicon | Option2 | So the NW has the same flexibility as in NR, i.e. lower and higher values than the RTT are supported |
| OPPO | Option 1 | It is straightforward to extend the timer by UE-eNB RTT. |
| Ericsson | Option 2 | Agree with Huawei |

**[Rapporteur summary]:**

As no clear majority, this can be further discussed if option 1 is agreed.

**Proposal 14: RAN2 to further discuss whether the offset is fixed or configured by the network, if RAN2 agrees to add an offset to the legacy value of sr-ProhibitTimer.**

## RLC t-Reordering timer extension

NR NTN has agreed to extend t-Reassembly timer: {ms210, ms220, ms340, ms350, ms550, ms1100, ms1650, ms2200} and it is suggested that IoT NTN reuses the same values for IoT NTN.

**Question 15: Do companies agree to extend RLC t-Reordering timer by adding values {ms210, ms220, ms340, ms350, ms550, ms1100, ms1650, ms2200}?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Additional comments** |
| ZTE | Disagree | Please note the maximum value of RLC *t-Reordering* for eMTC and NB-IoT is already ms1600.  We think a double value may be needed. So simply suggest to add ms2200 and ms3200. |
| NEC | See common | We also think even longer values may be needed for IoT case |
| MediaTek | Disagree | Value range should be optimized for IoT. 200 ms and 1600 ms are already possible to signal. |
| Qualcomm | Disagree | Agree with MediaTek. |
| Nokia | See comments | The values in NR NTN is derived with the assumption of {1, 2, 3, 4, 8} as set of *nrofHARQ-Retransmissons* and max. RTD of LEO/GEO. It does not consider the channel repetitions. Hence the value for IoT NTN should consider the typical repetition numbers for different channels. |
| Spreadtrum | Disagree | In view of the maximum value of RLC t-Reordering, the adding value should be adapted to it. For example, the adding value range {ms1650, ms2200…} can be taken into account. |
| Intel | Disagree | same view with MTK and Nokia |
| Huawei, HiSilicon | Disagree | When eMTC and NB-IoT were introduced in Rel-13, a additional value ms1600 was introduced to deal with the long transmission in these technologies. Having a single value is a show that we did not need a very fine granularity.  For IOT NTN, we think adding many small values is not needed as the application are supposed to be delay tolerant so values {ms210, ms220, ms340, ms350} can be removed. ‘ms1650’ can also be removed as ms1600 is already supported. We may also need higher values, e.g.ms 3200.  Thus we propose {ms550, ms1100, ms2200, ms3200}. |
| Apple | Disagree | OK with Huawei’s proposal |
| Lenovo, Motorola Mobility | Disagree | Agree with ZTE. |
| CATT | Disagree | Agree with ZTE. |
| OPPO | Disagree | Agree with ZTE. |
| CMCC | Disagree | The value extended needs to match the IoT characteristic. And we should consider the HARQ retransmission. |
| Xiaomi | Disagree | Can simply add a ms3200. |
| Transsion Holdings | Disagree | Agree with ZTE |
| InterDigital | Disagree | Same view as ZTE, MTK and others |
| Ericsson | Disagree | Reuse the same maximum values as in NR NTN, already up to 2200 ms have been agreed. |

**[Rapporteur summary]:**

To add ms2200: 10

To add ms3200: 9

Some companies propose to optimize for IoT, e.g. 200 ms and 1600 ms are already possible to signal, ms210, ms220 and ms1650 may be skipped.

Some companies propose to add ms550 and ms1100.

Considering majority companies’ preference on ms2200 and ms3200, following proposal is given and RAN2 can further discuss if to add any other values between 200 ms and 1600 ms.

**Proposal 15: (9/17) On extending RLC t-Reordering timer for IoT NTN, RAN2 to add values ms2200 and ms3200. RAN2 can further discuss if to add any other values between ms200 and ms1600.**

## 2.3 PDCP discardTimer extension

NR NTN has agreed to introduce a new discardTimerExt-r17 IE with a new value ms2000 and it is suggested that eMTC over NTN reuses the same values for IoT NTN.

**Question 16: Do companies agree to introduce a new discardTimer value ms2000 for eMTC over NTN?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Agree/Disagree** | **Additional comments** |
| ZTE | Agree | Fine with ms2000.  But it may be better to add one more value for eMTC NTN e.g., ms3000 (just a double value of the existing maximum value of ms1500 for eMTC).  BTW, the existing maximum value of *discardTimer* for NB-IoT is ms81920, that’s enough. |
| NEC |  | same for above question |
| MediaTek | Agree | This is needed for eMTC only. |
| Qualcomm | Agree |  |
| Nokia | See comments | The PDCP discardTimer should be greater than the RLC t-Reordering timer, it can be decided after RAN2 conclude the value range of t-Reordering timer. |
| Spreadtrum | Agree | It is also feasible to introduce such value for eMTC over NTN. |
| Intel | Agree |  |
| Huawei, HiSilicon | FFS | If we introduce longer values, e.g. 3200 ms, for RLC t-reordering then we may need a higher value, e.g. 3000 ms |
| Apple | Agree |  |
| Lenovo, Motorola Mobility | Agree |  |
| CATT | Agree |  |
| OPPO | Agree |  |
| CMCC | Agree |  |
| Xiaomi |  | The timer should be larger than t-Reordering timer. |
| Transsion Holdings | Agree |  |
| InterDigital | Agree |  |
| Ericsson | Agree | We shall reuse the NR NTN values |

**[Rapporteur summary]:**

Agree: 13

Larger than t-Reordering timer: 3

Considering majority companies’ views, following proposal is given. Regarding the concerns on larger value than t-Reordering timer (if ms2200 or ms3200 is configured for t-Reordering timer), rapporteur assumes that network can configure discardTimer as “infinite” in such case.

**Proposal 16: (13/17) RAN2 to introduce a new discardTimer value ms2000 for eMTC over NTN.**

# 3. Summary and Proposals

Below is the list of summary proposals. Proposals that are common for IoT NTN and NR NTN are marked with “IoT NTN/NR NTN common”.

*Proposal for agreements:*

**Proposal 1: (16/17) Align with NR NTN and use the name of “Differential UE-Specific K\_Offset MAC CE”. (IoT NTN/NR NTN common)**

**Proposal 2: (15/16) Align with NR NTN and capture the contents of Differential UE-Specific K\_Offset MAC CE as “Differential UE-Specific K\_Offset: This field contains the differential UE-specific K\_Offset. The length of the field is 8 bits”. FFS on whether to change “8 bits” to “6 bits” for both 36.321 and 38.321. (IoT NTN/NR NTN common)**

**Proposal 3: (15/17) A reserved LCID is used for the Differential UE-Specific K\_Offset MAC CE.**

**Proposal 4: (14/16) Align with NR NTN and use the name of “UE-specific TA MAC CE”. (IoT NTN/NR NTN common)**

**Proposal 5: (15/16) Align with NR NTN and capture the contents of UE-specific TA MAC CE as “UE-specific TA: This field contains the UE estimate of the full UE-specific TA (i.e., T\_TA as defined in the UE’s TA formula). The length of the field is 16 bits”. (IoT NTN/NR NTN common)**

**Proposal 6: (15/17) A reserved LCID is used for the UE-specific TA MAC CE.**

**Proposal 7: (17/17) On logical channel priority, put the UE-specific TA report MAC CE between “MAC control element for AUL confirmation” and “MAC control element for BSR, with exception of BSR included for padding”.**

**Proposal 8: (17/17) During RA procedure for RRC re-establishment procedure, the UE should trigger TA report if an indication is broadcasted by the target cell’s SI. (IoT NTN/NR NTN common)**

**Proposal 9: (17/17) During RA procedure for handover, the UE should trigger TA report if the target cell indicates this in the handover command. (IoT NTN/NR NTN common)**

**Proposal 10: (16/17) Other than re-establishment and handover procedure, TA reporting in connected mode is not controlled by enabling/disabling indication in SI. (IoT NTN/NR NTN common)**

**Proposal 11a: RAN2 to clarify the previous agreement as: Upon reception of configuration or reconfiguration of TA reporting trigger event, if UE has not reported TA to current serving cell before, the UE triggers a TA reporting. (IoT NTN/NR NTN common)**

**Proposal 12: (17/17) Threshold-based TA-Trigger will align with NR-NTN.**

*Proposal for discussion:*

**Proposal 11b: RAN2 to further discuss below open issues. (IoT NTN/NR NTN common)**

1. **Whether the** **TA reporting event configuration in reconfiguration message uses NEED OR or NEED ON?**
2. **Whether target cell can use delta configuration for the TA reporting event configuration in handover command?**
3. **If TA reporting event configuration is absent in handover command which supports delta configuration and if target cell’s SI disables TA reporting during RACH, how should the UE trigger TA reporting after handover?**

**Proposal 13: (13/17)** **Regarding how to extend sr-ProhibitTimer in IoT NTN, follow NR NTN and add more extended values (in number of SR periods).**

**Proposal 14: RAN2 to further discuss whether the offset is fixed or configured by the network, if RAN2 agrees to add an offset to the legacy value of sr-ProhibitTimer.**

**Proposal 15: (9/17) On extending RLC t-Reordering timer for IoT NTN, RAN2 to add values ms2200 and ms3200. RAN2 can further discuss if to add any other values between ms200 and ms1600.**

**Proposal 16: (13/17) RAN2 to introduce a new discardTimer value ms2000 for eMTC over NTN.**

# 4. References

1. R2-2200253, Discussion on UP impact for IoT over NTN, OPPO
2. R2-2200692, Discussion on TA information reporting for IoT NTN, CATT
3. R2-2200698, Remaining FFSs on UP in IoT NTN, ZTE Corporation, Sanechips
4. R2-2200878, Remaining issues on UP aspects for IoT-NTN, CMCC
5. R2-2201010, On User Plane left issues for IoT NTN, Nokia, Nokia Shanghai Bell
6. R2-2201454, User plane for IOT NTN, Huawei, HiSilicon
7. R2-2201547, Location Reporting in RRC\_CONNECTED, Interdigital, Inc.
8. R2-2201631, User plane aspects of NB-IoT and LTE-M in NTNs, Ericsson