/******************************************************************************/
// @copyright   Copyright Notification
//   No part may be reproduced except as authorized by written permission.
//   The copyright and the foregoing restriction extend to reproduction in all media.
//   Trademark 2010, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TTA, TTC).
//   All rights reserved.
// @version: IWD_10wk37
/******************************************************************************/

/******************************************************************************/
// AUTOMATICLLY GENERATED MODUEL - DO NOT MODIFY
// $Date:
// $Author:
// $Rev:
/******************************************************************************/

module CDMA2000_Parameters {

  import from CommonDefs all;
  import from CDMA2000_CommonDefs all;
  
  //****************************************************************************
  // PIXIT Parameters
  //----------------------------------------------------------------------------
  modulepar {
      ColorCode_Type              px_ColorCode                := 64;              // @desc  Color code of the subnet to which the sectors belong; Same for all HRPD cells
      
      BandclassCDMA2000_Type      px_HRPD_BandClass           := 1;               // @desc  Band Class; Table 1.5-1 of C.S0057_D. Default value corresponds to 1.8 to 2.0 GHz PCS band
      
      ARFCN_ValueCDMA2000_Type    px_HRPD_ChannelNum_F14      := 225;             // @desc  Channel number of frequency 14
      
      ARFCN_ValueCDMA2000_Type    px_HRPD_ChannelNum_F15      := 525;             // @desc  Channel number of frequency 15
      
      ARFCN_ValueCDMA2000_Type    px_HRPD_ChannelNum_F16      := 825;             // @desc  Channel number of frequency 16
      
      SectorID_HRPD_Type          px_HRPD_SectorID_Cell15     := oct2bit('FEA00000000000000000000000000001'O);
                                                                                  // @desc  Sector ID of Cell 15; Clause 13.9 of C.S0024_B
      
      SectorID_HRPD_Type          px_HRPD_SectorID_Cell16     := oct2bit('FEA00000000000000000000000000002'O);
                                                                                  // @desc  Sector ID of Cell 16; Clause 13.9 of C.S0024_B
      
      SectorID_HRPD_Type          px_HRPD_SectorID_Cell17     := oct2bit('FEA00000000000000000000000000003'O);
                                                                                  // @desc  Sector ID of Cell 17; Clause 13.9 of C.S0024_B
      
      SectorID_HRPD_Type          px_HRPD_SectorID_Cell18     := oct2bit('FEA00000000000000000000000000004'O);
                                                                                  // @desc  Sector ID of Cell 18; Clause 13.9 of C.S0024_B
      
      OpenLoopAdjust_Type         px_OpenLoopAdjust           := 10;              // @desc  The value of open loop adjust to be used by access terminals in the open loop power estimate, expressed as an unsigned value in units of 1 dB. The value  used by the access terminal is -1 times the value of this field
      
  }
  
}
