/******************************************************************************/
// @copyright   Copyright Notification
//   No part may be reproduced except as authorized by written permission.
//   The copyright and the foregoing restriction extend to reproduction in all media.
//   Trademark 2010, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TTA, TTC).
//   All rights reserved.
// @version: IWD_10wk37
/******************************************************************************/

/******************************************************************************/
// AUTOMATICLLY GENERATED MODUEL - DO NOT MODIFY
// $Date:
// $Author:
// $Rev:
/******************************************************************************/

module UTRAN_Parameters {

  import from CommonDefs all;
  import from UTRAN_RRC_ASN1_Definitions language "ASN.1:1997" all;
  import from UTRAN_ASP_Definitions language "ASN.1:1997" all;
  import from UTRAN_TypeDefs all;
  
  //****************************************************************************
  // PIXIT Parameters
  //----------------------------------------------------------------------------
  modulepar {
      B1_Type                     px_BcapDataCompression      := '0'B;            // @desc  Data compression supported (used in the Bearer Capability).Default value: Default IMSI
                                                                                  // Reference to other Spec: 34.123-3, Table B.2
      
      B5_Type                     px_BcapFNUR                 := '00001'B;        // @desc  ###########################################################################################
                                                                                  // Reference to other Spec: 34.123-3, Table B.2
      
      B3_Type                     px_CipherAlg                := '001'B;          // @desc  NAS Ciphering Algorithm, Default value: (GEA/1) '001'B
                                                                                  // Reference to other Spec: 34.123-3, Table B.1
      
      Edch_PhysicalLayerCat_Type  px_EDCH_UE_Category_FDD     := 1;               // @desc  Reference to other Spec: 34.123-2, Table A.18a.2
      
      Edch_PhysicalLayerCat_Type  px_EDCH_UE_Category_TDD     := 1;               // @desc  Reference to other Spec: 34.123-2, Table A.18b.2
      
      charstring                  px_EmergencyCallNumber      := "112";           // @desc  Emergency Number used by UE to initiate an emergency call
                                                                                  // Reference to other Spec: 34.123-3, Table B.1.2
      
      integer                     px_FDD_OperationBand;                           // @desc  ###########################################################################################
                                                                                  // Reference to other Spec: 34.123-3, Table B.1
      
      B32_Type                    px_FRESH;                                       // @desc  no default value can be proposed
                                                                                  // Reference to other Spec: 34.123-3, Table B.1
      
      HSDSCH_physical_layer_category px_HSDSCH_UE_Category_FDD   := 5;            // @desc  Reference to other Spec: 34.123-2, Table A.18a.1
      
      HSDSCH_physical_layer_category px_HSDSCH_UE_Category_TDD   := 5;            // @desc  Reference to other Spec: 34.123-2, Table A.18b.1
      
      B1_Type                     px_MS_ClsmkESIND            := '0'B;            // @desc  Default Early Sending Indication
                                                                                  // Reference to other Spec: 34.123-3, Table B.1
      
      B2_Type                     px_MS_ClsmkRevLvl           := '10'B;           // @desc  Default Revision Level
                                                                                  // Reference to other Spec: 34.123-3, Table B.1
      
      octetstring                 px_PTMSI_SigDef             := 'AB1234'O;       // @desc  Default PTMSI signature (3 octets, 3GPP 24.008 /  10.5.5.8).
                                                                                  // Reference to other Spec: 34.123-3, Table B.1
      
      RRC_ServTested              px_RRC_PS_ServTested        := ps_Interactive;  // @desc  PS Service to be tested
                                                                                  // Reference to other Spec: 34.123-3, Table B.1
      
      SRNC_Identity               px_SRNC_Id                  := '000000000001'B; // @desc  SRNC Id
                                                                                  // Reference to other Spec: 34.123-3, Table B.1
      
      S_RNTI                      px_SRNTI                    := '00000000000000000001'B;
                                                                                  // @desc  S RNTI
                                                                                  // Reference to other Spec: 34.123-3, Table B.1
      
      integer                     px_UARFCN_D_High            := 10837;           // @desc  High Range downlink UARFCN value
                                                                                  // Reference to other Spec: 34.123-3, Table B.1
      
      integer                     px_UARFCN_D_Low             := 10563;           // @desc  Low Range downlink UARFCN value
                                                                                  // Reference to other Spec: 34.123-3, Table B.1
      
      integer                     px_UARFCN_D_Mid             := 10700;           // @desc  Mid Range downlink UARFCN value
                                                                                  // Reference to other Spec: 34.123-3, Table B.1
      
      integer                     px_UARFCN_High              := 9596;            // @desc  High Range UARFCN value for LCR TDD
                                                                                  // Reference to other Spec: ?
      
      integer                     px_UARFCN_Low               := 9504;            // @desc  Low Range UARFCN value for LCR TDD
                                                                                  // Reference to other Spec: ?
      
      integer                     px_UARFCN_Mid               := 9550;            // @desc  Mid Range UARFCN value for LCR TDD
                                                                                  // Reference to other Spec: ?
      
      CipheringAlgorithm_r7       px_UTRAN_CipheringAlgorithm := uea2;            // @desc  UTRAN Ciphering algorithm
                                                                                  // Supported values: uea0, uea1, uea2
      
  }
  
  //****************************************************************************
  // PICS Parameters
  //----------------------------------------------------------------------------
  modulepar {
      boolean                     pc_AutomaticAttachSwitchON  := true;            // @desc  Support of automatic PS attach procedure at switch on.
                                                                                  // Reference: 34.123-2 A.20/38
      
      boolean                     pc_Background               := false;           // @desc  UE Supports Background QoS class
                                                                                  // Reference: 34.123-2 A.6/4
      
      boolean                     pc_Band10_Supp              := false;           // @desc  UE supports Frequency Band 10
                                                                                  // Reference: 34.123-2 A.15/22
      
      boolean                     pc_Band1_Supp               := false;           // @desc  UE supports Frequency Band 1
                                                                                  // Reference: 34.123-2 A.15/2
      
      boolean                     pc_Band2_Supp               := false;           // @desc  UE supports Frequency Band 2
                                                                                  // Reference: 34.123-2 A.15/3
      
      boolean                     pc_Band3_Supp               := false;           // @desc  UE supports Frequency Band 3
                                                                                  // Reference: 34.123-2 A.15/14
      
      boolean                     pc_Band4_Supp               := false;           // @desc  UE supports Frequency Band 4
                                                                                  // Reference: 34.123-2 A.15/15
      
      boolean                     pc_Band5_Supp               := false;           // @desc  UE supports Frequency Band 5
                                                                                  // Reference: 34.123-2 A.15/16
      
      boolean                     pc_Band6_Supp               := false;           // @desc  UE supports Frequency Band 6
                                                                                  // Reference: 34.123-2 A.15/17
      
      boolean                     pc_Band7_Supp               := false;           // @desc  UE supports Frequency Band 7
                                                                                  // Reference: 34.123-2 A.15/18
      
      boolean                     pc_Band8_Supp               := false;           // @desc  UE supports Frequency Band 8
                                                                                  // Reference: 34.123-2 A.15/19
      
      boolean                     pc_Band9_Supp               := false;           // @desc  UE supports Frequency Band 9
                                                                                  // Reference: 34.123-2 A.15/20
      
      boolean                     pc_InterRAT_DL_CompressedModeRequired := true;  // @desc  UE supports DL DPCH compressed mode
                                                                                  // Reference: 34.123-2 A.18a/9a
      
      boolean                     pc_InterRAT_UL_CompressedModeRequired := true;  // @desc  UE supports UL DPCH compressed mode
                                                                                  // Reference: 34.123-2 A.18a/8a
      
      boolean                     pc_Interactive              := false;           // @desc  UE Supports Interactive QoS class
                                                                                  // Reference: 34.123-2 A.6/3
      
      boolean                     pc_Streaming                := false;           // @desc  UE Supports Streaming QoS class
                                                                                  // Reference: 34.123-2 A.6/2
      
  }
  
}
