    Log Viewer 341.0.0.0
    Copyright © 2019, Keysight Technologies

    LogFile            : TC_8_2_3_5_1_20190806_065919_DC_5A_n260A_PASS_v56.0.alf
    Created            : 06/08/2019 17:56:25

| Details | Summary

    OperatorName = KEYS_FR2

    KEYS_FR2

    iutData = Manufacturer =
    Model =
    Hardware Version =
    Software Version =
    Serial Number =

    Manufacturer =
    Model =
    Hardware Version =
    Software Version =
    Serial Number =

    swName = Conformance Toolset (LTE)
    swVersion = Version 53.0 (0480)
    swDetails

    Conformance Toolset (LTE)

    swName = TTCN-3 Compiler
    swVersion = Version 4.3  p0, Compile Date 2019-02-27 16:35:08
    swDetails

    TTCN-3 Compiler

    swName = Anite IMS Enabler
    swVersion = Not Installed
    swDetails

    Anite IMS Enabler

    swName = Conformance Toolset (LTE): Common Library
    swVersion = Version 53.0 (0480), Compile Date: Aug  5 2019 10:31:14
    swDetails

    Conformance Toolset (LTE): Common Library

    swName = Conformance Toolset (LTE): Codec Library
    swVersion = Version 53.0 (0480), Compile Date: Aug  5 2019 10:30:46
    swDetails

    Conformance Toolset (LTE): Codec Library

    swName = Conformance Toolset (LTE): Logging Library
    swVersion = Version 53.0 (0480), Compile Date: Aug  5 2019 10:30:31
    swDetails

    Conformance Toolset (LTE): Logging Library

    swName = Conformance Toolset (LTE): Test Management Library
    swVersion = Version 53.0 (0480), Compile Date: Aug  5 2019 10:30:23
    swDetails

    Conformance Toolset (LTE): Test Management Library

    swName = Conformance Toolset (LTE): Platform Timer Library
    swVersion = Version 53.0 (0480), Compile Date: Aug  5 2019 10:30:48
    swDetails

    Conformance Toolset (LTE): Platform Timer Library

    swName = Conformance Toolset (LTE): System Adaptor Library
    swVersion = Version 53.0 (0480), Compile Date: Aug  5 2019 10:30:34
    swDetails

    Conformance Toolset (LTE): System Adaptor Library

    swName = Conformance Toolset (LTE): LTE Codec Library
    swVersion = Version 53.0 (0480), Compile Date: Aug  5 2019 10:30:12
    swDetails

    Conformance Toolset (LTE): LTE Codec Library

    swName = Conformance Toolset (LTE): LTE System Adaptor Library
    swVersion = Version 53.0 (0480), Compile Date: Aug  5 2019 10:30:01
    swDetails

    Conformance Toolset (LTE): LTE System Adaptor Library

    swName = Conformance Toolset (LTE): LTE External Function Library
    swVersion = Version 53.0 (0480), Compile Date: Aug  5 2019 10:28:48
    swDetails

    Conformance Toolset (LTE): LTE External Function Library

    recordType = 31
    fileName
    descriptionId
    lineNo = 0
    information = ********************************************************************************
          THIS TESTCASE HAS BEEN BUILT IN RELEASE (WITH LOGGING ENABLED) MODE

          PLEASE TEST IN FULL CUSTOMER RELEASE MODE - ASAP
    ********************************************************************************

    ********************************************************************************
          THIS TESTCASE HAS BEEN BUILT IN RELEASE (WITH LOGGING ENABLED) MODE

          PLEASE TEST IN FULL CUSTOMER RELEASE MODE - ASAP
    ********************************************************************************

    recordType = 31
    fileName
    descriptionId
    lineNo = 0
    information = This log file was produced by a test case that is NOT validated and the test results are not verified to be suitable for certification testing.

    This log file was produced by a test case that is NOT validated and the test results are not verified to be suitable for certification testing.

    recordType = 22
    fileName
    descriptionId
    lineNo = 0
    information = TTCN-3 Ctrl File              : C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v56.0\ENDC_Testsuite\ENDC_Testsuite_v56_0.ttcn

    TTCN-3 Ctrl File              : C:\Program Files (x86)\Anite\Conformance Toolset\LTE\TTCN-3\ETSI\v56.0\ENDC_Testsuite\ENDC_Testsuite_v56_0.ttcn

    recordType = 22
    fileName
    descriptionId
    lineNo = 0
    information = XML Parameter File            : C:\Keysight\CT\TestProjects\K2_5GNR_Project\Test\2019-08-06 06.49.37\TC_8_2_3_5_1_20190806_065919_DC_5A_n260A_%V_v56.0.xml

    XML Parameter File            : C:\Keysight\CT\TestProjects\K2_5GNR_Project\Test\2019-08-06 06.49.37\TC_8_2_3_5_1_20190806_065919_DC_5A_n260A_%V_v56.0.xml

    recordType = 22
    fileName
    descriptionId
    lineNo = 0
    information = Test Case Started By          : CT_PSCS.DLL v1,0,3211,784

    Test Case Started By          : CT_PSCS.DLL v1,0,3211,784

    recordType = 22
    fileName
    descriptionId
    lineNo = 0
    information = EMMI Automation               : AT Enabled, MMI Enabled

    EMMI Automation               : AT Enabled, MMI Enabled

    Sender = RequestServer
    Text = Connected event from Controller SAT Controller PC Received

    RequestServer:Connected event from Controller SAT Controller PC Received

    Sender = RequestServer
    Text = State changed from RunningNotConnected to RunningConnected

    RequestServer:State changed from RunningNotConnected to RunningConnected

    Sender = RequestServer
    Text = Startup Requests Completed Successfully

    RequestServer:Startup Requests Completed Successfully

    Server State Change to RunningConnected

    Sender = RequestServer
    Text = Request received [!TC_8_2_3_5_1_ENDC]

    RequestServer:Request received [!TC_8_2_3_5_1_ENDC]

    Sender = RequestServer
    Text = Request [!TC_8_2_3_5_1_ENDC] not found in message file, does not meet Pass Through criteria

    RequestServer:Request [!TC_8_2_3_5_1_ENDC] not found in message file, does not meet Pass Through criteria

    Sender = RequestServer
    Text = Acknowledgment to SAT Contoller PC !OK

    RequestServer:Acknowledgment to SAT Contoller PC !OK

    Sender = SAT Controller PC
    Text = Sent "!OK"

    SAT Controller PC:Sent "!OK"

    Sender = RequestServer
    Text = Received !TC_8_2_3_5_1_ENDC from SAT Controller PC

    RequestServer:Received !TC_8_2_3_5_1_ENDC from SAT Controller PC

    Sender = RequestServer
    Text = Received !POWER_OFF from SAT Controller PC

    RequestServer:Received !POWER_OFF from SAT Controller PC

    Sender = RequestServer
    Text = Request received [!POWER_OFF]

    RequestServer:Request received [!POWER_OFF]

    Sender = RequestServer
    Text = [!POWER_OFF] Started

    RequestServer:[!POWER_OFF] Started

    summary = Message Mismatch: IPCAN_RAN_Type
    MATCH_MISMATCH
    	Message Mismatch: IPCAN_RAN_Type
    		IPCAN_RAN_Type = FBBA (6)

    Message Mismatch: IPCAN_RAN_Type

    Sender = !POWER_OFF
    Text = Sending AT+CFUN=0

    !POWER_OFF:Sending AT+CFUN=0

    Sender = !POWER_OFF
    Text = Checking if "AT+CFUN=0" was sent successfully

    !POWER_OFF:Checking if "AT+CFUN=0" was sent successfully

    Sender = Device Under Test
    Text = Sent "AT+CFUN=0"

    Device Under Test:Sent "AT+CFUN=0"

    Sender = RequestServer
    Text = Received AT+CFUN=0 from Device Under Test

    RequestServer:Received AT+CFUN=0 from Device Under Test

    Sender = RequestServer
    Text = Received OK from Device Under Test

    RequestServer:Received OK from Device Under Test

    Sender = !POWER_OFF
    Text = String AT+CFUN=0 has been transmitted successfully

    !POWER_OFF:String AT+CFUN=0 has been transmitted successfully

    Sender = SAT Controller PC
    Text = Sent "!OK"

    SAT Controller PC:Sent "!OK"

    Sender = RequestServer
    Text = [!POWER_OFF] Complete

    RequestServer:[!POWER_OFF] Complete

    UT_SYSTEM_REQ
    	Cmd
    		MMI
    			Cmd = 'POWER_OFF'
    			ParameterList = Omit
    	CnfRequired = CNF_REQUIRED (1)

    Sent from port: MTC_ENDC:Ut

    UT_COMMON_CNF
    	Result = True
    	ResultString = Omit

    Received on port: MTC_ENDC:Ut

    timerEvent = 6
    fileName = C:\Users\FETCTTEST\Desktop\Dev_TTCNs\Deepak\7.1.3.3.x\ENDC_IWD_19wk23\ENDC_Testsuite.ttcn
    testName = TC_8_2_3_5_1_ENDC
    lineNo = 1760
    outStr = Timer: t_GuardTimer, Duration: 360s, Started: 06:59:54

    Timer: t_GuardTimer, Duration: 360s, Started: 06:59:54

    ConstraintMismatch::Received:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_8_2_3_5_1_ENDC'
    ConstraintMismatch::Expected:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_7_*'

    Message Mismatch: CharacterStringType

    ConstraintMismatch::Received:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_8_2_3_5_1_ENDC'
    ConstraintMismatch::Expected:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_7_*'

    Message Mismatch: CharacterStringType

    ConstraintMismatch::Received:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_8_2_3_5_1_ENDC'
    ConstraintMismatch::Expected:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_7_*'

    Message Mismatch: CharacterStringType

    ConstraintMismatch::Received:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_8_2_3_5_1_ENDC'
    ConstraintMismatch::Expected:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_7_*'

    Message Mismatch: CharacterStringType

    ConstraintMismatch::Received:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_8_2_3_5_1_ENDC'
    ConstraintMismatch::Expected:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_7_*'

    Message Mismatch: CharacterStringType

    ConstraintMismatch::Received:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_8_2_3_5_1_ENDC'
    ConstraintMismatch::Expected:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_7_*'

    Message Mismatch: CharacterStringType

    ConstraintMismatch::Received:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_8_2_3_5_1_ENDC'
    ConstraintMismatch::Expected:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_7_*'

    Message Mismatch: CharacterStringType

    ConstraintMismatch::Received:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_8_2_3_5_1_ENDC'
    ConstraintMismatch::Expected:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_7_*'

    Message Mismatch: CharacterStringType

    ConstraintMismatch::Received:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_8_2_3_5_1_ENDC'
    ConstraintMismatch::Expected:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_7_*'

    Message Mismatch: CharacterStringType

    ConstraintMismatch::Received:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_8_2_3_5_1_ENDC'
    ConstraintMismatch::Expected:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_7_*'

    Message Mismatch: CharacterStringType

    ConstraintMismatch::Received:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_8_2_3_5_1_ENDC'
    ConstraintMismatch::Expected:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_7_*'

    Message Mismatch: CharacterStringType

    ConstraintMismatch::Received:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_8_2_3_5_1_ENDC'
    ConstraintMismatch::Expected:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_7_*'

    Message Mismatch: CharacterStringType

    ConstraintMismatch::Received:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_8_2_3_5_1_ENDC'
    ConstraintMismatch::Expected:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_7_*'

    Message Mismatch: CharacterStringType

    ConstraintMismatch::Received:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_8_2_3_5_1_ENDC'
    ConstraintMismatch::Expected:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_7_*'

    Message Mismatch: CharacterStringType

    ConstraintMismatch::Received:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_8_2_3_5_1_ENDC'
    ConstraintMismatch::Expected:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_7_*'

    Message Mismatch: CharacterStringType

    BCCH-BCH-Message
    	message
    		dl-Bandwidth = n25
    		phich-Config
    			phich-Duration = normal
    			phich-Resource = one
    		systemFrameNumber = 00000000
    		schedulingInfoSIB1-BR-r13 = 0
    		spare = 00000

    MasterInformationBlock

    BCCH-DL-SCH-Message
    	message = c1 = systemInformationBlockType1 =
    		cellAccessRelatedInfo
    			plmn-IdentityList = SEQUENCE OF PLMN-IdentityInfo
    				PLMN-IdentityInfo(1)
    					plmn-Identity
    						mcc = SEQUENCE OF MCC-MNC-Digit
    							MCC-MNC-Digit(1) = 0
    							MCC-MNC-Digit(2) = 0
    							MCC-MNC-Digit(3) = 1
    						mnc = SEQUENCE OF MCC-MNC-Digit
    							MCC-MNC-Digit(1) = 0
    							MCC-MNC-Digit(2) = 1
    					cellReservedForOperatorUse = notReserved
    			trackingAreaCode = 0000000000000001
    			cellIdentity = 0000000000000000000100000000
    			cellBarred = notBarred
    			intraFreqReselection = notAllowed
    			csg-Indication = FALSE
    		cellSelectionInfo
    			q-RxLevMin = -53
    		freqBandIndicator = 5
    		schedulingInfoList = SEQUENCE OF SchedulingInfo
    			SchedulingInfo(1)
    				si-Periodicity = rf16
    				sib-MappingInfo = SEQUENCE OF
    			SchedulingInfo(2)
    				si-Periodicity = rf32
    				sib-MappingInfo = SEQUENCE OF SIB-Type
    					SIB-Type(1) = sibType3
    		si-WindowLength = ms20
    		systemInfoValueTag = 0
    		nonCriticalExtension
    			nonCriticalExtension
    				ims-EmergencySupport-r9 = true

    systemInformationBlockType1

    BCCH-DL-SCH-Message
    	message = c1 = systemInformation =
    		criticalExtensions = systemInformation-r8 =
    			sib-TypeAndInfo = SEQUENCE OF CHOICE
    				CHOICE(1) = sib2 =
    					radioResourceConfigCommon
    						rach-ConfigCommon
    							preambleInfo
    								numberOfRA-Preambles = n52
    							powerRampingParameters
    								powerRampingStep = dB2
    								preambleInitialReceivedTargetPower = dBm-104
    							ra-SupervisionInfo
    								preambleTransMax = n6
    								ra-ResponseWindowSize = sf10
    								mac-ContentionResolutionTimer = sf48
    							maxHARQ-Msg3Tx = 4
    						bcch-Config
    							modificationPeriodCoeff = n4
    						pcch-Config
    							defaultPagingCycle = rf128
    							nB = oneT
    						prach-Config
    							rootSequenceIndex = 22
    							prach-ConfigInfo
    								prach-ConfigIndex = 3
    								highSpeedFlag = FALSE
    								zeroCorrelationZoneConfig = 5
    								prach-FreqOffset = 2
    						pdsch-ConfigCommon
    							referenceSignalPower = 18
    							p-b = 0
    						pusch-ConfigCommon
    							pusch-ConfigBasic
    								n-SB = 1
    								hoppingMode = interSubFrame
    								pusch-HoppingOffset = 4
    								enable64QAM = FALSE
    							ul-ReferenceSignalsPUSCH
    								groupHoppingEnabled = TRUE
    								groupAssignmentPUSCH = 0
    								sequenceHoppingEnabled = FALSE
    								cyclicShift = 0
    						pucch-ConfigCommon
    							deltaPUCCH-Shift = ds2
    							nRB-CQI = 2
    							nCS-AN = 6
    							n1PUCCH-AN = 0
    						soundingRS-UL-ConfigCommon = setup =
    							srs-BandwidthConfig = bw3
    							srs-SubframeConfig = sc0
    							ackNackSRS-SimultaneousTransmission = TRUE
    						uplinkPowerControlCommon
    							p0-NominalPUSCH = -85
    							alpha = al08
    							p0-NominalPUCCH = -117
    							deltaFList-PUCCH
    								deltaF-PUCCH-Format1 = deltaF0
    								deltaF-PUCCH-Format1b = deltaF3
    								deltaF-PUCCH-Format2 = deltaF0
    								deltaF-PUCCH-Format2a = deltaF0
    								deltaF-PUCCH-Format2b = deltaF0
    							deltaPreambleMsg3 = 4
    						ul-CyclicPrefixLength = len1
    					ue-TimersAndConstants
    						t300 = ms1000
    						t301 = ms1000
    						t310 = ms1000
    						n310 = n1
    						t311 = ms10000
    						n311 = n1
    					freqInfo
    						additionalSpectrumEmission = 1
    					timeAlignmentTimerCommon = sf750
    					plmn-InfoList-r15 = SEQUENCE OF PLMN-Info-r15
    						PLMN-Info-r15(1)
    							upperLayerIndication-r15 = true

    systemInformation

    BCCH-DL-SCH-Message
    	message = c1 = systemInformation =
    		criticalExtensions = systemInformation-r8 =
    			sib-TypeAndInfo = SEQUENCE OF CHOICE
    				CHOICE(1) = sib3 =
    					cellReselectionInfoCommon
    						q-Hyst = dB0
    					cellReselectionServingFreqInfo
    						threshServingLow = 0
    						cellReselectionPriority = 4
    					intraFreqCellReselectionInfo
    						q-RxLevMin = -53
    						presenceAntennaPort1 = FALSE
    						neighCellConfig = 01
    						t-ReselectionEUTRA = 0

    systemInformation

    BCCH-BCH-Message
    	message = mib =
    		systemFrameNumber = 000000
    		subCarrierSpacingCommon = scs30or120
    		ssb-SubcarrierOffset = 11
    		dmrs-TypeA-Position = pos2
    		pdcch-ConfigSIB1
    			controlResourceSetZero = 0
    			searchSpaceZero = 0
    		cellBarred = notBarred
    		intraFreqReselection = allowed
    		spare = 0

    mib

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		Cell
    			AddOrReconfigure
    				Basic
    					ConfigCapability = fullCell (2)
    					StaticCellInfo
    						Common
    							RAT
    								FDD = True
    							PhysicalCellId = 0
    							eNB_CellId = Omit
    							EutraBand = 5
    							CellTimingInfo
    								TcOffset = 0
    								Tcell = 0
    								SfnOffset = 0
    								HsfnOffset = 0
    						Downlink
    							Earfcn = 2525
    							Bandwidth = n25 (2)
    							RBSize = n_RB_SC_12 (0)
    							CyclicPrefix = normal (0)
    						Uplink
    							Earfcn = 20525
    							Bandwidth = n25 (2)
    							CyclicPrefix = normal (0)
    					PhysicalLayerConfigDL
    						AntennaGroup
    							AntennaInfoCommon
    								R8
    									antennaPortsCount = an1 (0)
    							AntennaPort
    								AntennaPort_Type
    									Id = 0
    									Config
    										AddOrReconfigure
    											PowerAttenuation = True
    											PropagationDelay = True
    						Pbch
    							RelativeTxPower
    								RA = 0
    								RB = 0
    						Pcfich
    							CfiValue = 3
    							RelativeTxPower
    								RA = 0
    								RB = 0
    						Phich
    							PhichConfig
    								R8
    									phich_Duration = normal (0)
    									phich_Resource = one (2)
    							RelativeTxPower
    								RA = 0
    								RB = 0
    						Pdcch
    							CommonSearchSpaceFormat = 2
    							UeSpecificSearchSpaceFormat = 1
    							PdcchCandidateList
    								PdcchCandidate_Type
    									RNTI = 0001000000000001'B
    									CCE_StartIndexList
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 12
    											CCE_StartIndex_UL = 14
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 14
    											CCE_StartIndex_UL = 16
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 12
    											CCE_StartIndex_UL = 14
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 14
    											CCE_StartIndex_UL = 16
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 10
    											CCE_StartIndex_UL = 12
    								PdcchCandidate_Type
    									RNTI = 0001000000110100'B
    									CCE_StartIndexList
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 12
    											CCE_StartIndex_UL = 14
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 16
    											CCE_StartIndex_UL = 18
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 14
    											CCE_StartIndex_UL = 16
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 10
    											CCE_StartIndex_UL = 12
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 18
    											CCE_StartIndex_UL = 8
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 16
    											CCE_StartIndex_UL = 18
    								PdcchCandidate_Type
    									RNTI = 0001000100010001'B
    									CCE_StartIndexList
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 16
    											CCE_StartIndex_UL = 18
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 10
    											CCE_StartIndex_UL = 12
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 14
    											CCE_StartIndex_UL = 16
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 10
    											CCE_StartIndex_UL = 12
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 14
    											CCE_StartIndex_UL = 16
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 18
    											CCE_StartIndex_UL = 8
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    								PdcchCandidate_Type
    									RNTI = 0001111111110001'B
    									CCE_StartIndexList
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 12
    											CCE_StartIndex_UL = 14
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 12
    											CCE_StartIndex_UL = 14
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 18
    											CCE_StartIndex_UL = 8
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 16
    											CCE_StartIndex_UL = 18
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 18
    											CCE_StartIndex_UL = 8
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 18
    											CCE_StartIndex_UL = 8
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 18
    											CCE_StartIndex_UL = 8
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    								PdcchCandidate_Type
    									RNTI = 0000010011010010'B
    									CCE_StartIndexList
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 10
    											CCE_StartIndex_UL = 12
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 10
    											CCE_StartIndex_UL = 12
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 14
    											CCE_StartIndex_UL = 16
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 14
    											CCE_StartIndex_UL = 16
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 10
    											CCE_StartIndex_UL = 12
    								PdcchCandidate_Type
    									RNTI = 0000100100101001'B
    									CCE_StartIndexList
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 10
    											CCE_StartIndex_UL = 12
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 12
    											CCE_StartIndex_UL = 14
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 14
    											CCE_StartIndex_UL = 16
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    								PdcchCandidate_Type
    									RNTI = 0000110110000000'B
    									CCE_StartIndexList
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 16
    											CCE_StartIndex_UL = 18
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 18
    											CCE_StartIndex_UL = 8
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 14
    											CCE_StartIndex_UL = 16
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 14
    											CCE_StartIndex_UL = 16
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 16
    											CCE_StartIndex_UL = 18
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 14
    											CCE_StartIndex_UL = 16
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    								PdcchCandidate_Type
    									RNTI = 0001000111010111'B
    									CCE_StartIndexList
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 16
    											CCE_StartIndex_UL = 18
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 14
    											CCE_StartIndex_UL = 16
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 16
    											CCE_StartIndex_UL = 18
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    								PdcchCandidate_Type
    									RNTI = 0001011000101110'B
    									CCE_StartIndexList
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 12
    											CCE_StartIndex_UL = 14
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 12
    											CCE_StartIndex_UL = 14
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 16
    											CCE_StartIndex_UL = 18
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 16
    											CCE_StartIndex_UL = 18
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 18
    											CCE_StartIndex_UL = 8
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    								PdcchCandidate_Type
    									RNTI = 0001101010000101'B
    									CCE_StartIndexList
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 16
    											CCE_StartIndex_UL = 18
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 16
    											CCE_StartIndex_UL = 18
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 16
    											CCE_StartIndex_UL = 18
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    										CCE_StartIndex_DL_UL_Type
    											CCE_StartIndex_DL = 8
    											CCE_StartIndex_UL = 10
    							RelativeTxPower
    								RA = 0
    								RB = 0
    						Pdsch
    							RelativeTxPower
    								RachResponse
    									RA = 0
    									RB = 0
    								BcchOnPdsch
    									RA = 0
    									RB = 0
    								PcchOnPdsch
    									RA = 0
    									RB = 0
    								CcchOnPdsch
    									RA = 0
    									RB = 0
    								DcchDtchOnPdsch
    									RA = -3
    									RB = -3
    								OcngOnPdsch = Omit
    							PDSCH_ConfigCommon
    								pdsch_maxNumRepetitionCEmodeA_r13 = Omit
    								pdsch_maxNumRepetitionCEmodeB_r13 = Omit
    						Pss
    							RelativeTxPower
    								RA = 0
    								RB = 0
    						Sss
    							RelativeTxPower
    								RA = 0
    								RB = 0
    						CSI_RS_Config = Omit
    						Pmch = Omit
    						Epdcch = Omit
    						DS_RS_Config = Omit
    					InitialCellPower
    						MaxReferencePower = -85
    						Attenuation
    							Off = True
    					BcchConfig
    						Pbch = True
    						Pdsch
    							Sib1Schedul
    								DciInfo
    									Format = dci_1C (6)
    									ResourceAllocType = ra_2_Distributed (3)
    									Modulation_1stCW = qpsk (1)
    									Modulation_2ndCW = unused (0)
    									FreqDomainSchedul
    										FirstRbIndex = 0
    										MaxRbCnt = 4
    									RedundancyVersionList
    										RedundancyVersion_Type = 0
    									RepetitionNumber = Omit
    									DCISubframeRepetitionNumber = Omit
    							SiSchedul
    								WindowLength = ms20 (5)
    								SiList
    									SiSchedul_Type
    										Periodicity = rf16 (1)
    										Window
    											SingleSiSchedul_Type
    												DciInfo
    													Format = dci_1C (6)
    													ResourceAllocType = ra_2_Distributed (3)
    													Modulation_1stCW = qpsk (1)
    													Modulation_2ndCW = unused (0)
    													FreqDomainSchedul
    														FirstRbIndex = 0
    														MaxRbCnt = 4
    													RedundancyVersionList
    														RedundancyVersion_Type = 2
    													RepetitionNumber = Omit
    													DCISubframeRepetitionNumber = Omit
    												SubframeOffset = 1
    									SiSchedul_Type
    										Periodicity = rf32 (2)
    										Window
    											SingleSiSchedul_Type
    												DciInfo
    													Format = dci_1C (6)
    													ResourceAllocType = ra_2_Distributed (3)
    													Modulation_1stCW = qpsk (1)
    													Modulation_2ndCW = unused (0)
    													FreqDomainSchedul
    														FirstRbIndex = 0
    														MaxRbCnt = 4
    													RedundancyVersionList
    														RedundancyVersion_Type = 2
    													RepetitionNumber = Omit
    													DCISubframeRepetitionNumber = Omit
    												SubframeOffset = 1
    								SegmentedSiList = Omit
    						BcchInfo
    							MIB
    								message_
    									dl_Bandwidth = n25 (2)
    									phich_Config
    										phich_Duration = normal (0)
    										phich_Resource = one (2)
    									systemFrameNumber = 00000000'B
    									schedulingInfoSIB1_BR_r13 = 0
    									systemInfoUnchanged_BR_r15 = False
    									spare = 0000'B
    							SIB1
    								message_
    									c1
    										systemInformationBlockType1
    											cellAccessRelatedInfo
    												plmn_IdentityList
    													PLMN_IdentityInfo
    														plmn_Identity
    															mcc
    																MCC_MNC_Digit = 0
    																MCC_MNC_Digit = 0
    																MCC_MNC_Digit = 1
    															mnc
    																MCC_MNC_Digit = 0
    																MCC_MNC_Digit = 1
    														cellReservedForOperatorUse = notReserved (1)
    												trackingAreaCode = 0000000000000001'B
    												cellIdentity = 0000000000000000000100000000'B
    												cellBarred = notBarred (1)
    												intraFreqReselection = notAllowed (1)
    												csg_Indication = False
    												csg_Identity = Omit
    											cellSelectionInfo
    												q_RxLevMin = -53
    												q_RxLevMinOffset = Omit
    											p_Max = Omit
    											freqBandIndicator = 5
    											schedulingInfoList
    												SchedulingInfo
    													si_Periodicity = rf16 (1)
    													sib_MappingInfo
    												SchedulingInfo
    													si_Periodicity = rf32 (2)
    													sib_MappingInfo
    														SIB_Type = sibType3 (0)
    											tdd_Config = Omit
    											si_WindowLength = ms20 (5)
    											systemInfoValueTag = 0
    											nonCriticalExtension
    												lateNonCriticalExtension = Omit
    												nonCriticalExtension
    													ims_EmergencySupport_r9 = true_ (0)
    													cellSelectionInfo_v920 = Omit
    													nonCriticalExtension
    														tdd_Config_v1130 = Omit
    														cellSelectionInfo_v1130 = Omit
    														nonCriticalExtension
    															cellAccessRelatedInfo_v1250 = Omit
    															cellSelectionInfo_v1250 = Omit
    															freqBandIndicatorPriority_r12 = Omit
    															nonCriticalExtension
    																hyperSFN_r13 = Omit
    																eDRX_Allowed_r13 = Omit
    																cellSelectionInfoCE_r13 = Omit
    																bandwidthReducedAccessRelatedInfo_r13 = Omit
    																nonCriticalExtension = Omit
    							SIs
    								BCCH_DL_SCH_Message
    									message_
    										c1
    											systemInformation
    												criticalExtensions
    													systemInformation_r8
    														sib_TypeAndInfo
    															SystemInformation_r8_IEs___0___oftype
    																sib2
    																	ac_BarringInfo = Omit
    																	radioResourceConfigCommon
    																		rach_ConfigCommon
    																			preambleInfo
    																				numberOfRA_Preambles = n52 (12)
    																				preamblesGroupAConfig = Omit
    																			powerRampingParameters
    																				powerRampingStep = dB2 (1)
    																				preambleInitialReceivedTargetPower = dBm_104 (8)
    																			ra_SupervisionInfo
    																				preambleTransMax = n6 (3)
    																				ra_ResponseWindowSize = sf10 (7)
    																				mac_ContentionResolutionTimer = sf48 (5)
    																			maxHARQ_Msg3Tx = 4
    																			preambleTransMax_CE_r13 = Omit
    																			rach_CE_LevelInfoList_r13 = Omit
    																			edt_SmallTBS_Subset_r15 = Omit
    																		bcch_Config
    																			modificationPeriodCoeff = n4 (1)
    																		pcch_Config
    																			defaultPagingCycle = rf128 (2)
    																			nB = oneT (2)
    																		prach_Config
    																			rootSequenceIndex = 22
    																			prach_ConfigInfo
    																				prach_ConfigIndex = 3
    																				highSpeedFlag = False
    																				zeroCorrelationZoneConfig = 5
    																				prach_FreqOffset = 2
    																		pdsch_ConfigCommon
    																			referenceSignalPower = 18
    																			p_b = 0
    																		pusch_ConfigCommon
    																			pusch_ConfigBasic
    																				n_SB = 1
    																				hoppingMode = interSubFrame (0)
    																				pusch_HoppingOffset = 4
    																				enable64QAM = False
    																			ul_ReferenceSignalsPUSCH
    																				groupHoppingEnabled = True
    																				groupAssignmentPUSCH = 0
    																				sequenceHoppingEnabled = False
    																				cyclicShift = 0
    																		pucch_ConfigCommon
    																			deltaPUCCH_Shift = ds2 (1)
    																			nRB_CQI = 2
    																			nCS_AN = 6
    																			n1PUCCH_AN = 0
    																		soundingRS_UL_ConfigCommon
    																			setup
    																				srs_BandwidthConfig = bw3 (3)
    																				srs_SubframeConfig = sc0 (0)
    																				ackNackSRS_SimultaneousTransmission = True
    																				srs_MaxUpPts = Omit
    																		uplinkPowerControlCommon
    																			p0_NominalPUSCH = -85
    																			alpha = al08 (5)
    																			p0_NominalPUCCH = -117
    																			deltaFList_PUCCH
    																				deltaF_PUCCH_Format1 = deltaF0 (1)
    																				deltaF_PUCCH_Format1b = deltaF3 (1)
    																				deltaF_PUCCH_Format2 = deltaF0 (1)
    																				deltaF_PUCCH_Format2a = deltaF0 (1)
    																				deltaF_PUCCH_Format2b = deltaF0 (1)
    																			deltaPreambleMsg3 = 4
    																		ul_CyclicPrefixLength = len1 (0)
    																		uplinkPowerControlCommon_v1020 = Omit
    																		rach_ConfigCommon_v1250 = Omit
    																		pusch_ConfigCommon_v1270 = Omit
    																		bcch_Config_v1310 = Omit
    																		pcch_Config_v1310 = Omit
    																		freqHoppingParameters_r13 = Omit
    																		pdsch_ConfigCommon_v1310 = Omit
    																		pusch_ConfigCommon_v1310 = Omit
    																		prach_ConfigCommon_v1310 = Omit
    																		pucch_ConfigCommon_v1310 = Omit
    																		highSpeedConfig_r14 = Omit
    																		prach_Config_v1430 = Omit
    																		pucch_ConfigCommon_v1430 = Omit
    																		prach_Config_v1530 = Omit
    																		ce_RSS_Config_r15 = Omit
    																		wus_Config_r15 = Omit
    																		highSpeedConfig_v1530 = Omit
    																		uplinkPowerControlCommon_v1540 = Omit
    																	ue_TimersAndConstants
    																		t300 = ms1000 (5)
    																		t301 = ms1000 (5)
    																		t310 = ms1000 (5)
    																		n310 = n1 (0)
    																		t311 = ms10000 (3)
    																		n311 = n1 (0)
    																		t300_v1310 = Omit
    																		t301_v1310 = Omit
    																		t310_v1330 = Omit
    																		t300_r15 = Omit
    																	freqInfo
    																		ul_CarrierFreq = Omit
    																		ul_Bandwidth = Omit
    																		additionalSpectrumEmission = 1
    																	mbsfn_SubframeConfigList = Omit
    																	timeAlignmentTimerCommon = sf750 (1)
    																	lateNonCriticalExtension = Omit
    																	ssac_BarringForMMTEL_Voice_r9 = Omit
    																	ssac_BarringForMMTEL_Video_r9 = Omit
    																	ac_BarringForCSFB_r10 = Omit
    																	ac_BarringSkipForMMTELVoice_r12 = Omit
    																	ac_BarringSkipForMMTELVideo_r12 = Omit
    																	ac_BarringSkipForSMS_r12 = Omit
    																	ac_BarringPerPLMN_List_r12 = Omit
    																	voiceServiceCauseIndication_r12 = Omit
    																	acdc_BarringForCommon_r13 = Omit
    																	acdc_BarringPerPLMN_List_r13 = Omit
    																	udt_RestrictingForCommon_r13 = Omit
    																	udt_RestrictingPerPLMN_List_r13 = Omit
    																	cIoT_EPS_OptimisationInfo_r13 = Omit
    																	useFullResumeID_r13 = Omit
    																	unicastFreqHoppingInd_r13 = Omit
    																	mbsfn_SubframeConfigList_v1430 = Omit
    																	videoServiceCauseIndication_r14 = Omit
    																	plmn_InfoList_r15
    																		PLMN_Info_r15
    																			upperLayerIndication_r15 = true_ (0)
    																	cp_EDT_r15 = Omit
    																	up_EDT_r15 = Omit
    																	idleModeMeasurements_r15 = Omit
    																	reducedCP_LatencyEnabled_r15 = Omit
    																	mbms_ROM_ServiceIndication_r15 = Omit
    														nonCriticalExtension = Omit
    								BCCH_DL_SCH_Message
    									message_
    										c1
    											systemInformation
    												criticalExtensions
    													systemInformation_r8
    														sib_TypeAndInfo
    															SystemInformation_r8_IEs___0___oftype
    																sib3
    																	cellReselectionInfoCommon
    																		q_Hyst = dB0 (0)
    																		speedStateReselectionPars = Omit
    																	cellReselectionServingFreqInfo
    																		s_NonIntraSearch = Omit
    																		threshServingLow = 0
    																		cellReselectionPriority = 4
    																	intraFreqCellReselectionInfo
    																		q_RxLevMin = -53
    																		p_Max = Omit
    																		s_IntraSearch = Omit
    																		allowedMeasBandwidth = Omit
    																		presenceAntennaPort1 = False
    																		neighCellConfig = 01'B
    																		t_ReselectionEUTRA = 0
    																		t_ReselectionEUTRA_SF = Omit
    																	lateNonCriticalExtension = Omit
    																	s_IntraSearch_v920 = Omit
    																	s_NonIntraSearch_v920 = Omit
    																	q_QualMin_r9 = Omit
    																	threshServingLowQ_r9 = Omit
    																	q_QualMinWB_r11 = Omit
    																	q_QualMinRSRQ_OnAllSymbols_r12 = Omit
    																	cellReselectionServingFreqInfo_v1310 = Omit
    																	redistributionServingInfo_r13 = Omit
    																	cellSelectionInfoCE_r13 = Omit
    																	t_ReselectionEUTRA_CE_r13 = Omit
    																	cellSelectionInfoCE1_r13 = Omit
    																	cellSelectionInfoCE1_v1360 = Omit
    																	cellReselectionInfoCommon_v1460 = Omit
    																	cellReselectionInfoHSDN_r15 = Omit
    																	cellSelectionInfoCE_v1530 = Omit
    																	crs_IntfMitigNeighCellsCE_r15 = Omit
    														nonCriticalExtension = Omit
    							SegmentedSIs = Omit
    						StopSib1Transmission = Omit
    					PcchConfig
    						DciInfo
    							Format = dci_1C (6)
    							ResourceAllocType = ra_2_Distributed (3)
    							Modulation_1stCW = qpsk (1)
    							Modulation_2ndCW = unused (0)
    							FreqDomainSchedul
    								FirstRbIndex = 4
    								MaxRbCnt = 2
    							RedundancyVersionList
    								RedundancyVersion_Type = 0
    							RepetitionNumber = Omit
    							DCISubframeRepetitionNumber = Omit
    						PCCH_Config_v13
    							paging_narrowBands_r13 = Omit
    							mpdcch_NumRepetition_Paging_r13 = Omit
    							nB_v1310 = Omit
    					CA_CellInitialConfig = Omit
    					BRBcchConfig = Omit
    					LAA_SCellConfiguration = Omit
    					LAA_SCellConfiguration_v1430 = Omit
    				Active
    					C_RNTI = 0001000000000001'B
    					PhysicalLayerConfigUL
    						Prach
    							R8andLater
    								prach_Config
    									rootSequenceIndex = 22
    									prach_ConfigInfo
    										prach_ConfigIndex = 3
    										highSpeedFlag = False
    										zeroCorrelationZoneConfig = 5
    										prach_FreqOffset = 2
    								prach_Config_v1310
    									rsrp_ThresholdsPrachInfoList_r13 = Omit
    									mpdcch_startSF_CSS_RA_r13 = Omit
    									prach_HoppingOffset_r13 = Omit
    									prach_ParametersListCE_r13 = Omit
    									initial_CE_level_r13 = Omit
    								prach_Config_v1430 = Omit
    						Pucch
    							Common
    								R8andLater
    									pucch_ConfigCommon
    										deltaPUCCH_Shift = ds2 (1)
    										nRB_CQI = 2
    										nCS_AN = 6
    										n1PUCCH_AN = 0
    									pucch_ConfigCommon_v1310
    										n1PUCCH_AN_InfoList_r13 = Omit
    										pucch_NumRepetitionCE_Msg4_Level0_r13 = Omit
    										pucch_NumRepetitionCE_Msg4_Level1_r13 = Omit
    										pucch_NumRepetitionCE_Msg4_Level2_r13 = Omit
    										pucch_NumRepetitionCE_Msg4_Level3_r13 = Omit
    							Dedicated
    								R8andLater
    									pucch_ConfigDedicated
    										ackNackRepetition
    											release = Null
    										tdd_AckNackFeedbackMode = Omit
    									pucch_ConfigDedicated_v1020 = Omit
    									pucch_ConfigDedicated_v1130 = Omit
    									pucch_ConfigDedicated_v1250 = Omit
    						Pusch
    							Common
    								R8andLater
    									pusch_ConfigCommon
    										pusch_ConfigBasic
    											n_SB = 1
    											hoppingMode = interSubFrame (0)
    											pusch_HoppingOffset = 4
    											enable64QAM = False
    										ul_ReferenceSignalsPUSCH
    											groupHoppingEnabled = True
    											groupAssignmentPUSCH = 0
    											sequenceHoppingEnabled = False
    											cyclicShift = 0
    									pusch_ConfigCommon_v1270 = Omit
    									pusch_ConfigCommon_v1310
    										pusch_maxNumRepetitionCEmodeA_r13 = Omit
    										pusch_maxNumRepetitionCEmodeB_r13 = Omit
    										pusch_HoppingOffset_v1310 = Omit
    							Dedicated
    								R8andLater
    									pusch_ConfigDedicated
    										betaOffset_ACK_Index = 9
    										betaOffset_RI_Index = 6
    										betaOffset_CQI_Index = 6
    									pusch_ConfigDedicated_v1020 = Omit
    									pusch_ConfigDedicated_v1130 = Omit
    									pusch_ConfigDedicated_v1250 = Omit
    						TimingAdvance
    							InitialValue = 0
    						SRS_UL_Config
    							Common
    								R8
    									setup
    										srs_BandwidthConfig = bw3 (3)
    										srs_SubframeConfig = sc0 (0)
    										ackNackSRS_SimultaneousTransmission = True
    										srs_MaxUpPts = Omit
    							Dedicated
    								R8andLater
    									soundingRS_UL_ConfigDedicated
    										setup
    											srs_Bandwidth = bw0 (0)
    											srs_HoppingBandwidth = hbw0 (0)
    											freqDomainPosition = 0
    											duration = True
    											srs_ConfigIndex = 20
    											transmissionComb = 0
    											cyclicShift = cs0 (0)
    									soundingRS_UL_ConfigDedicated_v1020 = Omit
    									soundingRS_UL_ConfigDedicatedAperiodic_r10 = Omit
    						SR_Config
    							R8andLater
    								schedulingRequestConfig
    									setup
    										sr_PUCCH_ResourceIndex = 20
    										sr_ConfigIndex = 30
    										dsr_TransMax = n4 (0)
    								schedulingRequestConfig_v1020 = Omit
    						CQI_ReportConfig
    							R8andLater
    								cqi_ReportConfig
    									cqi_ReportModeAperiodic = rm30 (3)
    									nomPDSCH_RS_EPRE_Offset = 0
    									cqi_ReportPeriodic
    										setup
    											cqi_PUCCH_ResourceIndex = 0
    											cqi_pmi_ConfigIndex = 25
    											cqi_FormatIndicatorPeriodic
    												widebandCQI = Null
    											ri_ConfigIndex = 483
    											simultaneousAckNackAndCQI = False
    								cqi_ReportConfig_v920 = Omit
    						UplinkPowerControlCommon
    							R8andLater
    								uplinkPowerControlCommon
    									p0_NominalPUSCH = -85
    									alpha = al08 (5)
    									p0_NominalPUCCH = -117
    									deltaFList_PUCCH
    										deltaF_PUCCH_Format1 = deltaF0 (1)
    										deltaF_PUCCH_Format1b = deltaF3 (1)
    										deltaF_PUCCH_Format2 = deltaF0 (1)
    										deltaF_PUCCH_Format2a = deltaF0 (1)
    										deltaF_PUCCH_Format2b = deltaF0 (1)
    									deltaPreambleMsg3 = 4
    								uplinkPowerControlCommon_v1020 = Omit
    								uplinkPowerControlCommonSCell_v1130 = Omit
    								uplinkPowerControlCommonPSCell_r12 = Omit
    						UplinkPowerControlDedicated
    							R8andLater
    								uplinkPowerControlDedicated
    									p0_UE_PUSCH = 0
    									deltaMCS_Enabled = en0 (0)
    									accumulationEnabled = True
    									p0_UE_PUCCH = 0
    									pSRS_Offset = 3
    									filterCoefficient = fc4 (4)
    								uplinkPowerControlDedicated_v1020 = Omit
    								pathlossReferenceLinking = Omit
    								uplinkPowerControlDedicated_v1130 = Omit
    								uplinkPowerControlDedicated_v1250 = Omit
    					RachProcedureConfig
    						RACH_ConfigCommon
    							R8andLater
    								rach_ConfigCommon
    									preambleInfo
    										numberOfRA_Preambles = n52 (12)
    										preamblesGroupAConfig = Omit
    									powerRampingParameters
    										powerRampingStep = dB2 (1)
    										preambleInitialReceivedTargetPower = dBm_104 (8)
    									ra_SupervisionInfo
    										preambleTransMax = n6 (3)
    										ra_ResponseWindowSize = sf10 (7)
    										mac_ContentionResolutionTimer = sf48 (5)
    									maxHARQ_Msg3Tx = 4
    									preambleTransMax_CE_r13 = Omit
    									rach_CE_LevelInfoList_r13 = Omit
    									edt_SmallTBS_Subset_r15 = Omit
    								rach_ConfigCommon_v1250 = Omit
    						RACH_ConfigDedicated = Omit
    						RachProcedureList
    							RachProcedure_Type
    								RAResponse
    									Ctrl
    										DciInfo
    											Format = dci_1C (6)
    											ResourceAllocType = ra_2_Distributed (3)
    											Modulation_1stCW = qpsk (1)
    											Modulation_2ndCW = unused (0)
    											FreqDomainSchedul
    												FirstRbIndex = 6
    												MaxRbCnt = 4
    											RedundancyVersionList
    												RedundancyVersion_Type = 0
    												RedundancyVersion_Type = 2
    												RedundancyVersion_Type = 3
    												RedundancyVersion_Type = 1
    												RedundancyVersion_Type = 0
    											RepetitionNumber = Omit
    											DCISubframeRepetitionNumber = Omit
    										Rar
    											List
    												RandomAccessResponseParameters_Type
    													RapId
    														Automatic = True
    													InitialGrant
    														HoppingFlag = 0'B
    														RB_Allocation = 0000000000'B
    														ModAndCodScheme = 1111'B
    														TPC_Command = 011'B
    														UL_Delay = 0'B
    														CQI_Req = 0'B
    													TimingAdvance = 0
    													TempC_RNTI
    														SameAsC_RNTI = True
    													InitialGrantCE_Mode = Omit
    										BackoffInd
    											None = True
    								ContentionResolutionCtrl
    									TCRNTI_Based
    										MacPdu
    											ContainedId
    												XorMask = 000000000000000000000000000000000000000000000000'B
    											ContainedRlcPdu
    												RlcPduCCCH = '60129B3E8603B579E89664307B3800064F1A0082818141E0'O
    					CcchDcchDtchConfig
    						MeasGapCtrl
    							None = True
    						DL
    							DciInfo
    								Auto
    									Format = dci_1 (3)
    									ResourceAllocType = ra_0 (0)
    									Modulation_1stCW = qam64 (3)
    									Modulation_2ndCW = unused (0)
    									FreqDomainSchedul
    										FirstRbIndex = 2
    										MaxRbCnt = 23
    									RedundancyVersionList
    										RedundancyVersion_Type = 0
    										RedundancyVersion_Type = 2
    										RedundancyVersion_Type = 3
    										RedundancyVersion_Type = 1
    										RedundancyVersion_Type = 0
    									RepetitionNumber = Omit
    									DCISubframeRepetitionNumber = Omit
    							AntennaInfo
    								R8andLater
    									antennaInfo
    										transmissionMode = tm1 (0)
    										codebookSubsetRestriction = Omit
    										ue_TransmitAntennaSelection
    											release = Null
    									antennaInfo_v920 = Omit
    							HarqProcessConfig
    								AllProcesses = True
    						UL
    							DciInfo
    								Imcs
    									Value = 9
    								TransRetransmissionList
    									UL_TransRetransmission_Type
    										NewTransmission = True
    								FreqDomainSchedul
    									FirstRbIndex = 0
    									Nprb = 25
    								Format = Omit
    								HarqProcessId = Omit
    								RepetitionNumber = Omit
    								DCISubframeRepetitionNumber = Omit
    								PUSCH_TriggerA = Omit
    								TimingOffset = Omit
    								NumberOfScheduledSubframes = Omit
    							Hopping
    								Deactivated = True
    							PUCCH_Synch
    								None = True
    							UL_GrantConfig
    								None = True
    						DrxCtrl
    							None = True
    						TtiBundling
    							R8 = False
    						CifPresence = Omit
    					ServingCellConfig = Omit
    					SciSchedulingConfig = Omit
    					EIMTA_Config = Omit
    					CE_Mode = Omit

    Sent from port: EUTRA_5GS_PTC:SYS

    SYSTEM_CTRL_CNF
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		Cell = True

    Received on port: EUTRA_5GS_PTC:SYS

    ConstraintMismatch::Received:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_8_2_3_5_1_ENDC'
    ConstraintMismatch::Expected:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_7_*'

    Message Mismatch: CharacterStringType

    ConstraintMismatch::Received:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_8_2_3_5_1_ENDC'
    ConstraintMismatch::Expected:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = 'TC_12_*'

    Message Mismatch: CharacterStringType

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		Cell
    			AddOrReconfigure
    				StaticResourceConfig
    					CellCapability = fullCell (2)
    					CarrierAggregation = None (3)
    				CellConfigCommon
    					C_RNTI = 4097
    					CellTimingInfo
    						TcOffset = 0
    						Tcell = 0
    						SfnOffset = 0
    						HsfnOffset = 0
    					InitialCellPower
    						MaxReferencePower = -79
    						Attenuation
    							Off = True
    				PhysicalLayer
    					Common
    						PhysicalCellId = 0
    						DuplexMode
    							TDD
    								Config
    									Common
    										R15
    											referenceSubcarrierSpacing = kHz120 (3)
    											pattern1
    												dl_UL_TransmissionPeriodicity = ms0p625 (1)
    												nrofDownlinkSlots = 3
    												nrofDownlinkSymbols = 10
    												nrofUplinkSlots = 1
    												nrofUplinkSymbols = 2
    												dl_UL_TransmissionPeriodicity_v1530 = Omit
    											pattern2 = Omit
    									Dedicated = Omit
    					Downlink
    						FrequencyInfoDL
    							R15
    								absoluteFrequencySSB = 2229499
    								frequencyBandList
    									FreqBandIndicatorNR = 260
    								absoluteFrequencyPointA = 2229237
    								scs_SpecificCarrierList
    									SCS_SpecificCarrier
    										offsetToCarrier = 0
    										subcarrierSpacing = kHz120 (3)
    										carrierBandwidth = 66
    										txDirectCurrentLocation_v1530 = Omit
    						SSPbchBlock
    							SubCarrierSpacing = kHz120 (3)
    							SubcarrierOffset = 11
    							Periodicity = ms20 (2)
    							HalfFrameOffset = 0
    							BurstConfig
    								BlockPattern = caseD (3)
    								Bitmap
    									longBitmap = 0100000000000000000000000000000000000000000000000000000000000000'B
    								BeamArray = Omit
    							RelativeTxPower
    								Pbch = 0
    								Pss = 0
    								Sss = 0
    								Dmrs = 0
    						PdschCellLevelConfig
    							DMRS_TypeA_Position = pos2 (0)
    							RateMatchPattern
    								PatternList = Omit
    								PatternListLteCrs = Omit
    							ServingCellConfig
    								R15
    									codeBlockGroupTransmission = Omit
    									xOverhead = Omit
    									nrofHARQ_ProcessesForPDSCH = n16 (5)
    									pucch_Cell = Omit
    									maxMIMO_Layers = Omit
    									processingType2Enabled = Omit
    						BWPs
    							ActiveBWP = 0
    							BwpArray
    								NR_DownlinkBWP_Type
    									Id = 0
    									BWP
    										R15
    											locationAndBandwidth = 17875
    											subcarrierSpacing = kHz120 (3)
    											cyclicPrefix = Omit
    									Pdcch
    										SearchSpaceArray
    											NR_BWP_SearchSpaceConfig_Type
    												TypeAndPriorityList
    													NR_SearchSpaceTypeAndPriority_Type
    														NR_SearchSpaceType_Type = cssType0 (0)
    														NR_SearchSpaceCandidatePriority_Type = 0
    													NR_SearchSpaceTypeAndPriority_Type
    														NR_SearchSpaceType_Type = cssType2 (3)
    														NR_SearchSpaceCandidatePriority_Type = 3
    												AggregationLevel = AggregationLevel4 (2)
    												SearchSpaceConfigAtUE
    													R15
    														searchSpaceId = 0
    														controlResourceSetId = 0
    														monitoringSlotPeriodicityAndOffset
    															sl160 = 1
    														duration = 2
    														monitoringSymbolsWithinSlot = 10000000000000'B
    														nrofCandidates
    															aggregationLevel1 = n0 (0)
    															aggregationLevel2 = n0 (0)
    															aggregationLevel4 = n4 (4)
    															aggregationLevel8 = n2 (2)
    															aggregationLevel16 = n1 (1)
    														searchSpaceType
    															common
    																dci_Format0_0_AndFormat1_0
    																dci_Format2_0 = Omit
    																dci_Format2_1 = Omit
    																dci_Format2_2 = Omit
    																dci_Format2_3 = Omit
    											NR_BWP_SearchSpaceConfig_Type
    												TypeAndPriorityList
    													NR_SearchSpaceTypeAndPriority_Type
    														NR_SearchSpaceType_Type = cssType1 (2)
    														NR_SearchSpaceCandidatePriority_Type = 2
    													NR_SearchSpaceTypeAndPriority_Type
    														NR_SearchSpaceType_Type = cssType3 (4)
    														NR_SearchSpaceCandidatePriority_Type = 4
    												AggregationLevel = AggregationLevel4 (2)
    												SearchSpaceConfigAtUE
    													R15
    														searchSpaceId = 1
    														controlResourceSetId = 1
    														monitoringSlotPeriodicityAndOffset
    															sl1 = Null
    														duration = Omit
    														monitoringSymbolsWithinSlot = 10000000000000'B
    														nrofCandidates
    															aggregationLevel1 = n0 (0)
    															aggregationLevel2 = n4 (4)
    															aggregationLevel4 = n2 (2)
    															aggregationLevel8 = n1 (1)
    															aggregationLevel16 = n0 (0)
    														searchSpaceType
    															common
    																dci_Format0_0_AndFormat1_0
    																dci_Format2_0 = Omit
    																dci_Format2_1 = Omit
    																dci_Format2_2 = Omit
    																dci_Format2_3 = Omit
    											NR_BWP_SearchSpaceConfig_Type
    												TypeAndPriorityList
    													NR_SearchSpaceTypeAndPriority_Type
    														NR_SearchSpaceType_Type = ussDL (5)
    														NR_SearchSpaceCandidatePriority_Type = 5
    													NR_SearchSpaceTypeAndPriority_Type
    														NR_SearchSpaceType_Type = ussUL (6)
    														NR_SearchSpaceCandidatePriority_Type = 9
    												AggregationLevel = AggregationLevel4 (2)
    												SearchSpaceConfigAtUE
    													R15
    														searchSpaceId = 2
    														controlResourceSetId = 1
    														monitoringSlotPeriodicityAndOffset
    															sl1 = Null
    														duration = Omit
    														monitoringSymbolsWithinSlot = 10000000000000'B
    														nrofCandidates
    															aggregationLevel1 = n0 (0)
    															aggregationLevel2 = n4 (4)
    															aggregationLevel4 = n2 (2)
    															aggregationLevel8 = n1 (1)
    															aggregationLevel16 = n0 (0)
    														searchSpaceType
    															ue_Specific
    																dci_Formats = formats0_0_And_1_0 (0)
    											NR_BWP_SearchSpaceConfig_Type
    												TypeAndPriorityList
    													NR_SearchSpaceTypeAndPriority_Type
    														NR_SearchSpaceType_Type = cssType0A (1)
    														NR_SearchSpaceCandidatePriority_Type = 1
    												AggregationLevel = AggregationLevel4 (2)
    												SearchSpaceConfigAtUE
    													R15
    														searchSpaceId = 3
    														controlResourceSetId = 1
    														monitoringSlotPeriodicityAndOffset
    															sl10 = 5
    														duration = 2
    														monitoringSymbolsWithinSlot = 10000000000000'B
    														nrofCandidates
    															aggregationLevel1 = n0 (0)
    															aggregationLevel2 = n4 (4)
    															aggregationLevel4 = n2 (2)
    															aggregationLevel8 = n1 (1)
    															aggregationLevel16 = n0 (0)
    														searchSpaceType
    															common
    																dci_Format0_0_AndFormat1_0
    																dci_Format2_0 = Omit
    																dci_Format2_1 = Omit
    																dci_Format2_2 = Omit
    																dci_Format2_3 = Omit
    										CoresetArray
    											NR_ASN1_ControlResourceSet_Type
    												R15
    													controlResourceSetId = 0
    													frequencyDomainResources = 111100000000000000000000000000000000000000000'B
    													duration = 2
    													cce_REG_MappingType
    														interleaved
    															reg_BundleSize = n6 (2)
    															interleaverSize = n2 (0)
    															shiftIndex = 0
    													precoderGranularity = sameAsREG_bundle (0)
    													tci_StatesPDCCH_ToAddList = Omit
    													tci_StatesPDCCH_ToReleaseList = Omit
    													tci_PresentInDCI = Omit
    													pdcch_DMRS_ScramblingID = Omit
    											NR_ASN1_ControlResourceSet_Type
    												R15
    													controlResourceSetId = 1
    													frequencyDomainResources = 111100000000000000000000000000000000000000000'B
    													duration = 2
    													cce_REG_MappingType
    														nonInterleaved = Null
    													precoderGranularity = sameAsREG_bundle (0)
    													tci_StatesPDCCH_ToAddList = Omit
    													tci_StatesPDCCH_ToReleaseList = Omit
    													tci_PresentInDCI = Omit
    													pdcch_DMRS_ScramblingID = Omit
    										RelativeTxPower
    											PdcchToCell = 0
    											PdcchToDmrs = 0
    									Pdsch
    										ConfigCommon
    											R15
    												pdsch_TimeDomainAllocationList
    													PDSCH_TimeDomainResourceAllocation
    														k0 = Omit
    														mappingType = typeA (0)
    														startSymbolAndLength = 53
    										ConfigDedicated
    											R15
    												dataScramblingIdentityPDSCH = 0
    												dmrs_DownlinkForPDSCH_MappingTypeA
    													setup
    														dmrs_Type = Omit
    														dmrs_AdditionalPosition = pos0 (0)
    														maxLength = Omit
    														scramblingID0 = Omit
    														scramblingID1 = Omit
    														phaseTrackingRS
    															setup
    																frequencyDensity = Omit
    																timeDensity = Omit
    																epre_Ratio = 0
    																resourceElementOffset = Omit
    												dmrs_DownlinkForPDSCH_MappingTypeB = Omit
    												tci_StatesToAddModList
    													TCI_State
    														tci_StateId = 0
    														qcl_Type1
    															cell = Omit
    															bwp_Id = Omit
    															referenceSignal
    																ssb = 1
    															qcl_Type = typeD (3)
    														qcl_Type2 = Omit
    												tci_StatesToReleaseList = Omit
    												vrb_ToPRB_Interleaver = Omit
    												resourceAllocation = resourceAllocationType1 (1)
    												pdsch_TimeDomainAllocationList = Omit
    												pdsch_AggregationFactor = Omit
    												rateMatchPatternToAddModList = Omit
    												rateMatchPatternToReleaseList = Omit
    												rateMatchPatternGroup1 = Omit
    												rateMatchPatternGroup2 = Omit
    												rbg_Size = config1 (0)
    												mcs_Table = Omit
    												maxNrofCodeWordsScheduledByDCI = Omit
    												prb_BundlingType
    													staticBundling
    														bundleSize = wideband (1)
    												zp_CSI_RS_ResourceToAddModList = Omit
    												zp_CSI_RS_ResourceToReleaseList = Omit
    												aperiodic_ZP_CSI_RS_ResourceSetsToAddModList = Omit
    												aperiodic_ZP_CSI_RS_ResourceSetsToReleaseList = Omit
    												sp_ZP_CSI_RS_ResourceSetsToAddModList = Omit
    												sp_ZP_CSI_RS_ResourceSetsToReleaseList = Omit
    												p_ZP_CSI_RS_ResourceSet = Omit
    										RelativeTxPower
    											PdschToCell = -3
    											PdschToDmrs = -3
    											PdschToPtrs = -3
    									Sps = Omit
    									CSI_RS_Config
    										None = True
    					Uplink
    						Uplink
    							Config
    								FrequencyInfoUL
    									R15
    										frequencyBandList = Omit
    										absoluteFrequencyPointA = Omit
    										scs_SpecificCarrierList
    											SCS_SpecificCarrier
    												offsetToCarrier = 0
    												subcarrierSpacing = kHz120 (3)
    												carrierBandwidth = 66
    												txDirectCurrentLocation_v1530 = Omit
    										additionalSpectrumEmission = 0
    										p_Max = 20
    										frequencyShift7p5khz = Omit
    								BWPs
    									ActiveBWP
    										SameIdAsDL = True
    									BwpArray
    										NR_UplinkBWP_Type
    											Id = 0
    											Common
    												R15
    													genericParameters
    														locationAndBandwidth = 17875
    														subcarrierSpacing = kHz120 (3)
    														cyclicPrefix = Omit
    													rach_ConfigCommon
    														setup
    															rach_ConfigGeneric
    																prach_ConfigurationIndex = 149
    																msg1_FDM = one (0)
    																msg1_FrequencyStart = 0
    																zeroCorrelationZoneConfig = 15
    																preambleReceivedTargetPower = -118
    																preambleTransMax = n7 (4)
    																powerRampingStep = dB4 (2)
    																ra_ResponseWindow = sl20 (5)
    															totalNumberOfRA_Preambles = Omit
    															ssb_perRACH_OccasionAndCB_PreamblesPerSSB
    																one = n4 (0)
    															groupBconfigured = Omit
    															ra_ContentionResolutionTimer = sf64 (7)
    															rsrp_ThresholdSSB = 0
    															rsrp_ThresholdSSB_SUL = Omit
    															prach_RootSequenceIndex
    																l139 = 0
    															msg1_SubcarrierSpacing = kHz120 (3)
    															restrictedSetConfig = unrestrictedSet (0)
    															msg3_transformPrecoder = Omit
    													pusch_ConfigCommon
    														setup
    															groupHoppingEnabledTransformPrecoding = Omit
    															pusch_TimeDomainAllocationList
    																PUSCH_TimeDomainResourceAllocation
    																	k2 = 4
    																	mappingType = typeA (0)
    																	startSymbolAndLength = 27
    																PUSCH_TimeDomainResourceAllocation
    																	k2 = 3
    																	mappingType = typeA (0)
    																	startSymbolAndLength = 27
    															msg3_DeltaPreamble = 1
    															p0_NominalWithGrant = -90
    													pucch_ConfigCommon
    														setup
    															pucch_ResourceCommon = 0
    															pucch_GroupHopping = enable (1)
    															hoppingId = Omit
    															p0_nominal = -90
    											Dedicated
    												R15
    													pucch_Config
    														setup
    															resourceSetToAddModList
    																PUCCH_ResourceSet
    																	pucch_ResourceSetId = 0
    																	resourceList
    																		PUCCH_ResourceId = 0
    																		PUCCH_ResourceId = 1
    																		PUCCH_ResourceId = 2
    																		PUCCH_ResourceId = 3
    																		PUCCH_ResourceId = 4
    																		PUCCH_ResourceId = 5
    																		PUCCH_ResourceId = 6
    																		PUCCH_ResourceId = 7
    																	maxPayloadMinus1 = Omit
    																PUCCH_ResourceSet
    																	pucch_ResourceSetId = 1
    																	resourceList
    																		PUCCH_ResourceId = 8
    																		PUCCH_ResourceId = 9
    																		PUCCH_ResourceId = 10
    																		PUCCH_ResourceId = 11
    																		PUCCH_ResourceId = 12
    																		PUCCH_ResourceId = 13
    																		PUCCH_ResourceId = 14
    																		PUCCH_ResourceId = 15
    																	maxPayloadMinus1 = 256
    																PUCCH_ResourceSet
    																	pucch_ResourceSetId = 2
    																	resourceList
    																		PUCCH_ResourceId = 8
    																		PUCCH_ResourceId = 9
    																		PUCCH_ResourceId = 10
    																		PUCCH_ResourceId = 11
    																		PUCCH_ResourceId = 12
    																		PUCCH_ResourceId = 13
    																		PUCCH_ResourceId = 14
    																		PUCCH_ResourceId = 15
    																	maxPayloadMinus1 = 256
    																PUCCH_ResourceSet
    																	pucch_ResourceSetId = 3
    																	resourceList
    																		PUCCH_ResourceId = 8
    																		PUCCH_ResourceId = 9
    																		PUCCH_ResourceId = 10
    																		PUCCH_ResourceId = 11
    																		PUCCH_ResourceId = 12
    																		PUCCH_ResourceId = 13
    																		PUCCH_ResourceId = 14
    																		PUCCH_ResourceId = 15
    																	maxPayloadMinus1 = Omit
    															resourceSetToReleaseList = Omit
    															resourceToAddModList
    																PUCCH_Resource
    																	pucch_ResourceId = 0
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 0
    																PUCCH_Resource
    																	pucch_ResourceId = 1
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 2
    																PUCCH_Resource
    																	pucch_ResourceId = 2
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 4
    																PUCCH_Resource
    																	pucch_ResourceId = 3
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 6
    																PUCCH_Resource
    																	pucch_ResourceId = 4
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 8
    																PUCCH_Resource
    																	pucch_ResourceId = 5
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 10
    																PUCCH_Resource
    																	pucch_ResourceId = 6
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format0
    																			initialCyclicShift = 0
    																			nrofSymbols = 2
    																			startingSymbolIndex = 12
    																PUCCH_Resource
    																	pucch_ResourceId = 7
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format1
    																			initialCyclicShift = 0
    																			nrofSymbols = 14
    																			startingSymbolIndex = 0
    																			timeDomainOCC = 0
    																PUCCH_Resource
    																	pucch_ResourceId = 8
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 0
    																PUCCH_Resource
    																	pucch_ResourceId = 9
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 2
    																PUCCH_Resource
    																	pucch_ResourceId = 10
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 4
    																PUCCH_Resource
    																	pucch_ResourceId = 11
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 6
    																PUCCH_Resource
    																	pucch_ResourceId = 12
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 8
    																PUCCH_Resource
    																	pucch_ResourceId = 13
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 10
    																PUCCH_Resource
    																	pucch_ResourceId = 14
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format2
    																			nrofPRBs = 6
    																			nrofSymbols = 2
    																			startingSymbolIndex = 12
    																PUCCH_Resource
    																	pucch_ResourceId = 15
    																	startingPRB = 0
    																	intraSlotFrequencyHopping = enabled (0)
    																	secondHopPRB = 0
    																	format
    																		format3
    																			nrofPRBs = 1
    																			nrofSymbols = 14
    																			startingSymbolIndex = 0
    															resourceToReleaseList = Omit
    															format1
    																setup
    																	interslotFrequencyHopping = enabled (0)
    																	additionalDMRS = true_ (0)
    																	maxCodeRate = zeroDot25 (2)
    																	nrofSlots = Omit
    																	pi2BPSK = Omit
    																	simultaneousHARQ_ACK_CSI = true_ (0)
    															format2
    																setup
    																	interslotFrequencyHopping = enabled (0)
    																	additionalDMRS = true_ (0)
    																	maxCodeRate = zeroDot25 (2)
    																	nrofSlots = Omit
    																	pi2BPSK = Omit
    																	simultaneousHARQ_ACK_CSI = true_ (0)
    															format3
    																setup
    																	interslotFrequencyHopping = enabled (0)
    																	additionalDMRS = true_ (0)
    																	maxCodeRate = zeroDot25 (2)
    																	nrofSlots = Omit
    																	pi2BPSK = Omit
    																	simultaneousHARQ_ACK_CSI = true_ (0)
    															format4 = Omit
    															schedulingRequestResourceToAddModList
    																SchedulingRequestResourceConfig
    																	schedulingRequestResourceId = 1
    																	schedulingRequestID = 0
    																	periodicityAndOffset
    																		sl80 = 9
    																	resource = 0
    															schedulingRequestResourceToReleaseList = Omit
    															multi_CSI_PUCCH_ResourceList = Omit
    															dl_DataToUL_ACK
    																PUCCH_Config___11___oftype = 2
    																PUCCH_Config___11___oftype = 3
    																PUCCH_Config___11___oftype = 4
    																PUCCH_Config___11___oftype = 5
    																PUCCH_Config___11___oftype = 6
    																PUCCH_Config___11___oftype = 7
    																PUCCH_Config___11___oftype = 8
    																PUCCH_Config___11___oftype = 9
    															spatialRelationInfoToAddModList = Omit
    															spatialRelationInfoToReleaseList = Omit
    															pucch_PowerControl
    																deltaF_PUCCH_f0 = 0
    																deltaF_PUCCH_f1 = 0
    																deltaF_PUCCH_f2 = 0
    																deltaF_PUCCH_f3 = 0
    																deltaF_PUCCH_f4 = 0
    																p0_Set = Omit
    																pathlossReferenceRSs
    																	PUCCH_PathlossReferenceRS
    																		pucch_PathlossReferenceRS_Id = 0
    																		referenceSignal
    																			ssb_Index = 1
    																twoPUCCH_PC_AdjustmentStates = Omit
    													pusch_Config
    														setup
    															dataScramblingIdentityPUSCH = Omit
    															txConfig = Omit
    															dmrs_UplinkForPUSCH_MappingTypeA
    																setup
    																	dmrs_Type = Omit
    																	dmrs_AdditionalPosition = pos0 (0)
    																	phaseTrackingRS = Omit
    																	maxLength = Omit
    																	transformPrecodingDisabled
    																		scramblingID0 = Omit
    																		scramblingID1 = Omit
    																	transformPrecodingEnabled = Omit
    															dmrs_UplinkForPUSCH_MappingTypeB = Omit
    															pusch_PowerControl
    																tpc_Accumulation = Omit
    																msg3_Alpha = alpha08 (5)
    																p0_NominalWithoutGrant = -90
    																p0_AlphaSets
    																	P0_PUSCH_AlphaSet
    																		p0_PUSCH_AlphaSetId = 0
    																		p0 = 0
    																		alpha = alpha08 (5)
    																pathlossReferenceRSToAddModList
    																	PUSCH_PathlossReferenceRS
    																		pusch_PathlossReferenceRS_Id = 0
    																		referenceSignal
    																			ssb_Index = 1
    																pathlossReferenceRSToReleaseList = Omit
    																twoPUSCH_PC_AdjustmentStates = Omit
    																deltaMCS = Omit
    																sri_PUSCH_MappingToAddModList
    																	SRI_PUSCH_PowerControl
    																		sri_PUSCH_PowerControlId = 0
    																		sri_PUSCH_PathlossReferenceRS_Id = 0
    																		sri_P0_PUSCH_AlphaSetId = 0
    																		sri_PUSCH_ClosedLoopIndex = i0 (0)
    																sri_PUSCH_MappingToReleaseList = Omit
    															frequencyHopping = Omit
    															frequencyHoppingOffsetLists = Omit
    															resourceAllocation = resourceAllocationType1 (1)
    															pusch_TimeDomainAllocationList = Omit
    															pusch_AggregationFactor = Omit
    															mcs_Table = Omit
    															mcs_TableTransformPrecoder = Omit
    															transformPrecoder = Omit
    															codebookSubset = Omit
    															maxRank = Omit
    															rbg_Size = Omit
    															uci_OnPUSCH
    																setup
    																	betaOffsets
    																		semiStatic
    																			betaOffsetACK_Index1 = 9
    																			betaOffsetACK_Index2 = 9
    																			betaOffsetACK_Index3 = 9
    																			betaOffsetCSI_Part1_Index1 = 6
    																			betaOffsetCSI_Part1_Index2 = 6
    																			betaOffsetCSI_Part2_Index1 = 6
    																			betaOffsetCSI_Part2_Index2 = 6
    																	scaling = f1 (3)
    															tp_pi2BPSK = Omit
    													configuredGrantConfig = Omit
    													srs_Config = Omit
    													beamFailureRecoveryConfig = Omit
    								RACH_ConfigDedicated = Omit
    								SI_RequestConfig = Omit
    						SupplementaryUplink = Omit
    						TimingAdvance
    							InitialValue = 0
    						PUSCH_ServingCellConfig
    							R15
    								codeBlockGroupTransmission = Omit
    								rateMatching = Omit
    								xOverhead = Omit
    								maxMIMO_Layers = Omit
    								processingType2Enabled = Omit
    				BcchConfig
    					Pbch = True
    					Pdsch = Omit
    					BcchInfo
    						MIB
    							message_
    								mib
    									systemFrameNumber = 000000'B
    									subCarrierSpacingCommon = scs30or120 (1)
    									ssb_SubcarrierOffset = 11
    									dmrs_TypeA_Position = pos2 (0)
    									pdcch_ConfigSIB1
    										controlResourceSetZero = 0
    										searchSpaceZero = 0
    									cellBarred = notBarred (1)
    									intraFreqReselection = allowed (0)
    									spare = 0'B
    						SIB1 = Omit
    						SIs = Omit
    						SegmentedSIs = Omit
    				PcchConfig = Omit
    				RachProcedureConfig
    					RachProcedureList
    						NR_RachProcedure_Type
    							RandomAccessResponse
    								SearchSpaceAndDci
    									AssignedBWPs
    										ActiveBWP = Omit
    										InitialBWP = True
    										DedicatedBWPs
    									SearchSpaceType = cssType1 (2)
    									DciInfo
    										ResoureAssignment
    											ResourceAllocationType = resourceAllocationType1 (1)
    											FreqDomain
    												Automatic
    													FirstRbIndex = 7
    													MaxRbCnt = 17
    											TimeDomain
    												Index = 0000'B
    											TransportBlockScheduling
    												Automatic
    													TransportBlock1 = qpsk (0)
    													TransportBlock2 = Omit
    													RedundancyVersionList
    											HarqProcessConfig
    												None = True
    										VrbPrbMapping
    											Index = 0'B
    										Format
    											Format_1_0_RA_RNTI
    												TbScaling = 00'B
    								MacPdu
    									SubPduList
    										NR_RAR_SubPdu_Type
    											RapIdAndPayload
    												RapId
    													Automatic = True
    												Payload
    													TimingAdvance = 0
    													UplinkGrant
    														HoppingFlag = 0'B
    														Msg3FrequencyResourceAllocation = 00000100001000'B
    														Msg3TimeResourceAllocation = 0001'B
    														MCS = 0010'B
    														TPC_Command = 011'B
    														CQI_Req = 0'B
    													TempC_RNTI
    														Explicit = 4148
    									CrcError = False
    							ContentionResolution
    								CRNTI_Based
    									AssignedBWPs
    										ActiveBWP = True
    										InitialBWP = Omit
    										DedicatedBWPs
    									SearchSpaceType = ussUL (6)
    									DciInfo
    										ResoureAssignment
    											ResourceAllocationType = resourceAllocationType1 (1)
    											FreqDomain
    												FirstRbIndex = 0
    												Nprb = 1
    											TimeDomain
    												Index = 0000'B
    											TransportBlockScheduling
    												NR_TransportBlockSingleTransmission_Type
    													TimingOffset
    														None = True
    													ImcsValue = 0
    													RedundancyVersion = 0
    													ToggleNDI = True
    											HarqProcessConfig
    												AnyProcess = True
    										PuschHoppingCtrl
    											Flag = 0'B
    										TpcCommandPusch
    											Value = 01'B
    										UL_SUL_Indicator
    											None = True
    										Format
    											Format_0_0
    				CcchDcchDtchConfig
    					DL
    						SearchSpaceAndDci
    							AssignedBWPs
    								ActiveBWP = True
    								InitialBWP = Omit
    								DedicatedBWPs
    							SearchSpaceType = ussDL (5)
    							DciInfo
    								ResoureAssignment
    									ResourceAllocationType = resourceAllocationType1 (1)
    									FreqDomain
    										Automatic
    											FirstRbIndex = 7
    											MaxRbCnt = 17
    									TimeDomain
    										Index = 0000'B
    									TransportBlockScheduling
    										Automatic
    											TransportBlock1 = qam64 (2)
    											TransportBlock2 = Omit
    											RedundancyVersionList
    												NR_RedundancyVersion_Type = 0
    												NR_RedundancyVersion_Type = 2
    												NR_RedundancyVersion_Type = 3
    												NR_RedundancyVersion_Type = 1
    												NR_RedundancyVersion_Type = 0
    									HarqProcessConfig
    										AnyProcess = True
    								VrbPrbMapping
    									Index = 0'B
    								Format
    									Format_1_0
    										DAI
    											Index = 00'B
    										TpcCommandPucch
    											Value = 01'B
    										PucchResourceIndicator
    											Value = 000'B
    										PdschHarqTimingIndicator
    											Value = 110'B
    					UL
    						SearchSpaceAndDci
    							AssignedBWPs
    								ActiveBWP = True
    								InitialBWP = Omit
    								DedicatedBWPs
    							SearchSpaceType = ussUL (6)
    							DciInfo
    								ResoureAssignment
    									ResourceAllocationType = resourceAllocationType1 (1)
    									FreqDomain
    										FirstRbIndex = 0
    										Nprb = 24
    									TimeDomain
    										Index = 0000'B
    									TransportBlockScheduling
    										NR_TransportBlockSingleTransmission_Type
    											TimingOffset
    												None = True
    											ImcsValue = 9
    											RedundancyVersion = 0
    											ToggleNDI = True
    									HarqProcessConfig
    										AnyProcess = True
    								PuschHoppingCtrl
    									Flag = 0'B
    								TpcCommandPusch
    									Value = 01'B
    								UL_SUL_Indicator
    									None = True
    								Format
    									Format_0_0
    						PUCCH_Synch
    							None = True
    						GrantConfig
    							OnSR_Reception = True
    					DrxCtrl = Omit
    					MeasGapCtrl = Omit
    				ServingCellConfig
    					SpCell
    						ServingCellIndex = 1
    						CellGroupConfig
    							CellGroupId = 1
    							SCellList
    							MAC_CellGroupConfig
    								R15
    									drx_Config = Omit
    									schedulingRequestConfig
    										schedulingRequestToAddModList
    											SchedulingRequestToAddMod
    												schedulingRequestId = 0
    												sr_ProhibitTimer = Omit
    												sr_TransMax = n16 (2)
    										schedulingRequestToReleaseList = Omit
    									bsr_Config
    										periodicBSR_Timer = sf1 (0)
    										retxBSR_Timer = sf80 (3)
    										logicalChannelSR_DelayTimer = Omit
    									tag_Config
    										tag_ToReleaseList = Omit
    										tag_ToAddModList
    											TAG
    												tag_Id = 0
    												timeAlignmentTimer = infinity_ (7)
    									phr_Config
    										setup
    											phr_PeriodicTimer = sf10 (0)
    											phr_ProhibitTimer = sf0 (0)
    											phr_Tx_PowerFactorChange = dB1 (0)
    											multiplePHR = True
    											dummy = False
    											phr_Type2OtherCell = False
    											phr_ModeOtherCG = real (0)
    									skipUplinkTxDynamic = False
    									csi_Mask_v1530 = Omit
    									dataInactivityTimer_v1530 = Omit
    							PhysicalCellGroupConfig
    								R15
    									harq_ACK_SpatialBundlingPUCCH = Omit
    									harq_ACK_SpatialBundlingPUSCH = Omit
    									p_NR_FR1 = 20
    									pdsch_HARQ_ACK_Codebook = dynamic (1)
    									tpc_SRS_RNTI = Omit
    									tpc_PUCCH_RNTI = Omit
    									tpc_PUSCH_RNTI = Omit
    									sp_CSI_RNTI = Omit
    									cs_RNTI = Omit
    									mcs_C_RNTI = Omit
    									p_UE_FR1 = Omit
    									xScale = Omit

    Sent from port: ENDC_NR_PTC:SYS

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		RadioBearerList
    			RadioBearer_Type
    				Id
    					Srb = 0
    				Config
    					AddOrReconfigure
    						Pdcp
    							None = True
    						Rlc
    							Rb
    								TM = True
    							TestMode
    								None = True
    						LogicalChannelId = 0
    						Mac
    							LogicalChannel
    								Priority = 1
    								PrioritizedBitRate = infinity_ (7)
    								LAA_UL_Allowed = Omit
    							TestMode
    								None = True
    						DiscardULData = Omit
    			RadioBearer_Type
    				Id
    					Srb = 1
    				Config
    					AddOrReconfigure
    						Pdcp
    							Config
    								Rb
    									Srb = True
    								TestMode
    									None = True
    						Rlc
    							Rb
    								AM
    									Tx
    										R8
    											t_PollRetransmit = ms45 (8)
    											pollPDU = pInfinity (7)
    											pollByte = kBinfinity (14)
    											maxRetxThreshold = t4 (3)
    									Rx
    										R8
    											t_Reordering = ms35 (7)
    											t_StatusProhibit = ms0 (0)
    									ExtendedLI = Omit
    							TestMode
    								None = True
    						LogicalChannelId = 1
    						Mac
    							LogicalChannel
    								Priority = 1
    								PrioritizedBitRate = infinity_ (7)
    								LAA_UL_Allowed = Omit
    							TestMode
    								None = True
    						DiscardULData = Omit
    			RadioBearer_Type
    				Id
    					Srb = 2
    				Config
    					AddOrReconfigure
    						Pdcp
    							Config
    								Rb
    									Srb = True
    								TestMode
    									None = True
    						Rlc
    							Rb
    								AM
    									Tx
    										R8
    											t_PollRetransmit = ms45 (8)
    											pollPDU = pInfinity (7)
    											pollByte = kBinfinity (14)
    											maxRetxThreshold = t4 (3)
    									Rx
    										R8
    											t_Reordering = ms35 (7)
    											t_StatusProhibit = ms0 (0)
    									ExtendedLI = Omit
    							TestMode
    								None = True
    						LogicalChannelId = 2
    						Mac
    							LogicalChannel
    								Priority = 3
    								PrioritizedBitRate = infinity_ (7)
    								LAA_UL_Allowed = Omit
    							TestMode
    								None = True
    						DiscardULData = Omit

    Sent from port: EUTRA_5GS_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		Cell = True

    Received on port: ENDC_NR_PTC:SYS

    SYSTEM_CTRL_CNF
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		RadioBearerList = True

    Received on port: EUTRA_5GS_PTC:SYS

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		UE_Cat_Info
    			ue_Category = 4
    			ue_Category_V1020 = 6
    			ue_Category_v1170 = 9
    			ue_Category_v11a0 = 12
    			ue_Category_v1250 = Omit
    			ue_CategoryDL_r12 = Omit
    			ue_CategoryDL_v1260 = Omit
    			ue_CategoryDL_v1310 = Omit
    			ue_CategoryDL_v1330 = Omit
    			ue_CategoryDL_v1350 = Omit
    			ue_CategoryDL_v1450 = Omit
    			ue_CategoryDL_v1460 = Omit

    Sent from port: EUTRA_5GS_PTC:SYS

    SYSTEM_CTRL_CNF
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		UE_Cat_Info = True

    Received on port: EUTRA_5GS_PTC:SYS

    timerEvent = 6
    fileName = C:\Users\FETCTTEST\Desktop\Dev_TTCNs\Deepak\7.1.3.3.x\ENDC_IWD_19wk23\Common\EUTRA38\EUTRA38_CommonProcedures.ttcn
    testName = TC_8_2_3_5_1_ENDC
    lineNo = 229
    outStr = Timer: t_GuardTimer, Duration: 180s, Started: 07:00:08

    Timer: t_GuardTimer, Duration: 180s, Started: 07:00:08

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		CellAttenuationList
    			CellAttenuationConfig_Type
    				CellId = eutra_Cell1 (1)
    				Attenuation
    					Value = 11
    				TimingInfo = Omit

    Sent from port: EUTRA_5GS_PTC:SYS

    SYSTEM_CTRL_CNF
    	Common
    		CellId = eutra_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		CellAttenuationList = True

    Received on port: EUTRA_5GS_PTC:SYS

    IMS_IPCAN_Coordination_MSG
    	IPCAN_IMS_Control
    		Reset = True

    Inter-component message: IPCAN -> IMS_PTC:IPCAN

    IP_ConfigReq_Type
    	StartPDN
    		PdnId = PDN_1 (0)
    		DrbInfo
    			Eutra
    				CellId = eutra_Cell1 (1)
    				DrbId = 1

    Inter-component message: EUTRA_CTRL -> IP_PTC:EUTRA_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.55'
    				Port = 53
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.55'
    				Port = 53
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Sent from port: IPMUX_PTC:IP_SOCK

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		CTRL
    			ConnectionId
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote
    					IpAddr = Omit
    					Port = Omit
    			Ind
    				UDP
    					SocketCnf = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		DATA
    			ConnectionId
    				Protocol
    				Local
    					IpAddr
    						V4
    							Addr
    					Port
    				Remote
    					IpAddr
    					Port
    			Ind
    				UDP
    					SocketCnf

    Message Mismatch: IP_SOCKET_IND

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.55'
    				Port = 53
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    Received on port: IPMUX_PTC:IP_SOCK

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.55'
    				Port = 53
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit

    Sent from port: IP_PTC:IP_CTRL

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    Received on port: IP_PTC:IP_CTRL

    ConstraintMismatch::Received:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		ICMPv6_ServerAddress = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    ConstraintMismatch::Expected:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = '[0-9]+[.][0-9]+[.][0-9]+[.][0-9]+'

    Message Mismatch: CharacterStringType

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 53
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 53
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Sent from port: IPMUX_PTC:IP_SOCK

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		CTRL
    			ConnectionId
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 53
    				Remote
    					IpAddr = Omit
    					Port = Omit
    			Ind
    				UDP
    					SocketCnf = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		DATA
    			ConnectionId
    				Protocol
    				Local
    					IpAddr
    						V6
    							Addr
    							ScopeId
    					Port
    				Remote
    					IpAddr
    					Port
    			Ind
    				UDP
    					SocketCnf

    Message Mismatch: IP_SOCKET_IND

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 53
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    Received on port: IPMUX_PTC:IP_SOCK

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 53
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 53
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit

    Sent from port: IP_PTC:IP_CTRL

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    Received on port: IP_PTC:IP_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.55'
    				Port = 67
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.55'
    				Port = 67
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Sent from port: IPMUX_PTC:IP_SOCK

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		CTRL
    			ConnectionId
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote
    					IpAddr = Omit
    					Port = Omit
    			Ind
    				UDP
    					SocketCnf = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		DATA
    			ConnectionId
    				Protocol
    				Local
    					IpAddr
    						V4
    							Addr
    					Port
    				Remote
    					IpAddr
    					Port
    			Ind
    				UDP
    					SocketCnf

    Message Mismatch: IP_SOCKET_IND

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.55'
    				Port = 67
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    Received on port: IPMUX_PTC:IP_SOCK

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.55'
    				Port = 67
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 67
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.Port

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 67
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 67
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.Port

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 53
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.Port

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 67
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit

    Sent from port: IP_PTC:IP_CTRL

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    Received on port: IP_PTC:IP_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = Omit
    			Remote = Omit
    		Req
    			ICMP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = Omit
    			Remote = Omit
    		Req
    			ICMP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Sent from port: IPMUX_PTC:IP_SOCK

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		CTRL
    			ConnectionId
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote
    					IpAddr = Omit
    					Port = Omit
    			Ind
    				ICMP
    					SocketCnf = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		DATA
    			ConnectionId
    				Protocol
    				Local
    					IpAddr
    						V6
    							Addr
    							ScopeId
    					Port
    				Remote
    					IpAddr
    					Port
    			Ind
    				ICMP
    					SocketCnf

    Message Mismatch: IP_SOCKET_IND

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = Omit
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			ICMP
    				SocketCnf = True

    Received on port: IPMUX_PTC:IP_SOCK

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = Omit
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			ICMP
    				SocketCnf = True

    Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 53
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 67
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit

    Sent from port: IP_PTC:IP_CTRL

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    Received on port: IP_PTC:IP_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = Omit
    			Remote = Omit
    		Req
    			ICMP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = Omit
    			Remote = Omit
    		Req
    			ICMP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Sent from port: IPMUX_PTC:IP_SOCK

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		CTRL
    			ConnectionId
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote
    					IpAddr = Omit
    					Port = Omit
    			Ind
    				ICMP
    					SocketCnf = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		DATA
    			ConnectionId
    				Protocol
    				Local
    					IpAddr
    						V6
    							Addr
    							ScopeId
    					Port
    				Remote
    					IpAddr
    					Port
    			Ind
    				ICMP
    					SocketCnf

    Message Mismatch: IP_SOCKET_IND

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = Omit
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			ICMP
    				SocketCnf = True

    Received on port: IPMUX_PTC:IP_SOCK

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = Omit
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			ICMP
    				SocketCnf = True

    Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 53
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 67
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit

    Sent from port: IP_PTC:IP_CTRL

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    Received on port: IP_PTC:IP_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.55'
    				Port = 5060
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.55'
    				Port = 5060
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Sent from port: IPMUX_PTC:IP_SOCK

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		CTRL
    			ConnectionId
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote
    					IpAddr = Omit
    					Port = Omit
    			Ind
    				UDP
    					SocketCnf = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		DATA
    			ConnectionId
    				Protocol
    				Local
    					IpAddr
    						V4
    							Addr
    					Port
    				Remote
    					IpAddr
    					Port
    			Ind
    				UDP
    					SocketCnf

    Message Mismatch: IP_SOCKET_IND

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.55'
    				Port = 5060
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    Received on port: IPMUX_PTC:IP_SOCK

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.55'
    				Port = 5060
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.Port

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.Port

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.Port

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 53
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.Port

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.Port

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 67
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.Port

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit

    Sent from port: IP_PTC:IP_CTRL

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    Received on port: IP_PTC:IP_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 5060
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 5060
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Sent from port: IPMUX_PTC:IP_SOCK

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		CTRL
    			ConnectionId
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5060
    				Remote
    					IpAddr = Omit
    					Port = Omit
    			Ind
    				UDP
    					SocketCnf = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		DATA
    			ConnectionId
    				Protocol
    				Local
    					IpAddr
    						V6
    							Addr
    							ScopeId
    					Port
    				Remote
    					IpAddr
    					Port
    			Ind
    				UDP
    					SocketCnf

    Message Mismatch: IP_SOCKET_IND

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 5060
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    Received on port: IPMUX_PTC:IP_SOCK

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 5060
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.Port

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 53
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.Port

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.Port

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 67
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit

    Sent from port: IP_PTC:IP_CTRL

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    Received on port: IP_PTC:IP_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = tcp (1)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.55'
    				Port = 5060
    			Remote = Omit
    		Req
    			TCP
    				Listen
    					SockOptList
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500
    					Application = ims (0)
    					TLSConfig = Omit

    Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = tcp (1)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.55'
    				Port = 5060
    			Remote = Omit
    		Req
    			TCP
    				Listen
    					SockOptList
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500
    					Application = ims (0)
    					TLSConfig = Omit

    Sent from port: IPMUX_PTC:IP_SOCK

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 53
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 67
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit

    Sent from port: IP_PTC:IP_CTRL

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    Received on port: IP_PTC:IP_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = tcp (1)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 5060
    			Remote = Omit
    		Req
    			TCP
    				Listen
    					SockOptList
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500
    					Application = ims (0)
    					TLSConfig = Omit

    Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = tcp (1)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 5060
    			Remote = Omit
    		Req
    			TCP
    				Listen
    					SockOptList
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500
    					Application = ims (0)
    					TLSConfig = Omit

    Sent from port: IPMUX_PTC:IP_SOCK

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 53
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 67
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = AnyOrOmit
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 5060
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = tcp (1)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 5060
    		Remote = AnyOrOmit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit

    Sent from port: IP_PTC:IP_CTRL

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    Received on port: IP_PTC:IP_CTRL

    IP_Indication_Type
    	Cnf = True

    Inter-component message: IP -> EUTRA_5GS_PTC:IP

    ConstraintMismatch::Received:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = CNF_REQUIRED (1)
    ConstraintMismatch::Expected:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		CnfReq = NO_CNF_REQUIRED (0)

    Message Mismatch: Ut_CnfReq_Type

    ConstraintMismatch::Received:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = LOCAL_CNF_REQUIRED (2)
    ConstraintMismatch::Expected:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		CnfReq = NO_CNF_REQUIRED (0)

    Message Mismatch: Ut_CnfReq_Type

    UT_COMMON_CMD
    	Cmd = SWITCH_ON (113)
    	CnfReq = NO_CNF_REQUIRED (0)
    	ParameterList = Omit

    Inter-component message: PTC_Ut -> MTC_ENDC:PTC_Ut

    ConstraintMismatch::Received:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = CNF_REQUIRED (1)
    ConstraintMismatch::Expected:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		CnfReq = NO_CNF_REQUIRED (0)

    Message Mismatch: Ut_CnfReq_Type

    ConstraintMismatch::Received:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = LOCAL_CNF_REQUIRED (2)
    ConstraintMismatch::Expected:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		CnfReq = NO_CNF_REQUIRED (0)

    Message Mismatch: Ut_CnfReq_Type

    UT_SYSTEM_REQ
    	Cmd
    		MMI
    			Cmd = 'SWITCH_ON'
    			ParameterList = Omit
    	CnfRequired = NO_CNF_REQUIRED (0)

    Sent from port: MTC_ENDC:Ut

    Sender = RequestServer
    Text = Received !SWITCH_ON from SAT Controller PC

    RequestServer:Received !SWITCH_ON from SAT Controller PC

    Sender = RequestServer
    Text = Request received [!SWITCH_ON]

    RequestServer:Request received [!SWITCH_ON]

    Sender = RequestServer
    Text = [!SWITCH_ON] Started

    RequestServer:[!SWITCH_ON] Started

    Sender = SAT Controller PC
    Text = Sent "!OK"

    SAT Controller PC:Sent "!OK"

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		Cell
    			AddOrReconfigure
    				Basic
    					ConfigCapability = Omit
    					StaticCellInfo = Omit
    					PhysicalLayerConfigDL = Omit
    					InitialCellPower = Omit
    					BcchConfig = Omit
    					PcchConfig = Omit
    					CA_CellInitialConfig = Omit
    					BRBcchConfig = Omit
    					LAA_SCellConfiguration = Omit
    					LAA_SCellConfiguration_v1430 = Omit
    				Active
    					C_RNTI = Omit
    					PhysicalLayerConfigUL = Omit
    					RachProcedureConfig = Omit
    					CcchDcchDtchConfig
    						MeasGapCtrl = Omit
    						DL = Omit
    						UL
    							DciInfo
    								Imcs
    									Value = 9
    								TransRetransmissionList
    									UL_TransRetransmission_Type
    										NewTransmission = True
    								FreqDomainSchedul
    									FirstRbIndex = 0
    									Nprb = 25
    								Format = Omit
    								HarqProcessId = Omit
    								RepetitionNumber = Omit
    								DCISubframeRepetitionNumber = Omit
    								PUSCH_TriggerA = Omit
    								TimingOffset = Omit
    								NumberOfScheduledSubframes = Omit
    							Hopping
    								Deactivated = True
    							PUCCH_Synch
    								None = True
    							UL_GrantConfig
    								OnSR_Reception = True
    						DrxCtrl = Omit
    						TtiBundling = Omit
    						CifPresence = Omit
    					ServingCellConfig = Omit
    					SciSchedulingConfig = Omit
    					EIMTA_Config = Omit
    					CE_Mode = Omit

    Sent from port: EUTRA_5GS_PTC:SYS

    Sender = !SWITCH_ON
    Text = Sending AT+CFUN=1

    !SWITCH_ON:Sending AT+CFUN=1

    Sender = Device Under Test
    Text = Sent "AT+CFUN=1"

    Device Under Test:Sent "AT+CFUN=1"

    Sender = RequestServer
    Text = Received AT+CFUN=1 from Device Under Test

    RequestServer:Received AT+CFUN=1 from Device Under Test

    Sender = RequestServer
    Text = Received OK from Device Under Test

    RequestServer:Received OK from Device Under Test

    UL-CCCH-Message
    	message = c1 = rrcConnectionRequest =
    		criticalExtensions = rrcConnectionRequest-r8 =
    			ue-Identity = randomValue = 0000001100101101100111000101100101010100
    			establishmentCause = mo-Signalling
    			spare = 0

    rrcConnectionRequest

    RRC_PDU_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 0
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 296
    				Subframe
    					Number = 3
    				HSFN
    					Number = 78
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	RrcPdu
    		Ccch
    			message_
    				c1
    					rrcConnectionRequest
    						criticalExtensions
    							rrcConnectionRequest_r8
    								ue_Identity
    									randomValue = 0000001100101101100111000101100101010100'B
    								establishmentCause = mo_Signalling (3)
    								spare = 0'B

    Received on port: NASEMU_EUTRA_PTC:SYS_SRB

    SRB_COMMON_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 0
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 296
    				Subframe
    					Number = 3
    				HSFN
    					Number = 78
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc
    			Ccch
    				message_
    					c1
    						rrcConnectionRequest
    							criticalExtensions
    								rrcConnectionRequest_r8
    									ue_Identity
    										randomValue = 0000001100101101100111000101100101010100'B
    									establishmentCause = mo_Signalling (3)
    									spare = 0'B
    		Nas = Omit

    Inter-component message: SRB -> EUTRA_5GS_PTC:SRB

    UL-DCCH-Message
    	message = c1 = rrcConnectionSetupComplete =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = c1 = rrcConnectionSetupComplete-r8 =
    			selectedPLMN-Identity = 1
    			registeredMME
    				mmegi = 1000000000000001
    				mmec = 00000001
    			dedicatedInfoNAS = 17D6448B7C060741020BF600F110800101C234567807F070C0401100100005022DD031D15200F11000015C0A00310465E03E001300F110000111034F18A640080402600400021F025D0102E0C11002AC406F04F0007000
    			nonCriticalExtension
    				nonCriticalExtension
    					gummei-Type-r10 = native

    rrcConnectionSetupComplete

    Security Protected NAS Message
    	Security header type [4 bits] = 0x1 [ 1 ]
    	Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    	MAC = 0xD6448B7C [ 3594816380 ]
    	Sequence Number = 0x06 [ 6 ]
    	NAS message = 0x0741020BF600F110800101C234567807F070C0401100100005022DD031D15200F11000015C0A00310465E03E001300F110000111034F18A640080402600400021F025D0102E0C11002AC406F04F0007000

    Security Protected NAS Message UL PDU

    Attach Request
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    	Message Type [8 bits] = 0x41 - Attach Request [ 65 ]
    	NAS key set identifier
    		Type of security context flag [1 bit] = 0x0 [ 0 ]
    		key sequence indicator [3 bits] = 0x0 [ 0 ]
    	EPS attach type
    		Spare Bits [1 bit] = 0x0 [ 0 ]
    		Value [3 bits] = 0x2 [ 2 ]
    	EPS Mobile Identity
    		IE Length [8 bits] = 0xB [ 11 ]
    		constant / IMSI Identity Digit 1 [4 bits] = 0xF [ 15 ]
    		Odd / Even Indicator [1 bit] = 0x0 [ 0 ]
    		EPS Type of Identity [3 bits] = 0x6 - GUTI [ 6 ]
    		Mobile Country Code 1st and 2nd  Digits = 0x00 [ 0 ]
    		Mobile Network Code 3rd Digit = 0xF [ 15 ]
    		Mobile Country Code 3rd Digit = 0x1 [ 1 ]
    		Mobile Network Code 1st and 2nd  Digits = 0x10 [ 16 ]
    		MME group Id = 0x8001 [ 32769 ]
    		MME code = 0x01 [ 1 ]
    		M-TMSI = 0xC2345678 [ 3258209912 ]
    	UE network capability
    		IE Length [8 bits] = 0x7 [ 7 ]
    		eea0_128 [1 bit] = 0x1 [ 1 ]
    		eea1_128 [1 bit] = 0x1 [ 1 ]
    		eea2_128 [1 bit] = 0x1 [ 1 ]
    		eea3 [1 bit] = 0x1 [ 1 ]
    		eea4 [1 bit] = 0x0 [ 0 ]
    		eea5 [1 bit] = 0x0 [ 0 ]
    		eea6 [1 bit] = 0x0 [ 0 ]
    		eea7 [1 bit] = 0x0 [ 0 ]
    		eia0 [1 bit] = 0x0 [ 0 ]
    		eia1_128 [1 bit] = 0x1 [ 1 ]
    		eia2_128 [1 bit] = 0x1 [ 1 ]
    		eia3 [1 bit] = 0x1 [ 1 ]
    		eia4 [1 bit] = 0x0 [ 0 ]
    		eia5 [1 bit] = 0x0 [ 0 ]
    		eia6 [1 bit] = 0x0 [ 0 ]
    		eia7 [1 bit] = 0x0 [ 0 ]
    		uea0_7 [8 bits] = 0xC0 [ 192 ]
    		Ucs2 Treatment [1 bit] = 0x0 - The ME Has a Preference for the Default Alphabet Over UCS2 [ 0 ]
    		uia1_7 [7 bits] = 0x40 [ 64 ]
    		prose_dd [1 bit] = 0x0 [ 0 ]
    		prose [1 bit] = 0x0 [ 0 ]
    		h245_ash [1 bit] = 0x0 [ 0 ]
    		acc_csfb [1 bit] = 0x1 [ 1 ]
    		lpp [1 bit] = 0x0 [ 0 ]
    		lcs [1 bit] = 0x0 [ 0 ]
    		xsr_vcc [1 bit] = 0x0 [ 0 ]
    		nf [1 bit] = 0x1 [ 1 ]
    		epco [1 bit] = 0x0 [ 0 ]
    		hc_cp_clot [1 bit] = 0x0 [ 0 ]
    		er_wo_pdn [1 bit] = 0x0 [ 0 ]
    		s1_u_data [1 bit] = 0x0 [ 0 ]
    		up_clot [1 bit] = 0x0 [ 0 ]
    		cp_clot [1 bit] = 0x0 [ 0 ]
    		prose_relay [1 bit] = 0x0 [ 0 ]
    		prose_dc [1 bit] = 0x0 [ 0 ]
    		bearers [1 bit] = 0x0 [ 0 ]
    		sgc [1 bit] = 0x0 [ 0 ]
    		n1mod [1 bit] = 0x0 [ 0 ]
    		dcnr [1 bit] = 0x1 [ 1 ]
    		cp_bk_of [1 bit] = 0x0 [ 0 ]
    		restrict_ec [1 bit] = 0x0 [ 0 ]
    		v2x_pc5 [1 bit] = 0x0 [ 0 ]
    		multiple_edrb [1 bit] = 0x0 [ 0 ]
    	ESM message container
    		IE Length [16 bits] = 0x5 [ 5 ]
    		ESM message container contents = 0x022DD031D1
    	Last visited registered TAI
    		IE Identifier [8 bits] = 0x52 [ 82 ]
    		Mobile Country Code 1st and 2nd  Digits = 0x00 [ 0 ]
    		Mobile Network Code 3rd Digit = 0xF [ 15 ]
    		Mobile Country Code 3rd Digit = 0x1 [ 1 ]
    		Mobile Network Code 1st and 2nd  Digits = 0x10 [ 16 ]
    		Tracking area code = 0x0001 [ 1 ]
    	DRX Parameter
    		IE Identifier [8 bits] = 0x5C [ 92 ]
    		split_code = 0x0A [ 10 ]
    		DRX cycle lengtn coeff and value for S1 mode [4 bits] = 0x0 [ 0 ]
    		Split on CCCH [1 bit] = 0x0 - Split PG Cycle on CCCH is Not Supported by the Mobile Station [ 0 ]
    		non-DRX timer [3 bits] = 0x0 [ 0 ]
    	MS Network Capability
    		IE Identifier [8 bits] = 0x31 [ 49 ]
    		IE Length [8 bits] = 0x4 [ 4 ]
    		Value
    			Gea1Bits
    				Gea1 [1 bit] = 0x0 [ 0 ]
    			SmCapabilitiesViaDedicatedChannels [1 bit] = 0x1 [ 1 ]
    			SmCapabilitiesViaGprsChannels [1 bit] = 0x1 [ 1 ]
    			Ucs2Support [1 bit] = 0x0 [ 0 ]
    			SsScreeningIndicator [2 bits] = 0x1 [ 1 ]
    			SolsaCapability [1 bit] = 0x0 [ 0 ]
    			Revision Level Indicator [1 bit] = 0x1 - The ME is Release '98 Onwards [ 1 ]
    			BSS Packet Flow Support [1 bit] = 0x1 - Mobile Station Does Support BSS Packet Flow Procedures [ 1 ]
    			ExtendedGeaBits
    				Gea2 [1 bit] = 0x1 [ 1 ]
    				Gea3 [1 bit] = 0x1 [ 1 ]
    				Gea4 [1 bit] = 0x0 [ 0 ]
    				Gea5 [1 bit] = 0x0 [ 0 ]
    				Gea6 [1 bit] = 0x0 [ 0 ]
    				Gea7 [1 bit] = 0x0 [ 0 ]
    			LcsVaCapability [1 bit] = 0x0 [ 0 ]
    			PsInterRatHoFromGeranToUtranIuModeCapability [1 bit] = 0x0 [ 0 ]
    			PsInterRatHoFromGeranToEUtranS1ModeCapability [1 bit] = 0x0 [ 0 ]
    			EmmCombinedProceduresCapability [1 bit] = 0x1 [ 1 ]
    			IsrSupport [1 bit] = 0x1 [ 1 ]
    			SrvccToGeranOrUtranCapability [1 bit] = 0x1 [ 1 ]
    			EpcCapability [1 bit] = 0x1 [ 1 ]
    			NfCapability [1 bit] = 0x1 [ 1 ]
    			GeranNetworkSharingCapability [1 bit] = 0x0 [ 0 ]
    			RestrictionOnUseOfEnhancedCoverageCapability [1 bit] = 0x0 [ 0 ]
    			DualConnectivityOfEUtraWithNrCapability [1 bit] = 0x0 [ 0 ]
    			{ Spare Padding1 =
    			}
    	Old location area identification
    		IE Identifier [8 bits] = 0x13 [ 19 ]
    		Mobile Country Code 1st and 2nd  Digits = 0x00 [ 0 ]
    		Mobile Network Code 3rd Digit = 0xF [ 15 ]
    		Mobile Country Code 3rd Digit = 0x1 [ 1 ]
    		Mobile Network Code 1st and 2nd  Digits = 0x10 [ 16 ]
    		Location Area Code = 0x0001 [ 1 ]
    	MS classmark 2
    		IE Identifier [8 bits] = 0x11 [ 17 ]
    		IE Length [8 bits] = 0x3 [ 3 ]
    		Spare Bits [1 bit] = 0x0 [ 0 ]
    		rev_level [2 bits] = 0x2 [ 2 ]
    		es_ind [1 bit] = 0x0 [ 0 ]
    		A5/1 Algorithm Supported [1 bit] = 0x1 - Encryption Algorithm A5/1 Not Available [ 1 ]
    		rf_pwr_capability [3 bits] = 0x7 [ 7 ]
    		spare2 [1 bit] = 0x0 [ 0 ]
    		ps_capability [1 bit] = 0x0 [ 0 ]
    		ss_ind [2 bits] = 0x1 [ 1 ]
    		sm_capability [1 bit] = 0x1 [ 1 ]
    		VBS Notification Reception [1 bit] = 0x0 - No VBS Capability or No Notifications Wanted [ 0 ]
    		Voice Group Call Service [1 bit] = 0x0 - No VGCS capability or no notifications wanted [ 0 ]
    		Frequency Capability  [1 bit] = 0x0 - The MS does Not Support the E-GSM or R-GSM  Band [ 0 ]
    		Classmark 3 Indicator [1 bit] = 0x1 - The MS Supports Options that are Indicated in Classmark 3 IE [ 1 ]
    		spare3 [1 bit] = 0x0 [ 0 ]
    		LCS Value Added Capability [1 bit] = 0x1 - Location Request Notification via CS domain Supported [ 1 ]
    		vcs_2 [1 bit] = 0x0 [ 0 ]
    		so_lsa [1 bit] = 0x0 [ 0 ]
    		CM Service Prompt [1 bit] = 0x1 - Network Initiated MO CM Connection Request Supported for Atleast One CM Protocol [ 1 ]
    		A5/3 Algorithm Supported [1 bit] = 0x1 - Encryption Algorithm A5/3 Available [ 1 ]
    		A5/2 Algorithm Supported [1 bit] = 0x0 - Encryption Algorithm A5/2 Not Available [ 0 ]
    		N Spare Bits1 =
    	Supported codecs
    		IE Identifier [8 bits] = 0x40 [ 64 ]
    		IE Length [8 bits] = 0x8 [ 8 ]
    		system identification 1 = 0x04 [ 4 ]
    		Length Of Bitmap for SysID 1 = 0x02 [ 2 ]
    		codec bitmap sysID 1_b1_b8 = 0x60 [ 96 ]
    		codec bitmap sysID1_b9_b16 = 0x04 [ 4 ]
    		system identification 2 = 0x00 [ 0 ]
    		Length Of Bitmap for SysID 2 = 0x02 [ 2 ]
    		codec bitmap sysID2_b1_b8 = 0x1F [ 31 ]
    		codec bitmap sysID2_b9_b16 = 0x02 [ 2 ]
    	Voice domain preference and UE usage setting
    		IE Identifier [8 bits] = 0x5D [ 93 ]
    		IE Length [8 bits] = 0x1 [ 1 ]
    		Spare Bits [5 bits] = 0x0 [ 0 ]
    		UE usage setting [1 bit] = 0x0 [ 0 ]
    		voice preference [2 bits] = 0x2 [ 2 ]
    	old_guti_type
    		IE Identifier [4 bits] = 0xE [ 14 ]
    		Spare Bits [3 bits] = 0x0 [ 0 ]
    		GUTI_type [1 bit] = 0x0 [ 0 ]
    	ms_nfs
    		IE Identifier [4 bits] = 0xC [ 12 ]
    		Spare Bits [3 bits] = 0x0 [ 0 ]
    		ext_prio_timer [1 bit] = 0x1 [ 1 ]
    	tmsi_nric
    		IE Identifier [8 bits] = 0x10 [ 16 ]
    		IE Length [8 bits] = 0x2 [ 2 ]
    		nri_cont_value [10 bits] = 0x2B1 [ 689 ]
    		Spare Bits [6 bits] = 0x0 [ 0 ]
    	UE additional security capability
    		IE Identifier [8 bits] = 0x6F [ 111 ]
    		IE Length [8 bits] = 0x4 [ 4 ]
    		5G_EA0 [1 bit] = 0x1 [ 1 ]
    		5G_EA1 [1 bit] = 0x1 [ 1 ]
    		5G_EA2 [1 bit] = 0x1 [ 1 ]
    		5G_EA3 [1 bit] = 0x1 [ 1 ]
    		5G_EA4 [1 bit] = 0x0 [ 0 ]
    		5G_EA5 [1 bit] = 0x0 [ 0 ]
    		5G_EA6 [1 bit] = 0x0 [ 0 ]
    		5G_EA7 [1 bit] = 0x0 [ 0 ]
    		5G_EA8 [1 bit] = 0x0 [ 0 ]
    		5G_EA9 [1 bit] = 0x0 [ 0 ]
    		5G_EA10 [1 bit] = 0x0 [ 0 ]
    		5G_EA11 [1 bit] = 0x0 [ 0 ]
    		5G_EA12 [1 bit] = 0x0 [ 0 ]
    		5G_EA13 [1 bit] = 0x0 [ 0 ]
    		5G_EA14 [1 bit] = 0x0 [ 0 ]
    		5G_EA15 [1 bit] = 0x0 [ 0 ]
    		5G_IA0 [1 bit] = 0x0 [ 0 ]
    		5G_IA1 [1 bit] = 0x1 [ 1 ]
    		5G_IA2 [1 bit] = 0x1 [ 1 ]
    		5G_IA3 [1 bit] = 0x1 [ 1 ]
    		5G_IA4 [1 bit] = 0x0 [ 0 ]
    		5G_IA5 [1 bit] = 0x0 [ 0 ]
    		5G_IA6 [1 bit] = 0x0 [ 0 ]
    		5G_IA7 [1 bit] = 0x0 [ 0 ]
    		5G_IA8 [1 bit] = 0x0 [ 0 ]
    		5G_IA9 [1 bit] = 0x0 [ 0 ]
    		5G_IA10 [1 bit] = 0x0 [ 0 ]
    		5G_IA11 [1 bit] = 0x0 [ 0 ]
    		5G_IA12 [1 bit] = 0x0 [ 0 ]
    		5G_IA13 [1 bit] = 0x0 [ 0 ]
    		5G_IA14 [1 bit] = 0x0 [ 0 ]
    		5G_IA15 [1 bit] = 0x0 [ 0 ]

    Attach Request PDU

    PDN Connectivity Request
    	Protocol Discriminator [4 bits] = 0x2 - EPS Session Management Messages [ 2 ]
    	Procedure transaction identifier [8 bits] = 0x2D [ 45 ]
    	Message Type [8 bits] = 0xD0 [ 208 ]
    	PDN type
    		Spare Bits [1 bit] = 0x0 [ 0 ]
    		Value [3 bits] = 0x3 [ 3 ]
    	Request type
    		Spare Bits [1 bit] = 0x0 [ 0 ]
    		Value [3 bits] = 0x1 [ 1 ]
    	ESM information transfer flag
    		IE Identifier [4 bits] = 0xD [ 13 ]
    		Spare Bits [3 bits] = 0x0 [ 0 ]
    		eit value [1 bit] = 0x1 [ 1 ]

    PDN Connectivity Request PDU

    RRC_PDU_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 304
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcConnectionSetupComplete
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							c1
    								rrcConnectionSetupComplete_r8
    									selectedPLMN_Identity = 1
    									registeredMME
    										plmn_Identity = Omit
    										mmegi = 1000000000000001'B
    										mmec = 00000001'B
    									dedicatedInfoNAS = '17D6448B7C060741020BF600F110800101C234567807F070C0401100100005022DD031D15200F11000015C0A00310465E03E001300F110000111034F18A640080402600400021F025D0102E0C11002AC406F04F0007000'O
    									nonCriticalExtension
    										lateNonCriticalExtension = Omit
    										nonCriticalExtension
    											gummei_Type_r10 = native (0)
    											rlf_InfoAvailable_r10 = Omit
    											logMeasAvailable_r10 = Omit
    											rn_SubframeConfigReq_r10 = Omit
    											nonCriticalExtension = Omit

    Received on port: NASEMU_EUTRA_PTC:SYS_SRB

    SRB_COMMON_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 304
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcConnectionSetupComplete
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								c1
    									rrcConnectionSetupComplete_r8
    										selectedPLMN_Identity = 1
    										registeredMME
    											plmn_Identity = Omit
    											mmegi = 1000000000000001'B
    											mmec = 00000001'B
    										dedicatedInfoNAS = '17D6448B7C060741020BF600F110800101C234567807F070C0401100100005022DD031D15200F11000015C0A00310465E03E001300F110000111034F18A640080402600400021F025D0102E0C11002AC406F04F0007000'O
    										nonCriticalExtension
    											lateNonCriticalExtension = Omit
    											nonCriticalExtension
    												gummei_Type_r10 = native (0)
    												rlf_InfoAvailable_r10 = Omit
    												logMeasAvailable_r10 = Omit
    												rn_SubframeConfigReq_r10 = Omit
    												nonCriticalExtension = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0001'B
    					NasCount = '00000006'O
    				Pdu
    					Msg
    						aTTACH_REQUEST
    							securityHeaderType = 0000'B
    							protocolDiscriminator = 0111'B
    							messageType = 01000001'B
    							nasKeySetId
    								iei = Omit
    								tsc = 0'B
    								nasKeySetId = 000'B
    							epsAttachType
    								spare = 0'B
    								typeValue = 010'B
    							epsMobileIdentity
    								iei = Omit
    								iel = '0B'O
    								idDigit1 = 1111'B
    								oddEvenInd = 0'B
    								typeOfId = 110'B
    								otherDigits = '00F110800101C2345678'O
    							ueNetworkCapability
    								iei = Omit
    								iel = '07'O
    								eeaCap = 11110000'B
    								eiaCap = 01110000'B
    								ueaCap = 11000000'B
    								uiaCap = 01000000'B
    								srvcc_LPP_ProSeCap = 00010001'B
    								cIoT_proSeCap = 00000000'B
    								cIoT_V2X = 00010000'B
    								spare = Omit
    							esmMessage
    								iei = Omit
    								iel = '0005'O
    								esmPdu = '022DD031D1'O
    							oldPtmsiSignature = Omit
    							additionalGuti = Omit
    							lastVisitedRegisteredTai
    								iei = '52'O
    								plmnId = '00F110'O
    								tac = '0001'O
    							drxParameter
    								iei = '5C'O
    								splitPGcycleCode = 00001010'B
    								cnDRXcoef = 0000'B
    								splitOnCCCH = 0'B
    								nonDRXtimer = 000'B
    							msNetworkCapability
    								iei = '31'O
    								iel = '04'O
    								gea1 = 0'B
    								smCapDedicated = 1'B
    								smCapGPRS = 1'B
    								ucs2 = 0'B
    								ssScreeningIndicator = 01'B
    								soLSACap = 0'B
    								revLevelIndicator = 1'B
    								pfcFeatureMode = 1'B
    								gea2 = 1'B
    								gea3 = 1'B
    								gea4 = 0'B
    								gea5 = 0'B
    								gea6 = 0'B
    								gea7 = 0'B
    								lcsVACap = 0'B
    								psHOtoUTRAN_IuModeCap = 0'B
    								psHOtoEUTRAN_S1ModeCap = 0'B
    								emmCombinedCap = 1'B
    								isrSupport = 1'B
    								srvccToGERAN_UTRANCap = 1'B
    								epcCap = 1'B
    								nfCap = 1'B
    								gERANNtwkShareCap = 0'B
    								userPlaneIntegrityProtSupport = Omit
    								gia4 = Omit
    								gia5 = Omit
    								gia6 = Omit
    								gia7 = Omit
    								ePCOInd = Omit
    								restrictEnhancedCoverageCap = Omit
    								dualConnectivityEUTRA_NR = Omit
    								spareBits = 00000000'B
    							oldLai
    								iei = '13'O
    								plmn = '00F110'O
    								lac = '0001'O
    							tmsiStatus = Omit
    							msClassmark2
    								iei = '11'O
    								iel = '03'O
    								spare1_1 = 0'B
    								revLvl = 10'B
    								eSIND = 0'B
    								a5_1 = 1'B
    								rFPwrCap = 111'B
    								spare1_2 = 0'B
    								pSCap = 0'B
    								sSSI = 01'B
    								sMCap = 1'B
    								vBS = 0'B
    								vGCS = 0'B
    								fC = 0'B
    								cM3 = 1'B
    								spare1_3 = 0'B
    								lCSVA = 1'B
    								uCS2 = 0'B
    								soLSA = 0'B
    								cMSP = 1'B
    								a5_3 = 1'B
    								a5_2 = 0'B
    							msClassmark3 = Omit
    							supportedCodecList
    								iei = '40'O
    								iel = '08'O
    								codec
    									Codec
    										sysId = '04'O
    										len = '02'O
    										bitMap1to8 = 01100000'B
    										bitMap9to16 = 00000100'B
    									Codec
    										sysId = '00'O
    										len = '02'O
    										bitMap1to8 = 00011111'B
    										bitMap9to16 = 00000010'B
    							addUpdateType = Omit
    							voiceDomainPref
    								iei = '5D'O
    								iel = '01'O
    								spareBits = 00000'B
    								ueUsageSetting = 0'B
    								voiceDomainPrefEUTRA = 10'B
    							deviceProperties = Omit
    							oldGUTI_Type
    								iei = 'E'H
    								spare = 000'B
    								gutiType = 0'B
    							msNetworkFeatureSupport
    								iei = 'C'H
    								spare = 000'B
    								extdPeriodicTimers = 1'B
    							tmsiBasedNRIContainer
    								iei = '10'O
    								iel = '02'O
    								nriContainerValue = 1010110001'B
    								spareBits = 000000'B
    							t3324Value = Omit
    							t3412ExtdValue = Omit
    							extendedDRXParams = Omit
    							ueAddSecurityCap
    								iei = '6F'O
    								iel = '04'O
    								eaCap5G_0_7 = 'F0'O
    								eaCap5G_8_15 = '00'O
    								iaCap5G_0_7 = '70'O
    								iaCap5G_8_15 = '00'O
    							ueStatus = Omit
    							addInfoReq = Omit
    					PiggybackedPduList
    						NAS_UL_Pdu_Type
    							Msg
    								pDN_CONNECTIVITY_REQUEST
    									epsBearerId = '0'H
    									protocolDiscriminator = 0010'B
    									procedureTransactionIdentifier = '2D'O
    									messageType = 11010000'B
    									pdnType
    										spare = 0'B
    										typeValue = 011'B
    									requestType
    										spare = 0'B
    										typeValue = 001'B
    									esmInfoTransferFlag
    										iei = 'D'H
    										spare = 000'B
    										eitValue = 1'B
    									accessPointName = Omit
    									protocolConfigurationOptions = Omit
    									deviceProperties = Omit
    									nbifomContainer = Omit
    									headerCompressionConfig = Omit
    									extdProtocolConfigurationOptions = Omit
    							PiggybackedPduList = Omit

    Inter-component message: SRB -> EUTRA_5GS_PTC:SRB

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		Cell
    			AddOrReconfigure
    				Basic
    					ConfigCapability = Omit
    					StaticCellInfo = Omit
    					PhysicalLayerConfigDL = Omit
    					InitialCellPower = Omit
    					BcchConfig = Omit
    					PcchConfig = Omit
    					CA_CellInitialConfig = Omit
    					BRBcchConfig = Omit
    					LAA_SCellConfiguration = Omit
    					LAA_SCellConfiguration_v1430 = Omit
    				Active
    					C_RNTI = Omit
    					PhysicalLayerConfigUL = Omit
    					RachProcedureConfig = Omit
    					CcchDcchDtchConfig
    						MeasGapCtrl = Omit
    						DL = Omit
    						UL
    							DciInfo
    								Imcs = Omit
    								TransRetransmissionList = Omit
    								FreqDomainSchedul = Omit
    								Format = Omit
    								HarqProcessId = Omit
    								RepetitionNumber = Omit
    								DCISubframeRepetitionNumber = Omit
    								PUSCH_TriggerA = Omit
    								TimingOffset = Omit
    								NumberOfScheduledSubframes = Omit
    							Hopping
    								Deactivated = True
    							PUCCH_Synch
    								Auto
    									TimingAdvance = 31
    									TA_Period = 600
    									TA_Repetition
    										Continuous = True
    							UL_GrantConfig = Omit
    						DrxCtrl = Omit
    						TtiBundling = Omit
    						CifPresence = Omit
    					ServingCellConfig = Omit
    					SciSchedulingConfig = Omit
    					EIMTA_Config = Omit
    					CE_Mode = Omit

    Sent from port: EUTRA_5GS_PTC:SYS

    SYSTEM_CTRL_CNF
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		Cell = True

    Received on port: EUTRA_5GS_PTC:SYS

    SRB_COMMON_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc = Omit
    		Nas
    			NAS_MSG_Request_Type
    				SecurityProtection
    					Status = 0000'B
    					ForceMacError = False
    				Pdu
    					Msg
    						aUTHENTICATION_REQUEST
    							securityHeaderType = 0000'B
    							protocolDiscriminator = 0111'B
    							messageType = 01010010'B
    							spareHalfOctet = '0'H
    							asmeNasKeySetId
    								iei = Omit
    								tsc = 0'B
    								nasKeySetId = 000'B
    							rand
    								iei = Omit
    								randValue = 10100011110111100000110001101101001101100011111000110000110000110110010010100100000001111000111100011011111110001101010101110111'B
    							autn
    								iei = Omit
    								iel = '10'O
    								aUTN = 01101110001100100011101100110110110001000110110010000000000000001010001111011111000011100110111000110010001110111011011011000100'B
    					PiggybackedPduList = Omit

    Inter-component message: TC_SRB -> NASEMU_EUTRA_PTC:TC_SRB

    Authentication Request
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    	Message Type [8 bits] = 0x52 - Authentication Request [ 82 ]
    	Spare Half Octet [4 bits] = 0x0 [ 0 ]
    	NAS key set identifierASME
    		Type of security context flag [1 bit] = 0x0 [ 0 ]
    		key sequence indicator [3 bits] = 0x0 [ 0 ]
    		Authentication parameter random = 0xA3DE0C6D363E30C364A4078F1BF8D577
    	Authentication Parameter AUTN
    		IE Length [8 bits] = 0x10 [ 16 ]
    		value = 0x6E323B36C46C8000A3DF0E6E323BB6C4

    Authentication Request PDU

    DL-DCCH-Message
    	message = c1 = dlInformationTransfer =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = c1 = dlInformationTransfer-r8 =
    			dedicatedInfoType = dedicatedInfoNAS = 075200A3DE0C6D363E30C364A4078F1BF8D577106E323B36C46C8000A3DF0E6E323BB6C4

    dlInformationTransfer

    RRC_PDU_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				c1
    					dlInformationTransfer
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							c1
    								dlInformationTransfer_r8
    									dedicatedInfoType
    										dedicatedInfoNAS = '075200A3DE0C6D363E30C364A4078F1BF8D577106E323B36C46C8000A3DF0E6E323BB6C4'O
    									nonCriticalExtension = Omit

    Sent from port: NASEMU_EUTRA_PTC:SYS_SRB

    UL-DCCH-Message
    	message = c1 = ulInformationTransfer =
    		criticalExtensions = c1 = ulInformationTransfer-r8 =
    			dedicatedInfoType = dedicatedInfoNAS = 17B23635C807075308A3DF0E6E323B36C4

    ulInformationTransfer

    Security Protected NAS Message
    	Security header type [4 bits] = 0x1 [ 1 ]
    	Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    	MAC = 0x32363548 [ 842413384 ]
    	Sequence Number = 0x07 [ 7 ]
    	NAS message = 0x075308235F0E6E323B3644

    Security Protected NAS Message UL PDU

    Authentication Response
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    	Message Type [8 bits] = 0x53 - Authentication Response [ 83 ]
    	Authentication response parameter
    		IE Length [8 bits] = 0x8 [ 8 ]
    		Authentication response parameter information = 0x235F0E6E323B3644

    Authentication Response PDU

    RRC_PDU_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 324
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ulInformationTransfer
    						criticalExtensions
    							c1
    								ulInformationTransfer_r8
    									dedicatedInfoType
    										dedicatedInfoNAS = '17B23635C807075308A3DF0E6E323B36C4'O
    									nonCriticalExtension = Omit

    Received on port: NASEMU_EUTRA_PTC:SYS_SRB

    SRB_COMMON_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 324
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0001'B
    					NasCount = '00000007'O
    				Pdu
    					Msg
    						aUTHENTICATION_RESPONSE
    							securityHeaderType = 0000'B
    							protocolDiscriminator = 0111'B
    							messageType = 01010011'B
    							authenticationResponseParameter
    								iei = Omit
    								iel = '08'O
    								res = 1010001111011111000011100110111000110010001110110011011011000100'B
    					PiggybackedPduList = Omit

    Inter-component message: SRB -> EUTRA_5GS_PTC:SRB

    NAS_CTRL_REQ
    	Common
    		ControlInfo
    			CnfFlag = True
    	Request
    		Security
    			StartRestart
    				Integrity
    					Algorithm = 001'B
    					K_NAS = 01101111111110011000110110100011010010100010110100011011110001100010101010100110110101001011101100011010011000101010011001100100'B
    				Ciphering
    					Algorithm = 001'B
    					K_NAS = 00110010100110111011010001000010000101000111011000010111000110011110011011000000000100000101011110100001010001000001111110100001'B
    				NasCountReset = True

    Inter-component message: CTRL -> NASEMU_EUTRA_PTC:CTRL

    NAS_CTRL_CNF
    	Common
    	Confirm
    		Security = True

    Inter-component message: NASCTRL -> EUTRA_5GS_PTC:NASCTRL

    SRB_COMMON_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc = Omit
    		Nas
    			NAS_MSG_Request_Type
    				SecurityProtection
    					Status = 0011'B
    					ForceMacError = False
    				Pdu
    					Msg
    						sECURITY_MODE_COMMAND
    							securityHeaderType = 0000'B
    							protocolDiscriminator = 0111'B
    							messageType = 01011101'B
    							nasSecurityAlgorithms
    								iei = Omit
    								spare1 = 0'B
    								cipheringType = 001'B
    								spare2 = 0'B
    								integrityType = 001'B
    							spareHalfOctet = '0'H
    							asmeNasKeySetId
    								iei = Omit
    								tsc = 0'B
    								nasKeySetId = 000'B
    							replayedSecurityCapability
    								iei = None
    								iel = '05'O
    								eeaCap = 'F0'O
    								eiaCap = '70'O
    								ueaCap = 'C0'O
    								uiaCap = '40'O
    								geaCap = '30'O
    							imeisvRequest = Omit
    							replayedNonceUe = Omit
    							nonceMme = Omit
    							hashMME = Omit
    							replayedUEAddSecurityCap
    								iei = '6F'O
    								iel = '04'O
    								eaCap5G_0_7 = 'F0'O
    								eaCap5G_8_15 = '00'O
    								iaCap5G_0_7 = '70'O
    								iaCap5G_8_15 = '00'O
    					PiggybackedPduList = Omit

    Inter-component message: TC_SRB -> NASEMU_EUTRA_PTC:TC_SRB

    Security Mode Command
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    	Message Type [8 bits] = 0x5D - Security Mode Command [ 93 ]
    	Selected NAS security algorithms
    		Spare Bits [1 bit] = 0x0 [ 0 ]
    		Type of ciphering algorithm [3 bits] = 0x1 [ 1 ]
    		spare Bits_1 [1 bit] = 0x0 [ 0 ]
    		Type of integrity protection algorithm [3 bits] = 0x1 [ 1 ]
    	Spare Half Octet [4 bits] = 0x0 [ 0 ]
    	NAS key set identifierASME
    		Type of security context flag [1 bit] = 0x0 [ 0 ]
    		key sequence indicator [3 bits] = 0x0 [ 0 ]
    	Replayed UE security capabilities
    		IE Length [8 bits] = 0x5 [ 5 ]
    		eea0_128 [1 bit] = 0x1 [ 1 ]
    		eea1_128 [1 bit] = 0x1 [ 1 ]
    		eea2_128 [1 bit] = 0x1 [ 1 ]
    		eea3 [1 bit] = 0x1 [ 1 ]
    		eea4 [1 bit] = 0x0 [ 0 ]
    		eea5 [1 bit] = 0x0 [ 0 ]
    		eea6 [1 bit] = 0x0 [ 0 ]
    		eea7 [1 bit] = 0x0 [ 0 ]
    		Spare Bits [1 bit] = 0x0 [ 0 ]
    		eia1_128 [1 bit] = 0x1 [ 1 ]
    		eia2_128 [1 bit] = 0x1 [ 1 ]
    		eia3 [1 bit] = 0x1 [ 1 ]
    		eia4 [1 bit] = 0x0 [ 0 ]
    		eia5 [1 bit] = 0x0 [ 0 ]
    		eia6 [1 bit] = 0x0 [ 0 ]
    		eia7 [1 bit] = 0x0 [ 0 ]
    		uea0_7 [8 bits] = 0xC0 [ 192 ]
    		spare Bits_1 [1 bit] = 0x0 [ 0 ]
    		uia1_7 [7 bits] = 0x40 [ 64 ]
    		spare2 [1 bit] = 0x0 [ 0 ]
    		gea1_7 [7 bits] = 0x30 [ 48 ]
    	Replayed UE additional security capability
    		IE Identifier [8 bits] = 0x6F [ 111 ]
    		IE Length [8 bits] = 0x4 [ 4 ]
    		5G_EA0 [1 bit] = 0x1 [ 1 ]
    		5G_EA1 [1 bit] = 0x1 [ 1 ]
    		5G_EA2 [1 bit] = 0x1 [ 1 ]
    		5G_EA3 [1 bit] = 0x1 [ 1 ]
    		5G_EA4 [1 bit] = 0x0 [ 0 ]
    		5G_EA5 [1 bit] = 0x0 [ 0 ]
    		5G_EA6 [1 bit] = 0x0 [ 0 ]
    		5G_EA7 [1 bit] = 0x0 [ 0 ]
    		5G_EA8 [1 bit] = 0x0 [ 0 ]
    		5G_EA9 [1 bit] = 0x0 [ 0 ]
    		5G_EA10 [1 bit] = 0x0 [ 0 ]
    		5G_EA11 [1 bit] = 0x0 [ 0 ]
    		5G_EA12 [1 bit] = 0x0 [ 0 ]
    		5G_EA13 [1 bit] = 0x0 [ 0 ]
    		5G_EA14 [1 bit] = 0x0 [ 0 ]
    		5G_EA15 [1 bit] = 0x0 [ 0 ]
    		5G_IA0 [1 bit] = 0x0 [ 0 ]
    		5G_IA1 [1 bit] = 0x1 [ 1 ]
    		5G_IA2 [1 bit] = 0x1 [ 1 ]
    		5G_IA3 [1 bit] = 0x1 [ 1 ]
    		5G_IA4 [1 bit] = 0x0 [ 0 ]
    		5G_IA5 [1 bit] = 0x0 [ 0 ]
    		5G_IA6 [1 bit] = 0x0 [ 0 ]
    		5G_IA7 [1 bit] = 0x0 [ 0 ]
    		5G_IA8 [1 bit] = 0x0 [ 0 ]
    		5G_IA9 [1 bit] = 0x0 [ 0 ]
    		5G_IA10 [1 bit] = 0x0 [ 0 ]
    		5G_IA11 [1 bit] = 0x0 [ 0 ]
    		5G_IA12 [1 bit] = 0x0 [ 0 ]
    		5G_IA13 [1 bit] = 0x0 [ 0 ]
    		5G_IA14 [1 bit] = 0x0 [ 0 ]
    		5G_IA15 [1 bit] = 0x0 [ 0 ]

    Security Mode Command PDU

    Security Protected NAS Message
    	Security header type [4 bits] = 0x3 [ 3 ]
    	Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    	MAC = 0x4C2CE1FD [ 1278009853 ]
    	Sequence Number = 0x00 [ 0 ]
    	NAS message = 0x075D110005F070C040306F04F0007000

    Security Protected NAS Message DL PDU

    DL-DCCH-Message
    	message = c1 = dlInformationTransfer =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = c1 = dlInformationTransfer-r8 =
    			dedicatedInfoType = dedicatedInfoNAS = 374C2CE1FD00075D110005F070C040306F04F0007000

    dlInformationTransfer

    RRC_PDU_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				c1
    					dlInformationTransfer
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							c1
    								dlInformationTransfer_r8
    									dedicatedInfoType
    										dedicatedInfoNAS = '374C2CE1FD00075D110005F070C040306F04F0007000'O
    									nonCriticalExtension = Omit

    Sent from port: NASEMU_EUTRA_PTC:SYS_SRB

    UL-DCCH-Message
    	message = c1 = ulInformationTransfer =
    		criticalExtensions = c1 = ulInformationTransfer-r8 =
    			dedicatedInfoType = dedicatedInfoNAS = 4765DF4F7D000022

    ulInformationTransfer

    Security Protected NAS Message
    	Security header type [4 bits] = 0x4 [ 4 ]
    	Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    	MAC = 0x655F4F7D [ 1700745085 ]
    	Sequence Number = 0x00 [ 0 ]
    	NAS message = 0x0022 [ 34 ]

    Security Protected NAS Message UL PDU

    Ciphered NAS Message
    	0x0022

    Ciphered NAS Message UL PDU

    RRC_PDU_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 330
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ulInformationTransfer
    						criticalExtensions
    							c1
    								ulInformationTransfer_r8
    									dedicatedInfoType
    										dedicatedInfoNAS = '4765DF4F7D000022'O
    									nonCriticalExtension = Omit

    Received on port: NASEMU_EUTRA_PTC:SYS_SRB

    Security Mode Complete
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    	Message Type [8 bits] = 0x5E - Security Mode Complete [ 94 ]

    Security Mode Complete PDU

    SRB_COMMON_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 330
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0100'B
    					NasCount = '00000000'O
    				Pdu
    					Msg
    						sECURITY_MODE_COMPLETE
    							securityHeaderType = 0000'B
    							protocolDiscriminator = 0111'B
    							messageType = 01011110'B
    							imeisv = Omit
    							replayedNASMsg = Omit
    					PiggybackedPduList = Omit

    Inter-component message: SRB -> EUTRA_5GS_PTC:SRB

    SRB_COMMON_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc = Omit
    		Nas
    			NAS_MSG_Request_Type
    				SecurityProtection
    					Status = 0010'B
    					ForceMacError = False
    				Pdu
    					Msg
    						eSM_INFORMATION_REQUEST
    							epsBearerId = '0'H
    							protocolDiscriminator = 0010'B
    							procedureTransactionIdentifier = '2D'O
    							messageType = 11011001'B
    					PiggybackedPduList = Omit

    Inter-component message: TC_SRB -> NASEMU_EUTRA_PTC:TC_SRB

    ESM Information Request
    	EPS bearer identity [4 bits] = 0x0 [ 0 ]
    	Protocol Discriminator [4 bits] = 0x2 - EPS Session Management Messages [ 2 ]
    	Procedure transaction identifier [8 bits] = 0x2D [ 45 ]
    	Message Type [8 bits] = 0xD9 - ESM Information Request [ 217 ]

    ESM Information Request PDU

    Ciphered NAS Message
    	0x59100D

    Ciphered NAS Message DL PDU

    Security Protected NAS Message
    	Security header type [4 bits] = 0x2 [ 2 ]
    	Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    	MAC = 0xC259389E [ 3260627102 ]
    	Sequence Number = 0x01 [ 1 ]
    	NAS message = 0x59100D [ 5836813 ]

    Security Protected NAS Message DL PDU

    DL-DCCH-Message
    	message = c1 = dlInformationTransfer =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = c1 = dlInformationTransfer-r8 =
    			dedicatedInfoType = dedicatedInfoNAS = 27C259389E0159100D

    dlInformationTransfer

    RRC_PDU_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				c1
    					dlInformationTransfer
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							c1
    								dlInformationTransfer_r8
    									dedicatedInfoType
    										dedicatedInfoNAS = '27C259389E0159100D'O
    									nonCriticalExtension = Omit

    Sent from port: NASEMU_EUTRA_PTC:SYS_SRB

    UL-DCCH-Message
    	message = c1 = ulInformationTransfer =
    		criticalExtensions = c1 = ulInformationTransfer-r8 =
    			dedicatedInfoType = dedicatedInfoNAS = 2761821D4501D6FE61BF1C34E55FB80FA3F03D0E239624EC19D6A663935526FF6A55CCD45DB22924D72CDBA446D17C33D51B59FC4C4CB1F7C99EC54D8D05FDB97CCE69D2F181A067906013848258F6D997A2D26108755579DAB889764D9488E0D4CE1E

    ulInformationTransfer

    Security Protected NAS Message
    	Security header type [4 bits] = 0x2 [ 2 ]
    	Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    	MAC = 0x61021D45 [ 1627528517 ]
    	Sequence Number = 0x01 [ 1 ]
    	NAS message = 0x567E613F1C34655F380F23703D0E2316246C195626631355267F6A554C545D322924572C5B2446517C33551B597C4C4C3177491E454D0D057D397C4E695271012067106013040258765917225261087555795A3809764D140860544E1E

    Security Protected NAS Message UL PDU

    Ciphered NAS Message
    	0x567E613F1C34655F380F23703D0E2316246C195626631355267F6A554C545D322924572C5B2446517C33551B597C4C4C3177491E454D0D057D397C4E695271012067106013040258765917225261087555795A3809764D140860544E1E

    Ciphered NAS Message UL PDU

    RRC_PDU_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 336
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ulInformationTransfer
    						criticalExtensions
    							c1
    								ulInformationTransfer_r8
    									dedicatedInfoType
    										dedicatedInfoNAS = '2761821D4501D6FE61BF1C34E55FB80FA3F03D0E239624EC19D6A663935526FF6A55CCD45DB22924D72CDBA446D17C33D51B59FC4C4CB1F7C99EC54D8D05FDB97CCE69D2F181A067906013848258F6D997A2D26108755579DAB889764D9488E0D4CE1E'O
    									nonCriticalExtension = Omit

    Received on port: NASEMU_EUTRA_PTC:SYS_SRB

    ESM Information Response
    	EPS bearer identity [4 bits] = 0x0 [ 0 ]
    	Protocol Discriminator [4 bits] = 0x2 - EPS Session Management Messages [ 2 ]
    	Procedure transaction identifier [8 bits] = 0x2D [ 45 ]
    	Message Type [8 bits] = 0xDA - ESM Information Response [ 218 ]
    	Protocol Configuration Options
    		IE Identifier [8 bits] = 0x27 [ 39 ]
    		IE Length [8 bits] = 0x58 [ 88 ]
    		Extension Bit [1 bit] = 0x1 - Outgoing Calls Barred within CUG [ 1 ]
    		Spare Bits [4 bits] = 0x0 [ 0 ]
    		Configuration Protocol [3 bits] = 0x0 - PPP for Use with IP PDP Type [ 0 ]
    		Option1
    			Identifier = 0xC223 - Challenge Handshake Authentication Protocol [ 49699 ]
    			Length [8 bits] = 0x16 [ 22 ]
    			value = 0x01000016102006F9F92006F9F92006F9F92006F9F92A
    		Option2
    			Identifier = 0xC223 - Challenge Handshake Authentication Protocol [ 49699 ]
    			Length [8 bits] = 0x16 [ 22 ]
    			Value = 0x0200001610D7DE94EA508DD5AEE7429F78AFCA125D2A
    		Option3
    			Identifier = 0x8021 - Internet Protocol Control Protocol [ 32801 ]
    			Length [8 bits] = 0x10 [ 16 ]
    			Value = 0x01000010810600000000830600000000
    		Option4
    			Identifier = 0x000D [ 13 ]
    			Length [8 bits] = 0x0 [ 0 ]
    		Option5
    			Identifier = 0x0003 - DNS Server Address [ 3 ]
    			Length [8 bits] = 0x0 [ 0 ]
    		Option6
    			Identifier = 0x000A [ 10 ]
    			Length [8 bits] = 0x0 [ 0 ]
    		Option7
    			Identifier = 0x0005 [ 5 ]
    			Length [8 bits] = 0x0 [ 0 ]
    		Option8
    			Identifier = 0x0010 [ 16 ]
    			Length [8 bits] = 0x0 [ 0 ]
    		Option9
    			Identifier = 0x0011 [ 17 ]
    			Length [8 bits] = 0x0 [ 0 ]

    ESM Information Response PDU

    SRB_COMMON_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 336
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0010'B
    					NasCount = '00000001'O
    				Pdu
    					Msg
    						eSM_INFORMATION_RESPONSE
    							epsBearerId = '0'H
    							protocolDiscriminator = 0010'B
    							procedureTransactionIdentifier = '2D'O
    							messageType = 11011010'B
    							accessPointName = Omit
    							protocolConfigurationOptions
    								iei = '27'O
    								iel = '58'O
    								ext = 1'B
    								spare = 0000'B
    								configProtocol = 000'B
    								pco
    									ProtocolContainer
    										protocolID = 'C223'O
    										protocolLength = '16'O
    										content = '01000016102006F9F92006F9F92006F9F92006F9F92A'O
    									ProtocolContainer
    										protocolID = 'C223'O
    										protocolLength = '16'O
    										content = '0200001610D7DE94EA508DD5AEE7429F78AFCA125D2A'O
    									ProtocolContainer
    										protocolID = '8021'O
    										protocolLength = '10'O
    										content = '01000010810600000000830600000000'O
    									ProtocolContainer
    										protocolID = '000D'O
    										protocolLength = '00'O
    										content = Omit
    									ProtocolContainer
    										protocolID = '0003'O
    										protocolLength = '00'O
    										content = Omit
    									ProtocolContainer
    										protocolID = '000A'O
    										protocolLength = '00'O
    										content = Omit
    									ProtocolContainer
    										protocolID = '0005'O
    										protocolLength = '00'O
    										content = Omit
    									ProtocolContainer
    										protocolID = '0010'O
    										protocolLength = '00'O
    										content = Omit
    									ProtocolContainer
    										protocolID = '0011'O
    										protocolLength = '00'O
    										content = Omit
    							extdProtocolConfigurationOptions = Omit
    					PiggybackedPduList = Omit

    Inter-component message: SRB -> EUTRA_5GS_PTC:SRB

    IP_ConfigReq_Type
    	ChangeDrbInfo
    		PdnId = PDN_1 (0)
    		DrbInfo
    			Eutra
    				CellId = eutra_Cell1 (1)
    				DrbId = 8

    Inter-component message: EUTRA_CTRL -> IP_PTC:EUTRA_CTRL

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit

    Sent from port: IP_PTC:IP_CTRL

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    Received on port: IP_PTC:IP_CTRL

    IP_Indication_Type
    	Cnf = True

    Inter-component message: IP -> EUTRA_5GS_PTC:IP

    IP_ConfigReq_Type
    	StartPDN
    		PdnId = PDN_Internet (3)
    		DrbInfo
    			Eutra
    				CellId = eutra_Cell1 (1)
    				DrbId = 8

    Inter-component message: EUTRA_CTRL -> IP_PTC:EUTRA_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.55'
    				Port = 53
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.55'
    				Port = 53
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Sent from port: IPMUX_PTC:IP_SOCK

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		CTRL
    			ConnectionId
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote
    					IpAddr = Omit
    					Port = Omit
    			Ind
    				UDP
    					SocketCnf = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		DATA
    			ConnectionId
    				Protocol
    				Local
    					IpAddr
    						V4
    							Addr
    					Port
    				Remote
    					IpAddr
    					Port
    			Ind
    				UDP
    					SocketCnf

    Message Mismatch: IP_SOCKET_IND

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.55'
    				Port = 53
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    Received on port: IPMUX_PTC:IP_SOCK

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.55'
    				Port = 53
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit

    Sent from port: IP_PTC:IP_CTRL

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    Received on port: IP_PTC:IP_CTRL

    ConstraintMismatch::Received:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		ICMPv6_ServerAddress = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    ConstraintMismatch::Expected:
    summary = Message Mismatch: CharacterStringType
    MATCH_MISMATCH
    	Message Mismatch: CharacterStringType
    		CharacterStringType = '[0-9]+[.][0-9]+[.][0-9]+[.][0-9]+'

    Message Mismatch: CharacterStringType

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 53
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 53
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Sent from port: IPMUX_PTC:IP_SOCK

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		CTRL
    			ConnectionId
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 53
    				Remote
    					IpAddr = Omit
    					Port = Omit
    			Ind
    				UDP
    					SocketCnf = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		DATA
    			ConnectionId
    				Protocol
    				Local
    					IpAddr
    						V6
    							Addr
    							ScopeId
    					Port
    				Remote
    					IpAddr
    					Port
    			Ind
    				UDP
    					SocketCnf

    Message Mismatch: IP_SOCKET_IND

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 53
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    Received on port: IPMUX_PTC:IP_SOCK

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = 53
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit

    Sent from port: IP_PTC:IP_CTRL

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    Received on port: IP_PTC:IP_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.55'
    				Port = 67
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.55'
    				Port = 67
    			Remote = Omit
    		Req
    			UDP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Sent from port: IPMUX_PTC:IP_SOCK

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		CTRL
    			ConnectionId
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote
    					IpAddr = Omit
    					Port = Omit
    			Ind
    				UDP
    					SocketCnf = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		DATA
    			ConnectionId
    				Protocol
    				Local
    					IpAddr
    						V4
    							Addr
    					Port
    				Remote
    					IpAddr
    					Port
    			Ind
    				UDP
    					SocketCnf

    Message Mismatch: IP_SOCKET_IND

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.55'
    				Port = 67
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    Received on port: IPMUX_PTC:IP_SOCK

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = udp (0)
    			Local
    				IpAddr
    					V4
    						Addr = '192.168.198.55'
    				Port = 67
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			UDP
    				SocketCnf = True

    Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.Port
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.Port
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    			Port = 67
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.Port

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'
    					ScopeId
    			Port = 67
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit

    Sent from port: IP_PTC:IP_CTRL

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    Received on port: IP_PTC:IP_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = Omit
    			Remote = Omit
    		Req
    			ICMP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = Omit
    			Remote = Omit
    		Req
    			ICMP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Sent from port: IPMUX_PTC:IP_SOCK

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		CTRL
    			ConnectionId
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote
    					IpAddr = Omit
    					Port = Omit
    			Ind
    				ICMP
    					SocketCnf = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		DATA
    			ConnectionId
    				Protocol
    				Local
    					IpAddr
    						V6
    							Addr
    							ScopeId
    					Port
    				Remote
    					IpAddr
    					Port
    			Ind
    				ICMP
    					SocketCnf

    Message Mismatch: IP_SOCKET_IND

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = Omit
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			ICMP
    				SocketCnf = True

    Received on port: IPMUX_PTC:IP_SOCK

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = Omit
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			ICMP
    				SocketCnf = True

    Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit

    Sent from port: IP_PTC:IP_CTRL

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    Received on port: IP_PTC:IP_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = Omit
    			Remote = Omit
    		Req
    			ICMP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Inter-component message: IP_SOCK_CTRL -> IPMUX_PTC:IP_SOCK_CTRL

    IP_SOCKET_REQ
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = Omit
    			Remote = Omit
    		Req
    			ICMP
    				SocketReq
    					SockOptList
    						IP_SockOpt_Type
    							SO_BROADCAST = True
    						IP_SockOpt_Type
    							IP_MTU_SIZE = 1500

    Sent from port: IPMUX_PTC:IP_SOCK

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		CTRL
    			ConnectionId
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote
    					IpAddr = Omit
    					Port = Omit
    			Ind
    				ICMP
    					SocketCnf = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_SOCKET_IND
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND
    		DATA
    			ConnectionId
    				Protocol
    				Local
    					IpAddr
    						V6
    							Addr
    							ScopeId
    					Port
    				Remote
    					IpAddr
    					Port
    			Ind
    				ICMP
    					SocketCnf

    Message Mismatch: IP_SOCKET_IND

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = Omit
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			ICMP
    				SocketCnf = True

    Received on port: IPMUX_PTC:IP_SOCK

    IP_SOCKET_IND
    	CTRL
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = Omit
    			Remote
    				IpAddr = Omit
    				Port = Omit
    		Ind
    			ICMP
    				SocketCnf = True

    Inter-component message: IP_SOCK_CTRL -> IP_PTC:IP_SOCK_CTRL

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = 53
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = udp (0)
    		Local
    			IpAddr
    				V4
    					Addr = '192.168.198.55'

    			Port = 67
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Protocol
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Protocol
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Protocol

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    MATCH_MISMATCH
    	Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr
    		Protocol = icmpv6 (3)
    		Local
    			IpAddr
    				V6
    					Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    					ScopeId = Omit
    			Port = Omit
    		Remote = Omit

    Message Mismatch: IP_Connection_Type.Local.IpAddr.V6.Addr

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 8
    			DataMode = Omit

    Sent from port: IP_PTC:IP_CTRL

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    Received on port: IP_PTC:IP_CTRL

    IP_Indication_Type
    	Cnf = True

    Inter-component message: IP -> EUTRA_5GS_PTC:IP

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		RadioBearerList
    			RadioBearer_Type
    				Id
    					Drb = 1
    				Config
    					AddOrReconfigure
    						Pdcp
    							Config
    								Rb
    									Drb
    										R8
    											discardTimer = infinity_ (7)
    											rlc_AM
    												statusReportRequired = True
    											rlc_UM = Omit
    											headerCompression
    												notUsed = Null
    											rn_IntegrityProtection_r10 = Omit
    											pdcp_SN_Size_v1130 = Omit
    											ul_DataSplitDRB_ViaSCG_r12 = Omit
    											t_Reordering_r12 = Omit
    											ul_DataSplitThreshold_r13 = Omit
    											pdcp_SN_Size_v1310 = Omit
    											statusFeedback_r13 = Omit
    											ul_LWA_Config_r14 = Omit
    											uplinkOnlyHeaderCompression_r14 = Omit
    											uplinkDataCompression_r15 = Omit
    											pdcp_DuplicationConfig_r15 = Omit
    								TestMode
    									None = True
    						Rlc
    							Rb
    								AM
    									Tx
    										R8
    											t_PollRetransmit = ms80 (15)
    											pollPDU = p128 (5)
    											pollByte = kB125 (4)
    											maxRetxThreshold = t4 (3)
    									Rx
    										R8
    											t_Reordering = ms80 (16)
    											t_StatusProhibit = ms60 (12)
    									ExtendedLI = Omit
    							TestMode
    								None = True
    						LogicalChannelId = 3
    						Mac
    							LogicalChannel
    								Priority = 13
    								PrioritizedBitRate = kBps0 (0)
    								LAA_UL_Allowed = Omit
    							TestMode
    								None = True
    						DiscardULData = Omit
    			RadioBearer_Type
    				Id
    					Drb = 8
    				Config
    					AddOrReconfigure
    						Pdcp
    							Config
    								Rb
    									Drb
    										R8
    											discardTimer = infinity_ (7)
    											rlc_AM
    												statusReportRequired = True
    											rlc_UM = Omit
    											headerCompression
    												notUsed = Null
    											rn_IntegrityProtection_r10 = Omit
    											pdcp_SN_Size_v1130 = Omit
    											ul_DataSplitDRB_ViaSCG_r12 = Omit
    											t_Reordering_r12 = Omit
    											ul_DataSplitThreshold_r13 = Omit
    											pdcp_SN_Size_v1310 = Omit
    											statusFeedback_r13 = Omit
    											ul_LWA_Config_r14 = Omit
    											uplinkOnlyHeaderCompression_r14 = Omit
    											uplinkDataCompression_r15 = Omit
    											pdcp_DuplicationConfig_r15 = Omit
    								TestMode
    									None = True
    						Rlc
    							Rb
    								AM
    									Tx
    										R8
    											t_PollRetransmit = ms80 (15)
    											pollPDU = p128 (5)
    											pollByte = kB125 (4)
    											maxRetxThreshold = t4 (3)
    									Rx
    										R8
    											t_Reordering = ms80 (16)
    											t_StatusProhibit = ms60 (12)
    									ExtendedLI = Omit
    							TestMode
    								None = True
    						LogicalChannelId = 10
    						Mac
    							LogicalChannel
    								Priority = 13
    								PrioritizedBitRate = kBps0 (0)
    								LAA_UL_Allowed = Omit
    							TestMode
    								None = True
    						DiscardULData = Omit

    Sent from port: EUTRA_5GS_PTC:SYS

    SYSTEM_CTRL_CNF
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		RadioBearerList = True

    Received on port: EUTRA_5GS_PTC:SYS

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		PdcpCount
    			Get
    				AllRBs = True

    Sent from port: EUTRA_5GS_PTC:SYS

    SYSTEM_CTRL_CNF
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		PdcpCount
    			Get
    				PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 1
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000100'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000011'B
    				PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 2
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    				PdcpCountInfo_Type
    					RadioBearerId
    						Drb = 1
    					UL
    						Format = PdcpCount_DrbLongSQN (1)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_DrbLongSQN (1)
    						Value = 00000000000000000000000000000000'B
    				PdcpCountInfo_Type
    					RadioBearerId
    						Drb = 8
    					UL
    						Format = PdcpCount_DrbLongSQN (1)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_DrbLongSQN (1)
    						Value = 00000000000000000000000000000000'B

    Received on port: EUTRA_5GS_PTC:SYS

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		AS_Security
    			StartRestart
    				Integrity
    					Algorithm = eia1 (1)
    					KRRCint = 10001100011101101101010000010100100110110001001111000110110100001011000111101111101101010100111100101100100100110000111000100100'B
    					ActTimeList = Omit
    				Ciphering
    					Algorithm = eea1 (1)
    					KRRCenc = 10011101101111111000111001000000000111100110010111101011111110001100011010011101010111000111111100011000110000001111111110111001'B
    					KUPenc = 01010000000101011110110101010000010000100010010010001011001001000011010001111100011001000111000100100010000100010011011111100000'B
    					ActTimeList
    						SecurityActTime_Type
    							RadioBearerId
    								Srb = 1
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 5
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 4
    						SecurityActTime_Type
    							RadioBearerId
    								Srb = 2
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 0
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 0
    						SecurityActTime_Type
    							RadioBearerId
    								Drb = 1
    							UL
    								SQN
    									Format = PdcpCount_DrbLongSQN (1)
    									Value = 0
    							DL
    								SQN
    									Format = PdcpCount_DrbLongSQN (1)
    									Value = 0
    						SecurityActTime_Type
    							RadioBearerId
    								Drb = 8
    							UL
    								SQN
    									Format = PdcpCount_DrbLongSQN (1)
    									Value = 0
    							DL
    								SQN
    									Format = PdcpCount_DrbLongSQN (1)
    									Value = 0

    Sent from port: EUTRA_5GS_PTC:SYS

    SYSTEM_CTRL_CNF
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		AS_Security = True

    Received on port: EUTRA_5GS_PTC:SYS

    SRB_COMMON_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						securityModeCommand
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								c1
    									securityModeCommand_r8
    										securityConfigSMC
    											securityAlgorithmConfig
    												cipheringAlgorithm = eea1 (1)
    												integrityProtAlgorithm = eia1 (1)
    										nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: TC_SRB -> NASEMU_EUTRA_PTC:TC_SRB

    DL-DCCH-Message
    	message = c1 = securityModeCommand =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = c1 = securityModeCommand-r8 =
    			securityConfigSMC
    				securityAlgorithmConfig
    					cipheringAlgorithm = eea1
    					integrityProtAlgorithm = eia1

    securityModeCommand

    RRC_PDU_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				c1
    					securityModeCommand
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							c1
    								securityModeCommand_r8
    									securityConfigSMC
    										securityAlgorithmConfig
    											cipheringAlgorithm = eea1 (1)
    											integrityProtAlgorithm = eia1 (1)
    									nonCriticalExtension = Omit

    Sent from port: NASEMU_EUTRA_PTC:SYS_SRB

    UL-DCCH-Message
    	message = c1 = securityModeComplete =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = securityModeComplete-r8 =

    securityModeComplete

    RRC_PDU_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 374
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				c1
    					securityModeComplete
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							securityModeComplete_r8
    								nonCriticalExtension = Omit

    Received on port: NASEMU_EUTRA_PTC:SYS_SRB

    SRB_COMMON_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 374
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						securityModeComplete
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								securityModeComplete_r8
    									nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: SRB -> EUTRA_5GS_PTC:SRB

    SRB_COMMON_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						ueCapabilityEnquiry
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								c1
    									ueCapabilityEnquiry_r8
    										ue_CapabilityRequest
    											RAT_Type = eutra (0)
    										nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: TC_SRB -> NASEMU_EUTRA_PTC:TC_SRB

    DL-DCCH-Message
    	message = c1 = ueCapabilityEnquiry =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = c1 = ueCapabilityEnquiry-r8 =
    			ue-CapabilityRequest = SEQUENCE OF RAT-Type
    				RAT-Type(1) = eutra

    ueCapabilityEnquiry

    RRC_PDU_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ueCapabilityEnquiry
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							c1
    								ueCapabilityEnquiry_r8
    									ue_CapabilityRequest
    										RAT_Type = eutra (0)
    									nonCriticalExtension = Omit

    Sent from port: NASEMU_EUTRA_PTC:SYS_SRB

    Sender = RequestServer
    Text = [!SWITCH_ON] Complete

    RequestServer:[!SWITCH_ON] Complete

    Sender = !SWITCH_ON
    Text = Stopping and Starting Serial Device Device Under Test

    !SWITCH_ON:Stopping and Starting Serial Device Device Under Test

    Sender = RequestServer
    Text = Device Device Under Test Disconnected

    RequestServer:Device Device Under Test Disconnected

    Sender = Device Under Test
    Text = Opening RS232 Port COM9,9600,None,8,One,None,Timeout:25000 ms

    Device Under Test:Opening RS232 Port COM9,9600,None,8,One,None,Timeout:25000 ms

    Sender = RequestServer
    Text = Device Device Under Test Connected

    RequestServer:Device Device Under Test Connected

    UL-DCCH-Message
    	message = c1 = ueCapabilityInformation =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = c1 = ueCapabilityInformation-r8 =
    			ue-CapabilityRAT-ContainerList = SEQUENCE OF UE-CapabilityRAT-Container
    				UE-CapabilityRAT-Container(1)
    					rat-Type = eutra
    					ueCapabilityRAT-Container =
    	UE-CapabilityRAT-Container(1)
    		UE-EUTRA-Capability
    			accessStratumRelease = rel15
    			ue-Category = 4
    			pdcp-Parameters
    				supportedROHC-Profiles
    					profile0x0001-r15 = TRUE
    					profile0x0002-r15 = TRUE
    					profile0x0003-r15 = FALSE
    					profile0x0004-r15 = FALSE
    					profile0x0006-r15 = FALSE
    					profile0x0101-r15 = FALSE
    					profile0x0102-r15 = FALSE
    					profile0x0103-r15 = FALSE
    					profile0x0104-r15 = FALSE
    				maxNumberROHC-ContextSessions = cs24
    			phyLayerParameters
    				ue-TxAntennaSelectionSupported = FALSE
    				ue-SpecificRefSigsSupported = FALSE
    			rf-Parameters
    				supportedBandListEUTRA = SEQUENCE OF SupportedBandEUTRA
    					SupportedBandEUTRA(1)
    						bandEUTRA = 5
    						halfDuplex = FALSE
    					SupportedBandEUTRA(2)
    						bandEUTRA = 64
    						halfDuplex = FALSE
    					SupportedBandEUTRA(3)
    						bandEUTRA = 1
    						halfDuplex = FALSE
    					SupportedBandEUTRA(4)
    						bandEUTRA = 3
    						halfDuplex = FALSE
    					SupportedBandEUTRA(5)
    						bandEUTRA = 4
    						halfDuplex = FALSE
    			measParameters
    				bandListEUTRA = SEQUENCE OF BandInfoEUTRA
    					BandInfoEUTRA(1)
    						interFreqBandList = SEQUENCE OF InterFreqBandInfo
    							InterFreqBandInfo(1)
    								interFreqNeedForGaps = TRUE
    							InterFreqBandInfo(2)
    								interFreqNeedForGaps = TRUE
    							InterFreqBandInfo(3)
    								interFreqNeedForGaps = TRUE
    							InterFreqBandInfo(4)
    								interFreqNeedForGaps = TRUE
    							InterFreqBandInfo(5)
    								interFreqNeedForGaps = TRUE
    						interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    							InterRAT-BandInfo(1)
    								interRAT-NeedForGaps = TRUE
    							InterRAT-BandInfo(2)
    								interRAT-NeedForGaps = TRUE
    							InterRAT-BandInfo(3)
    								interRAT-NeedForGaps = TRUE
    					BandInfoEUTRA(2)
    						interFreqBandList = SEQUENCE OF InterFreqBandInfo
    							InterFreqBandInfo(1)
    								interFreqNeedForGaps = TRUE
    							InterFreqBandInfo(2)
    								interFreqNeedForGaps = TRUE
    							InterFreqBandInfo(3)
    								interFreqNeedForGaps = TRUE
    							InterFreqBandInfo(4)
    								interFreqNeedForGaps = TRUE
    							InterFreqBandInfo(5)
    								interFreqNeedForGaps = TRUE
    						interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    							InterRAT-BandInfo(1)
    								interRAT-NeedForGaps = TRUE
    							InterRAT-BandInfo(2)
    								interRAT-NeedForGaps = TRUE
    							InterRAT-BandInfo(3)
    								interRAT-NeedForGaps = TRUE
    					BandInfoEUTRA(3)
    						interFreqBandList = SEQUENCE OF InterFreqBandInfo
    							InterFreqBandInfo(1)
    								interFreqNeedForGaps = TRUE
    							InterFreqBandInfo(2)
    								interFreqNeedForGaps = TRUE
    							InterFreqBandInfo(3)
    								interFreqNeedForGaps = TRUE
    							InterFreqBandInfo(4)
    								interFreqNeedForGaps = TRUE
    							InterFreqBandInfo(5)
    								interFreqNeedForGaps = TRUE
    						interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    							InterRAT-BandInfo(1)
    								interRAT-NeedForGaps = TRUE
    							InterRAT-BandInfo(2)
    								interRAT-NeedForGaps = TRUE
    							InterRAT-BandInfo(3)
    								interRAT-NeedForGaps = TRUE
    					BandInfoEUTRA(4)
    						interFreqBandList = SEQUENCE OF InterFreqBandInfo
    							InterFreqBandInfo(1)
    								interFreqNeedForGaps = TRUE
    							InterFreqBandInfo(2)
    								interFreqNeedForGaps = TRUE
    							InterFreqBandInfo(3)
    								interFreqNeedForGaps = TRUE
    							InterFreqBandInfo(4)
    								interFreqNeedForGaps = TRUE
    							InterFreqBandInfo(5)
    								interFreqNeedForGaps = TRUE
    						interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    							InterRAT-BandInfo(1)
    								interRAT-NeedForGaps = TRUE
    							InterRAT-BandInfo(2)
    								interRAT-NeedForGaps = TRUE
    							InterRAT-BandInfo(3)
    								interRAT-NeedForGaps = TRUE
    					BandInfoEUTRA(5)
    						interFreqBandList = SEQUENCE OF InterFreqBandInfo
    							InterFreqBandInfo(1)
    								interFreqNeedForGaps = TRUE
    							InterFreqBandInfo(2)
    								interFreqNeedForGaps = TRUE
    							InterFreqBandInfo(3)
    								interFreqNeedForGaps = TRUE
    							InterFreqBandInfo(4)
    								interFreqNeedForGaps = TRUE
    							InterFreqBandInfo(5)
    								interFreqNeedForGaps = TRUE
    						interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    							InterRAT-BandInfo(1)
    								interRAT-NeedForGaps = TRUE
    							InterRAT-BandInfo(2)
    								interRAT-NeedForGaps = TRUE
    							InterRAT-BandInfo(3)
    								interRAT-NeedForGaps = TRUE
    			featureGroupIndicators = 01111111000011111111110010111010
    			interRAT-Parameters
    				utraFDD
    					supportedBandListUTRA-FDD = SEQUENCE OF SupportedBandUTRA-FDD
    						SupportedBandUTRA-FDD(1) = bandVIII
    						SupportedBandUTRA-FDD(2) = bandIX
    						SupportedBandUTRA-FDD(3) = bandXIX-8a0
    			nonCriticalExtension
    				phyLayerParameters-v920
    				interRAT-ParametersGERAN-v920
    				interRAT-ParametersUTRA-v920
    					e-RedirectionUTRA-r9 = supported
    				csg-ProximityIndicationParameters-r9
    				neighCellSI-AcquisitionParameters-r9
    					intraFreqSI-AcquisitionForHO-r9 = supported
    					interFreqSI-AcquisitionForHO-r9 = supported
    				son-Parameters-r9
    					rach-Report-r9 = supported
    				nonCriticalExtension
    					lateNonCriticalExtension = CONTAINING =
    						featureGroupIndRel9Add-r9 = 10000000000000000000000000000000
    						nonCriticalExtension
    							nonCriticalExtension
    								nonCriticalExtension
    									rf-Parameters-v9e0
    										supportedBandListEUTRA-v9e0 = SEQUENCE OF SupportedBandEUTRA-v9e0
    											SupportedBandEUTRA-v9e0(1)
    											SupportedBandEUTRA-v9e0(2)
    												bandEUTRA-v9e0 = 66
    											SupportedBandEUTRA-v9e0(3)
    											SupportedBandEUTRA-v9e0(4)
    											SupportedBandEUTRA-v9e0(5)
    									nonCriticalExtension
    										nonCriticalExtension
    											otdoa-PositioningCapabilities-r10
    												otdoa-UE-Assisted-r10 = supported
    											nonCriticalExtension
    												rf-Parameters-v10f0
    													modifiedMPR-Behavior-r10 = 11000000000000000000000000000000
    												nonCriticalExtension
    													rf-Parameters-v10i0
    														supportedBandCombination-v10i0 = SEQUENCE OF BandCombinationParameters-v10i0
    															BandCombinationParameters-v10i0(1)
    															BandCombinationParameters-v10i0(2)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(3)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(4)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(5)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(6)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(7)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(8)
    															BandCombinationParameters-v10i0(9)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(10)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(11)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(12)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(13)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(14)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(15)
    															BandCombinationParameters-v10i0(16)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(17)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(18)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(19)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(20)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(21)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(22)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(23)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(24)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(25)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(26)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(27)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(28)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(29)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(30)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(4)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(31)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(4)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(32)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(4)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(33)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(4)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(34)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(4)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(35)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(36)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(37)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(38)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(39)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(40)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(41)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(42)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(43)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(44)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(45)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(46)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(47)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(48)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(49)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(50)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(51)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(52)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(53)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(54)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(55)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(56)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(57)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(58)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(59)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(60)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(61)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(62)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(63)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(64)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(65)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(66)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(67)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(68)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(69)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(4)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(70)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(4)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(71)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(72)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(73)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(74)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(75)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(76)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(77)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(78)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(79)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(80)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(81)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(82)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(83)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(84)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(85)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(86)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(87)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(88)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(4)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(89)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(4)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(90)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(4)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(91)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(92)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(93)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(94)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(95)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(96)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(97)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(98)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(99)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(100)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(101)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(102)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(103)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(104)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(105)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(106)
    															BandCombinationParameters-v10i0(107)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(108)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(109)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(110)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(111)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(112)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(113)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(114)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(115)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(116)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(117)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(118)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(119)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(120)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(121)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    															BandCombinationParameters-v10i0(122)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(123)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(124)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(3)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(125)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(126)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(127)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    															BandCombinationParameters-v10i0(128)
    																bandParameterList-v10i0 = SEQUENCE OF BandParameters-v10i0
    																	BandParameters-v10i0(1)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    																	BandParameters-v10i0(2)
    																		bandParametersDL-v10i0 = SEQUENCE OF CA-MIMO-ParametersDL-v10i0
    																			CA-MIMO-ParametersDL-v10i0(1)
    																				fourLayerTM3-TM4-r10 = supported
    													nonCriticalExtension
    														nonCriticalExtension
    															nonCriticalExtension
    																rf-Parameters-v12b0
    																	maxLayersMIMO-Indication-r12 = supported
    					nonCriticalExtension
    						ue-Category-v1020 = 7
    						phyLayerParameters-v1020
    							tm9-With-8Tx-FDD-r10 = supported
    							multiClusterPUSCH-WithinCC-r10 = supported
    							nonContiguousUL-RA-WithinCC-List-r10 = SEQUENCE OF NonContiguousUL-RA-WithinCC-r10
    								NonContiguousUL-RA-WithinCC-r10(1)
    									nonContiguousUL-RA-WithinCC-Info-r10 = supported
    								NonContiguousUL-RA-WithinCC-r10(2)
    								NonContiguousUL-RA-WithinCC-r10(3)
    								NonContiguousUL-RA-WithinCC-r10(4)
    									nonContiguousUL-RA-WithinCC-Info-r10 = supported
    								NonContiguousUL-RA-WithinCC-r10(5)
    									nonContiguousUL-RA-WithinCC-Info-r10 = supported
    						rf-Parameters-v1020
    							supportedBandCombination-r10 = SEQUENCE OF BandCombinationParameters-r10
    								BandCombinationParameters-r10(1) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(2) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(3) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 1
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(4) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 3
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(5) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 4
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(6) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(7) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(8) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(9) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 4
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(10) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 4
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(11) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 3
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(12) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 3
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(13) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(14) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 1
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(15) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(16) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(17) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 4
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(18) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 4
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(19) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(20) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(21) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 3
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(22) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 3
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 1
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(23) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 1
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(24) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 1
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(25) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 3
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 3
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(26) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 3
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(27) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 3
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(28) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 4
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 4
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(29) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 4
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(30) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(4)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(31) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(4)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(32) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(4)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(33) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(4)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(34) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(4)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(35) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(36) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(37) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(38) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(39) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(40) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(41) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(42) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(43) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(44) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(45) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(46) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(47) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(48) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(49) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(50) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(51) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(52) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(53) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(54) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(55) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(56) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(57) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = d
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(58) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = d
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(59) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(60) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(61) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(62) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(63) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(64) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(65) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(66) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(67) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(68) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(69) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 4
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(4)
    										bandEUTRA-r10 = 4
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(70) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 4
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(4)
    										bandEUTRA-r10 = 4
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(71) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 4
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(72) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 4
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(73) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 4
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(74) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 4
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(75) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 4
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 4
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(76) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 4
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 4
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(77) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 4
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 4
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(78) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 4
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 4
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(79) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 4
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(80) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 4
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(81) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 4
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(82) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 4
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(83) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 4
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(84) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 4
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(85) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 4
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(86) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 3
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 3
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(87) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 3
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 3
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(88) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 3
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(4)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(89) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 3
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(4)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(90) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 3
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 1
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(4)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(91) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 3
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(92) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 3
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(93) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 3
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 1
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(94) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 3
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(95) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 3
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(96) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 3
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 1
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(97) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 3
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(98) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 3
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(99) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 3
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 1
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(100) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 3
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(101) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 3
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(102) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 3
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(103) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 3
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(104) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(105) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 1
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(106) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 5
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = b
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(107) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(108) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(109) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(110) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(111) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(112) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = d
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(113) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = c
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(114) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 64
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = b
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(115) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 3
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 3
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(116) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 3
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 3
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 1
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(117) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 3
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(118) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 3
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 1
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(119) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 3
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 1
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(120) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 3
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(121) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 3
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 1
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    								BandCombinationParameters-r10(122) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 3
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = b
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 1
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = twoLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(123) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 3
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(124) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 3
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 1
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(3)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(125) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 3
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(126) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 3
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 1
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(127) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 3
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = c
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    								BandCombinationParameters-r10(128) = SEQUENCE OF BandParameters-r10
    									BandParameters-r10(1)
    										bandEUTRA-r10 = 3
    										bandParametersUL-r10 = SEQUENCE OF CA-MIMO-ParametersUL-r10
    											CA-MIMO-ParametersUL-r10(1)
    												ca-BandwidthClassUL-r10 = a
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = c
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    									BandParameters-r10(2)
    										bandEUTRA-r10 = 1
    										bandParametersDL-r10 = SEQUENCE OF CA-MIMO-ParametersDL-r10
    											CA-MIMO-ParametersDL-r10(1)
    												ca-BandwidthClassDL-r10 = a
    												supportedMIMO-CapabilityDL-r10 = fourLayers
    						measParameters-v1020
    							bandCombinationListEUTRA-r10 = SEQUENCE OF BandInfoEUTRA
    								BandInfoEUTRA(1)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(2)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(3)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(4)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(5)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(6)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(7)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(8)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(9)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(10)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(11)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(12)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(13)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(14)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(15)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(16)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(17)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(18)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(19)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(20)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(21)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(22)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(23)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(24)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(25)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(26)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(27)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(28)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(29)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(30)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(31)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(32)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(33)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(34)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(35)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(36)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(37)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(38)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(39)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(40)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(41)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(42)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(43)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(44)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(45)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(46)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(47)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(48)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(49)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(50)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(51)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(52)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(53)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(54)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(55)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(56)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(57)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(58)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(59)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(60)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(61)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(62)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(63)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(64)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(65)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(66)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(67)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(68)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(69)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(70)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(71)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(72)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(73)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(74)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(75)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(76)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(77)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(78)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(79)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(80)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(81)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(82)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(83)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(84)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(85)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(86)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(87)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(88)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(89)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(90)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(91)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(92)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(93)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(94)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(95)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(96)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(97)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(98)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(99)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(100)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(101)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(102)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(103)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(104)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(105)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(106)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(107)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(108)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(109)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(110)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(111)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(112)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(113)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(114)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(115)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(116)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(117)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(118)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(119)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(120)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(121)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(122)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(123)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(124)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(125)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(126)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(127)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    								BandInfoEUTRA(128)
    									interFreqBandList = SEQUENCE OF InterFreqBandInfo
    										InterFreqBandInfo(1)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(2)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(3)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(4)
    											interFreqNeedForGaps = TRUE
    										InterFreqBandInfo(5)
    											interFreqNeedForGaps = TRUE
    									interRAT-BandList = SEQUENCE OF InterRAT-BandInfo
    										InterRAT-BandInfo(1)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(2)
    											interRAT-NeedForGaps = TRUE
    										InterRAT-BandInfo(3)
    											interRAT-NeedForGaps = TRUE
    						featureGroupIndRel10-r10 = 01101100111011000000000000000000
    						ue-BasedNetwPerfMeasParameters-r10
    							loggedMeasurementsIdle-r10 = supported
    							standaloneGNSS-Location-r10 = supported
    						nonCriticalExtension
    							rf-Parameters-v1060
    								supportedBandCombinationExt-r10 = SEQUENCE OF BandCombinationParametersExt-r10
    									BandCombinationParametersExt-r10(1)
    									BandCombinationParametersExt-r10(2)
    									BandCombinationParametersExt-r10(3)
    									BandCombinationParametersExt-r10(4)
    									BandCombinationParametersExt-r10(5)
    									BandCombinationParametersExt-r10(6)
    									BandCombinationParametersExt-r10(7)
    									BandCombinationParametersExt-r10(8)
    										supportedBandwidthCombinationSet-r10 = 11
    									BandCombinationParametersExt-r10(9)
    										supportedBandwidthCombinationSet-r10 = 11
    									BandCombinationParametersExt-r10(10)
    										supportedBandwidthCombinationSet-r10 = 11
    									BandCombinationParametersExt-r10(11)
    										supportedBandwidthCombinationSet-r10 = 11111
    									BandCombinationParametersExt-r10(12)
    										supportedBandwidthCombinationSet-r10 = 11111
    									BandCombinationParametersExt-r10(13)
    										supportedBandwidthCombinationSet-r10 = 11
    									BandCombinationParametersExt-r10(14)
    										supportedBandwidthCombinationSet-r10 = 11
    									BandCombinationParametersExt-r10(15)
    										supportedBandwidthCombinationSet-r10 = 11
    									BandCombinationParametersExt-r10(16)
    									BandCombinationParametersExt-r10(17)
    									BandCombinationParametersExt-r10(18)
    									BandCombinationParametersExt-r10(19)
    									BandCombinationParametersExt-r10(20)
    									BandCombinationParametersExt-r10(21)
    										supportedBandwidthCombinationSet-r10 = 11
    									BandCombinationParametersExt-r10(22)
    										supportedBandwidthCombinationSet-r10 = 11
    									BandCombinationParametersExt-r10(23)
    									BandCombinationParametersExt-r10(24)
    										supportedBandwidthCombinationSet-r10 = 11
    									BandCombinationParametersExt-r10(25)
    										supportedBandwidthCombinationSet-r10 = 111
    									BandCombinationParametersExt-r10(26)
    									BandCombinationParametersExt-r10(27)
    									BandCombinationParametersExt-r10(28)
    										supportedBandwidthCombinationSet-r10 = 11
    									BandCombinationParametersExt-r10(29)
    									BandCombinationParametersExt-r10(30)
    									BandCombinationParametersExt-r10(31)
    									BandCombinationParametersExt-r10(32)
    									BandCombinationParametersExt-r10(33)
    									BandCombinationParametersExt-r10(34)
    									BandCombinationParametersExt-r10(35)
    									BandCombinationParametersExt-r10(36)
    									BandCombinationParametersExt-r10(37)
    									BandCombinationParametersExt-r10(38)
    									BandCombinationParametersExt-r10(39)
    									BandCombinationParametersExt-r10(40)
    									BandCombinationParametersExt-r10(41)
    									BandCombinationParametersExt-r10(42)
    									BandCombinationParametersExt-r10(43)
    									BandCombinationParametersExt-r10(44)
    									BandCombinationParametersExt-r10(45)
    									BandCombinationParametersExt-r10(46)
    									BandCombinationParametersExt-r10(47)
    									BandCombinationParametersExt-r10(48)
    									BandCombinationParametersExt-r10(49)
    									BandCombinationParametersExt-r10(50)
    									BandCombinationParametersExt-r10(51)
    									BandCombinationParametersExt-r10(52)
    									BandCombinationParametersExt-r10(53)
    									BandCombinationParametersExt-r10(54)
    									BandCombinationParametersExt-r10(55)
    									BandCombinationParametersExt-r10(56)
    									BandCombinationParametersExt-r10(57)
    									BandCombinationParametersExt-r10(58)
    									BandCombinationParametersExt-r10(59)
    									BandCombinationParametersExt-r10(60)
    									BandCombinationParametersExt-r10(61)
    									BandCombinationParametersExt-r10(62)
    									BandCombinationParametersExt-r10(63)
    									BandCombinationParametersExt-r10(64)
    									BandCombinationParametersExt-r10(65)
    									BandCombinationParametersExt-r10(66)
    									BandCombinationParametersExt-r10(67)
    									BandCombinationParametersExt-r10(68)
    									BandCombinationParametersExt-r10(69)
    									BandCombinationParametersExt-r10(70)
    									BandCombinationParametersExt-r10(71)
    									BandCombinationParametersExt-r10(72)
    									BandCombinationParametersExt-r10(73)
    									BandCombinationParametersExt-r10(74)
    									BandCombinationParametersExt-r10(75)
    									BandCombinationParametersExt-r10(76)
    									BandCombinationParametersExt-r10(77)
    									BandCombinationParametersExt-r10(78)
    									BandCombinationParametersExt-r10(79)
    									BandCombinationParametersExt-r10(80)
    									BandCombinationParametersExt-r10(81)
    									BandCombinationParametersExt-r10(82)
    									BandCombinationParametersExt-r10(83)
    									BandCombinationParametersExt-r10(84)
    									BandCombinationParametersExt-r10(85)
    										supportedBandwidthCombinationSet-r10 = 11
    									BandCombinationParametersExt-r10(86)
    									BandCombinationParametersExt-r10(87)
    									BandCombinationParametersExt-r10(88)
    									BandCombinationParametersExt-r10(89)
    									BandCombinationParametersExt-r10(90)
    									BandCombinationParametersExt-r10(91)
    									BandCombinationParametersExt-r10(92)
    									BandCombinationParametersExt-r10(93)
    									BandCombinationParametersExt-r10(94)
    									BandCombinationParametersExt-r10(95)
    									BandCombinationParametersExt-r10(96)
    									BandCombinationParametersExt-r10(97)
    										supportedBandwidthCombinationSet-r10 = 11
    									BandCombinationParametersExt-r10(98)
    										supportedBandwidthCombinationSet-r10 = 11
    									BandCombinationParametersExt-r10(99)
    										supportedBandwidthCombinationSet-r10 = 11
    									BandCombinationParametersExt-r10(100)
    									BandCombinationParametersExt-r10(101)
    									BandCombinationParametersExt-r10(102)
    									BandCombinationParametersExt-r10(103)
    									BandCombinationParametersExt-r10(104)
    									BandCombinationParametersExt-r10(105)
    									BandCombinationParametersExt-r10(106)
    										supportedBandwidthCombinationSet-r10 = 11
    									BandCombinationParametersExt-r10(107)
    									BandCombinationParametersExt-r10(108)
    									BandCombinationParametersExt-r10(109)
    									BandCombinationParametersExt-r10(110)
    									BandCombinationParametersExt-r10(111)
    									BandCombinationParametersExt-r10(112)
    									BandCombinationParametersExt-r10(113)
    									BandCombinationParametersExt-r10(114)
    									BandCombinationParametersExt-r10(115)
    									BandCombinationParametersExt-r10(116)
    									BandCombinationParametersExt-r10(117)
    									BandCombinationParametersExt-r10(118)
    									BandCombinationParametersExt-r10(119)
    									BandCombinationParametersExt-r10(120)
    									BandCombinationParametersExt-r10(121)
    									BandCombinationParametersExt-r10(122)
    									BandCombinationParametersExt-r10(123)
    									BandCombinationParametersExt-r10(124)
    									BandCombinationParametersExt-r10(125)
    									BandCombinationParametersExt-r10(126)
    									BandCombinationParametersExt-r10(127)
    									BandCombinationParametersExt-r10(128)
    							nonCriticalExtension
    								rf-Parameters-v1090
    									supportedBandCombination-v1090 = SEQUENCE OF BandCombinationParameters-v1090
    										BandCombinationParameters-v1090(1) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    										BandCombinationParameters-v1090(2) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    										BandCombinationParameters-v1090(3) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    										BandCombinationParameters-v1090(4) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    										BandCombinationParameters-v1090(5) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    										BandCombinationParameters-v1090(6) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(7) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(8) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(9) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(10) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(11) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(12) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(13) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(14) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(15) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    										BandCombinationParameters-v1090(16) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    												bandEUTRA-v1090 = 66
    										BandCombinationParameters-v1090(17) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(18) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(19) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    										BandCombinationParameters-v1090(20) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    										BandCombinationParameters-v1090(21) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(22) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(23) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(24) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    										BandCombinationParameters-v1090(25) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(26) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    										BandCombinationParameters-v1090(27) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    										BandCombinationParameters-v1090(28) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(29) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    										BandCombinationParameters-v1090(30) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(3)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(4)
    										BandCombinationParameters-v1090(31) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(3)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(4)
    										BandCombinationParameters-v1090(32) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(3)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(4)
    										BandCombinationParameters-v1090(33) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(3)
    											BandParameters-v1090(4)
    										BandCombinationParameters-v1090(34) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(3)
    											BandParameters-v1090(4)
    										BandCombinationParameters-v1090(35) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(36) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(37) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(38) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(39) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(40) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(41) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(42) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(43) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(44) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(45) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(46) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(47) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(48) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(49) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(50) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(51) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(52) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(53) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(54) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(55) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(56) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(57) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(58) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(59) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(60) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(61) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(62) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(63) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(64) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(65) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(66) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(67) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(68) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(69) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    											BandParameters-v1090(4)
    										BandCombinationParameters-v1090(70) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    											BandParameters-v1090(4)
    										BandCombinationParameters-v1090(71) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(72) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(73) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(74) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(75) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(76) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(77) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(78) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(79) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(80) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(81) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(82) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(83) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(84) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(85) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(86) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(87) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(88) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    											BandParameters-v1090(4)
    										BandCombinationParameters-v1090(89) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    											BandParameters-v1090(4)
    										BandCombinationParameters-v1090(90) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    											BandParameters-v1090(4)
    										BandCombinationParameters-v1090(91) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(92) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(93) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(94) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(95) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(96) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(97) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(98) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(99) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(100) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(101) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(102) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(103) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(104) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(105) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(106) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    										BandCombinationParameters-v1090(107) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(3)
    												bandEUTRA-v1090 = 66
    										BandCombinationParameters-v1090(108) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    												bandEUTRA-v1090 = 66
    										BandCombinationParameters-v1090(109) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    												bandEUTRA-v1090 = 66
    										BandCombinationParameters-v1090(110) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    												bandEUTRA-v1090 = 66
    										BandCombinationParameters-v1090(111) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    											BandParameters-v1090(2)
    												bandEUTRA-v1090 = 66
    										BandCombinationParameters-v1090(112) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    										BandCombinationParameters-v1090(113) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    										BandCombinationParameters-v1090(114) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    												bandEUTRA-v1090 = 66
    										BandCombinationParameters-v1090(115) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(116) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(117) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(118) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(119) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(120) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(121) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(122) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(123) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(124) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    											BandParameters-v1090(3)
    										BandCombinationParameters-v1090(125) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(126) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(127) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    										BandCombinationParameters-v1090(128) = SEQUENCE OF BandParameters-v1090
    											BandParameters-v1090(1)
    											BandParameters-v1090(2)
    								nonCriticalExtension
    									pdcp-Parameters-v1130
    										pdcp-SN-Extension-r11 = supported
    									phyLayerParameters-v1130
    										crs-InterfHandl-r11 = supported
    									rf-Parameters-v1130
    										supportedBandCombination-v1130 = SEQUENCE OF BandCombinationParameters-v1130
    											BandCombinationParameters-v1130(1)
    											BandCombinationParameters-v1130(2)
    											BandCombinationParameters-v1130(3)
    											BandCombinationParameters-v1130(4)
    											BandCombinationParameters-v1130(5)
    											BandCombinationParameters-v1130(6)
    											BandCombinationParameters-v1130(7)
    											BandCombinationParameters-v1130(8)
    											BandCombinationParameters-v1130(9)
    											BandCombinationParameters-v1130(10)
    											BandCombinationParameters-v1130(11)
    											BandCombinationParameters-v1130(12)
    											BandCombinationParameters-v1130(13)
    											BandCombinationParameters-v1130(14)
    											BandCombinationParameters-v1130(15)
    											BandCombinationParameters-v1130(16)
    											BandCombinationParameters-v1130(17)
    											BandCombinationParameters-v1130(18)
    											BandCombinationParameters-v1130(19)
    											BandCombinationParameters-v1130(20)
    											BandCombinationParameters-v1130(21)
    											BandCombinationParameters-v1130(22)
    											BandCombinationParameters-v1130(23)
    											BandCombinationParameters-v1130(24)
    											BandCombinationParameters-v1130(25)
    											BandCombinationParameters-v1130(26)
    											BandCombinationParameters-v1130(27)
    											BandCombinationParameters-v1130(28)
    											BandCombinationParameters-v1130(29)
    											BandCombinationParameters-v1130(30)
    											BandCombinationParameters-v1130(31)
    											BandCombinationParameters-v1130(32)
    											BandCombinationParameters-v1130(33)
    											BandCombinationParameters-v1130(34)
    											BandCombinationParameters-v1130(35)
    											BandCombinationParameters-v1130(36)
    											BandCombinationParameters-v1130(37)
    											BandCombinationParameters-v1130(38)
    											BandCombinationParameters-v1130(39)
    											BandCombinationParameters-v1130(40)
    											BandCombinationParameters-v1130(41)
    											BandCombinationParameters-v1130(42)
    											BandCombinationParameters-v1130(43)
    											BandCombinationParameters-v1130(44)
    											BandCombinationParameters-v1130(45)
    											BandCombinationParameters-v1130(46)
    											BandCombinationParameters-v1130(47)
    											BandCombinationParameters-v1130(48)
    											BandCombinationParameters-v1130(49)
    											BandCombinationParameters-v1130(50)
    											BandCombinationParameters-v1130(51)
    											BandCombinationParameters-v1130(52)
    											BandCombinationParameters-v1130(53)
    											BandCombinationParameters-v1130(54)
    											BandCombinationParameters-v1130(55)
    											BandCombinationParameters-v1130(56)
    											BandCombinationParameters-v1130(57)
    											BandCombinationParameters-v1130(58)
    											BandCombinationParameters-v1130(59)
    											BandCombinationParameters-v1130(60)
    											BandCombinationParameters-v1130(61)
    											BandCombinationParameters-v1130(62)
    											BandCombinationParameters-v1130(63)
    											BandCombinationParameters-v1130(64)
    											BandCombinationParameters-v1130(65)
    											BandCombinationParameters-v1130(66)
    											BandCombinationParameters-v1130(67)
    											BandCombinationParameters-v1130(68)
    											BandCombinationParameters-v1130(69)
    											BandCombinationParameters-v1130(70)
    											BandCombinationParameters-v1130(71)
    											BandCombinationParameters-v1130(72)
    											BandCombinationParameters-v1130(73)
    											BandCombinationParameters-v1130(74)
    											BandCombinationParameters-v1130(75)
    											BandCombinationParameters-v1130(76)
    											BandCombinationParameters-v1130(77)
    											BandCombinationParameters-v1130(78)
    											BandCombinationParameters-v1130(79)
    											BandCombinationParameters-v1130(80)
    											BandCombinationParameters-v1130(81)
    											BandCombinationParameters-v1130(82)
    											BandCombinationParameters-v1130(83)
    											BandCombinationParameters-v1130(84)
    											BandCombinationParameters-v1130(85)
    												multipleTimingAdvance-r11 = supported
    											BandCombinationParameters-v1130(86)
    											BandCombinationParameters-v1130(87)
    											BandCombinationParameters-v1130(88)
    											BandCombinationParameters-v1130(89)
    											BandCombinationParameters-v1130(90)
    											BandCombinationParameters-v1130(91)
    											BandCombinationParameters-v1130(92)
    											BandCombinationParameters-v1130(93)
    											BandCombinationParameters-v1130(94)
    											BandCombinationParameters-v1130(95)
    											BandCombinationParameters-v1130(96)
    											BandCombinationParameters-v1130(97)
    											BandCombinationParameters-v1130(98)
    											BandCombinationParameters-v1130(99)
    											BandCombinationParameters-v1130(100)
    											BandCombinationParameters-v1130(101)
    											BandCombinationParameters-v1130(102)
    											BandCombinationParameters-v1130(103)
    											BandCombinationParameters-v1130(104)
    											BandCombinationParameters-v1130(105)
    											BandCombinationParameters-v1130(106)
    											BandCombinationParameters-v1130(107)
    											BandCombinationParameters-v1130(108)
    											BandCombinationParameters-v1130(109)
    											BandCombinationParameters-v1130(110)
    											BandCombinationParameters-v1130(111)
    											BandCombinationParameters-v1130(112)
    											BandCombinationParameters-v1130(113)
    											BandCombinationParameters-v1130(114)
    											BandCombinationParameters-v1130(115)
    											BandCombinationParameters-v1130(116)
    											BandCombinationParameters-v1130(117)
    											BandCombinationParameters-v1130(118)
    											BandCombinationParameters-v1130(119)
    											BandCombinationParameters-v1130(120)
    											BandCombinationParameters-v1130(121)
    											BandCombinationParameters-v1130(122)
    											BandCombinationParameters-v1130(123)
    											BandCombinationParameters-v1130(124)
    											BandCombinationParameters-v1130(125)
    											BandCombinationParameters-v1130(126)
    											BandCombinationParameters-v1130(127)
    											BandCombinationParameters-v1130(128)
    									measParameters-v1130
    									interRAT-ParametersCDMA2000-v1130
    									otherParameters-r11
    									nonCriticalExtension
    										ue-Category-v1170 = 10
    										nonCriticalExtension
    											rf-Parameters-v1180
    												freqBandRetrieval-r11 = supported
    											nonCriticalExtension
    												ue-Category-v11a0 = 12
    												nonCriticalExtension
    													phyLayerParameters-v1250
    														discoverySignalsInDeactSCell-r12 = supported
    													rf-Parameters-v1250
    														supportedBandListEUTRA-v1250 = SEQUENCE OF SupportedBandEUTRA-v1250
    															SupportedBandEUTRA-v1250(1)
    																dl-256QAM-r12 = supported
    																ul-64QAM-r12 = supported
    															SupportedBandEUTRA-v1250(2)
    																dl-256QAM-r12 = supported
    																ul-64QAM-r12 = supported
    															SupportedBandEUTRA-v1250(3)
    																dl-256QAM-r12 = supported
    																ul-64QAM-r12 = supported
    															SupportedBandEUTRA-v1250(4)
    																dl-256QAM-r12 = supported
    																ul-64QAM-r12 = supported
    															SupportedBandEUTRA-v1250(5)
    																dl-256QAM-r12 = supported
    																ul-64QAM-r12 = supported
    														freqBandPriorityAdjustment-r12 = supported
    													ue-CategoryDL-r12 = 12
    													ue-CategoryUL-r12 = 13
    													measParameters-v1250
    														incMonEUTRA-r12 = supported
    														extendedMaxMeasId-r12 = supported
    														crs-DiscoverySignalsMeas-r12 = supported
    													nonCriticalExtension
    														ue-CategoryDL-v1260 = 16
    														nonCriticalExtension
    															nonCriticalExtension
    																phyLayerParameters-v1280
    																	alternativeTBS-Indices-r12 = supported
    																nonCriticalExtension
    																	pdcp-Parameters-v1310
    																		pdcp-SN-Extension-18bits-r13 = supported
    																	rlc-Parameters-v1310
    																		extendedRLC-SN-SO-Field-r13 = supported
    																	phyLayerParameters-v1310
    																		aperiodicCSI-Reporting-r13 = 01
    																		codebook-HARQ-ACK-r13 = 00
    																	measParameters-v1310
    																		extendedMaxObjectId-r13 = supported
    																	interRAT-ParametersWLAN-r13
    																	wlan-IW-Parameters-v1310
    																	lwip-Parameters-r13
    																	nonCriticalExtension
    																		nonCriticalExtension
    																			ue-CategoryDL-v1330 = 19
    																			nonCriticalExtension
    																				nonCriticalExtension
    																					ce-Parameters-v1350
    																					nonCriticalExtension
    																						nonCriticalExtension
    																							phyLayerParameters-v1430
    																								alternativeTBS-Index-r14 = supported
    																							rlc-Parameters-v1430
    																								extendedPollByte-r14 = supported
    																							otherParameters-v1430
    																							ce-Parameters-v1430
    																							nonCriticalExtension
    																								lwa-Parameters-v1440
    																								mac-Parameters-v1440
    																								nonCriticalExtension
    																									otherParameters-v1450
    																									nonCriticalExtension
    																										otherParameters-v1460
    																										nonCriticalExtension
    																											irat-ParametersNR-r15
    																												en-DC-r15 = supported
    																												supportedBandListNR-r15 = SEQUENCE OF SupportedBandNR-r15
    																													SupportedBandNR-r15(1)
    																														bandNR-r15 = 257
    																													SupportedBandNR-r15(2)
    																														bandNR-r15 = 260
    																													SupportedBandNR-r15(3)
    																														bandNR-r15 = 261
    																											pdcp-ParametersNR-r15
    																												rohc-Profiles-r15
    																													profile0x0001-r15 = FALSE
    																													profile0x0002-r15 = FALSE
    																													profile0x0003-r15 = FALSE
    																													profile0x0004-r15 = FALSE
    																													profile0x0006-r15 = FALSE
    																													profile0x0101-r15 = FALSE
    																													profile0x0102-r15 = FALSE
    																													profile0x0103-r15 = FALSE
    																													profile0x0104-r15 = FALSE
    																												rohc-ContextMaxSessions-r15  = cs16
    																												rohc-ProfilesUL-Only-r15
    																													profile0x0006-r15 = FALSE

    ueCapabilityInformation

    RRC_PDU_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 514
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ueCapabilityInformation
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							c1
    								ueCapabilityInformation_r8
    									ue_CapabilityRAT_ContainerList
    										UE_CapabilityRAT_Container
    											rat_Type = eutra (0)
    											ueCapabilityRAT_Container = ' 'O
    									nonCriticalExtension = Omit

    Received on port: NASEMU_EUTRA_PTC:SYS_SRB

    SRB_COMMON_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 514
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						ueCapabilityInformation
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								c1
    									ueCapabilityInformation_r8
    										ue_CapabilityRAT_ContainerList
    											UE_CapabilityRAT_Container
    												rat_Type = eutra (0)
    												ueCapabilityRAT_Container = ' 'O
    										nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: SRB -> EUTRA_5GS_PTC:SRB

    EUTRA_NR_Coordination_MSG
    	OctetData
    		Data = '05'O
    		Description = 'EUTRA Band'

    Inter-component message: EUTRA -> ENDC_NR_PTC:EUTRA

    EUTRA_NR_Coordination_MSG
    	OctetData
    		Data = '0020120818'O
    		Description = 'MRDC_Freq'

    Inter-component message: NR -> EUTRA_5GS_PTC:NR

    SRB_COMMON_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						ueCapabilityEnquiry
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								c1
    									ueCapabilityEnquiry_r8
    										ue_CapabilityRequest
    											RAT_Type = nr (5)
    											RAT_Type = eutra_nr (6)
    										nonCriticalExtension
    											lateNonCriticalExtension = Omit
    											nonCriticalExtension
    												requestedFrequencyBands_r11 = Omit
    												nonCriticalExtension
    													requestReducedFormat_r13 = Omit
    													requestSkipFallbackComb_r13 = Omit
    													requestedMaxCCsDL_r13 = Omit
    													requestedMaxCCsUL_r13 = Omit
    													requestReducedIntNonContComb_r13 = Omit
    													nonCriticalExtension
    														requestDiffFallbackCombList_r14 = Omit
    														nonCriticalExtension
    															requestedFreqBandsNR_MRDC_r15 = '0020120818'O
    															nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: TC_SRB -> NASEMU_EUTRA_PTC:TC_SRB

    DL-DCCH-Message
    	message = c1 = ueCapabilityEnquiry =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = c1 = ueCapabilityEnquiry-r8 =
    			ue-CapabilityRequest = SEQUENCE OF RAT-Type
    				RAT-Type(1) = nr
    				RAT-Type(2) = eutra-nr
    			nonCriticalExtension
    				nonCriticalExtension
    					nonCriticalExtension
    						nonCriticalExtension
    							nonCriticalExtension
    								requestedFreqBandsNR-MRDC-r15 = 0020120818

    ueCapabilityEnquiry

    RRC_PDU_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ueCapabilityEnquiry
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							c1
    								ueCapabilityEnquiry_r8
    									ue_CapabilityRequest
    										RAT_Type = nr (5)
    										RAT_Type = eutra_nr (6)
    									nonCriticalExtension
    										lateNonCriticalExtension = Omit
    										nonCriticalExtension
    											requestedFrequencyBands_r11 = Omit
    											nonCriticalExtension
    												requestReducedFormat_r13 = Omit
    												requestSkipFallbackComb_r13 = Omit
    												requestedMaxCCsDL_r13 = Omit
    												requestedMaxCCsUL_r13 = Omit
    												requestReducedIntNonContComb_r13 = Omit
    												nonCriticalExtension
    													requestDiffFallbackCombList_r14 = Omit
    													nonCriticalExtension
    														requestedFreqBandsNR_MRDC_r15 = '0020120818'O
    														nonCriticalExtension = Omit

    Sent from port: NASEMU_EUTRA_PTC:SYS_SRB

    UL-DCCH-Message
    	message = c1 = ueCapabilityInformation =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = c1 = ueCapabilityInformation-r8 =
    			ue-CapabilityRAT-ContainerList = SEQUENCE OF UE-CapabilityRAT-Container
    				UE-CapabilityRAT-Container(1)
    					rat-Type = nr
    					ueCapabilityRAT-Container = E1000000014F760302000001404807062E03000180084D8000408820402A03050080A01000A05A07BC71B438084478F904108A0223F6CB0C480081000408820402A031FBF9015D7001009040F13781100A01C00000000000000000000B80500600000000005C0280200000000B805000001700A00801004012E0140180200802009700A000012E01400800001700A00401004B005BA46E1008040100000208210403004010040120820040000082084100801004012082004010080220821040300C0300C032082004000088208410080300C032082004000048208403576A2BB115CA8AE440
    				UE-CapabilityRAT-Container(2)
    					rat-Type = eutra-nr
    					ueCapabilityRAT-Container =

    ueCapabilityInformation

    UE-NR-Capability
    	accessStratumRelease = rel15
    	pdcp-Parameters
    		supportedROHC-Profiles
    			profile0x0000 = FALSE
    			profile0x0001 = FALSE
    			profile0x0002 = FALSE
    			profile0x0003 = FALSE
    			profile0x0004 = FALSE
    			profile0x0006 = FALSE
    			profile0x0101 = FALSE
    			profile0x0102 = FALSE
    			profile0x0103 = FALSE
    			profile0x0104 = FALSE
    		maxNumberROHC-ContextSessions = cs2
    	rlc-Parameters
    		um-WithLongSN = supported
    	mac-Parameters
    		mac-ParametersXDD-Diff
    			logicalChannelSR-DelayTimer = supported
    			longDRX-Cycle = supported
    			shortDRX-Cycle = supported
    			multipleSR-Configurations = supported
    	phy-Parameters
    		phy-ParametersCommon
    			dynamicHARQ-ACK-Codebook = supported
    			semiStaticHARQ-ACK-Codebook = supported
    			pdsch-MappingTypeA = supported
    			maxLayersMIMO-Indication = supported
    		phy-ParametersXDD-Diff
    			twoDifferentTPC-Loop-PUSCH = supported
    			twoDifferentTPC-Loop-PUCCH = supported
    		phy-ParametersFRX-Diff
    			supportedDMRS-TypeDL = type1
    			supportedDMRS-TypeUL = type1
    			onePortsPTRS = 11
    			pucch-F2-WithFH = supported
    			pucch-F3-WithFH = supported
    			pucch-F4-WithFH = supported
    			pusch-LBRM = supported
    			pdcch-BlindDetectionCA = 4
    			csi-RS-IM-ReceptionForFeedback
    				maxConfigNumberNZP-CSI-RS-PerCC = 2
    				maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 4
    				maxConfigNumberCSI-IM-PerCC = n2
    				maxNumberSimultaneousNZP-CSI-RS-PerCC = 2
    				totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 4
    			csi-ReportFramework
    				maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 1
    				maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 1
    				maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    				maxNumberPeriodicCSI-PerBWP-ForBeamReport = 3
    				maxNumberAperiodicCSI-PerBWP-ForBeamReport = 3
    				maxNumberAperidicCSI-triggeringStatePerCC = n63
    				maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    				simultaneousCSI-ReportsPerCC = 2
    			mux-SR-HARQ-ACK-CSI-PUCCH-OncePerSlot
    				sameSymbol = supported
    		phy-ParametersFR2
    			pdsch-RE-MappingFR2-PerSymbol = n6
    			pdsch-RE-MappingFR2-PerSlot = n16
    	rf-Parameters
    		supportedBandListNR = SEQUENCE OF BandNR
    			BandNR(1)
    				bandNR = 260
    				mimo-ParametersPerBand
    					tci-StatePDSCH
    						maxNumberConfiguredTCIstatesPerCC = n64
    						maxNumberActiveTCI-PerBWP = n1
    					pusch-TransCoherence = nonCoherent
    					beamCorrespondence = supported
    					periodicBeamReport = supported
    					aperiodicBeamReport = supported
    					maxNumberRxBeam = 4
    					maxNumberRxTxBeamSwitchDL
    						scs-120kHz = n4
    					maxNumberNonGroupBeamReporting = n4
    					maxNumberSSB-BFD = 16
    					maxNumberCSI-RS-SSB-CBD = 32
    					twoPortsPTRS-UL = supported
    					supportedSRS-Resources
    						maxNumberAperiodicSRS-PerBWP = n2
    						maxNumberAperiodicSRS-PerBWP-PerSlot = 1
    						maxNumberPeriodicSRS-PerBWP = n2
    						maxNumberPeriodicSRS-PerBWP-PerSlot = 1
    						maxNumberSemiPersitentSRS-PerBWP = n2
    						maxNumberSP-SRS-PerBWP-PerSlot = 1
    						maxNumberSRS-Ports-PerResource = n2
    					beamReportTiming
    						scs-120kHz = sym28
    					beamCorrespondenceCA = true
    					beamManagementSSB-CSI-RS
    						maxNumberSSB-CSI-RS-ResourceOneTx = n8
    						maxNumberCSI-RS-Resource = n16
    						maxNumberCSI-RS-ResourceTwoTx = n0
    						supportedCSI-RS-Density = three
    						maxNumberAperiodicCSI-RS-Resource = n16
    					beamSwitchTiming
    						scs-120kHz = sym28
    					codebookParameters
    						type1
    							singlePanel
    								supportedCSI-RS-ResourceList = SEQUENCE OF SupportedCSI-RS-Resource
    									SupportedCSI-RS-Resource(1)
    										maxNumberTxPortsPerResource = p2
    										maxNumberResourcesPerBand = 9
    										totalNumberTxPortsPerBand = 18
    								modes = mode1
    								maxNumberCSI-RS-PerResourceSet = 1
    					csi-RS-IM-ReceptionForFeedback
    						maxConfigNumberNZP-CSI-RS-PerCC = 2
    						maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC = 4
    						maxConfigNumberCSI-IM-PerCC = n2
    						maxNumberSimultaneousNZP-CSI-RS-PerCC = 2
    						totalNumberPortsSimultaneousNZP-CSI-RS-PerCC = 4
    					csi-ReportFramework
    						maxNumberPeriodicCSI-PerBWP-ForCSI-Report = 1
    						maxNumberAperiodicCSI-PerBWP-ForCSI-Report = 1
    						maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report = 0
    						maxNumberPeriodicCSI-PerBWP-ForBeamReport = 3
    						maxNumberAperiodicCSI-PerBWP-ForBeamReport = 3
    						maxNumberAperidicCSI-triggeringStatePerCC = n63
    						maxNumberSemiPersistentCSI-PerBWP-ForBeamReport = 0
    						simultaneousCSI-ReportsPerCC = 2
    					csi-RS-ForTracking
    						maxBurstLength = 2
    						maxSimultaneousResourceSetsPerCC = 1
    						maxConfiguredResourceSetsPerCC = 64
    						maxConfiguredResourceSetsAllCC = 128
    					spatialRelations
    						maxNumberConfiguredSpatialRelations = n16
    						maxNumberActiveSpatialRelations = n1
    						maxNumberDL-RS-QCL-TypeD = n1
    				multipleTCI = supported
    				ue-PowerClass = pc3
    				channelBWs-DL-v1530 = fr2 =
    					scs-120kHz = 110
    				channelBWs-UL-v1530 = fr2 =
    					scs-120kHz = 110
    		appliedFreqBandListFilter = SEQUENCE OF FreqBandInformation
    			FreqBandInformation(1) = bandInformationEUTRA =
    				bandEUTRA = 5
    			FreqBandInformation(2) = bandInformationNR =
    				bandNR = 260
    	measAndMobParameters
    		measAndMobParametersCommon
    			ssb-RLM = supported
    		measAndMobParametersXDD-Diff
    			intraAndInterF-MeasAndReport = supported
    			eventA-MeasAndReport = supported
    	featureSets
    		featureSetsDownlink = SEQUENCE OF FeatureSetDownlink
    			FeatureSetDownlink(1)
    				featureSetListPerDownlinkCC = SEQUENCE OF FeatureSetDownlinkPerCC-Id
    					FeatureSetDownlinkPerCC-Id(1) = 1
    					FeatureSetDownlinkPerCC-Id(2) = 1
    					FeatureSetDownlinkPerCC-Id(3) = 1
    					FeatureSetDownlinkPerCC-Id(4) = 1
    					FeatureSetDownlinkPerCC-Id(5) = 1
    					FeatureSetDownlinkPerCC-Id(6) = 1
    					FeatureSetDownlinkPerCC-Id(7) = 1
    					FeatureSetDownlinkPerCC-Id(8) = 1
    				intraBandFreqSeparationDL = c2
    				ue-SpecificUL-DL-Assignment = supported
    				timeDurationForQCL
    					scs-120kHz = s28
    			FeatureSetDownlink(2)
    				featureSetListPerDownlinkCC = SEQUENCE OF FeatureSetDownlinkPerCC-Id
    					FeatureSetDownlinkPerCC-Id(1) = 1
    					FeatureSetDownlinkPerCC-Id(2) = 1
    					FeatureSetDownlinkPerCC-Id(3) = 1
    					FeatureSetDownlinkPerCC-Id(4) = 1
    				intraBandFreqSeparationDL = c2
    				ue-SpecificUL-DL-Assignment = supported
    				timeDurationForQCL
    					scs-120kHz = s28
    			FeatureSetDownlink(3)
    				featureSetListPerDownlinkCC = SEQUENCE OF FeatureSetDownlinkPerCC-Id
    					FeatureSetDownlinkPerCC-Id(1) = 1
    					FeatureSetDownlinkPerCC-Id(2) = 1
    					FeatureSetDownlinkPerCC-Id(3) = 1
    				intraBandFreqSeparationDL = c2
    				ue-SpecificUL-DL-Assignment = supported
    				timeDurationForQCL
    					scs-120kHz = s28
    			FeatureSetDownlink(4)
    				featureSetListPerDownlinkCC = SEQUENCE OF FeatureSetDownlinkPerCC-Id
    					FeatureSetDownlinkPerCC-Id(1) = 1
    				intraBandFreqSeparationDL = c2
    				ue-SpecificUL-DL-Assignment = supported
    				timeDurationForQCL
    					scs-120kHz = s28
    			FeatureSetDownlink(5)
    				featureSetListPerDownlinkCC = SEQUENCE OF FeatureSetDownlinkPerCC-Id
    					FeatureSetDownlinkPerCC-Id(1) = 2
    					FeatureSetDownlinkPerCC-Id(2) = 2
    					FeatureSetDownlinkPerCC-Id(3) = 2
    				intraBandFreqSeparationDL = c2
    				ue-SpecificUL-DL-Assignment = supported
    				timeDurationForQCL
    					scs-120kHz = s28
    			FeatureSetDownlink(6)
    				featureSetListPerDownlinkCC = SEQUENCE OF FeatureSetDownlinkPerCC-Id
    					FeatureSetDownlinkPerCC-Id(1) = 2
    					FeatureSetDownlinkPerCC-Id(2) = 2
    					FeatureSetDownlinkPerCC-Id(3) = 2
    					FeatureSetDownlinkPerCC-Id(4) = 2
    				intraBandFreqSeparationDL = c2
    				ue-SpecificUL-DL-Assignment = supported
    				timeDurationForQCL
    					scs-120kHz = s28
    			FeatureSetDownlink(7)
    				featureSetListPerDownlinkCC = SEQUENCE OF FeatureSetDownlinkPerCC-Id
    					FeatureSetDownlinkPerCC-Id(1) = 2
    				intraBandFreqSeparationDL = c2
    				ue-SpecificUL-DL-Assignment = supported
    				timeDurationForQCL
    					scs-120kHz = s28
    			FeatureSetDownlink(8)
    				featureSetListPerDownlinkCC = SEQUENCE OF FeatureSetDownlinkPerCC-Id
    					FeatureSetDownlinkPerCC-Id(1) = 1
    					FeatureSetDownlinkPerCC-Id(2) = 1
    				intraBandFreqSeparationDL = c2
    				ue-SpecificUL-DL-Assignment = supported
    				timeDurationForQCL
    					scs-120kHz = s28
    			FeatureSetDownlink(9)
    				featureSetListPerDownlinkCC = SEQUENCE OF FeatureSetDownlinkPerCC-Id
    					FeatureSetDownlinkPerCC-Id(1) = 2
    					FeatureSetDownlinkPerCC-Id(2) = 2
    				intraBandFreqSeparationDL = c2
    				ue-SpecificUL-DL-Assignment = supported
    				timeDurationForQCL
    					scs-120kHz = s28
    		featureSetsDownlinkPerCC = SEQUENCE OF FeatureSetDownlinkPerCC
    			FeatureSetDownlinkPerCC(1)
    				supportedSubcarrierSpacingDL = kHz120
    				supportedBandwidthDL = fr2 = mhz100
    				maxNumberMIMO-LayersPDSCH = twoLayers
    				supportedModulationOrderDL = qam64
    			FeatureSetDownlinkPerCC(2)
    				supportedSubcarrierSpacingDL = kHz120
    				supportedBandwidthDL = fr2 = mhz50
    				maxNumberMIMO-LayersPDSCH = twoLayers
    				supportedModulationOrderDL = qam64
    		featureSetsUplink = SEQUENCE OF FeatureSetUplink
    			FeatureSetUplink(1)
    				featureSetListPerUplinkCC = SEQUENCE OF FeatureSetUplinkPerCC-Id
    					FeatureSetUplinkPerCC-Id(1) = 1
    					FeatureSetUplinkPerCC-Id(2) = 1
    				supportedSRS-Resources
    					maxNumberAperiodicSRS-PerBWP = n2
    					maxNumberAperiodicSRS-PerBWP-PerSlot = 1
    					maxNumberPeriodicSRS-PerBWP = n2
    					maxNumberPeriodicSRS-PerBWP-PerSlot = 1
    					maxNumberSemiPersitentSRS-PerBWP = n2
    					maxNumberSP-SRS-PerBWP-PerSlot = 1
    					maxNumberSRS-Ports-PerResource = n2
    			FeatureSetUplink(2)
    				featureSetListPerUplinkCC = SEQUENCE OF FeatureSetUplinkPerCC-Id
    					FeatureSetUplinkPerCC-Id(1) = 2
    					FeatureSetUplinkPerCC-Id(2) = 2
    					FeatureSetUplinkPerCC-Id(3) = 2
    					FeatureSetUplinkPerCC-Id(4) = 2
    				supportedSRS-Resources
    					maxNumberAperiodicSRS-PerBWP = n2
    					maxNumberAperiodicSRS-PerBWP-PerSlot = 1
    					maxNumberPeriodicSRS-PerBWP = n2
    					maxNumberPeriodicSRS-PerBWP-PerSlot = 1
    					maxNumberSemiPersitentSRS-PerBWP = n2
    					maxNumberSP-SRS-PerBWP-PerSlot = 1
    					maxNumberSRS-Ports-PerResource = n1
    			FeatureSetUplink(3)
    				featureSetListPerUplinkCC = SEQUENCE OF FeatureSetUplinkPerCC-Id
    					FeatureSetUplinkPerCC-Id(1) = 1
    				supportedSRS-Resources
    					maxNumberAperiodicSRS-PerBWP = n2
    					maxNumberAperiodicSRS-PerBWP-PerSlot = 1
    					maxNumberPeriodicSRS-PerBWP = n2
    					maxNumberPeriodicSRS-PerBWP-PerSlot = 1
    					maxNumberSemiPersitentSRS-PerBWP = n2
    					maxNumberSP-SRS-PerBWP-PerSlot = 1
    					maxNumberSRS-Ports-PerResource = n2
    			FeatureSetUplink(4)
    				featureSetListPerUplinkCC = SEQUENCE OF FeatureSetUplinkPerCC-Id
    					FeatureSetUplinkPerCC-Id(1) = 2
    					FeatureSetUplinkPerCC-Id(2) = 2
    					FeatureSetUplinkPerCC-Id(3) = 2
    				supportedSRS-Resources
    					maxNumberAperiodicSRS-PerBWP = n2
    					maxNumberAperiodicSRS-PerBWP-PerSlot = 1
    					maxNumberPeriodicSRS-PerBWP = n2
    					maxNumberPeriodicSRS-PerBWP-PerSlot = 1
    					maxNumberSemiPersitentSRS-PerBWP = n2
    					maxNumberSP-SRS-PerBWP-PerSlot = 1
    					maxNumberSRS-Ports-PerResource = n1
    			FeatureSetUplink(5)
    				featureSetListPerUplinkCC = SEQUENCE OF FeatureSetUplinkPerCC-Id
    					FeatureSetUplinkPerCC-Id(1) = 3
    					FeatureSetUplinkPerCC-Id(2) = 3
    				supportedSRS-Resources
    					maxNumberAperiodicSRS-PerBWP = n2
    					maxNumberAperiodicSRS-PerBWP-PerSlot = 1
    					maxNumberPeriodicSRS-PerBWP = n2
    					maxNumberPeriodicSRS-PerBWP-PerSlot = 1
    					maxNumberSemiPersitentSRS-PerBWP = n2
    					maxNumberSP-SRS-PerBWP-PerSlot = 1
    					maxNumberSRS-Ports-PerResource = n2
    			FeatureSetUplink(6)
    				featureSetListPerUplinkCC = SEQUENCE OF FeatureSetUplinkPerCC-Id
    					FeatureSetUplinkPerCC-Id(1) = 4
    					FeatureSetUplinkPerCC-Id(2) = 4
    					FeatureSetUplinkPerCC-Id(3) = 4
    					FeatureSetUplinkPerCC-Id(4) = 4
    				supportedSRS-Resources
    					maxNumberAperiodicSRS-PerBWP = n2
    					maxNumberAperiodicSRS-PerBWP-PerSlot = 1
    					maxNumberPeriodicSRS-PerBWP = n2
    					maxNumberPeriodicSRS-PerBWP-PerSlot = 1
    					maxNumberSemiPersitentSRS-PerBWP = n2
    					maxNumberSP-SRS-PerBWP-PerSlot = 1
    					maxNumberSRS-Ports-PerResource = n1
    			FeatureSetUplink(7)
    				featureSetListPerUplinkCC = SEQUENCE OF FeatureSetUplinkPerCC-Id
    					FeatureSetUplinkPerCC-Id(1) = 3
    				supportedSRS-Resources
    					maxNumberAperiodicSRS-PerBWP = n2
    					maxNumberAperiodicSRS-PerBWP-PerSlot = 1
    					maxNumberPeriodicSRS-PerBWP = n2
    					maxNumberPeriodicSRS-PerBWP-PerSlot = 1
    					maxNumberSemiPersitentSRS-PerBWP = n2
    					maxNumberSP-SRS-PerBWP-PerSlot = 1
    					maxNumberSRS-Ports-PerResource = n2
    			FeatureSetUplink(8)
    				featureSetListPerUplinkCC = SEQUENCE OF FeatureSetUplinkPerCC-Id
    					FeatureSetUplinkPerCC-Id(1) = 4
    					FeatureSetUplinkPerCC-Id(2) = 4
    					FeatureSetUplinkPerCC-Id(3) = 4
    				supportedSRS-Resources
    					maxNumberAperiodicSRS-PerBWP = n2
    					maxNumberAperiodicSRS-PerBWP-PerSlot = 1
    					maxNumberPeriodicSRS-PerBWP = n2
    					maxNumberPeriodicSRS-PerBWP-PerSlot = 1
    					maxNumberSemiPersitentSRS-PerBWP = n2
    					maxNumberSP-SRS-PerBWP-PerSlot = 1
    					maxNumberSRS-Ports-PerResource = n1
    			FeatureSetUplink(9)
    				featureSetListPerUplinkCC = SEQUENCE OF FeatureSetUplinkPerCC-Id
    					FeatureSetUplinkPerCC-Id(1) = 2
    				supportedSRS-Resources
    					maxNumberAperiodicSRS-PerBWP = n2
    					maxNumberAperiodicSRS-PerBWP-PerSlot = 1
    					maxNumberPeriodicSRS-PerBWP = n2
    					maxNumberPeriodicSRS-PerBWP-PerSlot = 1
    					maxNumberSemiPersitentSRS-PerBWP = n2
    					maxNumberSP-SRS-PerBWP-PerSlot = 1
    					maxNumberSRS-Ports-PerResource = n2
    		featureSetsUplinkPerCC = SEQUENCE OF FeatureSetUplinkPerCC
    			FeatureSetUplinkPerCC(1)
    				supportedSubcarrierSpacingUL = kHz120
    				supportedBandwidthUL = fr2 = mhz100
    				mimo-CB-PUSCH
    					maxNumberMIMO-LayersCB-PUSCH = twoLayers
    					maxNumberSRS-ResourcePerSet = 1
    				supportedModulationOrderUL = qam64
    			FeatureSetUplinkPerCC(2)
    				supportedSubcarrierSpacingUL = kHz120
    				supportedBandwidthUL = fr2 = mhz100
    				mimo-CB-PUSCH
    					maxNumberMIMO-LayersCB-PUSCH = oneLayer
    					maxNumberSRS-ResourcePerSet = 1
    				supportedModulationOrderUL = qam64
    			FeatureSetUplinkPerCC(3)
    				supportedSubcarrierSpacingUL = kHz120
    				supportedBandwidthUL = fr2 = mhz50
    				mimo-CB-PUSCH
    					maxNumberMIMO-LayersCB-PUSCH = twoLayers
    					maxNumberSRS-ResourcePerSet = 1
    				supportedModulationOrderUL = qam64
    			FeatureSetUplinkPerCC(4)
    				supportedSubcarrierSpacingUL = kHz120
    				supportedBandwidthUL = fr2 = mhz50
    				mimo-CB-PUSCH
    					maxNumberMIMO-LayersCB-PUSCH = oneLayer
    					maxNumberSRS-ResourcePerSet = 1
    				supportedModulationOrderUL = qam64

    UE-NR-Capability

    UE-MRDC-Capability
    	rf-ParametersMRDC
    		supportedBandCombinationList = SEQUENCE OF BandCombination
    			BandCombination(1)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = p
    						ca-BandwidthClassUL-NR = o
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = q
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 0
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(2)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = q
    						ca-BandwidthClassUL-NR = q
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 1
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(3)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    						ca-BandwidthClassUL-NR = a
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = q
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 2
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(4)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = q
    						ca-BandwidthClassUL-NR = o
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = p
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 3
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(5)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = p
    						ca-BandwidthClassUL-NR = p
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = q
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 4
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(6)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = q
    						ca-BandwidthClassUL-NR = a
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = p
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 5
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(7)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = p
    						ca-BandwidthClassUL-NR = a
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = q
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 6
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(8)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = q
    						ca-BandwidthClassUL-NR = a
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 7
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(9)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = q
    						ca-BandwidthClassUL-NR = q
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = p
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 8
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(10)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    						ca-BandwidthClassUL-NR = a
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = q
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = p
    				featureSetCombination = 9
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(11)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = q
    						ca-BandwidthClassUL-NR = o
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 10
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(12)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = h
    						ca-BandwidthClassUL-NR = g
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = h
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(5) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 11
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(13)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = h
    						ca-BandwidthClassUL-NR = h
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(5) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 12
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(14)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    						ca-BandwidthClassUL-NR = a
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = h
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = h
    					BandParameters(5) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 13
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(15)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    						ca-BandwidthClassUL-NR = a
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = h
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(5) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 14
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(16)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = h
    						ca-BandwidthClassUL-NR = a
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = h
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(5) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 15
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(17)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = h
    						ca-BandwidthClassUL-NR = g
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(5) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 16
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(18)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = h
    						ca-BandwidthClassUL-NR = a
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(5) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 17
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(19)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = h
    						ca-BandwidthClassUL-NR = h
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = h
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(5) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 18
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(20)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = o
    						ca-BandwidthClassUL-NR = o
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = p
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(5) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(6) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 19
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(21)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    						ca-BandwidthClassUL-NR = a
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = p
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = o
    					BandParameters(5) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(6) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 20
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(22)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    						ca-BandwidthClassUL-NR = a
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = p
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(5) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(6) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 21
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(23)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = p
    						ca-BandwidthClassUL-NR = o
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = o
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(5) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(6) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 22
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(24)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = o
    						ca-BandwidthClassUL-NR = a
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = p
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(5) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(6) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 23
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(25)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = p
    						ca-BandwidthClassUL-NR = o
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(5) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(6) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 24
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(26)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = p
    						ca-BandwidthClassUL-NR = a
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = o
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(5) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(6) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 25
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(27)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = p
    						ca-BandwidthClassUL-NR = a
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(5) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(6) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 26
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(28)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = p
    						ca-BandwidthClassUL-NR = p
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = o
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(5) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(6) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 27
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(29)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = p
    						ca-BandwidthClassUL-NR = p
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(5) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(6) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 28
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(30)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = o
    						ca-BandwidthClassUL-NR = o
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(5) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(6) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(7) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 29
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(31)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = o
    						ca-BandwidthClassUL-NR = a
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(5) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(6) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(7) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 30
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(32)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = o
    						ca-BandwidthClassUL-NR = a
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = o
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(5) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(6) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(7) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 31
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(33)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = o
    						ca-BandwidthClassUL-NR = o
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = o
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(5) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(6) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(7) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 32
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(34)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    						ca-BandwidthClassUL-NR = a
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = o
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = o
    					BandParameters(5) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(6) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(7) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 33
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(35)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    						ca-BandwidthClassUL-NR = a
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = o
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(5) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(6) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(7) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 34
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(36)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    						ca-BandwidthClassUL-NR = a
    					BandParameters(3) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(4) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(5) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(6) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(7) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(8) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    					BandParameters(9) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = a
    				featureSetCombination = 35
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(37)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = m
    						ca-BandwidthClassUL-NR = i
    				featureSetCombination = 36
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(38)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = m
    						ca-BandwidthClassUL-NR = a
    				featureSetCombination = 37
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    			BandCombination(39)
    				bandList = SEQUENCE OF BandParameters
    					BandParameters(1) = eutra =
    						bandEUTRA = 5
    						ca-BandwidthClassDL-EUTRA = a
    						ca-BandwidthClassUL-EUTRA = a
    					BandParameters(2) = nr =
    						bandNR = 260
    						ca-BandwidthClassDL-NR = m
    						ca-BandwidthClassUL-NR = g
    				featureSetCombination = 38
    				mrdc-Parameters
    					simultaneousRxTxInterBandENDC = supported
    		appliedFreqBandListFilter = SEQUENCE OF FreqBandInformation
    			FreqBandInformation(1) = bandInformationEUTRA =
    				bandEUTRA = 5
    			FreqBandInformation(2) = bandInformationNR =
    				bandNR = 260
    		supportedBandCombinationList-v1540 = SEQUENCE OF BandCombination-v1540
    			BandCombination-v1540(1)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(2)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(3)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(4)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(5)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(6)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(7)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(8)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(9)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(10)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(11)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(12)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    					BandParameters-v1540(5)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(13)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    					BandParameters-v1540(5)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(14)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    					BandParameters-v1540(5)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(15)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    					BandParameters-v1540(5)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(16)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    					BandParameters-v1540(5)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(17)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    					BandParameters-v1540(5)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(18)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    					BandParameters-v1540(5)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(19)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    					BandParameters-v1540(5)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(20)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    					BandParameters-v1540(5)
    					BandParameters-v1540(6)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(21)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    					BandParameters-v1540(5)
    					BandParameters-v1540(6)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(22)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    					BandParameters-v1540(5)
    					BandParameters-v1540(6)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(23)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    					BandParameters-v1540(5)
    					BandParameters-v1540(6)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(24)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    					BandParameters-v1540(5)
    					BandParameters-v1540(6)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(25)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    					BandParameters-v1540(5)
    					BandParameters-v1540(6)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(26)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    					BandParameters-v1540(5)
    					BandParameters-v1540(6)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(27)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    					BandParameters-v1540(5)
    					BandParameters-v1540(6)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(28)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    					BandParameters-v1540(5)
    					BandParameters-v1540(6)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(29)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    					BandParameters-v1540(5)
    					BandParameters-v1540(6)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(30)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    					BandParameters-v1540(5)
    					BandParameters-v1540(6)
    					BandParameters-v1540(7)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(31)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    					BandParameters-v1540(5)
    					BandParameters-v1540(6)
    					BandParameters-v1540(7)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(32)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    					BandParameters-v1540(5)
    					BandParameters-v1540(6)
    					BandParameters-v1540(7)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(33)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    					BandParameters-v1540(5)
    					BandParameters-v1540(6)
    					BandParameters-v1540(7)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(34)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    					BandParameters-v1540(5)
    					BandParameters-v1540(6)
    					BandParameters-v1540(7)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(35)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    					BandParameters-v1540(5)
    					BandParameters-v1540(6)
    					BandParameters-v1540(7)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(36)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    					BandParameters-v1540(3)
    					BandParameters-v1540(4)
    					BandParameters-v1540(5)
    					BandParameters-v1540(6)
    					BandParameters-v1540(7)
    					BandParameters-v1540(8)
    					BandParameters-v1540(9)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(37)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(38)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    			BandCombination-v1540(39)
    				bandList-v1540 = SEQUENCE OF BandParameters-v1540
    					BandParameters-v1540(1)
    					BandParameters-v1540(2)
    				ca-ParametersNR-v1540
    					csi-RS-IM-ReceptionForFeedbackPerBandComb
    						maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC = 9
    						totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC = 18
    					simultaneousCSI-ReportsAllCC = 5
    	featureSetCombinations = SEQUENCE OF FeatureSetCombination
    		FeatureSetCombination(1) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 5
    					uplinkSetNR = 5
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 6
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    		FeatureSetCombination(2) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 6
    					uplinkSetNR = 6
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    		FeatureSetCombination(3) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 7
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 6
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    		FeatureSetCombination(4) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 6
    					uplinkSetNR = 5
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 5
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    		FeatureSetCombination(5) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 5
    					uplinkSetNR = 8
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 6
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    		FeatureSetCombination(6) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 6
    					uplinkSetNR = 7
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 5
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    		FeatureSetCombination(7) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 5
    					uplinkSetNR = 7
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 6
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    		FeatureSetCombination(8) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 6
    					uplinkSetNR = 7
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    		FeatureSetCombination(9) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 6
    					uplinkSetNR = 6
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 5
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    		FeatureSetCombination(10) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 7
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 6
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 5
    					uplinkSetNR = 0
    		FeatureSetCombination(11) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 6
    					uplinkSetNR = 5
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    		FeatureSetCombination(12) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 3
    					uplinkSetNR = 1
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 3
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 0
    			FeatureSetsPerBand(5) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 0
    		FeatureSetCombination(13) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 3
    					uplinkSetNR = 4
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 0
    			FeatureSetsPerBand(5) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 0
    		FeatureSetCombination(14) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 3
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 3
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 3
    					uplinkSetNR = 0
    			FeatureSetsPerBand(5) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 0
    		FeatureSetCombination(15) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 3
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 3
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 0
    			FeatureSetsPerBand(5) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 0
    		FeatureSetCombination(16) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 3
    					uplinkSetNR = 3
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 3
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 0
    			FeatureSetsPerBand(5) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 0
    		FeatureSetCombination(17) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 3
    					uplinkSetNR = 1
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 0
    			FeatureSetsPerBand(5) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 0
    		FeatureSetCombination(18) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 3
    					uplinkSetNR = 3
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 0
    			FeatureSetsPerBand(5) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 0
    		FeatureSetCombination(19) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 3
    					uplinkSetNR = 4
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 3
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 0
    			FeatureSetsPerBand(5) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 0
    		FeatureSetCombination(20) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 9
    					uplinkSetNR = 5
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 5
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(5) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(6) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    		FeatureSetCombination(21) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 7
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 5
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 9
    					uplinkSetNR = 0
    			FeatureSetsPerBand(5) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(6) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    		FeatureSetCombination(22) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 7
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 5
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(5) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(6) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    		FeatureSetCombination(23) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 5
    					uplinkSetNR = 5
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 9
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(5) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(6) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    		FeatureSetCombination(24) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 9
    					uplinkSetNR = 7
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 5
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(5) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(6) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    		FeatureSetCombination(25) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 5
    					uplinkSetNR = 5
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(5) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(6) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    		FeatureSetCombination(26) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 5
    					uplinkSetNR = 7
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 9
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(5) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(6) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    		FeatureSetCombination(27) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 5
    					uplinkSetNR = 7
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(5) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(6) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    		FeatureSetCombination(28) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 5
    					uplinkSetNR = 8
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 9
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(5) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(6) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    		FeatureSetCombination(29) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 5
    					uplinkSetNR = 8
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(5) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(6) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    		FeatureSetCombination(30) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 9
    					uplinkSetNR = 5
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(5) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(6) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(7) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    		FeatureSetCombination(31) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 9
    					uplinkSetNR = 7
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(5) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(6) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(7) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    		FeatureSetCombination(32) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 9
    					uplinkSetNR = 7
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 9
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(5) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(6) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(7) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    		FeatureSetCombination(33) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 9
    					uplinkSetNR = 5
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 9
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(5) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(6) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(7) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    		FeatureSetCombination(34) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 7
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 9
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 9
    					uplinkSetNR = 0
    			FeatureSetsPerBand(5) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(6) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(7) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    		FeatureSetCombination(35) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 7
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 9
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(5) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(6) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    			FeatureSetsPerBand(7) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 7
    					uplinkSetNR = 0
    		FeatureSetCombination(36) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 3
    			FeatureSetsPerBand(3) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 0
    			FeatureSetsPerBand(4) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 0
    			FeatureSetsPerBand(5) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 0
    			FeatureSetsPerBand(6) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 0
    			FeatureSetsPerBand(7) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 0
    			FeatureSetsPerBand(8) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 0
    			FeatureSetsPerBand(9) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 4
    					uplinkSetNR = 0
    		FeatureSetCombination(37) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 1
    					uplinkSetNR = 2
    		FeatureSetCombination(38) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 1
    					uplinkSetNR = 3
    		FeatureSetCombination(39) = SEQUENCE OF FeatureSetsPerBand
    			FeatureSetsPerBand(1) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = eutra =
    					downlinkSetEUTRA = 2
    					uplinkSetEUTRA = 1
    			FeatureSetsPerBand(2) = SEQUENCE OF FeatureSet
    				FeatureSet(1) = nr =
    					downlinkSetNR = 1
    					uplinkSetNR = 1

    UE-MRDC-Capability

    RRC_PDU_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 626
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ueCapabilityInformation
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							c1
    								ueCapabilityInformation_r8
    									ue_CapabilityRAT_ContainerList
    										UE_CapabilityRAT_Container
    											rat_Type = nr (5)
    											ueCapabilityRAT_Container = 'E1000000014F760302000001404807062E03000180084D8000408820402A03050080A01000A05A07BC71B438084478F904108A0223F6CB0C480081000408820402A031FBF9015D7001009040F13781100A01C00000000000000000000B80500600000000005C0280200000000B805000001700A00801004012E0140180200802009700A000012E01400800001700A00401004B005BA46E1008040100000208210403004010040120820040000082084100801004012082004010080220821040300C0300C032082004000088208410080300C032082004000048208403576A2BB115CA8AE440'O
    										UE_CapabilityRAT_Container
    											rat_Type = eutra_nr (6)
    											ueCapabilityRAT_Container = ' 'O
    									nonCriticalExtension = Omit

    Received on port: NASEMU_EUTRA_PTC:SYS_SRB

    SRB_COMMON_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 626
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						ueCapabilityInformation
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								c1
    									ueCapabilityInformation_r8
    										ue_CapabilityRAT_ContainerList
    											UE_CapabilityRAT_Container
    												rat_Type = nr (5)
    												ueCapabilityRAT_Container = 'E1000000014F760302000001404807062E03000180084D8000408820402A03050080A01000A05A07BC71B438084478F904108A0223F6CB0C480081000408820402A031FBF9015D7001009040F13781100A01C00000000000000000000B80500600000000005C0280200000000B805000001700A00801004012E0140180200802009700A000012E01400800001700A00401004B005BA46E1008040100000208210403004010040120820040000082084100801004012082004010080220821040300C0300C032082004000088208410080300C032082004000048208403576A2BB115CA8AE440'O
    											UE_CapabilityRAT_Container
    												rat_Type = eutra_nr (6)
    												ueCapabilityRAT_Container = ' 'O
    										nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: SRB -> EUTRA_5GS_PTC:SRB

    EUTRA_NR_Coordination_MSG
    	OctetData
    		Data = 'E1000000014F760302000001404807062E03000180084D8000408820402A03050080A01000A05A07BC71B438084478F904108A0223F6CB0C480081000408820402A031FBF9015D7001009040F13781100A01C00000000000000000000B80500600000000005C0280200000000B805000001700A00801004012E0140180200802009700A000012E01400800001700A00401004B005BA46E1008040100000208210403004010040120820040000082084100801004012082004010080220821040300C0300C032082004000088208410080300C032082004000048208403576A2BB115CA8AE440'O
    		Description = 'NRCap'

    Inter-component message: EUTRA -> ENDC_NR_PTC:EUTRA

    EUTRA_NR_Coordination_MSG
    	OctetData
    		Data = ' 'O
    		Description = 'ENDCCap'

    Inter-component message: EUTRA -> ENDC_NR_PTC:EUTRA

    IP_ConfigReq_Type
    	ChangeEutraCell = eutra_Cell1 (1)

    Inter-component message: EUTRA_CTRL -> IP_PTC:EUTRA_CTRL

    IP_Indication_Type
    	Cnf = True

    Inter-component message: IP -> EUTRA_5GS_PTC:IP

    SRB_COMMON_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcConnectionReconfiguration
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								c1
    									rrcConnectionReconfiguration_r8
    										measConfig = Omit
    										mobilityControlInfo = Omit
    										dedicatedInfoNASList = Omit
    										radioResourceConfigDedicated
    											srb_ToAddModList
    												SRB_ToAddMod
    													srb_Identity = 2
    													rlc_Config
    														defaultValue = Null
    													logicalChannelConfig
    														defaultValue = Null
    													pdcp_verChange_r15 = Omit
    													rlc_Config_v1530 = Omit
    													rlc_BearerConfigDupl_r15 = Omit
    													srb_Identity_v1530 = Omit
    											drb_ToAddModList
    												DRB_ToAddMod
    													eps_BearerIdentity = 12
    													drb_Identity = 8
    													pdcp_Config
    														discardTimer = infinity_ (7)
    														rlc_AM
    															statusReportRequired = True
    														rlc_UM = Omit
    														headerCompression
    															notUsed = Null
    														rn_IntegrityProtection_r10 = Omit
    														pdcp_SN_Size_v1130 = Omit
    														ul_DataSplitDRB_ViaSCG_r12 = Omit
    														t_Reordering_r12 = Omit
    														ul_DataSplitThreshold_r13 = Omit
    														pdcp_SN_Size_v1310 = Omit
    														statusFeedback_r13 = Omit
    														ul_LWA_Config_r14 = Omit
    														uplinkOnlyHeaderCompression_r14 = Omit
    														uplinkDataCompression_r15 = Omit
    														pdcp_DuplicationConfig_r15 = Omit
    													rlc_Config
    														am
    															ul_AM_RLC
    																t_PollRetransmit = ms80 (15)
    																pollPDU = p128 (5)
    																pollByte = kB125 (4)
    																maxRetxThreshold = t4 (3)
    															dl_AM_RLC
    																t_Reordering = ms80 (16)
    																t_StatusProhibit = ms60 (12)
    													logicalChannelIdentity = 10
    													logicalChannelConfig
    														ul_SpecificParameters
    															priority = 6
    															prioritisedBitRate = kBps0 (0)
    															bucketSizeDuration = ms100 (1)
    															logicalChannelGroup = 1
    														logicalChannelSR_Mask_r9 = Omit
    														logicalChannelSR_Prohibit_r12 = Omit
    														laa_UL_Allowed_r14 = Omit
    														bitRateQueryProhibitTimer_r14 = Omit
    														allowedTTI_Lengths_r15 = Omit
    														logicalChannelSR_Restriction_r15 = Omit
    														channellAccessPriority_r15 = Omit
    														lch_CellRestriction_r15 = Omit
    													drb_TypeChange_r12 = Omit
    													rlc_Config_v1250 = Omit
    													rlc_Config_v1310 = Omit
    													drb_TypeLWA_r13 = Omit
    													drb_TypeLWIP_r13 = Omit
    													rlc_Config_v1430 = Omit
    													lwip_UL_Aggregation_r14 = Omit
    													lwip_DL_Aggregation_r14 = Omit
    													lwa_WLAN_AC_r14 = Omit
    													rlc_Config_v1510 = Omit
    													rlc_Config_v1530 = Omit
    													rlc_BearerConfigDupl_r15 = Omit
    													logicalChannelIdentity_r15 = Omit
    											drb_ToReleaseList = Omit
    											mac_MainConfig
    												explicitValue
    													ul_SCH_Config
    														maxHARQ_Tx = n5 (4)
    														periodicBSR_Timer = sf20 (3)
    														retxBSR_Timer = sf320 (0)
    														ttiBundling = False
    													drx_Config
    														setup
    															onDurationTimer = psf6 (5)
    															drx_InactivityTimer = psf1920 (20)
    															drx_RetransmissionTimer = psf16 (5)
    															longDRX_CycleStartOffset
    																sf1280 = 4
    															shortDRX = Omit
    													timeAlignmentTimerDedicated = sf750 (1)
    													phr_Config
    														setup
    															periodicPHR_Timer = sf500 (5)
    															prohibitPHR_Timer = sf200 (5)
    															dl_PathlossChange = dB3 (1)
    													sr_ProhibitTimer_r9 = Omit
    													mac_MainConfig_v1020 = Omit
    													stag_ToReleaseList_r11 = Omit
    													stag_ToAddModList_r11 = Omit
    													drx_Config_v1130 = Omit
    													e_HARQ_Pattern_r12 = Omit
    													dualConnectivityPHR = Omit
    													logicalChannelSR_Config_r12 = Omit
    													drx_Config_v1310 = Omit
    													extendedPHR2_r13 = Omit
    													eDRX_Config_CycleStartOffset_r13 = Omit
    													drx_Config_r13 = Omit
    													skipUplinkTx_r14 = Omit
    													dataInactivityTimerConfig_r14 = Omit
    													rai_Activation_r14 = Omit
    													shortTTI_AndSPT_r15 = Omit
    													mpdcch_UL_HARQ_ACK_FeedbackConfig_r15 = Omit
    													dormantStateTimers_r15 = Omit
    											sps_Config = Omit
    											physicalConfigDedicated
    												pdsch_ConfigDedicated = Omit
    												pucch_ConfigDedicated = Omit
    												pusch_ConfigDedicated = Omit
    												uplinkPowerControlDedicated = Omit
    												tpc_PDCCH_ConfigPUCCH
    													setup
    														tpc_RNTI = 0000001111111111'B
    														tpc_Index
    															indexOfFormat3 = 1
    												tpc_PDCCH_ConfigPUSCH
    													setup
    														tpc_RNTI = 0000000111111010'B
    														tpc_Index
    															indexOfFormat3 = 1
    												cqi_ReportConfig
    													cqi_ReportModeAperiodic = rm30 (3)
    													nomPDSCH_RS_EPRE_Offset = 0
    													cqi_ReportPeriodic
    														setup
    															cqi_PUCCH_ResourceIndex = 0
    															cqi_pmi_ConfigIndex = 25
    															cqi_FormatIndicatorPeriodic
    																widebandCQI = Null
    															ri_ConfigIndex = 483
    															simultaneousAckNackAndCQI = False
    												soundingRS_UL_ConfigDedicated
    													setup
    														srs_Bandwidth = bw0 (0)
    														srs_HoppingBandwidth = hbw0 (0)
    														freqDomainPosition = 0
    														duration = True
    														srs_ConfigIndex = 20
    														transmissionComb = 0
    														cyclicShift = cs0 (0)
    												antennaInfo
    													defaultValue = Null
    												schedulingRequestConfig = Omit
    												cqi_ReportConfig_v920 = Omit
    												antennaInfo_v920 = Omit
    												antennaInfo_r10 = Omit
    												antennaInfoUL_r10 = Omit
    												cif_Presence_r10 = Omit
    												cqi_ReportConfig_r10 = Omit
    												csi_RS_Config_r10 = Omit
    												pucch_ConfigDedicated_v1020 = Omit
    												pusch_ConfigDedicated_v1020 = Omit
    												schedulingRequestConfig_v1020 = Omit
    												soundingRS_UL_ConfigDedicated_v1020 = Omit
    												soundingRS_UL_ConfigDedicatedAperiodic_r10 = Omit
    												uplinkPowerControlDedicated_v1020 = Omit
    												additionalSpectrumEmissionCA_r10 = Omit
    												csi_RS_ConfigNZPToReleaseList_r11 = Omit
    												csi_RS_ConfigNZPToAddModList_r11 = Omit
    												csi_RS_ConfigZPToReleaseList_r11 = Omit
    												csi_RS_ConfigZPToAddModList_r11 = Omit
    												epdcch_Config_r11 = Omit
    												pdsch_ConfigDedicated_v1130 = Omit
    												cqi_ReportConfig_v1130 = Omit
    												pucch_ConfigDedicated_v1130 = Omit
    												pusch_ConfigDedicated_v1130 = Omit
    												uplinkPowerControlDedicated_v1130 = Omit
    												antennaInfo_v1250 = Omit
    												eimta_MainConfig_r12 = Omit
    												eimta_MainConfigPCell_r12 = Omit
    												pucch_ConfigDedicated_v1250 = Omit
    												cqi_ReportConfigPCell_v1250 = Omit
    												uplinkPowerControlDedicated_v1250 = Omit
    												pusch_ConfigDedicated_v1250 = Omit
    												csi_RS_Config_v1250 = Omit
    												pdsch_ConfigDedicated_v1280 = Omit
    												pdsch_ConfigDedicated_v1310 = Omit
    												pucch_ConfigDedicated_r13 = Omit
    												pusch_ConfigDedicated_r13 = Omit
    												pdcch_CandidateReductions_r13 = Omit
    												cqi_ReportConfig_v1310 = Omit
    												soundingRS_UL_ConfigDedicated_v1310 = Omit
    												soundingRS_UL_ConfigDedicatedUpPTsExt_r13 = Omit
    												soundingRS_UL_ConfigDedicatedAperiodic_v1310 = Omit
    												soundingRS_UL_ConfigDedicatedAperiodicUpPTsExt_r13 = Omit
    												csi_RS_Config_v1310 = Omit
    												ce_Mode_r13 = Omit
    												csi_RS_ConfigNZPToAddModListExt_r13 = Omit
    												csi_RS_ConfigNZPToReleaseListExt_r13 = Omit
    												cqi_ReportConfig_v1320 = Omit
    												typeA_SRS_TPC_PDCCH_Group_r14 = Omit
    												must_Config_r14 = Omit
    												pusch_EnhancementsConfig_r14 = Omit
    												ce_pdsch_pusch_EnhancementConfig_r14 = Omit
    												antennaInfo_v1430 = Omit
    												pucch_ConfigDedicated_v1430 = Omit
    												pdsch_ConfigDedicated_v1430 = Omit
    												pusch_ConfigDedicated_v1430 = Omit
    												soundingRS_UL_PeriodicConfigDedicatedList_r14 = Omit
    												soundingRS_UL_PeriodicConfigDedicatedUpPTsExtList_r14 = Omit
    												soundingRS_UL_AperiodicConfigDedicatedList_r14 = Omit
    												soundingRS_UL_ConfigDedicatedApUpPTsExtList_r14 = Omit
    												csi_RS_Config_v1430 = Omit
    												csi_RS_ConfigZP_ApList_r14 = Omit
    												cqi_ReportConfig_v1430 = Omit
    												semiOpenLoop_r14 = Omit
    												csi_RS_Config_v1480 = Omit
    												physicalConfigDedicatedSTTI_r15 = Omit
    												pdsch_ConfigDedicated_v1530 = Omit
    												pusch_ConfigDedicated_v1530 = Omit
    												cqi_ReportConfig_v1530 = Omit
    												antennaInfo_v1530 = Omit
    												csi_RS_Config_v1530 = Omit
    												uplinkPowerControlDedicated_v1530 = Omit
    												semiStaticCFI_Config_r15 = Omit
    												blindPDSCH_Repetition_Config_r15 = Omit
    											rlf_TimersAndConstants_r9 = Omit
    											measSubframePatternPCell_r10 = Omit
    											neighCellsCRS_Info_r11 = Omit
    											naics_Info_r12 = Omit
    											neighCellsCRS_Info_r13 = Omit
    											rlf_TimersAndConstants_r13 = Omit
    											sps_Config_v1430 = Omit
    											srb_ToAddModExtList_r15 = Omit
    											srb_ToReleaseExtList_r15 = Omit
    											sps_Config_v1530 = Omit
    											crs_IntfMitigConfig_r15 = Omit
    											neighCellsCRS_Info_r15 = Omit
    											drb_ToAddModList_r15 = Omit
    											drb_ToReleaseList_r15 = Omit
    											dummy = Omit
    											sps_Config_v1540 = Omit
    										securityConfigHO = Omit
    										nonCriticalExtension = Omit
    		Nas
    			NAS_MSG_Request_Type
    				SecurityProtection
    					Status = 0010'B
    					ForceMacError = False
    				Pdu
    					Msg
    						aTTACH_ACCEPT
    							securityHeaderType = 0000'B
    							protocolDiscriminator = 0111'B
    							messageType = 01000010'B
    							spareHalfOctet = '0'H
    							epsAttachResult
    								spare = 0'B
    								resultValue = 010'B
    							t3412
    								iei = Omit
    								unit = 111'B
    								timerValue = 00000'B
    							taiList
    								iei = Omit
    								iel = '06'O
    								listOfPartialTais
    									ListOfPartialTaiList
    										spareBit = 0'B
    										typeOfList = 00'B
    										numberOfElements = 00000'B
    										partialTaiList
    											type0List
    												Type0Element
    													plmnId = '00F110'O
    													tacList
    														NAS_Tac = '0001'O
    							esmMessage
    								iei = Omit
    								iel = '0000'O
    								esmPdu = ''O
    							guti
    								iei = '50'O
    								iel = '0B'O
    								idDigit1 = 1111'B
    								oddEvenInd = 0'B
    								typeOfId = 110'B
    								otherDigits = '00F110800101C2345678'O
    							lai
    								iei = '13'O
    								plmn = '00F110'O
    								lac = '0001'O
    							msIdentity
    								iei = '23'O
    								iel = '05'O
    								idDigit1 = 1111'B
    								oddEvenInd = 0'B
    								typeOfId = 100'B
    								otherDigits = '12345678'O
    							emmCause = Omit
    							t3402 = Omit
    							t3423 = Omit
    							equivalentPlmns = Omit
    							emergencyNumberList = Omit
    							epsNetworkFeatureSupport
    								iei = '64'O
    								iel = '01'O
    								cp_CIOT = 0'B
    								emmRegistered_withoutPDN = 0'B
    								esrps = 0'B
    								csLCS = 00'B
    								epcLCS = 0'B
    								emcBS = 0'B
    								imsVoPS = 1'B
    								bearers15 = Omit
    								iwkN26 = Omit
    								restrictDCNR = Omit
    								restrictEC = Omit
    								extdPCO = Omit
    								headerComp_CP_CIOT = Omit
    								s1_U_data = Omit
    								up_CIOT = Omit
    							addUpdateResult = Omit
    							t3412ExtdValue = Omit
    							t3324Value = Omit
    							extendedDRXParams = Omit
    							dcnId = Omit
    							smsServicesStatus = Omit
    							non3GPP_NW_ProvidedPolicies = Omit
    							t3448 = Omit
    							networkPolicy = Omit
    							t3447Value = Omit
    							xtdEmergencyNumList = Omit
    							cipheringKeyData = Omit
    					PiggybackedPduList
    						NAS_DL_Pdu_Type
    							Msg
    								aCTIVATE_DEFAULT_EPS_BEARER_CONTEXT_REQUEST
    									epsBearerId = 'C'H
    									protocolDiscriminator = 0010'B
    									procedureTransactionIdentifier = '2D'O
    									messageType = 11000001'B
    									epsQos
    										iei = Omit
    										iel = '09'O
    										qci = 00001001'B
    										maxBitRateUl = 01000000'B
    										maxBitRateDl = 01000000'B
    										guaranteedBitRateUl = 01000000'B
    										guaranteedBitRateDl = 01000000'B
    										maxBitRateUlExt = 00000000'B
    										maxBitRateDlExt = 00000000'B
    										guaranteedBitRateUlExt = 00000000'B
    										guaranteedBitRateDlExt = 00000000'B
    										maxBitRateUL_Ext2 = Omit
    										maxBitRateDL_Ext2 = Omit
    										guaranteedBitRateUL_Ext2 = Omit
    										guaranteedBitRateDL_Ext2 = Omit
    									accessPointName
    										iei = Omit
    										iel = '04'O
    										nameValue = '0361706E'O
    									pdnAdress
    										iei = Omit
    										iel = '0D'O
    										spare = 00000'B
    										typeValue = 011'B
    										adressInfo = '0000000000000002C0A8001A'O
    									transactionIdentifier = Omit
    									negotiatedQos = Omit
    									negotiatedLlcSapi = Omit
    									radioPriority = Omit
    									packetFlowIdentifier = Omit
    									apnAggMaxBitRate = Omit
    									esmCause = Omit
    									protocolConfigurationOptions
    										iei = '27'O
    										iel = '1B'O
    										ext = 1'B
    										spare = 0000'B
    										configProtocol = 000'B
    										pco
    											ProtocolContainer
    												protocolID = '000D'O
    												protocolLength = '04'O
    												content = 'C0A8C637'O
    											ProtocolContainer
    												protocolID = '0003'O
    												protocolLength = '10'O
    												content = 'FD29CC437FB90002020C29FFFE66B4C7'O
    									connectivityType = Omit
    									wlanOffloadInd = Omit
    									nbifomContainer = Omit
    									headerCompressionConfig = Omit
    									controlPlaneOnlyIndication = Omit
    									extdProtocolConfigurationOptions = Omit
    									servingPLMNRateControl = Omit
    									extd_APN_AMBR = Omit
    							PiggybackedPduList = Omit

    Inter-component message: TC_SRB -> NASEMU_EUTRA_PTC:TC_SRB

    Activate Default EPS Bearer Context Request
    	EPS bearer identity [4 bits] = 0xC [ 12 ]
    	Protocol Discriminator [4 bits] = 0x2 - EPS Session Management Messages [ 2 ]
    	Procedure transaction identifier [8 bits] = 0x2D [ 45 ]
    	Message Type [8 bits] = 0xC1 - Activate Default EPS Bearer Context Request [ 193 ]
    	EPS QoS
    		IE Length [8 bits] = 0x9 [ 9 ]
    		QCI = 0x09 [ 9 ]
    		Maximum Bit Rate for Uplink = 0x40 - The Maximum Bit Rate is 64 kbps +  ((The Binary Coded Value in 8 Bits -01000000) * 8 Kbps) [ 64 ]
    		Maximum Bit Rate for Dlink = 0x40 - The Maximum Bit Rate is 64 kbps +  ((The Binary Coded Value in 8 Bits -01000000) * 8 Kbps) [ 64 ]
    		Guaranteed Bit Rate for Ulink = 0x40 [ 64 ]
    		Guaranteed Bit Rate for Dlink = 0x40 [ 64 ]
    		Maximum bit rate for uplink (extended) = 0x00 [ 0 ]
    		Maximum bit rate for downlink (extended) = 0x00 [ 0 ]
    		Guaranteed bit rate for uplink (extended) = 0x00 [ 0 ]
    		Guaranteed bit rate for downlink (extended) = 0x00 [ 0 ]
    	APN Address
    		IE Length [8 bits] = 0x4 [ 4 ]
    		Value = 0x0361706E [ 56717422 ]
    	PDN address
    		IE Length [8 bits] = 0xD [ 13 ]
    		Spare Bits [5 bits] = 0x0 [ 0 ]
    		PDN type value [3 bits] = 0x3 [ 3 ]
    		PDN address information = 0x0000000000000002C0A8001A
    	Protocol Configuration Options
    		IE Identifier [8 bits] = 0x27 [ 39 ]
    		IE Length [8 bits] = 0x1B [ 27 ]
    		Extension Bit [1 bit] = 0x1 - Outgoing Calls Barred within CUG [ 1 ]
    		Spare Bits [4 bits] = 0x0 [ 0 ]
    		Configuration Protocol [3 bits] = 0x0 - PPP for Use with IP PDP Type [ 0 ]
    		Option1
    			Identifier = 0x000D [ 13 ]
    			Length [8 bits] = 0x4 [ 4 ]
    			value = 0xC0A8C637 [ 3232286263 ]
    		Option2
    			Identifier = 0x0003 - DNS Server Address Request [ 3 ]
    			Length [8 bits] = 0x10 [ 16 ]
    			Value = 0xFD29CC437FB90002020C29FFFE66B4C7

    Activate Default EPS Bearer Context Request PDU

    Attach Accept
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    	Message Type [8 bits] = 0x42 - Attach Accept [ 66 ]
    	Spare Half Octet [4 bits] = 0x0 [ 0 ]
    	EPS attach result
    		Spare Bits [1 bit] = 0x0 [ 0 ]
    		Value [3 bits] = 0x2 [ 2 ]
    	T3412 value
    		Timer Value Unit [3 bits] = 0x7 - Value Indicates that the Timer is Deactivated [ 7 ]
    		Value [5 bits] = 0x0 [ 0 ]
    	Tracking area identity list
    		IE Length [8 bits] = 0x6 [ 6 ]
    		Spare Bits [1 bit] = 0x0 [ 0 ]
    		Type of list [2 bits] = 0x0 [ 0 ]
    		number of elements [5 bits] = 0x0 [ 0 ]
    		Mobile Country Code 1st and 2nd  Digits = 0x00 [ 0 ]
    		Mobile Network Code 3rd Digit = 0xF [ 15 ]
    		Mobile Country Code 3rd Digit = 0x1 [ 1 ]
    		Mobile Network Code 1st and 2nd  Digits = 0x10 [ 16 ]
    		Tracking area code 1 = 0x00 [ 0 ]
    		Tracking area code 1 continued = 0x01 [ 1 ]
    	ESM message container
    		IE Length [16 bits] = 0x3D [ 61 ]
    		ESM message container contents = 0xC22DC109094040404000000000040361706E0D030000000000000002C0A8001A271B80000D04C0A8C637000310FD29CC437FB90002020C29FFFE66B4C7
    	EPS mobile identity
    		IE Identifier [8 bits] = 0x50 [ 80 ]
    		IE Length [8 bits] = 0xB [ 11 ]
    		constant / IMSI Identity Digit 1 [4 bits] = 0xF [ 15 ]
    		Odd / Even Indicator [1 bit] = 0x0 [ 0 ]
    		EPS Type of Identity [3 bits] = 0x6 - GUTI [ 6 ]
    		Mobile Country Code 1st and 2nd  Digits = 0x00 [ 0 ]
    		Mobile Network Code 3rd Digit = 0xF [ 15 ]
    		Mobile Country Code 3rd Digit = 0x1 [ 1 ]
    		Mobile Network Code 1st and 2nd  Digits = 0x10 [ 16 ]
    		MME group Id = 0x8001 [ 32769 ]
    		MME code = 0x01 [ 1 ]
    		M-TMSI = 0xC2345678 [ 3258209912 ]
    	Location Area Identification
    		IE Identifier [8 bits] = 0x13 [ 19 ]
    		Mobile Country Code 1st and 2nd  Digits = 0x00 [ 0 ]
    		Mobile Network Code 3rd Digit = 0xF [ 15 ]
    		Mobile Country Code 3rd Digit = 0x1 [ 1 ]
    		Mobile Network Code 1st and 2nd  Digits = 0x10 [ 16 ]
    		Location Area Code = 0x0001 [ 1 ]
    	Mobile Identity
    		IE Identifier [8 bits] = 0x23 [ 35 ]
    		IE Length [8 bits] = 0x5 [ 5 ]
    		First Digit [4 bits] = 0xF - IMSI,IMEI or IMEISV [ 15 ]
    		Odd / Even Indicator [1 bit] = 0x0 [ 0 ]
    		Type of Identity [3 bits] = 0x4 - TMSI/P-TMSI [ 4 ]
    		Other Digits = 0x12345678 [ 305419896 ]
    	EPS Network feature support
    		IE Identifier [8 bits] = 0x64 [ 100 ]
    		IE Length [8 bits] = 0x1 [ 1 ]
    		cp_clot [1 bit] = 0x0 [ 0 ]
    		er_wo_pdn [1 bit] = 0x0 [ 0 ]
    		esr_ps [1 bit] = 0x0 [ 0 ]
    		Location Services Indicator in CS  [2 bits] = 0x0 - No information about support of location services via CS domain is available [ 0 ]
    		Location Services Indicator in EPC [1 bit] = 0x0 - Location services via EPC not supported [ 0 ]
    		Emergency Bearer Services Indicator  [1 bit] = 0x0 - Emergency bearer services in S1 mode not supported [ 0 ]
    		IMS VoPS [1 bit] = 0x1 [ 1 ]

    Attach Accept PDU

    Ciphered NAS Message
    	0xCE18D4BF1FA0C62AC75C1FB590D3A299B10C8B046C498C68BC2FCD1F09E5E257C7EAE465993A22575DDAA64A69F0C7FF15CACE3761E7BD7A18AE4F02FFB85971C6B9C8A5291FAA3ABA4D5E6CEB8DD9C3A1C2D661B3EDA3C83B4F98069637611312A6A9BB5825DF

    Ciphered NAS Message DL PDU

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		Cell
    			AddOrReconfigure
    				StaticResourceConfig = Omit
    				CellConfigCommon = Omit
    				PhysicalLayer = Omit
    				BcchConfig = Omit
    				PcchConfig = Omit
    				RachProcedureConfig = Omit
    				CcchDcchDtchConfig
    					DL = Omit
    					UL
    						SearchSpaceAndDci
    							AssignedBWPs = Omit
    							SearchSpaceType = Omit
    							DciInfo
    								ResoureAssignment
    									ResourceAllocationType = Omit
    									FreqDomain
    										FirstRbIndex = 0
    										Nprb = 24
    									TimeDomain = Omit
    									TransportBlockScheduling
    										NR_TransportBlockSingleTransmission_Type
    											TimingOffset
    												None = True
    											ImcsValue = 9
    											RedundancyVersion = 0
    											ToggleNDI = True
    									HarqProcessConfig = Omit
    								PuschHoppingCtrl = Omit
    								TpcCommandPusch = Omit
    								UL_SUL_Indicator = Omit
    								Format = Omit
    						PUCCH_Synch
    							Auto
    								TimingAdvance = 31
    								TA_Period = 600
    						GrantConfig
    							OnSR_Reception = True
    					DrxCtrl = Omit
    					MeasGapCtrl = Omit
    				ServingCellConfig = Omit

    Sent from port: ENDC_NR_PTC:SYS

    Security Protected NAS Message
    	Security header type [4 bits] = 0x2 [ 2 ]
    	Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    	MAC = 0x8F7D6EEF [ 2407362287 ]
    	Sequence Number = 0x02 [ 2 ]
    	NAS message = 0xCE18D4BF1FA0C62AC75C1FB590D3A299B10C8B046C498C68BC2FCD1F09E5E257C7EAE465993A22575DDAA64A69F0C7FF15CACE3761E7BD7A18AE4F02FFB85971C6B9C8A5291FAA3ABA4D5E6CEB8DD9C3A1C2D661B3EDA3C83B4F98069637611312A6A9BB5825DF

    Security Protected NAS Message DL PDU

    DL-DCCH-Message
    	message = c1 = rrcConnectionReconfiguration =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = c1 = rrcConnectionReconfiguration-r8 =
    			dedicatedInfoNASList = SEQUENCE OF DedicatedInfoNAS
    				DedicatedInfoNAS(1) = 278F7D6EEF02CE18D4BF1FA0C62AC75C1FB590D3A299B10C8B046C498C68BC2FCD1F09E5E257C7EAE465993A22575DDAA64A69F0C7FF15CACE3761E7BD7A18AE4F02FFB85971C6B9C8A5291FAA3ABA4D5E6CEB8DD9C3A1C2D661B3EDA3C83B4F98069637611312A6A9BB5825DF
    			radioResourceConfigDedicated
    				srb-ToAddModList = SEQUENCE OF SRB-ToAddMod
    					SRB-ToAddMod(1)
    						srb-Identity = 2
    						rlc-Config = defaultValue = NULL
    						logicalChannelConfig = defaultValue = NULL
    				drb-ToAddModList = SEQUENCE OF DRB-ToAddMod
    					DRB-ToAddMod(1)
    						eps-BearerIdentity = 12
    						drb-Identity = 8
    						pdcp-Config
    							discardTimer = infinity
    							rlc-AM
    								statusReportRequired = TRUE
    							headerCompression = notUsed = NULL
    						rlc-Config = am =
    							ul-AM-RLC
    								t-PollRetransmit = ms80
    								pollPDU = p128
    								pollByte = kB125
    								maxRetxThreshold = t4
    							dl-AM-RLC
    								t-Reordering = ms80
    								t-StatusProhibit = ms60
    						logicalChannelIdentity = 10
    						logicalChannelConfig
    							ul-SpecificParameters
    								priority = 6
    								prioritisedBitRate = kBps0
    								bucketSizeDuration = ms100
    								logicalChannelGroup = 1
    				mac-MainConfig = explicitValue =
    					ul-SCH-Config
    						maxHARQ-Tx = n5
    						periodicBSR-Timer = sf20
    						retxBSR-Timer = sf320
    						ttiBundling = FALSE
    					drx-Config = setup =
    						onDurationTimer = psf6
    						drx-InactivityTimer = psf1920
    						drx-RetransmissionTimer = psf16
    						longDRX-CycleStartOffset = sf1280 = 4
    					timeAlignmentTimerDedicated = sf750
    					phr-Config = setup =
    						periodicPHR-Timer = sf500
    						prohibitPHR-Timer = sf200
    						dl-PathlossChange = dB3
    				physicalConfigDedicated
    					tpc-PDCCH-ConfigPUCCH = setup =
    						tpc-RNTI = 0000001111111111
    						tpc-Index = indexOfFormat3 = 1
    					tpc-PDCCH-ConfigPUSCH = setup =
    						tpc-RNTI = 0000000111111010
    						tpc-Index = indexOfFormat3 = 1
    					cqi-ReportConfig
    						cqi-ReportModeAperiodic = rm30
    						nomPDSCH-RS-EPRE-Offset = 0
    						cqi-ReportPeriodic = setup =
    							cqi-PUCCH-ResourceIndex = 0
    							cqi-pmi-ConfigIndex = 25
    							cqi-FormatIndicatorPeriodic = widebandCQI = NULL
    							ri-ConfigIndex = 483
    							simultaneousAckNackAndCQI = FALSE
    					soundingRS-UL-ConfigDedicated = setup =
    						srs-Bandwidth = bw0
    						srs-HoppingBandwidth = hbw0
    						freqDomainPosition = 0
    						duration = TRUE
    						srs-ConfigIndex = 20
    						transmissionComb = 0
    						cyclicShift = cs0
    					antennaInfo = defaultValue = NULL

    rrcConnectionReconfiguration

    RRC_PDU_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcConnectionReconfiguration
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							c1
    								rrcConnectionReconfiguration_r8
    									measConfig = Omit
    									mobilityControlInfo = Omit
    									dedicatedInfoNASList
    										NAS_Message = '278F7D6EEF02CE18D4BF1FA0C62AC75C1FB590D3A299B10C8B046C498C68BC2FCD1F09E5E257C7EAE465993A22575DDAA64A69F0C7FF15CACE3761E7BD7A18AE4F02FFB85971C6B9C8A5291FAA3ABA4D5E6CEB8DD9C3A1C2D661B3EDA3C83B4F98069637611312A6A9BB5825DF'O
    									radioResourceConfigDedicated
    										srb_ToAddModList
    											SRB_ToAddMod
    												srb_Identity = 2
    												rlc_Config
    													defaultValue = Null
    												logicalChannelConfig
    													defaultValue = Null
    												pdcp_verChange_r15 = Omit
    												rlc_Config_v1530 = Omit
    												rlc_BearerConfigDupl_r15 = Omit
    												srb_Identity_v1530 = Omit
    										drb_ToAddModList
    											DRB_ToAddMod
    												eps_BearerIdentity = 12
    												drb_Identity = 8
    												pdcp_Config
    													discardTimer = infinity_ (7)
    													rlc_AM
    														statusReportRequired = True
    													rlc_UM = Omit
    													headerCompression
    														notUsed = Null
    													rn_IntegrityProtection_r10 = Omit
    													pdcp_SN_Size_v1130 = Omit
    													ul_DataSplitDRB_ViaSCG_r12 = Omit
    													t_Reordering_r12 = Omit
    													ul_DataSplitThreshold_r13 = Omit
    													pdcp_SN_Size_v1310 = Omit
    													statusFeedback_r13 = Omit
    													ul_LWA_Config_r14 = Omit
    													uplinkOnlyHeaderCompression_r14 = Omit
    													uplinkDataCompression_r15 = Omit
    													pdcp_DuplicationConfig_r15 = Omit
    												rlc_Config
    													am
    														ul_AM_RLC
    															t_PollRetransmit = ms80 (15)
    															pollPDU = p128 (5)
    															pollByte = kB125 (4)
    															maxRetxThreshold = t4 (3)
    														dl_AM_RLC
    															t_Reordering = ms80 (16)
    															t_StatusProhibit = ms60 (12)
    												logicalChannelIdentity = 10
    												logicalChannelConfig
    													ul_SpecificParameters
    														priority = 6
    														prioritisedBitRate = kBps0 (0)
    														bucketSizeDuration = ms100 (1)
    														logicalChannelGroup = 1
    													logicalChannelSR_Mask_r9 = Omit
    													logicalChannelSR_Prohibit_r12 = Omit
    													laa_UL_Allowed_r14 = Omit
    													bitRateQueryProhibitTimer_r14 = Omit
    													allowedTTI_Lengths_r15 = Omit
    													logicalChannelSR_Restriction_r15 = Omit
    													channellAccessPriority_r15 = Omit
    													lch_CellRestriction_r15 = Omit
    												drb_TypeChange_r12 = Omit
    												rlc_Config_v1250 = Omit
    												rlc_Config_v1310 = Omit
    												drb_TypeLWA_r13 = Omit
    												drb_TypeLWIP_r13 = Omit
    												rlc_Config_v1430 = Omit
    												lwip_UL_Aggregation_r14 = Omit
    												lwip_DL_Aggregation_r14 = Omit
    												lwa_WLAN_AC_r14 = Omit
    												rlc_Config_v1510 = Omit
    												rlc_Config_v1530 = Omit
    												rlc_BearerConfigDupl_r15 = Omit
    												logicalChannelIdentity_r15 = Omit
    										drb_ToReleaseList = Omit
    										mac_MainConfig
    											explicitValue
    												ul_SCH_Config
    													maxHARQ_Tx = n5 (4)
    													periodicBSR_Timer = sf20 (3)
    													retxBSR_Timer = sf320 (0)
    													ttiBundling = False
    												drx_Config
    													setup
    														onDurationTimer = psf6 (5)
    														drx_InactivityTimer = psf1920 (20)
    														drx_RetransmissionTimer = psf16 (5)
    														longDRX_CycleStartOffset
    															sf1280 = 4
    														shortDRX = Omit
    												timeAlignmentTimerDedicated = sf750 (1)
    												phr_Config
    													setup
    														periodicPHR_Timer = sf500 (5)
    														prohibitPHR_Timer = sf200 (5)
    														dl_PathlossChange = dB3 (1)
    												sr_ProhibitTimer_r9 = Omit
    												mac_MainConfig_v1020 = Omit
    												stag_ToReleaseList_r11 = Omit
    												stag_ToAddModList_r11 = Omit
    												drx_Config_v1130 = Omit
    												e_HARQ_Pattern_r12 = Omit
    												dualConnectivityPHR = Omit
    												logicalChannelSR_Config_r12 = Omit
    												drx_Config_v1310 = Omit
    												extendedPHR2_r13 = Omit
    												eDRX_Config_CycleStartOffset_r13 = Omit
    												drx_Config_r13 = Omit
    												skipUplinkTx_r14 = Omit
    												dataInactivityTimerConfig_r14 = Omit
    												rai_Activation_r14 = Omit
    												shortTTI_AndSPT_r15 = Omit
    												mpdcch_UL_HARQ_ACK_FeedbackConfig_r15 = Omit
    												dormantStateTimers_r15 = Omit
    										sps_Config = Omit
    										physicalConfigDedicated
    											pdsch_ConfigDedicated = Omit
    											pucch_ConfigDedicated = Omit
    											pusch_ConfigDedicated = Omit
    											uplinkPowerControlDedicated = Omit
    											tpc_PDCCH_ConfigPUCCH
    												setup
    													tpc_RNTI = 0000001111111111'B
    													tpc_Index
    														indexOfFormat3 = 1
    											tpc_PDCCH_ConfigPUSCH
    												setup
    													tpc_RNTI = 0000000111111010'B
    													tpc_Index
    														indexOfFormat3 = 1
    											cqi_ReportConfig
    												cqi_ReportModeAperiodic = rm30 (3)
    												nomPDSCH_RS_EPRE_Offset = 0
    												cqi_ReportPeriodic
    													setup
    														cqi_PUCCH_ResourceIndex = 0
    														cqi_pmi_ConfigIndex = 25
    														cqi_FormatIndicatorPeriodic
    															widebandCQI = Null
    														ri_ConfigIndex = 483
    														simultaneousAckNackAndCQI = False
    											soundingRS_UL_ConfigDedicated
    												setup
    													srs_Bandwidth = bw0 (0)
    													srs_HoppingBandwidth = hbw0 (0)
    													freqDomainPosition = 0
    													duration = True
    													srs_ConfigIndex = 20
    													transmissionComb = 0
    													cyclicShift = cs0 (0)
    											antennaInfo
    												defaultValue = Null
    											schedulingRequestConfig = Omit
    											cqi_ReportConfig_v920 = Omit
    											antennaInfo_v920 = Omit
    											antennaInfo_r10 = Omit
    											antennaInfoUL_r10 = Omit
    											cif_Presence_r10 = Omit
    											cqi_ReportConfig_r10 = Omit
    											csi_RS_Config_r10 = Omit
    											pucch_ConfigDedicated_v1020 = Omit
    											pusch_ConfigDedicated_v1020 = Omit
    											schedulingRequestConfig_v1020 = Omit
    											soundingRS_UL_ConfigDedicated_v1020 = Omit
    											soundingRS_UL_ConfigDedicatedAperiodic_r10 = Omit
    											uplinkPowerControlDedicated_v1020 = Omit
    											additionalSpectrumEmissionCA_r10 = Omit
    											csi_RS_ConfigNZPToReleaseList_r11 = Omit
    											csi_RS_ConfigNZPToAddModList_r11 = Omit
    											csi_RS_ConfigZPToReleaseList_r11 = Omit
    											csi_RS_ConfigZPToAddModList_r11 = Omit
    											epdcch_Config_r11 = Omit
    											pdsch_ConfigDedicated_v1130 = Omit
    											cqi_ReportConfig_v1130 = Omit
    											pucch_ConfigDedicated_v1130 = Omit
    											pusch_ConfigDedicated_v1130 = Omit
    											uplinkPowerControlDedicated_v1130 = Omit
    											antennaInfo_v1250 = Omit
    											eimta_MainConfig_r12 = Omit
    											eimta_MainConfigPCell_r12 = Omit
    											pucch_ConfigDedicated_v1250 = Omit
    											cqi_ReportConfigPCell_v1250 = Omit
    											uplinkPowerControlDedicated_v1250 = Omit
    											pusch_ConfigDedicated_v1250 = Omit
    											csi_RS_Config_v1250 = Omit
    											pdsch_ConfigDedicated_v1280 = Omit
    											pdsch_ConfigDedicated_v1310 = Omit
    											pucch_ConfigDedicated_r13 = Omit
    											pusch_ConfigDedicated_r13 = Omit
    											pdcch_CandidateReductions_r13 = Omit
    											cqi_ReportConfig_v1310 = Omit
    											soundingRS_UL_ConfigDedicated_v1310 = Omit
    											soundingRS_UL_ConfigDedicatedUpPTsExt_r13 = Omit
    											soundingRS_UL_ConfigDedicatedAperiodic_v1310 = Omit
    											soundingRS_UL_ConfigDedicatedAperiodicUpPTsExt_r13 = Omit
    											csi_RS_Config_v1310 = Omit
    											ce_Mode_r13 = Omit
    											csi_RS_ConfigNZPToAddModListExt_r13 = Omit
    											csi_RS_ConfigNZPToReleaseListExt_r13 = Omit
    											cqi_ReportConfig_v1320 = Omit
    											typeA_SRS_TPC_PDCCH_Group_r14 = Omit
    											must_Config_r14 = Omit
    											pusch_EnhancementsConfig_r14 = Omit
    											ce_pdsch_pusch_EnhancementConfig_r14 = Omit
    											antennaInfo_v1430 = Omit
    											pucch_ConfigDedicated_v1430 = Omit
    											pdsch_ConfigDedicated_v1430 = Omit
    											pusch_ConfigDedicated_v1430 = Omit
    											soundingRS_UL_PeriodicConfigDedicatedList_r14 = Omit
    											soundingRS_UL_PeriodicConfigDedicatedUpPTsExtList_r14 = Omit
    											soundingRS_UL_AperiodicConfigDedicatedList_r14 = Omit
    											soundingRS_UL_ConfigDedicatedApUpPTsExtList_r14 = Omit
    											csi_RS_Config_v1430 = Omit
    											csi_RS_ConfigZP_ApList_r14 = Omit
    											cqi_ReportConfig_v1430 = Omit
    											semiOpenLoop_r14 = Omit
    											csi_RS_Config_v1480 = Omit
    											physicalConfigDedicatedSTTI_r15 = Omit
    											pdsch_ConfigDedicated_v1530 = Omit
    											pusch_ConfigDedicated_v1530 = Omit
    											cqi_ReportConfig_v1530 = Omit
    											antennaInfo_v1530 = Omit
    											csi_RS_Config_v1530 = Omit
    											uplinkPowerControlDedicated_v1530 = Omit
    											semiStaticCFI_Config_r15 = Omit
    											blindPDSCH_Repetition_Config_r15 = Omit
    										rlf_TimersAndConstants_r9 = Omit
    										measSubframePatternPCell_r10 = Omit
    										neighCellsCRS_Info_r11 = Omit
    										naics_Info_r12 = Omit
    										neighCellsCRS_Info_r13 = Omit
    										rlf_TimersAndConstants_r13 = Omit
    										sps_Config_v1430 = Omit
    										srb_ToAddModExtList_r15 = Omit
    										srb_ToReleaseExtList_r15 = Omit
    										sps_Config_v1530 = Omit
    										crs_IntfMitigConfig_r15 = Omit
    										neighCellsCRS_Info_r15 = Omit
    										drb_ToAddModList_r15 = Omit
    										drb_ToReleaseList_r15 = Omit
    										dummy = Omit
    										sps_Config_v1540 = Omit
    									securityConfigHO = Omit
    									nonCriticalExtension = Omit

    Sent from port: NASEMU_EUTRA_PTC:SYS_SRB

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		Cell = True

    Received on port: ENDC_NR_PTC:SYS

    UL-DCCH-Message
    	message = c1 = rrcConnectionReconfigurationComplete =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcConnectionReconfigurationComplete-r8 =

    rrcConnectionReconfigurationComplete

    UL-DCCH-Message
    	message = c1 = ulInformationTransfer =
    		criticalExtensions = c1 = ulInformationTransfer-r8 =
    			dedicatedInfoType = dedicatedInfoNAS = 27A61CD45E02564FAF0A3F2963

    ulInformationTransfer

    Security Protected NAS Message
    	Security header type [4 bits] = 0x2 [ 2 ]
    	Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    	MAC = 0x261C545E [ 639390814 ]
    	Sequence Number = 0x02 [ 2 ]
    	NAS message = 0x564F2F0A3F2963

    Security Protected NAS Message UL PDU

    Ciphered NAS Message
    	0x564F2F0A3F2963

    Ciphered NAS Message UL PDU

    RRC_PDU_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 638
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcConnectionReconfigurationComplete
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcConnectionReconfigurationComplete_r8
    								nonCriticalExtension = Omit

    Received on port: NASEMU_EUTRA_PTC:SYS_SRB

    SRB_COMMON_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 638
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcConnectionReconfigurationComplete
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcConnectionReconfigurationComplete_r8
    									nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: SRB -> EUTRA_5GS_PTC:SRB

    RRC_PDU_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 2
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 638
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ulInformationTransfer
    						criticalExtensions
    							c1
    								ulInformationTransfer_r8
    									dedicatedInfoType
    										dedicatedInfoNAS = '27A61CD45E02564FAF0A3F2963'O
    									nonCriticalExtension = Omit

    Received on port: NASEMU_EUTRA_PTC:SYS_SRB

    Activate Default EPS Bearer Context Accept
    	EPS bearer identity [4 bits] = 0xC [ 12 ]
    	Protocol Discriminator [4 bits] = 0x2 - EPS Session Management Messages [ 2 ]
    	Procedure transaction identifier [8 bits] = 0x0 [ 0 ]
    	Message Type [8 bits] = 0xC2 - Activate Default EPS Bearer Context Accept [ 194 ]

    Activate Default EPS Bearer Context Accept PDU

    Attach Complete
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    	Message Type [8 bits] = 0x43 - Attach Complete [ 67 ]
    	ESM message container
    		IE Length [16 bits] = 0x3 [ 3 ]
    		ESM message container contents = 0xC200C2 [ 12714178 ]

    Attach Complete PDU

    SRB_COMMON_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 2
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 638
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0010'B
    					NasCount = '00000002'O
    				Pdu
    					Msg
    						aTTACH_COMPLETE
    							securityHeaderType = 0000'B
    							protocolDiscriminator = 0111'B
    							messageType = 01000011'B
    							esmMessage
    								iei = Omit
    								iel = '0003'O
    								esmPdu = 'C200C2'O
    					PiggybackedPduList
    						NAS_UL_Pdu_Type
    							Msg
    								aCTIVATE_DEFAULT_EPS_BEARER_CONTEXT_ACCEPT
    									epsBearerId = 'C'H
    									protocolDiscriminator = 0010'B
    									procedureTransactionIdentifier = '00'O
    									messageType = 11000010'B
    									protocolConfigurationOptions = Omit
    									extdProtocolConfigurationOptions = Omit
    							PiggybackedPduList = Omit

    Inter-component message: SRB -> EUTRA_5GS_PTC:SRB

    IMS_IPCAN_Coordination_MSG
    	IPCAN_IMS_Control
    		NoRegistration = True

    Inter-component message: IPCAN -> IMS_PTC:IPCAN

    timerEvent = 6
    fileName = C:\Users\FETCTTEST\Desktop\Dev_TTCNs\Deepak\7.1.3.3.x\ENDC_IWD_19wk23\Common\IMS\IMS_PTC_CoordMsg.ttcn
    testName = TC_8_2_3_5_1_ENDC
    lineNo = 413
    outStr = Timer: t_WaitForUPlaneSignalling, Duration: 1.2s, Started: 07:00:15

    Timer: t_WaitForUPlaneSignalling, Duration: 1.2s, Started: 07:00:15

    IP_SOCKET_IND
    	DATA
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FF02:0000:0000:0000:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    			Remote
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    		Ind
    			ICMP
    				RecvFrom
    					Buffer = '85007D3500000000'O
    					DrbInfo
    						Eutra
    							CellId = eutra_Cell1 (1)
    							DrbId = 8

    Received on port: IPMUX_PTC:IP_SOCK

    ConstraintMismatch::Received:
    summary = Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol
    		DATA
    			ConnectionId
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FF02:0000:0000:0000:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = Omit
    				Remote
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    							ScopeId = Omit
    					Port = Omit
    			Ind
    				ICMP
    					RecvFrom
    						Buffer = '85007D3500000000'O
    						DrbInfo
    							Eutra
    								CellId = eutra_Cell1 (1)
    								DrbId = 8
    ConstraintMismatch::Expected:
    summary = Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol
    MESSAGE_MISMATCH
    	Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol
    		DATA
    			ConnectionId
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr
    							ScopeId
    					Port = 67
    				Remote
    					IpAddr
    						V6
    							Addr
    							ScopeId
    					Port = AnyValue
    			Ind
    				UDP
    					RecvFrom
    						Buffer
    						DrbInfo
    							Eutra
    								CellId
    								DrbId

    Message Mismatch: IP_SOCKET_IND.DATA.ConnectionId.Protocol

    IP_SOCKET_IND
    	DATA
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FF02:0000:0000:0000:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    			Remote
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    		Ind
    			ICMP
    				RecvFrom
    					Buffer = '85007D3500000000'O
    					DrbInfo
    						Eutra
    							CellId = eutra_Cell1 (1)
    							DrbId = 8

    Inter-component message: IP_SOCK_DATA -> IP_PTC:IP_SOCK_DATA

    IP_SOCKET_REQ
    	DATA
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = Omit
    			Remote
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    		Req
    			ICMP
    				SendTo
    					Buffer = '8600EA104000FFFF000000000000000003044040FFFFFFFFFFFFFFFF0000000030000000000000020000000000000000'O

    Inter-component message: IP_SOCK_DATA -> IPMUX_PTC:IP_SOCK_DATA

    IP_SOCKET_REQ
    	DATA
    		ConnectionId
    			Protocol = icmpv6 (3)
    			Local
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    						ScopeId = Omit
    				Port = Omit
    			Remote
    				IpAddr
    					V6
    						Addr = 'FE80:0000:0000:0000:0000:0000:0000:0002'
    						ScopeId = Omit
    				Port = Omit
    		Req
    			ICMP
    				SendTo
    					Buffer = '8600EA104000FFFF000000000000000003044040FFFFFFFFFFFFFFFF0000000030000000000000020000000000000000'O

    Sent from port: IPMUX_PTC:IP_SOCK

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		CellAttenuationList
    			NR_CellAttenuationConfig_Type
    				CellId = nr_Cell1 (1)
    				Attenuation
    					Value = 3
    				TimingInfo = Omit

    Sent from port: ENDC_NR_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		CellAttenuationList = True

    Received on port: ENDC_NR_PTC:SYS

    timerEvent = 9
    fileName = C:\Users\FETCTTEST\Desktop\Dev_TTCNs\Deepak\7.1.3.3.x\ENDC_IWD_19wk23\Common\IMS\IMS_PTC_CoordMsg.ttcn
    testName = TC_8_2_3_5_1_ENDC
    lineNo = 415
    outStr = Timer: t_WaitForUPlaneSignalling, Expired: 07:00:16

    Timer: t_WaitForUPlaneSignalling, Expired: 07:00:16

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		EnquireTiming = True

    Sent from port: EUTRA_5GS_PTC:SYS

    SYSTEM_CTRL_CNF
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 766
    				Subframe
    					Number = 2
    				HSFN
    					Number = 78
    				Slot
    					FirstSlot = True
    		Result
    			Success = True
    	Confirm
    		EnquireTiming = True

    Received on port: EUTRA_5GS_PTC:SYS

    timerEvent = 6
    fileName = C:\Users\FETCTTEST\Desktop\Dev_TTCNs\Deepak\7.1.3.3.x\ENDC_IWD_19wk23\Common\EUTRA\EUTRA_RRCSteps.ttcn
    testName = TC_8_2_3_5_1_ENDC
    lineNo = 1607
    outStr = Timer: t_Timer, Duration: 2.02s, Started: 07:00:16

    Timer: t_Timer, Duration: 2.02s, Started: 07:00:16

    SRB_COMMON_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 876
    				Subframe
    					Number = 4
    				HSFN
    					Number = 78
    				Slot
    					FirstSlot = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcConnectionRelease
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								c1
    									rrcConnectionRelease_r8
    										releaseCause = other (1)
    										redirectedCarrierInfo = Omit
    										idleModeMobilityControlInfo = Omit
    										nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: TC_SRB -> NASEMU_EUTRA_PTC:TC_SRB

    DL-DCCH-Message
    	message = c1 = rrcConnectionRelease =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = c1 = rrcConnectionRelease-r8 =
    			releaseCause = other

    rrcConnectionRelease

    RRC_PDU_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 876
    				Subframe
    					Number = 4
    				HSFN
    					Number = 78
    				Slot
    					FirstSlot = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcConnectionRelease
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							c1
    								rrcConnectionRelease_r8
    									releaseCause = other (1)
    									redirectedCarrierInfo = Omit
    									idleModeMobilityControlInfo = Omit
    									nonCriticalExtension = Omit

    Sent from port: NASEMU_EUTRA_PTC:SYS_SRB

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		PdcpCount
    			Get
    				AllRBs = True

    Sent from port: EUTRA_5GS_PTC:SYS

    SYSTEM_CTRL_CNF
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		PdcpCount
    			Get
    				PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 1
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000001000'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000001000'B
    				PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 2
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000001'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    				PdcpCountInfo_Type
    					RadioBearerId
    						Drb = 1
    					UL
    						Format = PdcpCount_DrbLongSQN (1)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_DrbLongSQN (1)
    						Value = 00000000000000000000000000000000'B
    				PdcpCountInfo_Type
    					RadioBearerId
    						Drb = 8
    					UL
    						Format = PdcpCount_DrbLongSQN (1)
    						Value = 00000000000000000000000000000001'B
    					DL
    						Format = PdcpCount_DrbLongSQN (1)
    						Value = 00000000000000000000000000000001'B

    Received on port: EUTRA_5GS_PTC:SYS

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 876
    			Subframe
    				Number = 4
    			HSFN
    				Number = 78
    			Slot
    				FirstSlot = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		Now
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				FirstSlot

    Message Mismatch: TimingInfo_Type

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 876
    				Subframe
    					Number = 4
    				HSFN
    					Number = 78
    				Slot
    					FirstSlot = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		Cell
    			AddOrReconfigure
    				Basic
    					ConfigCapability = Omit
    					StaticCellInfo = Omit
    					PhysicalLayerConfigDL = Omit
    					InitialCellPower = Omit
    					BcchConfig = Omit
    					PcchConfig = Omit
    					CA_CellInitialConfig = Omit
    					BRBcchConfig = Omit
    					LAA_SCellConfiguration = Omit
    					LAA_SCellConfiguration_v1430 = Omit
    				Active
    					C_RNTI = Omit
    					PhysicalLayerConfigUL = Omit
    					RachProcedureConfig = Omit
    					CcchDcchDtchConfig
    						MeasGapCtrl = Omit
    						DL = Omit
    						UL
    							DciInfo
    								Imcs = Omit
    								TransRetransmissionList = Omit
    								FreqDomainSchedul = Omit
    								Format = Omit
    								HarqProcessId = Omit
    								RepetitionNumber = Omit
    								DCISubframeRepetitionNumber = Omit
    								PUSCH_TriggerA = Omit
    								TimingOffset = Omit
    								NumberOfScheduledSubframes = Omit
    							Hopping
    								Deactivated = True
    							PUCCH_Synch
    								None = True
    							UL_GrantConfig
    								None = True
    						DrxCtrl = Omit
    						TtiBundling = Omit
    						CifPresence = Omit
    					ServingCellConfig = Omit
    					SciSchedulingConfig = Omit
    					EIMTA_Config = Omit
    					CE_Mode = Omit

    Sent from port: EUTRA_5GS_PTC:SYS

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 876
    			Subframe
    				Number = 9
    			HSFN
    				Number = 78
    			Slot
    				FirstSlot = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		Now
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				FirstSlot

    Message Mismatch: TimingInfo_Type

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 876
    				Subframe
    					Number = 9
    				HSFN
    					Number = 78
    				Slot
    					FirstSlot = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		AS_Security
    			Release = True

    Sent from port: EUTRA_5GS_PTC:SYS

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 881
    			Subframe
    				Number = 9
    			HSFN
    				Number = 78
    			Slot
    				FirstSlot = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		Now
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				FirstSlot

    Message Mismatch: TimingInfo_Type

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 881
    				Subframe
    					Number = 9
    				HSFN
    					Number = 78
    				Slot
    					FirstSlot = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		RadioBearerList
    			RadioBearer_Type
    				Id
    					Srb = 1
    				Config
    					Release = True
    			RadioBearer_Type
    				Id
    					Srb = 2
    				Config
    					Release = True
    			RadioBearer_Type
    				Id
    					Drb = 1
    				Config
    					Release = True
    			RadioBearer_Type
    				Id
    					Drb = 8
    				Config
    					Release = True

    Sent from port: EUTRA_5GS_PTC:SYS

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 882
    			Subframe
    				Number = 4
    			HSFN
    				Number = 78
    			Slot
    				FirstSlot = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		Now
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				FirstSlot

    Message Mismatch: TimingInfo_Type

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 882
    				Subframe
    					Number = 4
    				HSFN
    					Number = 78
    				Slot
    					FirstSlot = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		RadioBearerList
    			RadioBearer_Type
    				Id
    					Srb = 1
    				Config
    					AddOrReconfigure
    						Pdcp
    							Config
    								Rb
    									Srb = True
    								TestMode
    									None = True
    						Rlc
    							Rb
    								AM
    									Tx
    										R8
    											t_PollRetransmit = ms45 (8)
    											pollPDU = pInfinity (7)
    											pollByte = kBinfinity (14)
    											maxRetxThreshold = t4 (3)
    									Rx
    										R8
    											t_Reordering = ms35 (7)
    											t_StatusProhibit = ms0 (0)
    									ExtendedLI = Omit
    							TestMode
    								None = True
    						LogicalChannelId = 1
    						Mac
    							LogicalChannel
    								Priority = 1
    								PrioritizedBitRate = infinity_ (7)
    								LAA_UL_Allowed = Omit
    							TestMode
    								None = True
    						DiscardULData = Omit
    			RadioBearer_Type
    				Id
    					Srb = 2
    				Config
    					AddOrReconfigure
    						Pdcp
    							Config
    								Rb
    									Srb = True
    								TestMode
    									None = True
    						Rlc
    							Rb
    								AM
    									Tx
    										R8
    											t_PollRetransmit = ms45 (8)
    											pollPDU = pInfinity (7)
    											pollByte = kBinfinity (14)
    											maxRetxThreshold = t4 (3)
    									Rx
    										R8
    											t_Reordering = ms35 (7)
    											t_StatusProhibit = ms0 (0)
    									ExtendedLI = Omit
    							TestMode
    								None = True
    						LogicalChannelId = 2
    						Mac
    							LogicalChannel
    								Priority = 3
    								PrioritizedBitRate = infinity_ (7)
    								LAA_UL_Allowed = Omit
    							TestMode
    								None = True
    						DiscardULData = Omit

    Sent from port: EUTRA_5GS_PTC:SYS

    timerEvent = 9
    fileName = C:\Users\FETCTTEST\Desktop\Dev_TTCNs\Deepak\7.1.3.3.x\ENDC_IWD_19wk23\Common\EUTRA\EUTRA_RRCSteps.ttcn
    testName = TC_8_2_3_5_1_ENDC
    lineNo = 1616
    outStr = Timer: t_Timer, Expired: 07:00:18

    Timer: t_Timer, Expired: 07:00:18

    timerEvent = 7
    fileName = C:\Users\FETCTTEST\Desktop\Dev_TTCNs\Deepak\7.1.3.3.x\ENDC_IWD_19wk23\Common\EUTRA38\EUTRA38_CommonProcedures.ttcn
    testName = TC_8_2_3_5_1_ENDC
    lineNo = 294
    outStr = Timer: t_GuardTimer, Stopped: 07:00:18

    Timer: t_GuardTimer, Stopped: 07:00:18

    EUTRA_NR_Coordination_MSG
    	Security
    		SK_Counter = 0
    		KeyToUse = S_KGNB (1)
    		Key = 0100111011011000100111011010000111001010110010010010110010011011101100110001010101101100000001000111001111100101010100000101110010011010000101001001101000010110100100001110010101000010010001111110110110111000110010011000010001001000011000011010011011110011'B
    		KSI = Omit
    		NASCount = Omit
    		E_NEACap
    			E_Nea0 = 1'B
    			E_Nea1 = 1'B
    			E_Nea2 = 1'B
    		E_NIACap
    			E_Nia0 = 0'B
    			E_Nia1 = 1'B
    			E_Nia2 = 1'B

    Inter-component message: EUTRA -> ENDC_NR_PTC:EUTRA

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		AS_Security
    			StartRestart
    				Integrity
    					Algorithm = nia1 (1)
    					KRRCint = 10100101101001111110111100101110101001011001000001100111000001000100101110001100111100011110010101111010011111101011111100011100'B
    					KUPint = Omit
    					ActTimeList = Omit
    				Ciphering
    					Algorithm = nea1 (1)
    					KRRCenc = 00001001000111101101000010111000100100011101000011000011111110011001001111100110111100001111101000100010111110111011010100101101'B
    					KUPenc = 10001101110111000100011000000111010011101111011101011011000010010110011001010001001010011001001110100100100010010101011100111001'B
    					ActTimeList
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Srb = 1
    							UL
    								None = True
    							DL
    								None = True
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Srb = 2
    							UL
    								None = True
    							DL
    								None = True
    						NR_SecurityActTime_Type
    							RadioBearerId
    								Srb = 3
    							UL
    								None = True
    							DL
    								None = True

    Sent from port: ENDC_NR_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		AS_Security = True

    Received on port: ENDC_NR_PTC:SYS

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		RadioBearerList
    			NR_RadioBearer_Type
    				Id
    					Drb = 2
    				Config
    					AddOrReconfigure
    						Sdap = Omit
    						Pdcp
    							RBTerminating
    								RbConfig
    									Params
    										Rb
    											Drb
    												SN_SizeUL = PDCP_SNLength18 (1)
    												SN_SizeDL = PDCP_SNLength18 (1)
    												HeaderCompression
    													None = True
    												IntegrityProtectionEnabled = False
    								LinkToOtherCellGroup
    									None = True
    						RlcBearer
    							Config
    								Rlc
    									Rb
    										AM
    											Tx
    												R15
    													sn_FieldLength = size18 (1)
    													t_PollRetransmit = ms30 (5)
    													pollPDU = p32768 (18)
    													pollByte = kB750 (14)
    													maxRetxThreshold = t8 (5)
    											Rx
    												R15
    													sn_FieldLength = size18 (1)
    													t_Reassembly = ms30 (6)
    													t_StatusProhibit = ms30 (6)
    									TestMode = Omit
    								LogicalChannelId = 5
    								Mac
    									LogicalChannel
    										Priority = 1
    										PrioritizedBitRate = infinity_ (15)
    									TestMode
    										None = True
    								DiscardULData = Omit

    Sent from port: ENDC_NR_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		RadioBearerList = True

    Received on port: ENDC_NR_PTC:SYS

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 2
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 2
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 1

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 2
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 3

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 0

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 2

    Message Mismatch: SearchSpaceId

    ConstraintMismatch::Received:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		SearchSpaceId = 1
    ConstraintMismatch::Expected:
    summary = Message Mismatch: SearchSpaceId
    MATCH_MISMATCH
    	Message Mismatch: SearchSpaceId
    		searchSpaceId = 3

    Message Mismatch: SearchSpaceId

    EUTRA_NR_Coordination_MSG
    	OctetData
    		Data = ' 'O
    		Description = 'Reconfig'

    Inter-component message: NR -> EUTRA_5GS_PTC:NR

    EUTRA_NR_Coordination_MSG
    	OctetData
    		Data = '14093053AFC34460'O
    		Description = 'RB'

    Inter-component message: NR -> EUTRA_5GS_PTC:NR

    timerEvent = 6
    fileName = C:\Users\FETCTTEST\Desktop\Dev_TTCNs\Deepak\7.1.3.3.x\ENDC_IWD_19wk23\Common\Common\CommonDefs.ttcn
    testName = TC_8_2_3_5_1_ENDC
    lineNo = 562
    outStr = Timer: t_Delay, Duration: 1s, Started: 07:00:18

    Timer: t_Delay, Duration: 1s, Started: 07:00:18

    timerEvent = 9
    fileName = C:\Users\FETCTTEST\Desktop\Dev_TTCNs\Deepak\7.1.3.3.x\ENDC_IWD_19wk23\Common\Common\CommonDefs.ttcn
    testName = TC_8_2_3_5_1_ENDC
    lineNo = 563
    outStr = Timer: t_Delay, Expired: 07:00:19

    Timer: t_Delay, Expired: 07:00:19

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		EnquireTiming = True

    Sent from port: EUTRA_5GS_PTC:SYS

    SYSTEM_CTRL_CNF
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 73
    				Subframe
    					Number = 7
    				HSFN
    					Number = 79
    				Slot
    					FirstSlot = True
    		Result
    			Success = True
    	Confirm
    		EnquireTiming = True

    Received on port: EUTRA_5GS_PTC:SYS

    PCCH-Message
    	message = c1 = paging =
    		pagingRecordList = SEQUENCE OF PagingRecord
    			PagingRecord(1)
    				ue-Identity = s-TMSI =
    					mmec = 00000001
    					m-TMSI = 11000010001101000101011001111000
    				cn-Domain = ps

    paging

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 149
    				Subframe
    					Number = 9
    				HSFN
    					Number = 79
    				Slot
    					FirstSlot = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		Paging
    			Paging
    				message_
    					c1
    						paging
    							pagingRecordList
    								PagingRecord
    									ue_Identity
    										s_TMSI
    											mmec = 00000001'B
    											m_TMSI = 11000010001101000101011001111000'B
    									cn_Domain = ps (0)
    							systemInfoModification = Omit
    							etws_Indication = Omit
    							nonCriticalExtension = Omit
    			SubframeOffsetList = Omit

    Sent from port: EUTRA_5GS_PTC:SYS

    ConstraintMismatch::Received:
    summary = Message Mismatch: BitStringType
    MATCH_MISMATCH
    	Message Mismatch: BitStringType = 1'B
    		BitStringType
    ConstraintMismatch::Expected:
    summary = Message Mismatch: BitStringType
    MATCH_MISMATCH
    	Message Mismatch: BitStringType = 0'B
    		BitStringType

    Message Mismatch: BitStringType

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		Cell
    			AddOrReconfigure
    				Basic
    					ConfigCapability = Omit
    					StaticCellInfo = Omit
    					PhysicalLayerConfigDL = Omit
    					InitialCellPower = Omit
    					BcchConfig = Omit
    					PcchConfig = Omit
    					CA_CellInitialConfig = Omit
    					BRBcchConfig = Omit
    					LAA_SCellConfiguration = Omit
    					LAA_SCellConfiguration_v1430 = Omit
    				Active
    					C_RNTI = Omit
    					PhysicalLayerConfigUL = Omit
    					RachProcedureConfig = Omit
    					CcchDcchDtchConfig
    						MeasGapCtrl = Omit
    						DL = Omit
    						UL
    							DciInfo
    								Imcs
    									Value = 9
    								TransRetransmissionList
    									UL_TransRetransmission_Type
    										NewTransmission = True
    								FreqDomainSchedul
    									FirstRbIndex = 0
    									Nprb = 25
    								Format = Omit
    								HarqProcessId = Omit
    								RepetitionNumber = Omit
    								DCISubframeRepetitionNumber = Omit
    								PUSCH_TriggerA = Omit
    								TimingOffset = Omit
    								NumberOfScheduledSubframes = Omit
    							Hopping
    								Deactivated = True
    							PUCCH_Synch
    								None = True
    							UL_GrantConfig
    								OnSR_Reception = True
    						DrxCtrl = Omit
    						TtiBundling = Omit
    						CifPresence = Omit
    					ServingCellConfig = Omit
    					SciSchedulingConfig = Omit
    					EIMTA_Config = Omit
    					CE_Mode = Omit

    Sent from port: EUTRA_5GS_PTC:SYS

    UL-CCCH-Message
    	message = c1 = rrcConnectionRequest =
    		criticalExtensions = rrcConnectionRequest-r8 =
    			ue-Identity = s-TMSI =
    				mmec = 00000001
    				m-TMSI = 11000010001101000101011001111000
    			establishmentCause = mt-Access
    			spare = 0

    rrcConnectionRequest

    RRC_PDU_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 0
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 155
    				Subframe
    					Number = 3
    				HSFN
    					Number = 79
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	RrcPdu
    		Ccch
    			message_
    				c1
    					rrcConnectionRequest
    						criticalExtensions
    							rrcConnectionRequest_r8
    								ue_Identity
    									s_TMSI
    										mmec = 00000001'B
    										m_TMSI = 11000010001101000101011001111000'B
    								establishmentCause = mt_Access (2)
    								spare = 0'B

    Received on port: NASEMU_EUTRA_PTC:SYS_SRB

    SRB_COMMON_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 0
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 155
    				Subframe
    					Number = 3
    				HSFN
    					Number = 79
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc
    			Ccch
    				message_
    					c1
    						rrcConnectionRequest
    							criticalExtensions
    								rrcConnectionRequest_r8
    									ue_Identity
    										s_TMSI
    											mmec = 00000001'B
    											m_TMSI = 11000010001101000101011001111000'B
    									establishmentCause = mt_Access (2)
    									spare = 0'B
    		Nas = Omit

    Inter-component message: SRB -> EUTRA_5GS_PTC:SRB

    UL-DCCH-Message
    	message = c1 = rrcConnectionSetupComplete =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = c1 = rrcConnectionSetupComplete-r8 =
    			selectedPLMN-Identity = 1
    			dedicatedInfoNAS = C7030314
    			nonCriticalExtension
    				nonCriticalExtension
    					nonCriticalExtension
    						nonCriticalExtension
    							mobilityState-r12 = normal

    rrcConnectionSetupComplete

    Service Request
    	Security header type [4 bits] = 0xC [ 12 ]
    	Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    	KSI and sequence number
    		key set identifier [3 bits] = 0x0 [ 0 ]
    		Sequence number (short) [5 bits] = 0x3 [ 3 ]
    	Message authentication code (short)
    		mac value = 0x0314 [ 788 ]

    Service Request PDU

    RRC_PDU_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 158
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcConnectionSetupComplete
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							c1
    								rrcConnectionSetupComplete_r8
    									selectedPLMN_Identity = 1
    									registeredMME = Omit
    									dedicatedInfoNAS = 'C7030314'O
    									nonCriticalExtension
    										lateNonCriticalExtension = Omit
    										nonCriticalExtension
    											gummei_Type_r10 = Omit
    											rlf_InfoAvailable_r10 = Omit
    											logMeasAvailable_r10 = Omit
    											rn_SubframeConfigReq_r10 = Omit
    											nonCriticalExtension
    												connEstFailInfoAvailable_r11 = Omit
    												nonCriticalExtension
    													mobilityState_r12 = normal (0)
    													mobilityHistoryAvail_r12 = Omit
    													logMeasAvailableMBSFN_r12 = Omit
    													nonCriticalExtension = Omit

    Received on port: NASEMU_EUTRA_PTC:SYS_SRB

    SRB_COMMON_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 158
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcConnectionSetupComplete
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								c1
    									rrcConnectionSetupComplete_r8
    										selectedPLMN_Identity = 1
    										registeredMME = Omit
    										dedicatedInfoNAS = 'C7030314'O
    										nonCriticalExtension
    											lateNonCriticalExtension = Omit
    											nonCriticalExtension
    												gummei_Type_r10 = Omit
    												rlf_InfoAvailable_r10 = Omit
    												logMeasAvailable_r10 = Omit
    												rn_SubframeConfigReq_r10 = Omit
    												nonCriticalExtension
    													connEstFailInfoAvailable_r11 = Omit
    													nonCriticalExtension
    														mobilityState_r12 = normal (0)
    														mobilityHistoryAvail_r12 = Omit
    														logMeasAvailableMBSFN_r12 = Omit
    														nonCriticalExtension = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0001'B
    					NasCount = '00000003'O
    				Pdu
    					Msg
    						sERVICE_REQUEST
    							securityHeaderType = 1100'B
    							protocolDiscriminator = 0111'B
    							ksiAndSN
    								iei = Omit
    								ksi = 000'B
    								sn = 00011'B
    							shortMAC
    								iei = Omit
    								macValue = 0000001100010100'B
    					PiggybackedPduList = Omit

    Inter-component message: SRB -> EUTRA_5GS_PTC:SRB

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		Cell
    			AddOrReconfigure
    				Basic
    					ConfigCapability = Omit
    					StaticCellInfo = Omit
    					PhysicalLayerConfigDL = Omit
    					InitialCellPower = Omit
    					BcchConfig = Omit
    					PcchConfig = Omit
    					CA_CellInitialConfig = Omit
    					BRBcchConfig = Omit
    					LAA_SCellConfiguration = Omit
    					LAA_SCellConfiguration_v1430 = Omit
    				Active
    					C_RNTI = Omit
    					PhysicalLayerConfigUL = Omit
    					RachProcedureConfig = Omit
    					CcchDcchDtchConfig
    						MeasGapCtrl = Omit
    						DL = Omit
    						UL
    							DciInfo
    								Imcs = Omit
    								TransRetransmissionList = Omit
    								FreqDomainSchedul = Omit
    								Format = Omit
    								HarqProcessId = Omit
    								RepetitionNumber = Omit
    								DCISubframeRepetitionNumber = Omit
    								PUSCH_TriggerA = Omit
    								TimingOffset = Omit
    								NumberOfScheduledSubframes = Omit
    							Hopping
    								Deactivated = True
    							PUCCH_Synch
    								Auto
    									TimingAdvance = 31
    									TA_Period = 600
    									TA_Repetition
    										Continuous = True
    							UL_GrantConfig = Omit
    						DrxCtrl = Omit
    						TtiBundling = Omit
    						CifPresence = Omit
    					ServingCellConfig = Omit
    					SciSchedulingConfig = Omit
    					EIMTA_Config = Omit
    					CE_Mode = Omit

    Sent from port: EUTRA_5GS_PTC:SYS

    SYSTEM_CTRL_CNF
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		Cell = True

    Received on port: EUTRA_5GS_PTC:SYS

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		PdcpCount
    			Get
    				AllRBs = True

    Sent from port: EUTRA_5GS_PTC:SYS

    SYSTEM_CTRL_CNF
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		PdcpCount
    			Get
    				PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 1
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000001'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    				PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 2
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    				PdcpCountInfo_Type
    					RadioBearerId
    						Drb = 1
    					UL
    						Format = PdcpCount_DrbLongSQN (1)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_DrbLongSQN (1)
    						Value = 00000000000000000000000000000000'B
    				PdcpCountInfo_Type
    					RadioBearerId
    						Drb = 8
    					UL
    						Format = PdcpCount_DrbLongSQN (1)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_DrbLongSQN (1)
    						Value = 00000000000000000000000000000000'B

    Received on port: EUTRA_5GS_PTC:SYS

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		AS_Security
    			StartRestart
    				Integrity
    					Algorithm = eia1 (1)
    					KRRCint = 00101101001111001011101001111000001001001100111010111110000101111101011010011110101100101000000101010100010000011010001110001010'B
    					ActTimeList = Omit
    				Ciphering
    					Algorithm = eea1 (1)
    					KRRCenc = 01111001010110010001111010011000101100010010101100101111100011101011101101101011100010000011110111100011000010010011010010000000'B
    					KUPenc = 00010111011100110010110101011100111001010010111110110010100110100010010110010011110001001010011011101010111001000100000100001010'B
    					ActTimeList
    						SecurityActTime_Type
    							RadioBearerId
    								Srb = 1
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 2
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 1
    						SecurityActTime_Type
    							RadioBearerId
    								Srb = 2
    							UL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 0
    							DL
    								SQN
    									Format = PdcpCount_Srb (0)
    									Value = 0
    						SecurityActTime_Type
    							RadioBearerId
    								Drb = 1
    							UL
    								SQN
    									Format = PdcpCount_DrbLongSQN (1)
    									Value = 0
    							DL
    								SQN
    									Format = PdcpCount_DrbLongSQN (1)
    									Value = 0
    						SecurityActTime_Type
    							RadioBearerId
    								Drb = 8
    							UL
    								SQN
    									Format = PdcpCount_DrbLongSQN (1)
    									Value = 0
    							DL
    								SQN
    									Format = PdcpCount_DrbLongSQN (1)
    									Value = 0

    Sent from port: EUTRA_5GS_PTC:SYS

    SYSTEM_CTRL_CNF
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		AS_Security = True

    Received on port: EUTRA_5GS_PTC:SYS

    SRB_COMMON_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						securityModeCommand
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								c1
    									securityModeCommand_r8
    										securityConfigSMC
    											securityAlgorithmConfig
    												cipheringAlgorithm = eea1 (1)
    												integrityProtAlgorithm = eia1 (1)
    										nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: TC_SRB -> NASEMU_EUTRA_PTC:TC_SRB

    DL-DCCH-Message
    	message = c1 = securityModeCommand =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = c1 = securityModeCommand-r8 =
    			securityConfigSMC
    				securityAlgorithmConfig
    					cipheringAlgorithm = eea1
    					integrityProtAlgorithm = eia1

    securityModeCommand

    RRC_PDU_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				c1
    					securityModeCommand
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							c1
    								securityModeCommand_r8
    									securityConfigSMC
    										securityAlgorithmConfig
    											cipheringAlgorithm = eea1 (1)
    											integrityProtAlgorithm = eia1 (1)
    									nonCriticalExtension = Omit

    Sent from port: NASEMU_EUTRA_PTC:SYS_SRB

    UL-DCCH-Message
    	message = c1 = securityModeComplete =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = securityModeComplete-r8 =

    securityModeComplete

    RRC_PDU_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 168
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				c1
    					securityModeComplete
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							securityModeComplete_r8
    								nonCriticalExtension = Omit

    Received on port: NASEMU_EUTRA_PTC:SYS_SRB

    SRB_COMMON_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 168
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						securityModeComplete
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								securityModeComplete_r8
    									nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: SRB -> EUTRA_5GS_PTC:SRB

    SRB_COMMON_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcConnectionReconfiguration
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								c1
    									rrcConnectionReconfiguration_r8
    										measConfig = Omit
    										mobilityControlInfo = Omit
    										dedicatedInfoNASList = Omit
    										radioResourceConfigDedicated
    											srb_ToAddModList
    												SRB_ToAddMod
    													srb_Identity = 2
    													rlc_Config
    														defaultValue = Null
    													logicalChannelConfig
    														defaultValue = Null
    													pdcp_verChange_r15 = Omit
    													rlc_Config_v1530 = Omit
    													rlc_BearerConfigDupl_r15 = Omit
    													srb_Identity_v1530 = Omit
    											drb_ToAddModList
    												DRB_ToAddMod
    													eps_BearerIdentity = 12
    													drb_Identity = 8
    													pdcp_Config
    														discardTimer = infinity_ (7)
    														rlc_AM
    															statusReportRequired = True
    														rlc_UM = Omit
    														headerCompression
    															notUsed = Null
    														rn_IntegrityProtection_r10 = Omit
    														pdcp_SN_Size_v1130 = Omit
    														ul_DataSplitDRB_ViaSCG_r12 = Omit
    														t_Reordering_r12 = Omit
    														ul_DataSplitThreshold_r13 = Omit
    														pdcp_SN_Size_v1310 = Omit
    														statusFeedback_r13 = Omit
    														ul_LWA_Config_r14 = Omit
    														uplinkOnlyHeaderCompression_r14 = Omit
    														uplinkDataCompression_r15 = Omit
    														pdcp_DuplicationConfig_r15 = Omit
    													rlc_Config
    														am
    															ul_AM_RLC
    																t_PollRetransmit = ms80 (15)
    																pollPDU = p128 (5)
    																pollByte = kB125 (4)
    																maxRetxThreshold = t4 (3)
    															dl_AM_RLC
    																t_Reordering = ms80 (16)
    																t_StatusProhibit = ms60 (12)
    													logicalChannelIdentity = 10
    													logicalChannelConfig
    														ul_SpecificParameters
    															priority = 6
    															prioritisedBitRate = kBps0 (0)
    															bucketSizeDuration = ms100 (1)
    															logicalChannelGroup = 1
    														logicalChannelSR_Mask_r9 = Omit
    														logicalChannelSR_Prohibit_r12 = Omit
    														laa_UL_Allowed_r14 = Omit
    														bitRateQueryProhibitTimer_r14 = Omit
    														allowedTTI_Lengths_r15 = Omit
    														logicalChannelSR_Restriction_r15 = Omit
    														channellAccessPriority_r15 = Omit
    														lch_CellRestriction_r15 = Omit
    													drb_TypeChange_r12 = Omit
    													rlc_Config_v1250 = Omit
    													rlc_Config_v1310 = Omit
    													drb_TypeLWA_r13 = Omit
    													drb_TypeLWIP_r13 = Omit
    													rlc_Config_v1430 = Omit
    													lwip_UL_Aggregation_r14 = Omit
    													lwip_DL_Aggregation_r14 = Omit
    													lwa_WLAN_AC_r14 = Omit
    													rlc_Config_v1510 = Omit
    													rlc_Config_v1530 = Omit
    													rlc_BearerConfigDupl_r15 = Omit
    													logicalChannelIdentity_r15 = Omit
    											drb_ToReleaseList = Omit
    											mac_MainConfig
    												explicitValue
    													ul_SCH_Config
    														maxHARQ_Tx = n5 (4)
    														periodicBSR_Timer = sf20 (3)
    														retxBSR_Timer = sf320 (0)
    														ttiBundling = False
    													drx_Config
    														setup
    															onDurationTimer = psf6 (5)
    															drx_InactivityTimer = psf1920 (20)
    															drx_RetransmissionTimer = psf16 (5)
    															longDRX_CycleStartOffset
    																sf1280 = 4
    															shortDRX = Omit
    													timeAlignmentTimerDedicated = sf750 (1)
    													phr_Config
    														setup
    															periodicPHR_Timer = sf500 (5)
    															prohibitPHR_Timer = sf200 (5)
    															dl_PathlossChange = dB3 (1)
    													sr_ProhibitTimer_r9 = Omit
    													mac_MainConfig_v1020 = Omit
    													stag_ToReleaseList_r11 = Omit
    													stag_ToAddModList_r11 = Omit
    													drx_Config_v1130 = Omit
    													e_HARQ_Pattern_r12 = Omit
    													dualConnectivityPHR = Omit
    													logicalChannelSR_Config_r12 = Omit
    													drx_Config_v1310 = Omit
    													extendedPHR2_r13 = Omit
    													eDRX_Config_CycleStartOffset_r13 = Omit
    													drx_Config_r13 = Omit
    													skipUplinkTx_r14 = Omit
    													dataInactivityTimerConfig_r14 = Omit
    													rai_Activation_r14 = Omit
    													shortTTI_AndSPT_r15 = Omit
    													mpdcch_UL_HARQ_ACK_FeedbackConfig_r15 = Omit
    													dormantStateTimers_r15 = Omit
    											sps_Config = Omit
    											physicalConfigDedicated
    												pdsch_ConfigDedicated = Omit
    												pucch_ConfigDedicated = Omit
    												pusch_ConfigDedicated = Omit
    												uplinkPowerControlDedicated = Omit
    												tpc_PDCCH_ConfigPUCCH
    													setup
    														tpc_RNTI = 0000001111111111'B
    														tpc_Index
    															indexOfFormat3 = 1
    												tpc_PDCCH_ConfigPUSCH
    													setup
    														tpc_RNTI = 0000000111111010'B
    														tpc_Index
    															indexOfFormat3 = 1
    												cqi_ReportConfig
    													cqi_ReportModeAperiodic = rm30 (3)
    													nomPDSCH_RS_EPRE_Offset = 0
    													cqi_ReportPeriodic
    														setup
    															cqi_PUCCH_ResourceIndex = 0
    															cqi_pmi_ConfigIndex = 25
    															cqi_FormatIndicatorPeriodic
    																widebandCQI = Null
    															ri_ConfigIndex = 483
    															simultaneousAckNackAndCQI = False
    												soundingRS_UL_ConfigDedicated
    													setup
    														srs_Bandwidth = bw0 (0)
    														srs_HoppingBandwidth = hbw0 (0)
    														freqDomainPosition = 0
    														duration = True
    														srs_ConfigIndex = 20
    														transmissionComb = 0
    														cyclicShift = cs0 (0)
    												antennaInfo
    													defaultValue = Null
    												schedulingRequestConfig = Omit
    												cqi_ReportConfig_v920 = Omit
    												antennaInfo_v920 = Omit
    												antennaInfo_r10 = Omit
    												antennaInfoUL_r10 = Omit
    												cif_Presence_r10 = Omit
    												cqi_ReportConfig_r10 = Omit
    												csi_RS_Config_r10 = Omit
    												pucch_ConfigDedicated_v1020 = Omit
    												pusch_ConfigDedicated_v1020 = Omit
    												schedulingRequestConfig_v1020 = Omit
    												soundingRS_UL_ConfigDedicated_v1020 = Omit
    												soundingRS_UL_ConfigDedicatedAperiodic_r10 = Omit
    												uplinkPowerControlDedicated_v1020 = Omit
    												additionalSpectrumEmissionCA_r10 = Omit
    												csi_RS_ConfigNZPToReleaseList_r11 = Omit
    												csi_RS_ConfigNZPToAddModList_r11 = Omit
    												csi_RS_ConfigZPToReleaseList_r11 = Omit
    												csi_RS_ConfigZPToAddModList_r11 = Omit
    												epdcch_Config_r11 = Omit
    												pdsch_ConfigDedicated_v1130 = Omit
    												cqi_ReportConfig_v1130 = Omit
    												pucch_ConfigDedicated_v1130 = Omit
    												pusch_ConfigDedicated_v1130 = Omit
    												uplinkPowerControlDedicated_v1130 = Omit
    												antennaInfo_v1250 = Omit
    												eimta_MainConfig_r12 = Omit
    												eimta_MainConfigPCell_r12 = Omit
    												pucch_ConfigDedicated_v1250 = Omit
    												cqi_ReportConfigPCell_v1250 = Omit
    												uplinkPowerControlDedicated_v1250 = Omit
    												pusch_ConfigDedicated_v1250 = Omit
    												csi_RS_Config_v1250 = Omit
    												pdsch_ConfigDedicated_v1280 = Omit
    												pdsch_ConfigDedicated_v1310 = Omit
    												pucch_ConfigDedicated_r13 = Omit
    												pusch_ConfigDedicated_r13 = Omit
    												pdcch_CandidateReductions_r13 = Omit
    												cqi_ReportConfig_v1310 = Omit
    												soundingRS_UL_ConfigDedicated_v1310 = Omit
    												soundingRS_UL_ConfigDedicatedUpPTsExt_r13 = Omit
    												soundingRS_UL_ConfigDedicatedAperiodic_v1310 = Omit
    												soundingRS_UL_ConfigDedicatedAperiodicUpPTsExt_r13 = Omit
    												csi_RS_Config_v1310 = Omit
    												ce_Mode_r13 = Omit
    												csi_RS_ConfigNZPToAddModListExt_r13 = Omit
    												csi_RS_ConfigNZPToReleaseListExt_r13 = Omit
    												cqi_ReportConfig_v1320 = Omit
    												typeA_SRS_TPC_PDCCH_Group_r14 = Omit
    												must_Config_r14 = Omit
    												pusch_EnhancementsConfig_r14 = Omit
    												ce_pdsch_pusch_EnhancementConfig_r14 = Omit
    												antennaInfo_v1430 = Omit
    												pucch_ConfigDedicated_v1430 = Omit
    												pdsch_ConfigDedicated_v1430 = Omit
    												pusch_ConfigDedicated_v1430 = Omit
    												soundingRS_UL_PeriodicConfigDedicatedList_r14 = Omit
    												soundingRS_UL_PeriodicConfigDedicatedUpPTsExtList_r14 = Omit
    												soundingRS_UL_AperiodicConfigDedicatedList_r14 = Omit
    												soundingRS_UL_ConfigDedicatedApUpPTsExtList_r14 = Omit
    												csi_RS_Config_v1430 = Omit
    												csi_RS_ConfigZP_ApList_r14 = Omit
    												cqi_ReportConfig_v1430 = Omit
    												semiOpenLoop_r14 = Omit
    												csi_RS_Config_v1480 = Omit
    												physicalConfigDedicatedSTTI_r15 = Omit
    												pdsch_ConfigDedicated_v1530 = Omit
    												pusch_ConfigDedicated_v1530 = Omit
    												cqi_ReportConfig_v1530 = Omit
    												antennaInfo_v1530 = Omit
    												csi_RS_Config_v1530 = Omit
    												uplinkPowerControlDedicated_v1530 = Omit
    												semiStaticCFI_Config_r15 = Omit
    												blindPDSCH_Repetition_Config_r15 = Omit
    											rlf_TimersAndConstants_r9 = Omit
    											measSubframePatternPCell_r10 = Omit
    											neighCellsCRS_Info_r11 = Omit
    											naics_Info_r12 = Omit
    											neighCellsCRS_Info_r13 = Omit
    											rlf_TimersAndConstants_r13 = Omit
    											sps_Config_v1430 = Omit
    											srb_ToAddModExtList_r15 = Omit
    											srb_ToReleaseExtList_r15 = Omit
    											sps_Config_v1530 = Omit
    											crs_IntfMitigConfig_r15 = Omit
    											neighCellsCRS_Info_r15 = Omit
    											drb_ToAddModList_r15 = Omit
    											drb_ToReleaseList_r15 = Omit
    											dummy = Omit
    											sps_Config_v1540 = Omit
    										securityConfigHO = Omit
    										nonCriticalExtension
    											lateNonCriticalExtension = Omit
    											nonCriticalExtension
    												otherConfig_r9 = Omit
    												fullConfig_r9 = Omit
    												nonCriticalExtension
    													sCellToReleaseList_r10 = Omit
    													sCellToAddModList_r10 = Omit
    													nonCriticalExtension
    														systemInformationBlockType1Dedicated_r11 = Omit
    														nonCriticalExtension
    															wlan_OffloadInfo_r12 = Omit
    															scg_Configuration_r12 = Omit
    															sl_SyncTxControl_r12 = Omit
    															sl_DiscConfig_r12 = Omit
    															sl_CommConfig_r12 = Omit
    															nonCriticalExtension
    																sCellToReleaseListExt_r13 = Omit
    																sCellToAddModListExt_r13 = Omit
    																lwa_Configuration_r13 = Omit
    																lwip_Configuration_r13 = Omit
    																rclwi_Configuration_r13 = Omit
    																nonCriticalExtension
    																	sl_V2X_ConfigDedicated_r14 = Omit
    																	sCellToAddModListExt_v1430 = Omit
    																	perCC_GapIndicationRequest_r14 = Omit
    																	systemInformationBlockType2Dedicated_r14 = Omit
    																	nonCriticalExtension
    																		nr_Config_r15
    																			setup
    																				endc_ReleaseAndAdd_r15 = False
    																				nr_SecondaryCellGroupConfig_r15 = ' 'O
    																				p_MaxEUTRA_r15 = 20
    																		sk_Counter_r15 = 0
    																		nr_RadioBearerConfig1_r15 = '14093053AFC34460'O
    																		nr_RadioBearerConfig2_r15 = Omit
    																		tdm_PatternConfig_r15 = Omit
    																		nonCriticalExtension = Omit
    		Nas
    			NAS_MSG_Request_Type
    				SecurityProtection
    					Status = 0010'B
    					ForceMacError = False
    				Pdu
    					Msg
    						aCTIVATE_DEDICATED_EPS_BEARER_CONTEXT_REQUEST
    							epsBearerId = '6'H
    							protocolDiscriminator = 0010'B
    							procedureTransactionIdentifier = '00'O
    							messageType = 11000101'B
    							spareHalfOctet = '0'H
    							linkedEpsBearerId
    								idValue = 1100'B
    							epsQos
    								iei = Omit
    								iel = '09'O
    								qci = 00001000'B
    								maxBitRateUl = 01101000'B
    								maxBitRateDl = 01101000'B
    								guaranteedBitRateUl = 01001000'B
    								guaranteedBitRateDl = 01001000'B
    								maxBitRateUlExt = 00000000'B
    								maxBitRateDlExt = 00000000'B
    								guaranteedBitRateUlExt = 00000000'B
    								guaranteedBitRateDlExt = 00000000'B
    								maxBitRateUL_Ext2 = Omit
    								maxBitRateDL_Ext2 = Omit
    								guaranteedBitRateUL_Ext2 = Omit
    								guaranteedBitRateDL_Ext2 = Omit
    							tft
    								iei = Omit
    								iel = '4D'O
    								tftOperationCode = 001'B
    								eBit = 0'B
    								noOfPktFilter = 0010'B
    								packetFilterList
    									PacketFilter
    										spare = 00'B
    										direction = 01'B
    										iei = '0'H
    										precedence = 00000000'B
    										iel = '23'O
    										contents
    											PacketFilterComponent
    												id = '20'O
    												packetFilterComponentValue
    													ipv6RemoteAddress = 'FD29CC437FB90002020C29FFFE66B4C7FFFFFFFFFFFFFFFFFFFFFFFFFFFFFFFF'O
    											PacketFilterComponent
    												id = '30'O
    												packetFilterComponentValue
    													protocolIdNextHeader = '3A'O
    									PacketFilter
    										spare = 00'B
    										direction = 10'B
    										iei = '1'H
    										precedence = 00001000'B
    										iel = '23'O
    										contents
    											PacketFilterComponent
    												id = '20'O
    												packetFilterComponentValue
    													ipv6RemoteAddress = 'FD29CC437FB90002020C29FFFE66B4C7FFFFFFFFFFFFFFFFFFFFFFFFFFFFFFFF'O
    											PacketFilterComponent
    												id = '30'O
    												packetFilterComponentValue
    													protocolIdNextHeader = '3A'O
    								parameterList = Omit
    							transactionIdentifier = Omit
    							negotiatedQos = Omit
    							negotiatedLlcSapi = Omit
    							radioPriority = Omit
    							packetFlowIdentifier = Omit
    							protocolConfigurationOptions = Omit
    							wlanOffloadInd = Omit
    							nbifomContainer = Omit
    							extdProtocolConfigurationOptions = Omit
    							extd_EPS_QOS = Omit
    					PiggybackedPduList = Omit

    Inter-component message: TC_SRB -> NASEMU_EUTRA_PTC:TC_SRB

    Activate Dedicated EPS Bearer Context Request
    	Decode Error = Error: Inconsistent information element length
    Field: Activate Dedicated EPS Bearer Context Request.Negotiated QoS
    Activate Dedicated EPS Bearer Context Request.Negotiated QoS.iel

    RecordData

    Activate Dedicated EPS Bearer Context Request PDU

    Ciphered NAS Message
    	0x2473A13B18720EA5D1681439B03AEFF71C8687BF40E7EB47765D557D986CFC2A67E369376A2F42454FAE993E59958CC2E66C218D3831337EB42959F0DC197E94B783508084B25FA84A67FF6459161E586133F462B3D109DDE4CD23B2

    Ciphered NAS Message DL PDU

    Security Protected NAS Message
    	Security header type [4 bits] = 0x2 [ 2 ]
    	Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    	MAC = 0x4806C07B [ 1208402043 ]
    	Sequence Number = 0x03 [ 3 ]
    	NAS message = 0x2473A13B18720EA5D1681439B03AEFF71C8687BF40E7EB47765D557D986CFC2A67E369376A2F42454FAE993E59958CC2E66C218D3831337EB42959F0DC197E94B783508084B25FA84A67FF6459161E586133F462B3D109DDE4CD23B2

    Security Protected NAS Message DL PDU

    RRCReconfiguration
    	rrc-TransactionIdentifier = 0
    	criticalExtensions = rrcReconfiguration =
    		secondaryCellGroup = CONTAINING =
    			cellGroupId = 1
    			rlc-BearerToAddModList = SEQUENCE OF RLC-BearerConfig
    				RLC-BearerConfig(1)
    					logicalChannelIdentity = 5
    					servedRadioBearer = drb-Identity = 2
    					rlc-Config = am =
    						ul-AM-RLC
    							sn-FieldLength = size18
    							t-PollRetransmit = ms30
    							pollPDU = p32768
    							pollByte = kB750
    							maxRetxThreshold = t8
    						dl-AM-RLC
    							sn-FieldLength = size18
    							t-Reassembly = ms30
    							t-StatusProhibit = ms30
    					mac-LogicalChannelConfig
    						ul-SpecificParameters
    							priority = 1
    							prioritisedBitRate = infinity
    							bucketSizeDuration = ms50
    							logicalChannelGroup = 1
    							schedulingRequestID = 0
    							logicalChannelSR-Mask = FALSE
    							logicalChannelSR-DelayTimerApplied = FALSE
    			mac-CellGroupConfig
    				schedulingRequestConfig
    					schedulingRequestToAddModList = SEQUENCE OF SchedulingRequestToAddMod
    						SchedulingRequestToAddMod(1)
    							schedulingRequestId = 0
    							sr-TransMax = n16
    				bsr-Config
    					periodicBSR-Timer = sf1
    					retxBSR-Timer = sf80
    				tag-Config
    					tag-ToAddModList = SEQUENCE OF TAG
    						TAG(1)
    							tag-Id = 0
    							timeAlignmentTimer = infinity
    				phr-Config = setup =
    					phr-PeriodicTimer = sf10
    					phr-ProhibitTimer = sf0
    					phr-Tx-PowerFactorChange = dB1
    					multiplePHR = TRUE
    					dummy = FALSE
    					phr-Type2OtherCell = FALSE
    					phr-ModeOtherCG = real
    				skipUplinkTxDynamic = FALSE
    			physicalCellGroupConfig
    				p-NR-FR1 = 20
    				pdsch-HARQ-ACK-Codebook = dynamic
    			spCellConfig
    				servCellIndex = 1
    				reconfigurationWithSync
    					spCellConfigCommon
    						physCellId = 0
    						downlinkConfigCommon
    							frequencyInfoDL
    								absoluteFrequencySSB = 2229499
    								frequencyBandList = SEQUENCE OF FreqBandIndicatorNR
    									FreqBandIndicatorNR(1) = 260
    								absoluteFrequencyPointA = 2229237
    								scs-SpecificCarrierList = SEQUENCE OF SCS-SpecificCarrier
    									SCS-SpecificCarrier(1)
    										offsetToCarrier = 0
    										subcarrierSpacing = kHz120
    										carrierBandwidth = 66
    							initialDownlinkBWP
    								genericParameters
    									locationAndBandwidth = 17875
    									subcarrierSpacing = kHz120
    								pdcch-ConfigCommon = setup =
    									controlResourceSetZero = 0
    									commonControlResourceSet
    										controlResourceSetId = 1
    										frequencyDomainResources = 111100000000000000000000000000000000000000000
    										duration = 2
    										cce-REG-MappingType = nonInterleaved = NULL
    										precoderGranularity = sameAsREG-bundle
    									searchSpaceZero = 0
    									commonSearchSpaceList = SEQUENCE OF SearchSpace
    										SearchSpace(1)
    											searchSpaceId = 1
    											controlResourceSetId = 1
    											monitoringSlotPeriodicityAndOffset = sl1 = NULL
    											monitoringSymbolsWithinSlot = 10000000000000
    											nrofCandidates
    												aggregationLevel1 = n0
    												aggregationLevel2 = n4
    												aggregationLevel4 = n2
    												aggregationLevel8 = n1
    												aggregationLevel16 = n0
    											searchSpaceType = common =
    												dci-Format0-0-AndFormat1-0
    									ra-SearchSpace = 1
    								pdsch-ConfigCommon = setup =
    									pdsch-TimeDomainAllocationList = SEQUENCE OF PDSCH-TimeDomainResourceAllocation
    										PDSCH-TimeDomainResourceAllocation(1)
    											mappingType = typeA
    											startSymbolAndLength = 53
    						uplinkConfigCommon
    							frequencyInfoUL
    								scs-SpecificCarrierList = SEQUENCE OF SCS-SpecificCarrier
    									SCS-SpecificCarrier(1)
    										offsetToCarrier = 0
    										subcarrierSpacing = kHz120
    										carrierBandwidth = 66
    								additionalSpectrumEmission = 0
    								p-Max = 20
    							initialUplinkBWP
    								genericParameters
    									locationAndBandwidth = 17875
    									subcarrierSpacing = kHz120
    								rach-ConfigCommon = setup =
    									rach-ConfigGeneric
    										prach-ConfigurationIndex = 149
    										msg1-FDM = one
    										msg1-FrequencyStart = 0
    										zeroCorrelationZoneConfig = 15
    										preambleReceivedTargetPower = -118
    										preambleTransMax = n7
    										powerRampingStep = dB4
    										ra-ResponseWindow = sl20
    									ssb-perRACH-OccasionAndCB-PreamblesPerSSB = one = n4
    									ra-ContentionResolutionTimer = sf64
    									rsrp-ThresholdSSB = 0
    									prach-RootSequenceIndex = l139 = 0
    									msg1-SubcarrierSpacing = kHz120
    									restrictedSetConfig = unrestrictedSet
    								pusch-ConfigCommon = setup =
    									pusch-TimeDomainAllocationList = SEQUENCE OF PUSCH-TimeDomainResourceAllocation
    										PUSCH-TimeDomainResourceAllocation(1)
    											k2 = 4
    											mappingType = typeA
    											startSymbolAndLength = 27
    										PUSCH-TimeDomainResourceAllocation(2)
    											k2 = 3
    											mappingType = typeA
    											startSymbolAndLength = 27
    									msg3-DeltaPreamble = 1
    									p0-NominalWithGrant = -90
    								pucch-ConfigCommon = setup =
    									pucch-ResourceCommon = 0
    									pucch-GroupHopping = enable
    									p0-nominal = -90
    							dummy = infinity
    						ssb-PositionsInBurst = longBitmap = 0100000000000000000000000000000000000000000000000000000000000000
    						ssb-periodicityServingCell = ms20
    						dmrs-TypeA-Position = pos2
    						subcarrierSpacing = kHz120
    						tdd-UL-DL-ConfigurationCommon
    							referenceSubcarrierSpacing = kHz120
    							pattern1
    								dl-UL-TransmissionPeriodicity = ms0p625
    								nrofDownlinkSlots = 3
    								nrofDownlinkSymbols = 10
    								nrofUplinkSlots = 1
    								nrofUplinkSymbols = 2
    						ss-PBCH-BlockPower = 0
    					newUE-Identity = 4097
    					t304 = ms1000
    				rlf-TimersAndConstants = setup =
    					t310 = ms1000
    					n310 = n1
    					n311 = n1
    				spCellConfigDedicated
    					initialDownlinkBWP
    						pdcch-Config = setup =
    							searchSpacesToAddModList = SEQUENCE OF SearchSpace
    								SearchSpace(1)
    									searchSpaceId = 2
    									controlResourceSetId = 1
    									monitoringSlotPeriodicityAndOffset = sl1 = NULL
    									monitoringSymbolsWithinSlot = 10000000000000
    									nrofCandidates
    										aggregationLevel1 = n0
    										aggregationLevel2 = n4
    										aggregationLevel4 = n2
    										aggregationLevel8 = n1
    										aggregationLevel16 = n0
    									searchSpaceType = ue-Specific =
    										dci-Formats = formats0-0-And-1-0
    						pdsch-Config = setup =
    							dataScramblingIdentityPDSCH = 0
    							dmrs-DownlinkForPDSCH-MappingTypeA = setup =
    								dmrs-AdditionalPosition = pos0
    								phaseTrackingRS = setup =
    									epre-Ratio = 0
    							tci-StatesToAddModList = SEQUENCE OF TCI-State
    								TCI-State(1)
    									tci-StateId = 0
    									qcl-Type1
    										referenceSignal = ssb = 1
    										qcl-Type = typeD
    							resourceAllocation = resourceAllocationType1
    							rbg-Size = config1
    							prb-BundlingType = staticBundling =
    								bundleSize = wideband
    					firstActiveDownlinkBWP-Id = 0
    					defaultDownlinkBWP-Id = 0
    					uplinkConfig
    						initialUplinkBWP
    							pucch-Config = setup =
    								resourceSetToAddModList = SEQUENCE OF PUCCH-ResourceSet
    									PUCCH-ResourceSet(1)
    										pucch-ResourceSetId = 0
    										resourceList = SEQUENCE OF PUCCH-ResourceId
    											PUCCH-ResourceId(1) = 0
    											PUCCH-ResourceId(2) = 1
    											PUCCH-ResourceId(3) = 2
    											PUCCH-ResourceId(4) = 3
    											PUCCH-ResourceId(5) = 4
    											PUCCH-ResourceId(6) = 5
    											PUCCH-ResourceId(7) = 6
    											PUCCH-ResourceId(8) = 7
    									PUCCH-ResourceSet(2)
    										pucch-ResourceSetId = 1
    										resourceList = SEQUENCE OF PUCCH-ResourceId
    											PUCCH-ResourceId(1) = 8
    											PUCCH-ResourceId(2) = 9
    											PUCCH-ResourceId(3) = 10
    											PUCCH-ResourceId(4) = 11
    											PUCCH-ResourceId(5) = 12
    											PUCCH-ResourceId(6) = 13
    											PUCCH-ResourceId(7) = 14
    											PUCCH-ResourceId(8) = 15
    										maxPayloadMinus1 = 256
    									PUCCH-ResourceSet(3)
    										pucch-ResourceSetId = 2
    										resourceList = SEQUENCE OF PUCCH-ResourceId
    											PUCCH-ResourceId(1) = 8
    											PUCCH-ResourceId(2) = 9
    											PUCCH-ResourceId(3) = 10
    											PUCCH-ResourceId(4) = 11
    											PUCCH-ResourceId(5) = 12
    											PUCCH-ResourceId(6) = 13
    											PUCCH-ResourceId(7) = 14
    											PUCCH-ResourceId(8) = 15
    										maxPayloadMinus1 = 256
    									PUCCH-ResourceSet(4)
    										pucch-ResourceSetId = 3
    										resourceList = SEQUENCE OF PUCCH-ResourceId
    											PUCCH-ResourceId(1) = 8
    											PUCCH-ResourceId(2) = 9
    											PUCCH-ResourceId(3) = 10
    											PUCCH-ResourceId(4) = 11
    											PUCCH-ResourceId(5) = 12
    											PUCCH-ResourceId(6) = 13
    											PUCCH-ResourceId(7) = 14
    											PUCCH-ResourceId(8) = 15
    								resourceToAddModList = SEQUENCE OF PUCCH-Resource
    									PUCCH-Resource(1)
    										pucch-ResourceId = 0
    										startingPRB = 0
    										intraSlotFrequencyHopping = enabled
    										secondHopPRB = 0
    										format = format0 =
    											initialCyclicShift = 0
    											nrofSymbols = 2
    											startingSymbolIndex = 0
    									PUCCH-Resource(2)
    										pucch-ResourceId = 1
    										startingPRB = 0
    										intraSlotFrequencyHopping = enabled
    										secondHopPRB = 0
    										format = format0 =
    											initialCyclicShift = 0
    											nrofSymbols = 2
    											startingSymbolIndex = 2
    									PUCCH-Resource(3)
    										pucch-ResourceId = 2
    										startingPRB = 0
    										intraSlotFrequencyHopping = enabled
    										secondHopPRB = 0
    										format = format0 =
    											initialCyclicShift = 0
    											nrofSymbols = 2
    											startingSymbolIndex = 4
    									PUCCH-Resource(4)
    										pucch-ResourceId = 3
    										startingPRB = 0
    										intraSlotFrequencyHopping = enabled
    										secondHopPRB = 0
    										format = format0 =
    											initialCyclicShift = 0
    											nrofSymbols = 2
    											startingSymbolIndex = 6
    									PUCCH-Resource(5)
    										pucch-ResourceId = 4
    										startingPRB = 0
    										intraSlotFrequencyHopping = enabled
    										secondHopPRB = 0
    										format = format0 =
    											initialCyclicShift = 0
    											nrofSymbols = 2
    											startingSymbolIndex = 8
    									PUCCH-Resource(6)
    										pucch-ResourceId = 5
    										startingPRB = 0
    										intraSlotFrequencyHopping = enabled
    										secondHopPRB = 0
    										format = format0 =
    											initialCyclicShift = 0
    											nrofSymbols = 2
    											startingSymbolIndex = 10
    									PUCCH-Resource(7)
    										pucch-ResourceId = 6
    										startingPRB = 0
    										intraSlotFrequencyHopping = enabled
    										secondHopPRB = 0
    										format = format0 =
    											initialCyclicShift = 0
    											nrofSymbols = 2
    											startingSymbolIndex = 12
    									PUCCH-Resource(8)
    										pucch-ResourceId = 7
    										startingPRB = 0
    										intraSlotFrequencyHopping = enabled
    										secondHopPRB = 0
    										format = format1 =
    											initialCyclicShift = 0
    											nrofSymbols = 14
    											startingSymbolIndex = 0
    											timeDomainOCC = 0
    									PUCCH-Resource(9)
    										pucch-ResourceId = 8
    										startingPRB = 0
    										intraSlotFrequencyHopping = enabled
    										secondHopPRB = 0
    										format = format2 =
    											nrofPRBs = 6
    											nrofSymbols = 2
    											startingSymbolIndex = 0
    									PUCCH-Resource(10)
    										pucch-ResourceId = 9
    										startingPRB = 0
    										intraSlotFrequencyHopping = enabled
    										secondHopPRB = 0
    										format = format2 =
    											nrofPRBs = 6
    											nrofSymbols = 2
    											startingSymbolIndex = 2
    									PUCCH-Resource(11)
    										pucch-ResourceId = 10
    										startingPRB = 0
    										intraSlotFrequencyHopping = enabled
    										secondHopPRB = 0
    										format = format2 =
    											nrofPRBs = 6
    											nrofSymbols = 2
    											startingSymbolIndex = 4
    									PUCCH-Resource(12)
    										pucch-ResourceId = 11
    										startingPRB = 0
    										intraSlotFrequencyHopping = enabled
    										secondHopPRB = 0
    										format = format2 =
    											nrofPRBs = 6
    											nrofSymbols = 2
    											startingSymbolIndex = 6
    									PUCCH-Resource(13)
    										pucch-ResourceId = 12
    										startingPRB = 0
    										intraSlotFrequencyHopping = enabled
    										secondHopPRB = 0
    										format = format2 =
    											nrofPRBs = 6
    											nrofSymbols = 2
    											startingSymbolIndex = 8
    									PUCCH-Resource(14)
    										pucch-ResourceId = 13
    										startingPRB = 0
    										intraSlotFrequencyHopping = enabled
    										secondHopPRB = 0
    										format = format2 =
    											nrofPRBs = 6
    											nrofSymbols = 2
    											startingSymbolIndex = 10
    									PUCCH-Resource(15)
    										pucch-ResourceId = 14
    										startingPRB = 0
    										intraSlotFrequencyHopping = enabled
    										secondHopPRB = 0
    										format = format2 =
    											nrofPRBs = 6
    											nrofSymbols = 2
    											startingSymbolIndex = 12
    									PUCCH-Resource(16)
    										pucch-ResourceId = 15
    										startingPRB = 0
    										intraSlotFrequencyHopping = enabled
    										secondHopPRB = 0
    										format = format3 =
    											nrofPRBs = 1
    											nrofSymbols = 14
    											startingSymbolIndex = 0
    								format1 = setup =
    									interslotFrequencyHopping = enabled
    									additionalDMRS = true
    									maxCodeRate = zeroDot25
    									simultaneousHARQ-ACK-CSI = true
    								format2 = setup =
    									interslotFrequencyHopping = enabled
    									additionalDMRS = true
    									maxCodeRate = zeroDot25
    									simultaneousHARQ-ACK-CSI = true
    								format3 = setup =
    									interslotFrequencyHopping = enabled
    									additionalDMRS = true
    									maxCodeRate = zeroDot25
    									simultaneousHARQ-ACK-CSI = true
    								schedulingRequestResourceToAddModList = SEQUENCE OF SchedulingRequestResourceConfig
    									SchedulingRequestResourceConfig(1)
    										schedulingRequestResourceId = 1
    										schedulingRequestID = 0
    										periodicityAndOffset = sl80 = 9
    										resource = 0
    								dl-DataToUL-ACK = SEQUENCE OF INTEGER
    									INTEGER(1) = 2
    									INTEGER(2) = 3
    									INTEGER(3) = 4
    									INTEGER(4) = 5
    									INTEGER(5) = 6
    									INTEGER(6) = 7
    									INTEGER(7) = 8
    									INTEGER(8) = 9
    								pucch-PowerControl
    									deltaF-PUCCH-f0 = 0
    									deltaF-PUCCH-f1 = 0
    									deltaF-PUCCH-f2 = 0
    									deltaF-PUCCH-f3 = 0
    									deltaF-PUCCH-f4 = 0
    									pathlossReferenceRSs = SEQUENCE OF PUCCH-PathlossReferenceRS
    										PUCCH-PathlossReferenceRS(1)
    											pucch-PathlossReferenceRS-Id = 0
    											referenceSignal = ssb-Index = 1
    							pusch-Config = setup =
    								dmrs-UplinkForPUSCH-MappingTypeA = setup =
    									dmrs-AdditionalPosition = pos0
    									transformPrecodingDisabled
    								pusch-PowerControl
    									msg3-Alpha = alpha08
    									p0-NominalWithoutGrant = -90
    									p0-AlphaSets = SEQUENCE OF P0-PUSCH-AlphaSet
    										P0-PUSCH-AlphaSet(1)
    											p0-PUSCH-AlphaSetId = 0
    											p0 = 0
    											alpha = alpha08
    									pathlossReferenceRSToAddModList = SEQUENCE OF PUSCH-PathlossReferenceRS
    										PUSCH-PathlossReferenceRS(1)
    											pusch-PathlossReferenceRS-Id = 0
    											referenceSignal = ssb-Index = 1
    									sri-PUSCH-MappingToAddModList = SEQUENCE OF SRI-PUSCH-PowerControl
    										SRI-PUSCH-PowerControl(1)
    											sri-PUSCH-PowerControlId = 0
    											sri-PUSCH-PathlossReferenceRS-Id = 0
    											sri-P0-PUSCH-AlphaSetId = 0
    											sri-PUSCH-ClosedLoopIndex = i0
    								resourceAllocation = resourceAllocationType1
    								uci-OnPUSCH = setup =
    									betaOffsets = semiStatic =
    										betaOffsetACK-Index1 = 9
    										betaOffsetACK-Index2 = 9
    										betaOffsetACK-Index3 = 9
    										betaOffsetCSI-Part1-Index1 = 6
    										betaOffsetCSI-Part1-Index2 = 6
    										betaOffsetCSI-Part2-Index1 = 6
    										betaOffsetCSI-Part2-Index2 = 6
    									scaling = f1
    						firstActiveUplinkBWP-Id = 0
    						pusch-ServingCellConfig = setup =
    					pdcch-ServingCellConfig = setup =
    					pdsch-ServingCellConfig = setup =
    						nrofHARQ-ProcessesForPDSCH = n16
    					tag-Id = 0

    RRCReconfiguration

    RadioBearerConfig
    	drb-ToAddModList = SEQUENCE OF DRB-ToAddMod
    		DRB-ToAddMod(1)
    			cnAssociation = eps-BearerIdentity = 6
    			drb-Identity = 2
    			pdcp-Config
    				drb
    					discardTimer = infinity
    					pdcp-SN-SizeUL = len18bits
    					pdcp-SN-SizeDL = len18bits
    					headerCompression = notUsed = NULL
    					statusReportRequired = true
    	securityConfig
    		securityAlgorithmConfig
    			cipheringAlgorithm = nea1
    			integrityProtAlgorithm = nia1
    		keyToUse = secondary

    RadioBearerConfig

    DL-DCCH-Message
    	message = c1 = rrcConnectionReconfiguration =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = c1 = rrcConnectionReconfiguration-r8 =
    			dedicatedInfoNASList = SEQUENCE OF DedicatedInfoNAS
    				DedicatedInfoNAS(1) = 274806C07B032473A13B18720EA5D1681439B03AEFF71C8687BF40E7EB47765D557D986CFC2A67E369376A2F42454FAE993E59958CC2E66C218D3831337EB42959F0DC197E94B783508084B25FA84A67FF6459161E586133F462B3D109DDE4CD23B2
    			radioResourceConfigDedicated
    				srb-ToAddModList = SEQUENCE OF SRB-ToAddMod
    					SRB-ToAddMod(1)
    						srb-Identity = 2
    						rlc-Config = defaultValue = NULL
    						logicalChannelConfig = defaultValue = NULL
    				drb-ToAddModList = SEQUENCE OF DRB-ToAddMod
    					DRB-ToAddMod(1)
    						eps-BearerIdentity = 12
    						drb-Identity = 8
    						pdcp-Config
    							discardTimer = infinity
    							rlc-AM
    								statusReportRequired = TRUE
    							headerCompression = notUsed = NULL
    						rlc-Config = am =
    							ul-AM-RLC
    								t-PollRetransmit = ms80
    								pollPDU = p128
    								pollByte = kB125
    								maxRetxThreshold = t4
    							dl-AM-RLC
    								t-Reordering = ms80
    								t-StatusProhibit = ms60
    						logicalChannelIdentity = 10
    						logicalChannelConfig
    							ul-SpecificParameters
    								priority = 6
    								prioritisedBitRate = kBps0
    								bucketSizeDuration = ms100
    								logicalChannelGroup = 1
    				mac-MainConfig = explicitValue =
    					ul-SCH-Config
    						maxHARQ-Tx = n5
    						periodicBSR-Timer = sf20
    						retxBSR-Timer = sf320
    						ttiBundling = FALSE
    					drx-Config = setup =
    						onDurationTimer = psf6
    						drx-InactivityTimer = psf1920
    						drx-RetransmissionTimer = psf16
    						longDRX-CycleStartOffset = sf1280 = 4
    					timeAlignmentTimerDedicated = sf750
    					phr-Config = setup =
    						periodicPHR-Timer = sf500
    						prohibitPHR-Timer = sf200
    						dl-PathlossChange = dB3
    				physicalConfigDedicated
    					tpc-PDCCH-ConfigPUCCH = setup =
    						tpc-RNTI = 0000001111111111
    						tpc-Index = indexOfFormat3 = 1
    					tpc-PDCCH-ConfigPUSCH = setup =
    						tpc-RNTI = 0000000111111010
    						tpc-Index = indexOfFormat3 = 1
    					cqi-ReportConfig
    						cqi-ReportModeAperiodic = rm30
    						nomPDSCH-RS-EPRE-Offset = 0
    						cqi-ReportPeriodic = setup =
    							cqi-PUCCH-ResourceIndex = 0
    							cqi-pmi-ConfigIndex = 25
    							cqi-FormatIndicatorPeriodic = widebandCQI = NULL
    							ri-ConfigIndex = 483
    							simultaneousAckNackAndCQI = FALSE
    					soundingRS-UL-ConfigDedicated = setup =
    						srs-Bandwidth = bw0
    						srs-HoppingBandwidth = hbw0
    						freqDomainPosition = 0
    						duration = TRUE
    						srs-ConfigIndex = 20
    						transmissionComb = 0
    						cyclicShift = cs0
    					antennaInfo = defaultValue = NULL
    			nonCriticalExtension
    				nonCriticalExtension
    					nonCriticalExtension
    						nonCriticalExtension
    							nonCriticalExtension
    								nonCriticalExtension
    									nonCriticalExtension
    										nonCriticalExtension
    											nr-Config-r15 = setup =
    												endc-ReleaseAndAdd-r15 = FALSE
    												nr-SecondaryCellGroupConfig-r15 =
    												p-MaxEUTRA-r15 = 20
    											sk-Counter-r15 = 0
    											nr-RadioBearerConfig1-r15 = 14093053AFC34460

    rrcConnectionReconfiguration

    RRC_PDU_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcConnectionReconfiguration
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							c1
    								rrcConnectionReconfiguration_r8
    									measConfig = Omit
    									mobilityControlInfo = Omit
    									dedicatedInfoNASList
    										NAS_Message = '274806C07B032473A13B18720EA5D1681439B03AEFF71C8687BF40E7EB47765D557D986CFC2A67E369376A2F42454FAE993E59958CC2E66C218D3831337EB42959F0DC197E94B783508084B25FA84A67FF6459161E586133F462B3D109DDE4CD23B2'O
    									radioResourceConfigDedicated
    										srb_ToAddModList
    											SRB_ToAddMod
    												srb_Identity = 2
    												rlc_Config
    													defaultValue = Null
    												logicalChannelConfig
    													defaultValue = Null
    												pdcp_verChange_r15 = Omit
    												rlc_Config_v1530 = Omit
    												rlc_BearerConfigDupl_r15 = Omit
    												srb_Identity_v1530 = Omit
    										drb_ToAddModList
    											DRB_ToAddMod
    												eps_BearerIdentity = 12
    												drb_Identity = 8
    												pdcp_Config
    													discardTimer = infinity_ (7)
    													rlc_AM
    														statusReportRequired = True
    													rlc_UM = Omit
    													headerCompression
    														notUsed = Null
    													rn_IntegrityProtection_r10 = Omit
    													pdcp_SN_Size_v1130 = Omit
    													ul_DataSplitDRB_ViaSCG_r12 = Omit
    													t_Reordering_r12 = Omit
    													ul_DataSplitThreshold_r13 = Omit
    													pdcp_SN_Size_v1310 = Omit
    													statusFeedback_r13 = Omit
    													ul_LWA_Config_r14 = Omit
    													uplinkOnlyHeaderCompression_r14 = Omit
    													uplinkDataCompression_r15 = Omit
    													pdcp_DuplicationConfig_r15 = Omit
    												rlc_Config
    													am
    														ul_AM_RLC
    															t_PollRetransmit = ms80 (15)
    															pollPDU = p128 (5)
    															pollByte = kB125 (4)
    															maxRetxThreshold = t4 (3)
    														dl_AM_RLC
    															t_Reordering = ms80 (16)
    															t_StatusProhibit = ms60 (12)
    												logicalChannelIdentity = 10
    												logicalChannelConfig
    													ul_SpecificParameters
    														priority = 6
    														prioritisedBitRate = kBps0 (0)
    														bucketSizeDuration = ms100 (1)
    														logicalChannelGroup = 1
    													logicalChannelSR_Mask_r9 = Omit
    													logicalChannelSR_Prohibit_r12 = Omit
    													laa_UL_Allowed_r14 = Omit
    													bitRateQueryProhibitTimer_r14 = Omit
    													allowedTTI_Lengths_r15 = Omit
    													logicalChannelSR_Restriction_r15 = Omit
    													channellAccessPriority_r15 = Omit
    													lch_CellRestriction_r15 = Omit
    												drb_TypeChange_r12 = Omit
    												rlc_Config_v1250 = Omit
    												rlc_Config_v1310 = Omit
    												drb_TypeLWA_r13 = Omit
    												drb_TypeLWIP_r13 = Omit
    												rlc_Config_v1430 = Omit
    												lwip_UL_Aggregation_r14 = Omit
    												lwip_DL_Aggregation_r14 = Omit
    												lwa_WLAN_AC_r14 = Omit
    												rlc_Config_v1510 = Omit
    												rlc_Config_v1530 = Omit
    												rlc_BearerConfigDupl_r15 = Omit
    												logicalChannelIdentity_r15 = Omit
    										drb_ToReleaseList = Omit
    										mac_MainConfig
    											explicitValue
    												ul_SCH_Config
    													maxHARQ_Tx = n5 (4)
    													periodicBSR_Timer = sf20 (3)
    													retxBSR_Timer = sf320 (0)
    													ttiBundling = False
    												drx_Config
    													setup
    														onDurationTimer = psf6 (5)
    														drx_InactivityTimer = psf1920 (20)
    														drx_RetransmissionTimer = psf16 (5)
    														longDRX_CycleStartOffset
    															sf1280 = 4
    														shortDRX = Omit
    												timeAlignmentTimerDedicated = sf750 (1)
    												phr_Config
    													setup
    														periodicPHR_Timer = sf500 (5)
    														prohibitPHR_Timer = sf200 (5)
    														dl_PathlossChange = dB3 (1)
    												sr_ProhibitTimer_r9 = Omit
    												mac_MainConfig_v1020 = Omit
    												stag_ToReleaseList_r11 = Omit
    												stag_ToAddModList_r11 = Omit
    												drx_Config_v1130 = Omit
    												e_HARQ_Pattern_r12 = Omit
    												dualConnectivityPHR = Omit
    												logicalChannelSR_Config_r12 = Omit
    												drx_Config_v1310 = Omit
    												extendedPHR2_r13 = Omit
    												eDRX_Config_CycleStartOffset_r13 = Omit
    												drx_Config_r13 = Omit
    												skipUplinkTx_r14 = Omit
    												dataInactivityTimerConfig_r14 = Omit
    												rai_Activation_r14 = Omit
    												shortTTI_AndSPT_r15 = Omit
    												mpdcch_UL_HARQ_ACK_FeedbackConfig_r15 = Omit
    												dormantStateTimers_r15 = Omit
    										sps_Config = Omit
    										physicalConfigDedicated
    											pdsch_ConfigDedicated = Omit
    											pucch_ConfigDedicated = Omit
    											pusch_ConfigDedicated = Omit
    											uplinkPowerControlDedicated = Omit
    											tpc_PDCCH_ConfigPUCCH
    												setup
    													tpc_RNTI = 0000001111111111'B
    													tpc_Index
    														indexOfFormat3 = 1
    											tpc_PDCCH_ConfigPUSCH
    												setup
    													tpc_RNTI = 0000000111111010'B
    													tpc_Index
    														indexOfFormat3 = 1
    											cqi_ReportConfig
    												cqi_ReportModeAperiodic = rm30 (3)
    												nomPDSCH_RS_EPRE_Offset = 0
    												cqi_ReportPeriodic
    													setup
    														cqi_PUCCH_ResourceIndex = 0
    														cqi_pmi_ConfigIndex = 25
    														cqi_FormatIndicatorPeriodic
    															widebandCQI = Null
    														ri_ConfigIndex = 483
    														simultaneousAckNackAndCQI = False
    											soundingRS_UL_ConfigDedicated
    												setup
    													srs_Bandwidth = bw0 (0)
    													srs_HoppingBandwidth = hbw0 (0)
    													freqDomainPosition = 0
    													duration = True
    													srs_ConfigIndex = 20
    													transmissionComb = 0
    													cyclicShift = cs0 (0)
    											antennaInfo
    												defaultValue = Null
    											schedulingRequestConfig = Omit
    											cqi_ReportConfig_v920 = Omit
    											antennaInfo_v920 = Omit
    											antennaInfo_r10 = Omit
    											antennaInfoUL_r10 = Omit
    											cif_Presence_r10 = Omit
    											cqi_ReportConfig_r10 = Omit
    											csi_RS_Config_r10 = Omit
    											pucch_ConfigDedicated_v1020 = Omit
    											pusch_ConfigDedicated_v1020 = Omit
    											schedulingRequestConfig_v1020 = Omit
    											soundingRS_UL_ConfigDedicated_v1020 = Omit
    											soundingRS_UL_ConfigDedicatedAperiodic_r10 = Omit
    											uplinkPowerControlDedicated_v1020 = Omit
    											additionalSpectrumEmissionCA_r10 = Omit
    											csi_RS_ConfigNZPToReleaseList_r11 = Omit
    											csi_RS_ConfigNZPToAddModList_r11 = Omit
    											csi_RS_ConfigZPToReleaseList_r11 = Omit
    											csi_RS_ConfigZPToAddModList_r11 = Omit
    											epdcch_Config_r11 = Omit
    											pdsch_ConfigDedicated_v1130 = Omit
    											cqi_ReportConfig_v1130 = Omit
    											pucch_ConfigDedicated_v1130 = Omit
    											pusch_ConfigDedicated_v1130 = Omit
    											uplinkPowerControlDedicated_v1130 = Omit
    											antennaInfo_v1250 = Omit
    											eimta_MainConfig_r12 = Omit
    											eimta_MainConfigPCell_r12 = Omit
    											pucch_ConfigDedicated_v1250 = Omit
    											cqi_ReportConfigPCell_v1250 = Omit
    											uplinkPowerControlDedicated_v1250 = Omit
    											pusch_ConfigDedicated_v1250 = Omit
    											csi_RS_Config_v1250 = Omit
    											pdsch_ConfigDedicated_v1280 = Omit
    											pdsch_ConfigDedicated_v1310 = Omit
    											pucch_ConfigDedicated_r13 = Omit
    											pusch_ConfigDedicated_r13 = Omit
    											pdcch_CandidateReductions_r13 = Omit
    											cqi_ReportConfig_v1310 = Omit
    											soundingRS_UL_ConfigDedicated_v1310 = Omit
    											soundingRS_UL_ConfigDedicatedUpPTsExt_r13 = Omit
    											soundingRS_UL_ConfigDedicatedAperiodic_v1310 = Omit
    											soundingRS_UL_ConfigDedicatedAperiodicUpPTsExt_r13 = Omit
    											csi_RS_Config_v1310 = Omit
    											ce_Mode_r13 = Omit
    											csi_RS_ConfigNZPToAddModListExt_r13 = Omit
    											csi_RS_ConfigNZPToReleaseListExt_r13 = Omit
    											cqi_ReportConfig_v1320 = Omit
    											typeA_SRS_TPC_PDCCH_Group_r14 = Omit
    											must_Config_r14 = Omit
    											pusch_EnhancementsConfig_r14 = Omit
    											ce_pdsch_pusch_EnhancementConfig_r14 = Omit
    											antennaInfo_v1430 = Omit
    											pucch_ConfigDedicated_v1430 = Omit
    											pdsch_ConfigDedicated_v1430 = Omit
    											pusch_ConfigDedicated_v1430 = Omit
    											soundingRS_UL_PeriodicConfigDedicatedList_r14 = Omit
    											soundingRS_UL_PeriodicConfigDedicatedUpPTsExtList_r14 = Omit
    											soundingRS_UL_AperiodicConfigDedicatedList_r14 = Omit
    											soundingRS_UL_ConfigDedicatedApUpPTsExtList_r14 = Omit
    											csi_RS_Config_v1430 = Omit
    											csi_RS_ConfigZP_ApList_r14 = Omit
    											cqi_ReportConfig_v1430 = Omit
    											semiOpenLoop_r14 = Omit
    											csi_RS_Config_v1480 = Omit
    											physicalConfigDedicatedSTTI_r15 = Omit
    											pdsch_ConfigDedicated_v1530 = Omit
    											pusch_ConfigDedicated_v1530 = Omit
    											cqi_ReportConfig_v1530 = Omit
    											antennaInfo_v1530 = Omit
    											csi_RS_Config_v1530 = Omit
    											uplinkPowerControlDedicated_v1530 = Omit
    											semiStaticCFI_Config_r15 = Omit
    											blindPDSCH_Repetition_Config_r15 = Omit
    										rlf_TimersAndConstants_r9 = Omit
    										measSubframePatternPCell_r10 = Omit
    										neighCellsCRS_Info_r11 = Omit
    										naics_Info_r12 = Omit
    										neighCellsCRS_Info_r13 = Omit
    										rlf_TimersAndConstants_r13 = Omit
    										sps_Config_v1430 = Omit
    										srb_ToAddModExtList_r15 = Omit
    										srb_ToReleaseExtList_r15 = Omit
    										sps_Config_v1530 = Omit
    										crs_IntfMitigConfig_r15 = Omit
    										neighCellsCRS_Info_r15 = Omit
    										drb_ToAddModList_r15 = Omit
    										drb_ToReleaseList_r15 = Omit
    										dummy = Omit
    										sps_Config_v1540 = Omit
    									securityConfigHO = Omit
    									nonCriticalExtension
    										lateNonCriticalExtension = Omit
    										nonCriticalExtension
    											otherConfig_r9 = Omit
    											fullConfig_r9 = Omit
    											nonCriticalExtension
    												sCellToReleaseList_r10 = Omit
    												sCellToAddModList_r10 = Omit
    												nonCriticalExtension
    													systemInformationBlockType1Dedicated_r11 = Omit
    													nonCriticalExtension
    														wlan_OffloadInfo_r12 = Omit
    														scg_Configuration_r12 = Omit
    														sl_SyncTxControl_r12 = Omit
    														sl_DiscConfig_r12 = Omit
    														sl_CommConfig_r12 = Omit
    														nonCriticalExtension
    															sCellToReleaseListExt_r13 = Omit
    															sCellToAddModListExt_r13 = Omit
    															lwa_Configuration_r13 = Omit
    															lwip_Configuration_r13 = Omit
    															rclwi_Configuration_r13 = Omit
    															nonCriticalExtension
    																sl_V2X_ConfigDedicated_r14 = Omit
    																sCellToAddModListExt_v1430 = Omit
    																perCC_GapIndicationRequest_r14 = Omit
    																systemInformationBlockType2Dedicated_r14 = Omit
    																nonCriticalExtension
    																	nr_Config_r15
    																		setup
    																			endc_ReleaseAndAdd_r15 = False
    																			nr_SecondaryCellGroupConfig_r15 = ' 'O
    																			p_MaxEUTRA_r15 = 20
    																	sk_Counter_r15 = 0
    																	nr_RadioBearerConfig1_r15 = '14093053AFC34460'O
    																	nr_RadioBearerConfig2_r15 = Omit
    																	tdm_PatternConfig_r15 = Omit
    																	nonCriticalExtension = Omit

    Sent from port: NASEMU_EUTRA_PTC:SYS_SRB

    UL-DCCH-Message
    	message = c1 = rrcConnectionReconfigurationComplete =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcConnectionReconfigurationComplete-r8 =
    			nonCriticalExtension
    				nonCriticalExtension
    					nonCriticalExtension
    						nonCriticalExtension
    							nonCriticalExtension
    								nonCriticalExtension
    									scg-ConfigResponseNR-r15 = 00

    rrcConnectionReconfigurationComplete

    UL-DCCH-Message
    	message = c1 = ulInformationTransfer =
    		criticalExtensions = c1 = ulInformationTransfer-r8 =
    			dedicatedInfoType = dedicatedInfoNAS = 27CCECB6B904682535

    ulInformationTransfer

    Security Protected NAS Message
    	Security header type [4 bits] = 0x2 [ 2 ]
    	Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    	MAC = 0x4C6C3639 [ 1282160185 ]
    	Sequence Number = 0x04 [ 4 ]
    	NAS message = 0x682535 [ 6825269 ]

    Security Protected NAS Message UL PDU

    Ciphered NAS Message
    	0x682535

    Ciphered NAS Message UL PDU

    RRC_PDU_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 182
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcConnectionReconfigurationComplete
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcConnectionReconfigurationComplete_r8
    								nonCriticalExtension
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension
    										rlf_InfoAvailable_r10 = Omit
    										logMeasAvailable_r10 = Omit
    										nonCriticalExtension
    											connEstFailInfoAvailable_r11 = Omit
    											nonCriticalExtension
    												logMeasAvailableMBSFN_r12 = Omit
    												nonCriticalExtension
    													perCC_GapIndicationList_r14 = Omit
    													numFreqEffective_r14 = Omit
    													numFreqEffectiveReduced_r14 = Omit
    													nonCriticalExtension
    														scg_ConfigResponseNR_r15 = '00'O
    														nonCriticalExtension = Omit

    Received on port: NASEMU_EUTRA_PTC:SYS_SRB

    SRB_COMMON_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 182
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcConnectionReconfigurationComplete
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcConnectionReconfigurationComplete_r8
    									nonCriticalExtension
    										lateNonCriticalExtension = Omit
    										nonCriticalExtension
    											rlf_InfoAvailable_r10 = Omit
    											logMeasAvailable_r10 = Omit
    											nonCriticalExtension
    												connEstFailInfoAvailable_r11 = Omit
    												nonCriticalExtension
    													logMeasAvailableMBSFN_r12 = Omit
    													nonCriticalExtension
    														perCC_GapIndicationList_r14 = Omit
    														numFreqEffective_r14 = Omit
    														numFreqEffectiveReduced_r14 = Omit
    														nonCriticalExtension
    															scg_ConfigResponseNR_r15 = '00'O
    															nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: SRB -> EUTRA_5GS_PTC:SRB

    RRC_PDU_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 2
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 182
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ulInformationTransfer
    						criticalExtensions
    							c1
    								ulInformationTransfer_r8
    									dedicatedInfoType
    										dedicatedInfoNAS = '27CCECB6B904682535'O
    									nonCriticalExtension = Omit

    Received on port: NASEMU_EUTRA_PTC:SYS_SRB

    Activate Dedicated EPS Bearer Context Accept
    	EPS bearer identity [4 bits] = 0x6 [ 6 ]
    	Protocol Discriminator [4 bits] = 0x2 - EPS Session Management Messages [ 2 ]
    	Procedure transaction identifier [8 bits] = 0x0 [ 0 ]
    	Message Type [8 bits] = 0xC6 - Activate Dedicated EPS Bearer Context Accept [ 198 ]

    Activate Dedicated EPS Bearer Context Accept PDU

    SRB_COMMON_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 2
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 182
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0010'B
    					NasCount = '00000004'O
    				Pdu
    					Msg
    						aCTIVATE_DEDICATED_EPS_BEARER_CONTEXT_ACCEPT
    							epsBearerId = '6'H
    							protocolDiscriminator = 0010'B
    							procedureTransactionIdentifier = '00'O
    							messageType = 11000110'B
    							protocolConfigurationOptions = Omit
    							nbifomContainer = Omit
    							extdProtocolConfigurationOptions = Omit
    					PiggybackedPduList = Omit

    Inter-component message: SRB -> EUTRA_5GS_PTC:SRB

    EUTRA_NR_Coordination_MSG
    	OctetData
    		Data = '00'O
    		Description = 'Complete'

    Inter-component message: EUTRA -> ENDC_NR_PTC:EUTRA

    EUTRA_NR_Coordination_MSG
    	SysInfo
    		NR
    			CoOrd_NRSysInfo_Type
    				Arfcn = 2229499
    				PhysCellId = 0
    				SCS = 120
    				IsFDD = False
    				IsFR1 = False
    				Band = 260

    Inter-component message: NR -> EUTRA_5GS_PTC:NR

    recordType = 24
    summary = Preamble

    Preamble

    IntermediateVerdict = (Pass)
    summary = Intermediate verdict: (PASS)
    TTCN-3 message: initial preliminary pass

    Intermediate verdict: (PASS)
    TTCN-3 message: initial preliminary pass

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		CellAttenuationList
    			CellAttenuationConfig_Type
    				CellId = eutra_Cell1 (1)
    				Attenuation
    					Value = 11
    				TimingInfo = Omit

    Sent from port: EUTRA_5GS_PTC:SYS

    SYSTEM_CTRL_CNF
    	Common
    		CellId = eutra_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		CellAttenuationList = True

    Received on port: EUTRA_5GS_PTC:SYS

    EUTRA_NR_Coordination_MSG
    	TriggerEvent
    		Reason = 'ChangePower'

    Inter-component message: EUTRA -> ENDC_NR_PTC:EUTRA

    recordType = 24
    summary = Preamble

    Preamble

    IntermediateVerdict = (Pass)
    summary = Intermediate verdict: (PASS)
    TTCN-3 message: initial preliminary pass

    Intermediate verdict: (PASS)
    TTCN-3 message: initial preliminary pass

    recordType = 24
    summary = Step 1-2 (8.2.3.4.1, 8.2.3.5.1, 8.2.3.7.1)

    Step 1-2 (8.2.3.4.1, 8.2.3.5.1, 8.2.3.7.1)

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		CellAttenuationList
    			NR_CellAttenuationConfig_Type
    				CellId = nr_Cell1 (1)
    				Attenuation
    					Value = 3
    				TimingInfo = Omit

    Sent from port: ENDC_NR_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		CellAttenuationList = True

    Received on port: ENDC_NR_PTC:SYS

    recordType = 24
    summary = Steps 1-2

    Steps 1-2

    EUTRA_NR_Coordination_MSG
    	OctetData
    		Data = '042A8000F2808813EDD0052C80000000000000019101FBDEF7BDE0205206000040478240BEE000000700080000'O
    		Description = 'Reconfig'

    Inter-component message: NR -> EUTRA_5GS_PTC:NR

    SRB_COMMON_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcConnectionReconfiguration
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								c1
    									rrcConnectionReconfiguration_r8
    										measConfig = Omit
    										mobilityControlInfo = Omit
    										dedicatedInfoNASList = Omit
    										radioResourceConfigDedicated = Omit
    										securityConfigHO = Omit
    										nonCriticalExtension
    											lateNonCriticalExtension = Omit
    											nonCriticalExtension
    												otherConfig_r9 = Omit
    												fullConfig_r9 = Omit
    												nonCriticalExtension
    													sCellToReleaseList_r10 = Omit
    													sCellToAddModList_r10 = Omit
    													nonCriticalExtension
    														systemInformationBlockType1Dedicated_r11 = Omit
    														nonCriticalExtension
    															wlan_OffloadInfo_r12 = Omit
    															scg_Configuration_r12 = Omit
    															sl_SyncTxControl_r12 = Omit
    															sl_DiscConfig_r12 = Omit
    															sl_CommConfig_r12 = Omit
    															nonCriticalExtension
    																sCellToReleaseListExt_r13 = Omit
    																sCellToAddModListExt_r13 = Omit
    																lwa_Configuration_r13 = Omit
    																lwip_Configuration_r13 = Omit
    																rclwi_Configuration_r13 = Omit
    																nonCriticalExtension
    																	sl_V2X_ConfigDedicated_r14 = Omit
    																	sCellToAddModListExt_v1430 = Omit
    																	perCC_GapIndicationRequest_r14 = Omit
    																	systemInformationBlockType2Dedicated_r14 = Omit
    																	nonCriticalExtension
    																		nr_Config_r15
    																			setup
    																				endc_ReleaseAndAdd_r15 = False
    																				nr_SecondaryCellGroupConfig_r15 = '042A8000F2808813EDD0052C80000000000000019101FBDEF7BDE0205206000040478240BEE000000700080000'O
    																				p_MaxEUTRA_r15 = 20
    																		sk_Counter_r15 = Omit
    																		nr_RadioBearerConfig1_r15 = Omit
    																		nr_RadioBearerConfig2_r15 = Omit
    																		tdm_PatternConfig_r15 = Omit
    																		nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: TC_SRB -> NASEMU_EUTRA_PTC:TC_SRB

    RRCReconfiguration
    	rrc-TransactionIdentifier = 0
    	criticalExtensions = rrcReconfiguration =
    		measConfig
    			measObjectToAddModList = SEQUENCE OF MeasObjectToAddMod
    				MeasObjectToAddMod(1)
    					measObjectId = 1
    					measObject = measObjectNR =
    						ssbFrequency = 2229499
    						ssbSubcarrierSpacing = kHz120
    						smtc1
    							periodicityAndOffset = sf160 = 0
    							duration = sf3
    						referenceSignalConfig
    							ssb-ConfigMobility
    								ssb-ToMeasure = setup = longBitmap = 0100000000000000000000000000000000000000000000000000000000000000
    								deriveSSB-IndexFromCell = TRUE
    						absThreshSS-BlocksConsolidation
    							thresholdRSRP = 68
    						nrofSS-BlocksToAverage = 2
    						quantityConfigIndex = 1
    						offsetMO
    							rsrpOffsetSSB = dB0
    							rsrqOffsetSSB = dB0
    							sinrOffsetSSB = dB0
    							rsrpOffsetCSI-RS = dB0
    							rsrqOffsetCSI-RS = dB0
    							sinrOffsetCSI-RS = dB0
    						freqBandIndicatorNR-v1530 = 260
    			reportConfigToAddModList = SEQUENCE OF ReportConfigToAddMod
    				ReportConfigToAddMod(1)
    					reportConfigId = 1
    					reportConfig = reportConfigNR =
    						reportType = eventTriggered =
    							eventId = eventA2 =
    								a2-Threshold = rsrp = 60
    								reportOnLeave = FALSE
    								hysteresis = 4
    								timeToTrigger = ms320
    							rsType = ssb
    							reportInterval = ms480
    							reportAmount = infinity
    							reportQuantityCell
    								rsrp = TRUE
    								rsrq = TRUE
    								sinr = FALSE
    							maxReportCells = 8
    							includeBeamMeasurements = FALSE
    			measIdToAddModList = SEQUENCE OF MeasIdToAddMod
    				MeasIdToAddMod(1)
    					measId = 1
    					measObjectId = 1
    					reportConfigId = 1
    			quantityConfig
    				quantityConfigNR-List = SEQUENCE OF QuantityConfigNR
    					QuantityConfigNR(1)
    						quantityConfigCell
    							ssb-FilterConfig
    								filterCoefficientRSRP  = fc4
    								filterCoefficientRSRQ  = fc4
    								filterCoefficientRS-SINR  = fc4
    							csi-RS-FilterConfig
    								filterCoefficientRSRP  = fc4
    								filterCoefficientRSRQ  = fc4
    								filterCoefficientRS-SINR  = fc4
    						quantityConfigRS-Index
    							ssb-FilterConfig
    								filterCoefficientRSRP  = fc4
    								filterCoefficientRSRQ  = fc4
    								filterCoefficientRS-SINR  = fc4
    							csi-RS-FilterConfig
    								filterCoefficientRSRP  = fc4
    								filterCoefficientRSRQ  = fc4
    								filterCoefficientRS-SINR  = fc4
    					QuantityConfigNR(2)
    						quantityConfigCell
    							ssb-FilterConfig
    								filterCoefficientRSRP  = fc4
    								filterCoefficientRSRQ  = fc4
    								filterCoefficientRS-SINR  = fc4
    							csi-RS-FilterConfig
    								filterCoefficientRSRP  = fc4
    								filterCoefficientRSRQ  = fc4
    								filterCoefficientRS-SINR  = fc4
    						quantityConfigRS-Index
    							ssb-FilterConfig
    								filterCoefficientRSRP  = fc4
    								filterCoefficientRSRQ  = fc4
    								filterCoefficientRS-SINR  = fc4
    							csi-RS-FilterConfig
    								filterCoefficientRSRP  = fc4
    								filterCoefficientRSRQ  = fc4
    								filterCoefficientRS-SINR  = fc4

    RRCReconfiguration

    DL-DCCH-Message
    	message = c1 = rrcConnectionReconfiguration =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = c1 = rrcConnectionReconfiguration-r8 =
    			nonCriticalExtension
    				nonCriticalExtension
    					nonCriticalExtension
    						nonCriticalExtension
    							nonCriticalExtension
    								nonCriticalExtension
    									nonCriticalExtension
    										nonCriticalExtension
    											nr-Config-r15 = setup =
    												endc-ReleaseAndAdd-r15 = FALSE
    												nr-SecondaryCellGroupConfig-r15 = 042A8000F2808813EDD0052C80000000000000019101FBDEF7BDE0205206000040478240BEE000000700080000
    												p-MaxEUTRA-r15 = 20

    rrcConnectionReconfiguration

    RRC_PDU_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcConnectionReconfiguration
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							c1
    								rrcConnectionReconfiguration_r8
    									measConfig = Omit
    									mobilityControlInfo = Omit
    									dedicatedInfoNASList = Omit
    									radioResourceConfigDedicated = Omit
    									securityConfigHO = Omit
    									nonCriticalExtension
    										lateNonCriticalExtension = Omit
    										nonCriticalExtension
    											otherConfig_r9 = Omit
    											fullConfig_r9 = Omit
    											nonCriticalExtension
    												sCellToReleaseList_r10 = Omit
    												sCellToAddModList_r10 = Omit
    												nonCriticalExtension
    													systemInformationBlockType1Dedicated_r11 = Omit
    													nonCriticalExtension
    														wlan_OffloadInfo_r12 = Omit
    														scg_Configuration_r12 = Omit
    														sl_SyncTxControl_r12 = Omit
    														sl_DiscConfig_r12 = Omit
    														sl_CommConfig_r12 = Omit
    														nonCriticalExtension
    															sCellToReleaseListExt_r13 = Omit
    															sCellToAddModListExt_r13 = Omit
    															lwa_Configuration_r13 = Omit
    															lwip_Configuration_r13 = Omit
    															rclwi_Configuration_r13 = Omit
    															nonCriticalExtension
    																sl_V2X_ConfigDedicated_r14 = Omit
    																sCellToAddModListExt_v1430 = Omit
    																perCC_GapIndicationRequest_r14 = Omit
    																systemInformationBlockType2Dedicated_r14 = Omit
    																nonCriticalExtension
    																	nr_Config_r15
    																		setup
    																			endc_ReleaseAndAdd_r15 = False
    																			nr_SecondaryCellGroupConfig_r15 = '042A8000F2808813EDD0052C80000000000000019101FBDEF7BDE0205206000040478240BEE000000700080000'O
    																			p_MaxEUTRA_r15 = 20
    																	sk_Counter_r15 = Omit
    																	nr_RadioBearerConfig1_r15 = Omit
    																	nr_RadioBearerConfig2_r15 = Omit
    																	tdm_PatternConfig_r15 = Omit
    																	nonCriticalExtension = Omit

    Sent from port: NASEMU_EUTRA_PTC:SYS_SRB

    UL-DCCH-Message
    	message = c1 = rrcConnectionReconfigurationComplete =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = rrcConnectionReconfigurationComplete-r8 =
    			nonCriticalExtension
    				nonCriticalExtension
    					nonCriticalExtension
    						nonCriticalExtension
    							nonCriticalExtension
    								nonCriticalExtension
    									scg-ConfigResponseNR-r15 = 00

    rrcConnectionReconfigurationComplete

    RRC_PDU_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 206
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcConnectionReconfigurationComplete
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							rrcConnectionReconfigurationComplete_r8
    								nonCriticalExtension
    									lateNonCriticalExtension = Omit
    									nonCriticalExtension
    										rlf_InfoAvailable_r10 = Omit
    										logMeasAvailable_r10 = Omit
    										nonCriticalExtension
    											connEstFailInfoAvailable_r11 = Omit
    											nonCriticalExtension
    												logMeasAvailableMBSFN_r12 = Omit
    												nonCriticalExtension
    													perCC_GapIndicationList_r14 = Omit
    													numFreqEffective_r14 = Omit
    													numFreqEffectiveReduced_r14 = Omit
    													nonCriticalExtension
    														scg_ConfigResponseNR_r15 = '00'O
    														nonCriticalExtension = Omit

    Received on port: NASEMU_EUTRA_PTC:SYS_SRB

    SRB_COMMON_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 206
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcConnectionReconfigurationComplete
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								rrcConnectionReconfigurationComplete_r8
    									nonCriticalExtension
    										lateNonCriticalExtension = Omit
    										nonCriticalExtension
    											rlf_InfoAvailable_r10 = Omit
    											logMeasAvailable_r10 = Omit
    											nonCriticalExtension
    												connEstFailInfoAvailable_r11 = Omit
    												nonCriticalExtension
    													logMeasAvailableMBSFN_r12 = Omit
    													nonCriticalExtension
    														perCC_GapIndicationList_r14 = Omit
    														numFreqEffective_r14 = Omit
    														numFreqEffectiveReduced_r14 = Omit
    														nonCriticalExtension
    															scg_ConfigResponseNR_r15 = '00'O
    															nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: SRB -> EUTRA_5GS_PTC:SRB

    recordType = 24
    summary = Step 3(8.2.3.4.1, 8.2.3.5.1, 8.2.3.7.1)/9(8.2.3.7.1)/15(8.2.3.7.1)/6(8.2.3.8.1)/12(8.2.3.8.1)

    Step 3(8.2.3.4.1, 8.2.3.5.1, 8.2.3.7.1)/9(8.2.3.7.1)/15(8.2.3.7.1)/6(8.2.3.8.1)/12(8.2.3.8.1)

    EUTRA_NR_Coordination_MSG
    	OctetData
    		Data = '00'O
    		Description = 'Complete'

    Inter-component message: EUTRA -> ENDC_NR_PTC:EUTRA

    recordType = 24
    summary = Step 3

    Step 3

    recordType = 24
    summary = Steps 4-5(8.2.3.4.1, 8.2.3.5.1, 8.2.3.7.1)/10-11(8.2.3.7.1)/16-17(8.2.3.7.1)/7-8(8.2.3.8.1)/13(8.2.3.8.1)

    Steps 4-5(8.2.3.4.1, 8.2.3.5.1, 8.2.3.7.1)/10-11(8.2.3.7.1)/16-17(8.2.3.7.1)/7-8(8.2.3.8.1)/13(8.2.3.8.1)

    EUTRA_NR_Coordination_MSG
    	TriggerEvent
    		Reason = 'ChangePower'

    Inter-component message: EUTRA -> ENDC_NR_PTC:EUTRA

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		CellAttenuationList
    			NR_CellAttenuationConfig_Type
    				CellId = nr_Cell1 (1)
    				Attenuation
    					Value = 21
    				TimingInfo = Omit

    Sent from port: ENDC_NR_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		CellAttenuationList = True

    Received on port: ENDC_NR_PTC:SYS

    recordType = 24
    summary = Steps 4-5

    Steps 4-5

    UL-DCCH-Message
    	message = messageClassExtension = c2 = ulInformationTransferMRDC-r15 =
    		criticalExtensions = c1 = ulInformationTransferMRDC-r15 =
    			ul-DCCH-MessageNR-r15 = 000000140059AC00

    ulInformationTransferMRDC-r15

    UL-DCCH-Message
    	message = c1 = measurementReport =
    		criticalExtensions = measurementReport =
    			measResults
    				measId = 1
    				measResultServingMOList = SEQUENCE OF MeasResultServMO
    					MeasResultServMO(1)
    						servCellId = 1
    						measResultServingCell
    							physCellId = 0
    							measResult
    								cellResults
    									resultsSSB-Cell
    										rsrp = 53
    										rsrq = 64

    measurementReport

    RRC_PDU_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 268
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				messageClassExtension
    					c2
    						ulInformationTransferMRDC_r15
    							criticalExtensions
    								c1
    									ulInformationTransferMRDC_r15
    										ul_DCCH_MessageNR_r15 = '000000140059AC00'O
    										lateNonCriticalExtension = Omit
    										nonCriticalExtension = Omit

    Received on port: NASEMU_EUTRA_PTC:SYS_SRB

    SRB_COMMON_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 268
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc
    			Dcch
    				message_
    					messageClassExtension
    						c2
    							ulInformationTransferMRDC_r15
    								criticalExtensions
    									c1
    										ulInformationTransferMRDC_r15
    											ul_DCCH_MessageNR_r15 = '000000140059AC00'O
    											lateNonCriticalExtension = Omit
    											nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: SRB -> EUTRA_5GS_PTC:SRB

    EUTRA_NR_Coordination_MSG
    	OctetData
    		Data = '000000140059AC00'O
    		Description = 'ULInfoTransferMRDC'

    Inter-component message: EUTRA -> ENDC_NR_PTC:EUTRA

    IntermediateVerdict = (Pass)
    summary = Intermediate verdict: (PASS)
    TTCN-3 message: Steps 4-5

    Intermediate verdict: (PASS)
    TTCN-3 message: Steps 4-5

    UL-DCCH-Message
    	message = messageClassExtension = c2 = ulInformationTransferMRDC-r15 =
    		criticalExtensions = c1 = ulInformationTransferMRDC-r15 =
    			ul-DCCH-MessageNR-r15 = 000000140059A400

    ulInformationTransferMRDC-r15

    UL-DCCH-Message
    	message = c1 = measurementReport =
    		criticalExtensions = measurementReport =
    			measResults
    				measId = 1
    				measResultServingMOList = SEQUENCE OF MeasResultServMO
    					MeasResultServMO(1)
    						servCellId = 1
    						measResultServingCell
    							physCellId = 0
    							measResult
    								cellResults
    									resultsSSB-Cell
    										rsrp = 52
    										rsrq = 64

    measurementReport

    RRC_PDU_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 316
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				messageClassExtension
    					c2
    						ulInformationTransferMRDC_r15
    							criticalExtensions
    								c1
    									ulInformationTransferMRDC_r15
    										ul_DCCH_MessageNR_r15 = '000000140059A400'O
    										lateNonCriticalExtension = Omit
    										nonCriticalExtension = Omit

    Received on port: NASEMU_EUTRA_PTC:SYS_SRB

    SRB_COMMON_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 316
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc
    			Dcch
    				message_
    					messageClassExtension
    						c2
    							ulInformationTransferMRDC_r15
    								criticalExtensions
    									c1
    										ulInformationTransferMRDC_r15
    											ul_DCCH_MessageNR_r15 = '000000140059A400'O
    											lateNonCriticalExtension = Omit
    											nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: SRB -> EUTRA_5GS_PTC:SRB

    EUTRA_NR_Coordination_MSG
    	OctetData
    		Data = '000000140059A400'O
    		Description = 'ULInfoTransferMRDC'

    Inter-component message: EUTRA -> ENDC_NR_PTC:EUTRA

    IntermediateVerdict = (Pass)
    summary = Intermediate verdict: (PASS)
    TTCN-3 message: Steps 4-5

    Intermediate verdict: (PASS)
    TTCN-3 message: Steps 4-5

    UL-DCCH-Message
    	message = messageClassExtension = c2 = ulInformationTransferMRDC-r15 =
    		criticalExtensions = c1 = ulInformationTransferMRDC-r15 =
    			ul-DCCH-MessageNR-r15 = 000000140059A400

    ulInformationTransferMRDC-r15

    UL-DCCH-Message
    	message = c1 = measurementReport =
    		criticalExtensions = measurementReport =
    			measResults
    				measId = 1
    				measResultServingMOList = SEQUENCE OF MeasResultServMO
    					MeasResultServMO(1)
    						servCellId = 1
    						measResultServingCell
    							physCellId = 0
    							measResult
    								cellResults
    									resultsSSB-Cell
    										rsrp = 52
    										rsrq = 64

    measurementReport

    RRC_PDU_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 364
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				messageClassExtension
    					c2
    						ulInformationTransferMRDC_r15
    							criticalExtensions
    								c1
    									ulInformationTransferMRDC_r15
    										ul_DCCH_MessageNR_r15 = '000000140059A400'O
    										lateNonCriticalExtension = Omit
    										nonCriticalExtension = Omit

    Received on port: NASEMU_EUTRA_PTC:SYS_SRB

    SRB_COMMON_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 364
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc
    			Dcch
    				message_
    					messageClassExtension
    						c2
    							ulInformationTransferMRDC_r15
    								criticalExtensions
    									c1
    										ulInformationTransferMRDC_r15
    											ul_DCCH_MessageNR_r15 = '000000140059A400'O
    											lateNonCriticalExtension = Omit
    											nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: SRB -> EUTRA_5GS_PTC:SRB

    EUTRA_NR_Coordination_MSG
    	OctetData
    		Data = '000000140059A400'O
    		Description = 'ULInfoTransferMRDC'

    Inter-component message: EUTRA -> ENDC_NR_PTC:EUTRA

    IntermediateVerdict = (Pass)
    summary = Intermediate verdict: (PASS)
    TTCN-3 message: Steps 4-5

    Intermediate verdict: (PASS)
    TTCN-3 message: Steps 4-5

    UL-DCCH-Message
    	message = messageClassExtension = c2 = ulInformationTransferMRDC-r15 =
    		criticalExtensions = c1 = ulInformationTransferMRDC-r15 =
    			ul-DCCH-MessageNR-r15 = 000000140059A400

    ulInformationTransferMRDC-r15

    UL-DCCH-Message
    	message = c1 = measurementReport =
    		criticalExtensions = measurementReport =
    			measResults
    				measId = 1
    				measResultServingMOList = SEQUENCE OF MeasResultServMO
    					MeasResultServMO(1)
    						servCellId = 1
    						measResultServingCell
    							physCellId = 0
    							measResult
    								cellResults
    									resultsSSB-Cell
    										rsrp = 52
    										rsrq = 64

    measurementReport

    RRC_PDU_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 412
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				messageClassExtension
    					c2
    						ulInformationTransferMRDC_r15
    							criticalExtensions
    								c1
    									ulInformationTransferMRDC_r15
    										ul_DCCH_MessageNR_r15 = '000000140059A400'O
    										lateNonCriticalExtension = Omit
    										nonCriticalExtension = Omit

    Received on port: NASEMU_EUTRA_PTC:SYS_SRB

    SRB_COMMON_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 412
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc
    			Dcch
    				message_
    					messageClassExtension
    						c2
    							ulInformationTransferMRDC_r15
    								criticalExtensions
    									c1
    										ulInformationTransferMRDC_r15
    											ul_DCCH_MessageNR_r15 = '000000140059A400'O
    											lateNonCriticalExtension = Omit
    											nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: SRB -> EUTRA_5GS_PTC:SRB

    EUTRA_NR_Coordination_MSG
    	OctetData
    		Data = '000000140059A400'O
    		Description = 'ULInfoTransferMRDC'

    Inter-component message: EUTRA -> ENDC_NR_PTC:EUTRA

    recordType = 24
    summary = Step 7(8.2.3.4.1, 8.2.3.5.1, 8.2.3.7.1)/10(8.2.3.8.1)/15(8.2.3.8.1)

    Step 7(8.2.3.4.1, 8.2.3.5.1, 8.2.3.7.1)/10(8.2.3.8.1)/15(8.2.3.8.1)

    IntermediateVerdict = (Pass)
    summary = Intermediate verdict: (PASS)
    TTCN-3 message: Steps 4-5

    Intermediate verdict: (PASS)
    TTCN-3 message: Steps 4-5

    recordType = 24
    summary = Step 6

    Step 6

    timerEvent = 6
    fileName = C:\Users\FETCTTEST\Desktop\Dev_TTCNs\Deepak\7.1.3.3.x\ENDC_IWD_19wk23\Common\Common\CommonDefs.ttcn
    testName = TC_8_2_3_5_1_ENDC
    lineNo = 562
    outStr = Timer: t_Delay, Duration: 15s, Started: 07:00:22

    Timer: t_Delay, Duration: 15s, Started: 07:00:22

    EUTRA_NR_Coordination_MSG
    	TriggerEvent
    		Reason = 'ChangePower'

    Inter-component message: EUTRA -> ENDC_NR_PTC:EUTRA

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    	Request
    		CellAttenuationList
    			NR_CellAttenuationConfig_Type
    				CellId = nr_Cell1 (1)
    				Attenuation
    					Value = 3
    				TimingInfo = Omit

    Sent from port: ENDC_NR_PTC:SYS

    NR_SYSTEM_CTRL_CNF
    	Common
    		CellId = nr_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		CellAttenuationList = True

    Received on port: ENDC_NR_PTC:SYS

    UL-DCCH-Message
    	message = messageClassExtension = c2 = ulInformationTransferMRDC-r15 =
    		criticalExtensions = c1 = ulInformationTransferMRDC-r15 =
    			ul-DCCH-MessageNR-r15 = 00000014005A2400

    ulInformationTransferMRDC-r15

    UL-DCCH-Message
    	message = c1 = measurementReport =
    		criticalExtensions = measurementReport =
    			measResults
    				measId = 1
    				measResultServingMOList = SEQUENCE OF MeasResultServMO
    					MeasResultServMO(1)
    						servCellId = 1
    						measResultServingCell
    							physCellId = 0
    							measResult
    								cellResults
    									resultsSSB-Cell
    										rsrp = 68
    										rsrq = 64

    measurementReport

    RRC_PDU_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 460
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				messageClassExtension
    					c2
    						ulInformationTransferMRDC_r15
    							criticalExtensions
    								c1
    									ulInformationTransferMRDC_r15
    										ul_DCCH_MessageNR_r15 = '00000014005A2400'O
    										lateNonCriticalExtension = Omit
    										nonCriticalExtension = Omit

    Received on port: NASEMU_EUTRA_PTC:SYS_SRB

    SRB_COMMON_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 460
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc
    			Dcch
    				message_
    					messageClassExtension
    						c2
    							ulInformationTransferMRDC_r15
    								criticalExtensions
    									c1
    										ulInformationTransferMRDC_r15
    											ul_DCCH_MessageNR_r15 = '00000014005A2400'O
    											lateNonCriticalExtension = Omit
    											nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: SRB -> EUTRA_5GS_PTC:SRB

    timerEvent = 9
    fileName = C:\Users\FETCTTEST\Desktop\Dev_TTCNs\Deepak\7.1.3.3.x\ENDC_IWD_19wk23\Common\Common\CommonDefs.ttcn
    testName = TC_8_2_3_5_1_ENDC
    lineNo = 563
    outStr = Timer: t_Delay, Expired: 07:00:37

    Timer: t_Delay, Expired: 07:00:37

    recordType = 24
    summary = Step 8(8.2.3.4.1, 8.2.3.5.1, 8.2.3.7.1)/11(8.2.3.8.1)/16(8.2.3.8.1)

    Step 8(8.2.3.4.1, 8.2.3.5.1, 8.2.3.7.1)/11(8.2.3.8.1)/16(8.2.3.8.1)

    timerEvent = 6
    fileName = C:\Users\FETCTTEST\Desktop\Dev_TTCNs\Deepak\7.1.3.3.x\ENDC_IWD_19wk23\ENDC\8_2_3\RRCMeasurement_ENDC_EUTRA.ttcn
    testName = TC_8_2_3_5_1_ENDC
    lineNo = 1029
    outStr = Timer: t_Watchlog, Duration: 10s, Started: 07:00:37

    Timer: t_Watchlog, Duration: 10s, Started: 07:00:37

    timerEvent = 9
    fileName = C:\Users\FETCTTEST\Desktop\Dev_TTCNs\Deepak\7.1.3.3.x\ENDC_IWD_19wk23\ENDC\8_2_3\RRCMeasurement_ENDC_EUTRA.ttcn
    testName = TC_8_2_3_5_1_ENDC
    lineNo = 1037
    outStr = Timer: t_Watchlog, Expired: 07:00:47

    Timer: t_Watchlog, Expired: 07:00:47

    recordType = 24
    summary = Postamble

    Postamble

    IntermediateVerdict = (Pass)
    summary = Intermediate verdict: (PASS)
    TTCN-3 message: Step 8

    Intermediate verdict: (PASS)
    TTCN-3 message: Step 8

    IP_ConfigReq_Type
    	ChangeDrbInfo
    		PdnId = PDN_1 (0)
    		DrbInfo
    			Eutra
    				CellId = eutra_Cell1 (1)
    				DrbId = 1

    Inter-component message: EUTRA_CTRL -> IP_PTC:EUTRA_CTRL

    DRBMUX_CONFIG_REQ
    	RoutingInfo
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 53
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 67
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = icmpv6 (3)
    				Local
    					IpAddr
    						V6
    							Addr = 'FE80:0000:0000:0000:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = Omit
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = udp (0)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V4
    							Addr = '192.168.198.55'
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit
    		IP_RoutingInfo_Type
    			IpInfo
    				Protocol = tcp (1)
    				Local
    					IpAddr
    						V6
    							Addr = 'FD29:CC43:7FB9:0002:020C:29FF:FE66:B4C7'
    							ScopeId = Omit
    					Port = 5060
    				Remote = Omit
    			DRB
    				Eutra
    					CellId = eutra_Cell1 (1)
    					DrbId = 1
    			DataMode = Omit

    Sent from port: IP_PTC:IP_CTRL

    DRBMUX_COMMON_IND_CNF
    	Confirm = True

    Received on port: IP_PTC:IP_CTRL

    IP_Indication_Type
    	Cnf = True

    Inter-component message: IP -> EUTRA_5GS_PTC:IP

    ConstraintMismatch::Received:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = CNF_REQUIRED (1)
    ConstraintMismatch::Expected:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		CnfReq = NO_CNF_REQUIRED (0)

    Message Mismatch: Ut_CnfReq_Type

    ConstraintMismatch::Received:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = LOCAL_CNF_REQUIRED (2)
    ConstraintMismatch::Expected:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		CnfReq = NO_CNF_REQUIRED (0)

    Message Mismatch: Ut_CnfReq_Type

    UT_COMMON_CMD
    	Cmd = SWITCH_OFF (112)
    	CnfReq = NO_CNF_REQUIRED (0)
    	ParameterList = Omit

    Inter-component message: PTC_Ut -> MTC_ENDC:PTC_Ut

    ConstraintMismatch::Received:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = CNF_REQUIRED (1)
    ConstraintMismatch::Expected:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		CnfReq = NO_CNF_REQUIRED (0)

    Message Mismatch: Ut_CnfReq_Type

    ConstraintMismatch::Received:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		Ut_CnfReq_Type = LOCAL_CNF_REQUIRED (2)
    ConstraintMismatch::Expected:
    summary = Message Mismatch: Ut_CnfReq_Type
    MATCH_MISMATCH
    	Message Mismatch: Ut_CnfReq_Type
    		CnfReq = NO_CNF_REQUIRED (0)

    Message Mismatch: Ut_CnfReq_Type

    Sender = RequestServer
    Text = Received !SWITCH_OFF from SAT Controller PC

    RequestServer:Received !SWITCH_OFF from SAT Controller PC

    ConstraintMismatch::Received:
    summary = Message Mismatch: BitStringType
    MATCH_MISMATCH
    	Message Mismatch: BitStringType = 111'B
    		BitStringType
    ConstraintMismatch::Expected:
    summary = Message Mismatch: BitStringType
    MATCH_MISMATCH
    	Message Mismatch: BitStringType = 000'B
    		KSIasme

    Message Mismatch: BitStringType

    Sender = RequestServer
    Text = Request received [!SWITCH_OFF]

    RequestServer:Request received [!SWITCH_OFF]

    UT_SYSTEM_REQ
    	Cmd
    		MMI
    			Cmd = 'SWITCH_OFF'
    			ParameterList = Omit
    	CnfRequired = NO_CNF_REQUIRED (0)

    Sent from port: MTC_ENDC:Ut

    Sender = RequestServer
    Text = [!SWITCH_OFF] Started

    RequestServer:[!SWITCH_OFF] Started

    Sender = !SWITCH_OFF
    Text = Sending AT+CFUN=0

    !SWITCH_OFF:Sending AT+CFUN=0

    Sender = !SWITCH_OFF
    Text = Checking if "AT+CFUN=0" was sent successfully

    !SWITCH_OFF:Checking if "AT+CFUN=0" was sent successfully

    Sender = Device Under Test
    Text = Sent "AT+CFUN=0"

    Device Under Test:Sent "AT+CFUN=0"

    Sender = RequestServer
    Text = Received AT+CFUN=0 from Device Under Test

    RequestServer:Received AT+CFUN=0 from Device Under Test

    UL-DCCH-Message
    	message = c1 = ulInformationTransfer =
    		criticalExtensions = c1 = ulInformationTransfer-r8 =
    			dedicatedInfoType = dedicatedInfoNAS = 27C7D5D49F0591B2655B494977D13D4B67A8EA64E5

    ulInformationTransfer

    Security Protected NAS Message
    	Security header type [4 bits] = 0x2 [ 2 ]
    	Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    	MAC = 0x4755541F [ 1196774431 ]
    	Sequence Number = 0x05 [ 5 ]
    	NAS message = 0x1132655B494977513D4B67286A6465

    Security Protected NAS Message UL PDU

    Ciphered NAS Message
    	0x1132655B494977513D4B67286A6465

    Ciphered NAS Message UL PDU

    RRC_PDU_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 2
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 970
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				c1
    					ulInformationTransfer
    						criticalExtensions
    							c1
    								ulInformationTransfer_r8
    									dedicatedInfoType
    										dedicatedInfoNAS = '27C7D5D49F0591B2655B494977D13D4B67A8EA64E5'O
    									nonCriticalExtension = Omit

    Received on port: NASEMU_EUTRA_PTC:SYS_SRB

    Detach Request UE Originating
    	Security header type [4 bits] = 0x0 [ 0 ]
    	Protocol Discriminator [4 bits] = 0x7 - EPS Mobility Management Messages [ 7 ]
    	Message Type [8 bits] = 0x45 - Detach Request UE Originating [ 69 ]
    	NAS key set identifier
    		Type of security context flag [1 bit] = 0x0 [ 0 ]
    		key sequence indicator [3 bits] = 0x0 [ 0 ]
    	Detach Type
    		switch off [1 bit] = 0x1 - switch off [ 1 ]
    		EPS Detach type [3 bits] = 0x3 - IMSI Detach [ 3 ]
    	GUTI or IMSI
    		IE Length [8 bits] = 0xB [ 11 ]
    		constant / IMSI Identity Digit 1 [4 bits] = 0xF [ 15 ]
    		Odd / Even Indicator [1 bit] = 0x0 [ 0 ]
    		EPS Type of Identity [3 bits] = 0x6 - GUTI [ 6 ]
    		Mobile Country Code 1st and 2nd  Digits = 0x00 [ 0 ]
    		Mobile Network Code 3rd Digit = 0xF [ 15 ]
    		Mobile Country Code 3rd Digit = 0x1 [ 1 ]
    		Mobile Network Code 1st and 2nd  Digits = 0x10 [ 16 ]
    		MME group Id = 0x8001 [ 32769 ]
    		MME code = 0x01 [ 1 ]
    		M-TMSI = 0xC2345678 [ 3258209912 ]

    Detach Request UE Originating PDU

    SRB_COMMON_IND
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 2
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 970
    				Subframe
    					Number = 3
    				HSFN
    					Number = 0
    				Slot
    					Any = True
    		Status
    			Ok = True
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc = Omit
    		Nas
    			NasIndication
    				SecurityProtection
    					Status = 0010'B
    					NasCount = '00000005'O
    				Pdu
    					Msg
    						dETACH_REQUEST_MO
    							securityHeaderType = 0000'B
    							protocolDiscriminator = 0111'B
    							messageType = 01000101'B
    							asmeNasKeySetId
    								iei = Omit
    								tsc = 0'B
    								nasKeySetId = 000'B
    							detachType
    								switchOff = 1'B
    								typeOfDetach = 011'B
    							epsMobileIdentity
    								iei = Omit
    								iel = '0B'O
    								idDigit1 = 1111'B
    								oddEvenInd = 0'B
    								typeOfId = 110'B
    								otherDigits = '00F110800101C2345678'O
    					PiggybackedPduList = Omit

    Inter-component message: SRB -> EUTRA_5GS_PTC:SRB

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		EnquireTiming = True

    Sent from port: EUTRA_5GS_PTC:SYS

    SYSTEM_CTRL_CNF
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 972
    				Subframe
    					Number = 8
    				HSFN
    					Number = 81
    				Slot
    					FirstSlot = True
    		Result
    			Success = True
    	Confirm
    		EnquireTiming = True

    Received on port: EUTRA_5GS_PTC:SYS

    timerEvent = 6
    fileName = C:\Users\FETCTTEST\Desktop\Dev_TTCNs\Deepak\7.1.3.3.x\ENDC_IWD_19wk23\Common\EUTRA\EUTRA_RRCSteps.ttcn
    testName = TC_8_2_3_5_1_ENDC
    lineNo = 1607
    outStr = Timer: t_Timer, Duration: 2.02s, Started: 07:00:49

    Timer: t_Timer, Duration: 2.02s, Started: 07:00:49

    SRB_COMMON_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 59
    				Subframe
    					Number = 4
    				HSFN
    					Number = 82
    				Slot
    					FirstSlot = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Signalling
    		Rrc
    			Dcch
    				message_
    					c1
    						rrcConnectionRelease
    							rrc_TransactionIdentifier = 0
    							criticalExtensions
    								c1
    									rrcConnectionRelease_r8
    										releaseCause = other (1)
    										redirectedCarrierInfo = Omit
    										idleModeMobilityControlInfo = Omit
    										nonCriticalExtension = Omit
    		Nas = Omit

    Inter-component message: TC_SRB -> NASEMU_EUTRA_PTC:TC_SRB

    DL-DCCH-Message
    	message = c1 = rrcConnectionRelease =
    		rrc-TransactionIdentifier = 0
    		criticalExtensions = c1 = rrcConnectionRelease-r8 =
    			releaseCause = other

    rrcConnectionRelease

    RRC_PDU_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			RadioBearerId
    				Srb = 1
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 59
    				Subframe
    					Number = 4
    				HSFN
    					Number = 82
    				Slot
    					FirstSlot = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	RrcPdu
    		Dcch
    			message_
    				c1
    					rrcConnectionRelease
    						rrc_TransactionIdentifier = 0
    						criticalExtensions
    							c1
    								rrcConnectionRelease_r8
    									releaseCause = other (1)
    									redirectedCarrierInfo = Omit
    									idleModeMobilityControlInfo = Omit
    									nonCriticalExtension = Omit

    Sent from port: NASEMU_EUTRA_PTC:SYS_SRB

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = True
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		PdcpCount
    			Get
    				AllRBs = True

    Sent from port: EUTRA_5GS_PTC:SYS

    Sender = !SWITCH_OFF
    Text = String AT+CFUN=0 has been transmitted successfully

    !SWITCH_OFF:String AT+CFUN=0 has been transmitted successfully

    SYSTEM_CTRL_CNF
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		Result
    			Success = True
    	Confirm
    		PdcpCount
    			Get
    				PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 1
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000001001'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000100'B
    				PdcpCountInfo_Type
    					RadioBearerId
    						Srb = 2
    					UL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000010'B
    					DL
    						Format = PdcpCount_Srb (0)
    						Value = 00000000000000000000000000000000'B
    				PdcpCountInfo_Type
    					RadioBearerId
    						Drb = 1
    					UL
    						Format = PdcpCount_DrbLongSQN (1)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_DrbLongSQN (1)
    						Value = 00000000000000000000000000000000'B
    				PdcpCountInfo_Type
    					RadioBearerId
    						Drb = 8
    					UL
    						Format = PdcpCount_DrbLongSQN (1)
    						Value = 00000000000000000000000000000000'B
    					DL
    						Format = PdcpCount_DrbLongSQN (1)
    						Value = 00000000000000000000000000000000'B

    Received on port: EUTRA_5GS_PTC:SYS

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 59
    			Subframe
    				Number = 4
    			HSFN
    				Number = 82
    			Slot
    				FirstSlot = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		Now
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				FirstSlot

    Message Mismatch: TimingInfo_Type

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 59
    				Subframe
    					Number = 4
    				HSFN
    					Number = 82
    				Slot
    					FirstSlot = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		Cell
    			AddOrReconfigure
    				Basic
    					ConfigCapability = Omit
    					StaticCellInfo = Omit
    					PhysicalLayerConfigDL = Omit
    					InitialCellPower = Omit
    					BcchConfig = Omit
    					PcchConfig = Omit
    					CA_CellInitialConfig = Omit
    					BRBcchConfig = Omit
    					LAA_SCellConfiguration = Omit
    					LAA_SCellConfiguration_v1430 = Omit
    				Active
    					C_RNTI = Omit
    					PhysicalLayerConfigUL = Omit
    					RachProcedureConfig = Omit
    					CcchDcchDtchConfig
    						MeasGapCtrl = Omit
    						DL = Omit
    						UL
    							DciInfo
    								Imcs = Omit
    								TransRetransmissionList = Omit
    								FreqDomainSchedul = Omit
    								Format = Omit
    								HarqProcessId = Omit
    								RepetitionNumber = Omit
    								DCISubframeRepetitionNumber = Omit
    								PUSCH_TriggerA = Omit
    								TimingOffset = Omit
    								NumberOfScheduledSubframes = Omit
    							Hopping
    								Deactivated = True
    							PUCCH_Synch
    								None = True
    							UL_GrantConfig
    								None = True
    						DrxCtrl = Omit
    						TtiBundling = Omit
    						CifPresence = Omit
    					ServingCellConfig = Omit
    					SciSchedulingConfig = Omit
    					EIMTA_Config = Omit
    					CE_Mode = Omit

    Sent from port: EUTRA_5GS_PTC:SYS

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 59
    			Subframe
    				Number = 9
    			HSFN
    				Number = 82
    			Slot
    				FirstSlot = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		Now
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				FirstSlot

    Message Mismatch: TimingInfo_Type

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 59
    				Subframe
    					Number = 9
    				HSFN
    					Number = 82
    				Slot
    					FirstSlot = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		AS_Security
    			Release = True

    Sent from port: EUTRA_5GS_PTC:SYS

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 64
    			Subframe
    				Number = 9
    			HSFN
    				Number = 82
    			Slot
    				FirstSlot = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		Now
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				FirstSlot

    Message Mismatch: TimingInfo_Type

    Sender = RequestServer
    Text = Received OK from Device Under Test

    RequestServer:Received OK from Device Under Test

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 64
    				Subframe
    					Number = 9
    				HSFN
    					Number = 82
    				Slot
    					FirstSlot = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		RadioBearerList
    			RadioBearer_Type
    				Id
    					Srb = 1
    				Config
    					Release = True
    			RadioBearer_Type
    				Id
    					Srb = 2
    				Config
    					Release = True
    			RadioBearer_Type
    				Id
    					Drb = 1
    				Config
    					Release = True
    			RadioBearer_Type
    				Id
    					Drb = 8
    				Config
    					Release = True

    Sent from port: EUTRA_5GS_PTC:SYS

    ConstraintMismatch::Received:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		SubFrame
    			SFN
    				Number = 65
    			Subframe
    				Number = 4
    			HSFN
    				Number = 82
    			Slot
    				FirstSlot = True
    ConstraintMismatch::Expected:
    summary = Message Mismatch: TimingInfo_Type
    MATCH_MISMATCH
    	Message Mismatch: TimingInfo_Type
    		Now
    			SFN
    				Number
    			Subframe
    				Number
    			HSFN
    				Number
    			Slot
    				FirstSlot

    Message Mismatch: TimingInfo_Type

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell1 (1)
    		RoutingInfo
    			None = True
    		TimingInfo
    			SubFrame
    				SFN
    					Number = 65
    				Subframe
    					Number = 4
    				HSFN
    					Number = 82
    				Slot
    					FirstSlot = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		RadioBearerList
    			RadioBearer_Type
    				Id
    					Srb = 1
    				Config
    					AddOrReconfigure
    						Pdcp
    							Config
    								Rb
    									Srb = True
    								TestMode
    									None = True
    						Rlc
    							Rb
    								AM
    									Tx
    										R8
    											t_PollRetransmit = ms45 (8)
    											pollPDU = pInfinity (7)
    											pollByte = kBinfinity (14)
    											maxRetxThreshold = t4 (3)
    									Rx
    										R8
    											t_Reordering = ms35 (7)
    											t_StatusProhibit = ms0 (0)
    									ExtendedLI = Omit
    							TestMode
    								None = True
    						LogicalChannelId = 1
    						Mac
    							LogicalChannel
    								Priority = 1
    								PrioritizedBitRate = infinity_ (7)
    								LAA_UL_Allowed = Omit
    							TestMode
    								None = True
    						DiscardULData = Omit
    			RadioBearer_Type
    				Id
    					Srb = 2
    				Config
    					AddOrReconfigure
    						Pdcp
    							Config
    								Rb
    									Srb = True
    								TestMode
    									None = True
    						Rlc
    							Rb
    								AM
    									Tx
    										R8
    											t_PollRetransmit = ms45 (8)
    											pollPDU = pInfinity (7)
    											pollByte = kBinfinity (14)
    											maxRetxThreshold = t4 (3)
    									Rx
    										R8
    											t_Reordering = ms35 (7)
    											t_StatusProhibit = ms0 (0)
    									ExtendedLI = Omit
    							TestMode
    								None = True
    						LogicalChannelId = 2
    						Mac
    							LogicalChannel
    								Priority = 3
    								PrioritizedBitRate = infinity_ (7)
    								LAA_UL_Allowed = Omit
    							TestMode
    								None = True
    						DiscardULData = Omit

    Sent from port: EUTRA_5GS_PTC:SYS

    timerEvent = 9
    fileName = C:\Users\FETCTTEST\Desktop\Dev_TTCNs\Deepak\7.1.3.3.x\ENDC_IWD_19wk23\Common\EUTRA\EUTRA_RRCSteps.ttcn
    testName = TC_8_2_3_5_1_ENDC
    lineNo = 1616
    outStr = Timer: t_Timer, Expired: 07:00:51

    Timer: t_Timer, Expired: 07:00:51

    Sender = SAT Controller PC
    Text = Sent "!OK"

    SAT Controller PC:Sent "!OK"

    Sender = RequestServer
    Text = [!SWITCH_OFF] Complete

    RequestServer:[!SWITCH_OFF] Complete

    SYSTEM_CTRL_REQ
    	Common
    		CellId = eutra_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    		RlcBearerRouting = Omit
    	Request
    		Cell
    			Release = True

    Sent from port: EUTRA_5GS_PTC:SYS

    EUTRA_NR_Coordination_MSG
    	TriggerEvent
    		Reason = 'Postamble'

    Inter-component message: EUTRA -> ENDC_NR_PTC:EUTRA

    IntermediateVerdict = (Pass)
    summary = Intermediate verdict: (PASS)

    Intermediate verdict: (PASS)

    NR_SYSTEM_CTRL_REQ
    	Common
    		CellId = nr_Cell_NonSpecific (0)
    		RoutingInfo
    			None = True
    		RlcBearerRouting
    			None = True
    		TimingInfo
    			Now = True
    		ControlInfo
    			CnfFlag = False
    			FollowOnFlag = False
    	Request
    		Cell
    			Release = True

    Sent from port: ENDC_NR_PTC:SYS

    IntermediateVerdict = (Pass)
    summary = Intermediate verdict: (PASS)

    Intermediate verdict: (PASS)

    IntermediateVerdict = (Pass)
    summary = Intermediate verdict: (PASS)

    Intermediate verdict: (PASS)

    verdict = PASS
    summary = Test case ended: TC_8_2_3_5_1_ENDC, Verdict: PASS

    Test case ended: TC_8_2_3_5_1_ENDC, Verdict: PASS

    IntermediateVerdict = (None)
    summary = Intermediate verdict: (NONE)

    Intermediate verdict: (NONE)

    IntermediateVerdict = (None)
    summary = Intermediate verdict: (NONE)

    Intermediate verdict: (NONE)

    IntermediateVerdict = (None)
    summary = Intermediate verdict: (NONE)

    Intermediate verdict: (NONE)

    IntermediateVerdict = (None)
    summary = Intermediate verdict: (NONE)

    Intermediate verdict: (NONE)

    IntermediateVerdict = (None)
    summary = Intermediate verdict: (NONE)

    Intermediate verdict: (NONE)

    Sender = RequestServer
    Text = Received !Stop, PASS from SAT Controller PC

    RequestServer:Received !Stop, PASS from SAT Controller PC

    Sender = RequestServer
    Text = Request received [!Stop, PASS]

    RequestServer:Request received [!Stop, PASS]

    Sender = RequestServer
    Text = [!Stop*] Started

    RequestServer:[!Stop*] Started

    Sender = !Stop*
    Text = Processing Compound Request [!Stop, PASS]

    !Stop*:Processing Compound Request [!Stop, PASS]

    Sender = !Stop*
    Text =     --> Processing Request [DirectSerial AT+CFUN=0] Started

    !Stop*:    --> Processing Request [DirectSerial AT+CFUN=0] Started

    Sender = !Stop*
    Text = Sending AT+CFUN=0

    !Stop*:Sending AT+CFUN=0

    Sender = !Stop*
    Text =     --> Processing Request [DirectSerial AT+CFUN=0] Complete

    !Stop*:    --> Processing Request [DirectSerial AT+CFUN=0] Complete

    Sender = !Stop*
    Text = Compound Request execution successful, sending PASS ACK

    !Stop*:Compound Request execution successful, sending PASS ACK

    Sender = Device Under Test
    Text = Sent "AT+CFUN=0"

    Device Under Test:Sent "AT+CFUN=0"

    Sender = SAT Controller PC
    Text = Sent "!OK"

    SAT Controller PC:Sent "!OK"

    Sender = RequestServer
    Text = [!Stop*] Complete

    RequestServer:[!Stop*] Complete

    Sender = RequestServer
    Text = Received AT+CFUN=0 from Device Under Test

    RequestServer:Received AT+CFUN=0 from Device Under Test

    Sender = RequestServer
    Text = Received OK from Device Under Test

    RequestServer:Received OK from Device Under Test

    recordType = 24
    summary = Final Verdict

    Final Verdict

    verdict = PASS
    summary = TEST CASE ENDED: TC_8_2_3_5_1_ENDC

    TEST CASE ENDED: TC_8_2_3_5_1_ENDC

    Sender = RequestServer
    Text = Disconnected event from Controller SAT Controller PC Received

    RequestServer:Disconnected event from Controller SAT Controller PC Received

    Sender = RequestServer
    Text = State changed from RunningConnected to RunningNotConnected

    RequestServer:State changed from RunningConnected to RunningNotConnected

    Sender = SAT Controller PC
    Text = Binding TCP Server to port 6667

    SAT Controller PC:Binding TCP Server to port 6667

    Sender = SAT Controller PC
    Text = Listening TCP Server to port 6667

    SAT Controller PC:Listening TCP Server to port 6667

    Server State Change to RunningNotConnected