**SA WG2 Meeting #143eS2-2100228**

**Feb 24th – March 9th, 2021 ; Elbonia (revision of S2-2100228)**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **23.502** | **CR** | **2477** | **rev** | **-** | **Current version:** | **16.7.1** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | SRVCC procedure in case of PDN connections without TI | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Nokia, Nokia Shanghai Bell | | | | | | | | | |
| ***Source to TSG:*** | S2 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | 5GS\_Ph1, TEI16 | | | | |  | ***Date:*** | | | 2021-01-18 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | LS on E-RABs that cannot be handed over to 2G/3G or 5G (R3-211273 / S2-2100108) | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | For 5G SRVCC to 3G it is described in 23.501 § 5.17.2.4 “Mobility between 5GS and GERAN/UTRAN” that “After the 5G SRVCC to UTRAN, all the PDU sessions of the UE are released”;  The same behaviour may take place at the indirect mobility 5G 🡪 4G 🡪 (SRVCC) 3G  The MME issues a Forward Relocation Request message to the SGSN and only includes those EPS Bearer/PDP contexts that are associated with a TI. No impact is thus expected to the ENB. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Failure of the SRVCC procedure | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 4.11.0a.x (new) ; 2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **x** | Other core specifications | | | |  | | |
| ***affected:*** | |  | **x** | Test specifications | | | |  | | |
| ***(show related CRs)*** | |  | **x** | O&M Specifications | | | |  | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

*FIRST CHANGE all text is new*

#### 4.11.0a.x Impacts to SRVCC procedures from EPC.

A UE that has moved from 5GS to EPS may later be subject to a SRVCC procedure from EPS as defined in TS 23.216 [xx]. When such a SRVCC procedure takes place, the MME issues a Forward Relocation Request message to the SGSN and includes only those EPS Bearers/PDP context that are associated with a Transaction Identifier (TI, see TS 23.401 [13]) .

After the SRVCC procedure, the UE and the MME locally release any EPS Bearers for which no TI had been communicated to the UE by the network.

*NEXT CHANGE (2)*

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.501: "System Architecture for the 5G System; Stage 2".

[3] IETF RFC 7296: "Internet Key Exchange Protocol Version 2 (IKEv2)".

[4] Void.

[5] Void.

[6] IETF RFC 4861: "Neighbor Discovery for IP version 6 (IPv6)".

[7] 3GPP TS 23.040: "Technical realization of the Short Message Service (SMS)".

[8] IETF RFC 4862: "IPv6 Stateless Address Autoconfiguration".

[9] 3GPP TS 38.300: "NR and NG-RAN Overall Description; Stage 2".

[10] 3GPP TS 38.413: "NG-RAN; NG Application Protocol (NGAP)".

[11] Void.

[12] 3GPP TS 38.331: "NR; Radio Resource Control (RRC); Protocol Specification".

[13] 3GPP TS 23.401: "General Packet Radio Service (GPRS) enhancements for Evolved Universal Terrestrial Radio Access Network (E-UTRAN) access".

[14] Void.

[15] 3GPP TS 33.501: "Security Architecture and Procedures for 5G System".

[16] 3GPP TS 36.331: "Evolved Universal Terrestrial Radio Access (E-UTRA); Radio Resource Control (RRC); Protocol specification".

[17] 3GPP TS 29.500: "5G System; Technical Realization of Service Based Architecture; Stage 3".

[18] 3GPP TS 29.518: "5G System; Access and Mobility Management Services; Stage 3".

[19] Void.

[20] 3GPP TS 23.503: "Policy and Charging Control Framework for the 5G System ".

[21] IETF RFC 4191: "Default Router Preferences and More-Specific Routes".

[22] 3GPP TS 23.122: "Non-Access-Stratum (NAS) functions related to Mobile Station in idle mode".

[23] 3GPP TS 23.682: "Architecture enhancements to facilitate communications with packet data networks and applications".

[24] 3GPP TS 23.203: "Policy and charging control architecture".

[25] 3GPP TS 24.501: "Non-Access-Stratum (NAS) protocol for 5G System (5GS); Stage 3".

[26] 3GPP TS 23.402: "Architecture enhancements for non-3GPP accesses".

[27] Void.

[28] 3GPP TS 23.167: "IP Multimedia Subsystem (IMS) emergency sessions".

[29] Void.

[30] Void.

[31] Void.

[32] 3GPP TS 29.507: "Access and Mobility Policy Control Service; Stage 3".

[33] 3GPP TS 23.003: "Numbering, Addressing and Identification".

[34] Void.

[35] 3GPP TS 23.251: "Network sharing; Architecture and functional description".

[36] 3GPP TS 29.502: "5G System; Session Management Services; Stage 3".

[37] 3GPP TS 29.510: "5G System; Network function repository services; Stage 3".

[38] 3GPP TS 23.380: "IMS Restoration Procedures".

[39] 3GPP TS 32.421: "Telecommunication management; Subscriber and equipment trace; Trace concepts and requirements".

[40] IETF RFC 4555: "IKEv2 Mobility and Multihoming Protocol (MOBIKE)".

[41] 3GPP TS 24.502: "Access to the 3GPP 5G Core Network (5GCN) via Non-3GPP Access Networks (N3AN); Stage 3".

[42] 3GPP TS 32.290: "Services, operations and procedures of charging using Service Based Interface (SBI)".

[43] 3GPP TS 36.304: "Evolved Universal Terrestrial Radio Access (E-UTRA); User Equipment (UE) procedures in idle mode".

[44] 3GPP TS 38.304: "NR; User Equipment (UE) procedures in idle mode".

[45] 3GPP TS 32.255: "5G system; 5G data connectivity domain charging; Stage 2".

[46] 3GPP TS 36.300: "Evolved Universal Terrestrial Radio Access (E-UTRA) and Evolved Universal Terrestrial Radio Access Network (E-UTRAN); Overall description; Stage 2".

[47] 3GPP TS 29.513: "5G System; Policy and Charging Control signalling flows and QoS parameter mapping; Stage 3".

[48] IEEE Std 802.11-2016 (Revision of IEEE Std 802.11-2012): "IEEE Standard for Information technology - Telecommunications and information exchange between systems Local and metropolitan area networks - Specific requirements - Part 11: Wireless LAN Medium Access Control (MAC) and Physical Layer (PHY) Specifications".

[49] IETF RFC 2410: "The NULL Encryption Algorithm and its use with IPsec".

[50] 3GPP TS 23.288: "Architecture enhancements for 5G System (5GS) to support network data analytics services; Stage 2".

[51] 3GPP TS 23.273: "5G System (5GS) Location Services (LCS); Stage 2".

[52] 3GPP TS 29.503: "5G System; Unified Data Management Services; Stage 3".

[53] 3GPP TS 23.316: "Wireless and wireline convergence access support for the 5G System (5GS)".

[54] 3GPP TS 23.222: "Functional architecture and information flows to support Common API Framework for 3GPP Northbound APIs; Stage 2".

[55] 3GPP TS 23.228: "IP Multimedia Subsystem (IMS); Stage 2".

[56] 3GPP TS 36.321: "Evolved Universal Terrestrial Radio Access (E-UTRA); Medium Access Control (MAC) protocol specification".

[57] 3GPP TS 29.512: "5G System; Session Management Policy Control Service; Stage 3".

[58] 3GPP TS 29.525: "5G System; UE Policy Control Service; Stage 3".

[59] IETF RFC 6696: "EAP Extensions for the EAP Re-authentication Protocol (ERP)", July 2012.

[60] IETF RFC 5295: "Specification for the Derivation of Root Keys from an Extended Master Session Key (EMSK)", Aug. 2008.

[61] 3GPP TS 23.272: "Circuit Switched (CS) fallback in Evolved Packet System (EPS); Stage 2".

[62] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[63] 3GPP TS 29.561: "5G System; Interworking between 5G Network and external Data Networks; Stage 3".

[64] 3GPP TS 29.413: "Application of the NG Application Protocol (NGAP) to non-3GPP access".

[65] IEEE Std 802.1Qcc-2018: "Standard for Local and metropolitan area networks - Bridges and Bridged Networks - Amendment: Stream Reservation Protocol (SRP) Enhancements and Performance Improvements".

[66] IEEE Std 802.1Q-2018: "IEEE Standard for Local and Metropolitan Area Networks-Bridges and Bridged Networks".

[67] Void.

[68] 3GPP TS 23.632: "User Data Interworking, Coexistence and Migration".

[69] 3GPP TS 29.244: "Interface between the Control Plane and the User Plane nodes".

[70] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces; Stage 3".

[71] 3GPP TS 32.256: "Charging Management; 5G connection and mobility domain charging; Stage 2".

[72] 3GPP TS 38.423: "NG-RAN; Xn Application Protocol (XnAP)".

[73] 3GPP TS 23.287: "Architecture enhancements for 5G System (5GS) to support Vehicle-to-Everything (V2X) services".

[xx] 3GPP TS 23.216: "Single Radio Voice Call Continuity (SRVCC); Stage 2".

*END OF CHANGES*