|  |  |
| --- | --- |
| 3GPP TR 23.700-27 V0.3.0 (2022-05) | |
| Technical Report | |
| 3rd Generation Partnership Project;  Technical Specification Group Services and System Aspects;  Study on 5G System with Satellite Backhaul  (Release 18) | |
|  | |
|  |  |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 5

1 Scope 7

2 References 7

3 Definitions of terms, symbols and abbreviations 7

3.1 Terms 7

3.2 Abbreviations 8

4 Architecture Assumptions 8

5 Key Issues 8

5.1 Key Issue #1: PCC/QoS control enhancement considering dynamic satellite backhaul 8

5.1.1 Description 8

5.2 Key Issue #2: Support of Satellite Edge Computing via UPF on board 9

5.2.1 Description 9

5.3 Key Issue #3: Support of Local Data Switching via UPF on-board 9

5.3.1 Description 9

6 Solutions 9

6.0 Mapping of Solutions to Key Issues 9

6.1 Dynamic delay solution 9

6.1.1 Description 9

6.1.2 High level architecture principles 10

6.1.3 Impacts on services, entities and interfaces 12

6.2 Solution for KI#1: QoS control enhancements for dynamic satellite backhauling 12

6.2.1 Description 12

6.2.2 Procedures 13

6.2.3 Impacts on services, entities and interfaces 15

6.3 Solution for Key Issue #1: Information of satellite constellation and change of backhaul delay exposed to PCF/AF 16

6.3.1 Description 16

6.3.2 Procedures 17

6.3.3 Impacts on services, entities and interfaces 17

6.4 Solution for Key Issue #2 and Key Issue #3: Enable Satellite Edge Computing or local data switching via on-board UPF acting as UL CL/BP and local PSA 18

6.4.1 Description 18

6.4.2 Procedures 18

6.4.3 Impacts on services, entities and interfaces 19

6.5 Solution for KI#2: Support of Satellite Edge Computing via UPF on board 20

6.5.1 Description 20

6.5.2 Procedures 21

6.5.3 Impacts on services, entities and interfaces 23

6.6 Solution for Key Issue #2 and Key Issue #3: Enable on-board EC or local data switch based on GEO PSA UPF 23

6.6.1 Description 23

6.6.2 Procedures 23

6.6.3 Impacts on services, entities and interfaces 25

6.7 Solution for KI#3: Support of Local Data Switching via UPF on board 26

6.7.1 Description 26

6.7.2 Procedures 27

6.7.3 Impacts on services, entities and interfaces 30

6.8 Solution for Key Issue #1: In-sequence delivery 31

6.8.1 Description 31

6.8.2 Void 32

6.8.3 Impacts on services, entities and interfaces 32

6.9 Solution for Key Issue #1: QoS Monitoring for dynamic satellite backhaul delay control 32

6.9.1 Description 32

6.9.2 Procedures 33

6.9.3 Impacts on services, entities and interfaces 35

6.10 Solution for Key Issue #2: Enable Satellite EAS re-discovery and re-allocation by means of local DNS 36

6.10.1 Description 36

6.10.2 Procedures 36

6.10.3 Impacts on services, entities and interfaces 37

6.X Solution for Key Issue #X: <Solution Title> 37

6.X.1 Description 37

6.X.2 Procedures 37

6.X.3 Impacts on services, entities and interfaces 37

7 Overall Evaluation 37

8 Conclusions 37

Annex A: Change history 38

# Foreword

This Technical Report has been produced by the 3rd Generation Partnership Project (3GPP).

The contents of the present document are subject to continuing work within the TSG and may change following formal TSG approval. Should the TSG modify the contents of the present document, it will be re-released by the TSG with an identifying change of release date and an increase in version number as follows:

Version x.y.z

where:

x the first digit:

1 presented to TSG for information;

2 presented to TSG for approval;

3 or greater indicates TSG approved document under change control.

y the second digit is incremented for all changes of substance, i.e. technical enhancements, corrections, updates, etc.

z the third digit is incremented when editorial only changes have been incorporated in the document.

In the present document, modal verbs have the following meanings:

**shall** indicates a mandatory requirement to do something

**shall not** indicates an interdiction (prohibition) to do something

The constructions "shall" and "shall not" are confined to the context of normative provisions, and do not appear in Technical Reports.

The constructions "must" and "must not" are not used as substitutes for "shall" and "shall not". Their use is avoided insofar as possible, and they are not used in a normative context except in a direct citation from an external, referenced, non-3GPP document, or so as to maintain continuity of style when extending or modifying the provisions of such a referenced document.

**should** indicates a recommendation to do something

**should not** indicates a recommendation not to do something

**may** indicates permission to do something

**need not** indicates permission not to do something

The construction "may not" is ambiguous and is not used in normative elements. The unambiguous constructions "might not" or "shall not" are used instead, depending upon the meaning intended.

**can** indicates that something is possible

**cannot** indicates that something is impossible

The constructions "can" and "cannot" are not substitutes for "may" and "need not".

**will** indicates that something is certain or expected to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**will not** indicates that something is certain or expected not to happen as a result of action taken by an agency the behaviour of which is outside the scope of the present document

**might** indicates a likelihood that something will happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

**might not** indicates a likelihood that something will not happen as a result of action taken by some agency the behaviour of which is outside the scope of the present document

In addition:

**is** (or any other verb in the indicative mood) indicates a statement of fact

**is not** (or any other negative verb in the indicative mood) indicates a statement of fact

The constructions "is" and "is not" do not indicate requirements.

# 1 Scope

The scope of this Technical Report is to study the following aspects of 5GS with satellite backhaul:

1: Architecture enhancements for support of a backhaul with changing delay (e.g. brought by ISL in satellite networks or changed satellite backhaul on the UP path), and possibly limited bandwidth in case of a gNB with satellite backhaul only (e.g. restricted by the maximum data rate of a satellite beam):

- Policy/QoS control enhancements based on the detected packet delivery latency and/or bandwidth of the satellite backhaul on the UP path;

- Exposure of backhaul information to AFs.

2: Architecture enhancements for support of UPF deployed on GEO satellite with gNB on the ground:

- Whether and how to enable satellite edge computing services via UPF on-board e.g. to reduce the latency for data transmission, and minimize the backhaul resources consumption.

- How to enhance local switch for UEs in a communication when they are served by UPF on-board, e.g. to reduce end to end delay comparing with existing 5G LAN local switch at PSA on the ground.

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.501: "System Architecture for the 5G System; Stage 2".

[3] 3GPP TS 23.502: "Procedures for the 5G system, Stage 2".

[4] 3GPP TS 23.503: "Policy and Charging Control Framework for the 5G System".

[5] 3GPP TR 23.737: "Study on architecture aspects for using satellite access in 5G".

[6] 3GPP TS 23.548: "5G System Enhancements for Edge Computing; Stage 2".

# 3 Definitions of terms, symbols and abbreviations

This clause and its three (sub) clauses are mandatory. The contents shall be shown as "void" if the TS/TR does not define any terms, symbols, or abbreviations.

## 3.1 Terms

For the purposes of the present document, the terms given in TR 21.905 [1] and the following apply. A term defined in the present document takes precedence over the definition of the same term, if any, in TR 21.905 [1].

Definition format (Normal)

**<defined term>:** <definition>.

**example:** text used to clarify abstract rules by applying them literally.

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in TR 21.905 [1].

Abbreviation format (EW)

<ABBREVIATION> <Expansion>

# 4 Architecture Assumptions

The 5GS architecture specified in TS 23.501 [2], TS 23.502 [3] and TS 23.503 [4] is used as a baseline.

The following architectural assumptions are applied to the study:

- At least UP backhaul connection of a gNB is over satellite link.

- If available bandwidth information is needed in dynamic satellite backhaul link cases, the bandwidth detection is performed by the transport network layer.

# 5 Key Issues

## 5.1 Key Issue #1: PCC/QoS control enhancement considering dynamic satellite backhaul

### 5.1.1 Description

Satellite based backhaul is important for remote area or mission critical scenarios, in case it is not possible to build terrestrial backhaul connections.

In Release 17, a satellite backhaul category indication was defined to indicate the satellite backhaul information in. However, this indication may not enough if the satellite backhaul involves multi-hops of ISL or backhaul connections are over different satellites and terrestrial networks. In such case, the capabilities provided by the satellite backhaul can be changed/adjusted dynamically. For example, if inter-satellite links are used on the backhaul path, the delay and bandwidth of the backhaul may be impacted due to the traffic engineering on the links. Satellite backhaul category is not enough to describe such a dynamic satellite backhaul characteristics.

To better serve UEs connecting to 5GC via a gNB with satellite backhaul, the following topics are to be studied:

- Determination of packet delivery latency or bandwidth or both of the satellite backhaul on the UP path.

- Policy/QoS control enhancements based on the determined packet delivery latency or bandwidth or both of the satellite backhaul on the UP path.

- What kind of backhaul information can be exposed to the AF, and how to perform the exposure?

- Whether and how to solve packet out-of-sequence problems introduced by dynamic satellite backhaul.

## 5.2 Key Issue #2: Support of Satellite Edge Computing via UPF on board

### 5.2.1 Description

Whether and how to enable satellite edge computing services via UPF on-board e.g. to reduce the latency for data transmission, and minimize the backhaul resources consumption.

NOTE: Coordination with CT4 may be done on aspects related to N4 association between the UPF on board and 5GC NFs on the ground.

## 5.3 Key Issue #3: Support of Local Data Switching via UPF on-board

### 5.3.1 Description

How to support local data switch for UEs in a communication when they are served by UPF on-board, e.g. to reduce end to end delay comparing with existing 5G LAN local switch at PSA on the ground?

# 6 Solutions

## 6.0 Mapping of Solutions to Key Issues

Table 6.0-1: Mapping of Solutions to Key Issues

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | Key Issues | | | |
| Solutions | 1 | 2 | 3 |  |
| 1 | x |  |  |  |
| 2 | x |  |  |  |
| 3 | x |  |  |  |
| 4 |  | x | x |  |
| 5 |  | x |  |  |
| 6 |  | x | x |  |
| 7 |  |  | x |  |
| 8 | x |  |  |  |
| 9 | x |  |  |  |
| 10 |  | x |  |  |

## 6.1 Dynamic delay solution

### 6.1.1 Description

In Rel-17 reference architecture specified in TS 23.501 [2] and TS 23.502 [3], the AMF is configured with the awareness of satellite backhaul categories as specified in TS 23.501 [2] clause 5.8.2.15. The AMF informs the SMF of satellite backhaul category that is being used when PDU session is established and after change or handover causing different backhaul connection to be used. In roaming case, the V-SMF relays the satellite backhaul category to H-SMF. The PCF is informed of satellite backhaul category as the SMF includes it SM Policy Association establishment. Based on this knowledge, the PCF can set the QoS policies accordingly.

NOTE 1: For a gNB that only has single type of satellite backhaul, the AMF detection of satellite backhaul is based on local configuration, e.g. based on AMF awareness of Global RAN Node ID.

A gNB may have multiple candidate satellite backhaul on N2 and N3 interfaces, e.g. GEO satellite backhaul, LEO satellite backhaul, LEO satellite backhaul with ISL. The gNB uses a single satellite backhaul connection from the set of available candidate satellite backhauls for all UEs that the gNB is serving at any point in time. The following figure gives an example scenario:



Figure 6.1.1-1: Example scenario that gNB has multiple candidate satellite backhauls

For such scenario, the gNB may use different CP Transport Layer Information for different satellite backhaul on N2 interface. The AMF determines the Satellite backhaul category (i.e. GEO, MEO, LEO or OTHERSAT) based on local configuration gNB ID and CP Transport Layer Information used by the gNB on N2 interface.

NOTE 2: It is assumed that N2 and N3 interfaces of a gNB use the same satellite backhaul at a certain time.

NOTE 3: For the deployment that gNB use same CP Transport Layer Information for different satellite backhauls, it's assumed that the AMF will be updated by OAM with the latest satellite backhaul type of a gNB when the gNB switches to a different satellite backhaul.

Awareness of QoS changes is needed to adapt this Rel-17 solution to the dynamic delay requirement in Rel-18. That awareness of variable delay can be obtained by re-using the capability for the SMF to request QoS monitoring from the UPF that is specified in clause 5.33.3.3 of TS 23.501 [2]. The SMF can be configured to request QoS monitoring depending on the satellite backhaul type category signalled from AMF e.g. for GEO but not LEO, the UE location and also be configured to request (again) QoS monitoring based on certain triggers e.g. time related or UE location related.

In addition to the already specified use cases where the SMF informs the PCF of the satellite category, the SMF needs to be enhanced to measure the N3 using the echo procedure and to inform the PCF of not only satellite category but also the observed delay.

### 6.1.2 High level architecture principles

Figure 6.1.2-1 shows the call flow that will say the following:



Figure 6.1.2-1: Dynamic delay monitoring and QoS adaptation

1. During PDU session establishment, PDU session modification or handover that leads to NG-RAN with different backhaul category, the AMF determines the satellite backhaul category based on configuration.

2. The AMF informs the SMF of satellite backhaul by including the Satellite Backhaul Category in Nsmf\_PDUSession\_CreateSMContext or in Nsmf\_PDUSession\_UpdateSMContext message as specified in clause 4.3.2.2 of TS 23.502 [3].

3. SMF responds by Nsmf\_PDUSession\_CreateSMContext Responsed message or Nsmf\_PDUSession\_UpdateSMContext Response.

4. SMF informs PCF of the satellite backhaul by including Satellite Backhaul Category in Npcf\_SMPolicyControl\_Create Request during SM Policy Association Establishment as specified in TS 23.502 [3] clause 4.16.4 or Npcf\_SMPolicyControl\_Update Request during SM Policy Association Modification as specified in TS23.502[3] clause 4.16.5.

The PCF takes the policy decision based on the information that it has received so far but at this point, the PCF is not yet aware of any dynamic changes in the observed backhaul delay.

Based on the Satellite Backhaul Category, the PCF may indicate SMF to activate QoS monitoring in the PCC rules

5. Since SMF knows based on indication received from the AMF in step 2 that satellite backhaul is used, and/or based on the received PCC rules, the SMF initiates GTP-U path monitoring as specified in clause 5.33.3.3 of TS 23.501 [2], no matter whether the GTP-U path is over a satellite backhaul with dynamical delay.

NOTE 1: The SMF need not request echo procedure for every PDU session of every UE that are served by the same gNB.

6. SMF receives GTP-U path monitoring results indicating the observed delay.

7. Upon receiving the observed delay from the UPF in step 6, the SMF initiates SM Policy Association Modification in order to inform the PCF of the Satellite Backhaul Category and (optionally) the observed delay. The SMF may be configured with margins of the observed delay to determine the actualSatellite Backhaul Category in use to report to PCF.

8. [Conditional] The SMF may inform the CHF of the Satellite Backhaul Category and the observed delay. This information may be used for charging, network statistics and sorting out customer complaints. This step is asynchronous and the SMF can initiate it at any time after having received the delay information at step 6.

NOTE 2: Step 8 can be supported in stage 3 using Charging Data Request / Charging Data Response message.

9. PCF adjusts the QoS policy according to the observed N3 delay. PCF may need to report the delay or Satellite Backhaul category or both to AF for application specific reasons.

### 6.1.3 Impacts on services, entities and interfaces

This solution impacts the following system entities.

SMF:

- Capability to trigger GTP-U path monitoring when satellite backhaul is used.

- Capability to report the observed delay resulting from GTP-U path monitoring to CHF.

PCF:

- If observed delay is reported from SMF, PCF needs to have the capability to receive observed delay and to take it into account for policy control decisions.

It is assumed that OAM can provide the AMF with the satellite backhaul type used between a gNB and the AMF.

## 6.2 Solution for KI#1: QoS control enhancements for dynamic satellite backhauling

### 6.2.1 Description

In Rel-17, only a single satellite backhaul category refers to the type of the satellite (i.e. GEO, MEO, LEO or OTHERSAT) can be indicated.

In Rel-18, the multi-hops ISL or multi-types of backhaul will be considered, for example, as shown in the Figure 6.2.1-1, a gNB may have UP connections each of which is over different satellites. Before establishing UP connection of the PDU session, the AMF may not know what kind of satellite backhaul is used to serve the PDU session. In such case, only a single satellite backhaul category is not enough to describe the dynamic satellite backhaul characteristics.



Figure 6.2.1-1: gNB has multiple satellite backhaul UP connections

Moreover, due to dynamic satellite network topology and distinguished transmission capabilities provided by different type of satellites, statically configured QoS parameters for the PDU session may not always be suitable. Therefore, the QoS control for the case of satellite backhaul needs to be enhanced.

In addition, since the backhaul information (e.g. backhaul delay, backhaul category) can be changed/ adjusted dynamically, the AF may request the backhaul information for application layer optimization or adjustment.

### 6.2.2 Procedures

Figure 6.2.2-1 shows the procedure of the PDU session establishment when gNB has multiple satellite backhaul UP connections.



Figure 6.2.2-1: PDU session establishment when gNB has multiple satellite backhaul UP connections

0. During the procedure of NG setup, the gNB may inform the AMF whether CP connections of this gNB, or UP connections of this gNB or both are over a satellite(s).

1. The UE initiates the PDU Session Establishment procedure by invoking the PDU Session Establishment Request as specified in clause 4.3.2.2 of TS 23.502 [3].

2. The AMF selects the SMF/I-SMF as specified in clause 6.3.2 of TS 23.501 [2] and clause 4.3.2.2.3 of TS 23.502 [3]. If the AMF is aware that the serving gNB uses satellite backhaul UP connections, the AMF may invoke Nsmf\_PDUSession\_CreateSMContext Request to send satellite backhaul information.

- Case 1: if only CP connections of this gNB are over satellite(s), the AMF may not send satellite backhaul information;

- Case 2: If UP connections of this gNB are over a single satellite, the AMF just sends satellite backhaul category indication as defined in Rel-17;

- Case 3: If UP connections of this gNB are over multi-types of satellites or multi-hops of ISL, the AMF notifies the SMF of satellite backhaul information indicating dynamic satellite backhaul in use, and possibly the gNB ID.

The following steps are only applicable to case 3:

3. SMF informs the PCF of the satellite backhaul information by including "dynamic satellite backhaul in use" indication in Npcf\_SMPolicyControl\_Create Request during SM Policy Association Establishment as specified in clause 4.16.4 of TS 23.502 [3].

4. Based on the indication, the PCF generates PCC rules suitable for satellite backhaul, where the PCC rules indicate to activate QoS monitoring. In addition, if downgraded QoS requirements are allowed, the PCF may also provide Alternative QoS Profile for downgraded QoS requirements.

5. The SMF selects the candidate UPF(s) as specified in clause 6.3.3 of TS 23.501 [2]. Based on the received PCC rules, the SMF requests to activate QoS monitoring for the GTP-U path(s) between at least one of the candidates UPF(s) and the (R)AN indicated by the gNB ID via N4 Association Update Request.

6. The candidate UPF(s) confirm to perform the GTP-U path monitoring.

7. If a candidate UPF doesn't activate QoS monitoring for the GTP-U path already, it sends an Echo Request message to the gNB.

8. The gNB responds an Echo Response message that may contain the delay or satellite backhaul category indication to the candidate UPF(s).

9. The candidate UPF(s) sends the QoS monitoring results to the SMF.

10. Upon receiving the QoS monitoring results from the UPF(s) in step 7, the SMF selects the suitable I-UPF and/or PSA UPF, e.g. a UPF with the minimum backhaul latency.

Based on the received QoS monitoring results, the SMF may determine to apply the QoS profile for downgraded QoS requirements, or initiate an SM Policy Association Modification procedure.

The SMF also reports the QoS monitoring results to the PCF. In addition, the SMF may indicate the bandwidth on the N3 interface between the gNB and the selected UPF to the PCF, where the bandwidth is obtained from the satellite system using implantation method, i.e. the interaction between SMF and satellite system will not be standardized in this release.

11. Complete the follow-up PDU session establishment process with the existing steps as specified in clause 4.3.2.2 of TS 23.502 [3].

12. The AF may request to obtain the satellite backhaul information for an AF session using Nnef\_AFsessionWithQoS\_Create request message (satellite backhaul information) to the NEF, e.g., when the AF would like to adjust data transmission strategy.

13. The NEF authorizes the AF request and interacts with the PCF to obtain the satellite backhaul information by invoking Npcf\_PolicyAuthorization\_Create Request.

If the AF is considered to be trusted by the operator, the AF uses the Npcf\_PolicyAuthorization\_Create request message to interact directly with PCF to request satellite backhaul information for an AF session.

14. The PCF exposes the satellite backhaul information (e.g. backhaul delay and/or bandwidth) to the NEF.

15. The NEF exposes the satellite backhaul information to the AF.

If the AF is considered to be trusted by the operator, the PCF sends the Npcf\_PolicyAuthorization\_Create response message (satellite backhaul information) directly to AF.

### 6.2.3 Impacts on services, entities and interfaces

This solution impacts the following system entities.

AMF:

- Capability to send the satellite backhaul UP connections to the SMF.

SMF:

- Capability to trigger GTP-U path monitoring when satellite backhaul is used.

- Capability to report the QoS monitoring results from GTP-U path monitoring to PCF.

PCF:

- Capability to receive satellite backhaul UP connections information and to take it into account for policy control decisions.

- Capability to expose dynamical satellite backhaul information to the NEF.

AF

- Capability to request dynamical satellite backhaul information

NEF

- Capability to expose dynamical satellite backhaul information

gNB:

- Capability to send the satellite backhaul category corresponding to UP connections to the AMF.

NOTE: The gNB impact is to be verified with RAN WGs.

## 6.3 Solution for Key Issue #1: Information of satellite constellation and change of backhaul delay exposed to PCF/AF

### 6.3.1 Description

If the satellite backhaul involves multi-hops of ISL, in some cases, the propagation delay of backhaul paths may change dramatically with the movement of satellite and such kind of change normally be periodic and can be well predicated based on the operation information of satellite constellation.

If a polar-orbit satellite constellation is used and it does not support cross-seam ISLs, the backhaul delay may change dramatically when cross-seam transits or leave. If cross-seam ISLs are supported, there will be frequent ISL handover with the movement of satellites on the different side of the cross-seam, the backhaul delay may not change dramatically, but the delay jitter will be larger due to the frequent handover of ISL.

As the cross-seam transit may last for minutes or even hours (dependent on density of the satellites orbits in the constellation and location of gNB and 5GC), it is worthwhile to report such kind of predictable and crucial event and its lasting time to PCF/AF, e.g. to help them understand that the dramatic packet latency/jitter increase is inevitable over a period time, then AF may start to perform application layer coding compensation or PCF may make a firm decision to release the PDU session if the QoS requirement is not satisfied.

### 6.3.2 Procedures



Figure 6.3.2-1: Information of satellite constellation and change of backhaul delay exposed to PCF/AF

1. AMF reports the satellite constellation information to PCF/AF during the PDU session establishment procedure. Besides the satellite backhaul category indication, AMF also reports the satellite constellation information including 'LEO or MEO polar-orbit satellite constellation with or without cross-seam ISLs supported', if multi-hops of ISLs are involved by a polar-orbit satellite constellation. AMF determines the Satellite constellation information based on local configuration using the same mechanism as defined in TS 23.501 i.e. based on local configuration, for example based on Global RAN Node IDs associated with satellite backhaul.

Editor’s Note: It is for FFS whether need to distinguish whether cross-seam ISLs supported for a polar-orbit satellite constellation.

2. If satellite backhaul with LEO or MEO polar-orbit satellite constellation information is received, AF/PCF requests report of backhaul delay change information based on PCRT mechanism as described in clause 6.1.3.18 of TS 23.503 [4].

3-4. Based on satellite operation information which is a timer including the time when cross-seam transit or leave event starts and stops, AMF determines that backhaul delay will change and reports the delay change information (the time of the event is expected to last) to PCF/AF based on PCRT mechanism as described in clause 4.16.5.1 of TS 23.502 [3] AMF utilizes the Nsmf\_PDUSession\_UpdateSMContext service to report the delay change information to SMF.

NOTE: AMF can obtain the satellite operation information by local configuration or from a satellite operation centre outside the 3GPP domain.

### 6.3.3 Impacts on services, entities and interfaces

This solution impacts the following system entities.

AMF:

- Capability to report polar-orbit satellite constellation information.

- Capability to determine and report of duration time of cross-seam transit or leave event of polar-orbit satellite constellation to PCF and AF.

PCF/AF:

- Capability to ask report of backhaul delay change information if polar-orbit satellite constellation information received.

## 6.4 Solution for Key Issue #2 and Key Issue #3: Enable Satellite Edge Computing or local data switching via on-board UPF acting as UL CL/BP and local PSA

### 6.4.1 Description

This solution corresponds to KI#2 and KI#3.

UE establishes a PDU Session with PSA on ground via GEO satellite backhaul. SMF needs to:

1) determine whether to insert a UL CL/BP on the GEO UPF; and

2) obtain the target IP of traffic to be local routed to configure the traffic steering rule to the GEO UPF (UL CL/BP/local PSA).

### 6.4.2 Procedures

Figure 6.4.2-1 shows the procedure to enable satellite edge computing or local data switching via on-board UPF acting as UL CL/BP and local PSA.



Figure 6.4.2-1: Enabling GEO satellite edge computing via on-board UPF

0. During PDU Session establishment procedure, the AMF determines the GEO satellite ID serving the UE as backhaul and send the GEO satellite ID to the SMF in Nsmf\_PDUSession\_CreateSMContext Request.

NOTE 1: It is assumed that the AMF can determine the GEO satellite ID for the notification to the SMF based on local configuration, e.g. based on Global RAN Node IDs associated with satellite backhaul.

1. SMF determines to insert GEO UPF as UL CL/BP and local PSA with the following triggers:

1a. (For edge computing case) During the PDU Session establishment procedure, SMF determines the UE traffic can be local routed at a DNAI assigned to the GEO satellite based on the following information: 1) UE location, 2) GEO satellite ID, 3) the existing policy from PCF based on AF influenced information on what DNAIs the UE can access to, 4) EAS Deployment Information.

SMF determines the traffic steering rules based on the IP range of the EAS deployed on the GEO UPF.

1b. (For UE-to-UE case) AF initiates UE-to-UE communication for two UEs by providing UE ID/IPs of both UEs to the SMF.

NOTE 2: AF might be triggered by application layer negotiation which is not in the scope of this study.

The SMF determines two UEs are under the same GEO satellite.

If the same SMF is used for the two UEs, the SMF determines whether two UEs are served under the same GEO satellite based on stored correlation between the GEO satellite ID and UE IP/DNN. If the two UEs are under same GEO satellite, then SMF determines the two UEs can be served by the same GEO UPF.

If different SMFs are used for two UEs, the SMF checks whether the two UEs are served by the same GEO satellite via UDM. The SMF retrieves UE IP list corresponding to the GEO satellite from UDM and checks whether the two UEs are included in the UE IP list. If yes, the SMF determines the two UEs are served by the same GEO UPF. The SMF also registers the UE IP/DNN and the GEO satellite ID to the UDM.

When one UE quits the UE-to-UE communication, the SMF is notified by the AF. The SMF initiates PDU Session Modification procedures for both of the UEs to update the traffic steering rules or release the UL CL/BP/local PSA.

SMF determines traffic steering rules for the two UEs based on the target UE IP.

1c. (For edge computing and UE-to-UE case) UE sends UL packet to PSA UPF on ground and the PSA UPF on ground reports related information, e.g. FQDN in DNS query as described in clause 6.2.3 of TS 23.548 [6], target IP, to SMF.

For edge computing case, the SMF determines UE is accessing local services on the GEO UPF via e.g. mechanisms described in clause 6.2.3 of TS 23.548 [6].

For UE-to-UE case, the SMF determines the two UEs, i.e. the source UE and the target UE, are under the same GEO satellite.

SMF determines traffic steering rules based on the target IP address detected and reported by the PSA UPF.

NOTE 1: For step 1a/1b/1c, a DNAI value needs to be assigned by the operator to each GEO satellite, so that existing UPF selection and other EC procedures can be reused to support the local routing on the GEO satellite.

2. SMF selects and inserts the GEO UPF as UL CL/BP and local PSA and sends traffic steering rules to the GEO UPF.

For edge computing case, the traffic steering rules indicate the ULCL/BP to perform local routing for the packets targeting the EC services on the GEO satellite.

For UE-to-UE case, the traffic steering rules indicate the ULCL to perform local routing for the packets to the target UE.

If the GEO satellite does not server the UE anymore due to e.g. UE mobility, the AMF will trigger PDU Session Modification procedure to update the SMF with new (or none) GEO satellite ID/backhaul category. Then the SMF will reconfigure the user plane based on the updated backhaul information as described in step 1 and 2. This may cause ULCL insertion/relocation or removal.

### 6.4.3 Impacts on services, entities and interfaces

AF:

For UE-to-UE case:

- Provide/Update UE ID/IP for UE-to-UE communication to the SMF.

AMF:

* Determines GEO Satellite ID based on local configuration and RAN ID and provides to SMF during PDU Session Establishment/Modification procedures.

SMF:

- Receives GEO Satellite ID from AMF during PDU Session Establishment/Modification procedures.

- Be configured by the operator a DNAI value for each GEO satellite.

For edge computing case:

- Determine whether a ULCL/BP should be inserted on the GEO Satellite.

For UE-to-UE case:

- Determine whether local data switching should be performed for UEs served by same GEO satellite based on AF request or PSA UPF reporting.

- Interact with UDM to check whether two UEs are served by same GEO satellite in case of different SMFs serving UEs in communication.

UDM:

For UE-to-UE case, when different SMFs are used:

- Receive and store GEO Satellite ID and UE IP/DNN from SMF.

## 6.5 Solution for KI#2: Support of Satellite Edge Computing via UPF on board

### 6.5.1 Description

As states in TS 23.548 [6]: "The Edge Computing enables operator and 3rd party services to be hosted close to the UE's access point of attachment, so as to achieve an efficient service delivery through the reduced end-to-end latency and load on the transport network". In Rel-18, in order to enable GEO satellite edge computing, a UPF can be deployed on the satellite. The following figure shows the high level architecture of the Satellite Edge Computing via UPF on board.



Figure 6.5.1-1: Satellite Edge Computing via UPF on-board

Based on the existing Edge Computing(EC) specification, for providing the application service timely, the Edge Application Servers(EAS) can be deployed on-board and connected to the UPF on-board via a N6 interface. As specified in clause 6.2.3 of TS 23.548 [6], in order to start the EC application service, the UE can initiate the EAS discovery procedure which can discover the IP address(es) of the EAS using Domain Name System (DNS). Therefore, if the EAS can be selected by the UE, the UPF on-board can also be selected to support the Satellite Edge Computing service.

As specified in clause 5.2.1 of TS 23.548 [6], the Edge DNS Client (EDC) functionality in UE ensures that DNS requests from applications are sent to the DNS Server's (e.g. EASDF/DNS resolver) IP address received from the SMF and can ensure the usage of the EAS discovery procedure. If a UE without EDC functionality, it can also use the EAS (re-)discovery functionalities provided by EASDF but cannot be ensured. As specified in clause 5.1.1 of TS 23.548 [6], according to the instruction from the SMF, the Edge Application Server Discovery Function (EASDF) can forward the DNS messages to the DNS server which can resolve the IP address(es) of the EAS. Due to the SMF and the DNS server are all deployed on the ground, the EASDF can also be deployed on the ground.

As specified in clause 6.2.3.2 of TS 23.548 [6], due to the IP address(es) of the EAS needs to be resolved by the DNS server that is on the ground first, a PDU session with the UPF on the ground needs to be established. Then, based on the UE's subscription data, UE location, the information from Application Function (AF), the EAS information reported from EASDF, the SMF may select the target DNAI and trigger UL CL/BP and L-PSA insertion.

For the Satellite Edge Computing case, the SMF has to select a UL CL/BP and a L-PSA on the satellite serving a gNB, e.g. taking the identity of the satellite serving the gNB into account to select a UPF on-board.

As specified in clause 5.13 of TS 23.501[2], the UPF can be selected by the SMF based on the DNAI. The DNAI may correspond to multiple UPFs on-board. However, the satellites that deploying the selected UPF may not be able to provide the satellite backhaul service to the gNB serving the UE.

The connectable gNB IDs/IPs are proposed to be included in the UPF profile. Based on the UPF profile and the gNB serving the UE, the SMF can select the UPF on-board that can provide the satellite backhaul service to the gNB serving the UE.

When a GTP-U path is activated (echo request/response) between gNB and UPF on-board, the UPF on-board can know the gNB IP address. If UPF profile includes gNB ID, then the UPF on-board needs to be configured with the mapping between gNB ID and the gNB IP, so that the UPF can report gNB ID to the SMF via N4 node level procedure, e.g. N4 report procedure. The UPFs are assumed to be configured with the possible gNB IP addresses so that UPF can initiate GTP-U path monitoring towards this gNBs using echo request/response.

### 6.5.2 Procedures

Figure 6.5.2-1 shows the procedure of EAS(UPF on-board) discovery procedure with EASDF.



Figure 6.5.2-1: EAS(UPF on-board) discovery procedure with EASDF

0. During the procedure of NG setup, the gNB may inform the AMF of satellite backhaul information and the gNB ID.

1. The UE initiates the PDU Session Establishment procedure by invoking the PDU Session Establishment Request as specified in clause 4.3.2.2 of TS 23.502 [3]. If the AMF is aware that the serving gNB uses satellite backhaul UP connections, the AMF invokes Nsmf\_PDUSession\_CreateSMContext Request to send satellite backhaul UP connections information and the gNB ID. The SMF retrieves the UE subscription information from the UDM (which may optionally include an indication on UE authorization for EAS discovery via EASDF) and checks if the UE is authorized to discover the EAS via EASDF. If not authorized, this procedure is terminated.

2. Based on the UE subscription information, the SMF selects EASDF as described in clause 6.3 of TS 23.501 [2].

3. The SMF invokes Neasdf\_DNSContext\_Create/Update Request (UE IP address, SUPI, DNN, notification endpoint, (DNS message handling rules)) to the selected EASDF as specified in clause 6.2.3.2.2 of TS 23.548 [6].

4. The EASDF invokes Neasdf\_DNSContext\_Create/Update Response (IP address of the EASDF) to the SMF.

5. The Application in the UE uses the EDC functionality as described in TS 23.548 [6] clause 6.2.4 sends the DNS Query to the EASDF.

6. The EASDF handles the DNS Query message received from the UE as specified in clause 6.2.3.2.2 step 12 of TS 23.548 [6].

7. The EASDF sends the EAS IP addresses which are determined by the DNS system to the SMF as specified in clause 6.2.3.2.2 of TS 23.548 [6].

8. The SMF selects a UL CL/BP and Local PSA on-board.

Based on the EAS information received from the EASDF, UPF selection criteria, and possibly Service Experience or DN performance analytics for an Edge Application, the SMF may determine the DNAI and determine the associated N6 traffic routing information for the DNAI.

The SMF may utilize the NRF to obtain the UPF profile(s), or, the SMF may obtain the UPF profile(s) from the UPFs associated with the DNAI via N4 node level procedure, e.g. N4 report, where each UPF profile includes one or more gNB IDs/IPs which is connecting with the UPF on-board. Based on the UPF profile and the gNB ID received from the AMF, the SMF determines the UL CL/BP and Local PSA on-board.

Note: The UL CL/BP and L-PSA on the satellite are combined in this release of the specification.

9. The SMF inserts UL CL/BP and Local PSA as described in TS 23.502 [3].

10. The EASDF sends the DNS Response(s) to the UE if it is indicated to send the buffered DNS response(s) to UE.

### 6.5.3 Impacts on services, entities and interfaces

This solution impacts the following system entities.

SMF:

- Capability to determine UL CL/BP and Local PSA on-board which has connection with the gNB serving the UE.

UPF:

- Configure the connectable gNB ID list or gNB IP range in the UPF profile.

## 6.6 Solution for Key Issue #2 and Key Issue #3: Enable on-board EC or local data switch based on GEO PSA UPF

### 6.6.1 Description

This solution resolves the Key Issue #3 to support local data switch for UEs in a communication when they are served by PSA UPF on-board. This solution also resolves the Key Issue #2 to support satellite edge computing via PSA UPF on board.

For the case a UE communicates with another UE directly via 5GC without preconfigured VN Group association, e.g. via point-to-point application and protocols, the existing 5G LAN local switch cannot be reused. In this case, especially for the scenario that UPF is deployed on GEO satellite with gNB on the ground, on-board local data switch would be very beneficial to reduce end-to-end latency. This solution proposes a UPF-level session based approach to support local data switch.

In this solution, the on-board UPF is a PSA UPF and it is assumed that a single SMF is used.. UE establishes a PDU Session with the GEO UPF acting as PSA.

UE initiates PDU Session Establishment procedure based on URSP rules and sends DNN/S-NSSAI to AMF as described in clause 4.3.2 of TS 23.502 [3]. SMF selects GEO UPF as the PDU Session anchor based on the DNN/S-NSSAI sent by AMF. PCF determines the URSP rules based on GEO satellite backhaul category from AMF and send it to the UE including DNN/S-NSSAI for services deployed in GEO satellite or UE-to-UE services. The N4 rules of the UPF-level session applies to the DNN/S-NSSAI.

After the PDU Session Establishment, the UE can access to the edge computing services deployed on the satellite via normal N6 routing.

### 6.6.2 Procedures

To support UE-UE local data switch via UPF on board, the following procedure is performed:



Figure 6.6.2-1: High-level procedure for UPF-level N4 session solution

1. The SMF gets all on-board UPFs' address pools information per DNN and creates address mapping information based on these on-board UPFs' address pools information. The address mapping information is for traffic routing between on-board UPFs. The address mapping information includes UE IP address range and next UPF information corresponding to the address range.

2. The SMF creates a UPF-level N4 session on the on-board UPFs, i.e. UPF1 and UPF2. During the corresponding UPF-level N4 sessions establishment, the SMF provides N4 rules, which including several PDR and FAR pairs.

One PDR and FAR pair includes:

- a PDR detecting that the destination address is in the current UPF address pool; and

- a FAR instructing the UPF to forward the traffic to the UPF internal interface.

One PDR and FAR pair per UPF (excluding current UPF) includes:

- a PDR detecting that the destination address is in the another UPF address pool; and

- a FAR instructing the UPF to add an outer header (e.g. address information of next UPF) and forward the traffic to the next UPF.

3. The UE1, UE2 and UE3 establish PDU sessions. The UE1 and UE2 are served by UPF1. The UE3 is served by UPF2. During corresponding N4 sessions establishment, the SMF provides N4 rules to instruct the UPF forwarding the user plane packet from UPF internal interface to the target UE.

4. The UE1 sends data to the UE2. Upon receipt of a user plane packet, the UPF1 forwards the packet based the UPF1 address pool and the destination address of the packet. The UPF1 handles the packet as follows:

- identify the UPF-level N4 session is the first N4 session to which the packet corresponds;

- determines that the destination address is in the UPF1 address pool and then forward the packet to the UPF internal interface;

- the packet will match the N4 session corresponding to the UE2's PDU session; and

- the packet is then forwarded to the UE2.

5. The UE1 sends data to the UE3. Upon receipt of a user plane packet, the UPF1 forwards the packet based the UPF1 address pool and the destination address of the packet. The packet would be handled as follows:

- the UPF1 identifies the UPF-level N4 session is the first N4 session to which the packet corresponds;

- the UPF2 determines that the destination address is out of the UPF1 address pool and then forwards the packet to UPF2 based on the address mapping information in the corresponding FAR, in which case the destination address is in the address range of one term of address mapping information and the corresponding next UPF is the UPF2; and

- the UPF2 identifies the UPF-level N4 session is the first N4 session to which the packet corresponds;

- the UPF2 determines that the destination address is in the UPF2 address pool and then forward the packet to the UPF internal interface;

- the packet will match the N4 session corresponding to the UE3's PDU session; and

- the packet is then forwarded to the UE3.

### 6.6.3 Impacts on services, entities and interfaces

This solution impacts the following system entities.

AMF:

- Send satellite backhaul category to PCF.

PCF:

- Determine UE policy based on satellite backhaul category.

The following impacts are for UE-to-UE local data switch only:

SMF:

- Request UPF to establish UPF-level N4 session.

- Provides UPF N4 rules to enable local data switch.

UPF:

- Establish a UPF-level N4 session.

- Implement local data switch based on received N4 rules.

## 6.7 Solution for KI#3: Support of Local Data Switching via UPF on board

### 6.7.1 Description

As specified in TS 23.501 [2], for UEs belong to the same enterprise or organization, and if they belong to the same 5G VN group, 5G LAN-type services can be applied among them.

For UEs in a communication that are served by satellite backhaul, if local data switching via UPF on-board can be enabled, then the communication path between two UEs can be significantly shorten by avoiding using ISL and feeder link on the way towards the PSA on the ground. If some UEs are served by satellite backhaul and if they are closing to each other, local data switching via a UPF on-board for system efficiency and QoE improvement can be achieved as shown in the Figure 6.7.1-1. If UEs are served by different satellites, in order to enable the local data switching between them, N19 forwarding between UPFs on-board should be supported as shown in the Figure 6.7.1-2. The UPF on-board can be configured to send usage report for traffic subject to local data switching to the SMF on the ground.

NOTE: It is assumed that two UEs are served by same SMF while enabling local data switching, and for data subject to local data switching, same QoS treatment is applied on both UE sides.



Figure 6.7.1-1: Local Data Switching via a UPF on-board



Figure 6.7.1-2: Local Data Switching via multiple UPFs on-board

The possible interactions via the satellite backhaul between UEs are shown in the Figure 6.7.1-3. The Local Data Switching via a UPF on-board is shown as the blue line. The Local Data Switching via multiple UPFs on-board is shown as the red line. The Local Data Switching via the PSA UPF is shown as the green line.



Figure 6.7.1-3: Local Data Switching via multiple UPFs on-board

In order to reduce end to end delay comparing with existing 5G LAN local switch at PSA on the ground, the method of how the UPF on-board can be selected by the SMF to support the 5G LAN-type services needs to be achieved.

### 6.7.2 Procedures

Figure 6.7.2-1 shows the procedure of the PDU session establishment between UEs served by the UPF on-board in a communication.



Figure 6.7.2-1: PDU session establishment between UEs served by the UPF on-board.

0. During the procedure of NG setup, the gNB may inform the AMF of satellite backhaul information and the gNB ID.

1. UE1 initiates the PDU Session Establishment procedure by invoking the PDU Session Establishment Request (DNN, S-NSSAI, PDU Session Type) as specified in clause 4.3.2.2 of TS 23.502 [3].

2. If the DNN/S-NSSAI obtained from the AMF is associated with a 5G VN group, a dedicated SMF is to be selected as specified in clause 5.29.3 of TS 23.501 [2]. The SMF retrieves the UE subscription information from the UDM (which may optionally include the VN group ID).

If the AMF is aware that the serving gNB uses satellite backhaul UP connections, the AMF may invoke Nsmf\_PDUSession\_CreateSMContext Request to send satellite backhaul information and the gNB ID.

3. Based on the DNN and backhaul information, the SMF determines whether to insert an I-UPF on-board to activate local data switching.

NOTE: If there are no other PDU sessions established over satellite backhaul for this VN group, the SMF may decide to not select an I-UPF on-board to enable local data switching.

4. The SMF selects the PSA UPF on the ground and possibly a I-UPF on-board.

5. The PDU session is established for UE1.

6. UE2 initiates the PDU Session Establishment procedure by invoking the PDU Session Establishment Request (DNN, S-NSSAI, PDU Session Type) as specified in clause 4.3.2.2 of TS 23.502 [3].

7. If the DNN/S-NSSAI obtained from the AMF is associated with a 5G VN group, a dedicated SMF is to be selected as specified in clause 5.29.3 of TS 23.501 [2]. The SMF retrieves the UE subscription information from the UDM (which may optionally include the VN group ID).

If the AMF is aware that the serving gNB uses satellite backhaul UP connections, the AMF may invoke Nsmf\_PDUSession\_CreateSMContext Request to send satellite backhaul information and the gNB ID.

8. Based on the DNN and backhaul information and existing PDU sessions for the VN group, the SMF determines to insert an I-UPF on-board to activate local data switching.

9. The SMF selects the PSA UPF on the ground and an I-UPF on-board.

The SMF may utilize the NRF to obtain the I-UPF profile(s), or, the SMF may obtain the I-UPF profile(s) from the UPFs associated with the DNN by via N4 Node Level Procedure, e.g. N4 report procedure, where each I-UPF profile includes one or more gNB IDs/IPs that the I-UPF currently connects. Based on the UPF profile and the gNB ID received from AMF, the SMF determines the I-UPF on-board.

10. The SMF confirms to initiate the N4 Session Establishment including the PDR and FAR to the I-UPF on-board serving the PDU session 2 to enable local data switching. If both of UE1 and UE2 are served by satellite backhaul via the same GEO UPF1 on-board, the SMF will enable local switch via UPF1 on board the GEO satellite. If the UE1 and UE2 are served by satellite backhaul via different GEO UPFs on-board, the SMF will establish N19 tunnels between GEO UPFs on-board to enable local data switching.

The PDR and FAR indicates that, all UL traffic towards group members (identified by destination IP addresses) served by UPF(s) on-board will be forwarded via I-UPF to the gNB or other I-UPFs, and all DL traffic towards this UE (identified by the destination IP address) will be forwarded to the gNB via N3 tunnel.

To enable unicast traffic forwarding in a UPF, the following applies:

- The SMF provides for each 5G VN group member's N4 Session (i.e. N4 Session corresponding to PDU Session) the following N4 rules that enable the processing of packets received from this UE.

- in order to detect the traffic, a PDR containing Source Interface set to "access side", and CN Tunnel Information set to PDU Session tunnel header (i.e. N3 or N9 GTP-U F-TEID); and

- in order to forward the traffic, a FAR containing Destination Interface set to "5G VN internal".

- The SMF provides for each 5G VN group member's N4 Session (i.e. N4 session corresponding to PDU Session) the following N4 rules that enable the processing of packets towards this UE.

- in order to detect the traffic, a PDR containing Source Interface set to "5G VN internal", and Destination Address set to the IP/MAC address (es) of this 5G VN group member; and

- in order to forward the traffic, a FAR containing Outer Header Creation indicating the N3/N9 tunnel information, and Destination Interface set "access side".

- If N19-based forwarding is applied, the SMF configures the group-level N4 Session for processing packets received from a N19 tunnel with the following N4 rules for each N19 tunnel.

- in order to detect the traffic, a PDR containing Source Interface set to "core side", and CN Tunnel Information set to N19 tunnel header (i.e. N19 GTP-U F-TEID); and

- in order to forward the traffic, a FAR containing Destination Interface set to "5G VN internal".

- If N19-based forwarding is applied, the SMF configures the group-level N4 Session for processing packets towards 5G VN group members with the following N4 rules for each N19 tunnel.

- in order to detect the traffic, a PDR containing Source Interface set to "5G VN internal", and Destination Address set to the IP/MAC address (es) of UEs of this N19 tunnel; and

- in order to forward the traffic to a 5G VN group member via the N19 tunnel, a FAR containing Outer Header Creation indicating the N19 tunnel information, Destination Interface set to " access side".

To enable broadcast traffic forwarding of a 5G VN group in a UPF, the following applies:

- The SMF provides for each 5G VN group member' N4 Session (i.e. N4 session corresponding to PDU Session) the following N4 rules that enable the processing of broadcast packets towards this UE.

- in order to detect the traffic, a PDR containing Source Interface set to "5G VN internal", Destination Address set to the broadcast address, the Packet replication skip information set to the IP/MAC address (es) of this 5G VN group member, and the indication to carry on matching; and

- in order to forward the traffic, a FAR containing Outer Header Creation indicating the PDU Session tunnel information, and Destination Interface set "access side".

- The SMF configures the group-level N4 Session for processing packets received from a N19 tunnel with the following N4 rules for each N19 tunnel.

- in order to detect the traffic, a PDR containing Source Interface set to "core side", Destination Address set to the broadcast address, and CN Tunnel Information set to N19 tunnel header (i.e. N19 GTP-U TEID); and

- in order to forward the traffic, a FAR containing Destination Interface set to "5G VN internal", Outer Header Creation with the N19 indication.

- The SMF provides for the group-level N4 Session the following N4 rules that enable the processing of broadcast packets towards the other UPFs.

- in order to detect the traffic, a PDR containing Source Interface set to "5G VN internal", Destination Address set to the broadcast address, the Packet replication skip information set to the N19 indication, and the indication to carry on matching; and

- in order to forward the traffic to each involved UPF via the corresponding N19 tunnel, a FAR containing "Duplication" instruction, Outer Header Creation indicating the N19 tunnel information, Destination Interface set to "core side".

For any SDF subject to local data switching, the SMF may provide particular reporting rules to the I-UPF on-board for minimization of N4 signalling exchange.

11. The PDU session is established for UE2.

12. The SMF triggers to select an I-UPF on-board for PDU session1 to enable local data switching between UEs served by UPF on-board.

13. The SMF initiates the N4 Session Modification including PDR and FAR to the UPF on-board serving the PDU session 1 to enable local data switching.

### 6.7.3 Impacts on services, entities and interfaces

This solution impacts the following system entities.

AMF:

- Capability to send the satellite backhaul UP connections to the SMF.

SMF:

- Capability to determine whether to insert an I-UPF on-board to activate local data switching based on DNN and backhaul information.

- Capability to generate specific PDR and FAR to enable local data switching between UEs.

UPF:

- Configure the connectable gNB ID list or gNB IP range in the UPF profile.

## 6.8 Solution for Key Issue #1: In-sequence delivery

### 6.8.1 Description

When backhaul between gNB and UPF involves satellite, the inter satellite link may switch due to the satellite movement. This handover of transmission path may happen without UE mobility, caused by the transport network itself and usually is not perceived by 5GC, which will cause performance decline and user experience degradation, especially for TCP-based applications.

The following solution is proposed to solve the packet out-of-sequence issue introduced by dynamic satellite backhaul:

For a non 5G LAN PDU session:



1. The backhaul type is indicated to SMF by AMF.

2. Based on the service requirements/type mapped to a QoS flow, if backhaul involves LEO/MEO satellite(s), the SMF decides to initiate the in-order-delivery for the QoS flow.

3. During PDU Session establishment, or during mobility/handover procedure, the SMF indicates the UPF and gNB, which are all located on ground, to enable Sequence number based in order delivery for the QoS flow:

For uplink traffic:

- The gNB adds the GTP-U sequence number for the QoS flow according to the PDCP order of the received packets for this QoS flow.

- The UPF delivers the packets in order based on GTP-U sequence number. The UPF monitors the sequence and initiates timer to wait out of sequence packets.

For downlink traffic:

- The UPF adds the GTP-U sequence number for the QoS flow according to packet order received from DN.

- The gNB delivers the packets in order based on GTP-U sequence number. The gNB monitors the sequence and initiates timer to wait out of sequence packets.

For a 5G LAN PDU session:



The UE1 establishes a 5G LAN PDU session which is anchored at UPF1, and uses this PDU Session to send packets to UE2 and UE3, anchored at UPF2 and UPF3. When the UE1 maps packets sent to UE2 and UE3 into the same QoS flow, the QoS flow level based in order delivery mechanism described above for a non 5G LAN PDU session will not work, since the GTP-U SN received at UPF2 and UPF3 will not be in sequence. For example, if UE1 sends the first packet to UE2, the second packet to UE3, the third packet to UE2 and the forth packet to UE3, then the UPF3 may receive two packets with #N+2 and #N+4 and UPF2 may receive two packets with #N+1 and #N+3. UPF2 cannot determine whether there is a packet with number #N+2 sent to it but lost or still on the path. UPF3 has the same issue.

In order to solve this issue, the GTP-U SN is removed over N19 tunnel. Since UPFs are located on ground, the transport links between UPFs are regarded stable. The UE1’s gNB and UPF1 guarantees the in-sequence delivery of packets between UE1’s gNB and UPF1, and UE2’s gNB and UPF2 guarantees the in-sequence delivery of packets between UE2’s gNB and UPF2.

The in order delivery mechanism described above for a non 5G LAN PDU is thus enhanced:

- The SMF indicates the UPF to remove the GTP-U SN of the packets of a 5G LAN PDU Session, before deliver it to internal interface.

- The SMF indicates the UPF to add GTP-U SN to packets received from N19 tunnel before sending to gNB.

In summary:

The out-of-order problem is introduced by dynamic satellite links, thus SMF needs the satellite backhaul category information to ‘active’ the sequence number.

For 5G-LAN N19 tunnel on ground in this scenario, SMF should not ‘active’ the sequence number.

Editor’s Note: It is FSS whether N19 over satellite links (i.e., GEO inter-satellite links) has the problem of out-of-order and needs a solution.

### 6.8.2 Void

### 6.8.3 Impacts on services, entities and interfaces

gNB:

- Support SN based in-sequence delivery.

SMF:

- Support enabling SN based in-sequence delivery. For 5G LAN, SMF indicates UPF to remove SN when transferring packets via N19 tunnel, and add SN before sending via N3 tunnel.

UPF:

- Support SN based in-sequence delivery.

- For 5G LAN case, remove GTP-U SN when transferring packets over N19.

## 6.9 Solution for Key Issue #1: QoS Monitoring for dynamic satellite backhaul delay control

### 6.9.1 Description

In Rel-17, the single satellite backhaul network is used and the AMF reports to the SMF the satellite backhaul category and the change of satellite backhaul category, as specified in clause 5.8.2.15 of TS 23.501 [2].



Figure 6.9.1-1: Example scenarios of satellite backhaul network with dynamic delay

As example scenarios depicted above, the RAN may use one or more type of backhaul networks with the 5GC, and also the RAN may use different type of backhaul networks in CP and UP which is differed with the single satellite backhaul network assumed in Rel-17.

In order to adapt Policy/QoS control for dynamic delay in satellite backhaul network used in UP, the QoS monitoring over GTP-U path between RAN and UPF is required. For efficient and precise monitoring, the PCF needs to generate the appropriate QoS Monitoring Policy and needs to adjust the PCC rules based on the monitoring results in time.

### 6.9.2 Procedures

Figure 6.9.2-1 below depicts the key steps of the solution, which enables the QoS monitoring for dynamic satellite backhaul delay control.



Figure 6.9.2-1: Procedure for enabling QoS monitoring for dynamic satellite backhaul delay control

1. The UE initiates the PDU Session Establishment procedure as specified in clause 4.3.2.2 of TS 23.502 [3].
2. The AMF determines the Satellite backhaul category (as specified in clause 4.3.2.2 of TS 23.502 [3]), and the following criteria of the network:

Criteria #1: whether more than one type of backhaul networks can be used with the NG-RAN.

Criteria #2: whether different backhaul networks can be used in the CP and the UP at the same time

If the AMF determines that the more than one type of backhaul networks can be used with the NG-RAN, or different backhaul networks can be used in the CP and the UP at the same time, or both, the AMF informs to the SMF that the backhaul network delay is dynamically change by providing ‘dynamic satellite backhaul delay control request’ in Nsmf\_PDU\_Session\_CreateSMContext Request.

The AMF provides ‘dynamic satellite backhaul delay’ even when the satellite backhaul network is not used in the CP, if more than one type of backhaul networks can be used or if different type of backhaul network can be used in the UP.

The AMF determines the above criteria based on the RAN ID (e.g., Global RAN Node ID), or its configuration.

1. The SMF initiates SM Policy Association establishment with the PCF. The SMF provides Satellite backhaul category, and/or dynamic satellite backhaul delay control request to the PCF, if it received from the AMF.
2. The PCF generates and provides to the SMF, the PCC rules with the Policy Control Request Trigger. In the Policy Control Request Trigger, the PCF requests to the SMF to interact again when the SMF selects an UPF for the PDU Session by performing GTP-U path monitoring in the available UPFs, and it is aware of the QoS(s) fulfilled in the selected UPF.

Editor's note: It is FFS how the PCF requests to the SMF to inform the QoSs which can be fulfilled in the UPF before UPF selection. The proper name of parameters can be further studied.

1. The SMF initiates GTP-U path monitoring as specified in clause 5.33.3.3 of TS 23.501 [2] with the available UPFs. Based on the measured backhaul delay received from the available UPFs and the PCC rules received from the PCF, the SMF selects an UPF for the PDU Session.
2. After UPF selection, the SMF verifies the QoS rule(s) fulfilled in the UPF (e.g. the measured backhaul delay received from the UPF is fulfilled the CN PDB), and initiates SM Policy Association modification with the PCF due to the PCRT received in step 3 is met.
3. Based on received backhaul network delay measurement information, the PCF evaluates the provided PCC rules and decides whether to adjust the PCC rules. The PCF provides PCC rules (if it needs to be updated), and the Policy Control Request Trigger of ‘QoS Monitoring information for dynamic satellite backhaul delay control’ information. This ‘QoS Monitoring information for dynamic satellite backhaul delay control’ information includes the information in ‘QoS Monitoring for URLLC’ as specified in Table 6.3.1 of TS 23.503 [4], and may provide additionally ‘Threshold Values’. According this information, the SMF reports to the PCF when the backhaul network delay exceeds the threshold value.

Editor's note: It is FFS whether and how the measured delay can be reported to PCF by event triggered based.

1. SMF performs N4 Session Establishment/Modification as specified in clause 4.3.2.2 of TS 23.502 [3].
2. SMF provides to the RAN, the QoS Monitoring Indication, QoS Monitoring reporting frequency, and QoS Monitoring Threshold value, which are derived from the PCC rule information received in step 7, via AMF by invoking Namf\_Communication\_N1N2Message Transfer.
3. The AMF sends N2 PDU Session Request to the RAN as specified in clause 4.3.2.2 of TS 23.502 [3]..
4. The RAN setups AN-specific resources with the UE as specified in clause 4.3.2.2 of TS 23.502 [3].
5. The RAN indicates its rejection to perform QoS Monitoring, e.g. due to RAN load condition, if any. The SMF is responsible to ensure the QoS Monitoring for satellite backhaul network delay between the RAN and the UPF. If SMF determines that there are no other PDU Sessions that use the same backhaul network on this RAN and UPF, then the SMF concludes that this backhaul network cannot be monitored in the RAN side.
6. The AMF sends Nsmf\_PDUSession\_UpdateSMContext Request to the SMF.
7. The SMF initiates N4 Session Modification with the UPF and provides QoS Monitoring Policy for dynamic satellite backhaul delay control, which are derived from the PCC rule information received in step 7.
8. The SMF sends Nsmf\_PDUSession\_UpdateSMContext Response as specified in clause 4.3.2.2 of TS 23.502 [3].
9. Optionally, if the SMF concluded that the backhaul network cannot be monitored in the RAN side (as described in step 12), and it is configured that the satellite backhaul network monitoring in both RAN and UPF side is mandatory, then the SMF informs the AMF by invoking Nsmf\_PDUSession\_SMContextStatusNotify (Release), and related steps are performed as specified in clause 4.3.2.2 of TS 23.502 [3].

### 6.9.3 Impacts on services, entities and interfaces

AMF:

- During the PDU Session Establishment procedure, determines whether more than one type of backhaul networks can be used with the RAN, and whether the different type of backhaul networks can be used in CP and UP.

- Indicates to the SMF that the satellite backhaul network with dynamic delay can be used with the RAN during the PDU Session Establishment procedure.

SMF:

- Upon receiving dynamic satellite backhaul delay control request from the AMF, forwards the request to PCF.

- Derives the information of QoS Monitoring for dynamic satellite backhaul delay control for RAN and UPF based on the PCC rule information provided by the PCF.

- Initiates the GTP-U path monitoring upon receiving dynamic satellite backhaul delay control request from the AMF.

- During the PDU Session Establishment procedure, selects the UPF based on the GTP-U path minoring results received from the available UPFs.

PCF:

- Upon receiving dynamic satellite backhaul delay control request from the SMF, generates PCC rule information for QoS Monitoring for the satellite backhaul with dynamic delay, and the Policy Control Request Triggers for the SMF.

## 6.10 Solution for Key Issue #2: Enable Satellite EAS re-discovery and re-allocation by means of local DNS

### 6.10.1 Description

This solution corresponds to KI#2.

UE has established a PDU Session with the local PSA on a GEO satellite and with the corresponding EAS. The procedure described below covers the cases when the local EAS on satellite needs to be changed to another local EAS on the same satellite or when the local EAS on one satellite is substituted with another local EAS on another satellite due to the mobility of the gNB.

### 6.10.2 Procedures

Figure 6.10.2-1 shows the procedure to enable changes of EAS by means of local DNS located on the satellite.



Figure 6.10.2-1: Enabling EAS re-discovery or EAS re-selection by means of a local DNS

1. A change from one EAS to another EAS can be performed by using local DNS. The local DNS needs to be aware of various EAS located in the satellite or in the neighbouring GEO satellites. This information is provided during the PDU session establishment procedure by the SMF located on the ground. By storing this information on board satellite a switch from one EAS to another can be performed without SMF intervention and saves the backhauling resources accordingly. After the EAS change the local DNS only reports this change to the SMF.

### 6.10.3 Impacts on services, entities and interfaces

SMF:

- Update the procedure such that SMF stores the info on the L-DNS located on a GEO satellite about the EAS that provide the same application services and are can be used as alternatives for the currently used EASs..

- L-DNS should be able to receive and store information about the EAS on neighboring GEO Satellites.

## 6.X Solution for Key Issue #X: <Solution Title>

### 6.X.1 Description

Editor's note: This clause will describe the solution principles and architecture assumptions for corresponding key issue(s). (Sub-) clause(s) may be added to capture details.

### 6.X.2 Procedures

Editor's note: This clause describes services and related procedures for the solution.

### 6.X.3 Impacts on services, entities and interfaces

Editor's note: This clause captures impacts on existing services, entities and interfaces.

# 7 Overall Evaluation

Editor's note: This clause will provide evaluation of different solutions.

# 8 Conclusions

Editor's note: This clause will list conclusions that have been agreed during the course of the study item activities.

Annex A:  
Change history

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Change history | | | | | | | |
| Date | Meeting | TDoc | CR | Rev | Cat | Subject/Comment | New version |
| 2022-02 | SA2#149 | S2-2200380 | - | - | - | Proposed skeleton agreed at SA2#149e | 0.0.0 |
| 2022-02 | SA2#149 | S2-2201593 | - | - | - | Scope of FS\_5GSATB. | 0.1.0 |
| 2022-02 | SA2#149 | S2-2201594 | - | - | - | Architectural assumptions of FS\_5GSATB. | 0.1.0 |
| 2022-02 | SA2#149 | S2-2201595 | - | - | - | Key Issues on support of satellite edge computing via UPF on board and support of local data switching via UPF on-board. | 0.1.0 |
| 2022-02 | SA2#149 | S2-2201596 | - | - | - | Key issue on PCC/QoS control enhancement considering dynamic satellite backhaul. | 0.1.0 |
| 2022-02 | SA2#149 | S2-2201597 | - | - | - | Dynamic delay solution for key issue#1. | 0.1.0 |
| 2022-04 | SA2#150 | S2-2202586 | - | - | - | Solution for KI#1: QoS control enhancements for dynamic satellite backhauling. | 0.2.0 |
| 2022-04 | SA2#150 | S2-2203307 | - | - | - | Update KI#1 to cover packet out-of-sequence problems. | 0.2.0 |
| 2022-04 | SA2#150 | S2-2203308 | - | - | - | Update on Solution#1 to support multiple satellite backhaul. | 0.2.0 |
| 2022-04 | SA2#150 | S2-2203309 | - | - | - | Solution for Key Issue #1: Information of satellite constellation and change of backhaul delay exposed to PCF/AF. | 0.2.0 |
| 2022-04 | SA2#150 | S2-2203310 | - | - | - | Update of solution#1: Dynamic delay solution enhancement. | 0.2.0 |
| 2022-04 | SA2#150 | S2-2203311 | - | - | - | Solution for KI#2 and KI#3: Enable Satellite Edge Computing or Local Data Switching via on-board UPF acting as ULCL/BP and local PSA | 0.2.0 |
| 2022-04 | SA2#150 | S2-2203312 | - | - | - | Solution for KI#2: Support of Satellite Edge Computing via UPF on board. | 0.2.0 |
| 2022-04 | SA2#150 | S2-2203313 | - | - | - | Solution for Key Issue #3: Enable on-board local data switch based on UPF-level N4 sessions. | 0.2.0 |
| 2022-04 | SA2#150 | S2-2203314 | - | - | - | Solution for KI#3: Support of Local Data Switching via UPF on-board. | 0.2.0 |
| 2022-05 | SA2#151 | S2-2204177 | - | - | - | Update architecture assumption to cover bandwidth detection. | 0.3.0 |
| 2022-05 | SA2#151 | S2-2205018 | - | - | - | Update solution#1 to clarify the generation of QoS monitoring policies | 0.3.0 |
| 2022-05 | SA2#151 | S2-2205019 | - | - | - | New solution for KI#1: in order of packet delivery with dynamic satellite backhaul links. | 0.3.0 |
| 2022-05 | SA2#151 | S2-2205020 | - | - | - | Update to solution#3: Clarification on delay change information and satellite operation information. | 0.3.0 |
| 2022-05 | SA2#151 | S2-2205021 | - | - | - | Update of solution #1 to reduce the impacts to PCF. | 0.3.0 |
| 2022-05 | SA2#151 | S2-2205022 | - | - | - | New solution for KI#1: QoS Monitoring for dynamic satellite backhaul delay control | 0.3.0 |
| 2022-05 | SA2#151 | S2-2205023 | - | - | - | Update of Solution#2 to expose dynamic satellite backhaul information. | 0.3.0 |
| 2022-05 | SA2#151 | S2-2205024 | - | - | - | Update of solution#4 to remove ENs.. | 0.3.0 |
| 2022-05 | SA2#151 | S2-2205025 | - | - | - | Update of Solution#6 to solve ENs. | 0.3.0 |
| 2022-05 | SA2#151 | S2-2205026 | - | - | - | Update of Solution#5 to remove ENs. | 0.3.0 |
| 2022-05 | SA2#151 | S2-2205027 | - | - | - | New Solution for KI#2: Enable Satellite EAS re-discovery and re-allocation by means of local DNS. | 0.3.0 |
| 2022-05 | SA2#151 | S2-2205028 | - | - | - | Update of Solution#6 to remove ENs and clarify the QoS handling and charging. | 0.3.0 |