**3GPP TSG-SA3 Meeting #101e *draft\_S3-203203-r5***

**e-meeting, 9 – 20 November 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **33.501** | **CR** | **1006** | **rev** | **1** | **Current version:** | **16.4.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | Authorization between NFs and SCP |
|  |  |
| ***Source to WG:*** |  Nokia, Nokia Shanghai Bell |
| ***Source to TSG:*** | S3 |
|  |  |
| ***Work item code:*** | 5G\_eSBA |  | ***Date:*** | 2020-11-20 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | In TS33.501 in clause 13.3.6 there is a Ed Note stating authorization between NFs and SCP is ffs |
|  |  |
| ***Summary of change:*** | Addition of authorization mechanism between NFs and SCP |
|  |  |
| ***Consequences if not approved:*** | There will be no authorization mechanism defined between NFs and SCP and Ed Note will be unresolved.  |
|  |  |
| ***Clauses affected:*** | 13.3.6, 13.4.1.3.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* Start of Change \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

###

### 13.3.6 Authentication and authorization between SCP and network functions

The SCP and network functions shall use one of the following methods described in clause 13.1 to mutually authenticate each other before service layer messages can be exchanged on that interface:

- If the PLMN uses protection at the transport layer, authentication provided by the transport layer protection solution shall be used for mutual authentication of the SCP and the network functions.

- If the PLMN does not use protection at the transport layer, mutual authentication of the SCP and network functions may be implicit by NDS/IP or physical security.

Authentication between the SCP and the Network Function may be implicit by co-location.

Authorization between the SCP and NFs is based on local authorization policy. Regarding the authorization of access token requests sent by an SCP on behalf of an NF Service Consumer, NOTE 3 in clause 13.3.1.2 applies.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* End of Change \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*