**3GPP TSG SA WG4 #112e *S4-210276***

**1st – 10th February 2021**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.0* | | | | | | | | |
| **Draft CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **26.511** | **CR** | **0003** | **rev** | **-** | **Current version:** | **16.1.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | 8K Decoding Capabilities | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Qualcomm Incorporated, Intel | | | | | | | | | |
| ***Source to TSG:*** | SA4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | 8K\_VR\_5G | | | | |  | ***Date:*** | | | 2021-01-16 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12)* *Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | 5G Media Streaming does not yet support 8K decoding capabilities. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | * Defines 8K Decoding capabilities * Adds 8K VR to VR Streaming profiles | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | See work item description. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 4.2.2.1, 4.2.2.3.4 (new), 5.5.1.1, 5.5.1.2 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | | **x** |  | Other core specifications | | | | CR 26.118-00XX | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
| ***56*** | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

**===== CHANGE =====**

#### 4.2.2.1 Decoding

The following H.265 (HEVC) media decoding capabilities are defined:

- **HEVC-HD-Dec**: the capability to decode H.265 (HEVC) Main Profile, Main Tier, Level 3.1[3] bitstreams that have general\_progressive\_source\_flag equal to 1, general interlaced\_source\_flag equal to 0, general\_non\_packed\_constraint\_flag equal to 1, and general\_frame\_only\_constraint\_flag equal to 1.

- **HEVC-FullHD-Dec**: the capability to decode H.265 (HEVC) Main10 Profile, Main Tier, Level 4.1[3] bitstreams that have general\_progressive\_source\_flag equal to 1, general interlaced\_source\_flag equal to 0, general\_non\_packed\_constraint\_flag equal to 1, and general\_frame\_only\_constraint\_flag equal to 1.

- **HEVC-UHD-Dec**: the capability to decode H.265 (HEVC) Main10 Profile, Main Tier, Level 5.1[3] bitstreams that have general\_progressive\_source\_flag equal to 1, general interlaced\_source\_flag equal to 0, general\_non\_packed\_constraint\_flag equal to 1, and general\_frame\_only\_constraint\_flag equal to 1.

- **HEVC-8K-Dec**: the capability to decode H.265 (HEVC) Main10 Profile, Main Tier, Level 6.1[3] bitstreams that have general\_progressive\_source\_flag equal to 1, general interlaced\_source\_flag equal to 0, general\_non\_packed\_constraint\_flag equal to 1, and general\_frame\_only\_constraint\_flag equal to 1 with the following further limitations:

- the bitstream does not exceed the maximum luma picture size in samples of 33,554,432,

- the maximum VCL Bit Rate is constrained to be 80 Mbps with CpbVclFactor and CpbNalFactor being fixed to be 1000 and 1100, respectively.

**===== CHANGE =====**

##### 4.2.2.3.4 HEVC-8K

4.2.2.3.4.1 ISO BMFF File Format

If HEVC-8K media is provided in a bitstream that is decodable by a decoder capable of the **HEVC-8K-Dec** decoding capabilities as defined in clause 4.2.2.1 and the media is encapsulated in an ISO BMFF Track [14], then the file format track shall conform to the requirements of the codec entry 'hvc1' or 'hev1' as defined in ISO/IEC 14496-15 [15].

4.2.2.3.4.2 CMAF Track Definition

If HEVC-UHD media is provided in a CMAF track, then the CMAF track shall conform to

- the requirements of the ISO BMFF File format track defined in clause 4.2.2.3.4.1;

- the general CMAF Track constraints in ISO/IEC 23000-19, clause 7, and

- the general video track constraints defined in ISO/IEC 23000-19, clause 9.

4.2.2.3.4.3 CMAF Switching Set Definition

If HEVC-UHD media is provided in a CMAF Switching Set, then

- every CMAF track in the CMAF Switching Set shall conform to the requirements of CMAF Track in clause 4.2.2.3.4.2;

- the general CMAF Switching Set constraints in ISO/IEC 23000-19 [27], clause 7; and

- the general CMAF video track Switching Set constraints defined in ISO/IEC 23000-19 [7], clause 9.

4.2.2.3.4.4 Playback Requirements

For a receiver supporting the HEVC-UHD media profile the following applies:

- It shall support the **HEVC-8K-Dec** decoding capabilities as defined in clause 4.2.2.1.

- It shall support the following playback requirements as documented in clause 8 of CTA-WAVE 5003 [9] for any content conforming to a CMAF Switching Set as defined in clause 4.2.2.3.4.3 namely:

- 8.2 Sequential Track Playback

- 8.3 Random Access to Fragment

- 8.4 Random Access to Time

- 8.5 Switching Set Playback

- 8.6 Regular Playback of Chunked Content

- 8.7 Regular Playback of Chunked Content, non-aligned append

- It should support the following playback requirements as documented in clause 8 of CTA-WAVE 5003 [9] for any content conforming to a CMAF Switching Set as defined in clause 4.2.2.3.4.3 namely:

- 8.9 Out-Of-Order Loading

- 8.10 Overlapping Fragments

- 8.12 Playback of Encrypted Content

**===== CHANGE =====**

#### 5.5.1.1 Operation Points

If the 5GMS UE supports 360 VR video, it shall include a receiver that complies with:

- the *Basic H.264/AVC* Operation Point Receiver requirements as specified in TS 26.118 [13], clause 5.1.4.

If the 5GMS UE supports 360 VR video, it should include a receiver that complies with:

- the *Main* *H.265/HEVC* Operation Point Receiver requirements as specified in TS 26.118 [13], clause 5.1.5.

If the 5GMS UE supports 360 VR video, it may include a receiver that complies with:

- the *Flexible* *H.265/HEVC* Operation Point Receiver requirements as specified in TS 26.118 [13], clause 5.1.6.

If the 5GMS UE supports 360 VR video, it may include a receiver that complies with:

- the *H.265/HEVC 8K* Operation Point Receiver requirements as specified in TS 26.118 [13], clause 5.1.7 and the **HEVC-8K-Dec** decoding capabilities as defined in clause 4.2.2.1.

**===== CHANGE =====**

#### 5.5.1.2 DASH encapsulation

If the 5GMS UE supports 360 VR video for DASH services, it shall include a receiver that complies with:

- the Basic Video Media Profile Receiver requirements for DASH as specified in TS 26.118 [13], clause 5.2.2.3.

If the 5GMS UE supports 360 VR video for DASH services, it should include a receiver that complies with:

- the Main Video Media Profile Receiver requirements for DASH as specified in TS 26.118 [13], clause 5.2.3.3.

If the 5GMS UE supports 360 VR video for DASH services, it may include a receiver that complies with:

- the Advanced Video Media Profile Receiver requirements for DASH as specified in TS 26.118 [13], clause 5.2.3.4.

If the 5GMS UE supports 360 VR video, it may include a receiver that complies with:

- the 8K Media Profile Receiver requirements for DASH as specified in TS 26.118 [13], clause 5.2.3.5 and the HEVC-8K playback requirements as defined in clause 4.2.2.3.4.4.