**3GPP TSG-S4 Meeting #131 S4-250157**

**Geneva, 17-21 February 2025**

|  |
| --- |
| *CR-Form-v12.2* |
| **PSEUDO CHANGE REQUEST** |
|  |
|  | **26.567** | **CR** |  | **rev** |  | **Current version:** | **0.4.1** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | [SR\_IMS] General introduction of user plane protocol stack  |
|  |  |
| ***Source to WG:*** | Nokia |
| ***Source to TSG:*** | S4 |
|  |  |
| ***Work item code:*** | SR\_IMS  |  | ***Date:*** | 2025-02-11 |
|  |  |  |  |  |
| ***Category:*** | B |  | ***Release:*** | Rel-19 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19) Rel-20 (Release 20)* |
|  |  |
| ***Reason for change:*** | To address edtiro’s note, add general introduction of user-plane protocol stack |
|  |  |
| ***Summary of change:*** | Add introduction text in clause 5.1Add references in clause 2.  |
|  |  |
| ***Consequences if not approved:*** | Incompleted specification.  |
|  |  |
| ***Clauses affected:*** | 5.1, 2.  |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **1st Change** |

5 Media codecs, configuration, and data transport

5.1 General

The SR-DCMTSI Client should support the user plane protocol stack defined in TS 26.114 (Figure 4.3). All media components except data media components are transported over RTP with each respective payload format mapped onto RTP (RFC 3550 [x1]) streams. The data media components are transported over the data channels using SCTP (RFC 4960 [x2]) over DTLS (RFC 8261 [x3]), as specified for WebRTC data channels (RFC 8831 [x4]).

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ End of 1st Change\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

|  |
| --- |
| **2nd Change** |

2 References

[x1] IETF RFC 3550 (2003): "RTP: A Transport Protocol for Real-Time Applications", H. Schulzrinne, S. Casner, R. Frederick and V. Jacobson.

[x2] IETF RFC 4960 (2007): "Stream Control Transmission Protocol"

[x3] IETF RFC 8261 (2017): "Datagram Transport Layer Security (DTLS) Encapsulation of SCTP Packets"

[x4] IETF RFC 8831 (2021): "WebRTC Data Channels".

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ End of 2nd Change\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**