**3GPP TSG-SA5 Meeting #133e *S5-205034r3***

**e-meeting 12th - 21st October 2020**

**Title:** LS on Network Slice PA Charging per maximum utilized bandwidth

**Response to:** -

**Release:** Release 17

**Work Item:** 5GS\_NSPACH

**Source:** SA5

**To:** SA2

**Contact Person:** Dong Jia

**Name:**

**Tel. Number:**

**E-mail Address:** dongjia (at) chinamobile (dot) com

**Send any reply LS to: 3GPP Liaisons Coordinator,** **mailto:3GPPLiaison@etsi.org**

**Attachments:** None

**1. Overall Description:**

SA5 would like to inform SA2 that SA5 may consider a new “maximum utilized bandwidth” for Network Slice Performance and Analytics charging, , which means the maximum value of utilized bandwidth of accumulated total UEs in a network slice.

**Question**：Do the NWDAF intend to support maximum utilized bandwidth of a network slice in Release 17?

**2. Actions:**

**To SA2 group.**

**ACTION:** SA5 kindly asks SA2 to respond to the above question.

**3. Date of Next TSG-SA WG5 Meetings:**

SA5#134e 16 - 25 November 2020 Online

SA5#135e 25 - 29 January 2021 Online