3GPP TSG SA WG5 Meeting 134-e TDoc S5-205122rev6

**electronic meeting, online, 16th - 25th November 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **32.260** | **CR** | **0407** | **rev** | **1** | **Current version:** | **16.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Add service based architecture for offline charging |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | 5GSIMSCH |  | ***Date:*** | 2020-11-19 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | Offline only charging triggers for IMS service based charging is missing. |
|  |  |
| ***Summary of change:*** | Adding Offline only charging triggers for IMS service based charging. |
|  |  |
| ***Consequences if not approved:*** | Offline only charging for IMS service based charging architecture options won’t be specified. |
|  |  |
| ***Clauses affected:*** | 5.4.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **First change** |

### 5.4.3 Applicable triggers for IMS charging

The IMS nodes for which SIP method a charging Data Request is sent shall be operator configurable. The tables below describe all possible Charging Data Requests that might be sent from IMS nodes.

The generation of a Charging Data Request message by the IMS nodes in response to a particular "triggering SIP method" shall be operator configurable (enable or disable).

Table 5.4.3.1: Default Trigger conditions in or MRFC

| Trigger Conditions | Trigger level | Converged Charging default category | Offline only charging default category | CHF allowed to change category | CHF allowed to enable and disable | Message when "immediate reporting" category |
| --- | --- | --- | --- | --- | --- | --- |
| SIP INVITE for initiating a multimedia ad hoc conferencing session | - | Immediate | Not Applicable | Not Applicable | Not Applicable | SCUR: Charging Data Request [Initial] |
| SIP 2xx acknowledging an SIP INVITE for initiating a multimedia ad hoc conferencing session, and no charging session exists. | - | Immediate | Immediate | Not Applicable | Not Applicable |
| SIP ACK acknowledging a SIP INVITE to connect an UE to the conferencing session | - | Immediate | Immediate | Not Applicable | Not Applicable | SCUR: Charging Data Request [Update] |
| SIP RE-INVITE or SIP UPDATE[e.g. change in media components] | - | Immediate | Immediate | Not Applicable | Not Applicable |
| SIP BYE(NOTE 1) | - | Immediate | Immediate | Not Applicable | Not Applicable |
| Expiration of Interim  | - | Immediate | Immediate | Not Applicable | Not Applicable |
| Expiration of quota, Validity time expiry or other authorization triggers (quota threshold reached, …). | - | Immediate | Not Applicable | Not Applicable | Not Applicable |
| SIP BYE message (both normal and abnormal session termination cases) (NOTE 2) | - | Immediate | Immediate | Not Applicable | Not Applicable | SCUR: Charging Data Request [Termination] |
| SIP CANCEL | - | Immediate | Immediate | Not Applicable | Not Applicable |
| SIP Final Response with error codes 4xx, 5xx or 6xx indicating termination of an ongoing session | - | Immediate | Immediate | Not Applicable | Not Applicable |
|  | NOTE 1: This trigger only applies to a user leaving an ongoing conferencing sessionNOTE 2: This trigger only applies if this causes the ongoing conferencing session to terminate |

Table 5.4.3.2: Default Trigger conditions in or IMS-GWF or AS

| Trigger Conditions | Trigger level | Converged Charging default category | Offline only charging default category | CHF allowed to change category | CHF allowed to enable and disable | Message when "immediate reporting" category |
| --- | --- | --- | --- | --- | --- | --- |
| SIP INVITE | - | Immediate | Immediate | Not Applicable | Not Applicable | SCUR: Charging Data Request [Initial]ECUR: Charging Data Request [Initial] |
| SIP NOTIFY | - | Immediate | Not Applicable | Not Applicable | Not Applicable |
| SIP MESSAGE | - | Immediate | Not Applicable | Not Applicable | Not Applicable |
| SIP REGISTER | - | Immediate | Not Applicable | Not Applicable | Not Applicable |
| SIP SUBSCRIBE | - | Immediate | Not Applicable | Not Applicable | Not Applicable |
| SIP REFER | - | Immediate | Not Applicable | Not Applicable | Not Applicable |
| SIP PUBLISH | - | Immediate | Not Applicable | Not Applicable | Not Applicable |
| SIP 2xx acknowledging a SIP INVITE, RE-INVITE or SIP UPDATE [e.g. change in media components]  | - | Immediate | Immediate | Not Applicable | Not Applicable | SCUR: Charging Data Request [Update] |
| RE-INVITE or SIP UPDATE [e.g. change in media components, terminating identity change]  | - | Immediate | Immediate | Not Applicable | Not Applicable |
| Expiration of quota, Validity time expiry or other authorization triggers (quota threshold reached, …). | - | Immediate | Not Applicable | Not Applicable | Not Applicable |
| Any SIP message (except those triggering a Debit / Reserve Units Request[Initial] or those not covered by the above triggers for Reserve Units Request[Update] conveying a SDP offer or its associated SDP answer before SIP session establishment  | - | Immediate | Not Applicable | Not Applicable | Not Applicable |
| SIP 1xx provisional response, mid-dialog requests, mid-dialog responses and SIP INFO embedding RTTI XML body | - | Immediate | Not Applicable | Not Applicable | Not Applicable |
|  |  |  |  |  |  |
| SIP BYE message (both normal and abnormal session termination cases)  | - | Immediate | Immediate | Not Applicable | Not Applicable | SCUR: Charging Data Request [Termination] |
| SIP 2xx acknowledging a SIP BYE message (only when last user location information of originating/ terminating party is required by operator for legal purpose). | - | Immediate | Immediate | Not Applicable | Not Applicable |
| SIP Final Response (4xx, 5xx or 6xx), indicating an unsuccessful SIP session set-up procedure | - | Immediate | Immediate | Not Applicable | Not Applicable |
| SIP 2xx acknowledging non-session related SIP messages | - | Immediate | Not Applicable | Not Applicable | Not Applicable | ECUR: Charging Data Request [Termination] |
| SIP Final Response (4xx, 5xx or 6xx), indicating an unsuccessful session-unrelated procedure | - | Immediate | Not Applicable | Not Applicable | Not Applicable |
| Aborting a SIP session set-up procedure, using an internal trigger, or a SIP CANCEL | - | Immediate | Not Applicable | Not Applicable | Not Applicable | ECUR: Charging Data Request [Termination]SCUR: Charging Data Request [Termination] |
| Deregistration  | - | Immediate | Not Applicable | Not Applicable | Not Applicable |
| SIP Final/Redirection Response 3xx | - | Immediate | Not Applicable | Not Applicable | Not Applicable |
| SIP NOTIFY | - | Immediate | Immediate | Not Applicable | Not Applicable | IEC: Charging Data Request [Event] |
| SIP MESSAGE | - | Immediate | Immediate | Not Applicable | Not Applicable |
| SIP REGISTER | - | Immediate | Immediate | Not Applicable | Not Applicable |
| SIP SUBSCRIBE | - | Immediate | Immediate | Not Applicable | Not Applicable |
| SIP REFER | - | Immediate | Immediate | Not Applicable | Not Applicable |
| SIP PUBLISH | - | Immediate | Immediate | Not Applicable | Not Applicable |
| SIP Final Response (4xx, 5xx or 6xx), indicating an unsuccessful session-unrelated procedure | - | Immediate | Immediate | Not Applicable | Not Applicable |

|  |
| --- |
| **End of changes** |