**3GPP TSG-SA5 Meeting #143-e *S5-223462rev1***

**e-meeting, 9 - 17 May 2022**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **32.291** | **CR** | **0405** | **rev** | **1** | **Current version:** | **17.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Update Nchf\_ConvergedCharging service API for Edge Computing |
|  |  |
| ***Source to WG:*** | Intel |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | EDGE\_CH |  | ***Date:*** | 2022-04-28 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)**Rel-17 (Release 17)* |
|  |  |
| ***Reason for change:*** | The Edge Computing domain charging has been defined in TS 32.257, the Nchf\_ConvergedCharging service API needs to be updated accordingly. |
|  |  |
| ***Summary of change:*** | Added bindings for Edge Computing domain charging;Updated Nchf\_ConvergedCharging service API for Edge Computing domain charging. |
|  |  |
| ***Consequences if not approved:*** | The Nchf\_ConvergedCharging service API cannot support Edge Computing domain charging. |
|  |  |
| ***Clauses affected:*** | 2, 7.x, A.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| **Start of modification** |

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TS 32.240: "Telecommunication management; Charging management; Charging architecture and principles".

[2] - [13] Void.

[14] 3GPP TS 32.254: "Telecommunication management; Charging management; Exposure function Northbound Application Program Interfaces (APIs) charging ".

[15] - [28] Void.

[29] 3GPP TS 32.274: "Telecommunication management; Charging management;Short Message Service (SMS) charging".

[30] 3GPP TS 32.255: "Telecommunication management; Charging management; 5G Data connectivity domain charging; stage 2".

[31] 3GPP TS 32.256: "Telecommunication management; Charging management; 5G connection and mobility domain charging; stage 2".

[32] 3GPP TS 32.260: "Telecommunication management; Charging management; IP Multimedia Subsystem (IMS) charging".

[33] 3GPP TS 32.275: "Telecommunication management; Charging management; MultiMedia Telephony (MMTel) charging".

[34] 3GPP TS 32.281: "Telecommunication management; Charging management; Announcement

[35] 3GPP TS 32.257: "Telecommunication management; Charging management; Edge computing domain charging; stage 2".

[36] - [49] Void.

[50] - [57] Void.

[58] 3GPP TS 32.290: "Telecommunication management; Charging management; 5G system; Services, operations and procedures of charging using Service Based Interface (SBI).

[59] - [69] Void.[70] 3GPP TS 28.201: "Charging management; Network slice performance and analytics charging in the 5G System (5GS); Stage 2".

[71] 3GPP TS 28.202: "Charging management; Network slice management charging in the 5G System (5GS); Stage 2".

[72] - [99] Void.

[100] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[101] 3GPP TR 21.900: "Technical Specification Group working methods".

[102] 3GPP TS 24.605: "Conference (CONF) using IP Multimedia (IM) Core Network (CN) subsystem; Protocol specification".

[103] - [199] Void

[200] - [252] Void

[253] 3GPP TS 28.532: "Management and orchestration; Management services".

[254] 3GPP TS 28.541: "Management and orchestration; 5G Network Resource Model (NRM); Stage 2 and stage 3".

[255] 3GPP TS 32.300: "Telecommunication management; Configuration Management (CM); Name convention for Managed Objects".

[256] 3GPP TS 28.554: "Management and orchestration;5G end to end Key Performance Indicators (KPI)".

[257] 3GPP TS 28.623: "Telecommunication management; Generic Network Resource Model (NRM) Integration Reference Point (IRP); Solution Set (SS) definitions".

[258] 3GPP TS 24.229: "IP Multimedia Call Control Protocol based on SIP and SDP; Stage 3".

[259] 3GPP TS 29.078: "Customised Applications for Mobile network Enhanced Logic (CAMEL); CAMEL Application Part (CAP) specification".".

[260] 3GPP TS 29.228: "IP Multimedia (IM) Subsystem Cx and Dx interface; signalling flows and message contents".

[261] 3GPP TS 29.002: "Mobile Application Part (MAP) specification".

[262] 3GPP TS 28.550: "Management and orchestration; Performance assurance ".

[263] 3GPP TS 28.552: "Management and orchestration; 5G performance measurements ".

[262] - [298] Void

[299] 3GPP TS 29.500: "5G System; Technical Realization of Service Based Architecture; Stage 3".

[300] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[301] 3GPP TS 29.594: "5G System; Spending Limit Control Service; Stage 3".

[302] 3GPP TS 29.512: "5G System; Session Management Policy Control Service; Stage 3".

[303] 3GPP TS 24.501: "Non-Access-Stratum (NAS) Protocol for 5G System (5GS); Stage 3".

[304] 3GPP TS 38.413: "NG-RAN; NG Application Protocol (NGAP)".

[305] 3GPP TS 29.510: "Network Function Repository Services; Stage 3".

[306] 3GPP TS 29.520: "5G System; Network Data Analytics Services;Stage 3".

[307] 3GPP TS 29.558: "Enabling Edge Applications; Application Programming Interface (API) specification; stage 3".

[308] 3GPP TS 32.538: "Management and orchestration; Edge Computing Management".

[309] 3GPP TS 24.558: "Enabling Edge Applications; Protocol specification".

[310] - [370] Void

[371] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces; Stage 3".

[372] - [389] Void

[390] 3GPP TS 33.501: "Security architecture and procedures for 5G System".

[391] - [399] Void

[400] Void.

[401] IETF RFC 7540: "Hypertext Transfer Protocol Version 2 (HTTP/2) ".

[402] IETF RFC 8259: "The JavaScript Object Notation (JSON) Data Interchange Format ".

[403] IETF RFC 6749: "The OAuth 2.0 Authorization Framework".

[404] IETF RFC 3986: "Uniform Resource Identifiers (URI): Generic Syntax".

[405] IETF RFC 7315: "Private Extensions to the Session Initiation Protocol (SIP) for the 3rd Generation Partnership Projects (3GPP)".

[406] IETF RFC 3261: "SIP: Session Initiation Protocol".

[407] IETF RFC 8866: "SDP: Session Description Protocol".

[408] IETF RFC 5646: "Tags for Identifying Languages".

[409] - [499] Void.

[500] OpenAPI: "OpenAPI 3.0.0 Specification", <https://github.com/OAI/OpenAPI-Specification/blob/master/versions/3.0.0.md>.

[501] - [599] Void.

|  |
| --- |
| **Next modification** |

##### 6.1.6.2.x Edge computing domain charging specified data type

###### 6.1.6.2.x.1 Type ChargingDataRequest

This clause is additional attributes of the type ChargingDataRequest defined in clause 6.1.6.2.1.1 for edge computing domain charging described in TS 32.257 [35].

Table 6.1.6.2.x.1-1: Edge computing domain specified attribute of type ChargingDataRequest

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| edgeInfrastructureUsageChargingInformation | EdgeInfrastructureUsageChargingInformation | OC | 0..1 | This field holds the for edge enabling infrastructure resource usage charging specific information. |  |
| eASDeploymentChargingInformation | EASDeploymentChargingInformatio | OC | 0..1 | This field holds the for EAS deployment charging specific information. |  |
| directEdgeEnablingServiceChargingInformation | DirectEdgeEnablingServiceChargingInformation | OC | 0..1 | This field holds the charging information the edge enabling services directly provided by EES, only used if structured charging information is required. |  |
| nEFCharging Information | NEFChargingInformation  | OC  | 0..1 | This field may hold both the charging information of the 5G NF services exposed by EES as well as the edge enabling services directly provided by the EES. |  |

Editor’s note: all attribute names and data types are FFS dependent TS 24.558 [309] and TS 29.558 [307] release.

###### 6.1.6.2.x.2 Type ChargingDataResponse

This clause specifies additional attributes of the type ChargingDataResponse defined in clause 6.1.6.2.1.2 for edge computing domain charging described in TS 32.257 [35].

Table 6.1.6.2.x.2-1: Edge computing domain specified attribute of type ChargingDataResponse

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
|  |  |  |  |  |  |

###### 6.1.6.2.x.3 Type EdgeInfrastructureUsageChargingInformation

Table  6.1.6.2.x.3-2: Definition of type EdgeInfrastructureUsageChargingInformation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| meanVirtualCPUUsage | Float | OC | 0..1 | This field holds the information of mean virtual CPU usage for the EAS, see VR.VCpuUsageMean in clause 5.7.1.1.1 of T TS 28.552 [263]. |  |
| meanVirtualMemoryUsage | Float | OC | 0..1 | This field holds the information of mean virtual memory usage for the EAS, see VR.VMemoryUsageMean in clause 5.7.1.2.1 of TS 28.552 [263]. |  |
| meanVirtualDiskUsage | Float | OC | 0..1 | This field holds the information of mean virtual disk usage for the EAS, see VR.VDiskUsageMean in clause 5.7.1.2.1 of TS 28.552 [263]. |  |
| durationStartTime | DateTime | OC | 0..1 | This field holds the start time of the collection period, see TS 28.550 [262]. |  |
| durationEndTime | DateTime | OC | 0..1 | This field holds the end time of the collection period, see TS 28.550 [262]. |  |

###### 6.1.6.2.x.4 Type EASDeploymentChargingInformation

Table  6.1.6.2.x.4-2: Definition of type DirectEdgeEnablingServiceChargingInformation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| eEASDeploymentRequirements | EASRequirements | OC | 0..1 | This field holds the EAS Deployment Requirements, see TS 23.558 [9], including the Required EAS Serving Location, Software Image Info, Affinity Anti Affinity and Service Continuity. |  |
| lCMStartTime | DateTime | OM | 0..1 | This field holds the start time of the EAS LCM process, see Start Time in clause 8.3.6.5 Type measJobInfo-ResourceType in TS 28.550 [262]. |  |
| lCMEndTime | DateTime | OM | 0..1 | This field holds the end time of the EAS LCM process, see Stop Time in clause 8.3.6.5 Type measJobInfo-ResourceType in TS 28.550 [262]. |  |

###### 6.1.6.2.x.5 Type DirectEdgeEnablingServiceChargingInformation

Table  6.1.6.2.x.5-2: Definition of type DirectEdgeEnablingServiceChargingInformation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
|  |  |  |  |  |  |
| uEidentifier | Gpsi | OC | 0..1 |  |  |
| uElocation  | LocationInfo | OC | 0..1 |  |  |
| tEASDNAIs | Arry(Dnai) | OC | 0..1 |  |  |
| easProfiles | array(EASProfile) | OC | 1..N | List of the profile information of the EAS(s). |  |
| acInfs | array(ACInformation) | OC | 1..N |  |  |
| acId | string | OC | 0..1 |  |  |
| tEasEndpoint | EndPoint | OC | 0..1 |  |  |
| sEasEndpoint | EndPoint | OC | 0..1 |  |  |
| prevTEasEndpoint | EndPoint | OC | 0..1 |  |  |
| routeReq | RouteToLocation | OC | 0..1 |  |  |
| eECContext | EECContext | OC | 0..1 |  |  |
| actResult | ACTResultInfo | OC | 0..1 |  |  |

|  |
| --- |
| **Next modification** |

## 7.x Bindings for Edge Computing domain charging

Table 7.x-1: Bindings of Edge Computing domain charging CDR field, Information Element and Resource Attribute

| Information Element | CDR Field | Resource Attribute |
| --- | --- | --- |
|  |  | **ChargingDataRequest** |
| Edge Enabling Infrastructure Resource Usage Charging Information | Edge Enabling Infrastructure Resource Usage Charging Information | /edgeInfrastructureUsageChargingInformation |
| Mean Virtual CPU Usage | Mean Virtual CPU Usage | /edgeInfrastructureUsageChargingInformation/meanVirtualCPUUsage |
| Mean Virtual Memory Usage | Mean Virtual Memory Usage | /edgeInfrastructureUsageChargingInformation/meanVirtualMemoryUsage |
| Mean Virtual Disk Usage | Mean Virtual Disk Usage | /edgeInfrastructureUsageChargingInformation/meanVirtualDiskUsage |
| Duration Start Time | Duration Start Time | /edgeInfrastructureUsageChargingInformation/durationStartTime |
| Duration End Time | Duration End Time | /edgeInfrastructureUsageChargingInformation/durationEndTime |
| EAS Deployment Charging Information | EAS Deployment Charging Information | /eASDeploymentChargingInformation |
| EAS Deployment Requirements | EAS Deployment Requirements | /eASDeploymentChargingInformation/eEASDeploymentRequirements |
| LCM Start Time | LCM Start Time | /eASDeploymentChargingInformation/lCMStartTime |
| LCM End Time | LCM End Time | /eASDeploymentChargingInformation/lCMEndTime |
| Direct Edge Enabling Service Charging Information | Direct Edge Enabling Service Charging Information | / directEdgeEnablingServiceChargingInformation |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
| UE Identifier | UE Identifier | / directEdgeEnablingServiceChargingInformation/uEIdentifier |
| UE Location  | UE Location  | / directEdgeEnablingServiceChargingInformation/uELocation |
|  |  |  |
|  |  |  |
| DNAI of the T-EAS | DNAI of the T-EAS | / directEdgeEnablingServiceChargingInformation/tEASDNAI |
| EAS Profiles | EAS Profiles | directEdgeEnablingServiceChargingInformation/easProfiles |
| AC Info | AC Info | directEdgeEnablingServiceChargingInformation/acInfs |
| T-EAS Endpoint | T-EAS Endpoint | directEdgeEnablingServiceChargingInformation/tEasEndpoint |
| S-EAS Endpoint | S-EAS Endpoint | directEdgeEnablingServiceChargingInformation/sEasEndpoint |
| Previous T-EAS Endpoint | Previous T-EAS Endpoint | directEdgeEnablingServiceChargingInformation/prevTEasEndpoint |
| Route Req | Route Req | directEdgeEnablingServiceChargingInformation/routeReq |
| AC Id | AC Id | directEdgeEnablingServiceChargingInformation/acId |
| EEC Context | EEC Context | / directEdgeEnablingServiceChargingInformation/eECContext |
|  |  |  |
|  |  |  |
| ACT Result | ACT Result | / directEdgeEnablingServiceChargingInformation/aCTResult |
| Exposed Edge Enabling Service Charging Information | ExposureFunctionAPIInformation | /nEFChargingInformation |
| UE Identifier | externalIndividualIdentifier | /nEFChargingInformation/externalIndividualIdentifier |
| API Direction | aPIDirection | /nEFChargingInformation/aPIDirection |
| API Target Network Function | aPITargetNetworkFunction | /nEFChargingInformation/aPITargetNetworkFunction |
| API Result Code | aPIResultCode | /nEFChargingInformation/aPIResultCode |
| API Name | aPIName | /nEFChargingInformation/aPIName |
| API Reference | aPIReference | /nEFChargingInformation/aPIReference |
| API Content | aPIContent | /nEFChargingInformation/aPIContent |
|  |  | **ChargingDataResponse** |
| - | - | - |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

|  |
| --- |
| **Next modification** |

## A.2 Nchf\_ConvergedCharging API

openapi: 3.0.0

info:

 title: Nchf\_ConvergedCharging

 version: 3.1.0-alpha.3

 description: |

 ConvergedCharging Service © 2021, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: >

 3GPP TS 32.291 V17.2.0: Telecommunication management; Charging management;

 5G system, charging service; Stage 3.

 url: 'http://www.3gpp.org/ftp/Specs/archive/32\_series/32.291/'

servers:

 - url: '{apiRoot}/nchf-convergedcharging/v3'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in subclause 4.4 of 3GPP TS 29.501.

security:

 - {}

 - oAuth2ClientCredentials:

 - nchf-convergedcharging

paths:

 /chargingdata:

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ChargingDataRequest'

 responses:

 '201':

 description: Created

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ChargingDataResponse'

 '400':

 description: Bad request

 content:

 application/problem+json:

 schema:

 oneOf:

 - $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 - $ref: '#/components/schemas/ChargingDataResponse'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 description: Forbidden

 content:

 application/problem+json:

 schema:

 oneOf:

 - $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 - $ref: '#/components/schemas/ChargingDataResponse'

 '404':

 description: Not Found

 content:

 application/problem+json:

 schema:

 oneOf:

 - $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 - $ref: '#/components/schemas/ChargingDataResponse'

 '405':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/405'

 '408':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/408'

 '410':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/410'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 chargingNotification:

 '{$request.body#/notifyUri}':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ChargingNotifyRequest'

 responses:

 '200':

 description: OK.

 content:

 application/ json:

 schema:

 $ref: '#/components/schemas/ChargingNotifyResponse'

 '204':

 description: 'No Content, Notification was succesfull'

 '400':

 description: Bad request

 content:

 application/problem+json:

 schema:

 oneOf:

 - $ref: TS29571\_CommonData.yaml#/components/schemas/ProblemDetails

 - $ref: '#/components/schemas/ChargingNotifyResponse'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 '/chargingdata/{ChargingDataRef}/update':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ChargingDataRequest'

 parameters:

 - name: ChargingDataRef

 in: path

 description: a unique identifier for a charging data resource in a PLMN

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK. Updated Charging Data resource is returned

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ChargingDataResponse'

 '400':

 description: Bad request

 content:

 application/problem+json:

 schema:

 oneOf:

 - $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 - $ref: '#/components/schemas/ChargingDataResponse'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '403':

 description: Forbidden

 content:

 application/problem+json:

 schema:

 oneOf:

 - $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 - $ref: '#/components/schemas/ChargingDataResponse'

 '404':

 description: Not Found

 content:

 application/problem+json:

 schema:

 oneOf:

 - $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 - $ref: '#/components/schemas/ChargingDataResponse'

 '405':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/405'

 '408':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/408'

 '410':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/410'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 '/chargingdata/{ChargingDataRef}/release':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ChargingDataRequest'

 parameters:

 - name: ChargingDataRef

 in: path

 description: a unique identifier for a charging data resource in a PLMN

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No Content.

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '404':

 description: Not Found

 content:

 application/problem+json:

 schema:

 oneOf:

 - $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 - $ref: '#/components/schemas/ChargingDataResponse'

 '410':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/410'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

 securitySchemes:

 oAuth2ClientCredentials:

 type: oauth2

 flows:

 clientCredentials:

 tokenUrl: '{nrfApiRoot}/oauth2/token'

 scopes:

 nchf-convergedcharging: Access to the Nchf\_ConvergedCharging API

 schemas:

 ChargingDataRequest:

 type: object

 properties:

 subscriberIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 tenantIdentifier:

 type: string

 chargingId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

 mnSConsumerIdentifier:

 type: string

 nfConsumerIdentification:

 $ref: '#/components/schemas/NFIdentification'

 invocationTimeStamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 invocationSequenceNumber:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 retransmissionIndicator:

 type: boolean

 oneTimeEvent:

 type: boolean

 oneTimeEventType:

 $ref: '#/components/schemas/oneTimeEventType'

 notifyUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 supportedFeatures:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 serviceSpecificationInfo:

 type: string

 multipleUnitUsage:

 type: array

 items:

 $ref: '#/components/schemas/MultipleUnitUsage'

 minItems: 0

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/Trigger'

 minItems: 0

 pDUSessionChargingInformation:

 $ref: '#/components/schemas/PDUSessionChargingInformation'

 roamingQBCInformation:

 $ref: '#/components/schemas/RoamingQBCInformation'

 sMSChargingInformation:

 $ref: '#/components/schemas/SMSChargingInformation'

 nEFChargingInformation:

 $ref: '#/components/schemas/NEFChargingInformation'

 registrationChargingInformation:

 $ref: '#/components/schemas/RegistrationChargingInformation'

 n2ConnectionChargingInformation:

 $ref: '#/components/schemas/N2ConnectionChargingInformation'

 locationReportingChargingInformation:

 $ref: '#/components/schemas/LocationReportingChargingInformation'

 nSPAChargingInformation:

 $ref: '#/components/schemas/NSPAChargingInformation'

 nSMChargingInformation:

 $ref: '#/components/schemas/NSMChargingInformation'

 mMTelChargingInformation:

 $ref: '#/components/schemas/MMTelChargingInformation'

 iMSChargingInformation:

 $ref: '#/components/schemas/IMSChargingInformation'

 edgeInfrastructureUsageChargingInformation':

 $ref: '#/components/schemas/EdgeInfrastructureUsageChargingInformation'

 eASDeploymentChargingInformation:

 $ref: '#/components/schemas/EASDeploymentChargingInformation'

 directEdgeEnablingServiceChargingInformation:

 $ref: '#/components/schemas/DirectEdgeEnablingServiceChargingInformation'

 required:

 - nfConsumerIdentification

 - invocationTimeStamp

 - invocationSequenceNumber

 ChargingDataResponse:

 type: object

 properties:

 invocationTimeStamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 invocationSequenceNumber:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 invocationResult:

 $ref: '#/components/schemas/InvocationResult'

 sessionFailover:

 $ref: '#/components/schemas/SessionFailover'

 supportedFeatures:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 multipleUnitInformation:

 type: array

 items:

 $ref: '#/components/schemas/MultipleUnitInformation'

 minItems: 0

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/Trigger'

 minItems: 0

 pDUSessionChargingInformation:

 $ref: '#/components/schemas/PDUSessionChargingInformation'

 roamingQBCInformation:

 $ref: '#/components/schemas/RoamingQBCInformation'

 locationReportingChargingInformation:

 $ref: '#/components/schemas/LocationReportingChargingInformation'

 required:

 - invocationTimeStamp

 - invocationSequenceNumber

 ChargingNotifyRequest:

 type: object

 properties:

 notificationType:

 $ref: '#/components/schemas/NotificationType'

 reauthorizationDetails:

 type: array

 items:

 $ref: '#/components/schemas/ReauthorizationDetails'

 minItems: 0

 required:

 - notificationType

 ChargingNotifyResponse:

 type: object

 properties:

 invocationResult:

 $ref: '#/components/schemas/InvocationResult'

 NFIdentification:

 type: object

 properties:

 nFName:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 nFIPv4Address:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 nFIPv6Address:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 nFPLMNID:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 nodeFunctionality:

 $ref: '#/components/schemas/NodeFunctionality'

 nFFqdn:

 type: string

 required:

 - nodeFunctionality

 MultipleUnitUsage:

 type: object

 properties:

 ratingGroup:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatingGroup'

 requestedUnit:

 $ref: '#/components/schemas/RequestedUnit'

 usedUnitContainer:

 type: array

 items:

 $ref: '#/components/schemas/UsedUnitContainer'

 minItems: 0

 uPFID:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 multihomedPDUAddress:

 $ref: '#/components/schemas/PDUAddress'

 required:

 - ratingGroup

 InvocationResult:

 type: object

 properties:

 error:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 failureHandling:

 $ref: '#/components/schemas/FailureHandling'

 Trigger:

 type: object

 properties:

 triggerType:

 $ref: '#/components/schemas/TriggerType'

 triggerCategory:

 $ref: '#/components/schemas/TriggerCategory'

 timeLimit:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 volumeLimit:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 volumeLimit64:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 eventLimit:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 maxNumberOfccc:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 tariffTimeChange:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 required:

 - triggerType

 - triggerCategory

 MultipleUnitInformation:

 type: object

 properties:

 resultCode:

 $ref: '#/components/schemas/ResultCode'

 ratingGroup:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatingGroup'

 grantedUnit:

 $ref: '#/components/schemas/GrantedUnit'

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/Trigger'

 minItems: 0

 validityTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 quotaHoldingTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 finalUnitIndication:

 $ref: '#/components/schemas/FinalUnitIndication'

 timeQuotaThreshold:

 type: integer

 volumeQuotaThreshold:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 unitQuotaThreshold:

 type: integer

 uPFID:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 announcementInformation:

 $ref: '#/components/schemas/AnnouncementInformation'

 required:

 - ratingGroup

 RequestedUnit:

 type: object

 properties:

 time:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 totalVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 uplinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 downlinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 serviceSpecificUnits:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 UsedUnitContainer:

 type: object

 properties:

 serviceId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceId'

 quotaManagementIndicator:

 $ref: '#/components/schemas/QuotaManagementIndicator'

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/Trigger'

 minItems: 0

 triggerTimestamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 time:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 totalVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 uplinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 downlinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 serviceSpecificUnits:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 eventTimeStamps:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 minItems: 0

 localSequenceNumber:

 type: integer

 pDUContainerInformation:

 $ref: '#/components/schemas/PDUContainerInformation'

 nSPAContainerInformation:

 $ref: '#/components/schemas/NSPAContainerInformation'

 required:

 - localSequenceNumber

 GrantedUnit:

 type: object

 properties:

 tariffTimeChange:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 time:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 totalVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 uplinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 downlinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 serviceSpecificUnits:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 FinalUnitIndication:

 type: object

 properties:

 finalUnitAction:

 $ref: '#/components/schemas/FinalUnitAction'

 restrictionFilterRule:

 $ref: '#/components/schemas/IPFilterRule'

 restrictionFilterRuleList:

 type: array

 items:

 $ref: '#/components/schemas/IPFilterRule'

 minItems: 1

 filterId:

 type: string

 filterIdList:

 type: array

 items:

 type: string

 minItems: 1

 redirectServer:

 $ref: '#/components/schemas/RedirectServer'

 required:

 - finalUnitAction

 RedirectServer:

 type: object

 properties:

 redirectAddressType:

 $ref: '#/components/schemas/RedirectAddressType'

 redirectServerAddress:

 type: string

 required:

 - redirectAddressType

 - redirectServerAddress

 ReauthorizationDetails:

 type: object

 properties:

 serviceId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceId'

 ratingGroup:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatingGroup'

 quotaManagementIndicator:

 $ref: '#/components/schemas/QuotaManagementIndicator'

 PDUSessionChargingInformation:

 type: object

 properties:

 chargingId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

 homeProvidedChargingId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

 userInformation:

 $ref: '#/components/schemas/UserInformation'

 userLocationinfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 mAPDUNon3GPPUserLocationInfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 non3GPPUserLocationTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 mAPDUNon3GPPUserLocationTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 presenceReportingAreaInformation:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 minProperties: 0

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 pduSessionInformation:

 $ref: '#/components/schemas/PDUSessionInformation'

 unitCountInactivityTimer:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'
 rANSecondaryRATUsageReport:

 $ref: '#/components/schemas/RANSecondaryRATUsageReport'

 UserInformation:

 type: object

 properties:

 servedGPSI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 servedPEI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

 unauthenticatedFlag:

 type: boolean

 roamerInOut:

 $ref: '#/components/schemas/RoamerInOut'

 PDUSessionInformation:

 type: object

 properties:

 networkSlicingInfo:

 $ref: '#/components/schemas/NetworkSlicingInfo'

 pduSessionID:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionId'

 pduType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionType'

 sscMode:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SscMode'

 hPlmnId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 servingNetworkFunctionID:

 $ref: '#/components/schemas/ServingNetworkFunctionID'

 ratType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 mAPDUNon3GPPRATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 dnnId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 dnnSelectionMode:

 $ref: '#/components/schemas/dnnSelectionMode'

 chargingCharacteristics:

 type: string

 pattern: '^[0-9a-fA-F]{1,4}$'

 chargingCharacteristicsSelectionMode:

 $ref: '#/components/schemas/ChargingCharacteristicsSelectionMode'

 startTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 stopTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 3gppPSDataOffStatus:

 $ref: '#/components/schemas/3GPPPSDataOffStatus'

 sessionStopIndicator:

 type: boolean

 pduAddress:

 $ref: '#/components/schemas/PDUAddress'

 diagnostics:

 $ref: '#/components/schemas/Diagnostics'

 authorizedQoSInformation:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/AuthorizedDefaultQos'

 subscribedQoSInformation:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SubscribedDefaultQos'

 authorizedSessionAMBR:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ambr'

 subscribedSessionAMBR:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ambr'

 servingCNPlmnId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 mAPDUSessionInformation:

 $ref: '#/components/schemas/MAPDUSessionInformation'

 enhancedDiagnostics:

 $ref: '#/components/schemas/EnhancedDiagnostics5G'

 redundantTransmissionType:

 $ref: '#/components/schemas/RedundantTransmissionType'

 pDUSessionPairID:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 qosMonitoringReport:

 type: array

 items:

 $ref: '#/components/schemas/QosMonitoringReport'

 minItems: 0

 5GLANTypeService:

 $ref: '#/components/schemas/5GLANTypeService'

 required:

 - pduSessionID

 - dnnId

 PDUContainerInformation:

 type: object

 properties:

 timeofFirstUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 timeofLastUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 qoSInformation:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosData'

 qoSCharacteristics:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosCharacteristics'

 afChargingIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

 afChargingIdString:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ApplicationChargingId'

 userLocationInformation:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 rATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 servingNodeID:

 type: array

 items:

 $ref: '#/components/schemas/ServingNetworkFunctionID'

 minItems: 0

 presenceReportingAreaInformation:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 minProperties: 0

 3gppPSDataOffStatus:

 $ref: '#/components/schemas/3GPPPSDataOffStatus'

 sponsorIdentity:

 type: string

 applicationserviceProviderIdentity:

 type: string

 chargingRuleBaseName:

 type: string

 mAPDUSteeringFunctionality:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/SteeringFunctionality'

 mAPDUSteeringMode:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/SteeringMode'

 trafficForwardingWay:

 $ref: '#/components/schemas/TrafficForwardingWay'

 NSPAContainerInformation:

 type: object

 properties:

 latency:

 type: integer

 throughput:

 $ref: '#/components/schemas/Throughput'

 maximumPacketLossRate:

 type: string

 serviceExperienceStatisticsData:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/ServiceExperienceInfo'

 theNumberOfPDUSessions:

 type: integer

 theNumberOfRegisteredSubscribers:

 type: integer

 loadLevel:

 $ref: 'TS29520\_Nnwdaf\_EventsSubscription.yaml#/components/schemas/NsiLoadLevelInfo'

 NSPAChargingInformation:

 type: object

 properties:

 singleNSSAI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 required:

 - singleNSSAI

 NetworkSlicingInfo:

 type: object

 properties:

 sNSSAI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 required:

 - sNSSAI

 PDUAddress:

 type: object

 properties:

 pduIPv4Address:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 pduIPv6AddresswithPrefix:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 pduAddressprefixlength:

 type: integer

 iPv4dynamicAddressFlag:

 type: boolean

 iPv6dynamicPrefixFlag:

 type: boolean

 addIpv6AddrPrefixes:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Prefix'

 ServingNetworkFunctionID:

 type: object

 properties:

 servingNetworkFunctionInformation:

 $ref: '#/components/schemas/NFIdentification'

 aMFId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/AmfId'

 required:

 - servingNetworkFunctionInformation

 RoamingQBCInformation:

 type: object

 properties:

 multipleQFIcontainer:

 type: array

 items:

 $ref: '#/components/schemas/MultipleQFIcontainer'

 minItems: 0

 uPFID:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 roamingChargingProfile:

 $ref: '#/components/schemas/RoamingChargingProfile'

 MultipleQFIcontainer:

 type: object

 properties:

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/Trigger'

 minItems: 0

 triggerTimestamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 time:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 totalVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 uplinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 downlinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 localSequenceNumber:

 type: integer

 qFIContainerInformation:

 $ref: '#/components/schemas/QFIContainerInformation'

 required:

 - localSequenceNumber

 QFIContainerInformation:

 type: object

 properties:

 qFI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Qfi'

 reportTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 timeofFirstUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 timeofLastUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 qoSInformation:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosData'

 qoSCharacteristics:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosCharacteristics'

 userLocationInformation:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 presenceReportingAreaInformation:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 minProperties: 0

 rATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 servingNetworkFunctionID:

 type: array

 items:

 $ref: '#/components/schemas/ServingNetworkFunctionID'

 minItems: 0

 3gppPSDataOffStatus:

 $ref: '#/components/schemas/3GPPPSDataOffStatus'

 3gppChargingId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

 diagnostics:

 $ref: '#/components/schemas/Diagnostics'

 enhancedDiagnostics:

 type: array

 items:

 type: string

 required:

 - reportTime

 RoamingChargingProfile:

 type: object

 properties:

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/Trigger'

 minItems: 0

 partialRecordMethod:

 $ref: '#/components/schemas/PartialRecordMethod'

 SMSChargingInformation:

 type: object

 properties:

 originatorInfo:

 $ref: '#/components/schemas/OriginatorInfo'

 recipientInfo:

 type: array

 items:

 $ref: '#/components/schemas/RecipientInfo'

 minItems: 0

 userEquipmentInfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

 roamerInOut:

 $ref: '#/components/schemas/RoamerInOut'

 userLocationinfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 rATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 sMSCAddress:

 type: string

 sMDataCodingScheme:

 type: integer

 sMMessageType:

 $ref: '#/components/schemas/SMMessageType'

 sMReplyPathRequested:

 $ref: '#/components/schemas/ReplyPathRequested'

 sMUserDataHeader:

 type: string

 sMStatus:

 type: string

 pattern: '^[0-7]?[0-9a-fA-F]$'

 sMDischargeTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 numberofMessagesSent:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 sMServiceType:

 $ref: '#/components/schemas/SMServiceType'

 sMSequenceNumber:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 sMSresult:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 submissionTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 sMPriority:

 $ref: '#/components/schemas/SMPriority'

 messageReference:

 type: string

 messageSize:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 messageClass:

 $ref: '#/components/schemas/MessageClass'

 deliveryReportRequested:

 $ref: '#/components/schemas/DeliveryReportRequested'

 OriginatorInfo:

 type: object

 properties:

 originatorSUPI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 originatorGPSI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 originatorOtherAddress:

 $ref: '#/components/schemas/SMAddressInfo'

 originatorReceivedAddress:

 $ref: '#/components/schemas/SMAddressInfo'

 originatorSCCPAddress:

 type: string

 sMOriginatorInterface:

 $ref: '#/components/schemas/SMInterface'

 sMOriginatorProtocolId:

 type: string

 RecipientInfo:

 type: object

 properties:

 recipientSUPI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 recipientGPSI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 recipientOtherAddress:

 $ref: '#/components/schemas/SMAddressInfo'

 recipientReceivedAddress:

 $ref: '#/components/schemas/SMAddressInfo'

 recipientSCCPAddress:

 type: string

 sMDestinationInterface:

 $ref: '#/components/schemas/SMInterface'

 sMrecipientProtocolId:

 type: string

 SMAddressInfo:

 type: object

 properties:

 sMaddressType:

 $ref: '#/components/schemas/SMAddressType'

 sMaddressData:

 type: string

 sMaddressDomain:

 $ref: '#/components/schemas/SMAddressDomain'

 RecipientAddress:

 type: object

 properties:

 recipientAddressInfo:

 $ref: '#/components/schemas/SMAddressInfo'

 sMaddresseeType:

 $ref: '#/components/schemas/SMAddresseeType'

 MessageClass:

 type: object

 properties:

 classIdentifier:

 $ref: '#/components/schemas/ClassIdentifier'

 tokenText:

 type: string

 SMAddressDomain:

 type: object

 properties:

 domainName:

 type: string

 3GPPIMSIMCCMNC:

 type: string

 SMInterface:

 type: object

 properties:

 interfaceId:

 type: string

 interfaceText:

 type: string

 interfacePort:

 type: string

 interfaceType:

 $ref: '#/components/schemas/InterfaceType'

 RANSecondaryRATUsageReport:

 type: object

 properties:

 rANSecondaryRATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 qosFlowsUsageReports:

 type: array

 items:

 $ref: '#/components/schemas/QosFlowsUsageReport'

 Diagnostics:

 type: integer

 IPFilterRule:

 type: string

 QosFlowsUsageReport:

 type: object

 properties:

 qFI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Qfi'

 startTimestamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 endTimestamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 uplinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 downlinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 5GLANTypeService:

 type: object

 properties:

 internalGroupIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 NEFChargingInformation:

 type: object

 properties:

 externalIndividualIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 externalGroupIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ExternalGroupId'

 groupIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 aPIDirection:

 $ref: '#/components/schemas/APIDirection'

 aPITargetNetworkFunction:

 $ref: '#/components/schemas/NFIdentification'

 aPIResultCode:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 aPIName:

 type: string

 aPIReference:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 aPIContent:

 type: string

 required:

 - aPIName

 RegistrationChargingInformation:

 type: object

 properties:

 registrationMessagetype:

 $ref: '#/components/schemas/RegistrationMessageType'

 userInformation:

 $ref: '#/components/schemas/UserInformation'

 userLocationinfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 pSCellInformation:

 $ref: '#/components/schemas/PSCellInformation'

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 rATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 5GMMCapability:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

 mICOModeIndication:

 $ref: '#/components/schemas/MICOModeIndication'

 smsIndication:

 $ref: '#/components/schemas/SmsIndication'

 taiList:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Tai'

 minItems: 0

 serviceAreaRestriction:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceAreaRestriction'

 minItems: 0

 requestedNSSAI:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 0

 allowedNSSAI:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 0

 rejectedNSSAI:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 0

 nSSAIMapList:

 type: array

 items:

 $ref: '#/components/schemas/NSSAIMap'

 minItems: 0

 amfUeNgapId:

 type: integer

 ranUeNgapId:

 type: integer

 ranNodeId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GlobalRanNodeId'

 required:

 - registrationMessagetype

 PSCellInformation:

 type: object

 properties:

 nrcgi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ncgi'

 ecgi:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ecgi'

 NSSAIMap:

 type: object

 properties:

 servingSnssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 homeSnssai:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 required:

 - servingSnssai

 - homeSnssai

 N2ConnectionChargingInformation:

 type: object

 properties:

 n2ConnectionMessageType:

 $ref: '#/components/schemas/N2ConnectionMessageType'

 userInformation:

 $ref: '#/components/schemas/UserInformation'

 userLocationinfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 pSCellInformation:

 $ref: '#/components/schemas/PSCellInformation'

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 rATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 amfUeNgapId:

 type: integer

 ranUeNgapId:

 type: integer

 ranNodeId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GlobalRanNodeId'

 restrictedRatList:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 minItems: 0

 forbiddenAreaList:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Area'

 minItems: 0

 serviceAreaRestriction:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceAreaRestriction'

 minItems: 0

 restrictedCnList:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/CoreNetworkType'

 minItems: 0

 allowedNSSAI:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 0

 rrcEstCause:

 type: string

 pattern: '^[0-9a-fA-F]+$'

 required:

 - n2ConnectionMessageType

 LocationReportingChargingInformation:

 type: object

 properties:

 locationReportingMessageType:

 $ref: '#/components/schemas/LocationReportingMessageType'

 userInformation:

 $ref: '#/components/schemas/UserInformation'

 userLocationinfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 pSCellInformation:

 $ref: '#/components/schemas/PSCellInformation'

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 rATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 presenceReportingAreaInformation:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 minProperties: 0

 required:

 - locationReportingMessageType

 N2ConnectionMessageType:

 type: integer

 LocationReportingMessageType:

 type: integer

 NSMChargingInformation:

 type: object

 properties:

 managementOperation:

 $ref: '#/components/schemas/ManagementOperation'

 idNetworkSliceInstance:

 type: string

 listOfserviceProfileChargingInformation:

 type: array

 items:

 $ref: '#/components/schemas/ServiceProfileChargingInformation'

 minItems: 0

 managementOperationStatus:

 $ref: '#/components/schemas/ManagementOperationStatus'

# To be introduced once the reference to 'generic.yaml is resolved

# managementOperationalState:

# $ref: 'genericNrm.yaml#/components/schemas/OperationalState'

# managementAdministrativeState:

# $ref: 'genericNrm.yaml#/components/schemas/AdministrativeState'

 required:

 - managementOperation

 ServiceProfileChargingInformation:

 type: object

 properties:

 serviceProfileIdentifier:

 type: string

 sNSSAIList:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 0

# To be introduced once the reference to 'nrNrm.yaml is resolved

# sST:

# $ref: 'nrNrm.yaml#/components/schemas/Sst'

 latency:

 type: integer

 availability:

 type: number

# To be introduced once the reference to sliceNrm.yaml is resolved

# resourceSharingLevel:

# $ref: 'sliceNrm.yaml#/components/schemas/SharingLevel'

 jitter:

 type: integer

 reliability:

 type: string

 maxNumberofUEs:

 type: integer

 coverageArea:

 type: string

# To be introduced once the reference to sliceNrm.yaml is resolved

# uEMobilityLevel:

# $ref: 'sliceNrm.yaml#/components/schemas/MobilityLevel'

# delayToleranceIndicator:

# $ref: 'sliceNrm.yaml#/components/schemas/Support'

 dLThptPerSlice:

 $ref: '#/components/schemas/Throughput'

 dLThptPerUE:

 $ref: '#/components/schemas/Throughput'

 uLThptPerSlice:

 $ref: '#/components/schemas/Throughput'

 uLThptPerUE:

 $ref: '#/components/schemas/Throughput'

 maxNumberofPDUsessions:

 type: integer

 kPIMonitoringList:

 type: string

 supportedAccessTechnology:

 type: integer

# To be introduced once the reference to sliceNrm.yaml is resolved

# v2XCommunicationModeIndicator:

# $ref: 'sliceNrm.yaml#/components/schemas/Support'

 addServiceProfileInfo:

 type: string

 Throughput:

 type: object

 properties:

 guaranteedThpt:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 maximumThpt:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 MAPDUSessionInformation:

 type: object

 properties:

 mAPDUSessionIndicator:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/MaPduIndication'

 aTSSSCapability:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/AtsssCapability'

 EnhancedDiagnostics5G:

 $ref: '#/components/schemas/RanNasCauseList'

 RanNasCauseList:

 type: array

 items:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/RanNasRelCause'

 QosMonitoringReport:

 description: Contains reporting information on QoS monitoring.

 type: object

 properties:

 ulDelays:

 type: array

 items:

 type: integer

 minItems: 0

 dlDelays:

 type: array

 items:

 type: integer

 minItems: 0

 rtDelays:

 type: array

 items:

 type: integer

 minItems: 0

 AnnouncementInformation:

 type: object

 properties:

 announcementIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 announcementReference:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 variableParts:

 type: array

 items:

 $ref: '#/components/schemas/VariablePart'

 minItems: 0

 timeToPlay:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 quotaConsumptionIndicator:

 $ref: '#/components/schemas/QuotaConsumptionIndicator'

 announcementPriority:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 playToParty:

 $ref: '#/components/schemas/PlayToParty'

 announcementPrivacyIndicator:

 $ref: '#/components/schemas/AnnouncementPrivacyIndicator'

 Language:

 $ref: '#/components/schemas/Language'

 VariablePart:

 type: object

 properties:

 variablePartType:

 $ref: '#/components/schemas/VariablePartType'

 variablePartValue:

 type: array

 items:

 type: string

 minItems: 1

 variablePartOrder:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 required:

 - variablePartType

 - variablePartValue

 Language:

 type: string

 MMTelChargingInformation:

 type: object

 properties:

 supplementaryServices:

 type: array

 items:

 $ref: '#/components/schemas/SupplementaryService'

 minItems: 1

 SupplementaryService:

 type: object

 properties:

 supplementaryServiceType:

 $ref: '#/components/schemas/SupplementaryServiceType'

 supplementaryServiceMode:

 $ref: '#/components/schemas/SupplementaryServiceMode'

 numberOfDiversions:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 associatedPartyAddress:

 type: string

 conferenceId:

 type: string

 participantActionType:

 $ref: '#/components/schemas/ParticipantActionType'

 changeTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 numberOfParticipants:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 cUGInformation:

 $ref: '#/components/schemas/OctetString'

 IMSChargingInformation:

 type: object

 properties:

 eventType:

 $ref: '#/components/schemas/SIPEventType'

 iMSNodeFunctionality:

 $ref: '#/components/schemas/IMSNodeFunctionality'

 roleOfNode:

 $ref: '#/components/schemas/RoleOfIMSNode'

 userInformation:

 $ref: '#/components/schemas/UserInformation'

 userLocationInfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 ueTimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 3gppPSDataOffStatus:

 $ref: '#/components/schemas/3GPPPSDataOffStatus'

 isupCause:

 $ref: '#/components/schemas/ISUPCause'

 controlPlaneAddress:

 $ref: '#/components/schemas/IMSAddress'

 vlrNumber:

 $ref: '#/components/schemas/E164'

 mscAddress:

 $ref: '#/components/schemas/E164'

 userSessionID:

 type: string

 outgoingSessionID:

 type: string

 sessionPriority:

 $ref: '#/components/schemas/IMSSessionPriority'

 callingPartyAddresses:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 minItems: 1

 calledPartyAddress:

 type: string

 numberPortabilityRoutinginformation:

 type: string

 carrierSelectRoutingInformation:

 type: string

 alternateChargedPartyAddress:

 type: string

 requestedPartyAddress:

 type: array

 items:

 type: string

 minItems: 1

 calledAssertedIdentities:

 type: array

 items:

 type: string

 minItems: 1

 calledIdentityChange:

 $ref: '#/components/schemas/CalledIdentityChange'

 associatedURI:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 minItems: 1

 timeStamps:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 applicationServerInformation:

 type: array

 items:

 type: string

 minItems: 1

 interOperatorIdentifier:

 type: array

 items:

 $ref: '#/components/schemas/InterOperatorIdentifier'

 minItems: 1

 imsChargingIdentifier:

 type: string

 relatedICID:

 type: string

 relatedICIDGenerationNode:

 type: string

 transitIOIList:

 type: array

 items:

 type: string

 minItems: 1

 earlyMediaDescription:

 type: array

 items:

 $ref: '#/components/schemas/EarlyMediaDescription'

 minItems: 1

 sdpSessionDescription:

 type: array

 items:

 type: string

 minItems: 1

 sdpMediaComponent:

 type: array

 items:

 $ref: '#/components/schemas/SDPMediaComponent'

 minItems: 1

 servedPartyIPAddress:

 $ref: '#/components/schemas/IMSAddress'

 serverCapabilities:

 $ref: '#/components/schemas/ServerCapabilities'

 trunkGroupID:

 $ref: '#/components/schemas/TrunkGroupID'

 bearerService:

 type: string

 imsServiceId:

 type: string

 messageBodies:

 type: array

 items:

 $ref: '#/components/schemas/MessageBody'

 minItems: 1

 accessNetworkInformation:

 type: array

 items:

 type: string

 minItems: 1

 additionalAccessNetworkInformation:

 type: string

 cellularNetworkInformation:

 type: string

 accessTransferInformation:

 type: array

 items:

 $ref: '#/components/schemas/AccessTransferInformation'

 minItems: 1

 accessNetworkInfoChange:

 type: array

 items:

 $ref: '#/components/schemas/AccessNetworkInfoChange'

 minItems: 1

 imsCommunicationServiceID:

 type: string

 imsApplicationReferenceID:

 type: string

 causeCode:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 reasonHeader:

 type: array

 items:

 type: string

 minItems: 1

 initialIMSChargingIdentifier:

 type: string

 nniInformation:

 type: array

 items:

 $ref: '#/components/schemas/NNIInformation'

 minItems: 1

 fromAddress:

 type: string

 imsEmergencyIndication:

 type: boolean

 imsVisitedNetworkIdentifier:

 type: string

 sipRouteHeaderReceived:

 type: string

 sipRouteHeaderTransmitted:

 type: string

 tadIdentifier:

 $ref: '#/components/schemas/TADIdentifier'

 feIdentifierList:

 type: string

 EdgeInfrastructureUsageChargingInformation:

 type: object

 properties:

 meanVirtualCPUUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 meanVirtualMemoryUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 meanVirtualDiskUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Float'

 durationStartTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 durationEndTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 EASDeploymentChargingInformation:

 type: object

 properties:

# To be introduced once the reference to EdgeNrm.yaml is resolved

# eEASDeploymentRequirements:

# $ref: 'EdgeNrm.yaml#/components/schemas/EASRequirements'

 lCMStartTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 lCMEndTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 DirectEdgeEnablingServiceChargingInformation:

 type: object

 properties:

 uEIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 uELocation:

 $ref: 'TS29122\_CommonData.yaml#/components/schemas/LocationArea5G'

 tEASDNAI:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnai'

 minItems: 1

 easProfiles:

 type: array

 items:

 $ref: 'TS29558\_Eecs\_EESRegistration.yaml#/components/schemas/EASProfile'

 minItems: 1

 acInfs:

 type: array

 items:

 $ref: 'TS29558\_Eees\_AppClientInformation.yaml#/components/schemas/ACInformation'

 minItems: 1

 acId:

 type: string

 tEasEndpoint:

 $ref: 'TS29558\_Eees\_EASRegistration.yaml#/components/schemas/EndPoint'

 sEasEndpoint:

 $ref: 'TS29558\_Eees\_EASRegistration.yaml#/components/schemas/EndPoint'

 prevTEasEndpoint:

 $ref: 'TS29558\_Eees\_EASRegistration.yaml#/components/schemas/EndPoint'

 routeReq :

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RouteToLocation'

 eECContext:

 $ref: 'TS29558\_Eees\_EECContextRelocation.yaml#/components/schemas/EECContext'

 aCTResult:

 $ref: 'TS29558\_Eees\_ACRStatusUpdate.yaml#/components/schemas/ACTResult'

 EASProfile:

 $ref: 'TS29558\_Eecs\_EESRegistration.yaml#/components/schemas/EASProfile'

 OctetString:

 type: string

 pattern: '^[0-9a-fA-F]+$'

 E164:

 type: string

 pattern: '^[0-9a-fA-F]+$'

 IMSAddress:

 type: object

 properties:

 ipv4Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 ipv6Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 e164:

 $ref: '#/components/schemas/E164'

 anyOf:

 - required: [ ipv4Addr ]

 - required: [ ipv6Addr ]

 - required: [ e164 ]

 ServingNodeAddress:

 type: object

 properties:

 ipv4Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 ipv6Addr:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 anyOf:

 - required: [ ipv4Addr ]

 - required: [ ipv6Addr ]

 SIPEventType:

 type: object

 properties:

 sIPMethod:

 type: string

 eventHeader:

 type: string

 expiresHeader:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 ISUPCause:

 type: object

 properties:

 iSUPCauseLocation:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 iSUPCauseValue:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 iSUPCauseDiagnostics:

 $ref: '#/components/schemas/OctetString'

 CalledIdentityChange:

 type: object

 properties:

 calledIdentity:

 type: string

 changeTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 InterOperatorIdentifier:

 type: object

 properties:

 originatingIOI:

 type: string

 terminatingIOI:

 type: string

 EarlyMediaDescription:

 type: object

 properties:

 sDPTimeStamps:

 $ref: '#/components/schemas/SDPTimeStamps'

 sDPMediaComponent:

 type: array

 items:

 $ref: '#/components/schemas/SDPMediaComponent'

 minItems: 0

 sDPSessionDescription:

 type: array

 items:

 type: string

 minItems: 0

 SDPTimeStamps:

 type: object

 properties:

 sDPOfferTimestamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 sDPAnswerTimestamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 SDPMediaComponent:

 type: object

 properties:

 sDPMediaName:

 type: string

 SDPMediaDescription:

 type: array

 items:

 type: string

 minItems: 0

 localGWInsertedIndication:

 type: boolean

 ipRealmDefaultIndication:

 type: boolean

 transcoderInsertedIndication:

 type: boolean

 mediaInitiatorFlag:

 $ref: '#/components/schemas/MediaInitiatorFlag'

 mediaInitiatorParty:

 type: string

 threeGPPChargingId:

 $ref: '#/components/schemas/OctetString'

 accessNetworkChargingIdentifierValue:

 $ref: '#/components/schemas/OctetString'

 sDPType:

 $ref: '#/components/schemas/SDPType'

 ServerCapabilities:

 type: object

 properties:

 mandatoryCapability:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 minItems: 0

 optionalCapability :

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 minItems: 0

 serverName:

 type: array

 items:

 type: string

 minItems: 0

 TrunkGroupID:

 type: object

 properties:

 incomingTrunkGroupID:

 type: string

 outgoingTrunkGroupID:

 type: string

 MessageBody:

 type: object

 properties:

 contentType:

 type: string

 contentLength:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 contentDisposition:

 type: string

 originator:

 $ref: '#/components/schemas/OriginatorPartyType'

 required:

 - contentType

 - contentLength

 AccessTransferInformation:

 type: object

 properties:

 accessTransferType:

 $ref: '#/components/schemas/AccessTransferType'

 accessNetworkInformation:

 type: array

 items:

 $ref: '#/components/schemas/OctetString'

 minItems: 0

 cellularNetworkInformation:

 $ref: '#/components/schemas/OctetString'

 interUETransfer:

 $ref: '#/components/schemas/UETransferType'

 userEquipmentInfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

 instanceId:

 type: string

 relatedIMSChargingIdentifier:

 type: string

 relatedIMSChargingIdentifierNode:

 $ref: '#/components/schemas/IMSAddress'

 changeTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 AccessNetworkInfoChange:

 type: object

 properties:

 accessNetworkInformation:

 type: array

 items:

 $ref: '#/components/schemas/OctetString'

 minItems: 0

 cellularNetworkInformation:

 $ref: '#/components/schemas/OctetString'

 changeTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 NNIInformation:

 type: object

 properties:

 sessionDirection:

 $ref: '#/components/schemas/NNISessionDirection'

 nNIType:

 $ref: '#/components/schemas/NNIType'

 relationshipMode:

 $ref: '#/components/schemas/NNIRelationshipMode'

 neighbourNodeAddress:

 $ref: '#/components/schemas/IMSAddress'

 NotificationType:

 anyOf:

 - type: string

 enum:

 - REAUTHORIZATION

 - ABORT\_CHARGING

 - type: string

 NodeFunctionality:

 anyOf:

 - type: string

 enum:

 - AMF

 - SMF

 - SMS

 - PGW\_C\_SMF

 - NEFF # Included for backwards compatibility, shall not be used

 - SGW

 - I\_SMF

 - ePDG

 - CEF

 - NEF

 - MnS\_Producer

 - SGSN

 - type: string

 ChargingCharacteristicsSelectionMode:

 anyOf:

 - type: string

 enum:

 - HOME\_DEFAULT

 - ROAMING\_DEFAULT

 - VISITING\_DEFAULT

 - type: string

 TriggerType:

 anyOf:

 - type: string

 enum:

 - QUOTA\_THRESHOLD

 - QHT

 - FINAL

 - QUOTA\_EXHAUSTED

 - VALIDITY\_TIME

 - OTHER\_QUOTA\_TYPE

 - FORCED\_REAUTHORISATION

 - UNUSED\_QUOTA\_TIMER # Included for backwards compatibility, shall not be used

 - UNIT\_COUNT\_INACTIVITY\_TIMER

 - ABNORMAL\_RELEASE

 - QOS\_CHANGE

 - VOLUME\_LIMIT

 - TIME\_LIMIT

 - EVENT\_LIMIT

 - PLMN\_CHANGE

 - USER\_LOCATION\_CHANGE

 - RAT\_CHANGE

 - SESSION\_AMBR\_CHANGE

 - UE\_TIMEZONE\_CHANGE

 - TARIFF\_TIME\_CHANGE

 - MAX\_NUMBER\_OF\_CHANGES\_IN\_CHARGING\_CONDITIONS

 - MANAGEMENT\_INTERVENTION

 - CHANGE\_OF\_UE\_PRESENCE\_IN\_PRESENCE\_REPORTING\_AREA

 - CHANGE\_OF\_3GPP\_PS\_DATA\_OFF\_STATUS

 - SERVING\_NODE\_CHANGE

 - REMOVAL\_OF\_UPF

 - ADDITION\_OF\_UPF

 - INSERTION\_OF\_ISMF

 - REMOVAL\_OF\_ISMF

 - CHANGE\_OF\_ISMF

 - START\_OF\_SERVICE\_DATA\_FLOW

 - ECGI\_CHANGE

 - TAI\_CHANGE

 - HANDOVER\_CANCEL

 - HANDOVER\_START

 - HANDOVER\_COMPLETE

 - GFBR\_GUARANTEED\_STATUS\_CHANGE

 - ADDITION\_OF\_ACCESS

 - REMOVAL\_OF\_ACCESS

 - START\_OF\_SDF\_ADDITIONAL\_ACCESS

 - REDUNDANT\_TRANSMISSION\_CHANGE

 - CGI\_SAI\_CHANGE

 - RAI\_CHANGE

 - type: string

 FinalUnitAction:

 anyOf:

 - type: string

 enum:

 - TERMINATE

 - REDIRECT

 - RESTRICT\_ACCESS

 - type: string

 RedirectAddressType:

 anyOf:

 - type: string

 enum:

 - IPV4

 - IPV6

 - URL

 - type: string

 TriggerCategory:

 anyOf:

 - type: string

 enum:

 - IMMEDIATE\_REPORT

 - DEFERRED\_REPORT

 - type: string

 QuotaManagementIndicator:

 anyOf:

 - type: string

 enum:

 - ONLINE\_CHARGING

 - OFFLINE\_CHARGING

 - QUOTA\_MANAGEMENT\_SUSPENDED

 - type: string

 FailureHandling:

 anyOf:

 - type: string

 enum:

 - TERMINATE

 - CONTINUE

 - RETRY\_AND\_TERMINATE

 - type: string

 SessionFailover:

 anyOf:

 - type: string

 enum:

 - FAILOVER\_NOT\_SUPPORTED

 - FAILOVER\_SUPPORTED

 - type: string

 3GPPPSDataOffStatus:

 anyOf:

 - type: string

 enum:

 - ACTIVE

 - INACTIVE

 - type: string

 ResultCode:

 anyOf:

 - type: string

 enum:

 - SUCCESS

 - END\_USER\_SERVICE\_DENIED

 - QUOTA\_MANAGEMENT\_NOT\_APPLICABLE

 - QUOTA\_LIMIT\_REACHED

 - END\_USER\_SERVICE\_REJECTED

 - USER\_UNKNOWN

 - RATING\_FAILED

 - QUOTA\_MANAGEMENT

 - type: string

 PartialRecordMethod:

 anyOf:

 - type: string

 enum:

 - DEFAULT

 - INDIVIDUAL

 - type: string

 RoamerInOut:

 anyOf:

 - type: string

 enum:

 - IN\_BOUND

 - OUT\_BOUND

 - type: string

 SMMessageType:

 anyOf:

 - type: string

 enum:

 - SUBMISSION

 - DELIVERY\_REPORT

 - SM\_SERVICE\_REQUEST

 - DELIVERY

 - type: string

 SMPriority:

 anyOf:

 - type: string

 enum:

 - LOW

 - NORMAL

 - HIGH

 - type: string

 DeliveryReportRequested:

 anyOf:

 - type: string

 enum:

 - YES

 - NO

 - type: string

 InterfaceType:

 anyOf:

 - type: string

 enum:

 - UNKNOWN

 - MOBILE\_ORIGINATING

 - MOBILE\_TERMINATING

 - APPLICATION\_ORIGINATING

 - APPLICATION\_TERMINATING

 - type: string

 ClassIdentifier:

 anyOf:

 - type: string

 enum:

 - PERSONAL

 - ADVERTISEMENT

 - INFORMATIONAL

 - AUTO

 - type: string

 SMAddressType:

 anyOf:

 - type: string

 enum:

 - EMAIL\_ADDRESS

 - MSISDN

 - IPV4\_ADDRESS

 - IPV6\_ADDRESS

 - NUMERIC\_SHORTCODE

 - ALPHANUMERIC\_SHORTCODE

 - OTHER

 - IMSI

 - type: string

 SMAddresseeType:

 anyOf:

 - type: string

 enum:

 - TO

 - CC

 - BCC

 - type: string

 SMServiceType:

 anyOf:

 - type: string

 enum:

 - VAS4SMS\_SHORT\_MESSAGE\_CONTENT\_PROCESSING

 - VAS4SMS\_SHORT\_MESSAGE\_FORWARDING

 - VAS4SMS\_SHORT\_MESSAGE\_FORWARDING\_MULTIPLE\_SUBSCRIPTIONS

 - VAS4SMS\_SHORT\_MESSAGE\_FILTERING

 - VAS4SMS\_SHORT\_MESSAGE\_RECEIPT

 - VAS4SMS\_SHORT\_MESSAGE\_NETWORK\_STORAGE

 - VAS4SMS\_SHORT\_MESSAGE\_TO\_MULTIPLE\_DESTINATIONS

 - VAS4SMS\_SHORT\_MESSAGE\_VIRTUAL\_PRIVATE\_NETWORK(VPN)

 - VAS4SMS\_SHORT\_MESSAGE\_AUTO\_REPLY

 - VAS4SMS\_SHORT\_MESSAGE\_PERSONAL\_SIGNATURE

 - VAS4SMS\_SHORT\_MESSAGE\_DEFERRED\_DELIVERY

 - type: string

 ReplyPathRequested:

 anyOf:

 - type: string

 enum:

 - NO\_REPLY\_PATH\_SET

 - REPLY\_PATH\_SET

 - type: string

 oneTimeEventType:

 anyOf:

 - type: string

 enum:

 - IEC

 - PEC

 - type: string

 dnnSelectionMode:

 anyOf:

 - type: string

 enum:

 - VERIFIED

 - UE\_DNN\_NOT\_VERIFIED

 - NW\_DNN\_NOT\_VERIFIED

 - type: string

 APIDirection:

 anyOf:

 - type: string

 enum:

 - INVOCATION

 - NOTIFICATION

 - type: string

 RegistrationMessageType:

 anyOf:

 - type: string

 enum:

 - INITIAL

 - MOBILITY

 - PERIODIC

 - EMERGENCY

 - DEREGISTRATION

 - type: string

 MICOModeIndication:

 anyOf:

 - type: string

 enum:

 - MICO\_MODE

 - NO\_MICO\_MODE

 - type: string

 SmsIndication:

 anyOf:

 - type: string

 enum:

 - SMS\_SUPPORTED

 - SMS\_NOT\_SUPPORTED

 - type: string

 ManagementOperation:

 anyOf:

 - type: string

 enum:

 - CreateMOI

 - ModifyMOIAttributes

 - DeleteMOI

 - type: string

 ManagementOperationStatus:

 anyOf:

 - type: string

 enum:

 - OPERATION\_SUCCEEDED

 - OPERATION\_FAILED

 - type: string

 RedundantTransmissionType:

 anyOf:

 - type: string

 enum:

 - NON\_TRANSMISSION

 - END\_TO\_END\_USER\_PLANE\_PATHS

 - N3/N9

 - TRANSPORT\_LAYER

 - type: string

 VariablePartType:

 anyOf:

 - type: string

 enum:

 - INTEGER

 - NUMBER

 - TIME

 - DATE

 - CURRENCY

 - type: string

 QuotaConsumptionIndicator:

 anyOf:

 - type: string

 enum:

 - QUOTA\_NOT\_USED

 - QUOTA\_IS\_USED

 - type: string

 PlayToParty:

 anyOf:

 - type: string

 enum:

 - SERVED

 - REMOTE

 - type: string

 AnnouncementPrivacyIndicator:

 anyOf:

 - type: string

 enum:

 - NOT\_PRIVATE

 - PRIVATE

 - type: string

 SupplementaryServiceType:

 anyOf:

 - type: string

 enum:

 - OIP

 - OIR

 - TIP

 - TIR

 - HOLD

 - CB

 - CDIV

 - CW

 - MWI

 - CONF

 - FA

 - CCBS

 - CCNR

 - MCID

 - CAT

 - CUG

 - PNM

 - CRS

 - ECT

 - type: string

 SupplementaryServiceMode:

 anyOf:

 - type: string

 enum:

 - CFU

 - CFB

 - CFNR

 - CFNL

 - CD

 - CFNRC

 - ICB

 - OCB

 - ACR

 - BLIND\_TRANFER

 - CONSULTATIVE\_TRANFER

 - type: string

 ParticipantActionType:

 anyOf:

 - type: string

 enum:

 - CREATE

 - JOIN

 - INVITE\_INTO

 - QUIT

 - type: string

 TrafficForwardingWay:

 anyOf:

 - type: string

 enum:

 - N6

 - N19

 - LOCAL\_SWITCH

 - type: string

 IMSNodeFunctionality:

 anyOf:

 - type: string

 enum:

 - S\_CSCF

 - P\_CSCF

 - I\_CSCF

 - MRFC

 - MGCF

 - BGCF

 - AS

 - IBCF

 - S-GW

 - P-GW

 - HSGW

 - E-CSCF

 - MME

 - TRF

 - TF

 - ATCF

 - PROXY

 - EPDG

 - TDF

 - TWAG

 - SCEF

 - IWK\_SCEF

 - type: string

 RoleOfIMSNode:

 anyOf:

 - type: string

 enum:

 - ORIGINATING

 - TERMINATING

 - FORWARDING

 - type: string

 IMSSessionPriority:

 anyOf:

 - type: string

 enum:

 - PRIORITY\_0

 - PRIORITY\_1

 - PRIORITY\_2

 - PRIORITY\_3

 - PRIORITY\_4

 - type: string

 MediaInitiatorFlag:

 anyOf:

 - type: string

 enum:

 - CALLED\_PARTY

 - CALLING\_PARTY

 - UNKNOWN

 - type: string

 SDPType:

 anyOf:

 - type: string

 enum:

 - OFFER

 - ANSWER

 - type: string

 OriginatorPartyType:

 anyOf:

 - type: string

 enum:

 - CALLING

 - CALLED

 - type: string

 AccessTransferType:

 anyOf:

 - type: string

 enum:

 - PS\_TO\_CS

 - CS\_TO\_PS

 - PS\_TO\_PS

 - CS\_TO\_CS

 - type: string

 UETransferType:

 anyOf:

 - type: string

 enum:

 - INTRA\_UE

 - INTER\_UE

 - type: string

 NNISessionDirection:

 anyOf:

 - type: string

 enum:

 - INBOUND

 - OUTBOUND

 - type: string

 NNIType:

 anyOf:

 - type: string

 enum:

 - NON\_ROAMING

 - ROAMING\_NO\_LOOPBACK

 - ROAMING\_LOOPBACK

 - type: string

 NNIRelationshipMode:

 anyOf:

 - type: string

 enum:

 - TRUSTED

 - NON\_TRUSTED

 - type: string

 TADIdentifier:

 anyOf:

 - type: string

 enum:

 - CS

 - PS

 - type: string

|  |
| --- |
| **End of modifications** |