**3GPP TSG-SA5 Meeting #143-e *S5-223699***

e-meeting, 9 - 17 May 2022

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **32.255** | **CR** | **0393** | **rev** | **1** | **Current version:** | **17.5.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Correcting support of charging scenarios for roaming | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Ericsson LM | | | | | | | | | |
| ***Source to TSG:*** | S5 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | 5GSIMSCH | | | | |  | ***Date:*** | | | 2022-04-20 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Description for how IMS can be treated in the SMF is missing. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Adding a clause on how IMS traffic can be handled in the 5G data connectivity charging. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The impact on 5G data connectivity charging by IMS would be unspecified. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 2, 5.1.x (new) | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | First revision of S5-223099. | | | | | | | | |

|  |
| --- |
| **First change** |

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TS 32.240: "Telecommunication management; Charging management; Charging architecture and principles".

[2] 3GPP TS 32.260: "Telecommunication management; Charging management; IP Multimedia Subsystem (IMS) charging".

[3] - [50] Void.

[51] 3GPP TS 32.298: "Telecommunication management; Charging management; Charging Data Record (CDR) parameter description".

[52] 3GPP TS 32.297: "Telecommunication management; Charging management; Charging Data Record (CDR) file format and transfer".

[53] Void.

[54] 3GPP TS 32.295: "Telecommunication management; Charging management; Charging Data Record (CDR) transfer".

[55-56] Void.

[57] 3GPP TS 32.290: "Telecommunication management; Charging management; 5G system; Services, operations and procedures of charging using Service Based Interface (SBI)".

[58] 3GPP TS 32.291: " Telecommunication management; Charging management; 5G system; Charging service, stage 3".

[59] - [99] Void.

[100] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[101] 3GPP TS 22.115: "Service aspects; Charging and billing".

[102] 3GPP TS 22.261: "Service requirements for next generation new services and markets".

[103] - [199] Void

[200] 3GPP TS 23.501:"System Architecture for the 5G System".

[201] 3GPP TS 23.502:"Procedures for the 5G System".

[202] 3GPP TS 23.503:"Policy and Charging Control Framework for the 5G System; Stage 2".

[203] 3GPP TS 23.316: "Wireless and wireline convergence access support for the 5G System (5GS)".

[204] - [299] Void

[300] - [399] Void.

[400] - [499] Void.

[500] - [599] Void.

|  |
| --- |
| **Second change** |

### 5.1.x IMS Communication

#### 5.1.x.1 General

The SMF may support specific rating groups for IMS communication services based on e.g., QoS for the services to be able to correctly charge the service, for information on IMS communication service see TS 32.260 [2].

The charging identifier may be used for correlating the charging information from the IMS node, see TS 32.260 [2].

|  |
| --- |
| **End of changes** |