Identifies the number of currently contained idle TPs or GTPs that are free to be used for the intended management purpose.
Changes in the value of this attribute lead to a AVC notification.

Readable by NMS? Yes
Writeable by NMS? No
Invariant? No
