The attribute provide a means to store at the EMS a reference to the external representation of the TransmissionDescriptor (e.g., an XML file name). The contents of this attribute is opaque at the NML-EML interface and not utilized.
Changes in the value of this attribute lead to an AVC notification.

Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes
