Operation void getContainedCurrentCTPs (CIS SequenceOf Enums::LayerRate layerRateList = empty list, CIS SequenceOf ConnectionTerminationPoint ctps = NA), in Class TerminationPoint

Documentation
This operation is used to retrieve the "current" CTPs that are contained within a specific TP (PTP or CTP), at specific layer rates. A "current" CTP is defined as a CTP that is either cross-connectible or cross-connected, in the current mapping configuration.
Examples for contained Current TPs in different states of usage are contained in the associated supporting document ContainedTPs.
Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. INVALID_INPUT - Raised when layerRateList contains undefined rates.
3. NE_COMM_LOSS - Raised when communication to managed element is lost.
External Documents

SD1-6_ContainedTPs.pdf |

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
No change in the system.
Semantics

Arguments

layerRateList
/* in */ The list of rates of the contained current CTPs to be returned. An empty list indicates to the EMS to get all contained current CTPs (for all rates).
ctps
/* out */ Complete CTP object(s) for any contained CTP(s).