Indicates if the reroute (if allowed) should be computed by the network (YES), by the EMS (NO), or if it does not matter (NOT_SET).
Changes in the value of this attribute lead to a AVC notification.

Readable by NMS? Yes
Writeable by NMS? Yes
Invariant? No
