Operation void getAllEquipment (CIS SequenceOf Choice objects = NA), in Class ManagedElement

Documentation
This operation allows an NMS to request all of the equipments and equipment holders that are contained in the managed element.
Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
All Equipment and Equipment Holder objects returned.
Semantics

Arguments

objects
/* out */ List of Equipment objects, and/or list of EquipmentHolder objects.