Operation setCapacityAlarmThreshold (CIS SequenceOf Integer capacityAlarmThresholds = NA), in Class Log

Documentation
The operation sets the points at which an LogCapacityThresholdAlarm event will be generated.
Operation Exceptions:
1. NOT_IMPLEMENTED - If EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when input parameter is incorrectly formed.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
The log follows the requested behaviour.
Semantics

Arguments

capacityAlarmThresholds
/* in */ Contains a sequence of values that specifies, as a percentage of max log size, the points at which an LogCapacityThresholdAlarm event will be generated.