Class ServiceCategory {Analysis}

Documentation
Represents Service Categories used by traffic descriptor. The current Service Categories are defined as follows
(note that Guaranteed Bit Rate (GBR) is not defined because it is generally not used):
- CBR = Constant Bit Rate. For connections that require a sstatic amount of bandwidth that is continuously available
during the lifetime of the connection.
- rt-VBR = Real Time - Variable Bit Rate. For connections that require tightly constrained delay and delay variation.
- nrt-VBR = NonReal Time - Variable Bit Rate. For connections that have bursty traffic.
- UBR = Unspecified Bit Rate. For connections that do not require tightly constrained delay and delay variation.
- ABR = Available Bit Rate. For connections that do not require bounding the delay or delay variation. Not intended
for real-time applications.
- GFR = Guaranteed Frame Rate. For non-real-time applications that may require a minimum rate guarantee and can
benefit from accessing additional bandwidth dynamically available in the network.
- NA = Not Applicable.
Object Lifecycle: NA
Object Creation Notification Issued? No
Object Deletion Notification Issued? No

Parent Package | Enums | Abstract | No
Export Control | PublicAccess | Link Class for | None
Class Kind | NormalClass | Cardinality | n
Space |  | Concurrency | Sequential
Persistence | No |  |

Attributes

Name | Class | Type | Initial Value
CBR | ServiceCategory | Integer | 0
rt-VBR | ServiceCategory | Integer | 1
nrt-VBR | ServiceCategory | Integer | 2
UBR | ServiceCategory | Integer | 3
ABR | ServiceCategory | Integer | 4
GFR | ServiceCategory | Integer | 5
NA | ServiceCategory | Integer | 6