tmf854.v1 > ConnectionTerminationPoint_T > tpMappingMode
LOCATION: file:/xsd/networkResources/TerminationPoint.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The tpMappingMode Element
Within the facade definition, the CTP/FTP can act as an aggregate of associated G.805 TCPs, G.805 Termination Functions and G.805 CPs at one or more LayerRates. The CTP is contained within a PTP or FTP. The TerminationMode attribute indicates and controls the connection of the named CP at a specified LayerRate to the dedicated G.805 TCP and associated G.805 Termination Function at the same LayerRate within the CTP/FTP. The TerminationMode is used, for example, to control the Termination and mapping to VT1.5 of an STS1 Trail within an OC3 port. This capability could potentially be used to terminate an STS1 backbone Trail within a lower order mux that has the capability to alternatively cross-connect the STS1 unterminated. The same capability is used in SDH and is potentially applicable to any LayerRate.
Element ConnectionTerminationPoint_T/tpMappingMode : TerminationMode_T [0 .. 1]
The tpMappingMode element can have "xsi:nil" as an attribute. The tpMappingMode element in XML instance can be substituted with other elements.

XML Instance
Within the facade definition, the CTP/FTP can act as an aggregate of associated G.805 TCPs, G.805 Termination Functions and G.805 CPs at one or more LayerRates. The CTP is contained within a PTP or FTP. The TerminationMode attribute indicates and controls the connection of the named CP at a specified LayerRate to the dedicated G.805 TCP and associated G.805 Termination Function at the same LayerRate within the CTP/FTP. The TerminationMode is used, for example, to control the Termination and mapping to VT1.5 of an STS1 Trail within an OC3 port. This capability could potentially be used to terminate an STS1 backbone Trail within a lower order mux that has the capability to alternatively cross-connect the STS1 unterminated. The same capability is used in SDH and is potentially applicable to any LayerRate. <tpMappingMode>TerminationMode_T</tpMappingMode>

﻿

Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes

﻿

XML
-<xsd:element minOccurs="0" name="tpMappingMode" nillable="true" type="TerminationMode_T"> -<xsd:annotation> <xsd:documentation> Within the facade definition, the CTP/FTP can act as an aggregate of associated G.805 TCPs, G.805 Termination Functions and G.805 CPs at one or more LayerRates. The CTP is contained within a PTP or FTP. The TerminationMode attribute indicates and controls the connection of the named CP at a specified LayerRate to the dedicated G.805 TCP and associated G.805 Termination Function at the same LayerRate within the CTP/FTP. The TerminationMode is used, for example, to control the Termination and mapping to VT1.5 of an STS1 Trail within an OC3 port. This capability could potentially be used to terminate an STS1 backbone Trail within a lower order mux that has the capability to alternatively cross-connect the STS1 unterminated. The same capability is used in SDH and is potentially applicable to any LayerRate. </xsd:documentation> </xsd:annotation> </xsd:element>

﻿

Uses
Type (1) TerminationMode_T

Used-By

Generated by WSDLdoc ©