CIS Integer priority = 0, in Class SubnetworkConnection

Documentation
The attribute defines the priority of the SNC.
Allowed values are = "0" , "1" , "2" , ... where zero (0) is the highest priority.
Changes in the value of this attribute lead to a AVC notification.
Readable by NMS? Yes
Writeable by NMS? Yes
Invariant? No

Export Control | PrivateAccess | Containment | Unspecified
Static | No | Derived | No