CIS CharacterString X.733::BackedUpStatus = Absent from notification, in Class AlarmInformation

Documentation
The optional Backed Up Status parameter, when present in an alarm notification, specifies whether or not the object emitting the alarm has been backed-up, and services provided to the user have, therefore, not been disrupted.
This is consistent with the ITU-T X.733 definition.
Value is one of the following:
- "BACKED_UP"
- "NOT_BACKED_UP".
Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes

Export Control | PrivateAccess | Containment | Unspecified
Static | No | Derived | No