tmf854.v1 > TPData_T LOCATION: file:/xsd/networkResources/SubnetworkConnection.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The TPData_T Complex Type
This aggregate defines a set of attributes associated with a TP.

Local elements (5)
  tpName tpMappingMode transmissionParams ingressTransmissionDescriptorName egressTransmissionDescriptorName

Complex Type TPData_T
The TPData_T type does not allow mixed content. There is no restriction on type derivation.

XML Instance
<...> -Begin All [1...1] Specifies aEnd termination point. <tpName extVersion="xsd:string" extAuthor="xsd:string" tmf854Version="TMF854_Version_T">NamingAttributes_T</tpName> [1..1] The mapping mode to put the TP in. <tpMappingMode>TerminationMode_T</tpMappingMode> [0..1] When used as output to the NMS, this is the transmission parameters of the TP. When used as input to the EMS, this is a "delta" list that needs to be applied to the specified TP. Only a subset of the parameters may be specified in the list, and only those should be applied in the NE. If the list is empty then this means do nothing. To remove a parameter from the list, "-" should be specified in the value part of the structure. When a BLSR connection is created, the SPRING_NodeId parameter should be provided for the aEnd and zEnd CTPs. <transmissionParams>LayeredParametersList_T</transmissionParams> [0..1] A connection termination point may have an optional reference to an ingress (incoming)Transmission Descriptor. The Descriptor name will be empty if there is no associated Descriptor. <ingressTransmissionDescriptorName extVersion="xsd:string" extAuthor="xsd:string" tmf854Version="TMF854_Version_T">NamingAttributes_T</ingressTransmissionDescriptorName> [0..1] A connection termination point may have an optional reference to an egress (outgoing)Transmission Descriptor. The Transmission Descriptor name will be empty if there is no associated Descriptor. <egressTransmissionDescriptorName extVersion="xsd:string" extAuthor="xsd:string" tmf854Version="TMF854_Version_T">NamingAttributes_T</egressTransmissionDescriptorName> [0..1] End All </...>

﻿

Attributes |
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".

﻿

XML
-<xsd:complexType name="TPData_T"> -<xsd:annotation> <xsd:documentation> This aggregate defines a set of attributes associated with a TP. </xsd:documentation> </xsd:annotation> -<xsd:all> -<xsd:element name="tpName" type="NamingAttributes_T"> -<xsd:annotation> <xsd:documentation> Specifies aEnd termination point. </xsd:documentation> </xsd:annotation> </xsd:element> -<xsd:element minOccurs="0" name="tpMappingMode" nillable="true" type="TerminationMode_T"> -<xsd:annotation> <xsd:documentation> The mapping mode to put the TP in. </xsd:documentation> </xsd:annotation> </xsd:element> -<xsd:element minOccurs="0" name="transmissionParams" nillable="true" type="LayeredParametersList_T"> -<xsd:annotation> <xsd:documentation> When used as output to the NMS, this is the transmission parameters of the TP. When used as input to the EMS, this is a "delta" list that needs to be applied to the specified TP. Only a subset of the parameters may be specified in the list, and only those should be applied in the NE. If the list is empty then this means do nothing. To remove a parameter from the list, "-" should be specified in the value part of the structure. When a BLSR connection is created, the SPRING_NodeId parameter should be provided for the aEnd and zEnd CTPs. </xsd:documentation> </xsd:annotation> </xsd:element> -<xsd:element minOccurs="0" name="ingressTransmissionDescriptorName" nillable="true" type="NamingAttributes_T"> -<xsd:annotation> <xsd:documentation> A connection termination point may have an optional reference to an ingress (incoming)Transmission Descriptor. The Descriptor name will be empty if there is no associated Descriptor. </xsd:documentation> </xsd:annotation> </xsd:element> -<xsd:element minOccurs="0" name="egressTransmissionDescriptorName" nillable="true" type="NamingAttributes_T"> -<xsd:annotation> <xsd:documentation> A connection termination point may have an optional reference to an egress (outgoing)Transmission Descriptor. The Transmission Descriptor name will be empty if there is no associated Descriptor. </xsd:documentation> </xsd:annotation> </xsd:element> </xsd:all> </xsd:complexType>

﻿

Uses
Type (3) LayeredParametersList_T NamingAttributes_T TerminationMode_T

Used-By
Element (1) TPDataList_T/tpData

Generated by WSDLdoc ©